(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32WB05KZVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "STM32WB05KZVx"
			(at 7.62 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.7x3.7mm"
			(at -15.24 -30.48 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb05kz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 24KB RAM, 20 GPIO, VFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32WB0 STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB05KZVx_0_1")
		(symbol "STM32WB05KZVx_1_1"
			(pin power_in line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "RSTN")
				(number "29")
			)
			(pin power_in line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "VLXSD")
				(number "25")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "VFBSD")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "OSCIN")
				(number "17")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "OSCOUT")
				(number "16")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "RF1")
				(number "14")
				(alternate "RADIO_RF1" bidirectional line)
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDDA_VCAP")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "VSSSD")
				(number "26")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDRF")
				(number "15")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDDSD")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PWR_WKUP12" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PWR_WKUP13" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "6")
				(alternate "ADC1_VINM2" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "PWR_WKUP14" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "5")
				(alternate "ADC1_VINP2" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "PWR_WKUP15" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "9")
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "RADIO_RX_SEQUENCE" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "10")
				(alternate "I2S3_WS" bidirectional line)
				(alternate "PWR_WKUP9" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP10" bidirectional line)
				(alternate "RADIO_TX_SEQUENCE" bidirectional line)
				(alternate "RCC_LCO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "12")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "PWR_WKUP11" bidirectional line)
				(alternate "RADIO_RX_SEQUENCE" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "4")
				(alternate "ADC1_VINM1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP0" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB1")
				(number "3")
				(alternate "ADC1_VINP1" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "2")
				(alternate "ADC1_VINM0" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_2" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC1_VINP0" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_3" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "31")
				(alternate "ADC1_VINM3" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_4" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "30")
				(alternate "ADC1_VINP3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_5" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "23")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_6" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "22")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RADIO_ACTIVITY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB12")
				(number "21")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP16" bidirectional line)
				(alternate "RCC_LCO" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB13")
				(number "20")
				(alternate "PWR_WKUP17" bidirectional line)
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB14")
				(number "19")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "PWR_WKUP18" bidirectional line)
				(alternate "RADIO_TX_SEQUENCE" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB15")
				(number "18")
				(alternate "PWR_WKUP19" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB06KCVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "STM32WB06KCVx"
			(at 7.62 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.7x3.7mm"
			(at -15.24 -30.48 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb06kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 32KB RAM, 20 GPIO, VFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32WB0 STM32WBx6"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB06KCVx_0_1")
		(symbol "STM32WB06KCVx_1_1"
			(pin power_in line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "RSTN")
				(number "26")
			)
			(pin power_in line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "VLXSD")
				(number "24")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "VFBSD")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "OSCIN")
				(number "17")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "OSCOUT")
				(number "16")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "RF1")
				(number "14")
				(alternate "RADIO_RF1" bidirectional line)
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDDA_VCAP")
				(number "27")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "VSSSD")
				(number "23")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDRF")
				(number "15")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDDSD")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "PWR_WKUP12" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWR_WKUP13" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "PWR_WKUP14" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "PWR_WKUP15" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "8")
				(alternate "PWR_WKUP20" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "RADIO_RX_SEQUENCE" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "7")
				(alternate "I2S3_WS" bidirectional line)
				(alternate "PWR_WKUP21" bidirectional line)
				(alternate "PWR_WKUP9" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "6")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "PWR_WKUP10" bidirectional line)
				(alternate "PWR_WKUP22" bidirectional line)
				(alternate "RADIO_TX_SEQUENCE" bidirectional line)
				(alternate "RCC_LCO" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "5")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "PWR_WKUP11" bidirectional line)
				(alternate "PWR_WKUP23" bidirectional line)
				(alternate "RADIO_RX_SEQUENCE" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "4")
				(alternate "ADC1_VINM1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP0" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB1")
				(number "3")
				(alternate "ADC1_PDM_CLK" bidirectional line)
				(alternate "ADC1_VINP1" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "2")
				(alternate "ADC1_PDM_DATA" bidirectional line)
				(alternate "ADC1_PGA_CAP0" bidirectional line)
				(alternate "ADC1_VINM0" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC1_PGA_CAP1" bidirectional line)
				(alternate "ADC1_VINP0" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "31")
				(alternate "ADC1_PDM_DATA" bidirectional line)
				(alternate "ADC1_PGA_VIN" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "30")
				(alternate "ADC1_PDM_CLK" bidirectional line)
				(alternate "ADC1_PGA_VBIAS_MIC" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB12")
				(number "21")
				(alternate "ADC1_PDM_DATA" bidirectional line)
				(alternate "RCC_LCO" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB13")
				(number "20")
				(alternate "ADC1_PDM_CLK" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB14")
				(number "19")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB15")
				(number "18")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "RADIO_TX_SEQUENCE" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB07KCVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "STM32WB07KCVx"
			(at 7.62 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.7x3.7mm"
			(at -15.24 -30.48 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb07kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 64KB RAM, 20 GPIO, VFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32WB0 STM32WBx7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB07KCVx_0_1")
		(symbol "STM32WB07KCVx_1_1"
			(pin power_in line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "RSTN")
				(number "26")
			)
			(pin power_in line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "VLXSD")
				(number "24")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "VFBSD")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "OSCIN")
				(number "17")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "OSCOUT")
				(number "16")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "RF1")
				(number "14")
				(alternate "RADIO_RF1" bidirectional line)
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDDA_VCAP")
				(number "27")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "VSSSD")
				(number "23")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDRF")
				(number "15")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDDSD")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "PWR_WKUP12" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWR_WKUP13" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "PWR_WKUP14" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "PWR_WKUP15" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "8")
				(alternate "PWR_WKUP20" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "RADIO_RX_SEQUENCE" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "7")
				(alternate "I2S3_WS" bidirectional line)
				(alternate "PWR_WKUP21" bidirectional line)
				(alternate "PWR_WKUP9" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "6")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "PWR_WKUP10" bidirectional line)
				(alternate "PWR_WKUP22" bidirectional line)
				(alternate "RADIO_TX_SEQUENCE" bidirectional line)
				(alternate "RCC_LCO" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "5")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "PWR_WKUP11" bidirectional line)
				(alternate "PWR_WKUP23" bidirectional line)
				(alternate "RADIO_RX_SEQUENCE" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "4")
				(alternate "ADC1_VINM1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP0" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB1")
				(number "3")
				(alternate "ADC1_PDM_CLK" bidirectional line)
				(alternate "ADC1_VINP1" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "2")
				(alternate "ADC1_PDM_DATA" bidirectional line)
				(alternate "ADC1_PGA_CAP0" bidirectional line)
				(alternate "ADC1_VINM0" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC1_PGA_CAP1" bidirectional line)
				(alternate "ADC1_VINP0" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "31")
				(alternate "ADC1_PDM_DATA" bidirectional line)
				(alternate "ADC1_PGA_VIN" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "30")
				(alternate "ADC1_PDM_CLK" bidirectional line)
				(alternate "ADC1_PGA_VBIAS_MIC" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB12")
				(number "21")
				(alternate "ADC1_PDM_DATA" bidirectional line)
				(alternate "RCC_LCO" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB13")
				(number "20")
				(alternate "ADC1_PDM_CLK" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB14")
				(number "19")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB15")
				(number "18")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "RADIO_TX_SEQUENCE" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB09KEVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "STM32WB09KEVx"
			(at 7.62 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.7x3.7mm"
			(at -15.24 -30.48 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb09ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 64KB RAM, 20 GPIO, VFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32WB0 STM32WBx9"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB09KEVx_0_1")
		(symbol "STM32WB09KEVx_1_1"
			(pin power_in line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "RSTN")
				(number "29")
			)
			(pin power_in line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "VLXSD")
				(number "25")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "VFBSD")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "OSCIN")
				(number "17")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "OSCOUT")
				(number "16")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "RF1")
				(number "14")
				(alternate "RADIO_RF1" bidirectional line)
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDDA_VCAP")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "VSSSD")
				(number "26")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDRF")
				(number "15")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDDSD")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PWR_WKUP12" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PWR_WKUP13" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "6")
				(alternate "ADC1_VINM2" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "PWR_WKUP14" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "5")
				(alternate "ADC1_VINP2" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "PWR_WKUP15" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "9")
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "RADIO_RX_SEQUENCE" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "10")
				(alternate "I2S3_WS" bidirectional line)
				(alternate "PWR_WKUP9" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP10" bidirectional line)
				(alternate "RADIO_TX_SEQUENCE" bidirectional line)
				(alternate "RCC_LCO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "12")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "PWR_WKUP11" bidirectional line)
				(alternate "RADIO_RX_SEQUENCE" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "4")
				(alternate "ADC1_VINM1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP0" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB1")
				(number "3")
				(alternate "ADC1_VINP1" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "2")
				(alternate "ADC1_VINM0" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_2" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC1_VINP0" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_3" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "31")
				(alternate "ADC1_VINM3" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_4" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "30")
				(alternate "ADC1_VINP3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_5" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "23")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RADIO_ANTENNA_ID_6" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "22")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RADIO_ACTIVITY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB12")
				(number "21")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP16" bidirectional line)
				(alternate "RCC_LCO" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB13")
				(number "20")
				(alternate "PWR_WKUP17" bidirectional line)
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB14")
				(number "19")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "PWR_WKUP18" bidirectional line)
				(alternate "RADIO_TX_SEQUENCE" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB15")
				(number "18")
				(alternate "PWR_WKUP19" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB10CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 36.83 0)
		)
		(property "Value" "STM32WB10CCUx"
			(at 15.24 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -27.94 -33.02 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb10cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 320KB flash, 48KB RAM, 64 MHz, 2.0-3.6V, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB10CCUx_0_1")
		(symbol "STM32WB10CCUx_1_1"
			(pin input line
				(at -30.48 30.48 0)
				(length 2.54)
				(name "NRST(PB11)")
				(number "7")
			)
			(pin input line
				(at -30.48 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "25")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -30.48 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 2.54)
				(name "RF1")
				(number "21")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 2.54)
				(name "PH3")
				(number "4")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 2.54)
				(name "PE4")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "28")
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "29")
				(alternate "LPTIM2_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 2.54)
				(name "PB3")
				(number "43")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 2.54)
				(name "PB4")
				(number "44")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 2.54)
				(name "PB5")
				(number "45")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 2.54)
				(name "PB6")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 2.54)
				(name "PB7")
				(number "47")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 2.54)
				(name "PB8")
				(number "5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 2.54)
				(name "PB9")
				(number "6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin no_connect line
				(at -27.94 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "27")
			)
			(pin no_connect line
				(at -27.94 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "26")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "34")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSRF")
				(number "22")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 12.7 38.1 270)
				(length 2.54)
				(name "VDDRF")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "13")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "14")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "18")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "36")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 2.54)
				(name "PA12")
				(number "38")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "39")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "42")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB15CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 39.37 0)
		)
		(property "Value" "STM32WB15CCUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb15cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 320KB flash, 48KB RAM, 64 MHz, 1.71-3.6V, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB15CCUx_0_1")
		(symbol "STM32WB15CCUx_1_1"
			(pin input line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "NRST(PB11)")
				(number "7")
			)
			(pin power_in line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "33")
			)
			(pin input line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "OSC_IN")
				(number "25")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "RF1")
				(number "21")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PH3")
				(number "4")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PE4")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -25.4 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "27")
			)
			(pin no_connect line
				(at -25.4 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "26")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSSRF")
				(number "22")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "32")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "23")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "13")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "14")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "18")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "36")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "38")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA13")
				(number "39")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "42")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB1")
				(number "29")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB3")
				(number "43")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB4")
				(number "44")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB5")
				(number "45")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB6")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB7")
				(number "47")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB8")
				(number "5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB9")
				(number "6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB15CCUxE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 46.99 0)
		)
		(property "Value" "STM32WB15CCUxE"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb15cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 320KB flash, 48KB RAM, 64 MHz, 1.71-3.6V, 36 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB15CCUxE_0_1")
		(symbol "STM32WB15CCUxE_1_1"
			(pin input line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "NRST(PB11)")
				(number "7")
			)
			(pin input line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "OSC_IN")
				(number "25")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "RF1")
				(number "22")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PH3")
				(number "4")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PE4")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PC1")
				(number "40")
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "27")
			)
			(pin no_connect line
				(at -20.32 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "26")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "21")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "23")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "36")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "38")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "39")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "42")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "29")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "43")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "44")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "45")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "47")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "3")
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "13")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "TIM2_CH1" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB15CCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 36.83 0)
		)
		(property "Value" "STM32WB15CCYx"
			(at 12.7 36.83 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_3.3x3.38mm_Layout7x7_P0.4mm_Offcenter"
			(at -25.4 -33.02 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb15cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 320KB flash, 48KB RAM, 64 MHz, 1.71-3.6V, 26 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*3.3x3.38mm*Layout7x7*P0.4mm*Offcenter*"
			(at 0 0 0)
		)
		(symbol "STM32WB15CCYx_0_1")
		(symbol "STM32WB15CCYx_1_1"
			(pin input line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "NRST(PB11)")
				(number "C7")
			)
			(pin power_in line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "B1")
			)
			(pin input line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "OSC_IN")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "F2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "D2")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "RF1")
				(number "G4")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PH3")
				(number "B6")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC14")
				(number "A7")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC15")
				(number "B7")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -25.4 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "F3")
			)
			(pin no_connect line
				(at -25.4 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "E3")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "C5")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "A4")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "C3")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "D7")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSSRF")
				(number "F4")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G3")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "G5")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "C1")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "E7")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDDRF")
				(number "G2")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "A1")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "C4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "F7")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "E6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "D5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "G7")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "D4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "F6")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "E5")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "G6")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "D3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "A2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA12")
				(number "A3")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B3")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "E2")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB1")
				(number "E1")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB2")
				(number "E4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB7")
				(number "A6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB8")
				(number "C6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB30CEUxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 36.83 0)
		)
		(property "Value" "STM32WB30CEUxA"
			(at 15.24 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -22.86 -33.02 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb30ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 96KB RAM, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB30CEUxA_0_1")
		(symbol "STM32WB30CEUxA_1_1"
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "25")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "RF1")
				(number "21")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PH3")
				(number "4")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PE4")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "28")
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "29")
				(alternate "LPTIM2_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB3")
				(number "43")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB4")
				(number "44")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB5")
				(number "45")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB6")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB7")
				(number "47")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB8")
				(number "5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PB9")
				(number "6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin no_connect line
				(at -22.86 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "27")
			)
			(pin no_connect line
				(at -22.86 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "26")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "34")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSRF")
				(number "22")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 12.7 38.1 270)
				(length 2.54)
				(name "VDDRF")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "13")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "14")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "16")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "18")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "36")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA12")
				(number "38")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "39")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "42")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB35C_C-E_UxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WB35C_C-E_UxA"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb35cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256-512KB flash, 96KB RAM, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB35C_C-E_UxA_0_1")
		(symbol "STM32WB35C_C-E_UxA_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "33")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "OSC_IN")
				(number "25")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "RF1")
				(number "21")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PH3")
				(number "4")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PE4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "27")
			)
			(pin no_connect line
				(at -20.32 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "26")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSSRF")
				(number "22")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "32")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "23")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "34")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDUSB")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "13")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "14")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "16")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "18")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "36")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "38")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "39")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "42")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB1")
				(number "29")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB3")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB4")
				(number "44")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB5")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB6")
				(number "46")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB7")
				(number "47")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB8")
				(number "5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB9")
				(number "6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB50CGUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 36.83 0)
		)
		(property "Value" "STM32WB50CGUx"
			(at 15.24 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -22.86 -33.02 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb50cg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 1024KB flash, 128KB RAM, 64 MHz, 2.0-3.6V, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB50CGUx_0_1")
		(symbol "STM32WB50CGUx_1_1"
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "25")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "RF1")
				(number "21")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PH3")
				(number "4")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PE4")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "28")
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "29")
				(alternate "LPTIM2_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB3")
				(number "43")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB4")
				(number "44")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB5")
				(number "45")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB6")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB7")
				(number "47")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB8")
				(number "5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PB9")
				(number "6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin no_connect line
				(at -22.86 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "27")
			)
			(pin no_connect line
				(at -22.86 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "26")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "34")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSRF")
				(number "22")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 12.7 38.1 270)
				(length 2.54)
				(name "VDDRF")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "13")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "14")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "16")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "18")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "36")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA12")
				(number "38")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "39")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "42")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WB55CCUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 64 MHz, 1.71-3.6V, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB55CCUx_0_1")
		(symbol "STM32WB55CCUx_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "33")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "OSC_IN")
				(number "25")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "RF1")
				(number "21")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PH3")
				(number "4")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PE4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "27")
			)
			(pin no_connect line
				(at -20.32 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "26")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSSRF")
				(number "22")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "32")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "23")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "34")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDUSB")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "13")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "14")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "16")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "18")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "36")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "38")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "39")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "42")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB1")
				(number "29")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB3")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB4")
				(number "44")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB5")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB6")
				(number "46")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB7")
				(number "47")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB8")
				(number "5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB9")
				(number "6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WB55CEUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 256KB RAM, 64 MHz, 1.71-3.6V, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB55CEUx_0_1")
		(symbol "STM32WB55CEUx_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "33")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "OSC_IN")
				(number "25")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "RF1")
				(number "21")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PH3")
				(number "4")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PE4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "27")
			)
			(pin no_connect line
				(at -20.32 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "26")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSSRF")
				(number "22")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "32")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "23")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "34")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDUSB")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "13")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "14")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "16")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "18")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "36")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "38")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "39")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "42")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB1")
				(number "29")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB3")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB4")
				(number "44")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB5")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB6")
				(number "46")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB7")
				(number "47")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB8")
				(number "5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB9")
				(number "6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55CGUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WB55CGUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55cg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 1024KB flash, 256KB RAM, 64 MHz, 1.71-3.6V, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB55CGUx_0_1")
		(symbol "STM32WB55CGUx_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "33")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "OSC_IN")
				(number "25")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "RF1")
				(number "21")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PH3")
				(number "4")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PE4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "27")
			)
			(pin no_connect line
				(at -20.32 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "26")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSSRF")
				(number "22")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "32")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "23")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "34")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDUSB")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "11")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "12")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "13")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "14")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "16")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "18")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "36")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "38")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "39")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "42")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB1")
				(number "29")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB3")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB4")
				(number "44")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB5")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB6")
				(number "46")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB7")
				(number "47")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB8")
				(number "5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB9")
				(number "6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55RCVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 46.99 0)
		)
		(property "Value" "STM32WB55RCVx"
			(at 12.7 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at -20.32 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 64 MHz, 1.71-3.6V, 49 GPIO, VFQFPN68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB55RCVx_0_1")
		(symbol "STM32WB55RCVx_1_1"
			(pin input line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "8")
			)
			(pin power_in line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "43")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "13")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "OSC_IN")
				(number "35")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "34")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "RF1")
				(number "31")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PH3")
				(number "5")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PD0")
				(number "61")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PD1")
				(number "62")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC0")
				(number "9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC1")
				(number "10")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC2")
				(number "11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC3")
				(number "12")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PC6")
				(number "50")
				(alternate "LCD_SEG24" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PC10")
				(number "58")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PC11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PC12")
				(number "60")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "37")
			)
			(pin no_connect line
				(at -20.32 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "36")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "45")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "69")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "68")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "32")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "42")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "33")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "44")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "55")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "20")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "21")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "22")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "23")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "51")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "53")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "54")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "56")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "57")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "38")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "39")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "27")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "63")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "64")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "65")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "66")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "67")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "7")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "29")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "46")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "47")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "48")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "49")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55REVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 46.99 0)
		)
		(property "Value" "STM32WB55REVx"
			(at 12.7 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at -20.32 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 256KB RAM, 64 MHz, 1.71-3.6V, 49 GPIO, VFQFPN68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB55REVx_0_1")
		(symbol "STM32WB55REVx_1_1"
			(pin input line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "8")
			)
			(pin power_in line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "43")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "13")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "OSC_IN")
				(number "35")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "34")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "RF1")
				(number "31")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PH3")
				(number "5")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PD0")
				(number "61")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PD1")
				(number "62")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC0")
				(number "9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC1")
				(number "10")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC2")
				(number "11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC3")
				(number "12")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PC6")
				(number "50")
				(alternate "LCD_SEG24" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PC10")
				(number "58")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PC11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PC12")
				(number "60")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "37")
			)
			(pin no_connect line
				(at -20.32 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "36")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "45")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "69")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "68")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "32")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "42")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "33")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "44")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "55")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "20")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "21")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "22")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "23")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "51")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "53")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "54")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "56")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "57")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "38")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "39")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "27")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "63")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "64")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "65")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "66")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "67")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "7")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "29")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "46")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "47")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "48")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "49")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55RGVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 46.99 0)
		)
		(property "Value" "STM32WB55RGVx"
			(at 12.7 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at -20.32 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 1024KB flash, 256KB RAM, 64 MHz, 1.71-3.6V, 49 GPIO, VFQFPN68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB55RGVx_0_1")
		(symbol "STM32WB55RGVx_1_1"
			(pin input line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "8")
			)
			(pin power_in line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "43")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "13")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "OSC_IN")
				(number "35")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "34")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "RF1")
				(number "31")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PH3")
				(number "5")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PD0")
				(number "61")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PD1")
				(number "62")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC0")
				(number "9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC1")
				(number "10")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC2")
				(number "11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC3")
				(number "12")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PC6")
				(number "50")
				(alternate "LCD_SEG24" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PC10")
				(number "58")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PC11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PC12")
				(number "60")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "AT1")
				(number "37")
			)
			(pin no_connect line
				(at -20.32 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "AT0")
				(number "36")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "45")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "69")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "68")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "32")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "42")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "33")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "44")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "55")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "20")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "21")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "22")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "23")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "51")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "53")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "54")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "56")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "57")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "38")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "39")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "27")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "63")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "64")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "65")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "66")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "67")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "7")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "29")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "46")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "47")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "48")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "49")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55VCQx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 69.85 0)
		)
		(property "Value" "STM32WB55VCQx"
			(at 20.32 69.85 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-129_7x7mm_Layout13x13_P0.5mm"
			(at -30.48 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 64 MHz, 1.71-3.6V, 72 GPIO, UFBGA129"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB55VCQx_0_1")
		(symbol "STM32WB55VCQx_1_1"
			(pin input line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin power_in line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "F11")
			)
			(pin power_in line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "G11")
			)
			(pin input line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "OSC_IN")
				(number "M13")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "N13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "VFBSMPS")
				(number "H11")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "RF1")
				(number "M9")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PH1")
				(number "G2")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PH3")
				(number "G1")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "B2")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "A1")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "B1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "H12")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "H13")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PD0")
				(number "B11")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PD1")
				(number "C7")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PD3")
				(number "D8")
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PD4")
				(number "C6")
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PD6")
				(number "D6")
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PD7")
				(number "C5")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PD8")
				(number "B6")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PD9")
				(number "D4")
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PD10")
				(number "A7")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SYS_TRIG_INOUT" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PD11")
				(number "B5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PD12")
				(number "B4")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PD13")
				(number "C1")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PD14")
				(number "D3")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PD15")
				(number "C2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin no_connect line
				(at -30.48 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "AT1")
				(number "K12")
			)
			(pin no_connect line
				(at -30.48 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "AT0")
				(number "K11")
			)
			(pin power_in line
				(at -17.78 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D2")
			)
			(pin power_in line
				(at -15.24 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at -12.7 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H8")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "K3")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B12")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C11")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F3")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J11")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K4")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "A8")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "F2")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K10")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSRF")
				(number "K8")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L10")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L11")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L7")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L8")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L9")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M10")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M11")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M12")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M8")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "N11")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "N8")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "J12")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "G12")
			)
			(pin passive line
				(at 5.08 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSSMPS")
				(number "G13")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "N7")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDRF")
				(number "N12")
			)
			(pin power_in line
				(at 12.7 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "F12")
			)
			(pin power_in line
				(at 15.24 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "F13")
			)
			(pin power_in line
				(at 17.78 73.66 270)
				(length 5.08)
				(name "VDDUSB")
				(number "A12")
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "M1")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "L2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "N1")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "M2")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "N2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "M3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "N3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "M4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "L4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A13")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "C10")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "C9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "L13")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "L12")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "N6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "C4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "A3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "A2")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PB8")
				(number "G3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "H4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "M6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "H10")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "E12")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "E11")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "F10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "H1")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "J3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "M5")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "D10")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "D12")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "D11")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "C13")
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B9")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "F4")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "E3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55VCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 69.85 0)
		)
		(property "Value" "STM32WB55VCYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-100_4.4x4.38mm_Layout10x10_P0.4mm_Offcenter"
			(at -22.86 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 64 MHz, 1.71-3.6V, 72 GPIO, WLCSP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.4x4.38mm*Layout10x10*P0.4mm*Offcenter*"
			(at 0 0 0)
		)
		(symbol "STM32WB55VCYx_0_1")
		(symbol "STM32WB55VCYx_1_1"
			(pin input line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "F9")
			)
			(pin power_in line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "E1")
			)
			(pin input line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "VREF+")
				(number "H8")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "OSC_IN")
				(number "J1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "J2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "VFBSMPS")
				(number "F2")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "RF1")
				(number "K4")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PH0")
				(number "E10")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PH1")
				(number "E9")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PH3")
				(number "E8")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C8")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PE1")
				(number "B10")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PE2")
				(number "E6")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PE3")
				(number "G2")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PE4")
				(number "G1")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C4")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PD1")
				(number "C3")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PD2")
				(number "A7")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PD3")
				(number "C2")
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PD4")
				(number "D3")
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PD5")
				(number "B7")
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PD6")
				(number "C6")
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PD7")
				(number "A8")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PD8")
				(number "D4")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PD9")
				(number "D5")
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PD10")
				(number "E4")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SYS_TRIG_INOUT" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PD11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PD12")
				(number "B8")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PD13")
				(number "C9")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PD14")
				(number "D8")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PD15")
				(number "E7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin no_connect line
				(at -22.86 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "AT1")
				(number "H4")
			)
			(pin no_connect line
				(at -22.86 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "AT0")
				(number "H3")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "C10")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "J10")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "K5")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "H10")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "H9")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSRF")
				(number "J4")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K1")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K2")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K3")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDRF")
				(number "J3")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "F1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "D1")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B3")
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "G6")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "F6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "J8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "K10")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "H7")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "H6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "J7")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "K8")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "B5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "A1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A2")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A5")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A3")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "H2")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "H1")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "K7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A9")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "C7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "F5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "D7")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB8")
				(number "F7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "F10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "K6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "G3")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "C1")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "E2")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "F3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "G8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "G9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "G10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "H5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "D2")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E3")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F4")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "B4")
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "A6")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "G5")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D10")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55VEQx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 69.85 0)
		)
		(property "Value" "STM32WB55VEQx"
			(at 20.32 69.85 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-129_7x7mm_Layout13x13_P0.5mm"
			(at -30.48 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 256KB RAM, 64 MHz, 1.71-3.6V, 72 GPIO, UFBGA129"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB55VEQx_0_1")
		(symbol "STM32WB55VEQx_1_1"
			(pin input line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin power_in line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "F11")
			)
			(pin power_in line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "G11")
			)
			(pin input line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "OSC_IN")
				(number "M13")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "N13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "VFBSMPS")
				(number "H11")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "RF1")
				(number "M9")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PH1")
				(number "G2")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PH3")
				(number "G1")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "B2")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "A1")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "B1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "H12")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "H13")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PD0")
				(number "B11")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PD1")
				(number "C7")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PD3")
				(number "D8")
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PD4")
				(number "C6")
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PD6")
				(number "D6")
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PD7")
				(number "C5")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PD8")
				(number "B6")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PD9")
				(number "D4")
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PD10")
				(number "A7")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SYS_TRIG_INOUT" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PD11")
				(number "B5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PD12")
				(number "B4")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PD13")
				(number "C1")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PD14")
				(number "D3")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PD15")
				(number "C2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin no_connect line
				(at -30.48 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "AT1")
				(number "K12")
			)
			(pin no_connect line
				(at -30.48 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "AT0")
				(number "K11")
			)
			(pin power_in line
				(at -17.78 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D2")
			)
			(pin power_in line
				(at -15.24 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at -12.7 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H8")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "K3")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B12")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C11")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F3")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J11")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K4")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "A8")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "F2")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K10")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSRF")
				(number "K8")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L10")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L11")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L7")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L8")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L9")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M10")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M11")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M12")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M8")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "N11")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "N8")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "J12")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "G12")
			)
			(pin passive line
				(at 5.08 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSSMPS")
				(number "G13")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "N7")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDRF")
				(number "N12")
			)
			(pin power_in line
				(at 12.7 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "F12")
			)
			(pin power_in line
				(at 15.24 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "F13")
			)
			(pin power_in line
				(at 17.78 73.66 270)
				(length 5.08)
				(name "VDDUSB")
				(number "A12")
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "M1")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "L2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "N1")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "M2")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "N2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "M3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "N3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "M4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "L4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A13")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "C10")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "C9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "L13")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "L12")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "N6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "C4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "A3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "A2")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PB8")
				(number "G3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "H4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "M6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "H10")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "E12")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "E11")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "F10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "H1")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "J3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "M5")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "D10")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "D12")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "D11")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "C13")
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B9")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "F4")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "E3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55VEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 69.85 0)
		)
		(property "Value" "STM32WB55VEYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-100_4.4x4.38mm_Layout10x10_P0.4mm_Offcenter"
			(at -22.86 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 256KB RAM, 64 MHz, 1.71-3.6V, 72 GPIO, WLCSP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.4x4.38mm*Layout10x10*P0.4mm*Offcenter*"
			(at 0 0 0)
		)
		(symbol "STM32WB55VEYx_0_1")
		(symbol "STM32WB55VEYx_1_1"
			(pin input line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "F9")
			)
			(pin power_in line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "E1")
			)
			(pin input line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "VREF+")
				(number "H8")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "OSC_IN")
				(number "J1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "J2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "VFBSMPS")
				(number "F2")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "RF1")
				(number "K4")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PH0")
				(number "E10")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PH1")
				(number "E9")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PH3")
				(number "E8")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C8")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PE1")
				(number "B10")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PE2")
				(number "E6")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PE3")
				(number "G2")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PE4")
				(number "G1")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C4")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PD1")
				(number "C3")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PD2")
				(number "A7")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PD3")
				(number "C2")
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PD4")
				(number "D3")
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PD5")
				(number "B7")
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PD6")
				(number "C6")
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PD7")
				(number "A8")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PD8")
				(number "D4")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PD9")
				(number "D5")
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PD10")
				(number "E4")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SYS_TRIG_INOUT" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PD11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PD12")
				(number "B8")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PD13")
				(number "C9")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PD14")
				(number "D8")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PD15")
				(number "E7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin no_connect line
				(at -22.86 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "AT1")
				(number "H4")
			)
			(pin no_connect line
				(at -22.86 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "AT0")
				(number "H3")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "C10")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "J10")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "K5")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "H10")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "H9")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSRF")
				(number "J4")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K1")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K2")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K3")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDRF")
				(number "J3")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "F1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "D1")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B3")
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "G6")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "F6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "J8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "K10")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "H7")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "H6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "J7")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "K8")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "B5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "A1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A2")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A5")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A3")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "H2")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "H1")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "K7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A9")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "C7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "F5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "D7")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB8")
				(number "F7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "F10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "K6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "G3")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "C1")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "E2")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "F3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "G8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "G9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "G10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "H5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "D2")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E3")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F4")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "B4")
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "A6")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "G5")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D10")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55VGQx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 69.85 0)
		)
		(property "Value" "STM32WB55VGQx"
			(at 20.32 69.85 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-129_7x7mm_Layout13x13_P0.5mm"
			(at -30.48 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 1024KB flash, 256KB RAM, 64 MHz, 1.71-3.6V, 72 GPIO, UFBGA129"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB55VGQx_0_1")
		(symbol "STM32WB55VGQx_1_1"
			(pin input line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin power_in line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "F11")
			)
			(pin power_in line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "G11")
			)
			(pin input line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "OSC_IN")
				(number "M13")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "N13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "VFBSMPS")
				(number "H11")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "RF1")
				(number "M9")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PH1")
				(number "G2")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PH3")
				(number "G1")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "B2")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "A1")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "B1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "H12")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "H13")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PD0")
				(number "B11")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PD1")
				(number "C7")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PD3")
				(number "D8")
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PD4")
				(number "C6")
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PD6")
				(number "D6")
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PD7")
				(number "C5")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PD8")
				(number "B6")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PD9")
				(number "D4")
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PD10")
				(number "A7")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SYS_TRIG_INOUT" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PD11")
				(number "B5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PD12")
				(number "B4")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PD13")
				(number "C1")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PD14")
				(number "D3")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PD15")
				(number "C2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin no_connect line
				(at -30.48 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "AT1")
				(number "K12")
			)
			(pin no_connect line
				(at -30.48 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "AT0")
				(number "K11")
			)
			(pin power_in line
				(at -17.78 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D2")
			)
			(pin power_in line
				(at -15.24 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at -12.7 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H8")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "K3")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B12")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C11")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F3")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J11")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K4")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "A8")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "F2")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K10")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSRF")
				(number "K8")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L10")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L11")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L7")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L8")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "L9")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M10")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M11")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M12")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "M8")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "N11")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "N8")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "J12")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "G12")
			)
			(pin passive line
				(at 5.08 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSSMPS")
				(number "G13")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDCAP")
				(number "N7")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDRF")
				(number "N12")
			)
			(pin power_in line
				(at 12.7 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "F12")
			)
			(pin power_in line
				(at 15.24 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "F13")
			)
			(pin power_in line
				(at 17.78 73.66 270)
				(length 5.08)
				(name "VDDUSB")
				(number "A12")
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "M1")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "L2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "N1")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "M2")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "N2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "M3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "N3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "M4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "L4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A13")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "C10")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "C9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "L13")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "L12")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "N6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "C4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "A3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "A2")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PB8")
				(number "G3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "H4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "M6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "H10")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "E12")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "E11")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "F10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "H1")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "J3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "M5")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "D10")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "D12")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "D11")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "C13")
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B9")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "F4")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "E3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55VGYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 69.85 0)
		)
		(property "Value" "STM32WB55VGYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-100_4.4x4.38mm_Layout10x10_P0.4mm_Offcenter"
			(at -22.86 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 1024KB flash, 256KB RAM, 64 MHz, 1.71-3.6V, 72 GPIO, WLCSP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.4x4.38mm*Layout10x10*P0.4mm*Offcenter*"
			(at 0 0 0)
		)
		(symbol "STM32WB55VGYx_0_1")
		(symbol "STM32WB55VGYx_1_1"
			(pin input line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "F9")
			)
			(pin power_in line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "E1")
			)
			(pin input line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "VREF+")
				(number "H8")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "OSC_IN")
				(number "J1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "J2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "VFBSMPS")
				(number "F2")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "RF1")
				(number "K4")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PH0")
				(number "E10")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PH1")
				(number "E9")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PH3")
				(number "E8")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C8")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PE1")
				(number "B10")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PE2")
				(number "E6")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PE3")
				(number "G2")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PE4")
				(number "G1")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C4")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PD1")
				(number "C3")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PD2")
				(number "A7")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PD3")
				(number "C2")
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PD4")
				(number "D3")
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PD5")
				(number "B7")
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PD6")
				(number "C6")
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PD7")
				(number "A8")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PD8")
				(number "D4")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PD9")
				(number "D5")
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PD10")
				(number "E4")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SYS_TRIG_INOUT" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PD11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PD12")
				(number "B8")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PD13")
				(number "C9")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PD14")
				(number "D8")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PD15")
				(number "E7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin no_connect line
				(at -22.86 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "AT1")
				(number "H4")
			)
			(pin no_connect line
				(at -22.86 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "AT0")
				(number "H3")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "C10")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "J10")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "K5")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "H10")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "H9")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSRF")
				(number "J4")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K1")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K2")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K3")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDRF")
				(number "J3")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "F1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "D1")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B3")
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "G6")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "F6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "J8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "K10")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "H7")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "H6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "J7")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "K8")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "B5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "A1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A2")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A5")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A3")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "H2")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "H1")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "K7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A9")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "C7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "F5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "D7")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB8")
				(number "F7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "F10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "K6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "G3")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "C1")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "E2")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "F3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "G8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "G9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "G10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "H5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "D2")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E3")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F4")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "B4")
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "A6")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "G5")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D10")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB55VYYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 69.85 0)
		)
		(property "Value" "STM32WB55VYYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-100_4.4x4.38mm_Layout10x10_P0.4mm_Offcenter"
			(at -22.86 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb55vy.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 640KB flash, 256KB RAM, 64 MHz, 1.71-3.6V, 72 GPIO, WLCSP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.4x4.38mm*Layout10x10*P0.4mm*Offcenter*"
			(at 0 0 0)
		)
		(symbol "STM32WB55VYYx_0_1")
		(symbol "STM32WB55VYYx_1_1"
			(pin input line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "F9")
			)
			(pin power_in line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "E1")
			)
			(pin input line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "VREF+")
				(number "H8")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "OSC_IN")
				(number "J1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "J2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "VFBSMPS")
				(number "F2")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "RF1")
				(number "K4")
				(alternate "RF_RF1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PH0")
				(number "E10")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PH1")
				(number "E9")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PH3")
				(number "E8")
				(alternate "RCC_LSCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C8")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PE1")
				(number "B10")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PE2")
				(number "E6")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PE3")
				(number "G2")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PE4")
				(number "G1")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C4")
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PD1")
				(number "C3")
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PD2")
				(number "A7")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PD3")
				(number "C2")
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PD4")
				(number "D3")
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PD5")
				(number "B7")
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PD6")
				(number "C6")
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PD7")
				(number "A8")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PD8")
				(number "D4")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PD9")
				(number "D5")
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PD10")
				(number "E4")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SYS_TRIG_INOUT" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PD11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PD12")
				(number "B8")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PD13")
				(number "C9")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PD14")
				(number "D8")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PD15")
				(number "E7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin no_connect line
				(at -22.86 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "AT1")
				(number "H4")
			)
			(pin no_connect line
				(at -22.86 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "AT0")
				(number "H3")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "C10")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "J10")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B9")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J5")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "K5")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "H10")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "H9")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSRF")
				(number "J4")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K1")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K2")
			)
			(pin passive line
				(at 2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSSRF")
				(number "K3")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDRF")
				(number "J3")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "F1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "D1")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B3")
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "G6")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "F6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "J8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "K10")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "H7")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "H6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "J7")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "K8")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "B5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "A1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A2")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A5")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A3")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "H2")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RF_TX_MOD_EXT_PA" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "H1")
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "K7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A9")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "C7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "F5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "D7")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB8")
				(number "F7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "F10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "K6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "G3")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "C1")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "E2")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "F3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "G8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "G9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "G10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "H5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "D2")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E3")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F4")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "B4")
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "A6")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "G5")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D10")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA52CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "STM32WBA52CEUx"
			(at 12.7 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba52ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 96KB RAM, 100 MHz, 1.71-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA52CEUx_0_1")
		(symbol "STM32WBA52CEUx_1_1"
			(pin input line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "36")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "OSC_IN")
				(number "41")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "40")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "RF")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PH3")
				(number "34")
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "18")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "17")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "16")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "32")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PB2")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RF_ANTSW2" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "23")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "20")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "15")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "14")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "9")
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "2")
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "1")
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "48")
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "47")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "33")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin power_out line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "VCAP")
				(number "44")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "43")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "6")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDHPA")
				(number "38")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDRF")
				(number "39")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "13")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "7")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "5")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "4")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "3")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "46")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "45")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RF_ANTSW1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "28")
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "27")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "26")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA52CGUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "STM32WBA52CGUx"
			(at 12.7 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba52cg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 128KB RAM, 100 MHz, 1.71-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA52CGUx_0_1")
		(symbol "STM32WBA52CGUx_1_1"
			(pin input line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "36")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "OSC_IN")
				(number "41")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "40")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "RF")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PH3")
				(number "34")
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "18")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "17")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "16")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "32")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PB2")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RF_ANTSW2" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "23")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "20")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "15")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "14")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "9")
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "2")
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "1")
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "48")
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "47")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "33")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin power_out line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "VCAP")
				(number "44")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "43")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "6")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDHPA")
				(number "38")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDRF")
				(number "39")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "13")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "7")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "5")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "4")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "3")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "46")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "45")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RF_ANTSW1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "28")
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "27")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "26")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA52KEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 29.21 0)
		)
		(property "Value" "STM32WBA52KEUx"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -20.32 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba52ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 96KB RAM, 100 MHz, 1.71-3.6V, 22 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA52KEUx_0_1")
		(symbol "STM32WBA52KEUx_1_1"
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "NRST")
				(number "24")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_IN")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "28")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "RF")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PH3")
				(number "22")
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PC14")
				(number "13")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "12")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "VCAP")
				(number "32")
			)
			(pin power_in line
				(at -7.62 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDHPA")
				(number "26")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "VDDRF")
				(number "27")
			)
			(pin power_in line
				(at 7.62 30.48 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "6")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "4")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA8")
				(number "2")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "20")
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA14")
				(number "18")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "17")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "16")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "15")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "11")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "10")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB12")
				(number "1")
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB15")
				(number "21")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA52KGUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 29.21 0)
		)
		(property "Value" "STM32WBA52KGUx"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -20.32 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba52kg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 128KB RAM, 100 MHz, 1.71-3.6V, 22 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA52KGUx_0_1")
		(symbol "STM32WBA52KGUx_1_1"
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "NRST")
				(number "24")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_IN")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "28")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "RF")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PH3")
				(number "22")
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PC14")
				(number "13")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "12")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "VCAP")
				(number "32")
			)
			(pin power_in line
				(at -7.62 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDHPA")
				(number "26")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "VDDRF")
				(number "27")
			)
			(pin power_in line
				(at 7.62 30.48 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "6")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "4")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA8")
				(number "2")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "20")
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA14")
				(number "18")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "17")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "16")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "15")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "11")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "10")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB12")
				(number "1")
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB15")
				(number "21")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA54CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "STM32WBA54CEUx"
			(at 12.7 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba54ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 96KB RAM, 100 MHz, 1.71-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA54CEUx_0_1")
		(symbol "STM32WBA54CEUx_1_1"
			(pin input line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "36")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "OSC_IN")
				(number "41")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "40")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "RF")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PH3")
				(number "34")
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "18")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "17")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "16")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "32")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PB2")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RF_ANTSW2" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "23")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "20")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "15")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "14")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "9")
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "2")
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "1")
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "48")
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "47")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "33")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin power_out line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "VCAP")
				(number "44")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "43")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "6")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDHPA")
				(number "38")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDRF")
				(number "39")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "13")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "7")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "5")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "4")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "3")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "46")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "45")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RF_ANTSW1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "28")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "27")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "26")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA54CGUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "STM32WBA54CGUx"
			(at 12.7 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba54cg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 128KB RAM, 100 MHz, 1.71-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA54CGUx_0_1")
		(symbol "STM32WBA54CGUx_1_1"
			(pin input line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "36")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "OSC_IN")
				(number "41")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "40")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "RF")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PH3")
				(number "34")
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "18")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "17")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "16")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "32")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PB2")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RF_ANTSW2" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "23")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "20")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "15")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "14")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "9")
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "2")
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "1")
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "48")
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "47")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "33")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin power_out line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "VCAP")
				(number "44")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "43")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "6")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDHPA")
				(number "38")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDRF")
				(number "39")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "13")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "7")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "5")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "4")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "3")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "46")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "45")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RF_ANTSW1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "28")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "27")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "26")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA54KEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 29.21 0)
		)
		(property "Value" "STM32WBA54KEUx"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -20.32 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba54ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 96KB RAM, 100 MHz, 1.71-3.6V, 22 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA54KEUx_0_1")
		(symbol "STM32WBA54KEUx_1_1"
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "NRST")
				(number "24")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_IN")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "28")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "RF")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PH3")
				(number "22")
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PC14")
				(number "13")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "12")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "VCAP")
				(number "32")
			)
			(pin power_in line
				(at -7.62 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDHPA")
				(number "26")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "VDDRF")
				(number "27")
			)
			(pin power_in line
				(at 7.62 30.48 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "6")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "4")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA8")
				(number "2")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "20")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA14")
				(number "18")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "17")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "16")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "15")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "11")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "10")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB12")
				(number "1")
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB15")
				(number "21")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA54KGUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 29.21 0)
		)
		(property "Value" "STM32WBA54KGUx"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -20.32 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba54kg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 128KB RAM, 100 MHz, 1.71-3.6V, 22 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA54KGUx_0_1")
		(symbol "STM32WBA54KGUx_1_1"
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "NRST")
				(number "24")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_IN")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "28")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "RF")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PH3")
				(number "22")
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PC14")
				(number "13")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "12")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "VCAP")
				(number "32")
			)
			(pin power_in line
				(at -7.62 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDHPA")
				(number "26")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "VDDRF")
				(number "27")
			)
			(pin power_in line
				(at 7.62 30.48 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "9")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "6")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "4")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA8")
				(number "2")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "20")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA14")
				(number "18")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "17")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "16")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "15")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "11")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "10")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB12")
				(number "1")
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB15")
				(number "21")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA55CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 41.91 0)
		)
		(property "Value" "STM32WBA55CEUx"
			(at 15.24 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba55ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 96KB RAM, 100 MHz, 1.71-3.6V, 33 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA55CEUx_0_1")
		(symbol "STM32WBA55CEUx_1_1"
			(pin input line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "36")
			)
			(pin power_in line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "3")
			)
			(pin input line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "42")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "41")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "RF")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PH3")
				(number "34")
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC13")
				(number "18")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "17")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "16")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -12.7 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -10.16 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -7.62 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD11")
				(number "45")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDDANA")
				(number "39")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "1")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDHPA")
				(number "38")
			)
			(pin power_in line
				(at 7.62 43.18 270)
				(length 2.54)
				(name "VDDRF")
				(number "40")
			)
			(pin power_in line
				(at 10.16 43.18 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "43")
			)
			(pin power_in line
				(at 12.7 43.18 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "13")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "9")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "7")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "6")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "5")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "47")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "46")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RF_ANTSW1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "28")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "27")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "26")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "32")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RF_ANTSW2" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "23")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "20")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "15")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "14")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB12")
				(number "4")
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB14")
				(number "48")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB15")
				(number "33")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA55CGUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 41.91 0)
		)
		(property "Value" "STM32WBA55CGUx"
			(at 15.24 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba55cg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 128KB RAM, 100 MHz, 1.71-3.6V, 33 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA55CGUx_0_1")
		(symbol "STM32WBA55CGUx_1_1"
			(pin input line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "36")
			)
			(pin power_in line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "3")
			)
			(pin input line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "42")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "41")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "RF")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PH3")
				(number "34")
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC13")
				(number "18")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "17")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "16")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -12.7 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -10.16 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -7.62 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD11")
				(number "45")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDDANA")
				(number "39")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "1")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDHPA")
				(number "38")
			)
			(pin power_in line
				(at 7.62 43.18 270)
				(length 2.54)
				(name "VDDRF")
				(number "40")
			)
			(pin power_in line
				(at 10.16 43.18 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "43")
			)
			(pin power_in line
				(at 12.7 43.18 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "13")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "9")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "7")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "6")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "5")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "47")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "46")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RF_ANTSW1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "28")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "27")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "26")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "32")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RF_ANTSW2" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "23")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "20")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "15")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "14")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB12")
				(number "4")
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB14")
				(number "48")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB15")
				(number "33")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA55HGFx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 38.1 0)
		)
		(property "Value" "STM32WBA55HGFx"
			(at 12.446 38.1 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-41_2.98x2.76mm_Layout13x7_P0.4mm_Stagger"
			(at -19.558 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba55hg.pdf"
			(at -1.27 0.254 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 128KB RAM, 100 MHz, 1.71-3.6V, 20 GPIO, WLCSP41"
			(at -1.016 0.254 0)
		)
		(property "ki_keywords" "STM32WBA STM32WBAx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.98x2.76mm*Layout13x7*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32WBA55HGFx_0_1")
		(symbol "STM32WBA55HGFx_1_1"
			(pin input line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "NRST")
				(number "E2")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "OSC_IN")
				(number "A8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin output line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "OSC_OUT")
				(number "B7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RF")
				(number "C2")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "PH3")
				(number "C8")
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin power_in line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "VLXSMPS")
				(number "C12")
			)
			(pin power_in line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "VDDHPA")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 3.81)
				(name "VDDA")
				(number "E12")
			)
			(pin power_in line
				(at -7.62 -40.64 90)
				(length 3.81)
				(name "VSSA")
				(number "D13")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 3.81)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -5.08 -40.64 90)
				(length 3.81)
				(name "VSS")
				(number "B9")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 3.81)
				(name "VDD")
				(number "G4")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 3.81)
				(name "VSS")
				(number "G6")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "VDDSMPS")
				(number "B13")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 3.81)
				(name "VSSSMPS")
				(number "A12")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 3.81)
				(name "VDDRF")
				(number "A6")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 3.81)
				(name "VSSRF")
				(number "D1")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 3.81)
				(name "VDDRFPA")
				(number "C6")
			)
			(pin power_in line
				(at 5.08 -40.64 90)
				(length 3.81)
				(name "VSSRF")
				(number "D3")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 3.81)
				(name "VDDANA")
				(number "B5")
			)
			(pin power_in line
				(at 7.62 -40.64 90)
				(length 3.81)
				(name "VSSRF")
				(number "D5")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 3.81)
				(name "VDD11")
				(number "B11")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "PA0")
				(number "G12")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "PA1")
				(number "E10")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "PA2")
				(number "F11")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "PA5")
				(number "F13")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "PA6")
				(number "D9")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "PA7")
				(number "D11")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "PA8")
				(number "D7")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "PA12")
				(number "E6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "PA13")
				(number "E8")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "PA14")
				(number "F1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "PA15")
				(number "F3")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "PB3")
				(number "G2")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "PB4")
				(number "F5")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "PB8")
				(number "G10")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "PB9")
				(number "F9")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "PB12")
				(number "C10")
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "PB15")
				(number "E4")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "PC14")
				(number "G8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "PC15")
				(number "F7")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA55UEIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32WBA55UEIx"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-59_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba55ue.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 96KB RAM, 100 MHz, 1.71-3.6V, 37 GPIO, UFBGA59"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA55UEIx_0_1")
		(symbol "STM32WBA55UEIx_1_1"
			(pin input line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "B8")
			)
			(pin power_in line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "C1")
			)
			(pin input line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "OSC_IN")
				(number "B5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "A5")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "RF")
				(number "A8")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PH3")
				(number "C7")
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "G5")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "H4")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "G4")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PB0")
				(number "D7")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "D8")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "E7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RF_ANTSW2" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "G7")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "H8")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "H7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "G6")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "H6")
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "H5")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "H3")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "D2")
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "C2")
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "B2")
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "A2")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "C8")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin power_in line
				(at -12.7 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "C6")
			)
			(pin power_in line
				(at -10.16 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "D5")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD11")
				(number "C3")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "F1")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDANA")
				(number "B6")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSRF")
				(number "A7")
			)
			(pin passive line
				(at 2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "B7")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDHPA")
				(number "B4")
			)
			(pin power_in line
				(at 5.08 -43.18 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDRF")
				(number "A6")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "A4")
			)
			(pin power_in line
				(at 12.7 45.72 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "B1")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "H1")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "G3")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "G2")
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "G1")
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "F3")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "E1")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "E2")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "B3")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "A3")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "E8")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RF_ANTSW1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "F7")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "F8")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "F6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA15")
				(number "G8")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WBA55UGIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32WBA55UGIx"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-59_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba55ug.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 128KB RAM, 100 MHz, 1.71-3.6V, 37 GPIO, UFBGA59"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32WBA STM32WBAx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WBA55UGIx_0_1")
		(symbol "STM32WBA55UGIx_1_1"
			(pin input line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "B8")
			)
			(pin power_in line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "C1")
			)
			(pin input line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "OSC_IN")
				(number "B5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "A5")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "RF")
				(number "A8")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PH3")
				(number "C7")
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "G5")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "H4")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "G4")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PB0")
				(number "D7")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "D8")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "E7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RF_ANTSW2" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "G7")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "H8")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "PTA_ACTIVE" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "H7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "G6")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "H6")
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "H5")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "H3")
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "D2")
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "C2")
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "B2")
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "A2")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "C8")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PTA_GRANT" bidirectional line)
				(alternate "RF_EXTPABYP" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin power_in line
				(at -12.7 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "C6")
			)
			(pin power_in line
				(at -10.16 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "D5")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD11")
				(number "C3")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "F1")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDANA")
				(number "B6")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSRF")
				(number "A7")
			)
			(pin passive line
				(at 2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "B7")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDHPA")
				(number "B4")
			)
			(pin power_in line
				(at 5.08 -43.18 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDRF")
				(number "A6")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDDRFPA")
				(number "A4")
			)
			(pin power_in line
				(at 12.7 45.72 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "B1")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "H1")
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "G3")
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "G2")
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "G1")
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "F3")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "E1")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "E2")
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "B3")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "A3")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "E8")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RF_ANTSW1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "F7")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RF_ANTSW0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "F8")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "PTA_PRIORITY" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "F6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA15")
				(number "G8")
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "PTA_STATUS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB35CCUxA"
		(extends "STM32WB35C_C-E_UxA")
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WB35CCUxA"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb35cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 96KB RAM, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32WB35CEUxA"
		(extends "STM32WB35C_C-E_UxA")
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WB35CEUxA"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb35ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 96KB RAM, 30 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WB STM32WBx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32WBA55HEFx"
		(extends "STM32WBA55HGFx")
		(property "Reference" "U"
			(at -19.05 38.1 0)
		)
		(property "Value" "STM32WBA55HEFx"
			(at 12.446 38.1 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-41_2.98x2.76mm_Layout13x7_P0.4mm_Stagger"
			(at -19.558 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wba55he.pdf"
			(at -1.27 0.254 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 96KB RAM, 100 MHz, 1.71-3.6V, 20 GPIO, WLCSP41"
			(at -1.016 0.254 0)
		)
		(property "ki_keywords" "STM32WBA STM32WBAx5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.98x2.76mm*Layout13x7*P0.4mm*Stagger*"
			(at 0 0 0)
		)
	)
)
