(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32WL54CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WL54CCUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wl54cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 64KB RAM, 48 MHz, 1.8-3.6V, 29 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WL5x"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WL54CCUx_0_1")
		(symbol "STM32WL54CCUx_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "18")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "47")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_IN")
				(number "26")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "27")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RFI_N")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RFI_P")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "RFO_HP")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "RFO_LP")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PH3")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "38")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "39")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "40")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "37")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "41")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDPA")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "28")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "29")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "33")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "34")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "42")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "43")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "30")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB4")
				(number "2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB5")
				(number "3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB6")
				(number "4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB7")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WL54JCIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32WL54JCIx"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-73_5x5mm_Layout9x9_P0.5mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wl54jc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 64KB RAM, 48 MHz, 1.8-3.6V, 43 GPIO, UFBGA73"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WL5x"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WL54JCIx_0_1")
		(symbol "STM32WL54JCIx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "B1")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "B5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "VR_PA")
				(number "H9")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "G9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "F8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "B2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RFI_N")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RFI_P")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RFO_HP")
				(number "J9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RFO_LP")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PH3")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "F2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D4")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "D5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "E4")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "C7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A8")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "G6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "H6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "A5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDPA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "F7")
			)
			(pin power_in line
				(at 12.7 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G3")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J1")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "J2")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "J3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C8")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "A9")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B8")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A4")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B3")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "E7")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "D8")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "E1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "E6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "D7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "C6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "B4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WL55CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WL55CCUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wl55cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 64KB RAM, 48 MHz, 1.8-3.6V, 29 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WL5x"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WL55CCUx_0_1")
		(symbol "STM32WL55CCUx_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "18")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "47")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_IN")
				(number "26")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "27")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RFI_N")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RFI_P")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "RFO_HP")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "RFO_LP")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PH3")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "38")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "39")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "40")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "37")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "41")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDPA")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "28")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "29")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "33")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "34")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "42")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "43")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "30")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB4")
				(number "2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB5")
				(number "3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB6")
				(number "4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB7")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WL55JCIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32WL55JCIx"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-73_5x5mm_Layout9x9_P0.5mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wl55jc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 64KB RAM, 48 MHz, 1.8-3.6V, 43 GPIO, UFBGA73"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WL5x"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WL55JCIx_0_1")
		(symbol "STM32WL55JCIx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "B1")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "B5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "VR_PA")
				(number "H9")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "G9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "F8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "B2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RFI_N")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RFI_P")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RFO_HP")
				(number "J9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RFO_LP")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PH3")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "F2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D4")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "D5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "E4")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "C7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A8")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "G6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "H6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "A5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDPA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "F7")
			)
			(pin power_in line
				(at 12.7 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G3")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J1")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "J2")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "J3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C8")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "A9")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B8")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A4")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B3")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "E7")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "D8")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "E1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "E6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "D7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "C6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "B4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE4C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WLE4C8Ux"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle4c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 20KB RAM, 48 MHz, 1.8-3.6V, 29 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE4C8Ux_0_1")
		(symbol "STM32WLE4C8Ux_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "18")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "47")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_IN")
				(number "26")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "27")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RFI_N")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RFI_P")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "RFO_HP")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "RFO_LP")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PH3")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "38")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "39")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "40")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "37")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "41")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDPA")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "28")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "29")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "33")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "34")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "42")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "43")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "30")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB4")
				(number "2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB5")
				(number "3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB6")
				(number "4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB7")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE4CBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WLE4CBUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle4cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 48KB RAM, 48 MHz, 1.8-3.6V, 29 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE4CBUx_0_1")
		(symbol "STM32WLE4CBUx_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "18")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "47")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_IN")
				(number "26")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "27")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RFI_N")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RFI_P")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "RFO_HP")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "RFO_LP")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PH3")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "38")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "39")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "40")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "37")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "41")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDPA")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "28")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "29")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "33")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "34")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "42")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "43")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "30")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB4")
				(number "2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB5")
				(number "3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB6")
				(number "4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB7")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE4CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WLE4CCUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle4cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 64KB RAM, 48 MHz, 1.8-3.6V, 29 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE4CCUx_0_1")
		(symbol "STM32WLE4CCUx_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "18")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "47")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_IN")
				(number "26")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "27")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RFI_N")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RFI_P")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "RFO_HP")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "RFO_LP")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PH3")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "38")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "39")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "40")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "37")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "41")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDPA")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "28")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "29")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "33")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "34")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "42")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "43")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "30")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB4")
				(number "2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB5")
				(number "3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB6")
				(number "4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB7")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE4J8Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32WLE4J8Ix"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-73_5x5mm_Layout9x9_P0.5mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle4j8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 20KB RAM, 48 MHz, 1.8-3.6V, 43 GPIO, UFBGA73"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE4J8Ix_0_1")
		(symbol "STM32WLE4J8Ix_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "B1")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "B5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "VR_PA")
				(number "H9")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "G9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "F8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "B2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RFI_N")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RFI_P")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RFO_HP")
				(number "J9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RFO_LP")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PH3")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "F2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D4")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "D5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "E4")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "C7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A8")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "G6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "H6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "A5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDPA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "F7")
			)
			(pin power_in line
				(at 12.7 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G3")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J1")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "J2")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "J3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C8")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "A9")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B8")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A4")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B3")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "E7")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "D8")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "E1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "E6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "D7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "C6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "B4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE4JBIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32WLE4JBIx"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-73_5x5mm_Layout9x9_P0.5mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle4jb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 48KB RAM, 48 MHz, 1.8-3.6V, 43 GPIO, UFBGA73"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE4JBIx_0_1")
		(symbol "STM32WLE4JBIx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "B1")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "B5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "VR_PA")
				(number "H9")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "G9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "F8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "B2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RFI_N")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RFI_P")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RFO_HP")
				(number "J9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RFO_LP")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PH3")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "F2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D4")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "D5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "E4")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "C7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A8")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "G6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "H6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "A5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDPA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "F7")
			)
			(pin power_in line
				(at 12.7 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G3")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J1")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "J2")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "J3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C8")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "A9")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B8")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A4")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B3")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "E7")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "D8")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "E1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "E6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "D7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "C6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "B4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE4JCIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32WLE4JCIx"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-73_5x5mm_Layout9x9_P0.5mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle4jc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 64KB RAM, 48 MHz, 1.8-3.6V, 43 GPIO, UFBGA73"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE4JCIx_0_1")
		(symbol "STM32WLE4JCIx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "B1")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "B5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "VR_PA")
				(number "H9")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "G9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "F8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "B2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RFI_N")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RFI_P")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RFO_HP")
				(number "J9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RFO_LP")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PH3")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "F2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D4")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "D5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "E4")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "C7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A8")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "G6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "H6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "A5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDPA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "F7")
			)
			(pin power_in line
				(at 12.7 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G3")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J1")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "J2")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "J3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C8")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "A9")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B8")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A4")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B3")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "E7")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "D8")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "E1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "E6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "D7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "C6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "B4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE5C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WLE5C8Ux"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle5c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 20KB RAM, 48 MHz, 1.8-3.6V, 29 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE5C8Ux_0_1")
		(symbol "STM32WLE5C8Ux_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "18")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "47")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_IN")
				(number "26")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "27")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RFI_N")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RFI_P")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "RFO_HP")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "RFO_LP")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PH3")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "38")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "39")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "40")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "37")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "41")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDPA")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "28")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "29")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "33")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "34")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "42")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "43")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "30")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB4")
				(number "2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB5")
				(number "3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB6")
				(number "4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB7")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE5CBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WLE5CBUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle5cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 48KB RAM, 48 MHz, 1.8-3.6V, 29 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE5CBUx_0_1")
		(symbol "STM32WLE5CBUx_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "18")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "47")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_IN")
				(number "26")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "27")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RFI_N")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RFI_P")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "RFO_HP")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "RFO_LP")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PH3")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "38")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "39")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "40")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "37")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "41")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDPA")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "28")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "29")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "33")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "34")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "42")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "43")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "30")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB4")
				(number "2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB5")
				(number "3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB6")
				(number "4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB7")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE5CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 39.37 0)
		)
		(property "Value" "STM32WLE5CCUx"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -20.32 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle5cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 64KB RAM, 48 MHz, 1.8-3.6V, 29 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE5CCUx_0_1")
		(symbol "STM32WLE5CCUx_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "18")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "47")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "OSC_IN")
				(number "26")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "27")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RFI_N")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RFI_P")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "RFO_HP")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "RFO_LP")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PH3")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "38")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "39")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "40")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "37")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "41")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDPA")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDRF")
				(number "28")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "29")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "33")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "34")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "42")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "43")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "30")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB3")
				(number "1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB4")
				(number "2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB5")
				(number "3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB6")
				(number "4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB7")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB8")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE5J8Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32WLE5J8Ix"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-73_5x5mm_Layout9x9_P0.5mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle5j8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 20KB RAM, 48 MHz, 1.8-3.6V, 43 GPIO, UFBGA73"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE5J8Ix_0_1")
		(symbol "STM32WLE5J8Ix_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "B1")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "B5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "VR_PA")
				(number "H9")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "G9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "F8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "B2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RFI_N")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RFI_P")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RFO_HP")
				(number "J9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RFO_LP")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PH3")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "F2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D4")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "D5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "E4")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "C7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A8")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "G6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "H6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "A5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDPA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "F7")
			)
			(pin power_in line
				(at 12.7 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G3")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J1")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "J2")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "J3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C8")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "A9")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B8")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A4")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B3")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "E7")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "D8")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "E1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "E6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "D7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "C6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "B4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE5JBIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32WLE5JBIx"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-73_5x5mm_Layout9x9_P0.5mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle5jb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 48KB RAM, 48 MHz, 1.8-3.6V, 43 GPIO, UFBGA73"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE5JBIx_0_1")
		(symbol "STM32WLE5JBIx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "B1")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "B5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "VR_PA")
				(number "H9")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "G9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "F8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "B2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RFI_N")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RFI_P")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RFO_HP")
				(number "J9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RFO_LP")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PH3")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "F2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D4")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "D5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "E4")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "C7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A8")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "G6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "H6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "A5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDPA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "F7")
			)
			(pin power_in line
				(at 12.7 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G3")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J1")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "J2")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "J3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C8")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "A9")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B8")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A4")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B3")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "E7")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "D8")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "E1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "E6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "D7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "C6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "B4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WLE5JCIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32WLE5JCIx"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-73_5x5mm_Layout9x9_P0.5mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wle5jc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 64KB RAM, 48 MHz, 1.8-3.6V, 43 GPIO, UFBGA73"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32WL STM32WLEx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32WLE5JCIx_0_1")
		(symbol "STM32WLE5JCIx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "B1")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "B5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "VR_PA")
				(number "H9")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "OSC_IN")
				(number "G9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "F8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "VFBSMPS")
				(number "B2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RFI_N")
				(number "H7")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RFI_P")
				(number "J6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RFO_HP")
				(number "J9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RFO_LP")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PH3")
				(number "J5")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "F2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D4")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "D5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "E4")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "C7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A8")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSRF")
				(number "G6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "G8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSRF")
				(number "H6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "A5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDPA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDRF")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDRF1V55")
				(number "F7")
			)
			(pin power_in line
				(at 12.7 48.26 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "A2")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_PWR-REGLP1S" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G3")
				(alternate "DEBUG_PWR-REGLP2S" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_PWR-LDORDY" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J1")
				(alternate "DEBUG_SUBGHZSPI-NSSOUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "J2")
				(alternate "DEBUG_SUBGHZSPI-SCKOUT" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "DEBUG_SUBGHZSPI-MISOOUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DEBUG_SUBGHZSPI-MOSIOUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "J3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C8")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DEBUG_RF-HSE32RDY" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-NRESET" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "A9")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "DEBUG_RF-BUSY" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B8")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A4")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B3")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "VDDTCXO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "E7")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "D8")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_RF-SMPSRDY" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C1")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "DEBUG_RF-DTB1" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C2")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "DEBUG_RF-LDORDY" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "E1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "E6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "D7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "C6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "B4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
)
