(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM8AF6223"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 25.4 0)
		)
		(property "Value" "STM8AF6223"
			(at 1.27 22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 1.27 27.94 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/stm8af6223.pdf"
			(at -7.62 -7.62 0)
		)
		(property "Description" "16MHz, 8K Flash, 1K RAM, 640 EEPROM, USART, LIN,  I²C, SPI, ADC, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Automotive Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM8AF6223_0_1")
		(symbol "STM8AF6223_1_1"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "PA1")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "PA2")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "PA3")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "PB4")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "PC4")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "PC5")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PC6")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PC7")
				(number "17")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "VCAP")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "PD1")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "PD2")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "PD3")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "PD4")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "PD5")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "PD6")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8AF6223A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 25.4 0)
		)
		(property "Value" "STM8AF6223A"
			(at 1.27 22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 1.27 27.94 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/stm8af6223.pdf"
			(at -15.24 -10.16 0)
		)
		(property "Description" "16MHz, 8K Flash, 1K RAM, 640 EEPROM, USART, LIN,  I²C, SPI, ADC, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Automotive Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM8AF6223A_0_1")
		(symbol "STM8AF6223A_1_1"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "PA1")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "PA2")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "PB0")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "PB1")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "PB4")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "PB5")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "PC4")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "PC5")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PC6")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PC7")
				(number "17")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "VCAP")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "PD1")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "PD2")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "PD3")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "PD4")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "PD5")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "PD6")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8AL3188T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 38.735 0)
		)
		(property "Value" "STM8AL3188T"
			(at -10.16 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -39.37 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8al3188.pdf"
			(at 0 53.34 0)
		)
		(property "Description" "Automotive 8-bit ultra-low-power MCU, 64-Kbyte Flash, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 automotive ultra-low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8AL3188T_0_0"
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "NRST/PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PA5")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PA7")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PB3")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC0")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC1")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC2")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC3")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC4")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC5")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC6")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC7")
				(number "46")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VDD1")
				(number "10")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD2")
				(number "39")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "11")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS1/VSSA/VREF-")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSS2")
				(number "40")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VREF+")
				(number "12")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "RES1")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PD4")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PD5")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PD6")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PD7")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PE0")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PE1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PE2")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PE3")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PE4")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PE5")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PE6")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PE7")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PF0")
				(number "32")
			)
		)
		(symbol "STM8AL3188T_0_1")
		(embedded_fonts no)
	)
	(symbol "STM8AL3189T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 51.435 0)
		)
		(property "Value" "STM8AL3189T"
			(at -10.16 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -49.53 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8al3188.pdf"
			(at 0 66.04 0)
		)
		(property "Description" "Automotive 8-bit ultra-low-power MCU, 64-Kbyte Flash, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 automotive ultra-low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8AL3189T_0_0"
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "NRST/PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PA5")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PA7")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PB0")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PB1")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PB2")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PB3")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PB4")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PB5")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PB6")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PB7")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "54")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "57")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC6")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC7")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PD4")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PD5")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PD6")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PD7")
				(number "48")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 2.54)
				(name "VDD1")
				(number "11")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "VDD2")
				(number "55")
			)
			(pin power_in line
				(at -5.08 -48.26 90)
				(length 2.54)
				(name "VSS1")
				(number "10")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VDD3")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS2")
				(number "56")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS3")
				(number "30")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "RES1")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -48.26 90)
				(length 2.54)
				(name "VSSA/VREF-")
				(number "9")
			)
			(pin power_in line
				(at 7.62 50.8 270)
				(length 2.54)
				(name "VDDA")
				(number "12")
			)
			(pin power_in line
				(at 10.16 50.8 270)
				(length 2.54)
				(name "VREF+")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PE0")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PE1")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PE2")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PE3")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PE4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PE5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PE6")
				(number "63")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PE7")
				(number "64")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PF0")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PF1")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PF4")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PF5")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PF6")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PF7")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PG0")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PG1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PG2")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PG3")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PG4")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PG5")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PG6")
				(number "51")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PG7")
				(number "52")
			)
		)
		(symbol "STM8AL3189T_0_1")
		(embedded_fonts no)
	)
	(symbol "STM8AL318AT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 61.595 0)
		)
		(property "Value" "STM8AL318AT"
			(at -12.7 59.69 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at 8.89 -62.23 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8al3188.pdf"
			(at 0 76.2 0)
		)
		(property "Description" "Automotive 8-bit ultra-low-power MCU, 64-Kbyte Flash, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 automotive ultra-low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM8AL318AT_0_0"
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 2.54)
				(name "PA0")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 2.54)
				(name "NRST/PA1")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 2.54)
				(name "PA2")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 2.54)
				(name "PA3")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "PA5")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "PA6")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PA7")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PB0")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PB1")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PB2")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PB3")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PB4")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PB5")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PB7")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PC0")
				(number "65")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PC1")
				(number "66")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PC2")
				(number "69")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PC3")
				(number "70")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PC4")
				(number "71")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PC5")
				(number "72")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC6")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC7")
				(number "74")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PD0")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PD1")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PD2")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PD3")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PD4")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PD5")
				(number "58")
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PD6")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PD7")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PE0")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "PE1")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 2.54)
				(name "PE2")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 2.54)
				(name "PE3")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 2.54)
				(name "PE4")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -50.8 0)
				(length 2.54)
				(name "PE5")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -53.34 0)
				(length 2.54)
				(name "PE6")
				(number "75")
			)
			(pin bidirectional line
				(at -22.86 -55.88 0)
				(length 2.54)
				(name "PE7")
				(number "76")
			)
			(pin power_in line
				(at -10.16 60.96 270)
				(length 2.54)
				(name "VDD1")
				(number "15")
			)
			(pin power_in line
				(at -7.62 60.96 270)
				(length 2.54)
				(name "VDD2")
				(number "67")
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 2.54)
				(name "VDD3")
				(number "37")
			)
			(pin power_in line
				(at -5.08 -63.5 90)
				(length 2.54)
				(name "VSS1")
				(number "14")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 2.54)
				(name "VDD4")
				(number "47")
			)
			(pin power_in line
				(at -2.54 -63.5 90)
				(length 2.54)
				(name "VSS2")
				(number "68")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 2.54)
				(name "VSS3")
				(number "38")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 2.54)
				(name "VDDA")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 2.54)
				(name "VSS4")
				(number "48")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 2.54)
				(name "RES1")
				(number "22")
			)
			(pin power_in line
				(at 7.62 -63.5 90)
				(length 2.54)
				(name "VSSA/VREF-")
				(number "13")
			)
			(pin power_in line
				(at 12.7 60.96 270)
				(length 2.54)
				(name "VREF+")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 2.54)
				(name "PF0")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 2.54)
				(name "PF1")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 2.54)
				(name "PF2")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 2.54)
				(name "PF3")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "PF4")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PF5")
				(number "54")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PF7")
				(number "56")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PG0")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PG1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PG2")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PG3")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PG4")
				(number "61")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PG5")
				(number "62")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PG6")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PG7")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PH0")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PH1")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PH2")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PH3")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PH4")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PH5")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PH6")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PH7")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PI0")
				(number "77")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PI1")
				(number "78")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PI2")
				(number "79")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PI3")
				(number "80")
			)
		)
		(symbol "STM8AL318AT_0_1")
		(embedded_fonts no)
	)
	(symbol "STM8AL3L88T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 38.735 0)
		)
		(property "Value" "STM8AL3L88T"
			(at -10.16 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -39.37 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8al3188.pdf"
			(at 0 53.34 0)
		)
		(property "Description" "Automotive 8-bit ultra-low-power MCU, 64-Kbyte Flash with LCD, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 automotive ultra-low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8AL3L88T_0_0"
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "NRST/PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PA5")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PA7")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PB3")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC0")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC1")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC2")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC3")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC4")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC5")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC6")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC7")
				(number "46")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VDD1")
				(number "10")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD2")
				(number "39")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "11")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS1/VSSA/VREF-")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSS2")
				(number "40")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VLCD")
				(number "13")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "VREF+")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PD4")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PD5")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PD6")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PD7")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PE0")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PE1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PE2")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PE3")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PE4")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PE5")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PE6")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PE7")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PF0")
				(number "32")
			)
		)
		(symbol "STM8AL3L88T_0_1")
		(embedded_fonts no)
	)
	(symbol "STM8AL3L89T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 51.435 0)
		)
		(property "Value" "STM8AL3L89T"
			(at -10.16 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -49.53 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8al3188.pdf"
			(at 0 66.04 0)
		)
		(property "Description" "Automotive 8-bit ultra-low-power MCU, 64-Kbyte Flash with LCD, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 automotive ultra-low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8AL3L89T_0_0"
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "NRST/PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PA5")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PA7")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PB0")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PB1")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PB2")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PB3")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PB4")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PB5")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PB6")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PB7")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "54")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "57")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC6")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC7")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PD4")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PD5")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PD6")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PD7")
				(number "48")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 2.54)
				(name "VDD1")
				(number "11")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "VDD2")
				(number "55")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 2.54)
				(name "VSS1")
				(number "10")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VDD3")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 2.54)
				(name "VSS2")
				(number "56")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "VSS3")
				(number "30")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "VLCD")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -50.8 90)
				(length 2.54)
				(name "VSSA/VREF-")
				(number "9")
			)
			(pin power_in line
				(at 7.62 50.8 270)
				(length 2.54)
				(name "VDDA")
				(number "12")
			)
			(pin power_in line
				(at 10.16 50.8 270)
				(length 2.54)
				(name "VREF+")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PE0")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PE1")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PE2")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PE3")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PE4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PE5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PE6")
				(number "63")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PE7")
				(number "64")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PF0")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PF1")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PF4")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PF5")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PF6")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PF7")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PG0")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PG1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PG2")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PG3")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PG4")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PG5")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PG6")
				(number "51")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PG7")
				(number "52")
			)
		)
		(symbol "STM8AL3L89T_0_1")
		(embedded_fonts no)
	)
	(symbol "STM8AL3L8AT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 61.595 0)
		)
		(property "Value" "STM8AL3L8AT"
			(at -12.7 59.69 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at 8.89 -62.23 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8al3188.pdf"
			(at 0 76.2 0)
		)
		(property "Description" "Automotive 8-bit ultra-low-power MCU, 64-Kbyte Flash with LCD, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 automotive ultra-low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM8AL3L8AT_0_0"
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 2.54)
				(name "PA0")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 2.54)
				(name "NRST/PA1")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 2.54)
				(name "PA2")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 2.54)
				(name "PA3")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "PA5")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "PA6")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PA7")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PB0")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PB1")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PB2")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PB3")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PB4")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PB5")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PB7")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PC0")
				(number "65")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PC1")
				(number "66")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PC2")
				(number "69")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PC3")
				(number "70")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PC4")
				(number "71")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PC5")
				(number "72")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC6")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC7")
				(number "74")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PD0")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PD1")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PD2")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PD3")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PD4")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PD5")
				(number "58")
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PD6")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PD7")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PE0")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "PE1")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 2.54)
				(name "PE2")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 2.54)
				(name "PE3")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 2.54)
				(name "PE4")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -50.8 0)
				(length 2.54)
				(name "PE5")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -53.34 0)
				(length 2.54)
				(name "PE6")
				(number "75")
			)
			(pin bidirectional line
				(at -22.86 -55.88 0)
				(length 2.54)
				(name "PE7")
				(number "76")
			)
			(pin power_in line
				(at -10.16 60.96 270)
				(length 2.54)
				(name "VDD1")
				(number "15")
			)
			(pin power_in line
				(at -7.62 60.96 270)
				(length 2.54)
				(name "VDD2")
				(number "67")
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 2.54)
				(name "VDD3")
				(number "37")
			)
			(pin power_in line
				(at -5.08 -63.5 90)
				(length 2.54)
				(name "VSS1")
				(number "14")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 2.54)
				(name "VDD4")
				(number "47")
			)
			(pin power_in line
				(at -2.54 -63.5 90)
				(length 2.54)
				(name "VSS2")
				(number "68")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 2.54)
				(name "VSS3")
				(number "38")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 2.54)
				(name "VDDA")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 2.54)
				(name "VSS4")
				(number "48")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 2.54)
				(name "VLCD")
				(number "22")
			)
			(pin power_in line
				(at 7.62 -63.5 90)
				(length 2.54)
				(name "VSSA/VREF-")
				(number "13")
			)
			(pin power_in line
				(at 12.7 60.96 270)
				(length 2.54)
				(name "VREF+")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 2.54)
				(name "PF0")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 2.54)
				(name "PF1")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 2.54)
				(name "PF2")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 2.54)
				(name "PF3")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "PF4")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PF5")
				(number "54")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PF7")
				(number "56")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PG0")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PG1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PG2")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PG3")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PG4")
				(number "61")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PG5")
				(number "62")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PG6")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PG7")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PH0")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PH1")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PH2")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PH3")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PH4")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PH5")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PH6")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PH7")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PI0")
				(number "77")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PI1")
				(number "78")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PI2")
				(number "79")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PI3")
				(number "80")
			)
		)
		(symbol "STM8AL3L8AT_0_1")
		(embedded_fonts no)
	)
	(symbol "STM8L051F3P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 22.86 0)
		)
		(property "Value" "STM8L051F3P"
			(at 1.27 20.32 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 1.27 25.4 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00060484.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "16MHz, 8K Flash, 1K RAM, 256 EEPROM, RTC, USART,  I²C, SPI, ADC, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8L Microcontroller Value Line Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM8L051F3P_0_1")
		(symbol "STM8L051F3P_1_1"
			(pin power_in line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "PA0")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "PA1")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "PA2")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "PA3")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "PB7")
				(number "17")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "PC0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "PC1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "PC5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "PC6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "PD0")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8L101F1U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 23.495 0)
		)
		(property "Value" "STM8L101F1U"
			(at -2.54 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at 1.27 -21.59 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8l101f1.pdf"
			(at 0 38.1 0)
		)
		(property "Description" "16MHz, 2K Flash, 1.5K RAM, 2K EEPROM, USART,  I²C, SPI, ADC, UFQFPN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8L Microcontroller Value Line Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8L101F1U_0_1")
		(symbol "STM8L101F1U_1_1"
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA0")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "NRST/PA1")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA2")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA3")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "14")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC0")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC2")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC3")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC4")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PD0")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8L101F2P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 22.86 0)
		)
		(property "Value" "STM8L101F2P"
			(at 1.27 20.32 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 1.27 25.4 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00220591.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "16MHz, 4K Flash, 1.5K RAM, 2K EEPROM, USART,  I²C, SPI, ADC, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8L Microcontroller Value Line Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM8L101F2P_0_1")
		(symbol "STM8L101F2P_1_1"
			(pin power_in line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "PA0")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "PA1")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "PA2")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "PA3")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "PB7")
				(number "17")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "PC0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "PC1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "PC2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "PC3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "PC4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "PD0")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8L151C2T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 38.735 0)
		)
		(property "Value" "STM8L151C2T"
			(at -10.16 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -39.37 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8l151c3.pdf"
			(at 0 58.42 0)
		)
		(property "Description" "8-bit ultra-low-power MCU, 4 KB Flash, 256 bytes data EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 ultra-low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8L151C2T_0_0"
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "NRST/PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA5")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA7")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB3")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC0")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC1")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC2")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC3")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC4")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC5")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC6")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC7")
				(number "46")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "39")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "VSSIO")
				(number "40")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSS1/VSSA/VREF-")
				(number "9")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VREF+")
				(number "12")
			)
			(pin no_connect line
				(at 15.24 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PD4")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PD5")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PD6")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PD7")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PE0")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PE1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PE2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PE3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PE4")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PE5")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PE6")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PE7")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PF0")
				(number "32")
			)
		)
		(symbol "STM8L151C2T_0_1")
		(embedded_fonts no)
	)
	(symbol "STM8L152R8T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM8L152R8T"
			(at 8.89 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -7.62 -46.99 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8l152r8.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "16MHz, 64K Flash, 2K EEPROM, LCD, USART, I²C, SPI, ADC, DAC, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8L Microcontroller Low Power LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8L152R8T_0_0"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PB0")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PB1")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PB2")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PB3")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB4")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB5")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB6")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB7")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC0")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC1")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC2")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC3")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC4")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC5")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC6")
				(number "61")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC7")
				(number "62")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "55")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "29")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PD4")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PD5")
				(number "46")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PD6")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PD7")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PE2")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PE3")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PE4")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PE5")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PE6")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PE7")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PF0")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PF1")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PF4")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PF5")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PF6")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PF7")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PG4")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PG5")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PG6")
				(number "51")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PG7")
				(number "52")
			)
		)
		(symbol "STM8L152R8T_0_1")
		(symbol "STM8L152R8T_1_1"
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "NRST/PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA5")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA7")
				(number "8")
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "12")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VREF+")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA/VREF-")
				(number "9")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PE0")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PE1")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PG0")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PG1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PG2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PG3")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8S001J3M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 11.43 0)
		)
		(property "Value" "STM8S001J3M"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 1.27 13.97 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s001j3.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "16MHz, 8K Flash, 1K RAM, 128 EEPROM, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STM8S001J3M_0_1")
		(symbol "STM8S001J3M_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB4")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB5")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VCAP")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PD6")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PD5")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PC5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8S003F3P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 25.4 0)
		)
		(property "Value" "STM8S003F3P"
			(at 1.27 22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 1.27 27.94 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00024550.pdf"
			(at -1.27 -10.16 0)
		)
		(property "Description" "16MHz, 8K Flash, 1K RAM, 128 EEPROM, USART, I²C, SPI, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8S Mainstream Value line 8-bit, 16MHz, 1k RAM, 128 EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM8S003F3P_0_1")
		(symbol "STM8S003F3P_1_1"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "PA1")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "PA2")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "PA3")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "PB4")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "PC4")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "PC5")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PC6")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PC7")
				(number "17")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "NRST")
				(number "4")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "VCAP")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "PD1")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "PD2")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "PD3")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "PD4")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "PD5")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "PD6")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8S003F3U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 25.4 0)
		)
		(property "Value" "STM8S003F3U"
			(at 1.27 22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at 1.27 27.94 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00024550.pdf"
			(at -1.27 -10.16 0)
		)
		(property "Description" "16MHz, 8K Flash, 1K RAM, 128 EEPROM, USART, I²C, SPI, UFQFPN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8S Mainstream Value line 8-bit, 16MHz, 1k RAM, 128 EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8S003F3U_0_1")
		(symbol "STM8S003F3U_1_1"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "PA3")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "PB4")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "PB5")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "PC3")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "PC4")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "PC5")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PC6")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PC7")
				(number "14")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "NRST")
				(number "1")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "VCAP")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "PD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "PD2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "PD3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "PD4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "PD5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "PD6")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8S003K3T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 35.56 0)
		)
		(property "Value" "STM8S003K3T"
			(at 1.27 33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 1.27 38.1 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00024550.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8K Flash, 1K RAM, 128 EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM8S003K3T_0_1")
		(symbol "STM8S003K3T_1_1"
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 3.81)
				(name "PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 3.81)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 3.81)
				(name "PA3")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "PB0")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "PB4")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "PB6")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "PB7")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "PC1")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PC2")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PC3")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "PC4")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "PC5")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "PC6")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 3.81)
				(name "PC7")
				(number "24")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 3.81)
				(name "NRST")
				(number "1")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 3.81)
				(name "VCAP")
				(number "5")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "PD7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "PE5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "PF4")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8S207MB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.0359 58.42 0)
		)
		(property "Value" "STM8S207MB"
			(at 7.0359 55.88 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at 0 -67.31 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s207mb.pdf"
			(at 0 -69.85 0)
		)
		(property "Description" "24MHz, 128K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*80*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM8S207MB_0_1")
		(symbol "STM8S207MB_1_0"
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC0")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PH0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PH1")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PH2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PH3")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PH4")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PH5")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PH6")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PH7")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PI0")
				(number "57")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PI1")
				(number "58")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PI2")
				(number "59")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PI3")
				(number "60")
			)
			(pin bidirectional line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "PI4")
				(number "61")
			)
			(pin bidirectional line
				(at 15.24 -48.26 180)
				(length 2.54)
				(name "PI5")
				(number "62")
			)
			(pin bidirectional line
				(at 15.24 -50.8 180)
				(length 2.54)
				(name "PI6")
				(number "71")
			)
			(pin bidirectional line
				(at 15.24 -53.34 180)
				(length 2.54)
				(name "PI7")
				(number "72")
			)
		)
		(symbol "STM8S207MB_1_1"
			(pin bidirectional line
				(at -15.24 50.8 0)
				(length 2.54)
				(name "PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 48.26 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 45.72 0)
				(length 2.54)
				(name "PA3")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "PA4")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "PA5")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "PA6")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PB0")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PB1")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PB2")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PB3")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PB4")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PB5")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PB6")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PB7")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC1")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC2")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC3")
				(number "45")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC4")
				(number "46")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC5")
				(number "47")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC6")
				(number "50")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC7")
				(number "51")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PD0")
				(number "73")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PD1")
				(number "74")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PD2")
				(number "75")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PD3")
				(number "76")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PD4")
				(number "77")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PD5")
				(number "78")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PD6")
				(number "79")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PD7")
				(number "80")
			)
			(pin input line
				(at -15.24 -50.8 0)
				(length 2.54)
				(name "NRST")
				(number "1")
			)
			(pin input line
				(at -15.24 -53.34 0)
				(length 2.54)
				(name "VCAP")
				(number "6")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 2.54)
				(name "VDDA")
				(number "23")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "24")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 2.54)
				(name "VDDIO_1")
				(number "8")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSSIO_1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 2.54)
				(name "VDDIO_2")
				(number "49")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSIO_2")
				(number "48")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 2.54)
				(name "VREF+")
				(number "22")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 2.54)
				(name "VREF-")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 50.8 180)
				(length 2.54)
				(name "PE0")
				(number "70")
			)
			(pin bidirectional line
				(at 15.24 48.26 180)
				(length 2.54)
				(name "PE1")
				(number "69")
			)
			(pin bidirectional line
				(at 15.24 45.72 180)
				(length 2.54)
				(name "PE2")
				(number "68")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PE3")
				(number "67")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PE4")
				(number "66")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PE6")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PE7")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PF0")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PF3")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PF4")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PF5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PF6")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PF7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PG0")
				(number "52")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PG1")
				(number "53")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PG2")
				(number "54")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PG3")
				(number "55")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PG4")
				(number "56")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PG5")
				(number "63")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PG6")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PG7")
				(number "65")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8S208CB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 35.56 0)
		)
		(property "Value" "STM8S208CB"
			(at 12.7 33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208cb.pdf"
			(at 21.59 33.02 0)
		)
		(property "Description" "24MHz, 128K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, CAN, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8S208CB_0_1")
		(symbol "STM8S208CB_1_1"
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PA3")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA4")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA5")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA6")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PB0")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB1")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB3")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB7")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "34")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDDIO_1")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "VSSIO_1")
				(number "4")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDDIO_2")
				(number "32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "VSSIO_2")
				(number "31")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PD0")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PD1")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PD2")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PD3")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PD4")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PD5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PD6")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PD7")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PE0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PE1")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PE3")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PE5")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PE6")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PE7")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PG0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PG1")
				(number "36")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "NRST")
				(number "1")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "VCAP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8S208RB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 48.26 0)
		)
		(property "Value" "STM8S208RB"
			(at 13.97 45.72 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 1.27 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208rb.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "24MHz, 128K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, CAN, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM8S208RB_0_1")
		(symbol "STM8S208RB_1_1"
			(pin bidirectional line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "PA3")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PA4")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PA5")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PA6")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PB0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PB1")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PB3")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PB4")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PB5")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB6")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB7")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC2")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC3")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC4")
				(number "37")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC5")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PI0")
				(number "48")
			)
			(pin input line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "NRST")
				(number "1")
			)
			(pin input line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "VCAP")
				(number "6")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDIO_1")
				(number "8")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSSIO_1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDIO_2")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSIO_2")
				(number "39")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VREF+")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 2.54)
				(name "VREF-")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PD0")
				(number "57")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PD1")
				(number "58")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PD2")
				(number "59")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PD3")
				(number "60")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PD4")
				(number "61")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PD5")
				(number "62")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PD6")
				(number "63")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PD7")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PE0")
				(number "56")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PE1")
				(number "55")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PE2")
				(number "54")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PE3")
				(number "53")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PE4")
				(number "52")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PE5")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PE6")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PE7")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PF0")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PF3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PF4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PF5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PF6")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PF7")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PG0")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PG1")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PG2")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PG3")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PG4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PG5")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PG6")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PG7")
				(number "51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM8L101F2U"
		(extends "STM8L101F1U")
		(property "Reference" "U"
			(at -2.54 23.495 0)
		)
		(property "Value" "STM8L101F2U"
			(at -2.54 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at 1.27 -21.59 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8l101f1.pdf"
			(at 0 38.1 0)
		)
		(property "Description" "16MHz, 4K Flash, 1.5K RAM, 2K EEPROM, USART,  I²C, SPI, ADC, UFQFPN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8L Microcontroller Value Line Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8L101F3P"
		(extends "STM8L101F2P")
		(property "Reference" "U"
			(at 1.27 22.86 0)
		)
		(property "Value" "STM8L101F3P"
			(at 1.27 20.32 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 1.27 25.4 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00220591.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "16MHz, 8K Flash, 1.5K RAM, 2K EEPROM, USART, I²C, SPI, ADC, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8L Microcontroller Value Line Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8L101F3U"
		(extends "STM8L101F1U")
		(property "Reference" "U"
			(at -2.54 23.495 0)
		)
		(property "Value" "STM8L101F3U"
			(at -2.54 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at 1.27 -21.59 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8l101f1.pdf"
			(at 0 38.1 0)
		)
		(property "Description" "16MHz, 8K Flash, 1.5K RAM, 2K EEPROM, USART,  I²C, SPI, ADC, UFQFPN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8L Microcontroller Value Line Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8L151C3T"
		(extends "STM8L151C2T")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "STM8L151C3T"
			(at 13.97 38.1 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 -39.37 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8l151c3.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "8-bit ultra-low-power MCU, 8 KB Flash, 256 bytes data EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 ultra-low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8L152R6T"
		(extends "STM8L152R8T")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM8L152R6T"
			(at 8.89 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -7.62 -46.99 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8l152r6.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "16MHz, 32K Flash, 2K EEPROM, LCD, USART, I²C, SPI, ADC, DAC, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8L Microcontroller Low Power LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S207C6"
		(extends "STM8S208CB")
		(property "Reference" "U"
			(at 12.7 35.56 0)
		)
		(property "Value" "STM8S207C6"
			(at 12.7 33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208cb.pdf"
			(at 21.59 33.02 0)
		)
		(property "Description" "24MHz, 32K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S207C8"
		(extends "STM8S208CB")
		(property "Reference" "U"
			(at 12.7 35.56 0)
		)
		(property "Value" "STM8S207C8"
			(at 12.7 33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208cb.pdf"
			(at 21.59 33.02 0)
		)
		(property "Description" "24MHz, 64K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S207CB"
		(extends "STM8S208CB")
		(property "Reference" "U"
			(at 12.7 35.56 0)
		)
		(property "Value" "STM8S207CB"
			(at 12.7 33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208cb.pdf"
			(at 21.59 33.02 0)
		)
		(property "Description" "24MHz, 128K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S207R6"
		(extends "STM8S208RB")
		(property "Reference" "U"
			(at 13.97 48.26 0)
		)
		(property "Value" "STM8S207R6"
			(at 13.97 45.72 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 1.27 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208rb.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "24MHz, 32K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S207R8"
		(extends "STM8S208RB")
		(property "Reference" "U"
			(at 13.97 48.26 0)
		)
		(property "Value" "STM8S207R8"
			(at 13.97 45.72 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 1.27 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208rb.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "24MHz, 64K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S207RB"
		(extends "STM8S208RB")
		(property "Reference" "U"
			(at 13.97 48.26 0)
		)
		(property "Value" "STM8S207RB"
			(at 13.97 45.72 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 1.27 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208rb.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "24MHz, 128K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S208C6"
		(extends "STM8S208CB")
		(property "Reference" "U"
			(at 12.7 35.56 0)
		)
		(property "Value" "STM8S208C6"
			(at 12.7 33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208cb.pdf"
			(at 21.59 33.02 0)
		)
		(property "Description" "24MHz, 32K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, CAN, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S208C8"
		(extends "STM8S208CB")
		(property "Reference" "U"
			(at 12.7 35.56 0)
		)
		(property "Value" "STM8S208C8"
			(at 12.7 33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208cb.pdf"
			(at 21.59 33.02 0)
		)
		(property "Description" "24MHz, 64K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, CAN, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S208MB"
		(extends "STM8S207MB")
		(property "Reference" "U"
			(at 7.0359 58.42 0)
		)
		(property "Value" "STM8S208MB"
			(at 7.0359 55.88 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at 0 -67.31 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208mb.pdf"
			(at 0 -69.85 0)
		)
		(property "Description" "24MHz, 128K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, CAN, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*80*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S208R6"
		(extends "STM8S208RB")
		(property "Reference" "U"
			(at 13.97 48.26 0)
		)
		(property "Value" "STM8S208R6"
			(at 13.97 45.72 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 1.27 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208rb.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "24MHz, 32K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, CAN, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM8S208R8"
		(extends "STM8S208RB")
		(property "Reference" "U"
			(at 13.97 48.26 0)
		)
		(property "Value" "STM8S208R8"
			(at 13.97 45.72 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 1.27 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm8s208rb.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "24MHz, 64K Flash, 2K EEPROM, 10-bit ADC, 2 UARTs, SPI, I²C, CAN, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM8 Microcontroller Performance Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
