(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "FE310-G000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 29.21 0)
		)
		(property "Value" "FE310-G000"
			(at 12.7 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm_ThermalVias"
			(at 2.54 -29.21 0)
		)
		(property "Datasheet" "https://sifive.cdn.prismic.io/sifive%2Ffeb6f967-ff96-418f-9af4-a7f3b7fd1dfc_fe310-g000-ds.pdf"
			(at -27.94 31.75 0)
		)
		(property "Description" "RISC-V MCU, 8KB OTP Program Memory, 8KB ROM, 16KB Instruction Cache, 16KB SRAM, 320MHz, 1.8 and 3.6V, 24 GPIO, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller RISC-V SiFive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "FE310-G000_0_1")
		(symbol "FE310-G000_1_1"
			(pin input line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "XTAL_XI")
				(number "9")
			)
			(pin output line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "XTAL_XO")
				(number "10")
			)
			(pin input line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "JTAG_TCK")
				(number "13")
			)
			(pin output line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "JTAG_TDO")
				(number "14")
			)
			(pin input line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "JTAG_TMS")
				(number "15")
			)
			(pin input line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "JTAG_TDI")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "QSPI_DQ_0")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "QSPI_DQ_1")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "QSPI_DQ_2")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "QSPI_DQ_3")
				(number "1")
			)
			(pin output line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "~{QSPI_CS}")
				(number "5")
			)
			(pin output line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "QSPI_SCK")
				(number "48")
			)
			(pin output line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "AON_PMU_OUT_0")
				(number "22")
			)
			(pin output line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "AON_PMU_OUT_1")
				(number "17")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "~{AON_PMU_DWAKEUP}")
				(number "18")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "~{AON_ERST}")
				(number "24")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "AON_PSD_LFALTCLK")
				(number "20")
			)
			(pin input line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "AON_PSD_LFCLKSEL")
				(number "21")
			)
			(pin power_in line
				(at -7.62 30.48 270)
				(length 2.54)
				(name "AON_VDD")
				(number "23")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "AON_IVDD")
				(number "19")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "46")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "IVDD")
				(number "11")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "IVDD")
				(number "32")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "IVDD")
				(number "47")
			)
			(pin power_in line
				(at 5.08 -30.48 90)
				(length 2.54)
				(name "PLL_AVSS")
				(number "8")
			)
			(pin power_in line
				(at 7.62 30.48 270)
				(length 2.54)
				(name "OTP_AIVDD")
				(number "12")
			)
			(pin power_in line
				(at 10.16 30.48 270)
				(length 2.54)
				(name "PLL_AVDD")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "GPIO_0")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "GPIO_1")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "GPIO_2")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "GPIO_3")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "GPIO_4")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "GPIO_5")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "GPIO_9")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "GPIO_10")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "GPIO_11")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "GPIO_12")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "GPIO_13")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "GPIO_16")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "GPIO_17")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "GPIO_18")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "GPIO_19")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "GPIO_20")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "GPIO_21")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "GPIO_22")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "GPIO_23")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FU540-C000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "FU540-C000"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_BGA:BGA-484_23.0x23.0mm_Layout22x22_P1.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://static.dev.sifive.com/FU540-C000-v1.0.pdf"
			(at 0 127 0)
		)
		(property "Description" "64-bit RISC‑V SoC, BGA-484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "SiFive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*23.0x23.0mm*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "FU540-C000_1_1"
			(pin input line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "CL_0_B2C_CLK")
				(number "AA22")
			)
			(pin input line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "CL_0_B2C_D_0")
				(number "Y16")
			)
			(pin input line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "CL_0_B2C_D_1")
				(number "AB18")
			)
			(pin input line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "CL_0_B2C_D_2")
				(number "AA18")
			)
			(pin input line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "CL_0_B2C_D_3")
				(number "W17")
			)
			(pin input line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "CL_0_B2C_D_4")
				(number "W16")
			)
			(pin input line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "CL_0_B2C_D_5")
				(number "W18")
			)
			(pin input line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "CL_0_B2C_D_6")
				(number "Y18")
			)
			(pin input line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "CL_0_B2C_D_7")
				(number "Y17")
			)
			(pin input line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "CL_0_B2C_D_8")
				(number "AA19")
			)
			(pin input line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "CL_0_B2C_D_9")
				(number "V18")
			)
			(pin input line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "CL_0_B2C_D_10")
				(number "Y19")
			)
			(pin input line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "CL_0_B2C_D_11")
				(number "W19")
			)
			(pin input line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "CL_0_B2C_D_12")
				(number "V16")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "CL_0_B2C_D_13")
				(number "AB19")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "CL_0_B2C_D_14")
				(number "U18")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "CL_0_B2C_D_15")
				(number "V19")
			)
			(pin input line
				(at -27.94 0 0)
				(length 5.08)
				(name "CL_0_B2C_D_16")
				(number "V17")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "CL_0_B2C_D_17")
				(number "R18")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "CL_0_B2C_D_18")
				(number "U19")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "CL_0_B2C_D_19")
				(number "T18")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "CL_0_B2C_D_20")
				(number "U17")
			)
			(pin input line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "CL_0_B2C_D_21")
				(number "P18")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "CL_0_B2C_D_22")
				(number "AB20")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "CL_0_B2C_D_23")
				(number "AA20")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "CL_0_B2C_D_24")
				(number "R17")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "CL_0_B2C_D_25")
				(number "V20")
			)
			(pin input line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "CL_0_B2C_D_26")
				(number "AB21")
			)
			(pin input line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "CL_0_B2C_D_27")
				(number "Y20")
			)
			(pin input line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "CL_0_B2C_D_28")
				(number "W20")
			)
			(pin input line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "CL_0_B2C_D_29")
				(number "AA21")
			)
			(pin input line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "CL_0_B2C_D_30")
				(number "Y22")
			)
			(pin input line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "CL_0_B2C_D_31")
				(number "Y21")
			)
			(pin input line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "CL_0_B2C_RST")
				(number "P17")
			)
			(pin input line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "CL_0_B2C_SEND")
				(number "W21")
			)
			(pin output line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "CL_0_C2B_CLK")
				(number "P19")
			)
			(pin output line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "CL_0_C2B_D_0")
				(number "T19")
			)
			(pin output line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "CL_0_C2B_D_1")
				(number "R19")
			)
			(pin output line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "CL_0_C2B_D_2")
				(number "N18")
			)
			(pin output line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "CL_0_C2B_D_3")
				(number "R20")
			)
			(pin output line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "CL_0_C2B_D_4")
				(number "P20")
			)
			(pin output line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "CL_0_C2B_D_5")
				(number "U20")
			)
			(pin output line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "CL_0_C2B_D_6")
				(number "N19")
			)
			(pin output line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "CL_0_C2B_D_7")
				(number "U22")
			)
			(pin output line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "CL_0_C2B_D_8")
				(number "R21")
			)
			(pin output line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "CL_0_C2B_D_9")
				(number "W22")
			)
			(pin output line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "CL_0_C2B_D_10")
				(number "T22")
			)
			(pin output line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "CL_0_C2B_D_11")
				(number "U21")
			)
			(pin output line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "CL_0_C2B_D_12")
				(number "M20")
			)
			(pin output line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "CL_0_C2B_D_13")
				(number "T21")
			)
			(pin output line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "CL_0_C2B_D_14")
				(number "N22")
			)
			(pin output line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "CL_0_C2B_D_15")
				(number "M17")
			)
			(pin output line
				(at 27.94 0 180)
				(length 5.08)
				(name "CL_0_C2B_D_16")
				(number "N21")
			)
			(pin output line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "CL_0_C2B_D_17")
				(number "R22")
			)
			(pin output line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "CL_0_C2B_D_18")
				(number "L21")
			)
			(pin output line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "CL_0_C2B_D_19")
				(number "M18")
			)
			(pin output line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "CL_0_C2B_D_20")
				(number "L20")
			)
			(pin output line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "CL_0_C2B_D_21")
				(number "N20")
			)
			(pin output line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "CL_0_C2B_D_22")
				(number "M22")
			)
			(pin output line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "CL_0_C2B_D_23")
				(number "M19")
			)
			(pin output line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "CL_0_C2B_D_24")
				(number "K20")
			)
			(pin output line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "CL_0_C2B_D_25")
				(number "M21")
			)
			(pin output line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "CL_0_C2B_D_26")
				(number "K22")
			)
			(pin output line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "CL_0_C2B_D_27")
				(number "L19")
			)
			(pin output line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "CL_0_C2B_D_28")
				(number "K19")
			)
			(pin output line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "CL_0_C2B_D_29")
				(number "L22")
			)
			(pin output line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "CL_0_C2B_D_30")
				(number "L18")
			)
			(pin output line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "CL_0_C2B_D_31")
				(number "L17")
			)
			(pin output line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "CL_0_C2B_RST")
				(number "T20")
			)
			(pin output line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "CL_0_C2B_SEND")
				(number "N17")
			)
		)
		(symbol "FU540-C000_2_1"
			(pin output line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[15]")
				(number "V3")
			)
			(pin output line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[14]")
				(number "U3")
			)
			(pin output line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[13]")
				(number "T2")
			)
			(pin output line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[12]")
				(number "P5")
			)
			(pin output line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[11]")
				(number "R4")
			)
			(pin output line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[10]")
				(number "U1")
			)
			(pin output line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[9]")
				(number "T3")
			)
			(pin output line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[8]")
				(number "R3")
			)
			(pin output line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[7]")
				(number "R2")
			)
			(pin output line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[6]")
				(number "P4")
			)
			(pin output line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[5]")
				(number "N5")
			)
			(pin output line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[4]")
				(number "T1")
			)
			(pin output line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[3]")
				(number "P3")
			)
			(pin output line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[2]")
				(number "N4")
			)
			(pin output line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[1]")
				(number "R1")
			)
			(pin output line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "DDR_MEM_ADDR[0]")
				(number "N3")
			)
			(pin output line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "DDR_MEM_BANK[2]")
				(number "M5")
			)
			(pin output line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "DDR_MEM_BANK[1]")
				(number "N2")
			)
			(pin output line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "DDR_MEM_BANK[0]")
				(number "M4")
			)
			(pin output line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "DDR_MEM_CAS_N")
				(number "M3")
			)
			(pin output line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "DDR_MEM_RAS_N")
				(number "M2")
			)
			(pin output line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "DDR_MEM_WE_N")
				(number "N1")
			)
			(pin output line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "DDR_MEM_PARITY_IN")
				(number "U2")
			)
			(pin input line
				(at -33.02 0 0)
				(length 5.08)
				(name "DDR_MEM_ERROR_N")
				(number "W6")
			)
			(pin output line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "DDR_MEM_ODT[0]")
				(number "AA5")
			)
			(pin output line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "DDR_MEM_ODT[1]")
				(number "AB5")
			)
			(pin output line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "DDR_MEM_CKE[0]")
				(number "AB6")
			)
			(pin output line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "DDR_MEM_CKE[1]")
				(number "AA6")
			)
			(pin output line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "DDR_MEM_CS_N[0]")
				(number "Y6")
			)
			(pin output line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "DDR_MEM_CS_N[1]")
				(number "W7")
			)
			(pin output line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "DDR_MEM_RESET_N")
				(number "Y5")
			)
			(pin output line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "DDR_MEM_CLK")
				(number "K5")
			)
			(pin output line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "DDR_MEM_CLK_N")
				(number "L5")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "DDR_MEM_ECC_D[7]")
				(number "L3")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "DDR_MEM_ECC_D[6]")
				(number "M1")
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "DDR_MEM_ECC_D[5]")
				(number "L4")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "DDR_MEM_ECC_D[4]")
				(number "L1")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "DDR_MEM_ECC_D[3]")
				(number "L2")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "DDR_MEM_ECC_D[2]")
				(number "K4")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "DDR_MEM_ECC_D[1]")
				(number "K1")
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "DDR_MEM_ECC_D[0]")
				(number "H5")
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "DDR_MEM_ECC_DQS_P")
				(number "K2")
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "DDR_MEM_ECC_DQS_M")
				(number "K3")
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "DDR_MEM_ECC_DM")
				(number "J5")
			)
			(pin passive line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "DDR_RSVD0")
				(number "E8")
			)
			(pin passive line
				(at -33.02 -68.58 0)
				(length 5.08)
				(name "DDR_RSVD1")
				(number "D8")
			)
			(pin passive line
				(at -33.02 -71.12 0)
				(length 5.08)
				(name "DDR_RSVD2")
				(number "F8")
			)
			(pin passive line
				(at -33.02 -73.66 0)
				(length 5.08)
				(name "DDR_RSVD3")
				(number "F9")
			)
			(pin passive line
				(at -33.02 -119.38 0)
				(length 5.08)
				(name "DDR_CAL_0")
				(number "F6")
			)
			(pin bidirectional line
				(at 33.02 119.38 180)
				(length 5.08)
				(name "DDR_MEM_D[7]")
				(number "G3")
			)
			(pin bidirectional line
				(at 33.02 116.84 180)
				(length 5.08)
				(name "DDR_MEM_D[6]")
				(number "E1")
			)
			(pin bidirectional line
				(at 33.02 114.3 180)
				(length 5.08)
				(name "DDR_MEM_D[5]")
				(number "G4")
			)
			(pin bidirectional line
				(at 33.02 111.76 180)
				(length 5.08)
				(name "DDR_MEM_D[4]")
				(number "C1")
			)
			(pin bidirectional line
				(at 33.02 109.22 180)
				(length 5.08)
				(name "DDR_MEM_D[3]")
				(number "E2")
			)
			(pin bidirectional line
				(at 33.02 106.68 180)
				(length 5.08)
				(name "DDR_MEM_D[2]")
				(number "F4")
			)
			(pin bidirectional line
				(at 33.02 104.14 180)
				(length 5.08)
				(name "DDR_MEM_D[1]")
				(number "B1")
			)
			(pin bidirectional line
				(at 33.02 101.6 180)
				(length 5.08)
				(name "DDR_MEM_D[0]")
				(number "D2")
			)
			(pin bidirectional line
				(at 33.02 99.06 180)
				(length 5.08)
				(name "DDR_MEM_DQS_P[0]")
				(number "F2")
			)
			(pin bidirectional line
				(at 33.02 96.52 180)
				(length 5.08)
				(name "DDR_MEM_DQS_M[0]")
				(number "F3")
			)
			(pin bidirectional line
				(at 33.02 93.98 180)
				(length 5.08)
				(name "DDR_MEM_DM[0]")
				(number "E5")
			)
			(pin bidirectional line
				(at 33.02 88.9 180)
				(length 5.08)
				(name "DDR_MEM_D[15]")
				(number "J4")
			)
			(pin bidirectional line
				(at 33.02 86.36 180)
				(length 5.08)
				(name "DDR_MEM_D[14]")
				(number "J2")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "DDR_MEM_D[13]")
				(number "J3")
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "DDR_MEM_D[12]")
				(number "H1")
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "DDR_MEM_D[11]")
				(number "G1")
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "DDR_MEM_D[10]")
				(number "F5")
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "DDR_MEM_D[9]")
				(number "F1")
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "DDR_MEM_D[8]")
				(number "H4")
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "DDR_MEM_DQS_P[1]")
				(number "H2")
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "DDR_MEM_DQS_M[1]")
				(number "H3")
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "DDR_MEM_DM[1]")
				(number "G5")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "DDR_MEM_D[23]")
				(number "B6")
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "DDR_MEM_D[22]")
				(number "B3")
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "DDR_MEM_D[21]")
				(number "C5")
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "DDR_MEM_D[20]")
				(number "B5")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "DDR_MEM_D[19]")
				(number "A5")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "DDR_MEM_D[18]")
				(number "A4")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "DDR_MEM_D[17]")
				(number "B2")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "DDR_MEM_D[16]")
				(number "B4")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "DDR_MEM_DQS_P[2]")
				(number "A6")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "DDR_MEM_DQS_M[2]")
				(number "A7")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "DDR_MEM_DM[2]")
				(number "C6")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "DDR_MEM_D[31]")
				(number "C7")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "DDR_MEM_D[30]")
				(number "D3")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "DDR_MEM_D[29]")
				(number "C2")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "DDR_MEM_D[28]")
				(number "E6")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "DDR_MEM_D[27]")
				(number "C3")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "DDR_MEM_D[26]")
				(number "D6")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "DDR_MEM_D[25]")
				(number "D4")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "DDR_MEM_D[24]")
				(number "C4")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "DDR_MEM_DQS_P[3]")
				(number "E7")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "DDR_MEM_DQS_M[3]")
				(number "D7")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "DDR_MEM_DM[3]")
				(number "D5")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "DDR_MEM_D[39]")
				(number "U5")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "DDR_MEM_D[38]")
				(number "W2")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "DDR_MEM_D[37]")
				(number "W3")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "DDR_MEM_D[36]")
				(number "Y1")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "DDR_MEM_D[35]")
				(number "V2")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "DDR_MEM_D[34]")
				(number "T4")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "DDR_MEM_D[33]")
				(number "W1")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "DDR_MEM_D[32]")
				(number "R5")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "DDR_MEM_DQS_P[4]")
				(number "V4")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "DDR_MEM_DQS_M[4]")
				(number "U4")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "DDR_MEM_DM[4]")
				(number "T5")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "DDR_MEM_D[47]")
				(number "AA4")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "DDR_MEM_D[46]")
				(number "AB3")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "DDR_MEM_D[45]")
				(number "AA3")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "DDR_MEM_D[44]")
				(number "AB2")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "DDR_MEM_D[43]")
				(number "Y2")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "DDR_MEM_D[42]")
				(number "Y3")
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "DDR_MEM_D[41]")
				(number "AA1")
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "DDR_MEM_D[40]")
				(number "V5")
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "DDR_MEM_DQS_P[5]")
				(number "Y4")
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "DDR_MEM_DQS_M[5]")
				(number "W4")
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "DDR_MEM_DM[5]")
				(number "W5")
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "DDR_MEM_D[55]")
				(number "W9")
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "DDR_MEM_D[54]")
				(number "W12")
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "DDR_MEM_D[53]")
				(number "Y9")
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "DDR_MEM_D[52]")
				(number "Y10")
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "DDR_MEM_D[51]")
				(number "W8")
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "DDR_MEM_D[50]")
				(number "Y11")
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "DDR_MEM_D[49]")
				(number "W11")
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "DDR_MEM_D[48]")
				(number "Y12")
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "DDR_MEM_DQS_P[6]")
				(number "Y7")
			)
			(pin bidirectional line
				(at 33.02 -86.36 180)
				(length 5.08)
				(name "DDR_MEM_DQS_M[6]")
				(number "AA7")
			)
			(pin bidirectional line
				(at 33.02 -88.9 180)
				(length 5.08)
				(name "DDR_MEM_DM[6]")
				(number "W10")
			)
			(pin bidirectional line
				(at 33.02 -93.98 180)
				(length 5.08)
				(name "DDR_MEM_D[63]")
				(number "AA11")
			)
			(pin bidirectional line
				(at 33.02 -96.52 180)
				(length 5.08)
				(name "DDR_MEM_D[62]")
				(number "AA9")
			)
			(pin bidirectional line
				(at 33.02 -99.06 180)
				(length 5.08)
				(name "DDR_MEM_D[61]")
				(number "AA10")
			)
			(pin bidirectional line
				(at 33.02 -101.6 180)
				(length 5.08)
				(name "DDR_MEM_D[60]")
				(number "AB11")
			)
			(pin bidirectional line
				(at 33.02 -104.14 180)
				(length 5.08)
				(name "DDR_MEM_D[59]")
				(number "AB9")
			)
			(pin bidirectional line
				(at 33.02 -106.68 180)
				(length 5.08)
				(name "DDR_MEM_D[58]")
				(number "AA12")
			)
			(pin bidirectional line
				(at 33.02 -109.22 180)
				(length 5.08)
				(name "DDR_MEM_D[57]")
				(number "AB8")
			)
			(pin bidirectional line
				(at 33.02 -111.76 180)
				(length 5.08)
				(name "DDR_MEM_D[56]")
				(number "AA13")
			)
			(pin bidirectional line
				(at 33.02 -114.3 180)
				(length 5.08)
				(name "DDR_MEM_DQS_P[7]")
				(number "AA8")
			)
			(pin bidirectional line
				(at 33.02 -116.84 180)
				(length 5.08)
				(name "DDR_MEM_DQS_M[7]")
				(number "Y8")
			)
			(pin bidirectional line
				(at 33.02 -119.38 180)
				(length 5.08)
				(name "DDR_MEM_DM[7]")
				(number "AB12")
			)
		)
		(symbol "FU540-C000_3_1"
			(pin input line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "GEMGXL_0_GTX_CLK")
				(number "E12")
			)
			(pin input line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "GEMGXL_0_RX_CLK")
				(number "F12")
			)
			(pin input line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "GEMGXL_0_RXD_0")
				(number "A12")
			)
			(pin input line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "GEMGXL_0_RXD_1")
				(number "B10")
			)
			(pin input line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "GEMGXL_0_RXD_2")
				(number "A10")
			)
			(pin input line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "GEMGXL_0_RXD_3")
				(number "E11")
			)
			(pin input line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "GEMGXL_0_RXD_4")
				(number "E10")
			)
			(pin input line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "GEMGXL_0_RXD_5")
				(number "A8")
			)
			(pin input line
				(at -30.48 0 0)
				(length 5.08)
				(name "GEMGXL_0_RXD_6")
				(number "C9")
			)
			(pin input line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "GEMGXL_0_RXD_7")
				(number "E9")
			)
			(pin input line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "GEMGXL_0_RX_DV")
				(number "A11")
			)
			(pin input line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "GEMGXL_0_RX_ER")
				(number "B11")
			)
			(pin input line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "GEMGXL_0_CRS")
				(number "C13")
			)
			(pin input line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "GEMGXL_0_COL")
				(number "A13")
			)
			(pin output line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "GEMGXL_0_MDC")
				(number "B13")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "GEMGXL_0_MDIO")
				(number "C12")
			)
			(pin input line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "GEMGXL_0_TX_CLK")
				(number "C8")
			)
			(pin output line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "GEMGXL_0_TXD_0")
				(number "B12")
			)
			(pin output line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "GEMGXL_0_TXD_1")
				(number "C11")
			)
			(pin output line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "GEMGXL_0_TXD_2")
				(number "D11")
			)
			(pin output line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "GEMGXL_0_TXD_3")
				(number "F11")
			)
			(pin output line
				(at 30.48 0 180)
				(length 5.08)
				(name "GEMGXL_0_TXD_4")
				(number "C10")
			)
			(pin output line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "GEMGXL_0_TXD_5")
				(number "D10")
			)
			(pin output line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "GEMGXL_0_TXD_6")
				(number "B8")
			)
			(pin output line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "GEMGXL_0_TXD_7")
				(number "D9")
			)
			(pin output line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "GEMGXL_0_TX_EN")
				(number "B7")
			)
			(pin output line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "GEMGXL_0_TX_ER")
				(number "F10")
			)
		)
		(symbol "FU540-C000_4_1"
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "GPIO_0_P_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "GPIO_0_P_1")
				(number "C22")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "GPIO_0_P_2")
				(number "C21")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "GPIO_0_P_3")
				(number "D21")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "GPIO_0_P_4")
				(number "E18")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "GPIO_0_P_5")
				(number "D20")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "GPIO_0_P_6")
				(number "E20")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "GPIO_0_P_7")
				(number "C20")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "GPIO_0_P_8")
				(number "D19")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "GPIO_0_P_9")
				(number "A21")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "GPIO_0_P_10")
				(number "F18")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "GPIO_0_P_11")
				(number "B20")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "GPIO_0_P_12")
				(number "B21")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "GPIO_0_P_13")
				(number "E19")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "GPIO_0_P_14")
				(number "B22")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "GPIO_0_P_15")
				(number "G17")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "I2C_0_SCL")
				(number "Y14")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "I2C_0_SDA")
				(number "W13")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PWM_0_P_0")
				(number "G19")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PWM_0_P_1")
				(number "F21")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PWM_0_P_2")
				(number "F20")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PWM_0_P_3")
				(number "G20")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PWM_1_P_0")
				(number "D22")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PWM_1_P_1")
				(number "H17")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PWM_1_P_2")
				(number "G18")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PWM_1_P_3")
				(number "F19")
			)
			(pin output line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "UART_0_TXD")
				(number "Y13")
			)
			(pin input line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "UART_0_RXD")
				(number "W14")
			)
			(pin output line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "UART_1_TXD")
				(number "AA15")
			)
			(pin input line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "UART_1_RXD")
				(number "AA14")
			)
			(pin output line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "QSPI_2_SCK")
				(number "W15")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "QSPI_2_DQ_0")
				(number "AA16")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "QSPI_2_DQ_1")
				(number "AB15")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "QSPI_2_DQ_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "QSPI_2_DQ_3")
				(number "Y15")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "QSPI_2_CS_0")
				(number "AB14")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "QSPI_0_SCK")
				(number "K18")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "QSPI_0_DQ_0")
				(number "H21")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "QSPI_0_DQ_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "QSPI_0_DQ_2")
				(number "J21")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "QSPI_0_DQ_3")
				(number "H20")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "QSPI_0_CS_0")
				(number "J19")
			)
			(pin output line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "QSPI_1_SCK")
				(number "H18")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "QSPI_1_DQ_0")
				(number "G22")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "QSPI_1_DQ_1")
				(number "J18")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "QSPI_1_DQ_2")
				(number "F22")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "QSPI_1_DQ_3")
				(number "J17")
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "QSPI_1_CS_0")
				(number "K17")
			)
			(pin output line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "QSPI_1_CS_1")
				(number "G21")
			)
			(pin output line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "QSPI_1_CS_2")
				(number "H19")
			)
			(pin output line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "QSPI_1_CS_3")
				(number "J20")
			)
		)
		(symbol "FU540-C000_5_1"
			(pin passive line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PRCI_RSVD0")
				(number "A16")
			)
			(pin input line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PRCI_RTCXSEL")
				(number "D15")
			)
			(pin passive line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PRCI_RTCXALTCLKIN")
				(number "B16")
			)
			(pin passive line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PRCI_RSVD1")
				(number "D13")
			)
			(pin passive line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PRCI_RSVD2")
				(number "E13")
			)
			(pin passive line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PRCI_RSVD3")
				(number "D16")
			)
			(pin passive line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PRCI_RSVD4")
				(number "C16")
			)
			(pin passive line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PRCI_RSVD5")
				(number "E15")
			)
			(pin passive line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PRCI_RSVD6")
				(number "B17")
			)
			(pin passive line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PRCI_RSVD7")
				(number "G13")
			)
			(pin passive line
				(at -27.94 0 0)
				(length 5.08)
				(name "PRCI_RSVD8")
				(number "H13")
			)
			(pin passive line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PRCI_RSVD9")
				(number "E16")
			)
			(pin passive line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PRCI_RSVD10")
				(number "D17")
			)
			(pin passive line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PRCI_RSVD11")
				(number "D14")
			)
			(pin passive line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PRCI_RSVD12")
				(number "E14")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PRCI_HFXSEL")
				(number "C15")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PRCI_ERESET_N")
				(number "C17")
			)
			(pin input line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PRCI_PORESET_N")
				(number "A17")
			)
			(pin input line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "JTAG_TCK")
				(number "D18")
			)
			(pin input line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "JTAG_TDI")
				(number "C19")
			)
			(pin output line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "JTAG_TDO")
				(number "E17")
			)
			(pin input line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "JTAG_TMS")
				(number "F16")
			)
			(pin passive line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PRCI_RSVD13")
				(number "F14")
			)
			(pin passive line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PRCI_RSVD14")
				(number "F13")
			)
			(pin passive line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PRCI_RSVD15")
				(number "C14")
			)
			(pin input line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PRCI_HFXCLKIN")
				(number "F15")
			)
			(pin passive line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "HFXOSCIN")
				(number "A15")
			)
			(pin passive line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "HFXOSCOUT")
				(number "B15")
			)
			(pin input line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "MSEL_MSEL_0")
				(number "A19")
			)
			(pin input line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "MSEL_MSEL_1")
				(number "C18")
			)
			(pin input line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "MSEL_MSEL_2")
				(number "A20")
			)
			(pin input line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "MSEL_MSEL_3")
				(number "B19")
			)
		)
		(symbol "FU540-C000_6_1"
			(pin power_in line
				(at -15.24 22.86 270)
				(length 5.08)
				(name "IVDD")
				(number "K16")
			)
			(pin passive line
				(at -15.24 22.86 270)
				(length 5.08)
				(hide yes)
				(name "IVDD")
				(number "L16")
			)
			(pin passive line
				(at -15.24 22.86 270)
				(length 5.08)
				(hide yes)
				(name "IVDD")
				(number "M16")
			)
			(pin passive line
				(at -15.24 22.86 270)
				(length 5.08)
				(hide yes)
				(name "IVDD")
				(number "N16")
			)
			(pin power_in line
				(at -15.24 -22.86 90)
				(length 5.08)
				(name "IVSS")
				(number "K15")
			)
			(pin passive line
				(at -15.24 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "IVSS")
				(number "L15")
			)
			(pin passive line
				(at -15.24 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "IVSS")
				(number "M15")
			)
			(pin passive line
				(at -15.24 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "IVSS")
				(number "N15")
			)
			(pin power_in line
				(at -10.16 22.86 270)
				(length 5.08)
				(name "GEMGXLPLL_AVDD")
				(number "K12")
			)
			(pin power_in line
				(at -10.16 -22.86 90)
				(length 5.08)
				(name "GEMGXLPLL_AVSS")
				(number "J12")
			)
			(pin power_in line
				(at -7.62 22.86 270)
				(length 5.08)
				(name "GIVDD")
				(number "J11")
			)
			(pin power_in line
				(at -7.62 -22.86 90)
				(length 5.08)
				(name "GIVSS")
				(number "H11")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "AA17")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "B14")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "B18")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "B9")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E21")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E3")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "G11")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "G15")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "G9")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "H10")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "H12")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "H14")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "H16")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "H8")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "J15")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "J9")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "K10")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "K21")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "K8")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "L11")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "L13")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "M10")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "M12")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "M14")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "M8")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "N11")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "N13")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "N9")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P10")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P12")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P14")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P16")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P2")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P21")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P8")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "R11")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "R13")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "R15")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "R9")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "T10")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "T12")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "T14")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "T16")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "T8")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "U11")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "U13")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "U15")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "U9")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "V10")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "V12")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "V14")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "V21")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "V6")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "V8")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A14")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A18")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A2")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A22")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A3")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A9")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AA2")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB1")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB10")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB13")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB17")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB22")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB4")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB7")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D1")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D12")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E22")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G16")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H15")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J1")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J16")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J22")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K11")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L10")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L12")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L14")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L6")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L8")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M11")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M13")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N10")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N12")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N14")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N6")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N8")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P1")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P11")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P13")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P15")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P22")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P7")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P9")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R10")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R12")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R14")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R16")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R6")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R8")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T11")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T13")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T15")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T17")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T7")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T9")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "U10")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "U12")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "U14")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "U16")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "U6")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "U8")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V1")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V11")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V13")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V15")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V22")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V7")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V9")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 5.08)
				(name "DDR_VDDQ")
				(number "G7")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDQ")
				(number "H6")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDQ")
				(number "J7")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDQ")
				(number "K6")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDQ")
				(number "L7")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDQ")
				(number "M6")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDQ")
				(number "N7")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDQ")
				(number "P6")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDQ")
				(number "R7")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDQ")
				(number "T6")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 5.08)
				(name "DDR_VDDQCK")
				(number "U7")
			)
			(pin passive line
				(at 7.62 22.86 270)
				(length 5.08)
				(hide yes)
				(name "DDR_VDDPLL")
				(number "L9")
			)
			(pin power_in line
				(at 7.62 22.86 270)
				(length 5.08)
				(name "DDR_VDDPLL")
				(number "M9")
			)
			(pin power_in line
				(at 10.16 22.86 270)
				(length 5.08)
				(name "DDRPLL_AVDD")
				(number "K13")
			)
			(pin power_in line
				(at 10.16 -22.86 90)
				(length 5.08)
				(name "DDRPLL_AVSS")
				(number "J13")
			)
			(pin power_in line
				(at 15.24 22.86 270)
				(length 5.08)
				(name "OTP_VDD")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 22.86 270)
				(length 5.08)
				(name "COREPLL_AVDD")
				(number "K14")
			)
			(pin power_in line
				(at 17.78 -22.86 90)
				(length 5.08)
				(name "COREPLL_AVSS")
				(number "J14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FE310-G002"
		(extends "FE310-G000")
		(property "Reference" "U"
			(at -25.4 29.21 0)
		)
		(property "Value" "FE310-G002"
			(at 12.7 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm_ThermalVias"
			(at 2.54 -29.21 0)
		)
		(property "Datasheet" "https://sifive.cdn.prismic.io/sifive%2F3d777659-a0dd-49ed-a011-5bebba17aecf_fe310-g002-ds.pdf"
			(at -27.94 31.75 0)
		)
		(property "Description" "RISC-V MCU, 8KB OTP Program Memory, 8KB ROM, 16KB Instruction Cache, 16KB SRAM, 320MHz, 1.8 and 3.6V, 24 GPIO, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller RISC-V SiFive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*"
			(at 0 0 0)
		)
	)
)
