(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "C8051F321-GM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F321-GM"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at -0.508 -41.148 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F32x.pdf"
			(at -1.016 -38.608 0)
		)
		(property "Description" "16 KB ISP FLASH MCU Family with Full Speed USB, 2304 bytes internal RAM, 21 port I/O, 10-bit ADC, built-in temperature sensor, fully compatible with MCS-51 instruction set, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART SPI SMbus I2C VREF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*EP3.25*"
			(at 0 0 0)
		)
		(symbol "C8051F321-GM_0_1")
		(symbol "C8051F321-GM_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D-")
				(number "5")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RST}/C2CK")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "P3.0/C2D")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "P0.0")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "P0.1")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "P0.2")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "P0.3")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "P0.4")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "P0.5")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "P0.6")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "P0.7")
				(number "23")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "REGIN")
				(number "7")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "P1.0")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "P1.1")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "P1.2")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "P1.3")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "P1.4")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "P1.5")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "P1.6")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P1.7")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P2.0")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "P2.1")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "P2.2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "P2.3")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C8051F380-GQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 40.64 0)
		)
		(property "Value" "C8051F380-GQ"
			(at 12.7 40.64 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at -25.4 -38.1 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -12.7 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 64k flash, 4352 ram, 40 IO, EMIF, ADC, Temperature, VREF, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C ADC EMIF TQFP48"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "C8051F380-GQ_0_1")
		(symbol "C8051F380-GQ_1_1"
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "D+")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "D-")
				(number "9")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "VBUS")
				(number "12")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{RST}/C2CK")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "C2D")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "P0.0")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "P0.1")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "P0.2")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "P0.3")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "P0.4")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "P0.5")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "P0.6")
				(number "48")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "P0.7")
				(number "47")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "P1.0")
				(number "46")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "P1.1")
				(number "45")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "P1.2")
				(number "44")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "P1.3")
				(number "43")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "P1.4")
				(number "42")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "P1.5")
				(number "41")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "P1.6")
				(number "40")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "P1.7")
				(number "39")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "REGIN")
				(number "11")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "P2.0")
				(number "38")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "P2.1")
				(number "37")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "P2.2")
				(number "36")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "P2.3")
				(number "35")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "P2.4")
				(number "34")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "P2.5")
				(number "33")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "P2.6")
				(number "32")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "P2.7")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "P3.0")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "P3.1")
				(number "29")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "P3.2")
				(number "28")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P3.3")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "P3.4")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P3.5")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "P3.6")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "P3.7")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "P4.0")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "P4.1")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "P4.2")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "P4.3")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "P4.4")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "P4.5")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "P4.6")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "P4.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C8051F381-GM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F381-GM"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.3x3.3mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 64k flash, 4352 ram, 25 IO, ADC, Temperature, VREF, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C ADC QFN32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "C8051F381-GM_0_1")
		(symbol "C8051F381-GM_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D-")
				(number "5")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RST}/C2CK")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "P3.0/C2D")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "P0.0")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "P0.1")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "P0.2")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "P0.3")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "P0.4")
				(number "30")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "P0.5")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "P0.6")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "P0.7")
				(number "27")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "REGIN")
				(number "7")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "P1.0")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "P1.1")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "P1.2")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "P1.3")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "P1.4")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "P1.5")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P1.7")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P2.0")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "P2.1")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "P2.2")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "P2.3")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "P2.4")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "P2.6")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "P2.7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C8051F381-GQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F381-GQ"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 64k flash, 4352 ram, 25 IO, ADC, Temperature, VREF, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C ADC LQFP32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "C8051F381-GQ_0_1")
		(symbol "C8051F381-GQ_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D-")
				(number "5")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RST}/C2CK")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "P3.0/C2D")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "P0.0")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "P0.1")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "P0.2")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "P0.3")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "P0.4")
				(number "30")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "P0.5")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "P0.6")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "P0.7")
				(number "27")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "REGIN")
				(number "7")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "P1.0")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "P1.1")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "P1.2")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "P1.3")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "P1.4")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "P1.5")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P1.7")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P2.0")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "P2.1")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "P2.2")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "P2.3")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "P2.4")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "P2.6")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "P2.7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFM32G230F128G-E-QFN64"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 43.18 0)
		)
		(property "Value" "EFM32G230F128G-E-QFN64"
			(at 22.86 43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.3x7.3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32g-datasheet.pdf"
			(at 15.24 -12.7 0)
		)
		(property "Description" "32-bit ARM Cortex-M3 microcontroller, 128 kB flash, 16 kB x 8 RAM, Silicon Labs - Gecko, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EFM32G230F128G-E-QFN64_0_1")
		(symbol "EFM32G230F128G-E-QFN64_1_1"
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA5")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA8")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA9")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA15")
				(number "64")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PB7")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB8")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB11")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB12")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB13")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB14")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD0")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD1")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD2")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD3")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD4")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD5")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD6")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PD7")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PD8")
				(number "36")
			)
			(pin input line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin power_in line
				(at -7.62 43.18 270)
				(length 2.54)
				(name "VDD_DREG")
				(number "39")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "IOVDD")
				(number "26")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "IOVDD")
				(number "55")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "IOVDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "65")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "AVDD")
				(number "23")
			)
			(pin passive line
				(at 2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "27")
			)
			(pin passive line
				(at 7.62 43.18 270)
				(length 2.54)
				(name "DECOUPLE")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PC0")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PC1")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PC2")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PC3")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PC4")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PC5")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PC6")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PC7")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PC8")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PC9")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PC10")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PC11")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PC12")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PC13")
				(number "46")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PC14")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PC15")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PE8")
				(number "56")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PE9")
				(number "57")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PE10")
				(number "58")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PE11")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PE12")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PE13")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PE14")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PE15")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PF0")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PF1")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PF2")
				(number "51")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PF3")
				(number "52")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PF4")
				(number "53")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PF5")
				(number "54")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFM32HG108F32G-C-QFN24"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32HG108F32G-C-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32hg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32 kB flash, 4 kB  RAM, Silicon Labs - Happy Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 happy gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "EFM32HG108F32G-C-QFN24_0_1")
		(symbol "EFM32HG108F32G-C-QFN24_1_1"
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PB7")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB8")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB11")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB13")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB14")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC0")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC1")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "18")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD_DREG")
				(number "15")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "IOVDD")
				(number "2")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 2.54)
				(hide yes)
				(name "IOVDD")
				(number "22")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "12")
			)
			(pin passive line
				(at 7.62 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PD6")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PD7")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PE12")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PE13")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PF0")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PF1")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PF2")
				(number "21")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "DECOUPLE")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFM32HG308F32G-C-QFN24"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "EFM32HG308F32G-C-QFN24"
			(at 25.4 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32hg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32 kB flash, 4 kB  RAM, Silicon Labs - Happy Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 happy gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "EFM32HG308F32G-C-QFN24_0_1")
		(symbol "EFM32HG308F32G-C-QFN24_1_1"
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PB7")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB8")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB11")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB13")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB14")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC0")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC1")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "18")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "USB_VREGI")
				(number "15")
			)
			(pin power_out line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "USB_VREGO")
				(number "16")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD_DREG")
				(number "13")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "IOVDD_0")
				(number "2")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "IOVDD_5")
				(number "22")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "AVDD_0")
				(number "12")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "AVDD_2")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PE12")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PE13")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PF0")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PF1")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PF2")
				(number "21")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "DECOUPLE")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFM8BB10F8G-A-QFN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F8G-A-QFN20"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 8K flash, 512B RAM, -40 to +85 C, QFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QFN20"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EFM8BB10F8G-A-QFN20_0_1"
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "RSTb/C2CK")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "P0.0")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "P0.1")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "P0.2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "P0.3")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "P0.4")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "P0.5")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "P0.6")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "P0.7")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "P1.0")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "P1.1")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "P1.2")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "P1.4")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "P1.5")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "P2.0/C2D")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFM8BB10F8G-A-QSOP24"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F8G-A-QSOP24"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_SO:QSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 8K flash, 512B RAM, -40 to +85 C, QSOP24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QSOP24"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "EFM8BB10F8G-A-QSOP24_0_1"
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "RSTb/C2CK")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "P0.0")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "P0.1")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "P0.2")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "P0.3")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "P0.4")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "P0.5")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "P0.6")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "P0.7")
				(number "19")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "6")
			)
			(pin no_connect line
				(at 0 2.54 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 0 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 0 -2.54 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "P1.0")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "P1.1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "P1.2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "P1.4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "P1.5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "P1.6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "P1.7")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "P2.0/C2D")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "P2.1")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFM8BB10F8G-A-SOIC16"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F8G-A-SOIC16"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 8K flash, 512B RAM, -40 to +85 C, SOIC16"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC SOIC16"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "EFM8BB10F8G-A-SOIC16_0_1"
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "RSTb/C2CK")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "P0.0")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "P0.1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "P0.2")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "P0.3")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "P0.4")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "P0.5")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "P0.6")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "P0.7")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "P1.0")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "P1.1")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "P1.2")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "P2.0/C2D")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFM8LB12F32E-C-QFP32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 31.115 0)
		)
		(property "Value" "EFM8LB12F32E-C-QFP32"
			(at -5.08 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 1.27 -29.21 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8lb1-datasheet.pdf"
			(at 0 50.8 0)
		)
		(property "Description" "8051-compatible microcontroller, 72 MHz, 2.2 to 3.6V, 32K flash, 2304B RAM, -40 to +105 C, QFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "EFM8LB12F32E-C-QFP32_0_0"
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "P0.0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "P0.1")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "P0.2")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "P0.3")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "P0.4")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P0.5")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "P0.6")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "P0.7")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "P1.0")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "P1.1")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "P1.3")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P1.4")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P1.5")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "P1.7")
				(number "18")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "~{RST}")
				(number "5")
				(alternate "C2CK" input line)
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VIO")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "P2.0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "P2.1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P2.2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P2.3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P2.4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P2.5")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P2.6")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "P3.0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "P3.1")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P3.2")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P3.3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P3.7")
				(number "6")
				(alternate "C2D" bidirectional line)
			)
		)
		(symbol "EFM8LB12F32E-C-QFP32_0_1")
		(embedded_fonts no)
	)
	(symbol "EFM8UB30F40G-A-QFN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "EFM8UB30F40G-A-QFN20"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8ub3-datasheet.pdf"
			(at -15.24 -2.54 0)
		)
		(property "Description" "8051-compatible microcontroller, 48 MHz, 2.3 to 5.5V, 40K flash, 3.25K RAM, -40 to +85 C, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C USB LDOREG ADC QFN20"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EFM8UB30F40G-A-QFN20_0_1")
		(symbol "EFM8UB30F40G-A-QFN20_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{RST}/C2CK")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P2.0/C2D")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "P2.1/VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D-")
				(number "5")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VREGIN")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P0.0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P0.1")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P0.2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P0.3")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "P0.4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "P0.5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "P0.6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P0.7")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P1.0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "P1.1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P1.2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFM8UB31F40G-A-QFN24"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "EFM8UB31F40G-A-QFN24"
			(at 3.81 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8ub3-datasheet.pdf"
			(at -15.24 2.54 0)
		)
		(property "Description" "8051-compatible microcontroller, 48 MHz, 2.3 to 5.5V, 40K flash, 3.25K RAM, -40 to +85 C, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C USB LDOREG ADC QFN24"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EFM8UB31F40G-A-QFN24_0_1")
		(symbol "EFM8UB31F40G-A-QFN24_1_1"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{RST}/C2CK")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "P2.0/C2D")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P2.1/VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "D-")
				(number "4")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VREGIN")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "P0.0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P0.1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P0.2")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P0.3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P0.4")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P0.5")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "P0.6")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "P0.7")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P1.0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P1.1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "P1.3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P1.4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "P1.5")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P1.6")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFM8UB31F40G-A-QSOP24"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "EFM8UB31F40G-A-QSOP24"
			(at 3.81 24.13 0)
		)
		(property "Footprint" "Package_SO:QSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8ub3-datasheet.pdf"
			(at -15.24 2.54 0)
		)
		(property "Description" "8051-compatible microcontroller, 48 MHz, 2.3 to 5.5V, 40K flash, 3.25K RAM, -40 to +85 C, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C USB LDOREG ADC QSOP24"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "EFM8UB31F40G-A-QSOP24_1_1"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{RST}/C2CK")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "P2.0/C2D")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P2.1/VBUS")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "D+")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "D-")
				(number "6")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VIO")
				(number "7")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VREGIN")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "P0.0")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P0.1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P0.2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P0.3")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P0.4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P0.5")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "P0.6")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "P0.7")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P1.0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P1.1")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P1.2")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P1.4")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "P1.5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P1.6")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EFR32xG23xxxxF512xM48"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 34.29 0)
		)
		(property "Value" "EFR32xG23xxxxF512xM48"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.3x4.3mm"
			(at 2.54 -36.83 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efr32zg23-datasheet.pdf"
			(at 2.54 -39.37 0)
		)
		(property "Description" "ARM M33 SubGHz Radio +20dBm 512K Flash 64KRAM Z-Wave QFN-48"
			(at 1.016 1.27 0)
		)
		(property "Information" "https://drzwave.blog/2022/07/21/z-wave-800-gpio-decoder-ring/"
			(at -0.254 -1.016 0)
		)
		(property "ki_keywords" "Z-Wave ARM MCU CM33 Radio 900MHz SoC Silicon Labs Silabs 32-bit CPU EFR32 EFR32ZG23 EFR32M23 EFR32FG23 EFR32SG23 Sidewalk"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*48*1EP*6x6mm*EP4.3*"
			(at 0 0 0)
		)
		(symbol "EFR32xG23xxxxF512xM48_0_1")
		(symbol "EFR32xG23xxxxF512xM48_1_0"
			(text "EM4WakeUp"
				(at -12.7 16.51 900)
			)
			(text "DEBUG"
				(at -6.35 -15.494 900)
			)
			(text "MCU & SubGHz Radio"
				(at 2.54 13.97 0)
			)
		)
		(symbol "EFR32xG23xxxxF512xM48_1_1"
			(pin passive line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VREGSW")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PB01")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PB03")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PC00")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PC05")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PC07")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PD02")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PA06_TD2")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PA07_TD3")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PD04_PDATA")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PD05_PSYNC")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PA01_SWCLK")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PA02_SWDIO")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PA03_SWO")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PA04_TCLK")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PA05_TD1")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PA08_UTX")
				(number "33")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PA09_URX")
				(number "34")
			)
			(pin input line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin passive line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "DECOUPLE")
				(number "36")
			)
			(pin power_in line
				(at -10.16 35.56 270)
				(length 2.54)
				(name "DVDD")
				(number "40")
			)
			(pin power_in line
				(at -7.62 35.56 270)
				(length 2.54)
				(name "AVDD")
				(number "41")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 2.54)
				(name "IOVDD")
				(number "42")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VREGVSS")
				(number "39")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "RFVDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "RFVSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "PAVDD")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "PAD")
				(number "49")
			)
			(pin power_in line
				(at 7.62 35.56 270)
				(length 2.54)
				(name "VREGVDD")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "SUBG_I0")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "SUBG_I1")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "SUBG_O0")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "SUBG_O1")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA00")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB00")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB02")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PC01")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PC02")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PC03")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PC04")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PC06")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PC08")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PC09")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PD03")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PD00_LFXO")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PD01_LFXI")
				(number "47")
			)
			(pin input line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "HFXTAL_I")
				(number "11")
			)
			(pin output line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "HFXTAL_O")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C8051F320-GQ"
		(extends "C8051F381-GQ")
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F320-GQ"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F32x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "16 KB ISP FLASH MCU Family with Full Speed USB, 2304 bytes internal RAM, 25 port I/O, 10-bit ADC, built-in temperature sensor, fully compatible with MCS-51 instruction set, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART SPI SMbus I2C VREF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F382-GQ"
		(extends "C8051F380-GQ")
		(property "Reference" "U"
			(at -10.16 40.64 0)
		)
		(property "Value" "C8051F382-GQ"
			(at 12.7 40.64 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at -25.4 -38.1 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -12.7 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 32k flash, 2304 ram, 40 IO, EMIF, ADC, Temperature, VREF, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C ADC EMIF TQFP48"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F383-GM"
		(extends "C8051F381-GM")
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F383-GM"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.3x3.3mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 32k flash, 2304 ram, 25 IO, ADC, Temperature, VREF, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C ADC QFN32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F383-GQ"
		(extends "C8051F381-GQ")
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F383-GQ"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 32k flash, 2304 ram, 25 IO, ADC, Temperature, VREF, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C ADC LQFP32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F384-GQ"
		(extends "C8051F380-GQ")
		(property "Reference" "U"
			(at -10.16 40.64 0)
		)
		(property "Value" "C8051F384-GQ"
			(at 12.7 40.64 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at -25.4 -38.1 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -12.7 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 64k flash, 4352 ram, 40 IO, EMIF, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C EMIF TQFP48"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F385-GM"
		(extends "C8051F381-GM")
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F385-GM"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.3x3.3mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 64k flash, 4352 ram, 25 IO, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C QFN32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F385-GQ"
		(extends "C8051F381-GQ")
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F385-GQ"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 64k flash, 4352 ram, 25 IO, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C LQFP32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F386-GQ"
		(extends "C8051F380-GQ")
		(property "Reference" "U"
			(at -10.16 40.64 0)
		)
		(property "Value" "C8051F386-GQ"
			(at 12.7 40.64 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at -25.4 -38.1 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -12.7 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 32k flash, 2304 ram, 40 IO, EMIF, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C EMIF TQFP48"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F387-GM"
		(extends "C8051F381-GM")
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F387-GM"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.3x3.3mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 32k flash, 2304 ram, 25 IO, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C QFN32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F387-GQ"
		(extends "C8051F381-GQ")
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F387-GQ"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 32k flash, 2304 ram, 25 IO, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C LQFP32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F38C-GM"
		(extends "C8051F381-GM")
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F38C-GM"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.3x3.3mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 16k flash, 2304 ram, 25 IO, ADC, Temperature, VREF, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C ADC QFN32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "C8051F38C-GQ"
		(extends "C8051F381-GQ")
		(property "Reference" "U"
			(at -10.16 27.94 0)
		)
		(property "Value" "C8051F38C-GQ"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/C8051F38x.pdf"
			(at -22.86 -25.4 0)
		)
		(property "Description" "Full Speed USB Flash MCU Family, 16k flash, 2304 ram, 25 IO, ADC, Temperature, VREF, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PCA UART USB SPI I2C ADC LQFP32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32HG108F64G-C-QFN24"
		(extends "EFM32HG108F32G-C-QFN24")
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32HG108F64G-C-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32hg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 64 kB flash, 4 kB  RAM, Silicon Labs - Happy Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 happy gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32HG308F64G-C-QFN24"
		(extends "EFM32HG308F32G-C-QFN24")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "EFM32HG308F64G-C-QFN24"
			(at 25.4 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32hg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 64 kB flash, 4 kB  RAM, Silicon Labs - Happy Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 happy gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32ZG108F16-B-QFN24"
		(extends "EFM32HG108F32G-C-QFN24")
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32ZG108F16-B-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32zg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16 kB flash, 4 kB  RAM, Silicon Labs - Zero Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 zero gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32ZG108F32-B-QFN24"
		(extends "EFM32HG108F32G-C-QFN24")
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32ZG108F32-B-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32zg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32 kB flash, 4 kB  RAM, Silicon Labs - Zero Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 zero gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32ZG108F4-B-QFN24"
		(extends "EFM32HG108F32G-C-QFN24")
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32ZG108F4-B-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32zg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 4 kB flash, 2 kB  RAM, Silicon Labs - Zero Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 zero gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32ZG108F8-B-QFN24"
		(extends "EFM32HG108F32G-C-QFN24")
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32ZG108F8-B-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32zg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8 kB flash, 2 kB  RAM, Silicon Labs - Zero Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 zero gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32ZG110F16-B-QFN24"
		(extends "EFM32HG108F32G-C-QFN24")
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32ZG110F16-B-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32zg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16 kB flash, 4 kB  RAM, Silicon Labs - Zero Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 zero gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32ZG110F32-B-QFN24"
		(extends "EFM32HG108F32G-C-QFN24")
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32ZG110F32-B-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32zg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32 kB flash, 4 kB  RAM, Silicon Labs - Zero Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 zero gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32ZG110F4-B-QFN24"
		(extends "EFM32HG108F32G-C-QFN24")
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32ZG110F4-B-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32zg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 4 kB flash, 2 kB  RAM, Silicon Labs - Zero Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 zero gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM32ZG110F8-B-QFN24"
		(extends "EFM32HG108F32G-C-QFN24")
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "EFM32ZG110F8-B-QFN24"
			(at 24.13 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm32zg-datasheet.pdf"
			(at 1.27 -24.13 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8 kB flash, 2 kB  RAM, Silicon Labs - Zero Gecko, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU microcontroller silicon labs siliconlabs silabs EFM32 zero gecko"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F2A-A-QFN20"
		(extends "EFM8BB10F8G-A-QFN20")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F2A-A-QFN20"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 2K flash, 256B RAM, -40 to +125 C (automotive), QFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QFN20 automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F2G-A-QFN20"
		(extends "EFM8BB10F8G-A-QFN20")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F2G-A-QFN20"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 2K flash, 256B RAM, -40 to +85 C, QFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QFN20"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F2I-A-QFN20"
		(extends "EFM8BB10F8G-A-QFN20")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F2I-A-QFN20"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 2K flash, 256B RAM, -40 to +125 C, QFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QFN20"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F4A-A-QFN20"
		(extends "EFM8BB10F8G-A-QFN20")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F4A-A-QFN20"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 4K flash, 512B RAM, -40 to +125 C (automotive), QFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QFN20 automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F4G-A-QFN20"
		(extends "EFM8BB10F8G-A-QFN20")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F4G-A-QFN20"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 4K flash, 512B RAM, -40 to +85 C, QFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QFN20"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F4I-A-QFN20"
		(extends "EFM8BB10F8G-A-QFN20")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F4I-A-QFN20"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 4K flash, 512B RAM, -40 to +125 C, QFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QFN20"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F8A-A-QFN20"
		(extends "EFM8BB10F8G-A-QFN20")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F8A-A-QFN20"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 8K flash, 512B RAM, -40 to +125 C (automotive), QFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QFN20 automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F8I-A-QFN20"
		(extends "EFM8BB10F8G-A-QFN20")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F8I-A-QFN20"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 8K flash, 512B RAM, -40 to +125 C, QFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QFN20"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F8I-A-QSOP24"
		(extends "EFM8BB10F8G-A-QSOP24")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F8I-A-QSOP24"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_SO:QSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 8K flash, 512B RAM, -40 to +125 C, QSOP24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC QSOP24"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8BB10F8I-A-SOIC16"
		(extends "EFM8BB10F8G-A-SOIC16")
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "EFM8BB10F8I-A-SOIC16"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8051-compatible microcontroller, 25 MHz, 2.2 to 3.6V, 8K flash, 512B RAM, -40 to +125 C, SOIC16"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller PWM UART SPI I2C ADC SOIC16"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "EFM8LB12F64E-C-QFP32"
		(extends "EFM8LB12F32E-C-QFP32")
		(property "Reference" "U"
			(at -5.08 31.115 0)
		)
		(property "Value" "EFM8LB12F64E-C-QFP32"
			(at -5.08 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 1.27 -29.21 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/efm8lb1-datasheet.pdf"
			(at 0 50.8 0)
		)
		(property "Description" "8051-compatible microcontroller, 72 MHz, 2.2 to 3.6V, 64K flash, 2304B RAM, -40 to +105 C, QFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "8051 microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
)
