(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "LM3S6911-EQC50"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -36.83 55.88 0)
		)
		(property "Value" "LM3S6911-EQC50"
			(at 25.4 55.88 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 48.26 -58.42 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3s6911.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ti Stellaris ARM-M3 MCU Ethernet PHY, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM M3 Stellaris PHY ETH NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM3S6911-EQC50_0_1")
		(symbol "LM3S6911-EQC50_1_1"
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 3.81)
				(name "PD0")
				(number "10")
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 3.81)
				(name "PD1")
				(number "11")
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 3.81)
				(name "PD2/U1RX")
				(number "12")
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 3.81)
				(name "PD3/U1TX")
				(number "13")
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 3.81)
				(name "PD4")
				(number "95")
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 3.81)
				(name "PD5")
				(number "96")
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 3.81)
				(name "PD6")
				(number "99")
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 3.81)
				(name "PD7/CCP1")
				(number "100")
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 3.81)
				(name "PE0/SSI1CLK")
				(number "72")
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 3.81)
				(name "PE1/SSI1FSS")
				(number "73")
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 3.81)
				(name "PE2/SSI1RX")
				(number "74")
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 3.81)
				(name "PE3/SSI1TX")
				(number "75")
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 3.81)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 3.81)
				(name "PE5")
				(number "5")
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 3.81)
				(name "PE6/C1O")
				(number "2")
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 3.81)
				(name "PE7")
				(number "1")
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 3.81)
				(name "PF0")
				(number "47")
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 3.81)
				(name "PF1")
				(number "61")
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 3.81)
				(name "PF2/LED1")
				(number "60")
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 3.81)
				(name "PF3/LED0")
				(number "59")
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 3.81)
				(name "PG0/U2RX")
				(number "19")
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 3.81)
				(name "PG1/U2TX")
				(number "18")
			)
			(pin input line
				(at -40.64 -15.24 0)
				(length 3.81)
				(name "~{RST}")
				(number "64")
			)
			(pin input line
				(at -40.64 -20.32 0)
				(length 3.81)
				(name "CMOD0")
				(number "65")
			)
			(pin input line
				(at -40.64 -22.86 0)
				(length 3.81)
				(name "CMOD1")
				(number "76")
			)
			(pin passive line
				(at -40.64 -27.94 0)
				(length 3.81)
				(name "VBAT")
				(number "55")
			)
			(pin input line
				(at -40.64 -30.48 0)
				(length 3.81)
				(name "~{WAKE}")
				(number "50")
			)
			(pin open_collector line
				(at -40.64 -33.02 0)
				(length 3.81)
				(name "~{HIB}")
				(number "51")
			)
			(pin passive line
				(at -40.64 -38.1 0)
				(length 3.81)
				(name "XOSC0")
				(number "52")
			)
			(pin passive line
				(at -40.64 -40.64 0)
				(length 3.81)
				(name "XOSC1")
				(number "53")
			)
			(pin passive line
				(at -40.64 -45.72 0)
				(length 3.81)
				(name "OSC0")
				(number "48")
			)
			(pin passive line
				(at -40.64 -50.8 0)
				(length 3.81)
				(name "OSC1")
				(number "49")
			)
			(pin passive line
				(at -27.94 58.42 270)
				(length 3.81)
				(name "LDO")
				(number "7")
			)
			(pin power_in line
				(at -22.86 58.42 270)
				(length 3.81)
				(name "VDD25")
				(number "14")
			)
			(pin power_in line
				(at -22.86 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -20.32 58.42 270)
				(length 3.81)
				(name "VDD25")
				(number "38")
			)
			(pin power_in line
				(at -20.32 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at -17.78 58.42 270)
				(length 3.81)
				(name "VDD25")
				(number "62")
			)
			(pin power_in line
				(at -17.78 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at -15.24 58.42 270)
				(length 3.81)
				(name "VDD25")
				(number "88")
			)
			(pin power_in line
				(at -15.24 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at -12.7 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at -10.16 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -7.62 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "54")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at -5.08 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 3.81)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 3.81)
				(name "VDD")
				(number "56")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 3.81)
				(name "VDD")
				(number "68")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "82")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 3.81)
				(name "VDD")
				(number "81")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "87")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 3.81)
				(name "VDD")
				(number "93")
			)
			(pin power_in line
				(at 7.62 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "94")
			)
			(pin power_in line
				(at 10.16 58.42 270)
				(length 3.81)
				(name "VDDA")
				(number "98")
			)
			(pin power_in line
				(at 10.16 -58.42 90)
				(length 3.81)
				(name "GNDA")
				(number "4")
			)
			(pin power_in line
				(at 12.7 58.42 270)
				(length 3.81)
				(name "VDDA")
				(number "3")
			)
			(pin power_in line
				(at 12.7 -58.42 90)
				(length 3.81)
				(name "GNDA")
				(number "97")
			)
			(pin power_in line
				(at 17.78 58.42 270)
				(length 3.81)
				(name "VCCPHY")
				(number "84")
			)
			(pin power_in line
				(at 17.78 -58.42 90)
				(length 3.81)
				(name "GNDPHY")
				(number "42")
			)
			(pin power_in line
				(at 20.32 58.42 270)
				(length 3.81)
				(name "VCCPHY")
				(number "83")
			)
			(pin power_in line
				(at 20.32 -58.42 90)
				(length 3.81)
				(name "GNDPHY")
				(number "85")
			)
			(pin power_in line
				(at 22.86 58.42 270)
				(length 3.81)
				(name "VCCPHY")
				(number "36")
			)
			(pin power_in line
				(at 22.86 -58.42 90)
				(length 3.81)
				(name "GNDPHY")
				(number "86")
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 3.81)
				(name "U0RX/PA0")
				(number "26")
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 3.81)
				(name "U0TX/PA1")
				(number "27")
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 3.81)
				(name "SSI0CLK/PA2")
				(number "28")
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 3.81)
				(name "SSI0FSS/PA3")
				(number "29")
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 3.81)
				(name "SSI0RX/PA4")
				(number "30")
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 3.81)
				(name "SSI0TX/PA5")
				(number "31")
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 3.81)
				(name "I2C1SCL/PA6")
				(number "34")
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 3.81)
				(name "I2C1SDA/PA7")
				(number "35")
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 3.81)
				(name "CCP0/PB0")
				(number "66")
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 3.81)
				(name "CCP2/PB1")
				(number "67")
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 3.81)
				(name "I2C0SCL/PB2")
				(number "70")
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 3.81)
				(name "I2C0SDA/PB3")
				(number "71")
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 3.81)
				(name "C0-/PB4")
				(number "92")
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 3.81)
				(name "C1-/PB5")
				(number "91")
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 3.81)
				(name "C0+/PB6")
				(number "90")
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 3.81)
				(name "~{TRST}/PB7")
				(number "89")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 3.81)
				(name "SWCLK/TCK/PC0")
				(number "80")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 3.81)
				(name "SWDIO/TMS/PC1")
				(number "79")
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 3.81)
				(name "TDI/PC2")
				(number "78")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 3.81)
				(name "SWO/TDO/PC3")
				(number "77")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 3.81)
				(name "CCP5/PC4")
				(number "25")
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 3.81)
				(name "C1+/C0O/PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 3.81)
				(name "CCP3/PC6")
				(number "23")
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 3.81)
				(name "CCP4/PC7")
				(number "22")
			)
			(pin passive line
				(at 40.64 -17.78 180)
				(length 3.81)
				(name "TXOP")
				(number "43")
			)
			(pin passive line
				(at 40.64 -20.32 180)
				(length 3.81)
				(name "TXON")
				(number "46")
			)
			(pin passive line
				(at 40.64 -25.4 180)
				(length 3.81)
				(name "ERBIAS")
				(number "41")
			)
			(pin passive line
				(at 40.64 -30.48 180)
				(length 3.81)
				(name "RXIP")
				(number "40")
			)
			(pin passive line
				(at 40.64 -33.02 180)
				(length 3.81)
				(name "RXIN")
				(number "37")
			)
			(pin input line
				(at 40.64 -38.1 180)
				(length 3.81)
				(name "MDIO")
				(number "58")
			)
			(pin passive line
				(at 40.64 -45.72 180)
				(length 3.81)
				(name "XTALPPHY")
				(number "16")
			)
			(pin passive line
				(at 40.64 -50.8 180)
				(length 3.81)
				(name "XTALNPHY")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP432E401Y"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "MSP432E401Y"
			(at 25.4 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at 53.34 -91.44 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp432e401y.pdf"
			(at -17.78 -45.72 0)
		)
		(property "Description" "ARM Cortex-M4F MCU, 1024KB flash, 256KB RAM, 6KB EEPROM, 120MHz, 3.0-3.6V, TQFP-128"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Cortex-M4F MSP432 MSP432E4 MSP432E401"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MSP432E401Y_1_1"
			(pin input line
				(at -33.02 81.28 0)
				(length 5.08)
				(name "~{RST}")
				(number "70")
			)
			(pin output line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "~{HIB}")
				(number "65")
			)
			(pin input line
				(at -33.02 76.2 0)
				(length 5.08)
				(name "~{WAKE}")
				(number "64")
			)
			(pin input line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "OSC0")
				(number "88")
			)
			(pin output line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "OSC1")
				(number "89")
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "XOSC0")
				(number "66")
			)
			(pin output line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "XOSC1")
				(number "67")
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PL0")
				(number "81")
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PL1")
				(number "82")
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PL2")
				(number "83")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PL3")
				(number "84")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PL4")
				(number "85")
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PL5")
				(number "86")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PL6")
				(number "94")
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PL7")
				(number "93")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PM0")
				(number "78")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PM1")
				(number "77")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PM2")
				(number "76")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PM3")
				(number "75")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PM4")
				(number "74")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PM5")
				(number "73")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PM6")
				(number "72")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PM7")
				(number "71")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PN0")
				(number "107")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PN1")
				(number "108")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PN2")
				(number "109")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PN3")
				(number "110")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PN4")
				(number "111")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PN5")
				(number "112")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PP0")
				(number "118")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PP1")
				(number "119")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PP2")
				(number "103")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PP3")
				(number "104")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PP4")
				(number "105")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PP5")
				(number "106")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PQ0")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PQ1")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PQ2")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PQ3")
				(number "27")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PQ4")
				(number "102")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "EN0RXIN")
				(number "53")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "EN0RXIP")
				(number "54")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "EN0TXON")
				(number "56")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "EN0TXOP")
				(number "57")
			)
			(pin passive line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "RBIAS")
				(number "59")
			)
			(pin power_in line
				(at -25.4 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -22.86 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -20.32 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at -17.78 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "47")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "69")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "79")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "114")
			)
			(pin power_in line
				(at -2.54 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "58")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "90")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "101")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "GNDA")
				(number "10")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "113")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "122")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VREFA+")
				(number "9")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "68")
			)
			(pin power_in line
				(at 20.32 93.98 270)
				(length 5.08)
				(name "VDDC")
				(number "115")
			)
			(pin power_in line
				(at 22.86 93.98 270)
				(length 5.08)
				(name "VDDC")
				(number "87")
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "36")
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "37")
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "40")
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "41")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PB0")
				(number "95")
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PB1")
				(number "96")
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PB2")
				(number "91")
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PB3")
				(number "92")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PB4")
				(number "121")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PB5")
				(number "120")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PC0/TCK/SWCLK")
				(number "100")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PC1/TMS/SWDIO")
				(number "99")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PC2/TDI")
				(number "98")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PC3/TDO/SWO")
				(number "97")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PC4")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PC6")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PC7")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PD0")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PD1")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PD2")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PD3")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PD4")
				(number "125")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PD5")
				(number "126")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PD6")
				(number "127")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PD7")
				(number "128")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PE0")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PE1")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PE2")
				(number "13")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PE3")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PE4")
				(number "123")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PE5")
				(number "124")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PF0")
				(number "42")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PF1")
				(number "43")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PF2")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PF3")
				(number "45")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PF4")
				(number "46")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PG0")
				(number "49")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PG1")
				(number "50")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PH0")
				(number "29")
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PH1")
				(number "30")
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PH2")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PH3")
				(number "32")
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PJ0")
				(number "116")
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PJ1")
				(number "117")
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PK0")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PK1")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PK2")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PK3")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PK4")
				(number "63")
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PK5")
				(number "62")
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PK6")
				(number "61")
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PK7")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TM4C1230C3PM"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -31.75 48.26 0)
		)
		(property "Value" "TM4C1230C3PM"
			(at 16.51 48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 31.75 -50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1230c3pm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Tiva ARM 32bit CortexM4 Microcotroller, 80MHz, 32kB Flash, 12kB SRAM, 2k EEPROM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Tiva Cortex M4 MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TM4C1230C3PM_0_1")
		(symbol "TM4C1230C3PM_1_1"
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 3.81)
				(name "PE0/AIN3/U7RX")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 3.81)
				(name "PE1/AIN2/U7TX")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 3.81)
				(name "PE2/AIN1")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 3.81)
				(name "PE3/AIN0")
				(number "6")
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 3.81)
				(name "PE4/AIN9/U5RX/I2C2SCL/CAN0RX")
				(number "59")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 3.81)
				(name "PE5/AIN8/U5TX/I2C2SDA/CAN0TX")
				(number "60")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 3.81)
				(name "PF0/T0CCP0/SSI1RX/U1RTS/CAN0RX/C0O/NMI")
				(number "28")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 3.81)
				(name "PF1/T0CCP1/SSI1TX/U1CTS/C1O/TRD1")
				(number "29")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 3.81)
				(name "PF2/T1CCP0/SSI1CLK/TRD0")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 3.81)
				(name "PF3/T1CCP1/SSI1FSS/CAN0TX/TRCLK")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 3.81)
				(name "PF4/T2CCP0")
				(number "5")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 3.81)
				(name "PG0/T4CCP0/I2C3SCL")
				(number "37")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 3.81)
				(name "PG1/T4CCP1/I2C3SDA")
				(number "36")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 3.81)
				(name "PG2/T5CCP0/I2C4SCL")
				(number "35")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 3.81)
				(name "PG3/T5CCP1/I2C4SDA")
				(number "34")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 3.81)
				(name "PG4/WT0CCP0/U2RX/I2C1SCL")
				(number "33")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 3.81)
				(name "PG5/WT0CCP1/U2TX/I2C1SDA")
				(number "32")
			)
			(pin input line
				(at -35.56 -10.16 0)
				(length 3.81)
				(name "~{RST}")
				(number "38")
			)
			(pin passive line
				(at -35.56 -20.32 0)
				(length 3.81)
				(name "OSC0")
				(number "40")
			)
			(pin passive line
				(at -35.56 -25.4 0)
				(length 3.81)
				(name "OSC1")
				(number "41")
			)
			(pin power_in line
				(at -12.7 50.8 270)
				(length 3.81)
				(name "VDDC")
				(number "25")
			)
			(pin power_in line
				(at -10.16 50.8 270)
				(length 3.81)
				(name "VDDC")
				(number "56")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "42")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "55")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "54")
			)
			(pin power_in line
				(at 5.08 -50.8 90)
				(length 3.81)
				(name "GNDA")
				(number "3")
			)
			(pin power_in line
				(at 7.62 50.8 270)
				(length 3.81)
				(name "VDDA")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 3.81)
				(name "U0RX/PA0")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 3.81)
				(name "U0TX/PA1")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 3.81)
				(name "SSI0CLK/PA2")
				(number "19")
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 3.81)
				(name "SSI0FSS/PA3")
				(number "20")
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 3.81)
				(name "SSI0RX/PA4")
				(number "21")
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 3.81)
				(name "SSI0TX/PA5")
				(number "22")
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 3.81)
				(name "I2C1SCL/PA6")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 3.81)
				(name "I2C1SDA/PA7")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 3.81)
				(name "U1RX/T2CCP0/PB0")
				(number "45")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "U1TX/T2CCP1/PB1")
				(number "46")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "I2C0SCL/T3CCP0/PB2")
				(number "47")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "I2C0SDA/T3CCP1/PB3")
				(number "48")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "AIN10/CAN0RX/SSI2CLK/T1CCP0/PB4")
				(number "58")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "AIN11/CAN0TX/SSI2FSS/T1CCP1/PB5")
				(number "57")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "I2C5SCL/SSI2RX/T0CCP0/PB6")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "I2C5SDA/SSI2TX/T0CCP1/PB7")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 3.81)
				(name "TCK/SWCLK/T4CCP0/PC0")
				(number "52")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 3.81)
				(name "TMS/SWDIO/T4CCP1/PC1")
				(number "51")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 3.81)
				(name "TDI/T5CCP0/PC2")
				(number "50")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 3.81)
				(name "TDO/SWO/T5CCP1/PC3")
				(number "49")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 3.81)
				(name "C1-/U1RTS/U1RX/U4RX/WT0CCP0/PC4")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 3.81)
				(name "C1+/U1CTS/U1TX/U4TX/WT0CCP1/PC5")
				(number "15")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 3.81)
				(name "C0+/U3RX/WT1CCP0/PC6")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 3.81)
				(name "C0-/U3TX/WT1CCP1/PC7")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 3.81)
				(name "AIN7/I2C3SCL/SSI1CLK/SSI3CLK/WT2CCP0/PD0")
				(number "61")
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 3.81)
				(name "AIN6/I2C3SDA/SSI1FSS/SSI3FSS/WT2CCP1/PD1")
				(number "62")
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 3.81)
				(name "AIN5/SSI1RX/SSI3RX/WT3CCP0/PD2")
				(number "63")
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 3.81)
				(name "AIN4/SSI1TX/SSI3TX/WT3CCP1/PD3")
				(number "64")
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 3.81)
				(name "U6RX/WT4CCP0/PD4")
				(number "43")
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 3.81)
				(name "U6TX/WT4CCP1/PD5")
				(number "44")
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 3.81)
				(name "U2RX/WT5CCP0/PD6")
				(number "53")
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 3.81)
				(name "NMI/U2TX/WT5CCP1/PD7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TM4C1231C3PM"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -31.75 50.8 0)
		)
		(property "Value" "TM4C1231C3PM"
			(at 16.51 50.8 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 30.48 -53.34 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1231c3pm.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Tiva ARM 32bit CortexM4 Microcotroller, 80MHz, 32kB Flash, 12kB SRAM, 2k EEPROM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Tiva Cortex M4 MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5*"
			(at 0 0 0)
		)
		(symbol "TM4C1231C3PM_0_1")
		(symbol "TM4C1231C3PM_1_1"
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 3.81)
				(name "PE0/AIN3/U7RX")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 3.81)
				(name "PE1/AIN2/U7TX")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 3.81)
				(name "PE2/AIN1")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 3.81)
				(name "PE3/AIN0")
				(number "6")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 3.81)
				(name "PE4/AIN9/U5RX/I2C2SCL/CAN0RX")
				(number "59")
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 3.81)
				(name "PE5/AIN8/U5TX/I2C2SDA/CAN0TX")
				(number "60")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 3.81)
				(name "PF0/T0CCP0/SSI1RX/U1RTS/CAN0RX/C0O/MNI")
				(number "28")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 3.81)
				(name "PF1/T0CCP1/SSI1TX/U1CTS/C1O/TRD1")
				(number "29")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 3.81)
				(name "PF2/T1CCP0/SSI1CLK/TRD0")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 3.81)
				(name "PF3/T1CCP1/SSI1FSS/CAN0TX/TRCLK")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 3.81)
				(name "PF4/T2CCP0")
				(number "5")
			)
			(pin input line
				(at -35.56 10.16 0)
				(length 3.81)
				(name "~{RST}")
				(number "38")
			)
			(pin passive line
				(at -35.56 2.54 0)
				(length 3.81)
				(name "OSC0")
				(number "40")
			)
			(pin passive line
				(at -35.56 -2.54 0)
				(length 3.81)
				(name "OSC1")
				(number "41")
			)
			(pin input line
				(at -35.56 -10.16 0)
				(length 3.81)
				(name "~{WAKE}")
				(number "32")
			)
			(pin open_collector line
				(at -35.56 -12.7 0)
				(length 3.81)
				(name "~{HIB}")
				(number "33")
			)
			(pin passive line
				(at -35.56 -20.32 0)
				(length 3.81)
				(name "XOSC0")
				(number "34")
			)
			(pin passive line
				(at -35.56 -25.4 0)
				(length 3.81)
				(name "XOSC1")
				(number "36")
			)
			(pin passive line
				(at -35.56 -33.02 0)
				(length 3.81)
				(name "VBAT")
				(number "37")
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 3.81)
				(name "VDDC")
				(number "25")
			)
			(pin power_in line
				(at -10.16 -53.34 90)
				(length 3.81)
				(name "GNDX")
				(number "35")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 3.81)
				(name "VDDC")
				(number "56")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin bidirectional line
				(at 0 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 3.81)
				(name "VDD")
				(number "42")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "55")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 3.81)
				(name "VDD")
				(number "54")
			)
			(pin power_in line
				(at 7.62 -53.34 90)
				(length 3.81)
				(name "GNDA")
				(number "3")
			)
			(pin power_in line
				(at 10.16 53.34 270)
				(length 3.81)
				(name "VDDA")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 3.81)
				(name "U0RX/PA0")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 3.81)
				(name "U0TX/PA1")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 3.81)
				(name "SSI0CLK/PA2")
				(number "19")
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 3.81)
				(name "SSI0FSS/PA3")
				(number "20")
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 3.81)
				(name "SSI0RX/PA4")
				(number "21")
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 3.81)
				(name "SSI0TX/PA5")
				(number "22")
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 3.81)
				(name "I2C1SCL/PA6")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 3.81)
				(name "I2C1SDA/PA7")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 3.81)
				(name "U1RX/T2CCP0/PB0")
				(number "45")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 3.81)
				(name "U1TX/T2CCP1/PB1")
				(number "46")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "I2C0SCL/T3CCP0/PB2")
				(number "47")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "I2C0SDA/T3CCP1/PB3")
				(number "48")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "AIN10/CAN0RX/SSI2CLK/T1CCP0/PB4")
				(number "58")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "AIN11/CAN0TX/SSI2FSS/T1CCP1/PB5")
				(number "57")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "SSI2RX/T0CCP0/PB6")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "SSI2TX/T0CCP1/PB7")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 3.81)
				(name "TCK/SWCLK/T4CCP0/PC0")
				(number "52")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 3.81)
				(name "TMS/SWDIO/T4CCP1/PC1")
				(number "51")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 3.81)
				(name "TDI/T5CCP0/PC2")
				(number "50")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 3.81)
				(name "TDO/SWO/T5CCP1/PC3")
				(number "49")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 3.81)
				(name "C1-/U1RTS/U1RX/U4RX/WT0CCP0/PC4")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 3.81)
				(name "C1+/U1CTS/U1TX/U4TX/WT0CCP1/PC5")
				(number "15")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 3.81)
				(name "C0+/U3RX/WT1CCP0/PC6")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 3.81)
				(name "C0-/U3TX/WT1CCP1/PC7")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 3.81)
				(name "AIN7/I2C3SCL/SSI1CLK/SSI3CLK/WT2CCP0/PD0")
				(number "61")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 3.81)
				(name "AIN6/I2C3SDA/SSI1FSS/SSI3FSS/WT2CCP1/PD1")
				(number "62")
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 3.81)
				(name "AIN5/SSI1RX/SSI3RX/WT3CCP0/PD2")
				(number "63")
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 3.81)
				(name "AIN4/SSI1TX/SSI3TX/WT3CCP1/PD3")
				(number "64")
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 3.81)
				(name "U6RX/WT4CCP0/PD4")
				(number "43")
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 3.81)
				(name "U6TX/WT4CCP1/PD5")
				(number "44")
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 3.81)
				(name "U2RX/WT5CCP0/PD6")
				(number "53")
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 3.81)
				(name "NMI/U2TX/WT5CCP1/PD7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMS320LF2406"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 26.67 -60.96 0)
		)
		(property "Value" "TMS320LF2406"
			(at 26.67 60.96 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TMS320LF2406_0_1"
			(text "ANALOG"
				(at -21.59 34.29 0)
			)
			(text "COMMUNICATIONS"
				(at -10.16 -2.54 0)
			)
			(text "EVENT"
				(at 10.16 34.29 0)
			)
			(text "EVENT"
				(at 10.16 -2.54 0)
			)
			(pin input line
				(at -48.26 53.34 0)
				(length 7.62)
				(name "ADCIN1")
				(number "77")
			)
		)
		(symbol "TMS320LF2406_1_1"
			(pin input line
				(at -48.26 55.88 0)
				(length 7.62)
				(name "ADCIN0")
				(number "79")
			)
			(pin input line
				(at -48.26 50.8 0)
				(length 7.62)
				(name "ADCIN2")
				(number "74")
			)
			(pin input line
				(at -48.26 48.26 0)
				(length 7.62)
				(name "ADCIN3")
				(number "72")
			)
			(pin input line
				(at -48.26 45.72 0)
				(length 7.62)
				(name "ADCIN4")
				(number "72")
			)
			(pin input line
				(at -48.26 43.18 0)
				(length 7.62)
				(name "ADCIN5")
				(number "69")
			)
			(pin input line
				(at -48.26 40.64 0)
				(length 7.62)
				(name "ADCIN6")
				(number "67")
			)
			(pin input line
				(at -48.26 38.1 0)
				(length 7.62)
				(name "ADCIN7")
				(number "66")
			)
			(pin input line
				(at -48.26 35.56 0)
				(length 7.62)
				(name "ADCIN8")
				(number "80")
			)
			(pin input line
				(at -48.26 33.02 0)
				(length 7.62)
				(name "ADCIN9")
				(number "78")
			)
			(pin input line
				(at -48.26 30.48 0)
				(length 7.62)
				(name "ADCIN10")
				(number "76")
			)
			(pin input line
				(at -48.26 27.94 0)
				(length 7.62)
				(name "ADCIN11")
				(number "75")
			)
			(pin input line
				(at -48.26 25.4 0)
				(length 7.62)
				(name "ADCIN12")
				(number "73")
			)
			(pin input line
				(at -48.26 22.86 0)
				(length 7.62)
				(name "ADCIN13")
				(number "71")
			)
			(pin input line
				(at -48.26 20.32 0)
				(length 7.62)
				(name "ADCIN14")
				(number "68")
			)
			(pin input line
				(at -48.26 17.78 0)
				(length 7.62)
				(name "ADCIN15")
				(number "65")
			)
			(pin input line
				(at -48.26 12.7 0)
				(length 7.62)
				(name "VREFHI")
				(number "82")
			)
			(pin input line
				(at -48.26 10.16 0)
				(length 7.62)
				(name "VREFLO")
				(number "81")
			)
			(pin bidirectional line
				(at -48.26 5.08 0)
				(length 7.62)
				(name "CANRX/IOPC7")
				(number "49")
			)
			(pin bidirectional line
				(at -48.26 2.54 0)
				(length 7.62)
				(name "CANTX/IOPC6")
				(number "50")
			)
			(pin bidirectional line
				(at -48.26 -1.27 0)
				(length 7.62)
				(name "SCITxD/IOPA0")
				(number "17")
			)
			(pin bidirectional line
				(at -48.26 -3.81 0)
				(length 7.62)
				(name "SCIRxD/IOPA1")
				(number "18")
			)
			(pin bidirectional line
				(at -48.26 -7.62 0)
				(length 7.62)
				(name "SPICLK/IOPC4")
				(number "24")
			)
			(pin bidirectional line
				(at -48.26 -10.16 0)
				(length 7.62)
				(name "SPISIMO/IOPC2")
				(number "21")
			)
			(pin bidirectional line
				(at -48.26 -12.7 0)
				(length 7.62)
				(name "SPISOMI/IOPC3")
				(number "22")
			)
			(pin bidirectional line
				(at -48.26 -15.24 0)
				(length 7.62)
				(name "SPISTE*/IOPC5")
				(number "23")
			)
			(pin input inverted
				(at -48.26 -20.32 0)
				(length 7.62)
				(name "RESET")
				(number "93")
			)
			(pin input inverted
				(at -48.26 -22.86 0)
				(length 7.62)
				(name "PDPINTA")
				(number "6")
			)
			(pin input inverted
				(at -48.26 -25.4 0)
				(length 7.62)
				(name "PDPINTB")
				(number "95")
			)
			(pin bidirectional line
				(at -48.26 -29.21 0)
				(length 7.62)
				(name "XINT1/IOPA2")
				(number "16")
			)
			(pin bidirectional line
				(at -48.26 -31.75 0)
				(length 7.62)
				(name "XINT2/ADSOC/IOPD0")
				(number "15")
			)
			(pin bidirectional line
				(at -48.26 -35.56 0)
				(length 7.62)
				(name "CLKOUT/IOPE0")
				(number "51")
			)
			(pin input line
				(at -48.26 -40.64 0)
				(length 7.62)
				(name "XTAL1/CLKIN")
				(number "87")
			)
			(pin output line
				(at -48.26 -43.18 0)
				(length 7.62)
				(name "XTAL2")
				(number "88")
			)
			(pin input line
				(at -48.26 -46.99 0)
				(length 7.62)
				(name "BOOT_EN*/XF")
				(number "0")
			)
			(pin input line
				(at -48.26 -50.8 0)
				(length 7.62)
				(name "PLLF")
				(number "9")
			)
			(pin input line
				(at -48.26 -53.34 0)
				(length 7.62)
				(name "PLLF2")
				(number "8")
			)
			(pin input line
				(at -48.26 -57.15 0)
				(length 7.62)
				(name "VprogFLASH")
				(number "40")
			)
			(pin power_in line
				(at -27.94 62.23 270)
				(length 3.81)
				(name "VCCA")
				(number "83")
			)
			(pin power_in line
				(at -22.86 62.23 270)
				(length 3.81)
				(name "PLLVCCA")
				(number "10")
			)
			(pin power_in line
				(at -21.59 -63.5 90)
				(length 3.81)
				(name "GNDA")
				(number "84")
			)
			(pin power_in line
				(at -15.24 62.23 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -12.7 62.23 270)
				(length 3.81)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -12.7 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at -10.16 62.23 270)
				(length 3.81)
				(name "VDD")
				(number "59")
			)
			(pin power_in line
				(at -10.16 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "34")
			)
			(pin power_in line
				(at -7.62 62.23 270)
				(length 3.81)
				(name "VDD")
				(number "91")
			)
			(pin power_in line
				(at -7.62 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "58")
			)
			(pin power_in line
				(at -5.08 62.23 270)
				(length 3.81)
				(name "VDDO")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "90")
			)
			(pin power_in line
				(at -2.54 62.23 270)
				(length 3.81)
				(name "VDDO")
				(number "30")
			)
			(pin power_in line
				(at -2.54 -63.5 90)
				(length 3.81)
				(name "GNDO")
				(number "3")
			)
			(pin power_in line
				(at 0 62.23 270)
				(length 3.81)
				(name "VDDO")
				(number "54")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 3.81)
				(name "GNDO")
				(number "29")
			)
			(pin power_in line
				(at 2.54 62.23 270)
				(length 3.81)
				(name "VDDO")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 3.81)
				(name "GNDO")
				(number "46")
			)
			(pin power_in line
				(at 5.08 62.23 270)
				(length 3.81)
				(name "VDDO")
				(number "98")
			)
			(pin power_in line
				(at 5.08 -63.5 90)
				(length 3.81)
				(name "GNDO")
				(number "53")
			)
			(pin power_in line
				(at 7.62 -63.5 90)
				(length 3.81)
				(name "GNDO")
				(number "63")
			)
			(pin power_in line
				(at 10.16 -63.5 90)
				(length 3.81)
				(name "GNDO")
				(number "97")
			)
			(pin input line
				(at 45.72 -44.45 180)
				(length 5.08)
				(name "TMS2")
				(number "25")
			)
			(pin bidirectional line
				(at 48.26 55.88 180)
				(length 7.62)
				(name "CAP1/QEP1/IOPA3")
				(number "57")
			)
			(pin bidirectional line
				(at 48.26 53.34 180)
				(length 7.62)
				(name "CAP2/QEP2/IOPA4")
				(number "55")
			)
			(pin bidirectional line
				(at 48.26 50.8 180)
				(length 7.62)
				(name "CAP3/QEP3/IOPA5")
				(number "52")
			)
			(pin bidirectional line
				(at 48.26 46.99 180)
				(length 7.62)
				(name "PWM1/IOPA6")
				(number "39")
			)
			(pin bidirectional line
				(at 48.26 44.45 180)
				(length 7.62)
				(name "PWM2/IOPA7")
				(number "37")
			)
			(pin bidirectional line
				(at 48.26 41.91 180)
				(length 7.62)
				(name "PWM3/IOPB0")
				(number "36")
			)
			(pin bidirectional line
				(at 48.26 39.37 180)
				(length 7.62)
				(name "PWM4/IOPB1")
				(number "33")
			)
			(pin bidirectional line
				(at 48.26 36.83 180)
				(length 7.62)
				(name "PWM5/IOPB2")
				(number "31")
			)
			(pin bidirectional line
				(at 48.26 34.29 180)
				(length 7.62)
				(name "PWM6/IOPB3")
				(number "28")
			)
			(pin bidirectional line
				(at 48.26 31.75 180)
				(length 7.62)
				(name "T1PWM/T1CMP/IOPB4")
				(number "12")
			)
			(pin bidirectional line
				(at 48.26 29.21 180)
				(length 7.62)
				(name "T2PWM/T2CMP/IOPB5")
				(number "13")
			)
			(pin bidirectional line
				(at 48.26 25.4 180)
				(length 7.62)
				(name "TDIRA/IOPB6")
				(number "11")
			)
			(pin bidirectional line
				(at 48.26 22.86 180)
				(length 7.62)
				(name "TCLKINA/IOPB7")
				(number "26")
			)
			(pin bidirectional line
				(at 48.26 17.78 180)
				(length 7.62)
				(name "CAP4/QEP3/IOPE7")
				(number "60")
			)
			(pin bidirectional line
				(at 48.26 15.24 180)
				(length 7.62)
				(name "CAP5/QEP4/IOPF0")
				(number "56")
			)
			(pin bidirectional line
				(at 48.26 12.7 180)
				(length 7.62)
				(name "CAP6/IOPF1")
				(number "48")
			)
			(pin bidirectional line
				(at 48.26 8.89 180)
				(length 7.62)
				(name "PWM7/IOPE1")
				(number "45")
			)
			(pin bidirectional line
				(at 48.26 6.35 180)
				(length 7.62)
				(name "PWM8/IOPE2")
				(number "43")
			)
			(pin bidirectional line
				(at 48.26 3.81 180)
				(length 7.62)
				(name "PWM9/IOPE3")
				(number "41")
			)
			(pin bidirectional line
				(at 48.26 1.27 180)
				(length 7.62)
				(name "PWM10/IOPE4")
				(number "38")
			)
			(pin bidirectional line
				(at 48.26 -1.27 180)
				(length 7.62)
				(name "PWM11/IOPE5")
				(number "32")
			)
			(pin bidirectional line
				(at 48.26 -3.81 180)
				(length 7.62)
				(name "PWM12/IOPE6")
				(number "27")
			)
			(pin bidirectional line
				(at 48.26 -6.35 180)
				(length 7.62)
				(name "T3PWM/T3CMP/IOPF2")
				(number "7")
			)
			(pin bidirectional line
				(at 48.26 -8.89 180)
				(length 7.62)
				(name "T4PWM/T4CMP/IOPF3")
				(number "5")
			)
			(pin bidirectional line
				(at 48.26 -12.7 180)
				(length 7.62)
				(name "TDIRB/IOPF4")
				(number "2")
			)
			(pin bidirectional line
				(at 48.26 -15.24 180)
				(length 7.62)
				(name "TCKINB/IOPF5")
				(number "89")
			)
			(pin bidirectional line
				(at 48.26 -17.78 180)
				(length 7.62)
				(name "IOPF6")
				(number "92")
			)
			(pin bidirectional line
				(at 48.26 -21.59 180)
				(length 7.62)
				(name "IOPC0")
				(number "14")
			)
			(pin bidirectional line
				(at 48.26 -24.13 180)
				(length 7.62)
				(name "BIO*/IOPC1")
				(number "85")
			)
			(pin bidirectional line
				(at 48.26 -30.48 180)
				(length 7.62)
				(name "TCK")
				(number "94")
			)
			(pin input line
				(at 48.26 -33.02 180)
				(length 7.62)
				(name "TDI")
				(number "96")
			)
			(pin output line
				(at 48.26 -35.56 180)
				(length 7.62)
				(name "TDO")
				(number "99")
			)
			(pin input line
				(at 48.26 -38.1 180)
				(length 7.62)
				(name "TMS")
				(number "100")
			)
			(pin input inverted
				(at 48.26 -40.64 180)
				(length 7.62)
				(name "TRST")
				(number "1")
			)
			(pin bidirectional line
				(at 48.26 -50.8 180)
				(length 7.62)
				(name "EMU0")
				(number "61")
			)
			(pin bidirectional line
				(at 48.26 -53.34 180)
				(length 7.62)
				(name "EMU1/OFF*")
				(number "62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMS470R1B768"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -34.29 93.98 0)
		)
		(property "Value" "TMS470R1B768"
			(at 20.32 93.98 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tms470r1b768.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "ARM7TDM Microcontroller, 768KB Flash, 48KB RAM, PQFP-144"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM 7TDM uC TMS470"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFP-144*"
			(at 0 0 0)
		)
		(symbol "TMS470R1B768_0_1")
		(symbol "TMS470R1B768_1_1"
			(pin input inverted
				(at -38.1 88.9 0)
				(length 3.81)
				(name "~{RST}")
				(number "15")
			)
			(pin input inverted
				(at -38.1 86.36 0)
				(length 3.81)
				(name "~{PORST}")
				(number "32")
			)
			(pin input inverted
				(at -38.1 83.82 0)
				(length 3.81)
				(name "~{TRST}")
				(number "37")
			)
			(pin passive line
				(at -38.1 81.28 0)
				(length 3.81)
				(name "AWD")
				(number "72")
			)
			(pin passive line
				(at -38.1 78.74 0)
				(length 3.81)
				(name "TEST")
				(number "38")
			)
			(pin input line
				(at -38.1 73.66 0)
				(length 3.81)
				(name "GIOA[0]/INT0")
				(number "39")
			)
			(pin passive line
				(at -38.1 71.12 0)
				(length 3.81)
				(name "GIOA[1]/INT1/ECLK")
				(number "40")
			)
			(pin passive line
				(at -38.1 68.58 0)
				(length 3.81)
				(name "GIOA[2]/INT2")
				(number "41")
			)
			(pin passive line
				(at -38.1 66.04 0)
				(length 3.81)
				(name "GIOA[3]/INT3")
				(number "42")
			)
			(pin passive line
				(at -38.1 63.5 0)
				(length 3.81)
				(name "GIOA[4]/INT4")
				(number "36")
			)
			(pin passive line
				(at -38.1 60.96 0)
				(length 3.81)
				(name "GIOA[5]/INT5")
				(number "35")
			)
			(pin passive line
				(at -38.1 58.42 0)
				(length 3.81)
				(name "GIOA[6]/INT6")
				(number "34")
			)
			(pin passive line
				(at -38.1 55.88 0)
				(length 3.81)
				(name "GIOA[7]/INT7")
				(number "33")
			)
			(pin passive line
				(at -38.1 53.34 0)
				(length 3.81)
				(name "GIOB[7]")
				(number "84")
			)
			(pin passive line
				(at -38.1 48.26 0)
				(length 3.81)
				(name "GIOC[0]")
				(number "122")
			)
			(pin passive line
				(at -38.1 45.72 0)
				(length 3.81)
				(name "GIOC[1]")
				(number "143")
			)
			(pin passive line
				(at -38.1 43.18 0)
				(length 3.81)
				(name "GIOC[2]")
				(number "144")
			)
			(pin passive line
				(at -38.1 38.1 0)
				(length 3.81)
				(name "GIOD[0]")
				(number "21")
			)
			(pin passive line
				(at -38.1 35.56 0)
				(length 3.81)
				(name "GIOD[1]")
				(number "20")
			)
			(pin passive line
				(at -38.1 33.02 0)
				(length 3.81)
				(name "GIOD[2]")
				(number "19")
			)
			(pin passive line
				(at -38.1 30.48 0)
				(length 3.81)
				(name "GIOD[3]")
				(number "18")
			)
			(pin passive line
				(at -38.1 22.86 0)
				(length 3.81)
				(name "FLTP2")
				(number "133")
			)
			(pin passive line
				(at -38.1 20.32 0)
				(length 3.81)
				(name "FLTP1")
				(number "134")
			)
			(pin passive line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "HET[0]")
				(number "129")
			)
			(pin passive line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "HET[1]")
				(number "130")
			)
			(pin passive line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "HET[2]")
				(number "137")
			)
			(pin passive line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "HET[3]")
				(number "138")
			)
			(pin passive line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "HET[4]")
				(number "139")
			)
			(pin passive line
				(at -38.1 0 0)
				(length 3.81)
				(name "HET[5]")
				(number "140")
			)
			(pin passive line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "HET[6]")
				(number "141")
			)
			(pin passive line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "HET[7]")
				(number "142")
			)
			(pin passive line
				(at -38.1 -7.62 0)
				(length 3.81)
				(name "HET[8]")
				(number "79")
			)
			(pin passive line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "HET[9]")
				(number "80")
			)
			(pin passive line
				(at -38.1 -12.7 0)
				(length 3.81)
				(name "HET[10]")
				(number "29")
			)
			(pin passive line
				(at -38.1 -15.24 0)
				(length 3.81)
				(name "HET[11]")
				(number "28")
			)
			(pin passive line
				(at -38.1 -17.78 0)
				(length 3.81)
				(name "HET[12]")
				(number "27")
			)
			(pin passive line
				(at -38.1 -20.32 0)
				(length 3.81)
				(name "HET[13]")
				(number "26")
			)
			(pin passive line
				(at -38.1 -22.86 0)
				(length 3.81)
				(name "HET[14]")
				(number "25")
			)
			(pin passive line
				(at -38.1 -25.4 0)
				(length 3.81)
				(name "HET[15]")
				(number "24")
			)
			(pin passive line
				(at -38.1 -27.94 0)
				(length 3.81)
				(name "HET[16]")
				(number "23")
			)
			(pin passive line
				(at -38.1 -30.48 0)
				(length 3.81)
				(name "HET[17]")
				(number "22")
			)
			(pin passive line
				(at -38.1 -33.02 0)
				(length 3.81)
				(name "HET[18]")
				(number "71")
			)
			(pin passive line
				(at -38.1 -35.56 0)
				(length 3.81)
				(name "HET[19]")
				(number "70")
			)
			(pin passive line
				(at -38.1 -38.1 0)
				(length 3.81)
				(name "HET[20]")
				(number "69")
			)
			(pin passive line
				(at -38.1 -40.64 0)
				(length 3.81)
				(name "HET[21]")
				(number "68")
			)
			(pin passive line
				(at -38.1 -43.18 0)
				(length 3.81)
				(name "HET[22]")
				(number "67")
			)
			(pin passive line
				(at -38.1 -45.72 0)
				(length 3.81)
				(name "HET[23]")
				(number "123")
			)
			(pin passive line
				(at -38.1 -48.26 0)
				(length 3.81)
				(name "HET[24]")
				(number "51")
			)
			(pin passive line
				(at -38.1 -50.8 0)
				(length 3.81)
				(name "HET[25]")
				(number "124")
			)
			(pin passive line
				(at -38.1 -53.34 0)
				(length 3.81)
				(name "HET[26]")
				(number "125")
			)
			(pin passive line
				(at -38.1 -55.88 0)
				(length 3.81)
				(name "HET[27]")
				(number "126")
			)
			(pin passive line
				(at -38.1 -58.42 0)
				(length 3.81)
				(name "HET[28]")
				(number "47")
			)
			(pin passive line
				(at -38.1 -60.96 0)
				(length 3.81)
				(name "HET[29]")
				(number "48")
			)
			(pin passive line
				(at -38.1 -63.5 0)
				(length 3.81)
				(name "HET[30]")
				(number "49")
			)
			(pin passive line
				(at -38.1 -66.04 0)
				(length 3.81)
				(name "HET[31]")
				(number "50")
			)
			(pin passive line
				(at -38.1 -71.12 0)
				(length 3.81)
				(name "CLKOUT")
				(number "83")
			)
			(pin passive line
				(at -38.1 -73.66 0)
				(length 3.81)
				(name "PLLDIS")
				(number "73")
			)
			(pin passive line
				(at -38.1 -78.74 0)
				(length 3.81)
				(name "OSCOUT")
				(number "12")
			)
			(pin passive line
				(at -38.1 -81.28 0)
				(length 3.81)
				(name "OSCIN")
				(number "13")
			)
			(pin passive line
				(at -20.32 96.52 270)
				(length 3.81)
				(name "Vcc")
				(number "132")
			)
			(pin power_in line
				(at -17.78 96.52 270)
				(length 3.81)
				(name "Vcc")
				(number "14")
			)
			(pin power_in line
				(at -17.78 -96.52 90)
				(length 3.81)
				(name "Vss")
				(number "11")
			)
			(pin passive line
				(at -15.24 96.52 270)
				(length 3.81)
				(name "Vcc")
				(number "31")
			)
			(pin passive line
				(at -15.24 -96.52 90)
				(length 3.81)
				(name "Vss")
				(number "30")
			)
			(pin unspecified line
				(at -12.7 96.52 270)
				(length 3.81)
				(name "Vcc")
				(number "55")
			)
			(pin power_in line
				(at -12.7 -96.52 90)
				(length 3.81)
				(name "Vss")
				(number "54")
			)
			(pin passive line
				(at -10.16 96.52 270)
				(length 3.81)
				(name "Vcc")
				(number "128")
			)
			(pin passive line
				(at -10.16 -96.52 90)
				(length 3.81)
				(name "Vss")
				(number "131")
			)
			(pin passive line
				(at -7.62 96.52 270)
				(length 3.81)
				(name "Vcc")
				(number "86")
			)
			(pin passive line
				(at -7.62 -96.52 90)
				(length 3.81)
				(name "Vss")
				(number "127")
			)
			(pin passive line
				(at -5.08 96.52 270)
				(length 3.81)
				(name "Vcc")
				(number "93")
			)
			(pin passive line
				(at -5.08 -96.52 90)
				(length 3.81)
				(name "Vss")
				(number "92")
			)
			(pin passive line
				(at -2.54 -96.52 90)
				(length 3.81)
				(name "Vss")
				(number "85")
			)
			(pin passive line
				(at 0 96.52 270)
				(length 3.81)
				(name "VccP")
				(number "135")
			)
			(pin passive line
				(at 0 -96.52 90)
				(length 3.81)
				(name "Vss")
				(number "136")
			)
			(pin passive line
				(at 5.08 96.52 270)
				(length 3.81)
				(name "VccAD")
				(number "118")
			)
			(pin passive line
				(at 5.08 -96.52 90)
				(length 3.81)
				(name "VssAD")
				(number "119")
			)
			(pin passive line
				(at 10.16 96.52 270)
				(length 3.81)
				(name "VccIO")
				(number "82")
			)
			(pin passive line
				(at 10.16 -96.52 90)
				(length 3.81)
				(name "VssIO")
				(number "81")
			)
			(pin power_in line
				(at 12.7 96.52 270)
				(length 3.81)
				(name "VccIO")
				(number "17")
			)
			(pin power_in line
				(at 12.7 -96.52 90)
				(length 3.81)
				(name "VssIO")
				(number "16")
			)
			(pin power_in line
				(at 15.24 96.52 270)
				(length 3.81)
				(name "VccIO")
				(number "53")
			)
			(pin power_in line
				(at 15.24 -96.52 90)
				(length 3.81)
				(name "VssIO")
				(number "52")
			)
			(pin passive line
				(at 38.1 88.9 180)
				(length 3.81)
				(name "TMS2")
				(number "121")
			)
			(pin passive line
				(at 38.1 86.36 180)
				(length 3.81)
				(name "TMS")
				(number "120")
			)
			(pin passive line
				(at 38.1 83.82 180)
				(length 3.81)
				(name "TCK")
				(number "76")
			)
			(pin passive line
				(at 38.1 81.28 180)
				(length 3.81)
				(name "TDO5")
				(number "75")
			)
			(pin passive line
				(at 38.1 78.74 180)
				(length 3.81)
				(name "TDI")
				(number "74")
			)
			(pin passive line
				(at 38.1 73.66 180)
				(length 3.81)
				(name "ADIN[0]")
				(number "108")
			)
			(pin passive line
				(at 38.1 71.12 180)
				(length 3.81)
				(name "ADIN[1]")
				(number "107")
			)
			(pin passive line
				(at 38.1 68.58 180)
				(length 3.81)
				(name "ADIN[2]")
				(number "106")
			)
			(pin passive line
				(at 38.1 66.04 180)
				(length 3.81)
				(name "ADIN[3]")
				(number "105")
			)
			(pin passive line
				(at 38.1 63.5 180)
				(length 3.81)
				(name "ADIN[4]")
				(number "104")
			)
			(pin passive line
				(at 38.1 60.96 180)
				(length 3.81)
				(name "ADIN[5]")
				(number "102")
			)
			(pin passive line
				(at 38.1 58.42 180)
				(length 3.81)
				(name "ADIN[6]")
				(number "101")
			)
			(pin passive line
				(at 38.1 55.88 180)
				(length 3.81)
				(name "ADIN[7]")
				(number "100")
			)
			(pin passive line
				(at 38.1 53.34 180)
				(length 3.81)
				(name "ADIN[8]")
				(number "115")
			)
			(pin passive line
				(at 38.1 50.8 180)
				(length 3.81)
				(name "ADIN[9]")
				(number "113")
			)
			(pin passive line
				(at 38.1 48.26 180)
				(length 3.81)
				(name "ADIN[10]")
				(number "111")
			)
			(pin passive line
				(at 38.1 45.72 180)
				(length 3.81)
				(name "ADIN[11]")
				(number "109")
			)
			(pin passive line
				(at 38.1 43.18 180)
				(length 3.81)
				(name "ADIN[12]")
				(number "114")
			)
			(pin passive line
				(at 38.1 40.64 180)
				(length 3.81)
				(name "ADIN[13]")
				(number "112")
			)
			(pin passive line
				(at 38.1 38.1 180)
				(length 3.81)
				(name "ADIN[14]")
				(number "110")
			)
			(pin passive line
				(at 38.1 35.56 180)
				(length 3.81)
				(name "ADIN[15]")
				(number "103")
			)
			(pin passive line
				(at 38.1 30.48 180)
				(length 3.81)
				(name "ADRefHi")
				(number "116")
			)
			(pin passive line
				(at 38.1 27.94 180)
				(length 3.81)
				(name "ADRefLo")
				(number "117")
			)
			(pin passive line
				(at 38.1 22.86 180)
				(length 3.81)
				(name "ADEVT")
				(number "99")
			)
			(pin passive line
				(at 38.1 17.78 180)
				(length 3.81)
				(name "SCI1RX")
				(number "91")
			)
			(pin passive line
				(at 38.1 15.24 180)
				(length 3.81)
				(name "SCI1TX")
				(number "90")
			)
			(pin passive line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "SCI1CLK")
				(number "89")
			)
			(pin passive line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "SCI2RX")
				(number "43")
			)
			(pin passive line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "SCI2TX")
				(number "44")
			)
			(pin passive line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "SCI2CLK")
				(number "45")
			)
			(pin passive line
				(at 38.1 0 180)
				(length 3.81)
				(name "CAN1HTX")
				(number "88")
			)
			(pin passive line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "CAN1HRX")
				(number "87")
			)
			(pin passive line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "CAN3HTX")
				(number "78")
			)
			(pin passive line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "CAN3HRX")
				(number "77")
			)
			(pin passive line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "CAN2HTX")
				(number "56")
			)
			(pin passive line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "CAN2HRX")
				(number "57")
			)
			(pin passive inverted
				(at 38.1 -17.78 180)
				(length 3.81)
				(name "~{SPI1ENA}")
				(number "1")
			)
			(pin passive inverted
				(at 38.1 -20.32 180)
				(length 3.81)
				(name "~{SPI1SCS}")
				(number "2")
			)
			(pin passive line
				(at 38.1 -22.86 180)
				(length 3.81)
				(name "SPI1CLK")
				(number "5")
			)
			(pin passive line
				(at 38.1 -25.4 180)
				(length 3.81)
				(name "SPI1SIMO")
				(number "3")
			)
			(pin passive line
				(at 38.1 -27.94 180)
				(length 3.81)
				(name "SPI1SOMI")
				(number "4")
			)
			(pin passive inverted
				(at 38.1 -33.02 180)
				(length 3.81)
				(name "~{SPI2ENA}")
				(number "65")
			)
			(pin passive inverted
				(at 38.1 -35.56 180)
				(length 3.81)
				(name "~{SPI2SCS}")
				(number "66")
			)
			(pin passive line
				(at 38.1 -38.1 180)
				(length 3.81)
				(name "SPI2CLK")
				(number "62")
			)
			(pin passive line
				(at 38.1 -40.64 180)
				(length 3.81)
				(name "SPI2SIMO")
				(number "63")
			)
			(pin passive line
				(at 38.1 -43.18 180)
				(length 3.81)
				(name "SPI2SOMI")
				(number "64")
			)
			(pin passive inverted
				(at 38.1 -48.26 180)
				(length 3.81)
				(name "~{SPI3ENA}")
				(number "98")
			)
			(pin passive inverted
				(at 38.1 -50.8 180)
				(length 3.81)
				(name "~{SPI3SCS}")
				(number "97")
			)
			(pin passive line
				(at 38.1 -53.34 180)
				(length 3.81)
				(name "SPI3CLK")
				(number "94")
			)
			(pin passive line
				(at 38.1 -55.88 180)
				(length 3.81)
				(name "SPI3SIMO")
				(number "96")
			)
			(pin passive line
				(at 38.1 -58.42 180)
				(length 3.81)
				(name "SPI3SOMI")
				(number "95")
			)
			(pin passive inverted
				(at 38.1 -63.5 180)
				(length 3.81)
				(name "~{SPI4ENA}")
				(number "6")
			)
			(pin passive inverted
				(at 38.1 -66.04 180)
				(length 3.81)
				(name "~{SPI4SCS}")
				(number "7")
			)
			(pin passive line
				(at 38.1 -68.58 180)
				(length 3.81)
				(name "SPI4CLK")
				(number "10")
			)
			(pin passive line
				(at 38.1 -71.12 180)
				(length 3.81)
				(name "SPI4SIMO")
				(number "8")
			)
			(pin passive line
				(at 38.1 -73.66 180)
				(length 3.81)
				(name "SPI4SOMI")
				(number "9")
			)
			(pin passive inverted
				(at 38.1 -78.74 180)
				(length 3.81)
				(name "~{SPI5ENA}")
				(number "61")
			)
			(pin passive inverted
				(at 38.1 -81.28 180)
				(length 3.81)
				(name "~{SPI5SCS}")
				(number "46")
			)
			(pin passive line
				(at 38.1 -83.82 180)
				(length 3.81)
				(name "SPI5CLK")
				(number "60")
			)
			(pin passive line
				(at 38.1 -86.36 180)
				(length 3.81)
				(name "SPI5SIMO")
				(number "58")
			)
			(pin passive line
				(at 38.1 -88.9 180)
				(length 3.81)
				(name "SPI5SOMI")
				(number "59")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM3S6911-IQC50"
		(extends "LM3S6911-EQC50")
		(property "Reference" "U"
			(at -36.83 55.88 0)
		)
		(property "Value" "LM3S6911-IQC50"
			(at 25.4 55.88 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 48.26 -58.42 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3s6911.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ti Stellaris ARM-M3 MCU Ethernet PHY, Industrial grade, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM M3 Stellaris PHY ETH NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM4F110B2QR"
		(extends "TM4C1231C3PM")
		(property "Reference" "U"
			(at -31.75 50.8 0)
		)
		(property "Value" "LM4F110B2QR"
			(at 16.51 50.8 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 30.48 -53.34 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1231c3pm.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Replaced by TM4C1231C3PM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Stellaris Cortex M4 MCU NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5*"
			(at 0 0 0)
		)
	)
	(symbol "LM4F110C4QR"
		(extends "TM4C1231C3PM")
		(property "Reference" "U"
			(at -31.75 50.8 0)
		)
		(property "Value" "LM4F110C4QR"
			(at 16.51 50.8 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 30.48 -53.34 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1231d5pm.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Replaced by TM4C1231D5PM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Stellaris Cortex M4 MCU NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5*"
			(at 0 0 0)
		)
	)
	(symbol "LM4F110E5QR"
		(extends "TM4C1231C3PM")
		(property "Reference" "U"
			(at -31.75 50.8 0)
		)
		(property "Value" "LM4F110E5QR"
			(at 16.51 50.8 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 30.48 -53.34 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1231e6pm.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Replaced by TM4C1231E6PM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Stellaris Cortex M4 MCU NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5*"
			(at 0 0 0)
		)
	)
	(symbol "LM4F110H5QR"
		(extends "TM4C1231C3PM")
		(property "Reference" "U"
			(at -31.75 50.8 0)
		)
		(property "Value" "LM4F110H5QR"
			(at 16.51 50.8 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 30.48 -53.34 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1231h6pm.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Replaced by TM4C1231H6PM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Stellaris Cortex M4 MCU NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5*"
			(at 0 0 0)
		)
	)
	(symbol "LM4F111B2QR"
		(extends "TM4C1230C3PM")
		(property "Reference" "U"
			(at -31.75 48.26 0)
		)
		(property "Value" "LM4F111B2QR"
			(at 16.51 48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 31.75 -50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1230c3pm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Replaced by TM4C1230C3PM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Stellaris Cortex M4 MCU NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM4F111C4QR"
		(extends "TM4C1230C3PM")
		(property "Reference" "U"
			(at -31.75 48.26 0)
		)
		(property "Value" "LM4F111C4QR"
			(at 16.51 48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 31.75 -50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1230d5pm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Replaced by TM4C1230D5PM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Stellaris Cortex M4 MCU NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM4F111E5QR"
		(extends "TM4C1230C3PM")
		(property "Reference" "U"
			(at -31.75 48.26 0)
		)
		(property "Value" "LM4F111E5QR"
			(at 16.51 48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 31.75 -50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1230c3pm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Replaced by TM4C1230E6PM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Stellaris Cortex M4 MCU NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM4F111H5QR"
		(extends "TM4C1230C3PM")
		(property "Reference" "U"
			(at -31.75 48.26 0)
		)
		(property "Value" "LM4F111H5QR"
			(at 16.51 48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 31.75 -50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1230h6pm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Replaced by TM4C1230H6PM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Stellaris Cortex M4 MCU NRND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TM4C1230D5PM"
		(extends "TM4C1230C3PM")
		(property "Reference" "U"
			(at -31.75 48.26 0)
		)
		(property "Value" "TM4C1230D5PM"
			(at 16.51 48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 31.75 -50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1230d5pm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Tiva ARM 32bit CortexM4 Microcotroller, 80MHz, 64kB Flash, 24kB SRAM, 2k EEPROM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Tiva Cortex M4 MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TM4C1230E6PM"
		(extends "TM4C1230C3PM")
		(property "Reference" "U"
			(at -31.75 48.26 0)
		)
		(property "Value" "TM4C1230E6PM"
			(at 16.51 48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 31.75 -50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1230e6pm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Tiva ARM 32bit CortexM4 Microcotroller, 80MHz, 128kB Flash, 32kB SRAM, 2k EEPROM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Tiva Cortex M4 MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TM4C1230H6PM"
		(extends "TM4C1230C3PM")
		(property "Reference" "U"
			(at -31.75 48.26 0)
		)
		(property "Value" "TM4C1230H6PM"
			(at 16.51 48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 31.75 -50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1230h6pm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Tiva ARM 32bit CortexM4 Microcotroller, 80MHz, 256kB Flash, 32kB SRAM, 2k EEPROM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Tiva Cortex M4 MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TM4C1231D5PM"
		(extends "TM4C1231C3PM")
		(property "Reference" "U"
			(at -31.75 50.8 0)
		)
		(property "Value" "TM4C1231D5PM"
			(at 16.51 50.8 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 30.48 -53.34 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1231d5pm.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Tiva ARM 32bit CortexM4 Microcotroller, 80MHz, 64kB Flash, 24kB SRAM, 2k EEPROM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Tiva Cortex M4 MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5*"
			(at 0 0 0)
		)
	)
	(symbol "TM4C1231E6PM"
		(extends "TM4C1231C3PM")
		(property "Reference" "U"
			(at -31.75 50.8 0)
		)
		(property "Value" "TM4C1231E6PM"
			(at 16.51 50.8 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 30.48 -53.34 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1231e6pm.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Tiva ARM 32bit CortexM4 Microcotroller, 80MHz, 128kB Flash, 32kB SRAM, 2k EEPROM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Tiva Cortex M4 MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5*"
			(at 0 0 0)
		)
	)
	(symbol "TM4C1231H6PM"
		(extends "TM4C1231C3PM")
		(property "Reference" "U"
			(at -31.75 50.8 0)
		)
		(property "Value" "TM4C1231H6PM"
			(at 16.51 50.8 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 30.48 -53.34 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c1231h6pm.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Tiva ARM 32bit CortexM4 Microcotroller, 80MHz, 256kB Flash, 32kB SRAM, 2k EEPROM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM Tiva Cortex M4 MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5*"
			(at 0 0 0)
		)
	)
)
