(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CC430F5137xRGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 34.29 0)
		)
		(property "Value" "CC430F5137xRGZ"
			(at 13.97 34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-48-1EP_7x7mm_P0.5mm_EP4.1x4.1mm_ThermalVias"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cc430f5137.pdf"
			(at -10.16 31.75 0)
		)
		(property "Description" "32KB Flash, 4KB RAM, MSP430 core with integrated CC1101 radio transceiver, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 CC430 16-bit mixed signal microcontroller CC1101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CC430F5137xRGZ_0_1")
		(symbol "CC430F5137xRGZ_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "~{RST}")
				(number "40")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PJ.0/TDO")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PJ.1/TDI/TCLK")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PJ.2/TMS")
				(number "37")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PJ.3/TCK")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TEST")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "P3.0")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "P3.1")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "P3.2")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P3.3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "P3.4")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P3.5")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P3.6")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P3.7")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "P5.0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "P5.1")
				(number "43")
			)
			(pin output line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "RF_XOUT")
				(number "26")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "RF_XIN")
				(number "25")
			)
			(pin power_in line
				(at -7.62 35.56 270)
				(length 2.54)
				(name "VCORE")
				(number "7")
			)
			(pin passive line
				(at -5.08 35.56 270)
				(length 2.54)
				(hide yes)
				(name "DVCC")
				(number "22")
			)
			(pin passive line
				(at -5.08 35.56 270)
				(length 2.54)
				(hide yes)
				(name "DVCC")
				(number "41")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 2.54)
				(name "DVCC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "GUARD")
				(number "34")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "45")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "AVSS")
				(number "42")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC_RF")
				(number "27")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "AVCC_RF")
				(number "28")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 2.54)
				(name "AVCC_RF")
				(number "31")
			)
			(pin passive line
				(at 5.08 35.56 270)
				(length 2.54)
				(hide yes)
				(name "AVCC_RF")
				(number "32")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "RF_P")
				(number "29")
			)
			(pin passive line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "RF_N")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P1.1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P1.2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P1.3")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P1.4")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "P1.6")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "P1.7")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P2.0")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P2.1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "P2.2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P2.3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "P2.4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P2.5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "P2.6")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "P2.7")
				(number "23")
			)
			(pin passive line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "RBIAS")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430AFE221IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 19.05 0)
		)
		(property "Value" "MSP430AFE221IPW"
			(at 15.24 -19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at -21.59 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430afe221.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430AFE221IPW_0_1")
		(symbol "MSP430AFE221IPW_1_1"
			(pin input line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "11")
			)
			(pin passive line
				(at -27.94 8.89 0)
				(length 3.81)
				(name "A0.0+")
				(number "1")
			)
			(pin passive line
				(at -27.94 6.35 0)
				(length 3.81)
				(name "A0.0-")
				(number "2")
			)
			(pin passive line
				(at -27.94 1.27 0)
				(length 3.81)
				(name "(AVSS)")
				(number "3")
			)
			(pin passive line
				(at -27.94 -1.27 0)
				(length 3.81)
				(name "(AVSS)")
				(number "4")
			)
			(pin passive line
				(at -27.94 -6.35 0)
				(length 3.81)
				(name "(AVSS)")
				(number "8")
			)
			(pin passive line
				(at -27.94 -8.89 0)
				(length 3.81)
				(name "(AVSS)")
				(number "9")
			)
			(pin passive line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "Vref")
				(number "7")
			)
			(pin power_in line
				(at -5.08 21.59 270)
				(length 3.81)
				(name "AVCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -21.59 90)
				(length 3.81)
				(name "AVSS")
				(number "6")
			)
			(pin power_in line
				(at 5.08 21.59 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -21.59 90)
				(length 3.81)
				(name "DVSS")
				(number "13")
			)
			(pin input line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 11.43 180)
				(length 3.81)
				(name "TA2/SMCLK/TACLK/SVSIN/P1.0")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 8.89 180)
				(length 3.81)
				(name "SDCLK/TA1/P1.1")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 6.35 180)
				(length 3.81)
				(name "SD0DO/TA0/P1.2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 3.81 180)
				(length 3.81)
				(name "UTXD0/P1.3")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 1.27 180)
				(length 3.81)
				(name "URXD0/P1.4")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -1.27 180)
				(length 3.81)
				(name "TMS/SVSOUT/SIMO0/P1.5")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -3.81 180)
				(length 3.81)
				(name "TCK/TA2/SOMI0/P1.6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -6.35 180)
				(length 3.81)
				(name "TDI/TDO/TA1/UCLK0/P1.7")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "TCLK/TDI/TA0/STE0/P2.0")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "XT2IN/P2.6")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "XT2OUT/P2.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430AFE222IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 19.05 0)
		)
		(property "Value" "MSP430AFE222IPW"
			(at 15.24 -19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at -21.59 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430afe222.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430AFE222IPW_0_1")
		(symbol "MSP430AFE222IPW_1_1"
			(pin input line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "11")
			)
			(pin passive line
				(at -27.94 8.89 0)
				(length 3.81)
				(name "A0.0+")
				(number "1")
			)
			(pin passive line
				(at -27.94 6.35 0)
				(length 3.81)
				(name "A0.0-")
				(number "2")
			)
			(pin passive line
				(at -27.94 1.27 0)
				(length 3.81)
				(name "A1.0+")
				(number "3")
			)
			(pin passive line
				(at -27.94 -1.27 0)
				(length 3.81)
				(name "A1.0-")
				(number "4")
			)
			(pin passive line
				(at -27.94 -6.35 0)
				(length 3.81)
				(name "(AVSS)")
				(number "8")
			)
			(pin passive line
				(at -27.94 -8.89 0)
				(length 3.81)
				(name "(AVSS)")
				(number "9")
			)
			(pin passive line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "Vref")
				(number "7")
			)
			(pin power_in line
				(at -5.08 21.59 270)
				(length 3.81)
				(name "AVCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -21.59 90)
				(length 3.81)
				(name "AVSS")
				(number "6")
			)
			(pin power_in line
				(at 5.08 21.59 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -21.59 90)
				(length 3.81)
				(name "DVSS")
				(number "13")
			)
			(pin input line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 11.43 180)
				(length 3.81)
				(name "TA2/SMCLK/TACLK/SVSIN/P1.0")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 8.89 180)
				(length 3.81)
				(name "SDCLK/TA1/P1.1")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 6.35 180)
				(length 3.81)
				(name "SD0DO/TA0/P1.2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 3.81 180)
				(length 3.81)
				(name "SD1DO/UTXD0/P1.3")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 1.27 180)
				(length 3.81)
				(name "URXD0/P1.4")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -1.27 180)
				(length 3.81)
				(name "TMS/SVSOUT/SIMO0/P1.5")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -3.81 180)
				(length 3.81)
				(name "TCK/TA2/SOMI0/P1.6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -6.35 180)
				(length 3.81)
				(name "TDI/TDO/TA1/UCLK0/P1.7")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "TCLK/TDI/TA0/STE0/P2.0")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "XT2IN/P2.6")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "XT2OUT/P2.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430AFE223IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 19.05 0)
		)
		(property "Value" "MSP430AFE223IPW"
			(at 15.24 -19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at -21.59 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430afe223.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430AFE223IPW_0_1")
		(symbol "MSP430AFE223IPW_1_1"
			(pin input line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "11")
			)
			(pin passive line
				(at -27.94 8.89 0)
				(length 3.81)
				(name "A0.0+")
				(number "1")
			)
			(pin passive line
				(at -27.94 6.35 0)
				(length 3.81)
				(name "A0.0-")
				(number "2")
			)
			(pin passive line
				(at -27.94 1.27 0)
				(length 3.81)
				(name "A1.0+")
				(number "3")
			)
			(pin passive line
				(at -27.94 -1.27 0)
				(length 3.81)
				(name "A1.0-")
				(number "4")
			)
			(pin passive line
				(at -27.94 -6.35 0)
				(length 3.81)
				(name "A2.0+")
				(number "8")
			)
			(pin passive line
				(at -27.94 -8.89 0)
				(length 3.81)
				(name "A2.0-")
				(number "9")
			)
			(pin passive line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "Vref")
				(number "7")
			)
			(pin power_in line
				(at -5.08 21.59 270)
				(length 3.81)
				(name "AVCC")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -21.59 90)
				(length 3.81)
				(name "AVSS")
				(number "6")
			)
			(pin power_in line
				(at 5.08 21.59 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -21.59 90)
				(length 3.81)
				(name "DVSS")
				(number "13")
			)
			(pin input line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 11.43 180)
				(length 3.81)
				(name "TA2/SMCLK/TACLK/SVSIN/P1.0")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 8.89 180)
				(length 3.81)
				(name "SDCLK/TA1/P1.1")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 6.35 180)
				(length 3.81)
				(name "SD0DO/TA0/P1.2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 3.81 180)
				(length 3.81)
				(name "SD1DO/UTXD0/P1.3")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 1.27 180)
				(length 3.81)
				(name "SD2DO/URXD0/P1.4")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -1.27 180)
				(length 3.81)
				(name "TMS/SVSOUT/SIMO0/P1.5")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -3.81 180)
				(length 3.81)
				(name "TCK/TA2/SOMI0/P1.6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -6.35 180)
				(length 3.81)
				(name "TDI/TDO/TA1/UCLK0/P1.7")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "TCLK/TDI/TA0/STE0/P2.0")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "XT2IN/P2.6")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "XT2OUT/P2.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1101AIDGV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1101AIDGV"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1101a.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 128B Flash, 128B RAM, TVSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1101AIDGV_0_1")
		(symbol "MSP430F1101AIDGV_1_1"
			(pin input line
				(at -20.32 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "P2.0/ACLK")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "P2.1/INCLK")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "P2.2/CAOUT/TA0")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "P2.3/CA0/TA1")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "P2.4/CA1/TA2")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "P2.5/Rosc")
				(number "3")
			)
			(pin input line
				(at -20.32 -8.89 0)
				(length 3.81)
				(name "XIN")
				(number "6")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 20.32 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1101AIDW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1101AIDW"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1101a.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 128B Flash, 128B RAM, SOWB-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1101AIDW_0_1")
		(symbol "MSP430F1101AIDW_1_1"
			(pin input line
				(at -20.32 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "P2.0/ACLK")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "P2.1/INCLK")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "P2.2/CAOUT/TA0")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "P2.3/CA0/TA1")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "P2.4/CA1/TA2")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "P2.5/Rosc")
				(number "3")
			)
			(pin input line
				(at -20.32 -8.89 0)
				(length 3.81)
				(name "XIN")
				(number "6")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 20.32 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1101AIPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1101AIPW"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1101a.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 128B Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1101AIPW_0_1")
		(symbol "MSP430F1101AIPW_1_1"
			(pin input line
				(at -20.32 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "P2.0/ACLK")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "P2.1/INCLK")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "P2.2/CAOUT/TA0")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "P2.3/CA0/TA1")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "P2.4/CA1/TA2")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "P2.5/Rosc")
				(number "3")
			)
			(pin input line
				(at -20.32 -8.89 0)
				(length 3.81)
				(name "XIN")
				(number "6")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 20.32 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1101AIRGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1101AIRGE"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1101a.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 128B Flash, 128B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1101AIRGE_0_1")
		(symbol "MSP430F1101AIRGE_1_1"
			(pin input line
				(at -20.32 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "P2.0/ACLK")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "P2.1/INCLK")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "P2.2/CAOUT/TA0")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "P2.3/CA0/TA1")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "P2.4/CA1/TA2")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "P2.5/Rosc")
				(number "24")
			)
			(pin input line
				(at -20.32 -8.89 0)
				(length 3.81)
				(name "XIN")
				(number "4")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "XOUT")
				(number "3")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "2")
			)
			(pin input line
				(at 20.32 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1122IDW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 15.24 0)
		)
		(property "Value" "MSP430F1122IDW"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1122.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, SOWB-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1122IDW_0_1")
		(symbol "MSP430F1122IDW_1_1"
			(pin input line
				(at -27.94 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "P2.0/A0/ACLK")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "P2.1/A1/INCLK")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "P2.2/A2/TA0")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "P2.3/A3/VREF-/VeREF-/TA1")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "P2.4/A4/VREF+/VeREF+/TA2")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "P2.5/Rosc")
				(number "3")
			)
			(pin input line
				(at -27.94 -8.89 0)
				(length 3.81)
				(name "XIN")
				(number "6")
			)
			(pin output line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 27.94 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1122IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 15.24 0)
		)
		(property "Value" "MSP430F1122IPW"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1122.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1122IPW_0_1")
		(symbol "MSP430F1122IPW_1_1"
			(pin input line
				(at -27.94 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "P2.0/A0/ACLK")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "P2.1/A1/INCLK")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "P2.2/A2/TA0")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "P2.3/A3/VREF-/VeREF-/TA1")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "P2.4/A4/VREF+/VeREF+/TA2")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "P2.5/Rosc")
				(number "3")
			)
			(pin input line
				(at -27.94 -8.89 0)
				(length 3.81)
				(name "XIN")
				(number "6")
			)
			(pin output line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 27.94 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1122IRHB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 15.24 0)
		)
		(property "Value" "MSP430F1122IRHB"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1122.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1122IRHB_0_1")
		(symbol "MSP430F1122IRHB_1_1"
			(pin input line
				(at -27.94 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "P2.0/A0/ACLK")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "P2.1/A1/INCLK")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "P2.2/A2/TA0")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "P2.3/A3/VREF-/VeREF-/TA1")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "P2.4/A4/VREF+/VeREF+/TA2")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "P2.5/Rosc")
				(number "32")
			)
			(pin input line
				(at -27.94 -8.89 0)
				(length 3.81)
				(name "XIN")
				(number "3")
			)
			(pin output line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "XOUT")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "30")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "1")
			)
			(pin input line
				(at 27.94 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1222IDW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F1222IDW"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1222.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, SOWB-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1222IDW_0_1")
		(symbol "MSP430F1222IDW_1_1"
			(pin input line
				(at -22.86 19.05 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "P3.0/A5/STE0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "P3.1/SIMO0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "P3.2/SOMI0")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P3.3/UCLK0")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P3.4/UTXD0")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P3.5/URXD0")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P3.6/A6")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P3.7/A7")
				(number "18")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "XIN")
				(number "6")
			)
			(pin output line
				(at -22.86 -19.05 0)
				(length 3.81)
				(name "XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 22.86 19.05 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -6.35 180)
				(length 3.81)
				(name "ACLK/A0/P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -8.89 180)
				(length 3.81)
				(name "INCLK/A1/P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -11.43 180)
				(length 3.81)
				(name "TA0/A2/P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -13.97 180)
				(length 3.81)
				(name "TA1/VeREF-/VREF-/A3/P2.3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -16.51 180)
				(length 3.81)
				(name "TA2/VeREF+/VREF+/A4/P2.4")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -19.05 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1222IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F1222IPW"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1222.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1222IPW_0_1")
		(symbol "MSP430F1222IPW_1_1"
			(pin input line
				(at -22.86 19.05 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "P3.0/A5/STE0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "P3.1/SIMO0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "P3.2/SOMI0")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P3.3/UCLK0")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P3.4/UTXD0")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P3.5/URXD0")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P3.6/A6")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P3.7/A7")
				(number "18")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "XIN")
				(number "6")
			)
			(pin output line
				(at -22.86 -19.05 0)
				(length 3.81)
				(name "XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 22.86 19.05 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -6.35 180)
				(length 3.81)
				(name "ACLK/A0/P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -8.89 180)
				(length 3.81)
				(name "INCLK/A1/P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -11.43 180)
				(length 3.81)
				(name "TA0/A2/P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -13.97 180)
				(length 3.81)
				(name "TA1/VeREF-/VREF-/A3/P2.3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -16.51 180)
				(length 3.81)
				(name "TA2/VeREF+/VREF+/A4/P2.4")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -19.05 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F1222IRHB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F1222IRHB"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1222.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F1222IRHB_0_1")
		(symbol "MSP430F1222IRHB_1_1"
			(pin input line
				(at -22.86 19.05 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "P3.0/A5/STE0")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "P3.1/SIMO0")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "P3.2/SOMI0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P3.3/UCLK0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P3.4/UTXD0")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P3.5/URXD0")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P3.6/A6")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P3.7/A7")
				(number "16")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "XIN")
				(number "3")
			)
			(pin output line
				(at -22.86 -19.05 0)
				(length 3.81)
				(name "XOUT")
				(number "2")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "30")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "1")
			)
			(pin input line
				(at 22.86 19.05 180)
				(length 3.81)
				(name "TEST")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -6.35 180)
				(length 3.81)
				(name "ACLK/A0/P2.0")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -8.89 180)
				(length 3.81)
				(name "INCLK/A1/P2.1")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -11.43 180)
				(length 3.81)
				(name "TA0/A2/P2.2")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -13.97 180)
				(length 3.81)
				(name "TA1/VeREF-/VREF-/A3/P2.3")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -16.51 180)
				(length 3.81)
				(name "TA2/VeREF+/VREF+/A4/P2.4")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -19.05 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F122IDW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F122IDW"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f122.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, SOWB-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F122IDW_0_1")
		(symbol "MSP430F122IDW_1_1"
			(pin input line
				(at -22.86 19.05 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "P3.0/STE0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "P3.1/SIMO0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "P3.2/SOMI0")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P3.3/UCLK0")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P3.4/UTXD0")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P3.5/URXD0")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P3.6")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P3.7")
				(number "18")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "XIN")
				(number "6")
			)
			(pin output line
				(at -22.86 -19.05 0)
				(length 3.81)
				(name "XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 22.86 19.05 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -6.35 180)
				(length 3.81)
				(name "ACLK/P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -8.89 180)
				(length 3.81)
				(name "INCLK/P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -11.43 180)
				(length 3.81)
				(name "TA0/CAOUT/P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -13.97 180)
				(length 3.81)
				(name "TA1/CA0/P2.3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -16.51 180)
				(length 3.81)
				(name "TA2/CA1/P2.4")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -19.05 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F122IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F122IPW"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f122.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F122IPW_0_1")
		(symbol "MSP430F122IPW_1_1"
			(pin input line
				(at -22.86 19.05 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "P3.0/STE0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "P3.1/SIMO0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "P3.2/SOMI0")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P3.3/UCLK0")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P3.4/UTXD0")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P3.5/URXD0")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P3.6")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P3.7")
				(number "18")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "XIN")
				(number "6")
			)
			(pin output line
				(at -22.86 -19.05 0)
				(length 3.81)
				(name "XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 22.86 19.05 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -6.35 180)
				(length 3.81)
				(name "ACLK/P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -8.89 180)
				(length 3.81)
				(name "INCLK/P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -11.43 180)
				(length 3.81)
				(name "TA0/CAOUT/P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -13.97 180)
				(length 3.81)
				(name "TA1/CA0/P2.3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -16.51 180)
				(length 3.81)
				(name "TA2/CA1/P2.4")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -19.05 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F122IRHB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F122IRHB"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f122.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F122IRHB_0_1")
		(symbol "MSP430F122IRHB_1_1"
			(pin input line
				(at -22.86 19.05 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "P3.0/STE0")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "P3.1/SIMO0")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "P3.2/SOMI0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P3.3/UCLK0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P3.4/UTXD0")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P3.5/URXD0")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P3.6")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P3.7")
				(number "16")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "XIN")
				(number "3")
			)
			(pin output line
				(at -22.86 -19.05 0)
				(length 3.81)
				(name "XOUT")
				(number "2")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "30")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "1")
			)
			(pin input line
				(at 22.86 19.05 180)
				(length 3.81)
				(name "TEST")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -6.35 180)
				(length 3.81)
				(name "ACLK/P2.0")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -8.89 180)
				(length 3.81)
				(name "INCLK/P2.1")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -11.43 180)
				(length 3.81)
				(name "TA0/CAOUT/P2.2")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -13.97 180)
				(length 3.81)
				(name "TA1/CA0/P2.3")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -16.51 180)
				(length 3.81)
				(name "TA2/CA1/P2.4")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -19.05 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2001IN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2001IN"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2001.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2001IN_0_1")
		(symbol "MSP430F2001IN_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA1")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "CA0/TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "CA1/TA0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "CA2/TA1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "CA3/CAOUT/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "CA4/SMCLK/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "CA5/TA0/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "CA6/TA1/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "CA7/CAOUT/TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2001IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2001IPW"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2001.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2001IPW_0_1")
		(symbol "MSP430F2001IPW_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA1")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "CA0/TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "CA1/TA0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "CA2/TA1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "CA3/CAOUT/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "CA4/SMCLK/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "CA5/TA0/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "CA6/TA1/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "CA7/CAOUT/TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2001IRSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2001IRSA"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2001.pdf"
			(at -20.32 13.97 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2001IRSA_0_1")
		(symbol "MSP430F2001IRSA_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "CA0/TA0CLK/ACLK/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "CA1/TA0.0/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "CA2/TA0.1/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "CA3/CAOUT/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "CA4/TCK/SMCLK/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "CA5/TMS/TA0.0/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "CA6/TDI/TCLK/TA0.1/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "CA7/TDO/TDI/CAOUT/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2002IN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2002IN"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2002.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2002IN_0_1")
		(symbol "MSP430F2002IN_1_1"
			(pin input line
				(at -25.4 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA1")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 24.13 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 24.13 7.62 180)
				(length 3.81)
				(name "A0/TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 24.13 5.08 180)
				(length 3.81)
				(name "A1/TA0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 24.13 2.54 180)
				(length 3.81)
				(name "A2/TA1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 24.13 0 180)
				(length 3.81)
				(name "ADC10CLK/A3/VREF-/VeREF-/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 24.13 -2.54 180)
				(length 3.81)
				(name "SMCLK/A4/VREF+/VeREF+/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 24.13 -5.08 180)
				(length 3.81)
				(name "TA0/A5/SCLK/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 24.13 -7.62 180)
				(length 3.81)
				(name "TA1/A6/SDO/SCL/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 24.13 -10.16 180)
				(length 3.81)
				(name "A7/SDI/SDA/TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2002IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2002IPW"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2002.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2002IPW_0_1")
		(symbol "MSP430F2002IPW_1_1"
			(pin input line
				(at -25.4 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA1")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 24.13 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 24.13 7.62 180)
				(length 3.81)
				(name "A0/TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 24.13 5.08 180)
				(length 3.81)
				(name "A1/TA0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 24.13 2.54 180)
				(length 3.81)
				(name "A2/TA1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 24.13 0 180)
				(length 3.81)
				(name "ADC10CLK/A3/VREF-/VeREF-/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 24.13 -2.54 180)
				(length 3.81)
				(name "SMCLK/A4/VREF+/VeREF+/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 24.13 -5.08 180)
				(length 3.81)
				(name "TA0/A5/SCLK/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 24.13 -7.62 180)
				(length 3.81)
				(name "TA1/A6/SDO/SCL/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 24.13 -10.16 180)
				(length 3.81)
				(name "A7/SDI/SDA/TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2002IRSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2002IRSA"
			(at 11.43 -17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -13.97 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2002.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2002IRSA_0_1")
		(symbol "MSP430F2002IRSA_1_1"
			(pin input line
				(at -25.4 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA1")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "AVCC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin input line
				(at 25.4 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "A0/TA0CLK/ACLK/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "A1/TA0/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "A2/TA1/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "ADC10CLK/A3/VREF-/VeREF-/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "SMCLK/A4/VREF+/VeREF+/TCK/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "TA0/A5/SCLK/TMS/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "TA1/A6/SDO/SCL/TDI/TCLK/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "A7/SDI/SDA/TDO/TDI/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2003IN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2003IN"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2003.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2003IN_0_1")
		(symbol "MSP430F2003IN_1_1"
			(pin input line
				(at -25.4 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA1")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 25.4 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "TACLK/ACLK/A0+/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TA0/A0-/A4+/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "TA1/A1+/A4-/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "VREF/A1-/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "SMCLK/A2+/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "TA0/A2-/SCLK/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "TA1/A3+/SDO/SCL/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "A3-/SDI/SDA/TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2003IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2003IPW"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2003.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2003IPW_0_1")
		(symbol "MSP430F2003IPW_1_1"
			(pin input line
				(at -24.13 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -24.13 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA1")
				(number "13")
			)
			(pin bidirectional line
				(at -24.13 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 25.4 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "TACLK/ACLK/A0+/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TA0/A0-/A4+/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "TA1/A1+/A4-/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "VREF/A1-/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "SMCLK/A2+/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "TA0/A2-/SCLK/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "TA1/A3+/SDO/SCL/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "A3-/SDI/SDA/TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2003IRSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2003IRSA"
			(at 11.43 -17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -13.97 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2003.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2003IRSA_0_1")
		(symbol "MSP430F2003IRSA_1_1"
			(pin input line
				(at -25.4 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA1")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "AVCC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin input line
				(at 25.4 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "TACLK/ACLK/A0+/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TA0/A0-/A4+/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "TA1/A1+/A4-/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "VREF/A1-/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "SMCLK/A2+/TCK/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "TA0/A2-/SCLK/TMS/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "TA1/A3+/SDO/SCL/TDI/TCLK/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "A3-/SDI/SDA/TDO/TDI/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2101IDGV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2101IDGV"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2101.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, TVSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2101IDGV_0_1")
		(symbol "MSP430F2101IDGV_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P2.0/ACLK/CA2")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P2.1/INCLK/CA3")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P2.2/CAOUT/TA0/CA4")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P2.3/TA1/CA0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P2.4/TA2/CA1")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.5/CA5")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/CA6")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT/CA7")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -16.51 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "TA1/TCLK/TDI/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "TA2/TDI/TDO/P1.7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2101IDW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2101IDW"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2101.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, SOWB-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2101IDW_0_1")
		(symbol "MSP430F2101IDW_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P2.0/ACLK/CA2")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P2.1/INCLK/CA3")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P2.2/CAOUT/TA0/CA4")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P2.3/TA1/CA0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P2.4/TA2/CA1")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.5/CA5")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/CA6")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT/CA7")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -16.51 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "TA1/TCLK/TDI/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "TA2/TDI/TDO/P1.7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2101IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2101IPW"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2101.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2101IPW_0_1")
		(symbol "MSP430F2101IPW_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P2.0/ACLK/CA2")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P2.1/INCLK/CA3")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P2.2/CAOUT/TA0/CA4")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P2.3/TA1/CA0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P2.4/TA2/CA1")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.5/CA5")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/CA6")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT/CA7")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -16.51 90)
				(length 3.81)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "TA1/TCLK/TDI/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "TA2/TDI/TDO/P1.7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2101IRGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2101IRGE"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2101.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB + 256B Flash, 128B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2101IRGE_0_1")
		(symbol "MSP430F2101IRGE_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P2.0/ACLK/CA2")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P2.1/INCLK/CA3")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P2.2/CAOUT/TA0/CA4")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P2.3/TA1/CA0")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P2.4/TA2/CA1")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.5/CA5")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/CA6")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT/CA7")
				(number "3")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at 0 -16.51 90)
				(length 3.81)
				(name "VSS")
				(number "2")
			)
			(pin input line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "TEST")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "TA1/TCLK/TDI/P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "TA2/TDI/TDO/P1.7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2112IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 25.4 0)
		)
		(property "Value" "MSP430F2112IPW"
			(at 15.24 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -19.05 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2112.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2112IPW_0_1")
		(symbol "MSP430F2112IPW_1_1"
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "16")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "P3.6/A6/TA1.0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "P3.7/A7/TA1.1")
				(number "18")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "4")
			)
			(pin input line
				(at 30.48 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "CAOUT/TACLK/ADC10CLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TA1.0/TA0.0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "TA0.0/TMS/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TA0.1/TDI/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "TA0.2/TDI/TDO/P1.7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 -3.81 180)
				(length 3.81)
				(name "CA2/ACLK/A0/P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -6.35 180)
				(length 3.81)
				(name "CA3/TAINCLK/SMCLK/A1/P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -8.89 180)
				(length 3.81)
				(name "CAOUT/CA4/TA0.0/A2/P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -11.43 180)
				(length 3.81)
				(name "CA0/TA0.1/A3/VREF-/VeREF-/P2.3")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 -13.97 180)
				(length 3.81)
				(name "CA1/TA0.2/A4/VREF+/VeREF+/P2.4")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -16.51 180)
				(length 3.81)
				(name "CA5/Rosc/P2.5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -19.05 180)
				(length 3.81)
				(name "CA6/XIN/P2.6")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -21.59 180)
				(length 3.81)
				(name "CA7/XOUT/P2.7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2112IRHB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 25.4 0)
		)
		(property "Value" "MSP430F2112IRHB"
			(at 13.97 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -19.05 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2112.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2112IRHB_0_1")
		(symbol "MSP430F2112IRHB_1_1"
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "P3.6/A6/TA1.0")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "P3.7/A7/TA1.1")
				(number "16")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "30")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "1")
			)
			(pin input line
				(at 30.48 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "CAOUT/TACLK/ADC10CLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TA1.0/TA0.0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "TA0.0/TMS/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TA0.1/TDI/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "TA0.2/TDI/TDO/P1.7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 -3.81 180)
				(length 3.81)
				(name "CA2/ACLK/A0/P2.0")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -6.35 180)
				(length 3.81)
				(name "CA3/TAINCLK/SMCLK/A1/P2.1")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -8.89 180)
				(length 3.81)
				(name "CAOUT/CA4/TA0.0/A2/P2.2")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -11.43 180)
				(length 3.81)
				(name "CA0/TA0.1/A3/VREF-/VeREF-/P2.3")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -13.97 180)
				(length 3.81)
				(name "CA1/TA0.2/A4/VREF+/VeREF+/P2.4")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 -16.51 180)
				(length 3.81)
				(name "CA5/Rosc/P2.5")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -19.05 180)
				(length 3.81)
				(name "CA6/XIN/P2.6")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -21.59 180)
				(length 3.81)
				(name "CA7/XOUT/P2.7")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2112IRTV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 25.4 0)
		)
		(property "Value" "MSP430F2112IRTV"
			(at 13.97 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -19.05 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2112.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2112IRTV_0_1")
		(symbol "MSP430F2112IRTV_1_1"
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "P3.6/A6/TA1.0")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "P3.7/A7/TA1.1")
				(number "16")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "30")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "1")
			)
			(pin input line
				(at 30.48 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "CAOUT/TACLK/ADC10CLK/P1.0")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TA1.0/TA0.0/P1.1")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "TA0.0/TMS/P1.5")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TA0.1/TDI/P1.6")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "TA0.2/TDI/TDO/P1.7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 -3.81 180)
				(length 3.81)
				(name "CA2/ACLK/A0/P2.0")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -6.35 180)
				(length 3.81)
				(name "CA3/TAINCLK/SMCLK/A1/P2.1")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -8.89 180)
				(length 3.81)
				(name "CAOUT/CA4/TA0.0/A2/P2.2")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -11.43 180)
				(length 3.81)
				(name "CA0/TA0.1/A3/VREF-/VeREF-/P2.3")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -13.97 180)
				(length 3.81)
				(name "CA1/TA0.2/A4/VREF+/VeREF+/P2.4")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 -16.51 180)
				(length 3.81)
				(name "CA5/Rosc/P2.5")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -19.05 180)
				(length 3.81)
				(name "CA6/XIN/P2.6")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -21.59 180)
				(length 3.81)
				(name "CA7/XOUT/P2.7")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2232IDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2232IDA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2232.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2232IDA_0_1")
		(symbol "MSP430F2232IDA_1_1"
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P3.6/A6")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "P3.7/A7")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 -11.43 0)
				(length 3.81)
				(name "P4.3/TB0/A12")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 -13.97 0)
				(length 3.81)
				(name "P4.4/TB1/A13")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -16.51 0)
				(length 3.81)
				(name "P4.5/TB2/A14")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 -19.05 0)
				(length 3.81)
				(name "P4.6/TBOUTH/A15")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 -21.59 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "24")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "15")
			)
			(pin input line
				(at 30.48 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TA1/TDI/P1.6")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "TA2/TDI/TDO/P1.7")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 -3.81 180)
				(length 3.81)
				(name "ACLK/A0/P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -6.35 180)
				(length 3.81)
				(name "TAINCLK/SMCLK/A1/P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -8.89 180)
				(length 3.81)
				(name "TA0/A2/P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -11.43 180)
				(length 3.81)
				(name "TA1/A3/VREF-/VeREF-/P2.3")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -13.97 180)
				(length 3.81)
				(name "TA2/A4/VREF+/VeREF+/P2.4")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 -16.51 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2232IRHA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2232IRHA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2232.pdf"
			(at -22.86 -27.94 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
		(symbol "MSP430F2232IRHA_0_1")
		(symbol "MSP430F2232IRHA_1_1"
			(pin input line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P3.6/A6")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "P3.7/A7")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "16")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 -11.43 0)
				(length 3.81)
				(name "P4.3/TB0/A12")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 -13.97 0)
				(length 3.81)
				(name "P4.4/TB1/A13")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 -16.51 0)
				(length 3.81)
				(name "P4.5/TB2/A14")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 -19.05 0)
				(length 3.81)
				(name "P4.6/TBOUTH/A15")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -21.59 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "22")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "38")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "1")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "39")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin input line
				(at 30.48 21.59 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "P1.0/TACLK/ADC10CLK")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TA1/TDI/TCLK/P1.6")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "TA2/TDO/TDI/P1.7")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 -3.81 180)
				(length 3.81)
				(name "ACLK/A0/P2.0")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -6.35 180)
				(length 3.81)
				(name "TAINCLK/SMCLK/A1/P2.1")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -8.89 180)
				(length 3.81)
				(name "TA0/A2/P2.2")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -11.43 180)
				(length 3.81)
				(name "TA1/VREF-/VeREF-/A3/P2.3")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 -13.97 180)
				(length 3.81)
				(name "TA2/VREF+/VeREF+/A4/P2.4")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 -16.51 180)
				(length 3.81)
				(name "ROSC/P2.5")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2232IYFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 25.4 0)
		)
		(property "Value" "MSP430F2232IYFF"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -27.94 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2232.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2232IYFF_0_1")
		(symbol "MSP430F2232IYFF_1_1"
			(pin input line
				(at -36.83 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "B3")
			)
			(pin bidirectional line
				(at -36.83 17.78 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "B5")
			)
			(pin bidirectional line
				(at -36.83 15.24 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "A6")
			)
			(pin bidirectional line
				(at -36.83 12.7 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "A7")
			)
			(pin bidirectional line
				(at -36.83 10.16 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "B6")
			)
			(pin bidirectional line
				(at -36.83 7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "G6")
			)
			(pin bidirectional line
				(at -36.83 5.08 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "G5")
			)
			(pin bidirectional line
				(at -36.83 2.54 0)
				(length 3.81)
				(name "P3.6/A6")
				(number "F4")
			)
			(pin bidirectional line
				(at -36.83 0 0)
				(length 3.81)
				(name "P3.7/A7")
				(number "G4")
			)
			(pin bidirectional line
				(at -36.83 -3.81 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "D6")
			)
			(pin bidirectional line
				(at -36.83 -6.35 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "D7")
			)
			(pin bidirectional line
				(at -36.83 -8.89 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "E6")
			)
			(pin bidirectional line
				(at -36.83 -11.43 0)
				(length 3.81)
				(name "P4.3/TB0/A12")
				(number "E7")
			)
			(pin bidirectional line
				(at -36.83 -13.97 0)
				(length 3.81)
				(name "P4.4/TB1/A13")
				(number "F7")
			)
			(pin bidirectional line
				(at -36.83 -16.51 0)
				(length 3.81)
				(name "P4.5/TB2/A14")
				(number "F6")
			)
			(pin bidirectional line
				(at -36.83 -19.05 0)
				(length 3.81)
				(name "P4.6/TBOUTH/A15")
				(number "G7")
			)
			(pin bidirectional line
				(at -36.83 -21.59 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "F5")
			)
			(pin power_in line
				(at -12.7 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "C1")
			)
			(pin power_in line
				(at -12.7 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "A3")
			)
			(pin power_in line
				(at -10.16 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "D3")
			)
			(pin power_in line
				(at -10.16 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "B1")
			)
			(pin power_in line
				(at -7.62 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "D4")
			)
			(pin power_in line
				(at -7.62 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "B2")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "E4")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "C3")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "E5")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "C4")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "C6")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "B7")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "C7")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "C5")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "D5")
			)
			(pin input line
				(at 34.29 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "D1")
			)
			(pin bidirectional line
				(at 34.29 17.78 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "F2")
			)
			(pin bidirectional line
				(at 34.29 15.24 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "G2")
			)
			(pin bidirectional line
				(at 34.29 12.7 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "E2")
			)
			(pin bidirectional line
				(at 34.29 10.16 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "G1")
			)
			(pin bidirectional line
				(at 34.29 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "F1")
			)
			(pin bidirectional line
				(at 34.29 5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "E1")
			)
			(pin bidirectional line
				(at 34.29 2.54 180)
				(length 3.81)
				(name "TA1/TDI/TCLK/P1.6")
				(number "E3")
			)
			(pin bidirectional line
				(at 34.29 0 180)
				(length 3.81)
				(name "TA2/TDO/TDI/P1.7")
				(number "D2")
			)
			(pin bidirectional line
				(at 34.29 -3.81 180)
				(length 3.81)
				(name "ACLK/A0/P2.0")
				(number "A4")
			)
			(pin bidirectional line
				(at 34.29 -6.35 180)
				(length 3.81)
				(name "TAINCLK/SMCLK/A1/P2.1")
				(number "B4")
			)
			(pin bidirectional line
				(at 34.29 -8.89 180)
				(length 3.81)
				(name "TA0/A2/P2.2")
				(number "A5")
			)
			(pin bidirectional line
				(at 34.29 -11.43 180)
				(length 3.81)
				(name "TA1/VREF-/VeREF-/A3/P2.3")
				(number "F3")
			)
			(pin bidirectional line
				(at 34.29 -13.97 180)
				(length 3.81)
				(name "TA2/VREF+/VeREF+/A4/P2.4")
				(number "G3")
			)
			(pin bidirectional line
				(at 34.29 -16.51 180)
				(length 3.81)
				(name "ROSC/P2.5")
				(number "C2")
			)
			(pin bidirectional line
				(at 34.29 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "A2")
			)
			(pin bidirectional line
				(at 34.29 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "A1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2234IDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2234IDA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2234.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2234IDA_0_1")
		(symbol "MSP430F2234IDA_1_1"
			(pin bidirectional line
				(at -35.56 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "11")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "12")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "13")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "14")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "25")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 3.81)
				(name "P3.6/A6/OA0I2")
				(number "27")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 3.81)
				(name "P3.7/A7/OA1I2")
				(number "28")
			)
			(pin bidirectional line
				(at -35.56 -3.81 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "17")
			)
			(pin bidirectional line
				(at -35.56 -6.35 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "18")
			)
			(pin bidirectional line
				(at -35.56 -8.89 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 -11.43 0)
				(length 3.81)
				(name "P4.3/TB0/A12/OA0O")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 -13.97 0)
				(length 3.81)
				(name "P4.4/TB1/A13/OA1O")
				(number "21")
			)
			(pin bidirectional line
				(at -35.56 -16.51 0)
				(length 3.81)
				(name "P4.5/TB2/A14/OA0I3")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 -19.05 0)
				(length 3.81)
				(name "P4.6/TBOUTH/A15/OA1I3")
				(number "23")
			)
			(pin bidirectional line
				(at -35.56 -21.59 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "24")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "15")
			)
			(pin input line
				(at 35.56 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "31")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "32")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "33")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "34")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "35")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "36")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "TA1/TDI/P1.6")
				(number "37")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 3.81)
				(name "TA2/TDI/TDO/P1.7")
				(number "38")
			)
			(pin bidirectional line
				(at 35.56 -3.81 180)
				(length 3.81)
				(name "ACLK/A0/OA0I0/P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at 35.56 -6.35 180)
				(length 3.81)
				(name "TAINCLK/SMCLK/A1/OA0O/P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at 35.56 -8.89 180)
				(length 3.81)
				(name "TA0/A2/OA0I1/P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at 35.56 -11.43 180)
				(length 3.81)
				(name "TA1/A3/VREF-/VeREF-/OA1I1/OA1O/P2.3")
				(number "29")
			)
			(pin bidirectional line
				(at 35.56 -13.97 180)
				(length 3.81)
				(name "TA2/A4/VREF+/VeREF+/OA1I0/P2.4")
				(number "30")
			)
			(pin bidirectional line
				(at 35.56 -16.51 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "3")
			)
			(pin bidirectional line
				(at 35.56 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "6")
			)
			(pin bidirectional line
				(at 35.56 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2234IRHA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2234IRHA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2234.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
		(symbol "MSP430F2234IRHA_0_1")
		(symbol "MSP430F2234IRHA_1_1"
			(pin bidirectional line
				(at -36.83 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "5")
			)
			(pin bidirectional line
				(at -36.83 17.78 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "9")
			)
			(pin bidirectional line
				(at -36.83 15.24 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "10")
			)
			(pin bidirectional line
				(at -36.83 12.7 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -36.83 10.16 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "12")
			)
			(pin bidirectional line
				(at -36.83 7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "23")
			)
			(pin bidirectional line
				(at -36.83 5.08 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "24")
			)
			(pin bidirectional line
				(at -36.83 2.54 0)
				(length 3.81)
				(name "P3.6/A6/OA0I2")
				(number "25")
			)
			(pin bidirectional line
				(at -36.83 0 0)
				(length 3.81)
				(name "P3.7/A7/OA1I2")
				(number "26")
			)
			(pin bidirectional line
				(at -36.83 -3.81 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "15")
			)
			(pin bidirectional line
				(at -36.83 -6.35 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "16")
			)
			(pin bidirectional line
				(at -36.83 -8.89 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "17")
			)
			(pin bidirectional line
				(at -36.83 -11.43 0)
				(length 3.81)
				(name "P4.3/TB0/A12/OA0O")
				(number "18")
			)
			(pin bidirectional line
				(at -36.83 -13.97 0)
				(length 3.81)
				(name "P4.4/TB1/A13/OA1O")
				(number "19")
			)
			(pin bidirectional line
				(at -36.83 -16.51 0)
				(length 3.81)
				(name "P4.5/TB2/A14/OA0I3")
				(number "20")
			)
			(pin bidirectional line
				(at -36.83 -19.05 0)
				(length 3.81)
				(name "P4.6/TBOUTH/A15/OA1I3")
				(number "21")
			)
			(pin bidirectional line
				(at -36.83 -21.59 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "22")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "38")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "1")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "39")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin input line
				(at 35.56 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "37")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "29")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "30")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "31")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "32")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "33")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "34")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "TA1/TDI/P1.6")
				(number "35")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 3.81)
				(name "TA2/TDI/TDO/P1.7")
				(number "36")
			)
			(pin bidirectional line
				(at 35.56 -3.81 180)
				(length 3.81)
				(name "ACLK/A0/OA0I0/P2.0")
				(number "6")
			)
			(pin bidirectional line
				(at 35.56 -6.35 180)
				(length 3.81)
				(name "TAINCLK/SMCLK/A1/OA0O/P2.1")
				(number "7")
			)
			(pin bidirectional line
				(at 35.56 -8.89 180)
				(length 3.81)
				(name "TA0/A2/OA0I1/P2.2")
				(number "8")
			)
			(pin bidirectional line
				(at 35.56 -11.43 180)
				(length 3.81)
				(name "TA1/A3/VREF-/VeREF-/OA1I1/OA1O/P2.3")
				(number "27")
			)
			(pin bidirectional line
				(at 35.56 -13.97 180)
				(length 3.81)
				(name "TA2/A4/VREF+/VeREF+/OA1I0/P2.4")
				(number "28")
			)
			(pin bidirectional line
				(at 35.56 -16.51 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "40")
			)
			(pin bidirectional line
				(at 35.56 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "3")
			)
			(pin bidirectional line
				(at 35.56 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2234IYFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 25.4 0)
		)
		(property "Value" "MSP430F2234IYFF"
			(at 26.67 -25.4 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2234.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2234IYFF_0_1")
		(symbol "MSP430F2234IYFF_1_1"
			(pin input line
				(at -38.1 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "B3")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "B5")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "A7")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "G6")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "G5")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "P3.6/A6/OA0I2")
				(number "F4")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "P3.7/A7/OA1I2")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 -3.81 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "D6")
			)
			(pin bidirectional line
				(at -38.1 -6.35 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 -8.89 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "E6")
			)
			(pin bidirectional line
				(at -38.1 -11.43 0)
				(length 3.81)
				(name "P4.3/TB0/A12/OA0O")
				(number "E7")
			)
			(pin bidirectional line
				(at -38.1 -13.97 0)
				(length 3.81)
				(name "P4.4/TB1/A13/OA1O")
				(number "F7")
			)
			(pin bidirectional line
				(at -38.1 -16.51 0)
				(length 3.81)
				(name "P4.5/TB2/A14/OA0I3")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -19.05 0)
				(length 3.81)
				(name "P4.6/TBOUTH/A15/OA1I3")
				(number "G7")
			)
			(pin bidirectional line
				(at -38.1 -21.59 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "F5")
			)
			(pin power_in line
				(at -7.62 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "C1")
			)
			(pin power_in line
				(at -7.62 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "A3")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "D3")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "D4")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "B2")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "E4")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "C3")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "C4")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "C6")
			)
			(pin power_in line
				(at 7.62 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "B7")
			)
			(pin power_in line
				(at 10.16 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "C7")
			)
			(pin power_in line
				(at 10.16 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "C5")
			)
			(pin power_in line
				(at 12.7 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "D5")
			)
			(pin input line
				(at 38.1 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "G2")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "E2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "G1")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "TA0/TMS/P1.5")
				(number "E1")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "TA1/TDI/TCLK/P1.6")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "TA2/TDO/TDI/P1.7")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 -3.81 180)
				(length 3.81)
				(name "ACLK/A0/OA0I0/A0/P2.0")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 -6.35 180)
				(length 3.81)
				(name "TAINCLK/SMCLK/OA0O/A1/P2.1")
				(number "B4")
			)
			(pin bidirectional line
				(at 38.1 -8.89 180)
				(length 3.81)
				(name "TA0/OA0I1/A2/P2.2")
				(number "A5")
			)
			(pin bidirectional line
				(at 38.1 -11.43 180)
				(length 3.81)
				(name "TA1/VREF-/VeREF-/OA1I1/OA1O/A3/P2.3")
				(number "F3")
			)
			(pin bidirectional line
				(at 38.1 -13.97 180)
				(length 3.81)
				(name "TA2/VREF+/VeREF+/OA1I0/A4/P2.4")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 -16.51 180)
				(length 3.81)
				(name "ROSC/P2.5")
				(number "C2")
			)
			(pin bidirectional line
				(at 38.1 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "A2")
			)
			(pin bidirectional line
				(at 38.1 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "A1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2330IRHA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "MSP430F2330IRHA"
			(at 12.7 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -16.51 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2330.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 1kB RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
		(symbol "MSP430F2330IRHA_0_1")
		(symbol "MSP430F2330IRHA_1_1"
			(pin input line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 13.97 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 8.89 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 6.35 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 3.81 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 1.27 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -1.27 0)
				(length 3.81)
				(name "P3.6")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -3.81 0)
				(length 3.81)
				(name "P3.7")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "P4.3/TB0")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "P4.4/TB1")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "P4.5/TB2")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "P4.6/TBOUTH/ACLK")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "33")
			)
			(pin power_in line
				(at -2.54 31.75 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -31.75 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 2.54 31.75 270)
				(length 3.81)
				(name "AVCC")
				(number "40")
			)
			(pin input line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "TCK")
				(number "37")
			)
			(pin input line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "TDI/TCLK")
				(number "35")
			)
			(pin input line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "TMS")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "TDO/TDI")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 13.97 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 8.89 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 6.35 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 3.81 180)
				(length 3.81)
				(name "SMCLK/P1.4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 1.27 180)
				(length 3.81)
				(name "TA0/P1.5")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -1.27 180)
				(length 3.81)
				(name "TA1/P1.6")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -3.81 180)
				(length 3.81)
				(name "TA2/P1.7")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "ACLK/CA2/P2.0")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "TAINCLK/CA3/P2.1")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "TA0/CAOUT/CA4/P2.2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "TA1/CA0/P2.3")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "TA2/CA1/P2.4")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "ROSC/CA5/P2.5")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "XIN/CA6/P2.6")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "XOUT/CA7/P2.7")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2330IYFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "MSP430F2330IYFF"
			(at 12.7 -29.21 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -16.51 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2330.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 1kB RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2330IYFF_0_1")
		(symbol "MSP430F2330IYFF_1_1"
			(pin input line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "C2")
			)
			(pin bidirectional line
				(at -22.86 13.97 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK")
				(number "E6")
			)
			(pin bidirectional line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "F7")
			)
			(pin bidirectional line
				(at -22.86 8.89 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "F6")
			)
			(pin bidirectional line
				(at -22.86 6.35 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "G7")
			)
			(pin bidirectional line
				(at -22.86 3.81 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "G6")
			)
			(pin bidirectional line
				(at -22.86 1.27 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "G5")
			)
			(pin bidirectional line
				(at -22.86 -1.27 0)
				(length 3.81)
				(name "P3.6")
				(number "F5")
			)
			(pin bidirectional line
				(at -22.86 -3.81 0)
				(length 3.81)
				(name "P3.7")
				(number "G4")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "F4")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "G3")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "G2")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "P4.3/TB0")
				(number "F3")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "P4.4/TB1")
				(number "G1")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "P4.5/TB2")
				(number "F1")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "P4.6/TBOUTH/ACLK")
				(number "F2")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 31.75 270)
				(length 3.81)
				(name "DVCC")
				(number "B3")
			)
			(pin power_in line
				(at 0 -31.75 90)
				(length 3.81)
				(name "VSS")
				(number "B1")
			)
			(pin power_in line
				(at 2.54 31.75 270)
				(length 3.81)
				(name "AVCC")
				(number "A1")
			)
			(pin input line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "TCK")
				(number "C1")
			)
			(pin input line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "TDI/TCLK")
				(number "D1")
			)
			(pin input line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "TMS")
				(number "D2")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "TDO/TDI")
				(number "E1")
			)
			(pin bidirectional line
				(at 22.86 13.97 180)
				(length 3.81)
				(name "TACLK/P1.0")
				(number "B4")
			)
			(pin bidirectional line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "C4")
			)
			(pin bidirectional line
				(at 22.86 8.89 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "A5")
			)
			(pin bidirectional line
				(at 22.86 6.35 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "B5")
			)
			(pin bidirectional line
				(at 22.86 3.81 180)
				(length 3.81)
				(name "SMCLK/P1.4")
				(number "A6")
			)
			(pin bidirectional line
				(at 22.86 1.27 180)
				(length 3.81)
				(name "TA0/P1.5")
				(number "B6")
			)
			(pin bidirectional line
				(at 22.86 -1.27 180)
				(length 3.81)
				(name "TA1/P1.6")
				(number "A7")
			)
			(pin bidirectional line
				(at 22.86 -3.81 180)
				(length 3.81)
				(name "TA2/P1.7")
				(number "B7")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "ACLK/CA2/P2.0")
				(number "C5")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "TAINCLK/CA3/P2.1")
				(number "C7")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "TA0/CAOUT/CA4/P2.2")
				(number "C6")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "TA1/CA0/P2.3")
				(number "D7")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "TA2/CA1/P2.4")
				(number "D6")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "ROSC/CA5/P2.5")
				(number "E7")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "XIN/CA6/P2.6")
				(number "A2")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "XOUT/CA7/P2.7")
				(number "A3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F2618-EP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 53.34 0)
		)
		(property "Value" "MSP430F2618-EP"
			(at 20.32 53.34 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -67.31 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2618-ep.pdf"
			(at -8.89 22.86 0)
		)
		(property "Description" "116kB + 256B Flash, 8K RAM, 113-BGA"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F2618-EP_0_1")
		(symbol "MSP430F2618-EP_1_1"
			(pin input line
				(at -33.02 48.26 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "B5")
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 3.81)
				(name "P1.0/TACLK/CAOUT")
				(number "G2")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 3.81)
				(name "P1.1/TA0")
				(number "H1")
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 3.81)
				(name "P1.2/TA1")
				(number "H2")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 3.81)
				(name "P1.3/TA2")
				(number "J1")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "P1.4/SMCLK")
				(number "J2")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 3.81)
				(name "P1.5/TA0")
				(number "K1")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 3.81)
				(name "P1.6/TA1")
				(number "K2")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 3.81)
				(name "P1.7/TA2")
				(number "L1")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 3.81)
				(name "P2.0/ACLK/CA2")
				(number "M1")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "P2.1/TAINCLK/CA3")
				(number "M2")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "P2.2/CAOUT/TA0/CA4")
				(number "M3")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "P2.3/CA0/TA1")
				(number "L3")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "P2.4/CA1/TA2")
				(number "L4")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "P2.5/Rosc/CA5")
				(number "M4")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P2.6/ADC12CLK/DMAE0/CA6")
				(number "J4")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P2.7/TA0/CA7")
				(number "L5")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK")
				(number "M5")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "L6")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "M6")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "L7")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "M7")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "L8")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "P3.6/UCA1TXD/UCA1SIMO")
				(number "M8")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "P3.7/UCA1RXD/UCA1SOMI")
				(number "L9")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "M9")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "J9")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "M10")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 3.81)
				(name "P4.3/TB3")
				(number "L10")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 3.81)
				(name "P4.4/TB4")
				(number "M11")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 3.81)
				(name "P4.5/TB5")
				(number "M12")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 3.81)
				(name "P4.6/TB6")
				(number "L12")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "K11")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 3.81)
				(name "VeREF+/DAC0")
				(number "F2")
			)
			(pin output line
				(at -33.02 -45.72 0)
				(length 3.81)
				(name "XOUT")
				(number "F1")
			)
			(pin input line
				(at -33.02 -48.26 0)
				(length 3.81)
				(name "XIN")
				(number "E1")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 3.81)
				(name "VREF+")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 3.81)
				(name "DVCC")
				(number "F12")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 3.81)
				(name "DVSS")
				(number "A3")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "B11")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "D5")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "D6")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "D7")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "D8")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "E12")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "E4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "E5")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "E6")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "E7")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "E8")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "E9")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "F4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "F5")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "F8")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "F9")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "G4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "G5")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "G8")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "G9")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "H4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "H5")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "H6")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "H7")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "H8")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "H9")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "J5")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "J6")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "J7")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "J8")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "L11")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "DVSS")
				(number "L2")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 3.81)
				(name "DVCC")
				(number "A1")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 3.81)
				(name "AVSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "AVSS")
				(number "B3")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 3.81)
				(name "AVCC")
				(number "A2")
			)
			(pin bidirectional line
				(at 2.54 -55.88 90)
				(length 3.81)
				(name "VREF-/VeREF-")
				(number "G1")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "UCA1CLK/UCB1STE/P5.0")
				(number "K12")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "UCB1SDA/UCB1SIMO/P5.1")
				(number "J11")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "UCB1SCL/UCB1SOMI/P5.2")
				(number "J12")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "UCA1STE/UCB1CLK/P5.3")
				(number "H11")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "MCLK/P5.4")
				(number "H12")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "SMCLK/P5.5")
				(number "G11")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "ACLK/P5.6")
				(number "G12")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "SVSOUT/TBOUTH/P5.7")
				(number "F11")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "A0/P6.0")
				(number "D4")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "A1/P6.1")
				(number "A4")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "A2/P6.2")
				(number "B4")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "A3/P6.3")
				(number "B1")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "P6.4/A4")
				(number "C1")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "DAC1/A5/P6.5")
				(number "C2")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(hide yes)
				(name "DAC1/A5/P6.5")
				(number "C3")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "DAC0/A6/P6.6")
				(number "D1")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "SVSIN/DAC1/A7/P6.7")
				(number "D2")
			)
			(pin power_in line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "P7.0")
				(number "E11")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "P7.1")
				(number "D12")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "P7.2")
				(number "D11")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "P7.3")
				(number "C12")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "P7.4")
				(number "C11")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "P7.5")
				(number "B12")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "P7.6")
				(number "A12")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "P7.7")
				(number "A11")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "P8.0")
				(number "B10")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "P8.1")
				(number "A10")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "P8.2")
				(number "D9")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "P8.3")
				(number "A9")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "P8.4")
				(number "B9")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "P8.5")
				(number "B8")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "XT2OUT/P8.6")
				(number "A8")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "XT2IN/P8.7")
				(number "A7")
			)
			(pin input line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "TCK")
				(number "A5")
			)
			(pin input line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "TDI/TCLK")
				(number "A6")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "TDO/TDI")
				(number "B7")
			)
			(pin input line
				(at 33.02 -48.26 180)
				(length 3.81)
				(name "TMS")
				(number "B6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5217IRGC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5217IRGC"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5217.pdf"
			(at 0 0 0)
		)
		(property "Description" "64kB Flash, 8kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
		(symbol "MSP430F5217IRGC_0_1")
		(symbol "MSP430F5217IRGC_1_1"
			(pin bidirectional line
				(at -30.48 39.37 0)
				(length 3.81)
				(name "~{RSTDVCC}/SBWTDIO")
				(number "64")
			)
			(pin input line
				(at -30.48 36.83 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 31.75 0)
				(length 3.81)
				(name "BSLEN")
				(number "55")
			)
			(pin bidirectional line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 24.13 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P7.0/TB0.0")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P7.1/TB0.1")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P7.2/TB0.2")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P7.3/TB0.3")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P7.4/TB0.4")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P7.5/TB0.5")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/CB0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/CB1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/CB2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/CB3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -11.43 0)
				(length 3.81)
				(name "P6.4/CB4")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -13.97 0)
				(length 3.81)
				(name "P6.5/CB5")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -16.51 0)
				(length 3.81)
				(name "P6.6/CB6")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 -19.05 0)
				(length 3.81)
				(name "P6.7/CB7")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.0")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.1")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "13")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 3.81)
				(name "AVCC")
				(number "11")
			)
			(pin power_in line
				(at -3.81 -45.72 90)
				(length 3.81)
				(name "AVSS")
				(number "14")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "DVCC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "VCORE")
				(number "17")
			)
			(pin power_in line
				(at 3.81 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "16")
			)
			(pin power_in line
				(at 6.35 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "39")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 3.81)
				(name "DVIO")
				(number "40")
			)
			(pin input line
				(at 29.21 39.37 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "59")
			)
			(pin bidirectional line
				(at 29.21 35.56 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "18")
			)
			(pin bidirectional line
				(at 29.21 33.02 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "19")
			)
			(pin bidirectional line
				(at 29.21 30.48 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "20")
			)
			(pin bidirectional line
				(at 29.21 27.94 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "21")
			)
			(pin bidirectional line
				(at 29.21 25.4 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "22")
			)
			(pin bidirectional line
				(at 29.21 22.86 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "23")
			)
			(pin bidirectional line
				(at 29.21 20.32 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "24")
			)
			(pin bidirectional line
				(at 29.21 17.78 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "25")
			)
			(pin bidirectional line
				(at 29.21 13.97 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "26")
			)
			(pin bidirectional line
				(at 29.21 11.43 180)
				(length 3.81)
				(name "TA1.2/P2.1")
				(number "27")
			)
			(pin bidirectional line
				(at 29.21 8.89 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P2.2")
				(number "28")
			)
			(pin bidirectional line
				(at 29.21 6.35 180)
				(length 3.81)
				(name "TA2.0/P2.3")
				(number "29")
			)
			(pin bidirectional line
				(at 29.21 3.81 180)
				(length 3.81)
				(name "TA2.1/P2.4")
				(number "30")
			)
			(pin bidirectional line
				(at 29.21 1.27 180)
				(length 3.81)
				(name "TA2.2/P2.5")
				(number "31")
			)
			(pin bidirectional line
				(at 29.21 -1.27 180)
				(length 3.81)
				(name "RTCCLK/DMAE0/P2.6")
				(number "32")
			)
			(pin bidirectional line
				(at 29.21 -3.81 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "33")
			)
			(pin bidirectional line
				(at 29.21 -7.62 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "34")
			)
			(pin bidirectional line
				(at 29.21 -10.16 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "35")
			)
			(pin bidirectional line
				(at 29.21 -12.7 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "36")
			)
			(pin bidirectional line
				(at 29.21 -15.24 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "37")
			)
			(pin bidirectional line
				(at 29.21 -17.78 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "38")
			)
			(pin bidirectional line
				(at 29.21 -21.59 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "41")
			)
			(pin bidirectional line
				(at 29.21 -24.13 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "42")
			)
			(pin bidirectional line
				(at 29.21 -26.67 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "43")
			)
			(pin bidirectional line
				(at 29.21 -29.21 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "44")
			)
			(pin bidirectional line
				(at 29.21 -31.75 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "45")
			)
			(pin bidirectional line
				(at 29.21 -34.29 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "46")
			)
			(pin bidirectional line
				(at 29.21 -36.83 180)
				(length 3.81)
				(name "P4.6")
				(number "47")
			)
			(pin bidirectional line
				(at 29.21 -39.37 180)
				(length 3.81)
				(name "P4.7")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5217IYFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5217IYFF"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-64_3.415x3.535mm_Layout8x8_P0.4mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5217.pdf"
			(at 0 0 0)
		)
		(property "Description" "64kB Flash, 8kB RAM, BGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.415x3.535mm*Layout8x8*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5217IYFF_0_1")
		(symbol "MSP430F5217IYFF_1_1"
			(pin bidirectional line
				(at -30.48 39.37 0)
				(length 3.81)
				(name "~{RSTDVCC}/SBWTDIO")
				(number "D4")
			)
			(pin input line
				(at -30.48 36.83 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "E3")
			)
			(pin bidirectional line
				(at -30.48 31.75 0)
				(length 3.81)
				(name "BSLEN")
				(number "E2")
			)
			(pin bidirectional line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "D2")
			)
			(pin bidirectional line
				(at -30.48 24.13 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "B1")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P7.0/TB0.0")
				(number "H1")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P7.1/TB0.1")
				(number "G2")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P7.2/TB0.2")
				(number "F3")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P7.3/TB0.3")
				(number "G1")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P7.4/TB0.4")
				(number "F2")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P7.5/TB0.5")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/CB0")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/CB1")
				(number "A1")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/CB2")
				(number "B2")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/CB3")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 -11.43 0)
				(length 3.81)
				(name "P6.4/CB4")
				(number "A2")
			)
			(pin bidirectional line
				(at -30.48 -13.97 0)
				(length 3.81)
				(name "P6.5/CB5")
				(number "B3")
			)
			(pin bidirectional line
				(at -30.48 -16.51 0)
				(length 3.81)
				(name "P6.6/CB6")
				(number "C4")
			)
			(pin bidirectional line
				(at -30.48 -19.05 0)
				(length 3.81)
				(name "P6.7/CB7")
				(number "A3")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.0")
				(number "B4")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.1")
				(number "A4")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "D1")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "A5")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "A6")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 3.81)
				(name "AVCC")
				(number "B5")
			)
			(pin power_in line
				(at -3.81 -45.72 90)
				(length 3.81)
				(name "AVSS")
				(number "B6")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "DVCC")
				(number "A7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "VCORE")
				(number "B8")
			)
			(pin power_in line
				(at 3.81 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "A8")
			)
			(pin power_in line
				(at 6.35 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "H6")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 3.81)
				(name "DVIO")
				(number "H5")
			)
			(pin input line
				(at 29.21 39.37 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "E4")
			)
			(pin bidirectional line
				(at 29.21 35.56 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "B7")
			)
			(pin bidirectional line
				(at 29.21 33.02 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "C7")
			)
			(pin bidirectional line
				(at 29.21 30.48 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "C8")
			)
			(pin bidirectional line
				(at 29.21 27.94 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "C6")
			)
			(pin bidirectional line
				(at 29.21 25.4 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "C5")
			)
			(pin bidirectional line
				(at 29.21 22.86 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "D8")
			)
			(pin bidirectional line
				(at 29.21 20.32 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "D7")
			)
			(pin bidirectional line
				(at 29.21 17.78 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "D6")
			)
			(pin bidirectional line
				(at 29.21 13.97 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "E8")
			)
			(pin bidirectional line
				(at 29.21 11.43 180)
				(length 3.81)
				(name "TA1.2/P2.1")
				(number "D5")
			)
			(pin bidirectional line
				(at 29.21 8.89 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P2.2")
				(number "E7")
			)
			(pin bidirectional line
				(at 29.21 6.35 180)
				(length 3.81)
				(name "TA2.0/P2.3")
				(number "F8")
			)
			(pin bidirectional line
				(at 29.21 3.81 180)
				(length 3.81)
				(name "TA2.1/P2.4")
				(number "J7")
			)
			(pin bidirectional line
				(at 29.21 1.27 180)
				(length 3.81)
				(name "TA2.2/P2.5")
				(number "F7")
			)
			(pin bidirectional line
				(at 29.21 -1.27 180)
				(length 3.81)
				(name "RTCCLK/DMAE0/P2.6")
				(number "G8")
			)
			(pin bidirectional line
				(at 29.21 -3.81 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "F6")
			)
			(pin bidirectional line
				(at 29.21 -7.62 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "H8")
			)
			(pin bidirectional line
				(at 29.21 -10.16 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "G7")
			)
			(pin bidirectional line
				(at 29.21 -12.7 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "G6")
			)
			(pin bidirectional line
				(at 29.21 -15.24 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "H7")
			)
			(pin bidirectional line
				(at 29.21 -17.78 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "G5")
			)
			(pin bidirectional line
				(at 29.21 -21.59 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "F5")
			)
			(pin bidirectional line
				(at 29.21 -24.13 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "H4")
			)
			(pin bidirectional line
				(at 29.21 -26.67 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "E5")
			)
			(pin bidirectional line
				(at 29.21 -29.21 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "G4")
			)
			(pin bidirectional line
				(at 29.21 -31.75 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "H3")
			)
			(pin bidirectional line
				(at 29.21 -34.29 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "F4")
			)
			(pin bidirectional line
				(at 29.21 -36.83 180)
				(length 3.81)
				(name "P4.6")
				(number "H2")
			)
			(pin bidirectional line
				(at 29.21 -39.37 180)
				(length 3.81)
				(name "P4.7")
				(number "G3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5227IRGC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5227IRGC"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5227.pdf"
			(at 0 0 0)
		)
		(property "Description" "64kB Flash, 8kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
		(symbol "MSP430F5227IRGC_0_1")
		(symbol "MSP430F5227IRGC_1_1"
			(pin bidirectional line
				(at -30.48 39.37 0)
				(length 3.81)
				(name "~{RSTDVCC}/SBWTDIO")
				(number "64")
			)
			(pin input line
				(at -30.48 36.83 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 31.75 0)
				(length 3.81)
				(name "BSLEN")
				(number "55")
			)
			(pin bidirectional line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 24.13 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P7.0/TB0.0")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P7.1/TB0.1")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P7.2/TB0.2")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P7.3/TB0.3")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P7.4/TB0.4")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P7.5/TB0.5")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -11.43 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -13.97 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -16.51 0)
				(length 3.81)
				(name "P6.6/CB6/A6")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 -19.05 0)
				(length 3.81)
				(name "P6.7/CB7/A7")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "13")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 3.81)
				(name "AVCC")
				(number "11")
			)
			(pin power_in line
				(at -3.81 -45.72 90)
				(length 3.81)
				(name "AVSS")
				(number "14")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "DVCC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "VCORE")
				(number "17")
			)
			(pin power_in line
				(at 3.81 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "16")
			)
			(pin power_in line
				(at 6.35 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "39")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 3.81)
				(name "DVIO")
				(number "40")
			)
			(pin input line
				(at 29.21 39.37 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "59")
			)
			(pin bidirectional line
				(at 29.21 35.56 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "18")
			)
			(pin bidirectional line
				(at 29.21 33.02 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "19")
			)
			(pin bidirectional line
				(at 29.21 30.48 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "20")
			)
			(pin bidirectional line
				(at 29.21 27.94 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "21")
			)
			(pin bidirectional line
				(at 29.21 25.4 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "22")
			)
			(pin bidirectional line
				(at 29.21 22.86 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "23")
			)
			(pin bidirectional line
				(at 29.21 20.32 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "24")
			)
			(pin bidirectional line
				(at 29.21 17.78 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "25")
			)
			(pin bidirectional line
				(at 29.21 13.97 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "26")
			)
			(pin bidirectional line
				(at 29.21 11.43 180)
				(length 3.81)
				(name "TA1.2/P2.1")
				(number "27")
			)
			(pin bidirectional line
				(at 29.21 8.89 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P2.2")
				(number "28")
			)
			(pin bidirectional line
				(at 29.21 6.35 180)
				(length 3.81)
				(name "TA2.0/P2.3")
				(number "29")
			)
			(pin bidirectional line
				(at 29.21 3.81 180)
				(length 3.81)
				(name "TA2.1/P2.4")
				(number "30")
			)
			(pin bidirectional line
				(at 29.21 1.27 180)
				(length 3.81)
				(name "TA2.2/P2.5")
				(number "31")
			)
			(pin bidirectional line
				(at 29.21 -1.27 180)
				(length 3.81)
				(name "RTCCLK/DMAE0/P2.6")
				(number "32")
			)
			(pin bidirectional line
				(at 29.21 -3.81 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "33")
			)
			(pin bidirectional line
				(at 29.21 -7.62 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "34")
			)
			(pin bidirectional line
				(at 29.21 -10.16 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "35")
			)
			(pin bidirectional line
				(at 29.21 -12.7 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "36")
			)
			(pin bidirectional line
				(at 29.21 -15.24 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "37")
			)
			(pin bidirectional line
				(at 29.21 -17.78 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "38")
			)
			(pin bidirectional line
				(at 29.21 -21.59 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "41")
			)
			(pin bidirectional line
				(at 29.21 -24.13 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "42")
			)
			(pin bidirectional line
				(at 29.21 -26.67 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "43")
			)
			(pin bidirectional line
				(at 29.21 -29.21 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "44")
			)
			(pin bidirectional line
				(at 29.21 -31.75 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "45")
			)
			(pin bidirectional line
				(at 29.21 -34.29 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "46")
			)
			(pin bidirectional line
				(at 29.21 -36.83 180)
				(length 3.81)
				(name "P4.6")
				(number "47")
			)
			(pin bidirectional line
				(at 29.21 -39.37 180)
				(length 3.81)
				(name "P4.7")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5227IYFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5227IYFF"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-64_3.415x3.535mm_Layout8x8_P0.4mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5227.pdf"
			(at 0 0 0)
		)
		(property "Description" "64kB Flash, 8kB RAM, BGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.415x3.535mm*Layout8x8*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5227IYFF_0_1")
		(symbol "MSP430F5227IYFF_1_1"
			(pin bidirectional line
				(at -30.48 39.37 0)
				(length 3.81)
				(name "~{RSTDVCC}/SBWTDIO")
				(number "D4")
			)
			(pin input line
				(at -30.48 36.83 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "E3")
			)
			(pin bidirectional line
				(at -30.48 31.75 0)
				(length 3.81)
				(name "BSLEN")
				(number "E2")
			)
			(pin bidirectional line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "D2")
			)
			(pin bidirectional line
				(at -30.48 24.13 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "B1")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P7.0/TB0.0")
				(number "H1")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P7.1/TB0.1")
				(number "G2")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P7.2/TB0.2")
				(number "F3")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P7.3/TB0.3")
				(number "G1")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P7.4/TB0.4")
				(number "F2")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P7.5/TB0.5")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "A1")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "B2")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 -11.43 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "A2")
			)
			(pin bidirectional line
				(at -30.48 -13.97 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "B3")
			)
			(pin bidirectional line
				(at -30.48 -16.51 0)
				(length 3.81)
				(name "P6.6/CB6/A6")
				(number "C4")
			)
			(pin bidirectional line
				(at -30.48 -19.05 0)
				(length 3.81)
				(name "P6.7/CB7/A7")
				(number "A3")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "B4")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "A4")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "D1")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "A5")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "A6")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 3.81)
				(name "AVCC")
				(number "B5")
			)
			(pin power_in line
				(at -3.81 -45.72 90)
				(length 3.81)
				(name "AVSS")
				(number "B6")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "DVCC")
				(number "A7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "VCORE")
				(number "B8")
			)
			(pin power_in line
				(at 3.81 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "A8")
			)
			(pin power_in line
				(at 6.35 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "H6")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 3.81)
				(name "DVIO")
				(number "H5")
			)
			(pin input line
				(at 29.21 39.37 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "E4")
			)
			(pin bidirectional line
				(at 29.21 35.56 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "B7")
			)
			(pin bidirectional line
				(at 29.21 33.02 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "C7")
			)
			(pin bidirectional line
				(at 29.21 30.48 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "C8")
			)
			(pin bidirectional line
				(at 29.21 27.94 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "C6")
			)
			(pin bidirectional line
				(at 29.21 25.4 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "C5")
			)
			(pin bidirectional line
				(at 29.21 22.86 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "D8")
			)
			(pin bidirectional line
				(at 29.21 20.32 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "D7")
			)
			(pin bidirectional line
				(at 29.21 17.78 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "D6")
			)
			(pin bidirectional line
				(at 29.21 13.97 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "E8")
			)
			(pin bidirectional line
				(at 29.21 11.43 180)
				(length 3.81)
				(name "TA1.2/P2.1")
				(number "D5")
			)
			(pin bidirectional line
				(at 29.21 8.89 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P2.2")
				(number "E7")
			)
			(pin bidirectional line
				(at 29.21 6.35 180)
				(length 3.81)
				(name "TA2.0/P2.3")
				(number "F8")
			)
			(pin bidirectional line
				(at 29.21 3.81 180)
				(length 3.81)
				(name "TA2.1/P2.4")
				(number "J7")
			)
			(pin bidirectional line
				(at 29.21 1.27 180)
				(length 3.81)
				(name "TA2.2/P2.5")
				(number "F7")
			)
			(pin bidirectional line
				(at 29.21 -1.27 180)
				(length 3.81)
				(name "RTCCLK/DMAE0/P2.6")
				(number "G8")
			)
			(pin bidirectional line
				(at 29.21 -3.81 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "F6")
			)
			(pin bidirectional line
				(at 29.21 -7.62 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "H8")
			)
			(pin bidirectional line
				(at 29.21 -10.16 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "G7")
			)
			(pin bidirectional line
				(at 29.21 -12.7 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "G6")
			)
			(pin bidirectional line
				(at 29.21 -15.24 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "H7")
			)
			(pin bidirectional line
				(at 29.21 -17.78 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "G5")
			)
			(pin bidirectional line
				(at 29.21 -21.59 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "F5")
			)
			(pin bidirectional line
				(at 29.21 -24.13 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "H4")
			)
			(pin bidirectional line
				(at 29.21 -26.67 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "E5")
			)
			(pin bidirectional line
				(at 29.21 -29.21 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "G4")
			)
			(pin bidirectional line
				(at 29.21 -31.75 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "H3")
			)
			(pin bidirectional line
				(at 29.21 -34.29 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "F4")
			)
			(pin bidirectional line
				(at 29.21 -36.83 180)
				(length 3.81)
				(name "P4.6")
				(number "H2")
			)
			(pin bidirectional line
				(at 29.21 -39.37 180)
				(length 3.81)
				(name "P4.7")
				(number "G3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5232IRGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 35.56 0)
		)
		(property "Value" "MSP430F5232IRGZ"
			(at 20.32 -35.56 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -24.13 -35.56 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5232.pdf"
			(at -25.4 31.75 0)
		)
		(property "Description" "64kB Flash, 8kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
		(symbol "MSP430F5232IRGZ_0_1")
		(symbol "MSP430F5232IRGZ_1_1"
			(pin bidirectional line
				(at -30.48 29.21 0)
				(length 3.81)
				(name "~{RSTDVCC}/SBWTDIO")
				(number "45")
			)
			(pin input line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 11.43 0)
				(length 3.81)
				(name "P6.0/CB0")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 8.89 0)
				(length 3.81)
				(name "P6.1/CB1")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 6.35 0)
				(length 3.81)
				(name "P6.2/CB2")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 3.81 0)
				(length 3.81)
				(name "P6.3/CB3")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 1.27 0)
				(length 3.81)
				(name "P6.4/CB4")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.5/CB5")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "P5.0")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "P5.1")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "8")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 3.81)
				(name "AVCC")
				(number "6")
			)
			(pin power_in line
				(at -7.62 -38.1 90)
				(length 3.81)
				(name "AVSS")
				(number "9")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "DVCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "DVSS")
				(number "11")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 3.81)
				(name "DVCC")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "DVSS")
				(number "27")
			)
			(pin passive line
				(at 7.62 38.1 270)
				(length 3.81)
				(name "VCORE")
				(number "12")
			)
			(pin input line
				(at 30.48 29.21 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 3.81 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -13.97 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -16.51 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 -19.05 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -21.59 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -24.13 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 -26.67 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 -29.21 180)
				(length 3.81)
				(name "P4.6")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5237IRGC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5237IRGC"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5237.pdf"
			(at 0 0 0)
		)
		(property "Description" "64kB Flash, 8kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
		(symbol "MSP430F5237IRGC_0_1")
		(symbol "MSP430F5237IRGC_1_1"
			(pin bidirectional line
				(at -30.48 39.37 0)
				(length 3.81)
				(name "~{RSTDVCC}/SBWTDIO")
				(number "64")
			)
			(pin input line
				(at -30.48 36.83 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 24.13 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P7.0/TB0.0")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P7.1/TB0.1")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P7.2/TB0.2")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P7.3/TB0.3")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P7.4/TB0.4")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P7.5/TB0.5")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/CB0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/CB1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/CB2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/CB3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -11.43 0)
				(length 3.81)
				(name "P6.4/CB4")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -13.97 0)
				(length 3.81)
				(name "P6.5/CB5")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -16.51 0)
				(length 3.81)
				(name "P6.6/CB6")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 -19.05 0)
				(length 3.81)
				(name "P6.7/CB7")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.0")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.1")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "13")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 3.81)
				(name "AVCC")
				(number "11")
			)
			(pin power_in line
				(at -5.08 -45.72 90)
				(length 3.81)
				(name "AVSS")
				(number "14")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "DVCC")
				(number "15")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "DVCC")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "39")
			)
			(pin power_in line
				(at 6.35 45.72 270)
				(length 3.81)
				(name "VCORE")
				(number "17")
			)
			(pin input line
				(at 30.48 39.37 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "ACLK/TA0CLK/P1.0")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 13.97 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 11.43 180)
				(length 3.81)
				(name "TA1.2/P2.1")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 8.89 180)
				(length 3.81)
				(name "SMCLK/TA2CLK/P2.2")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 6.35 180)
				(length 3.81)
				(name "TA2.0/P2.3")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 3.81 180)
				(length 3.81)
				(name "TA2.1/P2.4")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 1.27 180)
				(length 3.81)
				(name "TA2.2/P2.5")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -1.27 180)
				(length 3.81)
				(name "RTCCLK/DMAE0/P2.6")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -3.81 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 -21.59 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -24.13 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 -26.67 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -29.21 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -31.75 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -34.29 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -36.83 180)
				(length 3.81)
				(name "P4.6")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -39.37 180)
				(length 3.81)
				(name "P4.7")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5242IRGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 35.56 0)
		)
		(property "Value" "MSP430F5242IRGZ"
			(at 20.32 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -24.13 -33.02 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5242.pdf"
			(at -25.4 33.02 0)
		)
		(property "Description" "64kB Flash, 8kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
		(symbol "MSP430F5242IRGZ_0_1")
		(symbol "MSP430F5242IRGZ_1_1"
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 3.81)
				(name "~{RSTDVCC}/SBWTDIO")
				(number "45")
			)
			(pin input line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 24.13 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 16.51 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P6.0/A0/CB0")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P6.1/A1/CB1")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P6.2/A2/CB2")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P6.3/A3/CB3")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P6.4/A4/CB4")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "P6.5/A5/CB5")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -11.43 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -13.97 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 -16.51 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "8")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 3.81)
				(name "AVCC")
				(number "6")
			)
			(pin power_in line
				(at -7.62 -35.56 90)
				(length 3.81)
				(name "AVSS")
				(number "9")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "DVCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "DVSS")
				(number "11")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 3.81)
				(name "DVCC")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "DVSS")
				(number "27")
			)
			(pin passive line
				(at 7.62 38.1 270)
				(length 3.81)
				(name "VCORE")
				(number "12")
			)
			(pin input line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 26.67 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 24.13 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 21.59 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 19.05 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 16.51 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 13.97 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 11.43 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 8.89 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 1.27 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 -1.27 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 -3.81 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 -6.35 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 -8.89 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "P4.6")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5247IRGC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5247IRGC"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5247.pdf"
			(at 0 0 0)
		)
		(property "Description" "64kB Flash, 8kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
		(symbol "MSP430F5247IRGC_0_1")
		(symbol "MSP430F5247IRGC_1_1"
			(pin bidirectional line
				(at -30.48 39.37 0)
				(length 3.81)
				(name "~{RSTDVCC}/SBWTDIO")
				(number "64")
			)
			(pin input line
				(at -30.48 36.83 0)
				(length 3.81)
				(name "~{RST}/NMI")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 24.13 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "P7.0/TB0.0")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "P7.1/TB0.1")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "P7.2/TB0.2")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "P7.3/TB0.3")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "P7.4/TB0.4")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "P7.5/TB0.5")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -11.43 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -13.97 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -16.51 0)
				(length 3.81)
				(name "P6.6/CB6/A6")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 -19.05 0)
				(length 3.81)
				(name "P6.7/CB7/A7")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "13")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 3.81)
				(name "AVCC")
				(number "11")
			)
			(pin power_in line
				(at -3.81 -45.72 90)
				(length 3.81)
				(name "AVSS")
				(number "14")
			)
			(pin power_in line
				(at -1.27 45.72 270)
				(length 3.81)
				(name "DVCC")
				(number "15")
			)
			(pin power_in line
				(at 1.27 45.72 270)
				(length 3.81)
				(name "DVCC")
				(number "40")
			)
			(pin power_in line
				(at 3.81 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 3.81)
				(name "VCORE")
				(number "17")
			)
			(pin power_in line
				(at 6.35 -45.72 90)
				(length 3.81)
				(name "DVSS")
				(number "39")
			)
			(pin input line
				(at 30.48 39.37 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "ACLK/TA0CLK/P1.0")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 13.97 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 11.43 180)
				(length 3.81)
				(name "TA1.2/P2.1")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 8.89 180)
				(length 3.81)
				(name "SMCLK/TA2CLK/P2.2")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 6.35 180)
				(length 3.81)
				(name "TA2.0/P2.3")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 3.81 180)
				(length 3.81)
				(name "TA2.1/P2.4")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 1.27 180)
				(length 3.81)
				(name "TA2.2/P2.5")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -1.27 180)
				(length 3.81)
				(name "RTCCLK/DMAE0/P2.6")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -3.81 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 -21.59 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -24.13 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 -26.67 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -29.21 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -31.75 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -34.29 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -36.83 180)
				(length 3.81)
				(name "P4.6")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -39.37 180)
				(length 3.81)
				(name "P4.7")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5304IPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "MSP430F5304IPT"
			(at 16.51 -29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5304.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 6kB RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5304IPT_0_1")
		(symbol "MSP430F5304IPT_1_1"
			(pin input line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "26")
			)
			(pin power_in line
				(at -30.48 11.43 0)
				(length 3.81)
				(name "LDOI")
				(number "41")
			)
			(pin power_out line
				(at -30.48 8.89 0)
				(length 3.81)
				(name "LDOO")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "PU.0")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "PU.1")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/A0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/A1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/A2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/A3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "9")
			)
			(pin power_in line
				(at -10.16 -31.75 90)
				(length 3.81)
				(name "VSSU")
				(number "37")
			)
			(pin power_in line
				(at -6.35 33.02 270)
				(length 3.81)
				(name "AVCC1")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -31.75 90)
				(length 3.81)
				(name "AVSS1")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -31.75 90)
				(length 3.81)
				(name "AVSS2")
				(number "44")
			)
			(pin power_in line
				(at -1.27 33.02 270)
				(length 3.81)
				(name "DVCC1")
				(number "11")
			)
			(pin power_in line
				(at 1.27 33.02 270)
				(length 3.81)
				(name "DVCC2")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -31.75 90)
				(length 3.81)
				(name "DVSS1")
				(number "12")
			)
			(pin bidirectional line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "VCORE")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -31.75 90)
				(length 3.81)
				(name "DVSS2")
				(number "27")
			)
			(pin input line
				(at 27.94 26.67 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "ACLK/TA0CLK/P1.0")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "TA1CLK/P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "PM_NONE/P4.6")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "PM_NONE/P4.7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5304IRGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "MSP430F5304IRGZ"
			(at 16.51 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -20.32 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5304.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 6kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
		(symbol "MSP430F5304IRGZ_0_1")
		(symbol "MSP430F5304IRGZ_1_1"
			(pin input line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "26")
			)
			(pin power_in line
				(at -30.48 11.43 0)
				(length 3.81)
				(name "LDOI")
				(number "41")
			)
			(pin power_out line
				(at -30.48 8.89 0)
				(length 3.81)
				(name "LDOO")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "PU.0")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "PU.1")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/A0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/A1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/A2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/A3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "9")
			)
			(pin power_in line
				(at -10.16 -31.75 90)
				(length 3.81)
				(name "VSSU")
				(number "37")
			)
			(pin power_in line
				(at -6.35 33.02 270)
				(length 3.81)
				(name "AVCC1")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -31.75 90)
				(length 3.81)
				(name "AVSS1")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -31.75 90)
				(length 3.81)
				(name "AVSS2")
				(number "44")
			)
			(pin power_in line
				(at -1.27 33.02 270)
				(length 3.81)
				(name "DVCC1")
				(number "11")
			)
			(pin power_in line
				(at 1.27 33.02 270)
				(length 3.81)
				(name "DVCC2")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -31.75 90)
				(length 3.81)
				(name "DVSS1")
				(number "12")
			)
			(pin bidirectional line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "VCORE")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -31.75 90)
				(length 3.81)
				(name "DVSS2")
				(number "27")
			)
			(pin input line
				(at 27.94 26.67 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "ACLK/TA0CLK/P1.0")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "TA1CLK/P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "PM_NONE/P4.6")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "PM_NONE/P4.7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5308IPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "MSP430F5308IPT"
			(at 16.51 -29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5308.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 6kB RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5308IPT_0_1")
		(symbol "MSP430F5308IPT_1_1"
			(pin input line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "26")
			)
			(pin power_in line
				(at -30.48 11.43 0)
				(length 3.81)
				(name "LDOI")
				(number "41")
			)
			(pin power_out line
				(at -30.48 8.89 0)
				(length 3.81)
				(name "LDOO")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "PU.0")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "PU.1")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/A0/CB0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/A1/CB1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/A2/CB2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/A3/CB3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "9")
			)
			(pin power_in line
				(at -10.16 -31.75 90)
				(length 3.81)
				(name "VSSU")
				(number "37")
			)
			(pin power_in line
				(at -6.35 33.02 270)
				(length 3.81)
				(name "AVCC1")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -31.75 90)
				(length 3.81)
				(name "AVSS1")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -31.75 90)
				(length 3.81)
				(name "AVSS2")
				(number "44")
			)
			(pin power_in line
				(at -1.27 33.02 270)
				(length 3.81)
				(name "DVCC1")
				(number "11")
			)
			(pin power_in line
				(at 1.27 33.02 270)
				(length 3.81)
				(name "DVCC2")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -31.75 90)
				(length 3.81)
				(name "DVSS1")
				(number "12")
			)
			(pin bidirectional line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "VCORE")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -31.75 90)
				(length 3.81)
				(name "DVSS2")
				(number "27")
			)
			(pin input line
				(at 27.94 26.67 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "ACLK/TA0CLK/P1.0")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "PM_NONE/P4.6")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "PM_NONE/P4.7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5308IRGC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 43.18 0)
		)
		(property "Value" "MSP430F5308IRGC"
			(at 21.59 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -26.67 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5308.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "16kB Flash, 6kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
		(symbol "MSP430F5308IRGC_0_1")
		(symbol "MSP430F5308IRGC_1_1"
			(pin input line
				(at -33.02 39.37 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "64")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "60")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "61")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "62")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "63")
			)
			(pin power_in line
				(at -33.02 24.13 0)
				(length 3.81)
				(name "LDOI")
				(number "53")
			)
			(pin power_out line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "LDOO")
				(number "54")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "PU.0")
				(number "50")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "PU.1")
				(number "52")
			)
			(pin bidirectional line
				(at -33.02 11.43 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "1")
			)
			(pin bidirectional line
				(at -33.02 8.89 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "2")
			)
			(pin bidirectional line
				(at -33.02 6.35 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 3.81 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "4")
			)
			(pin bidirectional line
				(at -33.02 1.27 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 -1.27 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 -3.81 0)
				(length 3.81)
				(name "P6.6/CB6/A6")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 -6.35 0)
				(length 3.81)
				(name "P6.7/CB7/A7")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "57")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "58")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "13")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 3.81)
				(name "AVCC1")
				(number "11")
			)
			(pin power_in line
				(at -7.62 -45.72 90)
				(length 3.81)
				(name "VSSU")
				(number "49")
			)
			(pin power_in line
				(at -1.27 45.72 270)
				(length 3.81)
				(name "DVCC1")
				(number "15")
			)
			(pin power_in line
				(at -1.27 -45.72 90)
				(length 3.81)
				(name "AVSS1")
				(number "14")
			)
			(pin power_in line
				(at 1.27 45.72 270)
				(length 3.81)
				(name "DVCC2")
				(number "40")
			)
			(pin power_in line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "AVSS2")
				(number "56")
			)
			(pin power_in line
				(at 6.35 -45.72 90)
				(length 3.81)
				(name "DVSS1")
				(number "16")
			)
			(pin bidirectional line
				(at 7.62 45.72 270)
				(length 3.81)
				(name "VCORE")
				(number "17")
			)
			(pin power_in line
				(at 8.89 -45.72 90)
				(length 3.81)
				(name "DVSS2")
				(number "39")
			)
			(pin input line
				(at 33.02 39.37 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "59")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "ACLK/TA0CLK/P1.0")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 13.97 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 11.43 180)
				(length 3.81)
				(name "TA1.2/P2.1")
				(number "27")
			)
			(pin bidirectional line
				(at 33.02 8.89 180)
				(length 3.81)
				(name "SMCLK/TA2CLK/P2.2")
				(number "28")
			)
			(pin bidirectional line
				(at 33.02 6.35 180)
				(length 3.81)
				(name "TA2.0/P2.3")
				(number "29")
			)
			(pin bidirectional line
				(at 33.02 3.81 180)
				(length 3.81)
				(name "TA2.1/P2.4")
				(number "30")
			)
			(pin bidirectional line
				(at 33.02 1.27 180)
				(length 3.81)
				(name "TA2.2/P2.5")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 -1.27 180)
				(length 3.81)
				(name "RTCCLK/DMAE0/P2.6")
				(number "32")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "36")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "37")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "41")
			)
			(pin bidirectional line
				(at 33.02 -24.13 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "42")
			)
			(pin bidirectional line
				(at 33.02 -26.67 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "43")
			)
			(pin bidirectional line
				(at 33.02 -29.21 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -31.75 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "45")
			)
			(pin bidirectional line
				(at 33.02 -34.29 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "46")
			)
			(pin bidirectional line
				(at 33.02 -36.83 180)
				(length 3.81)
				(name "PM_NONE/P4.6")
				(number "47")
			)
			(pin bidirectional line
				(at 33.02 -39.37 180)
				(length 3.81)
				(name "PM_NONE/P4.7")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5308IRGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "MSP430F5308IRGZ"
			(at 16.51 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -20.32 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5308.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 6kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
		(symbol "MSP430F5308IRGZ_0_1")
		(symbol "MSP430F5308IRGZ_1_1"
			(pin input line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "26")
			)
			(pin power_in line
				(at -30.48 11.43 0)
				(length 3.81)
				(name "LDOI")
				(number "41")
			)
			(pin power_out line
				(at -30.48 8.89 0)
				(length 3.81)
				(name "LDOO")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "PU.0")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "PU.1")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -1.27 0)
				(length 3.81)
				(name "P6.0/A0/CB0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -3.81 0)
				(length 3.81)
				(name "P6.1/A1/CB1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -6.35 0)
				(length 3.81)
				(name "P6.2/A2/CB2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -8.89 0)
				(length 3.81)
				(name "P6.3/A3/CB3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "9")
			)
			(pin power_in line
				(at -10.16 -31.75 90)
				(length 3.81)
				(name "VSSU")
				(number "37")
			)
			(pin power_in line
				(at -6.35 33.02 270)
				(length 3.81)
				(name "AVCC1")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -31.75 90)
				(length 3.81)
				(name "AVSS1")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -31.75 90)
				(length 3.81)
				(name "AVSS2")
				(number "44")
			)
			(pin power_in line
				(at -1.27 33.02 270)
				(length 3.81)
				(name "DVCC1")
				(number "11")
			)
			(pin power_in line
				(at 1.27 33.02 270)
				(length 3.81)
				(name "DVCC2")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -31.75 90)
				(length 3.81)
				(name "DVSS1")
				(number "12")
			)
			(pin bidirectional line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "VCORE")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -31.75 90)
				(length 3.81)
				(name "DVSS2")
				(number "27")
			)
			(pin input line
				(at 27.94 26.67 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "ACLK/TA0CLK/P1.0")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "PM_NONE/P4.6")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "PM_NONE/P4.7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5308IZQE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 46.99 0)
		)
		(property "Value" "MSP430F5308IZQE"
			(at -21.59 45.72 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-80_5.0x5.0mm_Layout9x9_P0.5mm"
			(at 26.67 45.72 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5308.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 6kB RAM, BGA-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*5.0x5.0mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5308IZQE_0_1")
		(symbol "MSP430F5308IZQE_1_1"
			(pin input line
				(at -33.02 41.91 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "A2")
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "C5")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "C4")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "A3")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "B3")
			)
			(pin power_in line
				(at -33.02 26.67 0)
				(length 3.81)
				(name "LDOI")
				(number "A7")
			)
			(pin power_out line
				(at -33.02 24.13 0)
				(length 3.81)
				(name "LDOO")
				(number "A6")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "PU.0")
				(number "A9")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "PU.1")
				(number "A8")
			)
			(pin bidirectional line
				(at -33.02 13.97 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "A1")
			)
			(pin bidirectional line
				(at -33.02 11.43 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "B2")
			)
			(pin bidirectional line
				(at -33.02 8.89 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "B1")
			)
			(pin bidirectional line
				(at -33.02 6.35 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "C2")
			)
			(pin bidirectional line
				(at -33.02 3.81 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "C1")
			)
			(pin bidirectional line
				(at -33.02 1.27 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "D2")
			)
			(pin bidirectional line
				(at -33.02 -1.27 0)
				(length 3.81)
				(name "P6.6/CB6/A6")
				(number "D1")
			)
			(pin bidirectional line
				(at -33.02 -3.81 0)
				(length 3.81)
				(name "P6.7/CB7/A7")
				(number "D3")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "E1")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "E2")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "B5")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "B4")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "F1")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "G1")
			)
			(pin power_in line
				(at -26.67 -48.26 90)
				(length 3.81)
				(name "VSSU")
				(number "B8")
			)
			(pin power_in line
				(at -24.13 -48.26 90)
				(length 3.81)
				(name "VSSU")
				(number "B9")
			)
			(pin power_in line
				(at -20.32 -48.26 90)
				(length 3.81)
				(name "AVSS1")
				(number "G2")
			)
			(pin power_in line
				(at -17.78 -48.26 90)
				(length 3.81)
				(name "AVSS2")
				(number "A5")
			)
			(pin power_in line
				(at -13.97 -48.26 90)
				(length 3.81)
				(name "DVSS1")
				(number "J1")
			)
			(pin power_in line
				(at -11.43 -48.26 90)
				(length 3.81)
				(name "DVSS2")
				(number "F9")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 3.81)
				(name "AVCC1")
				(number "F2")
			)
			(pin power_in line
				(at -7.62 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -5.08 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at -1.27 48.26 270)
				(length 3.81)
				(name "DVCC1")
				(number "H1")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at 1.27 48.26 270)
				(length 3.81)
				(name "DVCC2")
				(number "E9")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "E3")
			)
			(pin power_in line
				(at 5.08 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "E4")
			)
			(pin bidirectional line
				(at 7.62 48.26 270)
				(length 3.81)
				(name "VCORE")
				(number "J2")
			)
			(pin power_in line
				(at 7.62 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at 10.16 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at 12.7 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at 15.24 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at 17.78 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at 20.32 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "F6")
			)
			(pin power_in line
				(at 22.86 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at 25.4 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at 27.94 -48.26 90)
				(length 3.81)
				(name "GND")
				(number "G3")
			)
			(pin input line
				(at 33.02 41.91 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "A4")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "ACLK/TA0CLK/P1.0")
				(number "H2")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "H3")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "J3")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "G4")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "H4")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "J4")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P1.6")
				(number "G5")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "H5")
			)
			(pin bidirectional line
				(at 33.02 16.51 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "J5")
			)
			(pin bidirectional line
				(at 33.02 13.97 180)
				(length 3.81)
				(name "TA1.2/P2.1")
				(number "G6")
			)
			(pin bidirectional line
				(at 33.02 11.43 180)
				(length 3.81)
				(name "SMCLK/TA2CLK/P2.2")
				(number "J6")
			)
			(pin bidirectional line
				(at 33.02 8.89 180)
				(length 3.81)
				(name "TA2.0/P2.3")
				(number "H6")
			)
			(pin bidirectional line
				(at 33.02 6.35 180)
				(length 3.81)
				(name "TA2.1/P2.4")
				(number "J7")
			)
			(pin bidirectional line
				(at 33.02 3.81 180)
				(length 3.81)
				(name "TA2.2/P2.5")
				(number "J8")
			)
			(pin bidirectional line
				(at 33.02 1.27 180)
				(length 3.81)
				(name "RTCCLK/DMAE0/P2.6")
				(number "J9")
			)
			(pin bidirectional line
				(at 33.02 -1.27 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "H7")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "H8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "H9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "G8")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "G9")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "G7")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "E8")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "E7")
			)
			(pin bidirectional line
				(at 33.02 -24.13 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "D9")
			)
			(pin bidirectional line
				(at 33.02 -26.67 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "D8")
			)
			(pin bidirectional line
				(at 33.02 -29.21 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "D7")
			)
			(pin bidirectional line
				(at 33.02 -31.75 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "C9")
			)
			(pin bidirectional line
				(at 33.02 -34.29 180)
				(length 3.81)
				(name "PM_NONE/P4.6")
				(number "C8")
			)
			(pin bidirectional line
				(at 33.02 -36.83 180)
				(length 3.81)
				(name "PM_NONE/P4.7")
				(number "C7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5333IPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 60.96 0)
		)
		(property "Value" "MSP430F5333IPZ"
			(at 24.13 -63.5 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -27.94 -63.5 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5333.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "128kB Flash, 10kB RAM, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5333IPZ_0_1")
		(symbol "MSP430F5333IPZ_1_1"
			(pin input line
				(at -34.29 57.15 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "96")
			)
			(pin bidirectional line
				(at -34.29 53.34 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "92")
			)
			(pin bidirectional line
				(at -34.29 50.8 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "93")
			)
			(pin bidirectional line
				(at -34.29 48.26 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "94")
			)
			(pin bidirectional line
				(at -34.29 45.72 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "95")
			)
			(pin bidirectional line
				(at -34.29 40.64 0)
				(length 3.81)
				(name "LDOI")
				(number "80")
			)
			(pin bidirectional line
				(at -34.29 38.1 0)
				(length 3.81)
				(name "LDOO")
				(number "81")
			)
			(pin bidirectional line
				(at -34.29 34.29 0)
				(length 3.81)
				(name "PU.0")
				(number "77")
			)
			(pin bidirectional line
				(at -34.29 31.75 0)
				(length 3.81)
				(name "PU.1")
				(number "79")
			)
			(pin bidirectional line
				(at -34.29 26.67 0)
				(length 3.81)
				(name "VBAK")
				(number "86")
			)
			(pin bidirectional line
				(at -34.29 22.86 0)
				(length 3.81)
				(name "VBAT")
				(number "87")
			)
			(pin bidirectional line
				(at -34.29 17.78 0)
				(length 3.81)
				(name "P9.0")
				(number "68")
			)
			(pin bidirectional line
				(at -34.29 15.24 0)
				(length 3.81)
				(name "P9.1")
				(number "69")
			)
			(pin bidirectional line
				(at -34.29 12.7 0)
				(length 3.81)
				(name "P9.2")
				(number "70")
			)
			(pin bidirectional line
				(at -34.29 10.16 0)
				(length 3.81)
				(name "P9.3")
				(number "71")
			)
			(pin bidirectional line
				(at -34.29 7.62 0)
				(length 3.81)
				(name "P9.4")
				(number "72")
			)
			(pin bidirectional line
				(at -34.29 5.08 0)
				(length 3.81)
				(name "P9.5")
				(number "73")
			)
			(pin bidirectional line
				(at -34.29 2.54 0)
				(length 3.81)
				(name "P9.6")
				(number "74")
			)
			(pin bidirectional line
				(at -34.29 0 0)
				(length 3.81)
				(name "P9.7")
				(number "75")
			)
			(pin bidirectional line
				(at -34.29 -3.81 0)
				(length 3.81)
				(name "P8.0/TB0CLK")
				(number "58")
			)
			(pin bidirectional line
				(at -34.29 -6.35 0)
				(length 3.81)
				(name "P8.1/UCB1STE/UCA1CLK")
				(number "59")
			)
			(pin bidirectional line
				(at -34.29 -8.89 0)
				(length 3.81)
				(name "P8.2/UCA1TXD/UCA1SIMO")
				(number "60")
			)
			(pin bidirectional line
				(at -34.29 -11.43 0)
				(length 3.81)
				(name "P8.3/UCA1RXD/UCA1SOMI")
				(number "61")
			)
			(pin bidirectional line
				(at -34.29 -13.97 0)
				(length 3.81)
				(name "P8.4/UCB1CLK/UCA1STE")
				(number "62")
			)
			(pin bidirectional line
				(at -34.29 -16.51 0)
				(length 3.81)
				(name "P8.5/UCB1SIMO/UCB1SDA")
				(number "65")
			)
			(pin bidirectional line
				(at -34.29 -19.05 0)
				(length 3.81)
				(name "P8.6/UCB1SOMI/UCB1SCL")
				(number "66")
			)
			(pin bidirectional line
				(at -34.29 -21.59 0)
				(length 3.81)
				(name "P8.7")
				(number "67")
			)
			(pin bidirectional line
				(at -34.29 -25.4 0)
				(length 3.81)
				(name "P7.2/XT2IN")
				(number "84")
			)
			(pin bidirectional line
				(at -34.29 -27.94 0)
				(length 3.81)
				(name "P7.3/XT2OUT")
				(number "85")
			)
			(pin bidirectional line
				(at -34.29 -30.48 0)
				(length 3.81)
				(name "P7.4/CB8/A12")
				(number "5")
			)
			(pin bidirectional line
				(at -34.29 -33.02 0)
				(length 3.81)
				(name "P7.5/CB9/A13")
				(number "6")
			)
			(pin bidirectional line
				(at -34.29 -35.56 0)
				(length 3.81)
				(name "P7.6/CB10/A14")
				(number "7")
			)
			(pin bidirectional line
				(at -34.29 -38.1 0)
				(length 3.81)
				(name "P7.7/CB11/A15")
				(number "8")
			)
			(pin bidirectional line
				(at -34.29 -41.91 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "97")
			)
			(pin bidirectional line
				(at -34.29 -44.45 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "98")
			)
			(pin bidirectional line
				(at -34.29 -46.99 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "99")
			)
			(pin bidirectional line
				(at -34.29 -49.53 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "100")
			)
			(pin bidirectional line
				(at -34.29 -52.07 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "1")
			)
			(pin bidirectional line
				(at -34.29 -54.61 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "2")
			)
			(pin bidirectional line
				(at -34.29 -57.15 0)
				(length 3.81)
				(name "P6.6/CB6/A6")
				(number "3")
			)
			(pin bidirectional line
				(at -34.29 -59.69 0)
				(length 3.81)
				(name "P6.7/CB7/A7")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -66.04 90)
				(length 3.81)
				(name "VSSU")
				(number "76")
			)
			(pin power_in line
				(at -10.16 63.5 270)
				(length 3.81)
				(name "AVCC1")
				(number "11")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 3.81)
				(name "AVSS1")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 3.81)
				(name "AVSS2")
				(number "15")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 3.81)
				(name "DVCC1")
				(number "25")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 3.81)
				(name "AVSS3")
				(number "83")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 3.81)
				(name "DVCC2")
				(number "64")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 3.81)
				(name "DVCC3")
				(number "89")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 3.81)
				(name "DVSS")
				(number "29")
			)
			(pin power_in line
				(at 7.62 -66.04 90)
				(length 3.81)
				(name "DVSS1")
				(number "26")
			)
			(pin bidirectional line
				(at 10.16 63.5 270)
				(length 3.81)
				(name "VCORE")
				(number "27")
			)
			(pin power_in line
				(at 10.16 -66.04 90)
				(length 3.81)
				(name "DVSS2")
				(number "63")
			)
			(pin power_in line
				(at 12.7 -66.04 90)
				(length 3.81)
				(name "DVSS3")
				(number "90")
			)
			(pin input line
				(at 34.29 57.15 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "91")
			)
			(pin bidirectional line
				(at 34.29 53.34 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "34")
			)
			(pin bidirectional line
				(at 34.29 50.8 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "35")
			)
			(pin bidirectional line
				(at 34.29 48.26 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "36")
			)
			(pin bidirectional line
				(at 34.29 45.72 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "37")
			)
			(pin bidirectional line
				(at 34.29 43.18 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "38")
			)
			(pin bidirectional line
				(at 34.29 40.64 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "39")
			)
			(pin bidirectional line
				(at 34.29 38.1 180)
				(length 3.81)
				(name "TA0.1/P1.6")
				(number "40")
			)
			(pin bidirectional line
				(at 34.29 35.56 180)
				(length 3.81)
				(name "TA0.2/P1.7")
				(number "41")
			)
			(pin bidirectional line
				(at 34.29 31.75 180)
				(length 3.81)
				(name "P2MAP0/P2.0")
				(number "17")
			)
			(pin bidirectional line
				(at 34.29 29.21 180)
				(length 3.81)
				(name "P2MAP1/P2.1")
				(number "18")
			)
			(pin bidirectional line
				(at 34.29 26.67 180)
				(length 3.81)
				(name "P2MAP2/P2.2")
				(number "19")
			)
			(pin bidirectional line
				(at 34.29 24.13 180)
				(length 3.81)
				(name "P2MAP3/P2.3")
				(number "20")
			)
			(pin bidirectional line
				(at 34.29 21.59 180)
				(length 3.81)
				(name "P2MAP4/P2.4")
				(number "21")
			)
			(pin bidirectional line
				(at 34.29 19.05 180)
				(length 3.81)
				(name "P2MAP5/P2.5")
				(number "22")
			)
			(pin bidirectional line
				(at 34.29 16.51 180)
				(length 3.81)
				(name "P2MAP6/P2.6")
				(number "23")
			)
			(pin bidirectional line
				(at 34.29 13.97 180)
				(length 3.81)
				(name "P2MAP7/P2.7")
				(number "24")
			)
			(pin bidirectional line
				(at 34.29 10.16 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P3.0")
				(number "42")
			)
			(pin bidirectional line
				(at 34.29 7.62 180)
				(length 3.81)
				(name "TA1.0/P3.1")
				(number "43")
			)
			(pin bidirectional line
				(at 34.29 5.08 180)
				(length 3.81)
				(name "TA1.1/P3.2")
				(number "44")
			)
			(pin bidirectional line
				(at 34.29 2.54 180)
				(length 3.81)
				(name "TA1.2/P3.3")
				(number "45")
			)
			(pin bidirectional line
				(at 34.29 0 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P3.4")
				(number "46")
			)
			(pin bidirectional line
				(at 34.29 -2.54 180)
				(length 3.81)
				(name "TA2.0/P3.5")
				(number "47")
			)
			(pin bidirectional line
				(at 34.29 -5.08 180)
				(length 3.81)
				(name "TA2.1/P3.6")
				(number "48")
			)
			(pin bidirectional line
				(at 34.29 -7.62 180)
				(length 3.81)
				(name "TA2.2/P3.7")
				(number "49")
			)
			(pin bidirectional line
				(at 34.29 -11.43 180)
				(length 3.81)
				(name "TB0.0/P4.0")
				(number "50")
			)
			(pin bidirectional line
				(at 34.29 -13.97 180)
				(length 3.81)
				(name "TB0.1/P4.1")
				(number "51")
			)
			(pin bidirectional line
				(at 34.29 -16.51 180)
				(length 3.81)
				(name "TB0.2/P4.2")
				(number "52")
			)
			(pin bidirectional line
				(at 34.29 -19.05 180)
				(length 3.81)
				(name "TB0.3/P4.3")
				(number "53")
			)
			(pin bidirectional line
				(at 34.29 -21.59 180)
				(length 3.81)
				(name "TB0.4/P4.4")
				(number "54")
			)
			(pin bidirectional line
				(at 34.29 -24.13 180)
				(length 3.81)
				(name "TB0.5/P4.5")
				(number "55")
			)
			(pin bidirectional line
				(at 34.29 -26.67 180)
				(length 3.81)
				(name "TB0.6/P4.6")
				(number "56")
			)
			(pin bidirectional line
				(at 34.29 -29.21 180)
				(length 3.81)
				(name "TB0OUTH/SVMOUT/P4.7")
				(number "57")
			)
			(pin bidirectional line
				(at 34.29 -33.02 180)
				(length 3.81)
				(name "VREF+/VeREF+/P5.0")
				(number "9")
			)
			(pin bidirectional line
				(at 34.29 -35.56 180)
				(length 3.81)
				(name "VREF-/VeREF-/P5.1")
				(number "10")
			)
			(pin bidirectional line
				(at 34.29 -38.1 180)
				(length 3.81)
				(name "P5.2")
				(number "28")
			)
			(pin bidirectional line
				(at 34.29 -40.64 180)
				(length 3.81)
				(name "P5.3")
				(number "31")
			)
			(pin bidirectional line
				(at 34.29 -43.18 180)
				(length 3.81)
				(name "P5.4")
				(number "32")
			)
			(pin bidirectional line
				(at 34.29 -45.72 180)
				(length 3.81)
				(name "P5.5")
				(number "33")
			)
			(pin bidirectional line
				(at 34.29 -48.26 180)
				(length 3.81)
				(name "ADC12CLK/DMAE0/P5.6")
				(number "16")
			)
			(pin bidirectional line
				(at 34.29 -50.8 180)
				(length 3.81)
				(name "RTCCLK/P5.7")
				(number "88")
			)
			(pin bidirectional line
				(at 34.29 -55.88 180)
				(length 3.81)
				(name "XIN")
				(number "13")
			)
			(pin bidirectional line
				(at 34.29 -59.69 180)
				(length 3.81)
				(name "XOUT")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5333IZQW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 67.31 0)
		)
		(property "Value" "MSP430F5333IZQW"
			(at -22.86 66.04 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 66.04 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5333.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 10kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5333IZQW_0_1")
		(symbol "MSP430F5333IZQW_1_1"
			(pin input line
				(at -34.29 62.23 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "A3")
			)
			(pin bidirectional line
				(at -34.29 58.42 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "B5")
			)
			(pin bidirectional line
				(at -34.29 55.88 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "A4")
			)
			(pin bidirectional line
				(at -34.29 53.34 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "E7")
			)
			(pin bidirectional line
				(at -34.29 50.8 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "D6")
			)
			(pin bidirectional line
				(at -34.29 45.72 0)
				(length 3.81)
				(name "LDOI")
				(number "A10")
			)
			(pin bidirectional line
				(at -34.29 43.18 0)
				(length 3.81)
				(name "LDOO")
				(number "A9")
			)
			(pin bidirectional line
				(at -34.29 39.37 0)
				(length 3.81)
				(name "PU.0")
				(number "A12")
			)
			(pin bidirectional line
				(at -34.29 36.83 0)
				(length 3.81)
				(name "PU.1")
				(number "A11")
			)
			(pin bidirectional line
				(at -34.29 31.75 0)
				(length 3.81)
				(name "VBAK")
				(number "A7")
			)
			(pin bidirectional line
				(at -34.29 27.94 0)
				(length 3.81)
				(name "VBAT")
				(number "D8")
			)
			(pin bidirectional line
				(at -34.29 22.86 0)
				(length 3.81)
				(name "P9.0")
				(number "E11")
			)
			(pin bidirectional line
				(at -34.29 20.32 0)
				(length 3.81)
				(name "P9.1")
				(number "F9")
			)
			(pin bidirectional line
				(at -34.29 17.78 0)
				(length 3.81)
				(name "P9.2")
				(number "D12")
			)
			(pin bidirectional line
				(at -34.29 15.24 0)
				(length 3.81)
				(name "P9.3")
				(number "D11")
			)
			(pin bidirectional line
				(at -34.29 12.7 0)
				(length 3.81)
				(name "P9.4")
				(number "E9")
			)
			(pin bidirectional line
				(at -34.29 10.16 0)
				(length 3.81)
				(name "P9.5")
				(number "C12")
			)
			(pin bidirectional line
				(at -34.29 7.62 0)
				(length 3.81)
				(name "P9.6")
				(number "C11")
			)
			(pin bidirectional line
				(at -34.29 5.08 0)
				(length 3.81)
				(name "P9.7")
				(number "D9")
			)
			(pin bidirectional line
				(at -34.29 1.27 0)
				(length 3.81)
				(name "P8.0/TB0CLK")
				(number "J11")
			)
			(pin bidirectional line
				(at -34.29 -1.27 0)
				(length 3.81)
				(name "P8.1/UCB1STE/UCA1CLK")
				(number "J12")
			)
			(pin bidirectional line
				(at -34.29 -3.81 0)
				(length 3.81)
				(name "P8.2/UCA1TXD/UCA1SIMO")
				(number "H11")
			)
			(pin bidirectional line
				(at -34.29 -6.35 0)
				(length 3.81)
				(name "P8.3/UCA1RXD/UCA1SOMI")
				(number "H12")
			)
			(pin bidirectional line
				(at -34.29 -8.89 0)
				(length 3.81)
				(name "P8.4/UCB1CLK/UCA1STE")
				(number "G11")
			)
			(pin bidirectional line
				(at -34.29 -11.43 0)
				(length 3.81)
				(name "P8.5/UCB1SIMO/UCB1SDA")
				(number "F11")
			)
			(pin bidirectional line
				(at -34.29 -13.97 0)
				(length 3.81)
				(name "P8.6/UCB1SOMI/UCB1SCL")
				(number "G9")
			)
			(pin bidirectional line
				(at -34.29 -16.51 0)
				(length 3.81)
				(name "P8.7")
				(number "E12")
			)
			(pin bidirectional line
				(at -34.29 -20.32 0)
				(length 3.81)
				(name "P7.2/XT2IN")
				(number "B8")
			)
			(pin bidirectional line
				(at -34.29 -22.86 0)
				(length 3.81)
				(name "P7.3/XT2OUT")
				(number "B7")
			)
			(pin bidirectional line
				(at -34.29 -25.4 0)
				(length 3.81)
				(name "P7.4/CB8/A12")
				(number "C1")
			)
			(pin bidirectional line
				(at -34.29 -27.94 0)
				(length 3.81)
				(name "P7.5/CB9/A13")
				(number "C3")
			)
			(pin bidirectional line
				(at -34.29 -30.48 0)
				(length 3.81)
				(name "P7.6/CB10/A14")
				(number "D2")
			)
			(pin bidirectional line
				(at -34.29 -33.02 0)
				(length 3.81)
				(name "P7.7/CB11/A15")
				(number "D1")
			)
			(pin bidirectional line
				(at -34.29 -36.83 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "B4")
			)
			(pin bidirectional line
				(at -34.29 -39.37 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "B3")
			)
			(pin bidirectional line
				(at -34.29 -41.91 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "A2")
			)
			(pin bidirectional line
				(at -34.29 -44.45 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "D5")
			)
			(pin bidirectional line
				(at -34.29 -46.99 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "A1")
			)
			(pin bidirectional line
				(at -34.29 -49.53 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "B2")
			)
			(pin bidirectional line
				(at -34.29 -52.07 0)
				(length 3.81)
				(name "P6.6/CB6/A6")
				(number "B1")
			)
			(pin bidirectional line
				(at -34.29 -54.61 0)
				(length 3.81)
				(name "P6.7/CB7/A7")
				(number "C2")
			)
			(pin power_in line
				(at -27.94 -68.58 90)
				(length 3.81)
				(name "VSSU")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -68.58 90)
				(length 3.81)
				(name "VSSU")
				(number "B12")
			)
			(pin power_in line
				(at -20.32 -68.58 90)
				(length 3.81)
				(name "AVSS1")
				(number "F2")
			)
			(pin power_in line
				(at -17.78 -68.58 90)
				(length 3.81)
				(name "AVSS2")
				(number "G2")
			)
			(pin power_in line
				(at -15.24 -68.58 90)
				(length 3.81)
				(name "AVSS3")
				(number "A8")
			)
			(pin power_in line
				(at -10.16 68.58 270)
				(length 3.81)
				(name "AVCC1")
				(number "E1")
			)
			(pin power_in line
				(at -10.16 -68.58 90)
				(length 3.81)
				(name "DVSS")
				(number "M3")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 3.81)
				(name "AVCC1")
				(number "E2")
			)
			(pin power_in line
				(at -7.62 -68.58 90)
				(length 3.81)
				(name "DVSS1")
				(number "M1")
			)
			(pin power_in line
				(at -5.08 -68.58 90)
				(length 3.81)
				(name "DVSS2")
				(number "G12")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 3.81)
				(name "DVSS3")
				(number "A5")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 3.81)
				(name "DVCC1")
				(number "L1")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 3.81)
				(name "DVCC2")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at 5.08 68.58 270)
				(length 3.81)
				(name "DVCC3")
				(number "A6")
			)
			(pin power_in line
				(at 5.08 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E8")
			)
			(pin bidirectional line
				(at 10.16 68.58 270)
				(length 3.81)
				(name "VCORE")
				(number "M2")
			)
			(pin power_in line
				(at 10.16 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at 12.7 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at 15.24 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at 17.78 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 20.32 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at 22.86 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at 25.4 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 27.94 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H9")
			)
			(pin input line
				(at 34.29 62.23 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "B6")
			)
			(pin bidirectional line
				(at 34.29 58.42 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "L5")
			)
			(pin bidirectional line
				(at 34.29 55.88 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "M5")
			)
			(pin bidirectional line
				(at 34.29 53.34 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "J6")
			)
			(pin bidirectional line
				(at 34.29 50.8 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "H6")
			)
			(pin bidirectional line
				(at 34.29 48.26 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "M6")
			)
			(pin bidirectional line
				(at 34.29 45.72 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "L6")
			)
			(pin bidirectional line
				(at 34.29 43.18 180)
				(length 3.81)
				(name "TA0.1/P1.6")
				(number "J7")
			)
			(pin bidirectional line
				(at 34.29 40.64 180)
				(length 3.81)
				(name "TA0.2/P1.7")
				(number "M7")
			)
			(pin bidirectional line
				(at 34.29 36.83 180)
				(length 3.81)
				(name "P2MAP0/P2.0")
				(number "G4")
			)
			(pin bidirectional line
				(at 34.29 34.29 180)
				(length 3.81)
				(name "P2MAP1/P2.1")
				(number "H2")
			)
			(pin bidirectional line
				(at 34.29 31.75 180)
				(length 3.81)
				(name "P2MAP2/P2.2")
				(number "J1")
			)
			(pin bidirectional line
				(at 34.29 29.21 180)
				(length 3.81)
				(name "P2MAP3/P2.3")
				(number "H4")
			)
			(pin bidirectional line
				(at 34.29 26.67 180)
				(length 3.81)
				(name "P2MAP4/P2.4")
				(number "J2")
			)
			(pin bidirectional line
				(at 34.29 24.13 180)
				(length 3.81)
				(name "P2MAP5/P2.5")
				(number "K1")
			)
			(pin bidirectional line
				(at 34.29 21.59 180)
				(length 3.81)
				(name "P2MAP6/P2.6")
				(number "K2")
			)
			(pin bidirectional line
				(at 34.29 19.05 180)
				(length 3.81)
				(name "P2MAP7/P2.7")
				(number "L2")
			)
			(pin bidirectional line
				(at 34.29 15.24 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P3.0")
				(number "L7")
			)
			(pin bidirectional line
				(at 34.29 12.7 180)
				(length 3.81)
				(name "TA1.0/P3.1")
				(number "H7")
			)
			(pin bidirectional line
				(at 34.29 10.16 180)
				(length 3.81)
				(name "TA1.1/P3.2")
				(number "M8")
			)
			(pin bidirectional line
				(at 34.29 7.62 180)
				(length 3.81)
				(name "TA1.2/P3.3")
				(number "L8")
			)
			(pin bidirectional line
				(at 34.29 5.08 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P3.4")
				(number "J8")
			)
			(pin bidirectional line
				(at 34.29 2.54 180)
				(length 3.81)
				(name "TA2.0/P3.5")
				(number "M9")
			)
			(pin bidirectional line
				(at 34.29 0 180)
				(length 3.81)
				(name "TA2.1/P3.6")
				(number "L9")
			)
			(pin bidirectional line
				(at 34.29 -2.54 180)
				(length 3.81)
				(name "TA2.2/P3.7")
				(number "M10")
			)
			(pin bidirectional line
				(at 34.29 -6.35 180)
				(length 3.81)
				(name "TB0.0/P4.0")
				(number "J9")
			)
			(pin bidirectional line
				(at 34.29 -8.89 180)
				(length 3.81)
				(name "TB0.1/P4.1")
				(number "M11")
			)
			(pin bidirectional line
				(at 34.29 -11.43 180)
				(length 3.81)
				(name "TB0.2/P4.2")
				(number "L10")
			)
			(pin bidirectional line
				(at 34.29 -13.97 180)
				(length 3.81)
				(name "TB0.3/P4.3")
				(number "M12")
			)
			(pin bidirectional line
				(at 34.29 -16.51 180)
				(length 3.81)
				(name "TB0.4/P4.4")
				(number "L12")
			)
			(pin bidirectional line
				(at 34.29 -19.05 180)
				(length 3.81)
				(name "TB0.5/P4.5")
				(number "L11")
			)
			(pin bidirectional line
				(at 34.29 -21.59 180)
				(length 3.81)
				(name "TB0.6/P4.6")
				(number "K11")
			)
			(pin bidirectional line
				(at 34.29 -24.13 180)
				(length 3.81)
				(name "TB0OUTH/SVMOUT/P4.7")
				(number "K12")
			)
			(pin bidirectional line
				(at 34.29 -27.94 180)
				(length 3.81)
				(name "VREF+/VeREF+/P5.0")
				(number "D4")
			)
			(pin bidirectional line
				(at 34.29 -30.48 180)
				(length 3.81)
				(name "VREF-/VeREF-/P5.1")
				(number "E4")
			)
			(pin bidirectional line
				(at 34.29 -33.02 180)
				(length 3.81)
				(name "P5.2")
				(number "L3")
			)
			(pin bidirectional line
				(at 34.29 -35.56 180)
				(length 3.81)
				(name "P5.3")
				(number "L4")
			)
			(pin bidirectional line
				(at 34.29 -38.1 180)
				(length 3.81)
				(name "P5.4")
				(number "M4")
			)
			(pin bidirectional line
				(at 34.29 -40.64 180)
				(length 3.81)
				(name "P5.5")
				(number "J5")
			)
			(pin bidirectional line
				(at 34.29 -43.18 180)
				(length 3.81)
				(name "ADC12CLK/DMAE0/P5.6")
				(number "H1")
			)
			(pin bidirectional line
				(at 34.29 -45.72 180)
				(length 3.81)
				(name "RTCCLK/P5.7")
				(number "D7")
			)
			(pin bidirectional line
				(at 34.29 -50.8 180)
				(length 3.81)
				(name "XIN")
				(number "F1")
			)
			(pin bidirectional line
				(at 34.29 -54.61 180)
				(length 3.81)
				(name "XOUT")
				(number "G1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5336IPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 60.96 0)
		)
		(property "Value" "MSP430F5336IPZ"
			(at 24.13 -63.5 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -27.94 -63.5 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5336.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "128kB Flash, 18kB RAM, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5336IPZ_0_1")
		(symbol "MSP430F5336IPZ_1_1"
			(pin input line
				(at -34.29 57.15 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "96")
			)
			(pin bidirectional line
				(at -34.29 53.34 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "92")
			)
			(pin bidirectional line
				(at -34.29 50.8 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "93")
			)
			(pin bidirectional line
				(at -34.29 48.26 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "94")
			)
			(pin bidirectional line
				(at -34.29 45.72 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "95")
			)
			(pin bidirectional line
				(at -34.29 40.64 0)
				(length 3.81)
				(name "LDOI")
				(number "80")
			)
			(pin bidirectional line
				(at -34.29 38.1 0)
				(length 3.81)
				(name "LDOO")
				(number "81")
			)
			(pin bidirectional line
				(at -34.29 34.29 0)
				(length 3.81)
				(name "PU.0")
				(number "77")
			)
			(pin bidirectional line
				(at -34.29 31.75 0)
				(length 3.81)
				(name "PU.1")
				(number "79")
			)
			(pin bidirectional line
				(at -34.29 26.67 0)
				(length 3.81)
				(name "VBAK")
				(number "86")
			)
			(pin bidirectional line
				(at -34.29 22.86 0)
				(length 3.81)
				(name "VBAT")
				(number "87")
			)
			(pin bidirectional line
				(at -34.29 17.78 0)
				(length 3.81)
				(name "P9.0")
				(number "68")
			)
			(pin bidirectional line
				(at -34.29 15.24 0)
				(length 3.81)
				(name "P9.1")
				(number "69")
			)
			(pin bidirectional line
				(at -34.29 12.7 0)
				(length 3.81)
				(name "P9.2")
				(number "70")
			)
			(pin bidirectional line
				(at -34.29 10.16 0)
				(length 3.81)
				(name "P9.3")
				(number "71")
			)
			(pin bidirectional line
				(at -34.29 7.62 0)
				(length 3.81)
				(name "P9.4")
				(number "72")
			)
			(pin bidirectional line
				(at -34.29 5.08 0)
				(length 3.81)
				(name "P9.5")
				(number "73")
			)
			(pin bidirectional line
				(at -34.29 2.54 0)
				(length 3.81)
				(name "P9.6")
				(number "74")
			)
			(pin bidirectional line
				(at -34.29 0 0)
				(length 3.81)
				(name "P9.7")
				(number "75")
			)
			(pin bidirectional line
				(at -34.29 -3.81 0)
				(length 3.81)
				(name "P8.0/TB0CLK")
				(number "58")
			)
			(pin bidirectional line
				(at -34.29 -6.35 0)
				(length 3.81)
				(name "P8.1/UCB1STE/UCA1CLK")
				(number "59")
			)
			(pin bidirectional line
				(at -34.29 -8.89 0)
				(length 3.81)
				(name "P8.2/UCA1TXD/UCA1SIMO")
				(number "60")
			)
			(pin bidirectional line
				(at -34.29 -11.43 0)
				(length 3.81)
				(name "P8.3/UCA1RXD/UCA1SOMI")
				(number "61")
			)
			(pin bidirectional line
				(at -34.29 -13.97 0)
				(length 3.81)
				(name "P8.4/UCB1CLK/UCA1STE")
				(number "62")
			)
			(pin bidirectional line
				(at -34.29 -16.51 0)
				(length 3.81)
				(name "P8.5/UCB1SIMO/UCB1SDA")
				(number "65")
			)
			(pin bidirectional line
				(at -34.29 -19.05 0)
				(length 3.81)
				(name "P8.6/UCB1SOMI/UCB1SCL")
				(number "66")
			)
			(pin bidirectional line
				(at -34.29 -21.59 0)
				(length 3.81)
				(name "P8.7")
				(number "67")
			)
			(pin bidirectional line
				(at -34.29 -25.4 0)
				(length 3.81)
				(name "P7.2/XT2IN")
				(number "84")
			)
			(pin bidirectional line
				(at -34.29 -27.94 0)
				(length 3.81)
				(name "P7.3/XT2OUT")
				(number "85")
			)
			(pin bidirectional line
				(at -34.29 -30.48 0)
				(length 3.81)
				(name "P7.4/CB8/A12")
				(number "5")
			)
			(pin bidirectional line
				(at -34.29 -33.02 0)
				(length 3.81)
				(name "P7.5/CB9/A13")
				(number "6")
			)
			(pin bidirectional line
				(at -34.29 -35.56 0)
				(length 3.81)
				(name "P7.6/CB10/A14/DAC0")
				(number "7")
			)
			(pin bidirectional line
				(at -34.29 -38.1 0)
				(length 3.81)
				(name "P7.7/CB11/A15/DAC1")
				(number "8")
			)
			(pin bidirectional line
				(at -34.29 -41.91 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "97")
			)
			(pin bidirectional line
				(at -34.29 -44.45 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "98")
			)
			(pin bidirectional line
				(at -34.29 -46.99 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "99")
			)
			(pin bidirectional line
				(at -34.29 -49.53 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "100")
			)
			(pin bidirectional line
				(at -34.29 -52.07 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "1")
			)
			(pin bidirectional line
				(at -34.29 -54.61 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "2")
			)
			(pin bidirectional line
				(at -34.29 -57.15 0)
				(length 3.81)
				(name "P6.6/CB6/A6/DAC0")
				(number "3")
			)
			(pin bidirectional line
				(at -34.29 -59.69 0)
				(length 3.81)
				(name "P6.7/CB7/A7/DAC1")
				(number "4")
			)
			(pin power_in line
				(at -10.16 63.5 270)
				(length 3.81)
				(name "AVCC1")
				(number "11")
			)
			(pin power_in line
				(at -10.16 -66.04 90)
				(length 3.81)
				(name "VSSU")
				(number "76")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 3.81)
				(name "AVSS1")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 3.81)
				(name "AVSS2")
				(number "15")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 3.81)
				(name "DVCC1")
				(number "25")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 3.81)
				(name "AVSS3")
				(number "83")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 3.81)
				(name "DVCC2")
				(number "64")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 3.81)
				(name "DVCC3")
				(number "89")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 3.81)
				(name "DVSS")
				(number "29")
			)
			(pin power_in line
				(at 7.62 -66.04 90)
				(length 3.81)
				(name "DVSS1")
				(number "26")
			)
			(pin bidirectional line
				(at 10.16 63.5 270)
				(length 3.81)
				(name "VCORE")
				(number "27")
			)
			(pin power_in line
				(at 10.16 -66.04 90)
				(length 3.81)
				(name "DVSS2")
				(number "63")
			)
			(pin power_in line
				(at 12.7 -66.04 90)
				(length 3.81)
				(name "DVSS3")
				(number "90")
			)
			(pin input line
				(at 34.29 57.15 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "91")
			)
			(pin bidirectional line
				(at 34.29 53.34 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "34")
			)
			(pin bidirectional line
				(at 34.29 50.8 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "35")
			)
			(pin bidirectional line
				(at 34.29 48.26 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "36")
			)
			(pin bidirectional line
				(at 34.29 45.72 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "37")
			)
			(pin bidirectional line
				(at 34.29 43.18 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "38")
			)
			(pin bidirectional line
				(at 34.29 40.64 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "39")
			)
			(pin bidirectional line
				(at 34.29 38.1 180)
				(length 3.81)
				(name "TA0.1/P1.6")
				(number "40")
			)
			(pin bidirectional line
				(at 34.29 35.56 180)
				(length 3.81)
				(name "TA0.2/P1.7")
				(number "41")
			)
			(pin bidirectional line
				(at 34.29 31.75 180)
				(length 3.81)
				(name "P2MAP0/P2.0")
				(number "17")
			)
			(pin bidirectional line
				(at 34.29 29.21 180)
				(length 3.81)
				(name "P2MAP1/P2.1")
				(number "18")
			)
			(pin bidirectional line
				(at 34.29 26.67 180)
				(length 3.81)
				(name "P2MAP2/P2.2")
				(number "19")
			)
			(pin bidirectional line
				(at 34.29 24.13 180)
				(length 3.81)
				(name "P2MAP3/P2.3")
				(number "20")
			)
			(pin bidirectional line
				(at 34.29 21.59 180)
				(length 3.81)
				(name "P2MAP4/P2.4")
				(number "21")
			)
			(pin bidirectional line
				(at 34.29 19.05 180)
				(length 3.81)
				(name "P2MAP5/P2.5")
				(number "22")
			)
			(pin bidirectional line
				(at 34.29 16.51 180)
				(length 3.81)
				(name "P2MAP6/P2.6")
				(number "23")
			)
			(pin bidirectional line
				(at 34.29 13.97 180)
				(length 3.81)
				(name "P2MAP7/P2.7")
				(number "24")
			)
			(pin bidirectional line
				(at 34.29 10.16 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P3.0")
				(number "42")
			)
			(pin bidirectional line
				(at 34.29 7.62 180)
				(length 3.81)
				(name "TA1.0/P3.1")
				(number "43")
			)
			(pin bidirectional line
				(at 34.29 5.08 180)
				(length 3.81)
				(name "TA1.1/P3.2")
				(number "44")
			)
			(pin bidirectional line
				(at 34.29 2.54 180)
				(length 3.81)
				(name "TA1.2/P3.3")
				(number "45")
			)
			(pin bidirectional line
				(at 34.29 0 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P3.4")
				(number "46")
			)
			(pin bidirectional line
				(at 34.29 -2.54 180)
				(length 3.81)
				(name "TA2.0/P3.5")
				(number "47")
			)
			(pin bidirectional line
				(at 34.29 -5.08 180)
				(length 3.81)
				(name "TA2.1/P3.6")
				(number "48")
			)
			(pin bidirectional line
				(at 34.29 -7.62 180)
				(length 3.81)
				(name "TA2.2/P3.7")
				(number "49")
			)
			(pin bidirectional line
				(at 34.29 -11.43 180)
				(length 3.81)
				(name "TB0.0/P4.0")
				(number "50")
			)
			(pin bidirectional line
				(at 34.29 -13.97 180)
				(length 3.81)
				(name "TB0.1/P4.1")
				(number "51")
			)
			(pin bidirectional line
				(at 34.29 -16.51 180)
				(length 3.81)
				(name "TB0.2/P4.2")
				(number "52")
			)
			(pin bidirectional line
				(at 34.29 -19.05 180)
				(length 3.81)
				(name "TB0.3/P4.3")
				(number "53")
			)
			(pin bidirectional line
				(at 34.29 -21.59 180)
				(length 3.81)
				(name "TB0.4/P4.4")
				(number "54")
			)
			(pin bidirectional line
				(at 34.29 -24.13 180)
				(length 3.81)
				(name "TB0.5/P4.5")
				(number "55")
			)
			(pin bidirectional line
				(at 34.29 -26.67 180)
				(length 3.81)
				(name "TB0.6/P4.6")
				(number "56")
			)
			(pin bidirectional line
				(at 34.29 -29.21 180)
				(length 3.81)
				(name "TB0OUTH/SVMOUT/P4.7")
				(number "57")
			)
			(pin bidirectional line
				(at 34.29 -33.02 180)
				(length 3.81)
				(name "VREF+/VeREF+/P5.0")
				(number "9")
			)
			(pin bidirectional line
				(at 34.29 -35.56 180)
				(length 3.81)
				(name "VREF-/VeREF-/P5.1")
				(number "10")
			)
			(pin bidirectional line
				(at 34.29 -38.1 180)
				(length 3.81)
				(name "P5.2")
				(number "28")
			)
			(pin bidirectional line
				(at 34.29 -40.64 180)
				(length 3.81)
				(name "P5.3")
				(number "31")
			)
			(pin bidirectional line
				(at 34.29 -43.18 180)
				(length 3.81)
				(name "P5.4")
				(number "32")
			)
			(pin bidirectional line
				(at 34.29 -45.72 180)
				(length 3.81)
				(name "P5.5")
				(number "33")
			)
			(pin bidirectional line
				(at 34.29 -48.26 180)
				(length 3.81)
				(name "ADC12CLK/DMAE0/P5.6")
				(number "16")
			)
			(pin bidirectional line
				(at 34.29 -50.8 180)
				(length 3.81)
				(name "RTCCLK/P5.7")
				(number "88")
			)
			(pin bidirectional line
				(at 34.29 -55.88 180)
				(length 3.81)
				(name "XIN")
				(number "13")
			)
			(pin bidirectional line
				(at 34.29 -59.69 180)
				(length 3.81)
				(name "XOUT")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5336IZQW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 67.31 0)
		)
		(property "Value" "MSP430F5336IZQW"
			(at -22.86 66.04 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 66.04 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5336.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 18kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5336IZQW_0_1")
		(symbol "MSP430F5336IZQW_1_1"
			(pin input line
				(at -34.29 62.23 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "A3")
			)
			(pin bidirectional line
				(at -34.29 58.42 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "B5")
			)
			(pin bidirectional line
				(at -34.29 55.88 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "A4")
			)
			(pin bidirectional line
				(at -34.29 53.34 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "E7")
			)
			(pin bidirectional line
				(at -34.29 50.8 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "D6")
			)
			(pin bidirectional line
				(at -34.29 45.72 0)
				(length 3.81)
				(name "LDOI")
				(number "A10")
			)
			(pin bidirectional line
				(at -34.29 43.18 0)
				(length 3.81)
				(name "LDOO")
				(number "A9")
			)
			(pin bidirectional line
				(at -34.29 39.37 0)
				(length 3.81)
				(name "PU.0")
				(number "A12")
			)
			(pin bidirectional line
				(at -34.29 36.83 0)
				(length 3.81)
				(name "PU.1")
				(number "A11")
			)
			(pin bidirectional line
				(at -34.29 31.75 0)
				(length 3.81)
				(name "VBAK")
				(number "A7")
			)
			(pin bidirectional line
				(at -34.29 27.94 0)
				(length 3.81)
				(name "VBAT")
				(number "D8")
			)
			(pin bidirectional line
				(at -34.29 22.86 0)
				(length 3.81)
				(name "P9.0")
				(number "E11")
			)
			(pin bidirectional line
				(at -34.29 20.32 0)
				(length 3.81)
				(name "P9.1")
				(number "F9")
			)
			(pin bidirectional line
				(at -34.29 17.78 0)
				(length 3.81)
				(name "P9.2")
				(number "D12")
			)
			(pin bidirectional line
				(at -34.29 15.24 0)
				(length 3.81)
				(name "P9.3")
				(number "D11")
			)
			(pin bidirectional line
				(at -34.29 12.7 0)
				(length 3.81)
				(name "P9.4")
				(number "E9")
			)
			(pin bidirectional line
				(at -34.29 10.16 0)
				(length 3.81)
				(name "P9.5")
				(number "C12")
			)
			(pin bidirectional line
				(at -34.29 7.62 0)
				(length 3.81)
				(name "P9.6")
				(number "C11")
			)
			(pin bidirectional line
				(at -34.29 5.08 0)
				(length 3.81)
				(name "P9.7")
				(number "D9")
			)
			(pin bidirectional line
				(at -34.29 1.27 0)
				(length 3.81)
				(name "P8.0/TB0CLK")
				(number "J11")
			)
			(pin bidirectional line
				(at -34.29 -1.27 0)
				(length 3.81)
				(name "P8.1/UCB1STE/UCA1CLK")
				(number "J12")
			)
			(pin bidirectional line
				(at -34.29 -3.81 0)
				(length 3.81)
				(name "P8.2/UCA1TXD/UCA1SIMO")
				(number "H11")
			)
			(pin bidirectional line
				(at -34.29 -6.35 0)
				(length 3.81)
				(name "P8.3/UCA1RXD/UCA1SOMI")
				(number "H12")
			)
			(pin bidirectional line
				(at -34.29 -8.89 0)
				(length 3.81)
				(name "P8.4/UCB1CLK/UCA1STE")
				(number "G11")
			)
			(pin bidirectional line
				(at -34.29 -11.43 0)
				(length 3.81)
				(name "P8.5/UCB1SIMO/UCB1SDA")
				(number "F11")
			)
			(pin bidirectional line
				(at -34.29 -13.97 0)
				(length 3.81)
				(name "P8.6/UCB1SOMI/UCB1SCL")
				(number "G9")
			)
			(pin bidirectional line
				(at -34.29 -16.51 0)
				(length 3.81)
				(name "P8.7")
				(number "E12")
			)
			(pin bidirectional line
				(at -34.29 -20.32 0)
				(length 3.81)
				(name "P7.2/XT2IN")
				(number "B8")
			)
			(pin bidirectional line
				(at -34.29 -22.86 0)
				(length 3.81)
				(name "P7.3/XT2OUT")
				(number "B7")
			)
			(pin bidirectional line
				(at -34.29 -25.4 0)
				(length 3.81)
				(name "P7.4/CB8/A12")
				(number "C1")
			)
			(pin bidirectional line
				(at -34.29 -27.94 0)
				(length 3.81)
				(name "P7.5/CB9/A13")
				(number "C3")
			)
			(pin bidirectional line
				(at -34.29 -30.48 0)
				(length 3.81)
				(name "P7.6/CB10/A14/DAC0")
				(number "D2")
			)
			(pin bidirectional line
				(at -34.29 -33.02 0)
				(length 3.81)
				(name "P7.7/CB11/A15/DAC0")
				(number "D1")
			)
			(pin bidirectional line
				(at -34.29 -36.83 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "B4")
			)
			(pin bidirectional line
				(at -34.29 -39.37 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "B3")
			)
			(pin bidirectional line
				(at -34.29 -41.91 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "A2")
			)
			(pin bidirectional line
				(at -34.29 -44.45 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "D5")
			)
			(pin bidirectional line
				(at -34.29 -46.99 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "A1")
			)
			(pin bidirectional line
				(at -34.29 -49.53 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "B2")
			)
			(pin bidirectional line
				(at -34.29 -52.07 0)
				(length 3.81)
				(name "P6.6/CB6/A6/DAC0")
				(number "B1")
			)
			(pin bidirectional line
				(at -34.29 -54.61 0)
				(length 3.81)
				(name "P6.7/CB7/A7/DAC1")
				(number "C2")
			)
			(pin power_in line
				(at -27.94 -68.58 90)
				(length 3.81)
				(name "VSSU")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -68.58 90)
				(length 3.81)
				(name "VSSU")
				(number "B12")
			)
			(pin power_in line
				(at -20.32 -68.58 90)
				(length 3.81)
				(name "AVSS1")
				(number "F2")
			)
			(pin power_in line
				(at -17.78 -68.58 90)
				(length 3.81)
				(name "AVSS2")
				(number "G2")
			)
			(pin power_in line
				(at -15.24 -68.58 90)
				(length 3.81)
				(name "AVSS3")
				(number "A8")
			)
			(pin power_in line
				(at -10.16 68.58 270)
				(length 3.81)
				(name "AVCC1")
				(number "E1")
			)
			(pin power_in line
				(at -10.16 -68.58 90)
				(length 3.81)
				(name "DVSS")
				(number "M3")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 3.81)
				(name "AVCC1")
				(number "E2")
			)
			(pin power_in line
				(at -7.62 -68.58 90)
				(length 3.81)
				(name "DVSS1")
				(number "M1")
			)
			(pin power_in line
				(at -5.08 -68.58 90)
				(length 3.81)
				(name "DVSS2")
				(number "G12")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 3.81)
				(name "DVSS3")
				(number "A5")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 3.81)
				(name "DVCC1")
				(number "L1")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 3.81)
				(name "DVCC2")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at 5.08 68.58 270)
				(length 3.81)
				(name "DVCC3")
				(number "A6")
			)
			(pin power_in line
				(at 5.08 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E8")
			)
			(pin bidirectional line
				(at 10.16 68.58 270)
				(length 3.81)
				(name "VCORE")
				(number "M2")
			)
			(pin power_in line
				(at 10.16 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at 12.7 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at 15.24 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at 17.78 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 20.32 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at 22.86 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at 25.4 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 27.94 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H9")
			)
			(pin input line
				(at 34.29 62.23 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "B6")
			)
			(pin bidirectional line
				(at 34.29 58.42 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "L5")
			)
			(pin bidirectional line
				(at 34.29 55.88 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "M5")
			)
			(pin bidirectional line
				(at 34.29 53.34 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "J6")
			)
			(pin bidirectional line
				(at 34.29 50.8 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "H6")
			)
			(pin bidirectional line
				(at 34.29 48.26 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "M6")
			)
			(pin bidirectional line
				(at 34.29 45.72 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "L6")
			)
			(pin bidirectional line
				(at 34.29 43.18 180)
				(length 3.81)
				(name "TA0.1/P1.6")
				(number "J7")
			)
			(pin bidirectional line
				(at 34.29 40.64 180)
				(length 3.81)
				(name "TA0.2/P1.7")
				(number "M7")
			)
			(pin bidirectional line
				(at 34.29 36.83 180)
				(length 3.81)
				(name "P2MAP0/P2.0")
				(number "G4")
			)
			(pin bidirectional line
				(at 34.29 34.29 180)
				(length 3.81)
				(name "P2MAP1/P2.1")
				(number "H2")
			)
			(pin bidirectional line
				(at 34.29 31.75 180)
				(length 3.81)
				(name "P2MAP2/P2.2")
				(number "J1")
			)
			(pin bidirectional line
				(at 34.29 29.21 180)
				(length 3.81)
				(name "P2MAP3/P2.3")
				(number "H4")
			)
			(pin bidirectional line
				(at 34.29 26.67 180)
				(length 3.81)
				(name "P2MAP4/P2.4")
				(number "J2")
			)
			(pin bidirectional line
				(at 34.29 24.13 180)
				(length 3.81)
				(name "P2MAP5/P2.5")
				(number "K1")
			)
			(pin bidirectional line
				(at 34.29 21.59 180)
				(length 3.81)
				(name "P2MAP6/P2.6")
				(number "K2")
			)
			(pin bidirectional line
				(at 34.29 19.05 180)
				(length 3.81)
				(name "P2MAP7/P2.7")
				(number "L2")
			)
			(pin bidirectional line
				(at 34.29 15.24 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P3.0")
				(number "L7")
			)
			(pin bidirectional line
				(at 34.29 12.7 180)
				(length 3.81)
				(name "TA1.0/P3.1")
				(number "H7")
			)
			(pin bidirectional line
				(at 34.29 10.16 180)
				(length 3.81)
				(name "TA1.1/P3.2")
				(number "M8")
			)
			(pin bidirectional line
				(at 34.29 7.62 180)
				(length 3.81)
				(name "TA1.2/P3.3")
				(number "L8")
			)
			(pin bidirectional line
				(at 34.29 5.08 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P3.4")
				(number "J8")
			)
			(pin bidirectional line
				(at 34.29 2.54 180)
				(length 3.81)
				(name "TA2.0/P3.5")
				(number "M9")
			)
			(pin bidirectional line
				(at 34.29 0 180)
				(length 3.81)
				(name "TA2.1/P3.6")
				(number "L9")
			)
			(pin bidirectional line
				(at 34.29 -2.54 180)
				(length 3.81)
				(name "TA2.2/P3.7")
				(number "M10")
			)
			(pin bidirectional line
				(at 34.29 -6.35 180)
				(length 3.81)
				(name "TB0.0/P4.0")
				(number "J9")
			)
			(pin bidirectional line
				(at 34.29 -8.89 180)
				(length 3.81)
				(name "TB0.1/P4.1")
				(number "M11")
			)
			(pin bidirectional line
				(at 34.29 -11.43 180)
				(length 3.81)
				(name "TB0.2/P4.2")
				(number "L10")
			)
			(pin bidirectional line
				(at 34.29 -13.97 180)
				(length 3.81)
				(name "TB0.3/P4.3")
				(number "M12")
			)
			(pin bidirectional line
				(at 34.29 -16.51 180)
				(length 3.81)
				(name "TB0.4/P4.4")
				(number "L12")
			)
			(pin bidirectional line
				(at 34.29 -19.05 180)
				(length 3.81)
				(name "TB0.5/P4.5")
				(number "L11")
			)
			(pin bidirectional line
				(at 34.29 -21.59 180)
				(length 3.81)
				(name "TB0.6/P4.6")
				(number "K11")
			)
			(pin bidirectional line
				(at 34.29 -24.13 180)
				(length 3.81)
				(name "TB0OUTH/SVMOUT/P4.7")
				(number "K12")
			)
			(pin bidirectional line
				(at 34.29 -27.94 180)
				(length 3.81)
				(name "VREF+/VeREF+/P5.0")
				(number "D4")
			)
			(pin bidirectional line
				(at 34.29 -30.48 180)
				(length 3.81)
				(name "VREF-/VeREF-/P5.1")
				(number "E4")
			)
			(pin bidirectional line
				(at 34.29 -33.02 180)
				(length 3.81)
				(name "P5.2")
				(number "L3")
			)
			(pin bidirectional line
				(at 34.29 -35.56 180)
				(length 3.81)
				(name "P5.3")
				(number "L4")
			)
			(pin bidirectional line
				(at 34.29 -38.1 180)
				(length 3.81)
				(name "P5.4")
				(number "M4")
			)
			(pin bidirectional line
				(at 34.29 -40.64 180)
				(length 3.81)
				(name "P5.5")
				(number "J5")
			)
			(pin bidirectional line
				(at 34.29 -43.18 180)
				(length 3.81)
				(name "ADC12CLK/DMAE0/P5.6")
				(number "H1")
			)
			(pin bidirectional line
				(at 34.29 -45.72 180)
				(length 3.81)
				(name "RTCCLK/P5.7")
				(number "D7")
			)
			(pin bidirectional line
				(at 34.29 -50.8 180)
				(length 3.81)
				(name "XIN")
				(number "F1")
			)
			(pin bidirectional line
				(at 34.29 -54.61 180)
				(length 3.81)
				(name "XOUT")
				(number "G1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5340IRGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 34.29 0)
		)
		(property "Value" "MSP430F5340IRGZ"
			(at 17.78 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -25.4 -34.29 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5340.pdf"
			(at 0 0 0)
		)
		(property "Description" "64kB Flash, 6kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
		(symbol "MSP430F5340IRGZ_0_1")
		(symbol "MSP430F5340IRGZ_1_1"
			(pin input line
				(at -31.75 30.48 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "46")
			)
			(pin bidirectional line
				(at -31.75 26.67 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "42")
			)
			(pin bidirectional line
				(at -31.75 24.13 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "43")
			)
			(pin bidirectional line
				(at -31.75 21.59 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "44")
			)
			(pin bidirectional line
				(at -31.75 19.05 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "45")
			)
			(pin bidirectional line
				(at -31.75 15.24 0)
				(length 3.81)
				(name "P5.0/A8/VREF+/VeREF+")
				(number "4")
			)
			(pin bidirectional line
				(at -31.75 12.7 0)
				(length 3.81)
				(name "P5.1/A9/VREF-/VeREF-")
				(number "5")
			)
			(pin bidirectional line
				(at -31.75 10.16 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "39")
			)
			(pin bidirectional line
				(at -31.75 7.62 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "40")
			)
			(pin bidirectional line
				(at -31.75 5.08 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "7")
			)
			(pin bidirectional line
				(at -31.75 2.54 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "8")
			)
			(pin bidirectional line
				(at -31.75 0 0)
				(length 3.81)
				(name "P5.7/TB0.1")
				(number "37")
			)
			(pin bidirectional line
				(at -31.75 -3.81 0)
				(length 3.81)
				(name "P6.1/A1/CB1")
				(number "47")
			)
			(pin bidirectional line
				(at -31.75 -6.35 0)
				(length 3.81)
				(name "P6.2/A2/CB2")
				(number "48")
			)
			(pin bidirectional line
				(at -31.75 -8.89 0)
				(length 3.81)
				(name "P6.3/A3/CB3")
				(number "1")
			)
			(pin bidirectional line
				(at -31.75 -11.43 0)
				(length 3.81)
				(name "P6.4/A4/CB4")
				(number "2")
			)
			(pin bidirectional line
				(at -31.75 -13.97 0)
				(length 3.81)
				(name "P6.5/A5/CB5")
				(number "3")
			)
			(pin power_in line
				(at -8.89 36.83 270)
				(length 3.81)
				(name "AVCC1")
				(number "6")
			)
			(pin power_in line
				(at -8.89 -36.83 90)
				(length 3.81)
				(name "AVSS1")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -36.83 90)
				(length 3.81)
				(name "DVSS1")
				(number "11")
			)
			(pin power_in line
				(at -1.27 36.83 270)
				(length 3.81)
				(name "DVCC1")
				(number "10")
			)
			(pin power_in line
				(at 0 -36.83 90)
				(length 3.81)
				(name "DVSS2")
				(number "31")
			)
			(pin power_in line
				(at 1.27 36.83 270)
				(length 3.81)
				(name "DVCC2")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -36.83 90)
				(length 3.81)
				(name "DVSS3")
				(number "38")
			)
			(pin passive line
				(at 3.81 36.83 270)
				(length 3.81)
				(name "VCORE")
				(number "12")
			)
			(pin input line
				(at 29.21 30.48 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "41")
			)
			(pin bidirectional line
				(at 29.21 26.67 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "13")
			)
			(pin bidirectional line
				(at 29.21 24.13 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 29.21 21.59 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "15")
			)
			(pin bidirectional line
				(at 29.21 19.05 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "16")
			)
			(pin bidirectional line
				(at 29.21 16.51 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "17")
			)
			(pin bidirectional line
				(at 29.21 13.97 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "18")
			)
			(pin bidirectional line
				(at 29.21 11.43 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P1.6")
				(number "19")
			)
			(pin bidirectional line
				(at 29.21 8.89 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "20")
			)
			(pin bidirectional line
				(at 29.21 5.08 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "21")
			)
			(pin bidirectional line
				(at 29.21 1.27 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "22")
			)
			(pin bidirectional line
				(at 29.21 -1.27 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "23")
			)
			(pin bidirectional line
				(at 29.21 -3.81 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "24")
			)
			(pin bidirectional line
				(at 29.21 -6.35 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "25")
			)
			(pin bidirectional line
				(at 29.21 -8.89 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "26")
			)
			(pin bidirectional line
				(at 29.21 -12.7 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "27")
			)
			(pin bidirectional line
				(at 29.21 -15.24 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "28")
			)
			(pin bidirectional line
				(at 29.21 -17.78 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "29")
			)
			(pin bidirectional line
				(at 29.21 -20.32 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "30")
			)
			(pin bidirectional line
				(at 29.21 -22.86 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 29.21 -25.4 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 29.21 -27.94 180)
				(length 3.81)
				(name "PM_NONE/P4.6")
				(number "35")
			)
			(pin bidirectional line
				(at 29.21 -30.48 180)
				(length 3.81)
				(name "PM_NONE/P4.7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5358IZQW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 68.58 0)
		)
		(property "Value" "MSP430F5358IZQW"
			(at -22.86 67.31 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 27.94 67.31 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5358.pdf"
			(at 0 0 0)
		)
		(property "Description" "384kB Flash, 34kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5358IZQW_0_1")
		(symbol "MSP430F5358IZQW_1_1"
			(pin input line
				(at -34.29 63.5 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "A3")
			)
			(pin bidirectional line
				(at -34.29 59.69 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "B5")
			)
			(pin bidirectional line
				(at -34.29 57.15 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "A4")
			)
			(pin bidirectional line
				(at -34.29 54.61 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "E7")
			)
			(pin bidirectional line
				(at -34.29 52.07 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "D6")
			)
			(pin bidirectional line
				(at -34.29 46.99 0)
				(length 3.81)
				(name "LDOI")
				(number "A10")
			)
			(pin bidirectional line
				(at -34.29 44.45 0)
				(length 3.81)
				(name "LDOO")
				(number "A9")
			)
			(pin bidirectional line
				(at -34.29 40.64 0)
				(length 3.81)
				(name "PU.0")
				(number "A12")
			)
			(pin bidirectional line
				(at -34.29 38.1 0)
				(length 3.81)
				(name "PU.1")
				(number "A11")
			)
			(pin bidirectional line
				(at -34.29 33.02 0)
				(length 3.81)
				(name "VBAK")
				(number "A7")
			)
			(pin bidirectional line
				(at -34.29 29.21 0)
				(length 3.81)
				(name "VBAT")
				(number "D8")
			)
			(pin bidirectional line
				(at -34.29 24.13 0)
				(length 3.81)
				(name "P9.0")
				(number "E11")
			)
			(pin bidirectional line
				(at -34.29 21.59 0)
				(length 3.81)
				(name "P9.1/UCB2STE/UCA2CLK")
				(number "F9")
			)
			(pin bidirectional line
				(at -34.29 19.05 0)
				(length 3.81)
				(name "P9.2/UCA2TXD/UCA2SIMO")
				(number "D12")
			)
			(pin bidirectional line
				(at -34.29 16.51 0)
				(length 3.81)
				(name "P9.3/UCA2RXD/UCA2SOMI")
				(number "D11")
			)
			(pin bidirectional line
				(at -34.29 13.97 0)
				(length 3.81)
				(name "P9.4/UCB2CLK/UCA2STE")
				(number "E9")
			)
			(pin bidirectional line
				(at -34.29 11.43 0)
				(length 3.81)
				(name "P9.5/UCB2SIMO/UCB2SDA")
				(number "C12")
			)
			(pin bidirectional line
				(at -34.29 8.89 0)
				(length 3.81)
				(name "P9.6/UCB2SOMI/UCB2SCL")
				(number "C11")
			)
			(pin bidirectional line
				(at -34.29 6.35 0)
				(length 3.81)
				(name "P9.7")
				(number "D9")
			)
			(pin bidirectional line
				(at -34.29 2.54 0)
				(length 3.81)
				(name "P8.0/TB0CLK")
				(number "J11")
			)
			(pin bidirectional line
				(at -34.29 0 0)
				(length 3.81)
				(name "P8.1/UCB1STE/UCA1CLK")
				(number "J12")
			)
			(pin bidirectional line
				(at -34.29 -2.54 0)
				(length 3.81)
				(name "P8.2/UCA1TXD/UCA1SIMO")
				(number "H11")
			)
			(pin bidirectional line
				(at -34.29 -5.08 0)
				(length 3.81)
				(name "P8.3/UCA1RXD/UCA1SOMI")
				(number "H12")
			)
			(pin bidirectional line
				(at -34.29 -7.62 0)
				(length 3.81)
				(name "P8.4/UCB1CLK/UCA1STE")
				(number "G11")
			)
			(pin bidirectional line
				(at -34.29 -10.16 0)
				(length 3.81)
				(name "P8.5/UCB1SIMO/UCB1SDA")
				(number "F11")
			)
			(pin bidirectional line
				(at -34.29 -12.7 0)
				(length 3.81)
				(name "P8.6/UCB1SOMI/UCB1SCL")
				(number "G9")
			)
			(pin bidirectional line
				(at -34.29 -15.24 0)
				(length 3.81)
				(name "P8.7")
				(number "E12")
			)
			(pin bidirectional line
				(at -34.29 -19.05 0)
				(length 3.81)
				(name "P7.2/XT2IN")
				(number "B8")
			)
			(pin bidirectional line
				(at -34.29 -21.59 0)
				(length 3.81)
				(name "P7.3/XT2OUT")
				(number "B7")
			)
			(pin bidirectional line
				(at -34.29 -24.13 0)
				(length 3.81)
				(name "P7.4/CB8/A12")
				(number "C1")
			)
			(pin bidirectional line
				(at -34.29 -26.67 0)
				(length 3.81)
				(name "P7.5/CB9/A13")
				(number "C3")
			)
			(pin bidirectional line
				(at -34.29 -29.21 0)
				(length 3.81)
				(name "P7.6/CB10/A14/DAC0")
				(number "D2")
			)
			(pin bidirectional line
				(at -34.29 -31.75 0)
				(length 3.81)
				(name "P7.7/CB11/A15/DAC1")
				(number "D1")
			)
			(pin bidirectional line
				(at -34.29 -35.56 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "B4")
			)
			(pin bidirectional line
				(at -34.29 -38.1 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "B3")
			)
			(pin bidirectional line
				(at -34.29 -40.64 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "A2")
			)
			(pin bidirectional line
				(at -34.29 -43.18 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "D5")
			)
			(pin bidirectional line
				(at -34.29 -45.72 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "A1")
			)
			(pin bidirectional line
				(at -34.29 -48.26 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "B2")
			)
			(pin bidirectional line
				(at -34.29 -50.8 0)
				(length 3.81)
				(name "P6.6/CB6/A6/DAC0")
				(number "B1")
			)
			(pin bidirectional line
				(at -34.29 -53.34 0)
				(length 3.81)
				(name "P6.7/CB7/A7/DAC1")
				(number "C2")
			)
			(pin power_in line
				(at -27.94 -67.31 90)
				(length 3.81)
				(name "VSSU")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -67.31 90)
				(length 3.81)
				(name "VSSU")
				(number "B12")
			)
			(pin power_in line
				(at -20.32 -67.31 90)
				(length 3.81)
				(name "AVSS1")
				(number "F2")
			)
			(pin power_in line
				(at -17.78 -67.31 90)
				(length 3.81)
				(name "AVSS2")
				(number "G2")
			)
			(pin power_in line
				(at -15.24 -67.31 90)
				(length 3.81)
				(name "AVSS3")
				(number "A8")
			)
			(pin power_in line
				(at -10.16 69.85 270)
				(length 3.81)
				(name "AVCC1")
				(number "E1")
			)
			(pin power_in line
				(at -10.16 -67.31 90)
				(length 3.81)
				(name "DVSS")
				(number "M3")
			)
			(pin power_in line
				(at -7.62 69.85 270)
				(length 3.81)
				(name "AVCC1")
				(number "E2")
			)
			(pin power_in line
				(at -7.62 -67.31 90)
				(length 3.81)
				(name "DVSS1")
				(number "M1")
			)
			(pin power_in line
				(at -5.08 -67.31 90)
				(length 3.81)
				(name "DVSS2")
				(number "G12")
			)
			(pin power_in line
				(at -2.54 -67.31 90)
				(length 3.81)
				(name "DVSS3")
				(number "A5")
			)
			(pin power_in line
				(at 0 69.85 270)
				(length 3.81)
				(name "DVCC1")
				(number "L1")
			)
			(pin power_in line
				(at 2.54 69.85 270)
				(length 3.81)
				(name "DVCC2")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at 5.08 69.85 270)
				(length 3.81)
				(name "DVCC3")
				(number "A6")
			)
			(pin power_in line
				(at 5.08 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "E8")
			)
			(pin bidirectional line
				(at 10.16 69.85 270)
				(length 3.81)
				(name "VCORE")
				(number "M2")
			)
			(pin power_in line
				(at 10.16 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at 12.7 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at 15.24 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at 17.78 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 20.32 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at 22.86 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at 25.4 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 27.94 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "H9")
			)
			(pin input line
				(at 34.29 63.5 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "B6")
			)
			(pin bidirectional line
				(at 34.29 59.69 180)
				(length 3.81)
				(name "P1.0/TA0CLK/ACLK")
				(number "L5")
			)
			(pin bidirectional line
				(at 34.29 57.15 180)
				(length 3.81)
				(name "P1.1/TA0.0")
				(number "M5")
			)
			(pin bidirectional line
				(at 34.29 54.61 180)
				(length 3.81)
				(name "P1.2/TA0.1")
				(number "J6")
			)
			(pin bidirectional line
				(at 34.29 52.07 180)
				(length 3.81)
				(name "P1.3/TA0.2")
				(number "H6")
			)
			(pin bidirectional line
				(at 34.29 49.53 180)
				(length 3.81)
				(name "P1.4/TA0.3")
				(number "M6")
			)
			(pin bidirectional line
				(at 34.29 46.99 180)
				(length 3.81)
				(name "P1.5/TA0.4")
				(number "L6")
			)
			(pin bidirectional line
				(at 34.29 44.45 180)
				(length 3.81)
				(name "P1.6/TA0.1")
				(number "J7")
			)
			(pin bidirectional line
				(at 34.29 41.91 180)
				(length 3.81)
				(name "P1.7/TA0.2")
				(number "M7")
			)
			(pin bidirectional line
				(at 34.29 38.1 180)
				(length 3.81)
				(name "P2.0/P2MAP0")
				(number "G4")
			)
			(pin bidirectional line
				(at 34.29 35.56 180)
				(length 3.81)
				(name "P2.1/P2MAP1")
				(number "H2")
			)
			(pin bidirectional line
				(at 34.29 33.02 180)
				(length 3.81)
				(name "P2.2/P2MAP2")
				(number "J1")
			)
			(pin bidirectional line
				(at 34.29 30.48 180)
				(length 3.81)
				(name "P2.3/P2MAP3")
				(number "H4")
			)
			(pin bidirectional line
				(at 34.29 27.94 180)
				(length 3.81)
				(name "P2.4/P2MAP4")
				(number "J2")
			)
			(pin bidirectional line
				(at 34.29 25.4 180)
				(length 3.81)
				(name "P2.5/P2MAP5")
				(number "K1")
			)
			(pin bidirectional line
				(at 34.29 22.86 180)
				(length 3.81)
				(name "P2.6/P2MAP6")
				(number "K2")
			)
			(pin bidirectional line
				(at 34.29 20.32 180)
				(length 3.81)
				(name "P2.7/P2MAP7")
				(number "L2")
			)
			(pin bidirectional line
				(at 34.29 16.51 180)
				(length 3.81)
				(name "P3.0/TA1CLK/CBOUT")
				(number "L7")
			)
			(pin bidirectional line
				(at 34.29 13.97 180)
				(length 3.81)
				(name "P3.1/TA1.0")
				(number "H7")
			)
			(pin bidirectional line
				(at 34.29 11.43 180)
				(length 3.81)
				(name "P3.2/TA1.1")
				(number "M8")
			)
			(pin bidirectional line
				(at 34.29 8.89 180)
				(length 3.81)
				(name "P3.3/TA1.2")
				(number "L8")
			)
			(pin bidirectional line
				(at 34.29 6.35 180)
				(length 3.81)
				(name "P3.4/TA2CLK/SMCLK")
				(number "J8")
			)
			(pin bidirectional line
				(at 34.29 3.81 180)
				(length 3.81)
				(name "P3.5/TA2.0")
				(number "M9")
			)
			(pin bidirectional line
				(at 34.29 1.27 180)
				(length 3.81)
				(name "P3.6/TA2.1")
				(number "L9")
			)
			(pin bidirectional line
				(at 34.29 -1.27 180)
				(length 3.81)
				(name "P3.7/TA2.2")
				(number "M10")
			)
			(pin bidirectional line
				(at 34.29 -5.08 180)
				(length 3.81)
				(name "P4.0/TB0.0")
				(number "J9")
			)
			(pin bidirectional line
				(at 34.29 -7.62 180)
				(length 3.81)
				(name "P4.1/TB0.1")
				(number "M11")
			)
			(pin bidirectional line
				(at 34.29 -10.16 180)
				(length 3.81)
				(name "P4.2/TB0.2")
				(number "L10")
			)
			(pin bidirectional line
				(at 34.29 -12.7 180)
				(length 3.81)
				(name "P4.3/TB0.3")
				(number "M12")
			)
			(pin bidirectional line
				(at 34.29 -15.24 180)
				(length 3.81)
				(name "P4.4/TB0.4")
				(number "L12")
			)
			(pin bidirectional line
				(at 34.29 -17.78 180)
				(length 3.81)
				(name "P4.5/TB0.5")
				(number "L11")
			)
			(pin bidirectional line
				(at 34.29 -20.32 180)
				(length 3.81)
				(name "P4.6/TB0.6")
				(number "K11")
			)
			(pin bidirectional line
				(at 34.29 -22.86 180)
				(length 3.81)
				(name "P4.7/TB0OUTH/SVMOUT")
				(number "K12")
			)
			(pin bidirectional line
				(at 34.29 -26.67 180)
				(length 3.81)
				(name "P5.0/VREF+/VeREF+")
				(number "D4")
			)
			(pin bidirectional line
				(at 34.29 -29.21 180)
				(length 3.81)
				(name "P5.1/VREF-/VeREF-")
				(number "E4")
			)
			(pin bidirectional line
				(at 34.29 -31.75 180)
				(length 3.81)
				(name "P5.2")
				(number "L3")
			)
			(pin bidirectional line
				(at 34.29 -34.29 180)
				(length 3.81)
				(name "P5.3")
				(number "L4")
			)
			(pin bidirectional line
				(at 34.29 -36.83 180)
				(length 3.81)
				(name "P5.4")
				(number "M4")
			)
			(pin bidirectional line
				(at 34.29 -39.37 180)
				(length 3.81)
				(name "P5.5")
				(number "J5")
			)
			(pin bidirectional line
				(at 34.29 -41.91 180)
				(length 3.81)
				(name "P5.6/ADC12CLK/DMAE0")
				(number "H1")
			)
			(pin bidirectional line
				(at 34.29 -44.45 180)
				(length 3.81)
				(name "P5.7/RTCCLK")
				(number "D7")
			)
			(pin bidirectional line
				(at 34.29 -49.53 180)
				(length 3.81)
				(name "XIN")
				(number "F1")
			)
			(pin bidirectional line
				(at 34.29 -53.34 180)
				(length 3.81)
				(name "XOUT")
				(number "G1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5500IRGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "MSP430F5500IRGZ"
			(at 19.05 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5500.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "8kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
		(symbol "MSP430F5500IRGZ_0_1")
		(symbol "MSP430F5500IRGZ_1_1"
			(pin input line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 16.51 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 13.97 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 8.89 0)
				(length 3.81)
				(name "PUR")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 6.35 0)
				(length 3.81)
				(name "PU.0/DP")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 3.81 0)
				(length 3.81)
				(name "PU.1/DM")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "P6.0/CB0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "P6.1/CB1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "P6.2/CB2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "P6.3/CB3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "P5.0/VeREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "P5.1/VeREF-")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "9")
			)
			(pin power_in line
				(at -7.62 31.75 270)
				(length 3.81)
				(name "VBUS")
				(number "41")
			)
			(pin power_in line
				(at -6.35 -31.75 90)
				(length 3.81)
				(name "VSSU")
				(number "37")
			)
			(pin power_out line
				(at -5.08 31.75 270)
				(length 3.81)
				(name "VUSB")
				(number "42")
			)
			(pin power_in line
				(at -1.27 31.75 270)
				(length 3.81)
				(name "AVCC1")
				(number "7")
			)
			(pin power_in line
				(at -1.27 -31.75 90)
				(length 3.81)
				(name "AVSS1")
				(number "10")
			)
			(pin power_in line
				(at 1.27 -31.75 90)
				(length 3.81)
				(name "AVSS2")
				(number "44")
			)
			(pin power_in line
				(at 2.54 31.75 270)
				(length 3.81)
				(name "DVCC1")
				(number "11")
			)
			(pin power_in line
				(at 5.08 31.75 270)
				(length 3.81)
				(name "DVCC2")
				(number "28")
			)
			(pin power_in line
				(at 6.35 -31.75 90)
				(length 3.81)
				(name "DVSS1")
				(number "12")
			)
			(pin passive line
				(at 8.89 31.75 270)
				(length 3.81)
				(name "VCORE")
				(number "13")
			)
			(pin power_in line
				(at 8.89 -31.75 90)
				(length 3.81)
				(name "DVSS2")
				(number "27")
			)
			(pin passive line
				(at 11.43 31.75 270)
				(length 3.81)
				(name "V18")
				(number "43")
			)
			(pin input line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "P4.6")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "P4.7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5504IRGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 29.21 0)
		)
		(property "Value" "MSP430F5504IRGZ"
			(at 20.32 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -20.32 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5504.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
		(symbol "MSP430F5504IRGZ_0_1")
		(symbol "MSP430F5504IRGZ_1_1"
			(pin input line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 16.51 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 13.97 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "PUR")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "PU.0/DP")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "PU.1/DM")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "P6.0/A0")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "P6.1/A1")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "P6.2/A2")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "P6.3/A3")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "9")
			)
			(pin power_in line
				(at -7.62 31.75 270)
				(length 3.81)
				(name "VBUS")
				(number "41")
			)
			(pin power_in line
				(at -7.62 -31.75 90)
				(length 3.81)
				(name "VSSU")
				(number "37")
			)
			(pin power_out line
				(at -5.08 31.75 270)
				(length 3.81)
				(name "VUSB")
				(number "42")
			)
			(pin power_in line
				(at -2.54 -31.75 90)
				(length 3.81)
				(name "AVSS1")
				(number "10")
			)
			(pin power_in line
				(at 0 31.75 270)
				(length 3.81)
				(name "AVCC1")
				(number "7")
			)
			(pin power_in line
				(at 0 -31.75 90)
				(length 3.81)
				(name "AVSS2")
				(number "44")
			)
			(pin power_in line
				(at 5.08 31.75 270)
				(length 3.81)
				(name "DVCC1")
				(number "11")
			)
			(pin power_in line
				(at 5.08 -31.75 90)
				(length 3.81)
				(name "DVSS1")
				(number "12")
			)
			(pin power_in line
				(at 7.62 31.75 270)
				(length 3.81)
				(name "DVCC2")
				(number "28")
			)
			(pin power_in line
				(at 7.62 -31.75 90)
				(length 3.81)
				(name "DVSS2")
				(number "27")
			)
			(pin passive line
				(at 11.43 31.75 270)
				(length 3.81)
				(name "VCORE")
				(number "13")
			)
			(pin passive line
				(at 13.97 31.75 270)
				(length 3.81)
				(name "V18")
				(number "43")
			)
			(pin input line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "47")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "29")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "30")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "32")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "P4.6")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "P4.7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5508IRGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "MSP430F5508IRGZ"
			(at 19.05 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5508.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "16kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
		(symbol "MSP430F5508IRGZ_0_1")
		(symbol "MSP430F5508IRGZ_1_1"
			(pin input line
				(at -29.21 25.4 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "48")
			)
			(pin bidirectional line
				(at -29.21 21.59 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "23")
			)
			(pin bidirectional line
				(at -29.21 19.05 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -29.21 16.51 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "25")
			)
			(pin bidirectional line
				(at -29.21 13.97 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "26")
			)
			(pin bidirectional line
				(at -29.21 10.16 0)
				(length 3.81)
				(name "PUR")
				(number "39")
			)
			(pin bidirectional line
				(at -29.21 7.62 0)
				(length 3.81)
				(name "PU.0/DP")
				(number "38")
			)
			(pin bidirectional line
				(at -29.21 5.08 0)
				(length 3.81)
				(name "PU.1/DM")
				(number "40")
			)
			(pin bidirectional line
				(at -29.21 0 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "1")
			)
			(pin bidirectional line
				(at -29.21 -2.54 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "2")
			)
			(pin bidirectional line
				(at -29.21 -5.08 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "3")
			)
			(pin bidirectional line
				(at -29.21 -7.62 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "4")
			)
			(pin bidirectional line
				(at -29.21 -12.7 0)
				(length 3.81)
				(name "P5.0/A8/VeREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -29.21 -15.24 0)
				(length 3.81)
				(name "P5.1/A9/VeREF-")
				(number "6")
			)
			(pin bidirectional line
				(at -29.21 -17.78 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "45")
			)
			(pin bidirectional line
				(at -29.21 -20.32 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "46")
			)
			(pin bidirectional line
				(at -29.21 -22.86 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "8")
			)
			(pin bidirectional line
				(at -29.21 -25.4 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "9")
			)
			(pin power_in line
				(at -6.35 31.75 270)
				(length 3.81)
				(name "VBUS")
				(number "41")
			)
			(pin power_in line
				(at -6.35 -31.75 90)
				(length 3.81)
				(name "VSSU")
				(number "37")
			)
			(pin power_out line
				(at -3.81 31.75 270)
				(length 3.81)
				(name "VUSB")
				(number "42")
			)
			(pin power_in line
				(at -1.27 -31.75 90)
				(length 3.81)
				(name "AVSS1")
				(number "10")
			)
			(pin power_in line
				(at 0 31.75 270)
				(length 3.81)
				(name "AVCC1")
				(number "7")
			)
			(pin power_in line
				(at 1.27 -31.75 90)
				(length 3.81)
				(name "AVSS2")
				(number "44")
			)
			(pin power_in line
				(at 3.81 31.75 270)
				(length 3.81)
				(name "DVCC1")
				(number "11")
			)
			(pin power_in line
				(at 6.35 31.75 270)
				(length 3.81)
				(name "DVCC2")
				(number "28")
			)
			(pin power_in line
				(at 6.35 -31.75 90)
				(length 3.81)
				(name "DVSS1")
				(number "12")
			)
			(pin power_in line
				(at 8.89 -31.75 90)
				(length 3.81)
				(name "DVSS2")
				(number "27")
			)
			(pin passive line
				(at 10.16 31.75 270)
				(length 3.81)
				(name "VCORE")
				(number "13")
			)
			(pin passive line
				(at 12.7 31.75 270)
				(length 3.81)
				(name "V18")
				(number "43")
			)
			(pin input line
				(at 31.75 25.4 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "47")
			)
			(pin bidirectional line
				(at 31.75 20.32 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "14")
			)
			(pin bidirectional line
				(at 31.75 17.78 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "15")
			)
			(pin bidirectional line
				(at 31.75 15.24 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "16")
			)
			(pin bidirectional line
				(at 31.75 12.7 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "17")
			)
			(pin bidirectional line
				(at 31.75 10.16 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "18")
			)
			(pin bidirectional line
				(at 31.75 7.62 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "19")
			)
			(pin bidirectional line
				(at 31.75 5.08 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P1.6")
				(number "20")
			)
			(pin bidirectional line
				(at 31.75 2.54 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "21")
			)
			(pin bidirectional line
				(at 31.75 -2.54 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "22")
			)
			(pin bidirectional line
				(at 31.75 -7.62 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "29")
			)
			(pin bidirectional line
				(at 31.75 -10.16 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "30")
			)
			(pin bidirectional line
				(at 31.75 -12.7 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "31")
			)
			(pin bidirectional line
				(at 31.75 -15.24 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "32")
			)
			(pin bidirectional line
				(at 31.75 -17.78 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "33")
			)
			(pin bidirectional line
				(at 31.75 -20.32 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "34")
			)
			(pin bidirectional line
				(at 31.75 -22.86 180)
				(length 3.81)
				(name "P4.6")
				(number "35")
			)
			(pin bidirectional line
				(at 31.75 -25.4 180)
				(length 3.81)
				(name "P4.7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5524IYFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 43.18 0)
		)
		(property "Value" "MSP430F5524IYFF"
			(at 16.51 -43.18 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-64_3.415x3.535mm_Layout8x8_P0.4mm"
			(at -24.13 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5524.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "64kB Flash, 4kB + 2kB RAM, BGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.415x3.535mm*Layout8x8*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5524IYFF_0_1")
		(symbol "MSP430F5524IYFF_1_1"
			(pin input line
				(at -30.48 39.37 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "D5")
			)
			(pin bidirectional line
				(at -30.48 34.29 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 31.75 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 29.21 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 26.67 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "C2")
			)
			(pin power_in line
				(at -30.48 21.59 0)
				(length 3.81)
				(name "VBUS")
				(number "F2")
			)
			(pin power_out line
				(at -30.48 19.05 0)
				(length 3.81)
				(name "VUSB")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 13.97 0)
				(length 3.81)
				(name "PUR")
				(number "G2")
			)
			(pin bidirectional line
				(at -30.48 11.43 0)
				(length 3.81)
				(name "PU.0/DP")
				(number "H1")
			)
			(pin bidirectional line
				(at -30.48 8.89 0)
				(length 3.81)
				(name "PU.1/DM")
				(number "G1")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "P5.0/A8/VREF+/VeREF+")
				(number "B4")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "P5.1/A9/VREF-/VeREF-")
				(number "B5")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "P5.2/XT2IN")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "P5.3/XT2OUT")
				(number "D1")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "P5.4/XIN")
				(number "A5")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "P5.5/XOUT")
				(number "A6")
			)
			(pin bidirectional line
				(at -30.48 -21.59 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "B1")
			)
			(pin bidirectional line
				(at -30.48 -24.13 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 -26.67 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "A1")
			)
			(pin bidirectional line
				(at -30.48 -29.21 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "C4")
			)
			(pin bidirectional line
				(at -30.48 -31.75 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "B2")
			)
			(pin bidirectional line
				(at -30.48 -34.29 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "B3")
			)
			(pin bidirectional line
				(at -30.48 -36.83 0)
				(length 3.81)
				(name "P6.6/CB6/A6")
				(number "A2")
			)
			(pin bidirectional line
				(at -30.48 -39.37 0)
				(length 3.81)
				(name "P6.7/CB7/A7")
				(number "C5")
			)
			(pin power_in line
				(at -11.43 -45.72 90)
				(length 3.81)
				(name "VSSU")
				(number "H2")
			)
			(pin power_in line
				(at -6.35 45.72 270)
				(length 3.81)
				(name "AVCC1")
				(number "A3")
			)
			(pin power_in line
				(at -6.35 -45.72 90)
				(length 3.81)
				(name "AVSS1")
				(number "A4")
			)
			(pin power_in line
				(at -3.81 -45.72 90)
				(length 3.81)
				(name "AVSS2")
				(number "D2")
			)
			(pin power_in line
				(at -1.27 45.72 270)
				(length 3.81)
				(name "DVCC1")
				(number "A7")
			)
			(pin power_in line
				(at 1.27 45.72 270)
				(length 3.81)
				(name "DVCC2")
				(number "H5")
			)
			(pin power_in line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "DVSS1")
				(number "A8")
			)
			(pin power_in line
				(at 3.81 -45.72 90)
				(length 3.81)
				(name "DVSS2")
				(number "H6")
			)
			(pin bidirectional line
				(at 6.35 45.72 270)
				(length 3.81)
				(name "VCORE")
				(number "B8")
			)
			(pin passive line
				(at 8.89 45.72 270)
				(length 3.81)
				(name "V18")
				(number "E2")
			)
			(pin input line
				(at 30.48 39.37 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "E3")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "C7")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "D6")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P1.6")
				(number "D7")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "TA1.0/P1.7")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 13.97 180)
				(length 3.81)
				(name "TA1.1/P2.0")
				(number "E5")
			)
			(pin bidirectional line
				(at 30.48 11.43 180)
				(length 3.81)
				(name "TA1.2/P2.1")
				(number "E8")
			)
			(pin bidirectional line
				(at 30.48 8.89 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P2.2")
				(number "E7")
			)
			(pin bidirectional line
				(at 30.48 6.35 180)
				(length 3.81)
				(name "TA2.0/P2.3")
				(number "E6")
			)
			(pin bidirectional line
				(at 30.48 3.81 180)
				(length 3.81)
				(name "TA2.1/P2.4")
				(number "F8")
			)
			(pin bidirectional line
				(at 30.48 1.27 180)
				(length 3.81)
				(name "TA2.2/P2.5")
				(number "F7")
			)
			(pin bidirectional line
				(at 30.48 -1.27 180)
				(length 3.81)
				(name "RTCCLK/DMAE0/P2.6")
				(number "F6")
			)
			(pin bidirectional line
				(at 30.48 -3.81 180)
				(length 3.81)
				(name "UCB0STE/UCA0CLK/P2.7")
				(number "H8")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "UCB0SIMO/UCB0SDA/P3.0")
				(number "G8")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "UCB0SOMI/UCB0SCL/P3.1")
				(number "H7")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "UCB0CLK/UCA0STE/P3.2")
				(number "G7")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/P3.3")
				(number "G6")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/P3.4")
				(number "G5")
			)
			(pin bidirectional line
				(at 30.48 -21.59 180)
				(length 3.81)
				(name "PM_UCB1STE/PM_UCA1CLK/P4.0")
				(number "F5")
			)
			(pin bidirectional line
				(at 30.48 -24.13 180)
				(length 3.81)
				(name "PM_UCB1SIMO/PM_UCB1SDA/P4.1")
				(number "H4")
			)
			(pin bidirectional line
				(at 30.48 -26.67 180)
				(length 3.81)
				(name "PM_UCB1SOMI/PM_UCB1SCL/P4.2")
				(number "G4")
			)
			(pin bidirectional line
				(at 30.48 -29.21 180)
				(length 3.81)
				(name "PM_UCB1CLK/PM_UCA1STE/P4.3")
				(number "F4")
			)
			(pin bidirectional line
				(at 30.48 -31.75 180)
				(length 3.81)
				(name "PM_UCA1TXD/PM_UCA1SIMO/P4.4")
				(number "H3")
			)
			(pin bidirectional line
				(at 30.48 -34.29 180)
				(length 3.81)
				(name "PM_UCA1RXD/PM_UCA1SOMI/P4.5")
				(number "G3")
			)
			(pin bidirectional line
				(at 30.48 -36.83 180)
				(length 3.81)
				(name "P4.6")
				(number "F3")
			)
			(pin bidirectional line
				(at 30.48 -39.37 180)
				(length 3.81)
				(name "P4.7")
				(number "E4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5630IZQW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 66.04 0)
		)
		(property "Value" "MSP430F5630IZQW"
			(at -29.21 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5630.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 16kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5630IZQW_0_1")
		(symbol "MSP430F5630IZQW_1_1"
			(pin input line
				(at -33.02 60.96 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "A3")
			)
			(pin bidirectional line
				(at -33.02 57.15 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "B5")
			)
			(pin bidirectional line
				(at -33.02 54.61 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "A4")
			)
			(pin bidirectional line
				(at -33.02 52.07 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "E7")
			)
			(pin bidirectional line
				(at -33.02 49.53 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "D6")
			)
			(pin bidirectional line
				(at -33.02 44.45 0)
				(length 3.81)
				(name "VBAK")
				(number "A7")
			)
			(pin bidirectional line
				(at -33.02 41.91 0)
				(length 3.81)
				(name "VBAT")
				(number "D8")
			)
			(pin bidirectional line
				(at -33.02 36.83 0)
				(length 3.81)
				(name "VBUS")
				(number "A10")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "VUSB")
				(number "A9")
			)
			(pin bidirectional line
				(at -33.02 29.21 0)
				(length 3.81)
				(name "PUR")
				(number "B10")
			)
			(pin bidirectional line
				(at -33.02 26.67 0)
				(length 3.81)
				(name "PU.0/DP")
				(number "A12")
			)
			(pin bidirectional line
				(at -33.02 24.13 0)
				(length 3.81)
				(name "PU.1/DM")
				(number "A11")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "P9.0")
				(number "E11")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "P9.1")
				(number "F9")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "P9.2")
				(number "D12")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "P9.3")
				(number "D11")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "P9.4")
				(number "E9")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P9.5")
				(number "C12")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P9.6")
				(number "C11")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P9.7")
				(number "D9")
			)
			(pin bidirectional line
				(at -33.02 -1.27 0)
				(length 3.81)
				(name "P8.0/TB0CLK")
				(number "J11")
			)
			(pin bidirectional line
				(at -33.02 -3.81 0)
				(length 3.81)
				(name "P8.1/UCB1STE/UCA1CLK")
				(number "J12")
			)
			(pin bidirectional line
				(at -33.02 -6.35 0)
				(length 3.81)
				(name "P8.2/UCA1TXD/UCA1SIMO")
				(number "H11")
			)
			(pin bidirectional line
				(at -33.02 -8.89 0)
				(length 3.81)
				(name "P8.3/UCA1RXD/UCA1SOMI")
				(number "H12")
			)
			(pin bidirectional line
				(at -33.02 -11.43 0)
				(length 3.81)
				(name "P8.4/UCB1CLK/UCA1STE")
				(number "G11")
			)
			(pin bidirectional line
				(at -33.02 -13.97 0)
				(length 3.81)
				(name "P8.5/UCB1SIMO/UCB1SDA")
				(number "F11")
			)
			(pin bidirectional line
				(at -33.02 -16.51 0)
				(length 3.81)
				(name "P8.6/UCB1SOMI/UCB1SCL")
				(number "G9")
			)
			(pin bidirectional line
				(at -33.02 -19.05 0)
				(length 3.81)
				(name "P8.7")
				(number "E12")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "P7.2/XT2IN")
				(number "B8")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 3.81)
				(name "P7.3/XT2OUT")
				(number "B7")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 3.81)
				(name "P7.4/CB8")
				(number "C1")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 3.81)
				(name "P7.5/CB9")
				(number "C3")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 3.81)
				(name "P7.6/CB10")
				(number "D2")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 3.81)
				(name "P7.7/CB11")
				(number "D1")
			)
			(pin bidirectional line
				(at -33.02 -39.37 0)
				(length 3.81)
				(name "P6.0/CB0")
				(number "B4")
			)
			(pin bidirectional line
				(at -33.02 -41.91 0)
				(length 3.81)
				(name "P6.1/CB1")
				(number "B3")
			)
			(pin bidirectional line
				(at -33.02 -44.45 0)
				(length 3.81)
				(name "P6.2/CB2")
				(number "A2")
			)
			(pin bidirectional line
				(at -33.02 -46.99 0)
				(length 3.81)
				(name "P6.3/CB3")
				(number "D5")
			)
			(pin bidirectional line
				(at -33.02 -49.53 0)
				(length 3.81)
				(name "P6.4/CB4")
				(number "A1")
			)
			(pin bidirectional line
				(at -33.02 -52.07 0)
				(length 3.81)
				(name "P6.5/CB5")
				(number "B2")
			)
			(pin bidirectional line
				(at -33.02 -54.61 0)
				(length 3.81)
				(name "P6.6/CB6")
				(number "B1")
			)
			(pin bidirectional line
				(at -33.02 -57.15 0)
				(length 3.81)
				(name "P6.7/CB7")
				(number "C2")
			)
			(pin power_in line
				(at -26.67 -67.31 90)
				(length 3.81)
				(name "VSSU")
				(number "B11")
			)
			(pin power_in line
				(at -24.13 -67.31 90)
				(length 3.81)
				(name "VSSU")
				(number "B12")
			)
			(pin power_in line
				(at -19.05 -67.31 90)
				(length 3.81)
				(name "AVSS1")
				(number "F2")
			)
			(pin power_in line
				(at -16.51 -67.31 90)
				(length 3.81)
				(name "AVSS2")
				(number "G2")
			)
			(pin power_in line
				(at -13.97 -67.31 90)
				(length 3.81)
				(name "AVSS3")
				(number "A8")
			)
			(pin power_in line
				(at -10.16 67.31 270)
				(length 3.81)
				(name "AVCC1")
				(number "E1")
			)
			(pin power_in line
				(at -10.16 -67.31 90)
				(length 3.81)
				(name "DVSS")
				(number "M3")
			)
			(pin power_in line
				(at -7.62 67.31 270)
				(length 3.81)
				(name "AVCC1")
				(number "E2")
			)
			(pin power_in line
				(at -7.62 -67.31 90)
				(length 3.81)
				(name "DVSS1")
				(number "M1")
			)
			(pin power_in line
				(at -5.08 -67.31 90)
				(length 3.81)
				(name "DVSS2")
				(number "G12")
			)
			(pin power_in line
				(at -2.54 67.31 270)
				(length 3.81)
				(name "DVCC1")
				(number "L1")
			)
			(pin power_in line
				(at -2.54 -67.31 90)
				(length 3.81)
				(name "DVSS3")
				(number "A5")
			)
			(pin power_in line
				(at 0 67.31 270)
				(length 3.81)
				(name "DVCC2")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 67.31 270)
				(length 3.81)
				(name "DVCC3")
				(number "A6")
			)
			(pin power_in line
				(at 2.54 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at 5.08 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "E6")
			)
			(pin bidirectional line
				(at 7.62 67.31 270)
				(length 3.81)
				(name "VCORE")
				(number "M2")
			)
			(pin power_in line
				(at 7.62 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "F4")
			)
			(pin passive line
				(at 11.43 67.31 270)
				(length 3.81)
				(name "V18")
				(number "B9")
			)
			(pin power_in line
				(at 12.7 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at 15.24 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at 17.78 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 20.32 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at 22.86 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at 25.4 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 27.94 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "H9")
			)
			(pin input line
				(at 33.02 60.96 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "B6")
			)
			(pin bidirectional line
				(at 33.02 57.15 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "L5")
			)
			(pin bidirectional line
				(at 33.02 54.61 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "M5")
			)
			(pin bidirectional line
				(at 33.02 52.07 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "J6")
			)
			(pin bidirectional line
				(at 33.02 49.53 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "H6")
			)
			(pin bidirectional line
				(at 33.02 46.99 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "M6")
			)
			(pin bidirectional line
				(at 33.02 44.45 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "L6")
			)
			(pin bidirectional line
				(at 33.02 41.91 180)
				(length 3.81)
				(name "TA0.1/P1.6")
				(number "J7")
			)
			(pin bidirectional line
				(at 33.02 39.37 180)
				(length 3.81)
				(name "TA0.2/P1.7")
				(number "M7")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "P2MAP0/P2.0")
				(number "G4")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "P2MAP1/P2.1")
				(number "H2")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "P2MAP2/P2.2")
				(number "J1")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "P2MAP3/P2.3")
				(number "H4")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "P2MAP4/P2.4")
				(number "J2")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "P2MAP5/P2.5")
				(number "K1")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "P2MAP6/P2.6")
				(number "K2")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "P2MAP7/P2.7")
				(number "L2")
			)
			(pin bidirectional line
				(at 33.02 13.97 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P3.0")
				(number "L7")
			)
			(pin bidirectional line
				(at 33.02 11.43 180)
				(length 3.81)
				(name "TA1.0/P3.1")
				(number "H7")
			)
			(pin bidirectional line
				(at 33.02 8.89 180)
				(length 3.81)
				(name "TA1.1/P3.2")
				(number "M8")
			)
			(pin bidirectional line
				(at 33.02 6.35 180)
				(length 3.81)
				(name "TA1.2/P3.3")
				(number "L8")
			)
			(pin bidirectional line
				(at 33.02 3.81 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P3.4")
				(number "J8")
			)
			(pin bidirectional line
				(at 33.02 1.27 180)
				(length 3.81)
				(name "TA2.0/P3.5")
				(number "M9")
			)
			(pin bidirectional line
				(at 33.02 -1.27 180)
				(length 3.81)
				(name "TA2.1/P3.6")
				(number "L9")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA2.2/P3.7")
				(number "M10")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "TB0.0/P4.0")
				(number "J9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "TB0.1/P4.1")
				(number "M11")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "TB0.2/P4.2")
				(number "L10")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "TB0.3/P4.3")
				(number "M12")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "TB0.4/P4.4")
				(number "L12")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "TB0.5/P4.5")
				(number "L11")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "TB0.6/P4.6")
				(number "K11")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "TB0OUTH/SVMOUT/P4.7")
				(number "K12")
			)
			(pin bidirectional line
				(at 33.02 -29.21 180)
				(length 3.81)
				(name "VREF+/VeREF+/P5.0")
				(number "D4")
			)
			(pin bidirectional line
				(at 33.02 -31.75 180)
				(length 3.81)
				(name "VREF-/VeREF-/P5.1")
				(number "E4")
			)
			(pin bidirectional line
				(at 33.02 -34.29 180)
				(length 3.81)
				(name "P5.2")
				(number "L3")
			)
			(pin bidirectional line
				(at 33.02 -36.83 180)
				(length 3.81)
				(name "P5.3")
				(number "L4")
			)
			(pin bidirectional line
				(at 33.02 -39.37 180)
				(length 3.81)
				(name "P5.4")
				(number "M4")
			)
			(pin bidirectional line
				(at 33.02 -41.91 180)
				(length 3.81)
				(name "P5.5")
				(number "J5")
			)
			(pin bidirectional line
				(at 33.02 -44.45 180)
				(length 3.81)
				(name "DMAE0/P5.6")
				(number "H1")
			)
			(pin bidirectional line
				(at 33.02 -46.99 180)
				(length 3.81)
				(name "RTCCLK/P5.7")
				(number "D7")
			)
			(pin bidirectional line
				(at 33.02 -52.07 180)
				(length 3.81)
				(name "XIN")
				(number "F1")
			)
			(pin bidirectional line
				(at 33.02 -57.15 180)
				(length 3.81)
				(name "XOUT")
				(number "G1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5633IZQW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 66.04 0)
		)
		(property "Value" "MSP430F5633IZQW"
			(at -29.21 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5633.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 16kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5633IZQW_0_1")
		(symbol "MSP430F5633IZQW_1_1"
			(pin input line
				(at -33.02 60.96 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "A3")
			)
			(pin bidirectional line
				(at -33.02 57.15 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "B5")
			)
			(pin bidirectional line
				(at -33.02 54.61 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "A4")
			)
			(pin bidirectional line
				(at -33.02 52.07 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "E7")
			)
			(pin bidirectional line
				(at -33.02 49.53 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "D6")
			)
			(pin bidirectional line
				(at -33.02 44.45 0)
				(length 3.81)
				(name "VBAK")
				(number "A7")
			)
			(pin bidirectional line
				(at -33.02 41.91 0)
				(length 3.81)
				(name "VBAT")
				(number "D8")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 3.81)
				(name "VBUS")
				(number "A10")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "VUSB")
				(number "A9")
			)
			(pin bidirectional line
				(at -33.02 29.21 0)
				(length 3.81)
				(name "PUR")
				(number "B10")
			)
			(pin bidirectional line
				(at -33.02 26.67 0)
				(length 3.81)
				(name "PU.0/DP")
				(number "A12")
			)
			(pin bidirectional line
				(at -33.02 24.13 0)
				(length 3.81)
				(name "PU.1/DM")
				(number "A11")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "P9.0")
				(number "E11")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "P9.1")
				(number "F9")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "P9.2")
				(number "D12")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "P9.3")
				(number "D11")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "P9.4")
				(number "E9")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P9.5")
				(number "C12")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P9.6")
				(number "C11")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P9.7")
				(number "D9")
			)
			(pin bidirectional line
				(at -33.02 -1.27 0)
				(length 3.81)
				(name "P8.0/TB0CLK")
				(number "J11")
			)
			(pin bidirectional line
				(at -33.02 -3.81 0)
				(length 3.81)
				(name "P8.1/UCB1STE/UCA1CLK")
				(number "J12")
			)
			(pin bidirectional line
				(at -33.02 -6.35 0)
				(length 3.81)
				(name "P8.2/UCA1TXD/UCA1SIMO")
				(number "H11")
			)
			(pin bidirectional line
				(at -33.02 -8.89 0)
				(length 3.81)
				(name "P8.3/UCA1RXD/UCA1SOMI")
				(number "H12")
			)
			(pin bidirectional line
				(at -33.02 -11.43 0)
				(length 3.81)
				(name "P8.4/UCB1CLK/UCA1STE")
				(number "G11")
			)
			(pin bidirectional line
				(at -33.02 -13.97 0)
				(length 3.81)
				(name "P8.5/UCB1SIMO/UCB1SDA")
				(number "F11")
			)
			(pin bidirectional line
				(at -33.02 -16.51 0)
				(length 3.81)
				(name "P8.6/UCB1SOMI/UCB1SCL")
				(number "G9")
			)
			(pin bidirectional line
				(at -33.02 -19.05 0)
				(length 3.81)
				(name "P8.7")
				(number "E12")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "P7.2/XT2IN")
				(number "B8")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 3.81)
				(name "P7.3/XT2OUT")
				(number "B7")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 3.81)
				(name "P7.4/CB8/A12")
				(number "C1")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 3.81)
				(name "P7.5/CB9/A13")
				(number "C3")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 3.81)
				(name "P7.6/CB10/A14")
				(number "D2")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 3.81)
				(name "P7.7/CB11/A15")
				(number "D1")
			)
			(pin bidirectional line
				(at -33.02 -39.37 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "B4")
			)
			(pin bidirectional line
				(at -33.02 -41.91 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "B3")
			)
			(pin bidirectional line
				(at -33.02 -44.45 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "A2")
			)
			(pin bidirectional line
				(at -33.02 -46.99 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "D5")
			)
			(pin bidirectional line
				(at -33.02 -49.53 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "A1")
			)
			(pin bidirectional line
				(at -33.02 -52.07 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "B2")
			)
			(pin bidirectional line
				(at -33.02 -54.61 0)
				(length 3.81)
				(name "P6.6/CB6/A6")
				(number "B1")
			)
			(pin bidirectional line
				(at -33.02 -57.15 0)
				(length 3.81)
				(name "P6.7/CB7/A7")
				(number "C2")
			)
			(pin power_in line
				(at -26.67 -68.58 90)
				(length 3.81)
				(name "VSSU")
				(number "B11")
			)
			(pin power_in line
				(at -24.13 -68.58 90)
				(length 3.81)
				(name "VSSU")
				(number "B12")
			)
			(pin power_in line
				(at -19.05 -68.58 90)
				(length 3.81)
				(name "AVSS1")
				(number "F2")
			)
			(pin power_in line
				(at -16.51 -68.58 90)
				(length 3.81)
				(name "AVSS2")
				(number "G2")
			)
			(pin power_in line
				(at -13.97 -68.58 90)
				(length 3.81)
				(name "AVSS3")
				(number "A8")
			)
			(pin power_in line
				(at -10.16 67.31 270)
				(length 3.81)
				(name "AVCC1")
				(number "E1")
			)
			(pin power_in line
				(at -10.16 -68.58 90)
				(length 3.81)
				(name "DVSS")
				(number "M3")
			)
			(pin power_in line
				(at -7.62 67.31 270)
				(length 3.81)
				(name "AVCC1")
				(number "E2")
			)
			(pin power_in line
				(at -7.62 -68.58 90)
				(length 3.81)
				(name "DVSS1")
				(number "M1")
			)
			(pin power_in line
				(at -5.08 -68.58 90)
				(length 3.81)
				(name "DVSS2")
				(number "G12")
			)
			(pin power_in line
				(at -2.54 67.31 270)
				(length 3.81)
				(name "DVCC1")
				(number "L1")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 3.81)
				(name "DVSS3")
				(number "A5")
			)
			(pin power_in line
				(at 0 67.31 270)
				(length 3.81)
				(name "DVCC2")
				(number "F12")
			)
			(pin power_in line
				(at 1.27 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 67.31 270)
				(length 3.81)
				(name "DVCC3")
				(number "A6")
			)
			(pin power_in line
				(at 3.81 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at 6.35 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E8")
			)
			(pin bidirectional line
				(at 7.62 67.31 270)
				(length 3.81)
				(name "VCORE")
				(number "M2")
			)
			(pin power_in line
				(at 8.89 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F4")
			)
			(pin passive line
				(at 11.43 67.31 270)
				(length 3.81)
				(name "V18")
				(number "B9")
			)
			(pin power_in line
				(at 11.43 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at 13.97 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at 16.51 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 19.05 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at 21.59 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at 24.13 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 26.67 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H9")
			)
			(pin input line
				(at 33.02 60.96 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "B6")
			)
			(pin bidirectional line
				(at 33.02 57.15 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "L5")
			)
			(pin bidirectional line
				(at 33.02 54.61 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "M5")
			)
			(pin bidirectional line
				(at 33.02 52.07 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "J6")
			)
			(pin bidirectional line
				(at 33.02 49.53 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "H6")
			)
			(pin bidirectional line
				(at 33.02 46.99 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "M6")
			)
			(pin bidirectional line
				(at 33.02 44.45 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "L6")
			)
			(pin bidirectional line
				(at 33.02 41.91 180)
				(length 3.81)
				(name "TA0.1/P1.6")
				(number "J7")
			)
			(pin bidirectional line
				(at 33.02 39.37 180)
				(length 3.81)
				(name "TA0.2/P1.7")
				(number "M7")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "P2MAP0/P2.0")
				(number "G4")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "P2MAP1/P2.1")
				(number "H2")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "P2MAP2/P2.2")
				(number "J1")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "P2MAP3/P2.3")
				(number "H4")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "P2MAP4/P2.4")
				(number "J2")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "P2MAP5/P2.5")
				(number "K1")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "P2MAP6/P2.6")
				(number "K2")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "P2MAP7/P2.7")
				(number "L2")
			)
			(pin bidirectional line
				(at 33.02 13.97 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P3.0")
				(number "L7")
			)
			(pin bidirectional line
				(at 33.02 11.43 180)
				(length 3.81)
				(name "TA1.0/P3.1")
				(number "H7")
			)
			(pin bidirectional line
				(at 33.02 8.89 180)
				(length 3.81)
				(name "TA1.1/P3.2")
				(number "M8")
			)
			(pin bidirectional line
				(at 33.02 6.35 180)
				(length 3.81)
				(name "TA1.2/P3.3")
				(number "L8")
			)
			(pin bidirectional line
				(at 33.02 3.81 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P3.4")
				(number "J8")
			)
			(pin bidirectional line
				(at 33.02 1.27 180)
				(length 3.81)
				(name "TA2.0/P3.5")
				(number "M9")
			)
			(pin bidirectional line
				(at 33.02 -1.27 180)
				(length 3.81)
				(name "TA2.1/P3.6")
				(number "L9")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA2.2/P3.7")
				(number "M10")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "TB0.0/P4.0")
				(number "J9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "TB0.1/P4.1")
				(number "M11")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "TB0.2/P4.2")
				(number "L10")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "TB0.3/P4.3")
				(number "M12")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "TB0.4/P4.4")
				(number "L12")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "TB0.5/P4.5")
				(number "L11")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "TB0.6/P4.6")
				(number "K11")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "TB0OUTH/SVMOUT/P4.7")
				(number "K12")
			)
			(pin bidirectional line
				(at 33.02 -29.21 180)
				(length 3.81)
				(name "VREF+/VeREF+/P5.0")
				(number "D4")
			)
			(pin bidirectional line
				(at 33.02 -31.75 180)
				(length 3.81)
				(name "VREF-/VeREF-/P5.1")
				(number "E4")
			)
			(pin bidirectional line
				(at 33.02 -34.29 180)
				(length 3.81)
				(name "P5.2")
				(number "L3")
			)
			(pin bidirectional line
				(at 33.02 -36.83 180)
				(length 3.81)
				(name "P5.3")
				(number "L4")
			)
			(pin bidirectional line
				(at 33.02 -39.37 180)
				(length 3.81)
				(name "P5.4")
				(number "M4")
			)
			(pin bidirectional line
				(at 33.02 -41.91 180)
				(length 3.81)
				(name "P5.5")
				(number "J5")
			)
			(pin bidirectional line
				(at 33.02 -44.45 180)
				(length 3.81)
				(name "ADC12CLK/DMAE0/P5.6")
				(number "H1")
			)
			(pin bidirectional line
				(at 33.02 -46.99 180)
				(length 3.81)
				(name "RTCCLK/P5.7")
				(number "D7")
			)
			(pin bidirectional line
				(at 33.02 -52.07 180)
				(length 3.81)
				(name "XIN")
				(number "F1")
			)
			(pin bidirectional line
				(at 33.02 -57.15 180)
				(length 3.81)
				(name "XOUT")
				(number "G1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5636IZQW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 66.04 0)
		)
		(property "Value" "MSP430F5636IZQW"
			(at -29.21 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 25.4 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5636.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 16kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5636IZQW_0_1")
		(symbol "MSP430F5636IZQW_1_1"
			(pin input line
				(at -33.02 60.96 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "A3")
			)
			(pin bidirectional line
				(at -33.02 57.15 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "B5")
			)
			(pin bidirectional line
				(at -33.02 54.61 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "A4")
			)
			(pin bidirectional line
				(at -33.02 52.07 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "E7")
			)
			(pin bidirectional line
				(at -33.02 49.53 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "D6")
			)
			(pin bidirectional line
				(at -33.02 44.45 0)
				(length 3.81)
				(name "VBAK")
				(number "A7")
			)
			(pin bidirectional line
				(at -33.02 41.91 0)
				(length 3.81)
				(name "VBAT")
				(number "D8")
			)
			(pin bidirectional line
				(at -33.02 36.83 0)
				(length 3.81)
				(name "VBUS")
				(number "A10")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "VUSB")
				(number "A9")
			)
			(pin bidirectional line
				(at -33.02 29.21 0)
				(length 3.81)
				(name "PUR")
				(number "B10")
			)
			(pin bidirectional line
				(at -33.02 26.67 0)
				(length 3.81)
				(name "PU.0/DP")
				(number "A12")
			)
			(pin bidirectional line
				(at -33.02 24.13 0)
				(length 3.81)
				(name "PU.1/DM")
				(number "A11")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "P9.0")
				(number "E11")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "P9.1")
				(number "F9")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "P9.2")
				(number "D12")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "P9.3")
				(number "D11")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "P9.4")
				(number "E9")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P9.5")
				(number "C12")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P9.6")
				(number "C11")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P9.7")
				(number "D9")
			)
			(pin bidirectional line
				(at -33.02 -1.27 0)
				(length 3.81)
				(name "P8.0/TB0CLK")
				(number "J11")
			)
			(pin bidirectional line
				(at -33.02 -3.81 0)
				(length 3.81)
				(name "P8.1/UCB1STE/UCA1CLK")
				(number "J12")
			)
			(pin bidirectional line
				(at -33.02 -6.35 0)
				(length 3.81)
				(name "P8.2/UCA1TXD/UCA1SIMO")
				(number "H11")
			)
			(pin bidirectional line
				(at -33.02 -8.89 0)
				(length 3.81)
				(name "P8.3/UCA1RXD/UCA1SOMI")
				(number "H12")
			)
			(pin bidirectional line
				(at -33.02 -11.43 0)
				(length 3.81)
				(name "P8.4/UCB1CLK/UCA1STE")
				(number "G11")
			)
			(pin bidirectional line
				(at -33.02 -13.97 0)
				(length 3.81)
				(name "P8.5/UCB1SIMO/UCB1SDA")
				(number "F11")
			)
			(pin bidirectional line
				(at -33.02 -16.51 0)
				(length 3.81)
				(name "P8.6/UCB1SOMI/UCB1SCL")
				(number "G9")
			)
			(pin bidirectional line
				(at -33.02 -19.05 0)
				(length 3.81)
				(name "P8.7")
				(number "E12")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "P7.2/XT2IN")
				(number "B8")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 3.81)
				(name "P7.3/XT2OUT")
				(number "B7")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 3.81)
				(name "P7.4/CB8/A12")
				(number "C1")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 3.81)
				(name "P7.5/CB9/A13")
				(number "C3")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 3.81)
				(name "P7.6/CB10/A14/DAC0")
				(number "D2")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 3.81)
				(name "P7.7/CB11/A15/DAC1")
				(number "D1")
			)
			(pin bidirectional line
				(at -33.02 -39.37 0)
				(length 3.81)
				(name "P6.0/CB0/A0")
				(number "B4")
			)
			(pin bidirectional line
				(at -33.02 -41.91 0)
				(length 3.81)
				(name "P6.1/CB1/A1")
				(number "B3")
			)
			(pin bidirectional line
				(at -33.02 -44.45 0)
				(length 3.81)
				(name "P6.2/CB2/A2")
				(number "A2")
			)
			(pin bidirectional line
				(at -33.02 -46.99 0)
				(length 3.81)
				(name "P6.3/CB3/A3")
				(number "D5")
			)
			(pin bidirectional line
				(at -33.02 -49.53 0)
				(length 3.81)
				(name "P6.4/CB4/A4")
				(number "A1")
			)
			(pin bidirectional line
				(at -33.02 -52.07 0)
				(length 3.81)
				(name "P6.5/CB5/A5")
				(number "B2")
			)
			(pin bidirectional line
				(at -33.02 -54.61 0)
				(length 3.81)
				(name "P6.6/CB6/A6/DAC0")
				(number "B1")
			)
			(pin bidirectional line
				(at -33.02 -57.15 0)
				(length 3.81)
				(name "P6.7/CB7/A7/DAC1")
				(number "C2")
			)
			(pin power_in line
				(at -26.67 -68.58 90)
				(length 3.81)
				(name "VSSU")
				(number "B11")
			)
			(pin power_in line
				(at -24.13 -68.58 90)
				(length 3.81)
				(name "VSSU")
				(number "B12")
			)
			(pin power_in line
				(at -20.32 -68.58 90)
				(length 3.81)
				(name "AVSS1")
				(number "F2")
			)
			(pin power_in line
				(at -17.78 -68.58 90)
				(length 3.81)
				(name "AVSS2")
				(number "G2")
			)
			(pin power_in line
				(at -15.24 -68.58 90)
				(length 3.81)
				(name "AVSS3")
				(number "A8")
			)
			(pin power_in line
				(at -11.43 -68.58 90)
				(length 3.81)
				(name "DVSS")
				(number "M3")
			)
			(pin power_in line
				(at -10.16 67.31 270)
				(length 3.81)
				(name "AVCC1")
				(number "E1")
			)
			(pin power_in line
				(at -8.89 -68.58 90)
				(length 3.81)
				(name "DVSS1")
				(number "M1")
			)
			(pin power_in line
				(at -7.62 67.31 270)
				(length 3.81)
				(name "AVCC1")
				(number "E2")
			)
			(pin power_in line
				(at -6.35 -68.58 90)
				(length 3.81)
				(name "DVSS2")
				(number "G12")
			)
			(pin power_in line
				(at -3.81 -68.58 90)
				(length 3.81)
				(name "DVSS3")
				(number "A5")
			)
			(pin power_in line
				(at -2.54 67.31 270)
				(length 3.81)
				(name "DVCC1")
				(number "L1")
			)
			(pin power_in line
				(at 0 67.31 270)
				(length 3.81)
				(name "DVCC2")
				(number "F12")
			)
			(pin power_in line
				(at 1.27 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 67.31 270)
				(length 3.81)
				(name "DVCC3")
				(number "A6")
			)
			(pin power_in line
				(at 3.81 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at 6.35 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "E8")
			)
			(pin bidirectional line
				(at 7.62 67.31 270)
				(length 3.81)
				(name "VCORE")
				(number "M2")
			)
			(pin power_in line
				(at 8.89 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at 11.43 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at 12.7 67.31 270)
				(length 3.81)
				(name "V18")
				(number "B9")
			)
			(pin power_in line
				(at 13.97 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at 16.51 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 19.05 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at 21.59 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at 24.13 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 26.67 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "H9")
			)
			(pin input line
				(at 33.02 60.96 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "B6")
			)
			(pin bidirectional line
				(at 33.02 57.15 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "L5")
			)
			(pin bidirectional line
				(at 33.02 54.61 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "M5")
			)
			(pin bidirectional line
				(at 33.02 52.07 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "J6")
			)
			(pin bidirectional line
				(at 33.02 49.53 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "H6")
			)
			(pin bidirectional line
				(at 33.02 46.99 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "M6")
			)
			(pin bidirectional line
				(at 33.02 44.45 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "L6")
			)
			(pin bidirectional line
				(at 33.02 41.91 180)
				(length 3.81)
				(name "TA0.1/P1.6")
				(number "J7")
			)
			(pin bidirectional line
				(at 33.02 39.37 180)
				(length 3.81)
				(name "TA0.2/P1.7")
				(number "M7")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "P2MAP0/P2.0")
				(number "G4")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "P2MAP1/P2.1")
				(number "H2")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "P2MAP2/P2.2")
				(number "J1")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "P2MAP3/P2.3")
				(number "H4")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "P2MAP4/P2.4")
				(number "J2")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "P2MAP5/P2.5")
				(number "K1")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "P2MAP6/P2.6")
				(number "K2")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "P2MAP7/P2.7")
				(number "L2")
			)
			(pin bidirectional line
				(at 33.02 13.97 180)
				(length 3.81)
				(name "TA1CLK/CBOUT/P3.0")
				(number "L7")
			)
			(pin bidirectional line
				(at 33.02 11.43 180)
				(length 3.81)
				(name "TA1.0/P3.1")
				(number "H7")
			)
			(pin bidirectional line
				(at 33.02 8.89 180)
				(length 3.81)
				(name "TA1.1/P3.2")
				(number "M8")
			)
			(pin bidirectional line
				(at 33.02 6.35 180)
				(length 3.81)
				(name "TA1.2/P3.3")
				(number "L8")
			)
			(pin bidirectional line
				(at 33.02 3.81 180)
				(length 3.81)
				(name "TA2CLK/SMCLK/P3.4")
				(number "J8")
			)
			(pin bidirectional line
				(at 33.02 1.27 180)
				(length 3.81)
				(name "TA2.0/P3.5")
				(number "M9")
			)
			(pin bidirectional line
				(at 33.02 -1.27 180)
				(length 3.81)
				(name "TA2.1/P3.6")
				(number "L9")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA2.2/P3.7")
				(number "M10")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "TB0.0/P4.0")
				(number "J9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "TB0.1/P4.1")
				(number "M11")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "TB0.2/P4.2")
				(number "L10")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "TB0.3/P4.3")
				(number "M12")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "TB0.4/P4.4")
				(number "L12")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "TB0.5/P4.5")
				(number "L11")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "TB0.6/P4.6")
				(number "K11")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "TB0OUTH/SVMOUT/P4.7")
				(number "K12")
			)
			(pin bidirectional line
				(at 33.02 -29.21 180)
				(length 3.81)
				(name "VREF+/VeREF+/P5.0")
				(number "D4")
			)
			(pin bidirectional line
				(at 33.02 -31.75 180)
				(length 3.81)
				(name "VREF-/VeREF-/P5.1")
				(number "E4")
			)
			(pin bidirectional line
				(at 33.02 -34.29 180)
				(length 3.81)
				(name "P5.2")
				(number "L3")
			)
			(pin bidirectional line
				(at 33.02 -36.83 180)
				(length 3.81)
				(name "P5.3")
				(number "L4")
			)
			(pin bidirectional line
				(at 33.02 -39.37 180)
				(length 3.81)
				(name "P5.4")
				(number "M4")
			)
			(pin bidirectional line
				(at 33.02 -41.91 180)
				(length 3.81)
				(name "P5.5")
				(number "J5")
			)
			(pin bidirectional line
				(at 33.02 -44.45 180)
				(length 3.81)
				(name "ADC12CLK/DMAE0/P5.6")
				(number "H1")
			)
			(pin bidirectional line
				(at 33.02 -46.99 180)
				(length 3.81)
				(name "RTCCLK/P5.7")
				(number "D7")
			)
			(pin bidirectional line
				(at 33.02 -52.07 180)
				(length 3.81)
				(name "XIN")
				(number "F1")
			)
			(pin bidirectional line
				(at 33.02 -57.15 180)
				(length 3.81)
				(name "XOUT")
				(number "G1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430F5658IZQW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 66.04 0)
		)
		(property "Value" "MSP430F5658IZQW"
			(at -30.48 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 27.94 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5658.pdf"
			(at 0 0 0)
		)
		(property "Description" "384kB Flash, 32kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430F5658IZQW_0_1")
		(symbol "MSP430F5658IZQW_1_1"
			(pin input line
				(at -34.29 60.96 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "A3")
			)
			(pin bidirectional line
				(at -34.29 57.15 0)
				(length 3.81)
				(name "PJ.0/TDO")
				(number "B5")
			)
			(pin bidirectional line
				(at -34.29 54.61 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK")
				(number "A4")
			)
			(pin bidirectional line
				(at -34.29 52.07 0)
				(length 3.81)
				(name "PJ.2/TMS")
				(number "E7")
			)
			(pin bidirectional line
				(at -34.29 49.53 0)
				(length 3.81)
				(name "PJ.3/TCK")
				(number "D6")
			)
			(pin bidirectional line
				(at -34.29 44.45 0)
				(length 3.81)
				(name "PUR")
				(number "B10")
			)
			(pin bidirectional line
				(at -34.29 40.64 0)
				(length 3.81)
				(name "PU.0/DP")
				(number "A12")
			)
			(pin bidirectional line
				(at -34.29 38.1 0)
				(length 3.81)
				(name "PU.1/DM")
				(number "A11")
			)
			(pin passive line
				(at -34.29 33.02 0)
				(length 3.81)
				(name "VBAK")
				(number "A7")
			)
			(pin passive line
				(at -34.29 29.21 0)
				(length 3.81)
				(name "VBAT")
				(number "D8")
			)
			(pin bidirectional line
				(at -34.29 21.59 0)
				(length 3.81)
				(name "P9.0")
				(number "E11")
			)
			(pin bidirectional line
				(at -34.29 19.05 0)
				(length 3.81)
				(name "P9.1/UCB2STE/UCA2CLK")
				(number "F9")
			)
			(pin bidirectional line
				(at -34.29 16.51 0)
				(length 3.81)
				(name "P9.2/UCA2TXD/UCA2SIMO")
				(number "D12")
			)
			(pin bidirectional line
				(at -34.29 13.97 0)
				(length 3.81)
				(name "P9.3/UCA2RXD/UCA2SOMI")
				(number "D11")
			)
			(pin bidirectional line
				(at -34.29 11.43 0)
				(length 3.81)
				(name "P9.4/UCB2CLK/UCA2STE")
				(number "E9")
			)
			(pin bidirectional line
				(at -34.29 8.89 0)
				(length 3.81)
				(name "P9.5/UCB2SIMO/UCB2SDA")
				(number "C12")
			)
			(pin bidirectional line
				(at -34.29 6.35 0)
				(length 3.81)
				(name "P9.6/UCB2SOMI/UCB2SCL")
				(number "C11")
			)
			(pin bidirectional line
				(at -34.29 3.81 0)
				(length 3.81)
				(name "P9.7")
				(number "D9")
			)
			(pin bidirectional line
				(at -34.29 0 0)
				(length 3.81)
				(name "P8.0/TB0CLK")
				(number "J11")
			)
			(pin bidirectional line
				(at -34.29 -2.54 0)
				(length 3.81)
				(name "P8.1/UCB1STE/UCA1CLK")
				(number "J12")
			)
			(pin bidirectional line
				(at -34.29 -5.08 0)
				(length 3.81)
				(name "P8.2/UCA1TXD/UCA1SIMO")
				(number "H11")
			)
			(pin bidirectional line
				(at -34.29 -7.62 0)
				(length 3.81)
				(name "P8.3/UCA1RXD/UCA1SOMI")
				(number "H12")
			)
			(pin bidirectional line
				(at -34.29 -10.16 0)
				(length 3.81)
				(name "P8.4/UCB1CLK/UCA1STE")
				(number "G11")
			)
			(pin bidirectional line
				(at -34.29 -12.7 0)
				(length 3.81)
				(name "P8.5/UCB1SIMO/UCB1SDA")
				(number "F11")
			)
			(pin bidirectional line
				(at -34.29 -15.24 0)
				(length 3.81)
				(name "P8.6/UCB1SOMI/UCB1SCL")
				(number "G9")
			)
			(pin bidirectional line
				(at -34.29 -17.78 0)
				(length 3.81)
				(name "P8.7")
				(number "E12")
			)
			(pin bidirectional line
				(at -34.29 -21.59 0)
				(length 3.81)
				(name "P7.2/XT2IN")
				(number "B8")
			)
			(pin bidirectional line
				(at -34.29 -24.13 0)
				(length 3.81)
				(name "P7.3/XT2OUT")
				(number "B7")
			)
			(pin bidirectional line
				(at -34.29 -26.67 0)
				(length 3.81)
				(name "P7.4/A12/CB8")
				(number "C1")
			)
			(pin bidirectional line
				(at -34.29 -29.21 0)
				(length 3.81)
				(name "P7.5/A13/CB9")
				(number "C3")
			)
			(pin bidirectional line
				(at -34.29 -31.75 0)
				(length 3.81)
				(name "P7.6/A14/DAC0/CB10")
				(number "D2")
			)
			(pin bidirectional line
				(at -34.29 -34.29 0)
				(length 3.81)
				(name "P7.7/A15/DAC1/CB11")
				(number "D1")
			)
			(pin bidirectional line
				(at -34.29 -38.1 0)
				(length 3.81)
				(name "P6.0/A0/CB0")
				(number "B4")
			)
			(pin bidirectional line
				(at -34.29 -40.64 0)
				(length 3.81)
				(name "P6.1/A1/CB1")
				(number "B3")
			)
			(pin bidirectional line
				(at -34.29 -43.18 0)
				(length 3.81)
				(name "P6.2/A2/CB2")
				(number "A2")
			)
			(pin bidirectional line
				(at -34.29 -45.72 0)
				(length 3.81)
				(name "P6.3/A3/CB3")
				(number "D5")
			)
			(pin bidirectional line
				(at -34.29 -48.26 0)
				(length 3.81)
				(name "P6.4/A4/CB4")
				(number "A1")
			)
			(pin bidirectional line
				(at -34.29 -50.8 0)
				(length 3.81)
				(name "P6.5/A5/CB5")
				(number "B2")
			)
			(pin bidirectional line
				(at -34.29 -53.34 0)
				(length 3.81)
				(name "P6.6/A6/DAC0/CB6")
				(number "B1")
			)
			(pin bidirectional line
				(at -34.29 -55.88 0)
				(length 3.81)
				(name "P6.7/A7/DAC1/CB7")
				(number "C2")
			)
			(pin power_in line
				(at -27.94 -67.31 90)
				(length 3.81)
				(name "VSSU")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -67.31 90)
				(length 3.81)
				(name "VSSU")
				(number "B12")
			)
			(pin power_in line
				(at -20.32 -67.31 90)
				(length 3.81)
				(name "AVSS1")
				(number "F2")
			)
			(pin power_in line
				(at -17.78 -67.31 90)
				(length 3.81)
				(name "AVSS2")
				(number "G2")
			)
			(pin power_in line
				(at -15.24 -67.31 90)
				(length 3.81)
				(name "AVSS3")
				(number "A8")
			)
			(pin passive line
				(at -11.43 67.31 270)
				(length 3.81)
				(name "VBUS")
				(number "A10")
			)
			(pin power_in line
				(at -10.16 -67.31 90)
				(length 3.81)
				(name "DVSS")
				(number "M3")
			)
			(pin passive line
				(at -8.89 67.31 270)
				(length 3.81)
				(name "VUSB")
				(number "A9")
			)
			(pin power_in line
				(at -7.62 -67.31 90)
				(length 3.81)
				(name "DVSS1")
				(number "M1")
			)
			(pin power_in line
				(at -6.35 67.31 270)
				(length 3.81)
				(name "AVCC1")
				(number "E1")
			)
			(pin power_in line
				(at -5.08 -67.31 90)
				(length 3.81)
				(name "DVSS2")
				(number "G12")
			)
			(pin power_in line
				(at -3.81 67.31 270)
				(length 3.81)
				(name "AVCC1")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 -67.31 90)
				(length 3.81)
				(name "DVSS3")
				(number "A5")
			)
			(pin power_in line
				(at 1.27 67.31 270)
				(length 3.81)
				(name "DVCC1")
				(number "L1")
			)
			(pin power_in line
				(at 2.54 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at 3.81 67.31 270)
				(length 3.81)
				(name "DVCC2")
				(number "F12")
			)
			(pin power_in line
				(at 5.08 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at 6.35 67.31 270)
				(length 3.81)
				(name "DVCC3")
				(number "A6")
			)
			(pin power_in line
				(at 7.62 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "E8")
			)
			(pin power_in line
				(at 10.16 67.31 270)
				(length 3.81)
				(name "VCORE")
				(number "M2")
			)
			(pin power_in line
				(at 10.16 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at 12.7 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at 15.24 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at 17.78 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 20.32 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at 22.86 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at 25.4 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 27.94 -67.31 90)
				(length 3.81)
				(name "GND")
				(number "H9")
			)
			(pin input line
				(at 34.29 60.96 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "B6")
			)
			(pin bidirectional line
				(at 34.29 57.15 180)
				(length 3.81)
				(name "ACLK/TA0CLK/P1.0")
				(number "L5")
			)
			(pin bidirectional line
				(at 34.29 54.61 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "M5")
			)
			(pin bidirectional line
				(at 34.29 52.07 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "J6")
			)
			(pin bidirectional line
				(at 34.29 49.53 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "H6")
			)
			(pin bidirectional line
				(at 34.29 46.99 180)
				(length 3.81)
				(name "TA0.3/P1.4")
				(number "M6")
			)
			(pin bidirectional line
				(at 34.29 44.45 180)
				(length 3.81)
				(name "TA0.4/P1.5")
				(number "L6")
			)
			(pin bidirectional line
				(at 34.29 41.91 180)
				(length 3.81)
				(name "TA0.1/P1.6")
				(number "J7")
			)
			(pin bidirectional line
				(at 34.29 39.37 180)
				(length 3.81)
				(name "TA0.2/P1.7")
				(number "M7")
			)
			(pin bidirectional line
				(at 34.29 35.56 180)
				(length 3.81)
				(name "P2MAP0/P2.0")
				(number "G4")
			)
			(pin bidirectional line
				(at 34.29 33.02 180)
				(length 3.81)
				(name "P2MAP1/P2.1")
				(number "H2")
			)
			(pin bidirectional line
				(at 34.29 30.48 180)
				(length 3.81)
				(name "P2MAP2/P2.2")
				(number "J1")
			)
			(pin bidirectional line
				(at 34.29 27.94 180)
				(length 3.81)
				(name "P2MAP3/P2.3")
				(number "H4")
			)
			(pin bidirectional line
				(at 34.29 25.4 180)
				(length 3.81)
				(name "P2MAP4/P2.4")
				(number "J2")
			)
			(pin bidirectional line
				(at 34.29 22.86 180)
				(length 3.81)
				(name "P2MAP5/P2.5")
				(number "K1")
			)
			(pin bidirectional line
				(at 34.29 20.32 180)
				(length 3.81)
				(name "P2MAP6/P2.6")
				(number "K2")
			)
			(pin bidirectional line
				(at 34.29 17.78 180)
				(length 3.81)
				(name "P2MAP7/P2.7")
				(number "L2")
			)
			(pin bidirectional line
				(at 34.29 13.97 180)
				(length 3.81)
				(name "CBOUT/TA1CLK/P3.0")
				(number "L7")
			)
			(pin bidirectional line
				(at 34.29 11.43 180)
				(length 3.81)
				(name "TA1.0/P3.1")
				(number "H7")
			)
			(pin bidirectional line
				(at 34.29 8.89 180)
				(length 3.81)
				(name "TA1.1/P3.2")
				(number "M8")
			)
			(pin bidirectional line
				(at 34.29 6.35 180)
				(length 3.81)
				(name "TA1.2/P3.3")
				(number "L8")
			)
			(pin bidirectional line
				(at 34.29 3.81 180)
				(length 3.81)
				(name "SMCLK/TA2CLK/P3.4")
				(number "J8")
			)
			(pin bidirectional line
				(at 34.29 1.27 180)
				(length 3.81)
				(name "TA2.0/P3.5")
				(number "M9")
			)
			(pin bidirectional line
				(at 34.29 -1.27 180)
				(length 3.81)
				(name "TA2.1/P3.6")
				(number "L9")
			)
			(pin bidirectional line
				(at 34.29 -3.81 180)
				(length 3.81)
				(name "TA2.2/P3.7")
				(number "M10")
			)
			(pin bidirectional line
				(at 34.29 -7.62 180)
				(length 3.81)
				(name "TB0.0/P4.0")
				(number "J9")
			)
			(pin bidirectional line
				(at 34.29 -10.16 180)
				(length 3.81)
				(name "TB0.1/P4.1")
				(number "M11")
			)
			(pin bidirectional line
				(at 34.29 -12.7 180)
				(length 3.81)
				(name "TB0.2/P4.2")
				(number "L10")
			)
			(pin bidirectional line
				(at 34.29 -15.24 180)
				(length 3.81)
				(name "TB0.3/P4.3")
				(number "M12")
			)
			(pin bidirectional line
				(at 34.29 -17.78 180)
				(length 3.81)
				(name "TB0.4/P4.4")
				(number "L12")
			)
			(pin bidirectional line
				(at 34.29 -20.32 180)
				(length 3.81)
				(name "TB0.5/P4.5")
				(number "L11")
			)
			(pin bidirectional line
				(at 34.29 -22.86 180)
				(length 3.81)
				(name "TB0.6/P4.6")
				(number "K11")
			)
			(pin bidirectional line
				(at 34.29 -25.4 180)
				(length 3.81)
				(name "SVMOUT/TB0OUTH/P4.7")
				(number "K12")
			)
			(pin bidirectional line
				(at 34.29 -29.21 180)
				(length 3.81)
				(name "VREF+/VeREF+/P5.0")
				(number "D4")
			)
			(pin bidirectional line
				(at 34.29 -31.75 180)
				(length 3.81)
				(name "VREF-/VeREF-/P5.1")
				(number "E4")
			)
			(pin bidirectional line
				(at 34.29 -34.29 180)
				(length 3.81)
				(name "P5.2")
				(number "L3")
			)
			(pin bidirectional line
				(at 34.29 -36.83 180)
				(length 3.81)
				(name "P5.3")
				(number "L4")
			)
			(pin bidirectional line
				(at 34.29 -39.37 180)
				(length 3.81)
				(name "P5.4")
				(number "M4")
			)
			(pin bidirectional line
				(at 34.29 -41.91 180)
				(length 3.81)
				(name "P5.5")
				(number "J5")
			)
			(pin bidirectional line
				(at 34.29 -44.45 180)
				(length 3.81)
				(name "DMAE0/ADC12CLK/P5.6")
				(number "H1")
			)
			(pin bidirectional line
				(at 34.29 -46.99 180)
				(length 3.81)
				(name "RTCCLK/P5.7")
				(number "D7")
			)
			(pin input line
				(at 34.29 -52.07 180)
				(length 3.81)
				(name "XIN")
				(number "F1")
			)
			(pin output line
				(at 34.29 -55.88 180)
				(length 3.81)
				(name "XOUT")
				(number "G1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430FR5720IRGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5720IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5720.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
		(symbol "MSP430FR5720IRGE_0_1")
		(symbol "MSP430FR5720IRGE_1_1"
			(pin input line
				(at -38.1 8.89 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "PJ.0/TDO/TB0OUTH/SMCLK/CD6")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK/MCLK/CD7")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "PJ.2/TMS/ACLK/CD8")
				(number "9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "PJ.3/TCK/CD9")
				(number "10")
			)
			(pin input line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "PJ.4/XIN")
				(number "21")
			)
			(pin input line
				(at -38.1 -15.24 0)
				(length 3.81)
				(name "PJ.5/XOUT")
				(number "22")
			)
			(pin input line
				(at -15.24 21.59 270)
				(length 3.81)
				(name "VCORE")
				(number "18")
			)
			(pin power_in line
				(at -7.62 21.59 270)
				(length 3.81)
				(name "DVCC")
				(number "20")
			)
			(pin power_in line
				(at -7.62 -21.59 90)
				(length 3.81)
				(name "DVSS")
				(number "19")
			)
			(pin power_in line
				(at 0 21.59 270)
				(length 3.81)
				(name "AVCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -21.59 90)
				(length 3.81)
				(name "AVSS")
				(number "23")
			)
			(pin input line
				(at 38.1 15.24 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 11.43 180)
				(length 3.81)
				(name "TA0.1/DMAE0/RTCCLK/CD0/VeREF-/A0/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 38.1 8.89 180)
				(length 3.81)
				(name "TA0.2/TA1CLK/CDOUT/CD1/VeREF+/A1/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 6.35 180)
				(length 3.81)
				(name "TA1.1/TA0CLK/CDOUT/CD2/A2/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 3.81 180)
				(length 3.81)
				(name "TA1.2/UCB0STE/CD3/A3/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 1.27 180)
				(length 3.81)
				(name "TB0.1/UCA0STE/CD4/A4/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 -1.27 180)
				(length 3.81)
				(name "TB0.2/UCA0CLK/CD5/A5/P1.5")
				(number "6")
			)
			(pin input line
				(at 38.1 -3.81 180)
				(length 3.81)
				(name "TA0.0/UCB0SIMO/UCB0SDA/P1.6")
				(number "16")
			)
			(pin input line
				(at 38.1 -6.35 180)
				(length 3.81)
				(name "TA1.0/UCB0SOMI/UCB0SCL/P1.7")
				(number "17")
			)
			(pin input line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "TB0CLK/UCA0TXD/UCA0SIMO/ACLK/P2.0")
				(number "13")
			)
			(pin input line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "TB0.0/UCA0RXD/UCA0SOMI/P2.1")
				(number "14")
			)
			(pin input line
				(at 38.1 -15.24 180)
				(length 3.81)
				(name "UCB0CLK/P2.2")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430FR5722IRGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5722IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5722.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "8kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
		(symbol "MSP430FR5722IRGE_0_1")
		(symbol "MSP430FR5722IRGE_1_1"
			(pin input line
				(at -38.1 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "PJ.0/TDO/TB0OUTH/SMCLK/CD6")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "PJ.1/TDI/TCLK/MCLK/CD7")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "PJ.2/TMS/ACLK/CD8")
				(number "9")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "PJ.3/TCK/CD9")
				(number "10")
			)
			(pin input line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "PJ.4/XIN")
				(number "21")
			)
			(pin input line
				(at -38.1 -15.24 0)
				(length 3.81)
				(name "PJ.5/XOUT")
				(number "22")
			)
			(pin power_in line
				(at -7.62 21.59 270)
				(length 3.81)
				(name "DVCC")
				(number "20")
			)
			(pin power_in line
				(at -7.62 -21.59 90)
				(length 3.81)
				(name "DVSS")
				(number "19")
			)
			(pin input line
				(at -3.81 21.59 270)
				(length 3.81)
				(name "VCORE")
				(number "18")
			)
			(pin power_in line
				(at 0 21.59 270)
				(length 3.81)
				(name "AVCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -21.59 90)
				(length 3.81)
				(name "AVSS")
				(number "23")
			)
			(pin input line
				(at 38.1 15.24 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 11.43 180)
				(length 3.81)
				(name "TA0.1/DMAE0/RTCCLK/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 38.1 8.89 180)
				(length 3.81)
				(name "TA0.2/TA1CLK/CDOUT/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 6.35 180)
				(length 3.81)
				(name "TA1.1/TA0CLK/CDOUT/CD2/A2/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 3.81 180)
				(length 3.81)
				(name "TA1.2/UCB0STE/CD3/A3/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 1.27 180)
				(length 3.81)
				(name "TB0.1/UCA0STE/CD4/A4/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 -1.27 180)
				(length 3.81)
				(name "TB0.2/UCA0CLK/CD5/A5/P1.5")
				(number "6")
			)
			(pin input line
				(at 38.1 -3.81 180)
				(length 3.81)
				(name "TA0.0/UCB0SIMO/UCB0SDA/P1.6")
				(number "16")
			)
			(pin input line
				(at 38.1 -6.35 180)
				(length 3.81)
				(name "TA1.0/UCB0SOMI/UCB0SCL/P1.7")
				(number "17")
			)
			(pin input line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "TB0CLK/UCA0TXD/UCA0SIMO/ACLK/P2.0")
				(number "13")
			)
			(pin input line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "TB0.0/UCA0RXD/UCA0SOMI/P2.1")
				(number "14")
			)
			(pin input line
				(at 38.1 -15.24 180)
				(length 3.81)
				(name "UCB0CLK/P2.2")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2001IN14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2001IN14"
			(at 10.16 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at -15.24 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2001.pdf"
			(at 0 0 0)
		)
		(property "Description" "512B Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2001IN14_0_1")
		(symbol "MSP430G2001IN14_1_1"
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -16.51 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 20.32 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TA0.0/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "TA0.1/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2001IPW14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2001IPW14"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2001.pdf"
			(at 0 0 0)
		)
		(property "Description" "512B Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2001IPW14_0_1")
		(symbol "MSP430G2001IPW14_1_1"
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -16.51 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 20.32 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TA0.0/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "TA0.1/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2001IRSA16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2001IRSA16"
			(at 11.43 -15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -16.51 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2001.pdf"
			(at 0 0 0)
		)
		(property "Description" "512B Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2001IRSA16_0_1")
		(symbol "MSP430G2001IRSA16_1_1"
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 20.32 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TA0.0/TMS/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "TA0.1/TDI/TCLK/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "TDO/TDI/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2102IN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2102IN20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -17.78 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2102.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2102IN20_0_1")
		(symbol "MSP430G2102IN20_1_1"
			(pin input line
				(at -22.86 8.89 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P2.3")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.4")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 22.86 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "SMCLK/TCK/TA0.2/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TMS/TA0.0/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "SDO/SCL/TDI/TCLK/TA0.1/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "SDI/SDA/TDO/TDI/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2102IPW14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2102IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2102.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2102IPW14_0_1")
		(symbol "MSP430G2102IPW14_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 22.86 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "SMCLK/TCK/TA0.2/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "SDO/SCL/TDI/TCLK/TA0.1/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "SDI/SDA/TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2102IPW20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2102IPW20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2102.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2102IPW20_0_1")
		(symbol "MSP430G2102IPW20_1_1"
			(pin input line
				(at -22.86 8.89 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P2.3")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.4")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 22.86 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "SMCLK/TCK/TA0.2/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TMS/TA0.0/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "SDO/SCL/TDI/TCLK/TA0.1/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "SDI/SDA/TDO/TDI/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2102IRSA16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 17.78 0)
		)
		(property "Value" "MSP430G2102IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2102.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2102IRSA16_0_1")
		(symbol "MSP430G2102IRSA16_1_1"
			(pin input line
				(at -25.4 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "AVCC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -19.05 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin input line
				(at 25.4 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "SDO/SCL/TDI/TCLK/TA0.1/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "SDI/SDA/TDO/TDI/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2111IN14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2111IN14"
			(at 12.7 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2111.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2111IN14_0_1")
		(symbol "MSP430G2111IN14_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -16.51 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "CA0/TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "CA1/TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "CA2/TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "CAOUT/CA3/ADC10CLK/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "CA4/SMCLK/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "CA5/TA0.0/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "CA6/TA0.1/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "CA7/TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2111IPW14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2111IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2111.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2111IPW14_0_1")
		(symbol "MSP430G2111IPW14_1_1"
			(pin input line
				(at -22.86 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at 22.86 11.43 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "CA0/TA0CLK/ACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "CA1/TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "CA2/TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "CAOUT/CA3/ADC10CLK/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "CA4/SMCLK/TCK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "CA5/TA0.0/TMS/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "CA6/TA0.1/TDI/TCLK/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "CA7/TDO/TDI/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2111IRSA16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 17.78 0)
		)
		(property "Value" "MSP430G2111IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -20.32 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2111.pdf"
			(at -22.86 13.97 0)
		)
		(property "Description" "1kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2111IRSA16_0_1")
		(symbol "MSP430G2111IRSA16_1_1"
			(pin input line
				(at -26.67 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -26.67 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "12")
			)
			(pin bidirectional line
				(at -26.67 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 26.67 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 26.67 10.16 180)
				(length 3.81)
				(name "ACLK/TA0CLK/CA0/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 26.67 7.62 180)
				(length 3.81)
				(name "TA0.0/CA1/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 26.67 5.08 180)
				(length 3.81)
				(name "TA0.1/CA2/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 26.67 2.54 180)
				(length 3.81)
				(name "CAOUT/CA3/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 26.67 0 180)
				(length 3.81)
				(name "TCK/SMCLK/CA4/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 26.67 -2.54 180)
				(length 3.81)
				(name "TMS/TA0.0/CA5/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 26.67 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/CA6/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 26.67 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/CAOUT/CA7/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2112IN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2112IN20"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -29.21 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2112.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2112IN20_0_1")
		(symbol "MSP430G2112IN20_1_1"
			(pin input line
				(at -34.29 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -34.29 7.62 0)
				(length 3.81)
				(name "P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at -34.29 5.08 0)
				(length 3.81)
				(name "P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at -34.29 2.54 0)
				(length 3.81)
				(name "P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at -34.29 0 0)
				(length 3.81)
				(name "P2.3")
				(number "11")
			)
			(pin bidirectional line
				(at -34.29 -2.54 0)
				(length 3.81)
				(name "P2.4")
				(number "12")
			)
			(pin bidirectional line
				(at -34.29 -5.08 0)
				(length 3.81)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at -34.29 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -34.29 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 34.29 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "17")
			)
			(pin bidirectional line
				(at 34.29 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 34.29 7.62 180)
				(length 3.81)
				(name "TA0.0/CA1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 34.29 5.08 180)
				(length 3.81)
				(name "TA0.1/CA2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 34.29 2.54 180)
				(length 3.81)
				(name "CAOUT/CA3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 34.29 0 180)
				(length 3.81)
				(name "TCK/SMCLK/TA0.2/CA4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 34.29 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/CA5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 34.29 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/SDO/SCL/CA6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 34.29 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/SDI/SDA/CAOUT/CA7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2112IPW14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2112IPW14"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -27.94 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2112.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2112IPW14_0_1")
		(symbol "MSP430G2112IPW14_1_1"
			(pin input line
				(at -34.29 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -34.29 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -34.29 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 34.29 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 34.29 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 34.29 7.62 180)
				(length 3.81)
				(name "TA0.0/CA1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 34.29 5.08 180)
				(length 3.81)
				(name "TA0.1/CA2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 34.29 2.54 180)
				(length 3.81)
				(name "CAOUT/CA3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 34.29 0 180)
				(length 3.81)
				(name "TCK/SMCLK/TA0.2/CA4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 34.29 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/CA5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 34.29 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/SDO/SCL/CA6/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 34.29 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/SDI/SDA/CAOUT/CA7/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2112IPW20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2112IPW20"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -27.94 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2112.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2112IPW20_0_1")
		(symbol "MSP430G2112IPW20_1_1"
			(pin input line
				(at -34.29 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -34.29 7.62 0)
				(length 3.81)
				(name "P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at -34.29 5.08 0)
				(length 3.81)
				(name "P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at -34.29 2.54 0)
				(length 3.81)
				(name "P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at -34.29 0 0)
				(length 3.81)
				(name "P2.3")
				(number "11")
			)
			(pin bidirectional line
				(at -34.29 -2.54 0)
				(length 3.81)
				(name "P2.4")
				(number "12")
			)
			(pin bidirectional line
				(at -34.29 -5.08 0)
				(length 3.81)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at -34.29 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -34.29 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 34.29 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "17")
			)
			(pin bidirectional line
				(at 34.29 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 34.29 7.62 180)
				(length 3.81)
				(name "TA0.0/CA1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 34.29 5.08 180)
				(length 3.81)
				(name "TA0.1/CA2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 34.29 2.54 180)
				(length 3.81)
				(name "CAOUT/CA3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 34.29 0 180)
				(length 3.81)
				(name "TCK/SMCLK/TA0.2/CA4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 34.29 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/CA5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 34.29 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/SDO/SCL/CA6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 34.29 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/SDI/SDA/CAOUT/CA7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2112IRSA16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -33.02 15.24 0)
		)
		(property "Value" "MSP430G2112IRSA16"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2112.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2112IRSA16_0_1")
		(symbol "MSP430G2112IRSA16_1_1"
			(pin input line
				(at -38.1 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at -3.81 20.32 270)
				(length 3.81)
				(name "AVCC")
				(number "15")
			)
			(pin power_in line
				(at -3.81 -19.05 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin power_in line
				(at 3.81 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at 3.81 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 38.1 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "TA0.0/CA1/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "TA0.1/CA2/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "CAOUT/CA3/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "TCK/SMCLK/TA0.2/CA4/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/CA5/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/SDO/SCL/CA6/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/SDI/SDA/CAOUT/CA7/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2113IPW20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2113IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2153.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "1kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2113IPW20_0_1")
		(symbol "MSP430G2113IPW20_1_1"
			(pin input line
				(at -43.18 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 3.81)
				(name "P2.0/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 3.81)
				(name "P2.1/TA1.1")
				(number "9")
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 3.81)
				(name "P2.2/TA1.1")
				(number "10")
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 3.81)
				(name "P2.3/TA1.0")
				(number "11")
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 3.81)
				(name "P2.4/TA1.2")
				(number "12")
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 3.81)
				(name "P2.5/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 43.18 13.97 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "17")
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/TA0.0/CA1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/TA0.1/CA2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 3.81)
				(name "CAOUT/CA3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/CA4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 3.81)
				(name "TMS/UCB0CLK/UCA0STE/TA0.0/CA5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/UCB0SOMI/UCB0SCL/TA0.1/CA6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/CAOUT/CA7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2121IN14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2121IN14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2121.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2121IN14_0_1")
		(symbol "MSP430G2121IN14_1_1"
			(pin input line
				(at -24.13 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -24.13 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -24.13 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 24.13 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 24.13 10.16 180)
				(length 3.81)
				(name "ACLK/TACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 24.13 7.62 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 24.13 5.08 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 24.13 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 24.13 0 180)
				(length 3.81)
				(name "TCK/SMCLK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 24.13 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 24.13 -5.08 180)
				(length 3.81)
				(name "TDI/SDO/SCL/TCLK/TA0.1/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 24.13 -7.62 180)
				(length 3.81)
				(name "TDI/TDO/SDI/SDA/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2121IPW14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2121IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -17.78 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2121.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2121IPW14_0_1")
		(symbol "MSP430G2121IPW14_1_1"
			(pin input line
				(at -24.13 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -24.13 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -24.13 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 24.13 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 24.13 10.16 180)
				(length 3.81)
				(name "ACLK/TACLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 24.13 7.62 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 24.13 5.08 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 24.13 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 24.13 0 180)
				(length 3.81)
				(name "TCK/SMCLK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 24.13 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 24.13 -5.08 180)
				(length 3.81)
				(name "TDI/SDO/SCL/TCLK/TA0.1/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 24.13 -7.62 180)
				(length 3.81)
				(name "TDI/TDO/SDI/SDA/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2121IRSA16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2121IRSA16"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -17.78 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2121.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2121IRSA16_0_1")
		(symbol "MSP430G2121IRSA16_1_1"
			(pin input line
				(at -24.13 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -24.13 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "12")
			)
			(pin bidirectional line
				(at -24.13 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at -1.27 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "15")
			)
			(pin power_in line
				(at -1.27 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "13")
			)
			(pin power_in line
				(at 1.27 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at 1.27 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 24.13 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 24.13 10.16 180)
				(length 3.81)
				(name "ACLK/TACLK/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 24.13 7.62 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 24.13 5.08 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 24.13 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 24.13 0 180)
				(length 3.81)
				(name "TCK/SMCLK/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 24.13 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 24.13 -5.08 180)
				(length 3.81)
				(name "TDI/SDO/SCL/TCLK/TA0.1/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 24.13 -7.62 180)
				(length 3.81)
				(name "TDI/TDO/SDI/SDA/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2131IN14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2131IN14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2131.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2131IN14_0_1")
		(symbol "MSP430G2131IN14_1_1"
			(pin input line
				(at -24.13 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -24.13 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -24.13 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 24.13 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 24.13 10.16 180)
				(length 3.81)
				(name "ACLK/TACLK/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 24.13 7.62 180)
				(length 3.81)
				(name "TA0.0/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 24.13 5.08 180)
				(length 3.81)
				(name "TA0.1/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 24.13 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 24.13 0 180)
				(length 3.81)
				(name "TCK/SMCLK/VREF+/VeREF+/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 24.13 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 24.13 -5.08 180)
				(length 3.81)
				(name "TDI/SDO/SCL/TCLK/TA0.1/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 24.13 -7.62 180)
				(length 3.81)
				(name "TDI/TDO/SDI/SDA/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2131IPW14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2131IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -17.78 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2131.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2131IPW14_0_1")
		(symbol "MSP430G2131IPW14_1_1"
			(pin input line
				(at -24.13 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -24.13 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -24.13 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 24.13 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 24.13 10.16 180)
				(length 3.81)
				(name "ACLK/TACLK/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 24.13 7.62 180)
				(length 3.81)
				(name "TA0.0/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 24.13 5.08 180)
				(length 3.81)
				(name "TA0.1/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 24.13 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 24.13 0 180)
				(length 3.81)
				(name "TCK/SMCLK/VREF+/VeREF+/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 24.13 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 24.13 -5.08 180)
				(length 3.81)
				(name "TDI/SDO/SCL/TCLK/TA0.1/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 24.13 -7.62 180)
				(length 3.81)
				(name "TDI/TDO/SDI/SDA/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2131IRSA16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2131IRSA16"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -17.78 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2131.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2131IRSA16_0_1")
		(symbol "MSP430G2131IRSA16_1_1"
			(pin input line
				(at -24.13 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -24.13 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "12")
			)
			(pin bidirectional line
				(at -24.13 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at -1.27 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "15")
			)
			(pin power_in line
				(at -1.27 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "13")
			)
			(pin power_in line
				(at 1.27 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at 1.27 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 24.13 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 24.13 10.16 180)
				(length 3.81)
				(name "ACLK/TACLK/A0/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 24.13 7.62 180)
				(length 3.81)
				(name "TA0.0/A1/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 24.13 5.08 180)
				(length 3.81)
				(name "TA0.1/A2/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 24.13 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 24.13 0 180)
				(length 3.81)
				(name "TCK/SMCLK/VREF+/VeREF+/A4/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 24.13 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/A5/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 24.13 -5.08 180)
				(length 3.81)
				(name "TDI/SDO/SCL/TCLK/TA0.1/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 24.13 -7.62 180)
				(length 3.81)
				(name "TDI/TDO/SDI/SDA/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2132IN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2132IN20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2132.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2132IN20_0_1")
		(symbol "MSP430G2132IN20_1_1"
			(pin input line
				(at -27.94 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "P2.3")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "P2.4")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 27.94 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "A0/ACLK/TA0CLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "A1/TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "A2/TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TCK/VREF+/VeREF+/A4/SMCLK/TA0.2/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "TMS/A5/TA0.0/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "SDO/SCL/TDI/TCLK/A6/TA0.1/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "SDI/SDA/TDO/TDI/A7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2132IPW14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2132IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2132.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2132IPW14_0_1")
		(symbol "MSP430G2132IPW14_1_1"
			(pin input line
				(at -25.4 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 26.67 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 26.67 10.16 180)
				(length 3.81)
				(name "ACLK/A0/TA0CLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 26.67 7.62 180)
				(length 3.81)
				(name "A1/TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 26.67 5.08 180)
				(length 3.81)
				(name "A2/TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 26.67 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 26.67 0 180)
				(length 3.81)
				(name "SMCLK/TCK/A4/VREF+/VeREF+/TA0.2/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 26.67 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/A5/TA0.0/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 26.67 -5.08 180)
				(length 3.81)
				(name "SDO/SCL/TDI/TCLK/A6/TA0.1/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 26.67 -7.62 180)
				(length 3.81)
				(name "SDI/SDA/TDO/TDI/A7/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2132IPW20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2132IPW20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2132.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2132IPW20_0_1")
		(symbol "MSP430G2132IPW20_1_1"
			(pin input line
				(at -27.94 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "P2.3")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "P2.4")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 27.94 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "A0/ACLK/TA0CLK/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "A1/TA0.0/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "A2/TA0.1/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TCK/VREF+/VeREF+/A4/SMCLK/TA0.2/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "TMS/A5/TA0.0/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "SDO/SCL/TDI/TCLK/A6/TA0.1/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "SDI/SDA/TDO/TDI/A7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2132IRSA16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 17.78 0)
		)
		(property "Value" "MSP430G2132IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2132.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2132IRSA16_0_1")
		(symbol "MSP430G2132IRSA16_1_1"
			(pin input line
				(at -25.4 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "AVCC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -19.05 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin input line
				(at 25.4 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "ACLK/A0/TA0CLK/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "A1/TA0.0/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "A2/TA0.1/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "SMCLK/TCK/VREF+/VeREF+/A4/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/A5/TA0.0/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "SDO/SCL/TDI/TCLK/A6/TA0.1/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "SDI/SDA/TDO/TDI/A7/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2152IN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2152IN20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -33.02 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2152.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2152IN20_0_1")
		(symbol "MSP430G2152IN20_1_1"
			(pin input line
				(at -38.1 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "P2.3")
				(number "11")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "P2.4")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 38.1 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "17")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "TA0.0/CA1/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "TA0.1/CA2/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/CAOUT/CA3/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "TCK/SMCLK/TA0.2/VREF+/VeREF+/CA4/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/CA5/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/SDO/SCL/CA6/A6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/SDI/SDA/CAOUT/CA7/A7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2152IPW14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2152IPW14"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2152.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2152IPW14_0_1")
		(symbol "MSP430G2152IPW14_1_1"
			(pin input line
				(at -38.1 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "13")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 38.1 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "TA0.0/CA1/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "TA0.1/CA2/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/CAOUT/CA3/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "TCK/SMCLK/TA0.2/VREF+/VeREF+/CA4/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/CA5/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/SDO/SCL/CA6/A6/P1.6")
				(number "8")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/SDI/SDA/CAOUT/CA7/A7/P1.7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2152IPW20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2152IPW20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2152.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2152IPW20_0_1")
		(symbol "MSP430G2152IPW20_1_1"
			(pin input line
				(at -38.1 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "P2.3")
				(number "11")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "P2.4")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "P2.5")
				(number "13")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 38.1 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "17")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "TA0.0/CA1/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "TA0.1/CA2/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/CAOUT/CA3/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "TCK/SMCLK/TA0.2/VREF+/VeREF+/CA4/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "TMS/SCLK/TA0.0/CA5/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/SDO/SCL/CA6/A6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/SDI/SDA/CAOUT/CA7/A7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2152IRSA16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 17.78 0)
		)
		(property "Value" "MSP430G2152IRSA16"
			(at 29.21 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -34.29 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2152.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2152IRSA16_0_1")
		(symbol "MSP430G2152IRSA16_1_1"
			(pin input line
				(at -40.64 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "9")
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "12")
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "11")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "AVCC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -19.05 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "14")
			)
			(pin input line
				(at 40.64 13.97 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "10")
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/A0/CA0/P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 3.81)
				(name "TA0.0/A1/CA1/P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 3.81)
				(name "TA0.1/A2/CA2/P1.2")
				(number "3")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 3.81)
				(name "ADC10CLK/CAOUT/VREF-/VeREF-/A3/CA3/P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 3.81)
				(name "TCK/SMCLK/TA0.2/VREF+/VeREF+/A4/CA4/P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 3.81)
				(name "TMS/TA0.0/SCLK/A5/CA5/P1.5")
				(number "6")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/SDO/SCL/A6/CA6/P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/CAOUT/SDI/SDA/A7/CA7/P1.7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2153IN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2153IN20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2153.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "1kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2153IN20_0_1")
		(symbol "MSP430G2153IN20_1_1"
			(pin input line
				(at -43.18 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 3.81)
				(name "P2.0/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 3.81)
				(name "P2.1/TA1.1")
				(number "9")
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 3.81)
				(name "P2.2/TA1.1")
				(number "10")
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 3.81)
				(name "P2.3/TA1.0")
				(number "11")
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 3.81)
				(name "P2.4/TA1.2")
				(number "12")
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 3.81)
				(name "P2.5/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 43.18 13.97 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "17")
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/TA0.0/CA1/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/TA0.1/CA2/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 3.81)
				(name "CAOUT/VREF-/VeREF-/CA3/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/VREF+/VeREF+/CA4/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 3.81)
				(name "TMS/UCB0CLK/UCA0STE/TA0.0/CA5/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/UCB0SOMI/UCB0SCL/TA0.1/CA6/A6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/CAOUT/CA7/A7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2153IPW20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2153IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2153.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "1kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2153IPW20_0_1")
		(symbol "MSP430G2153IPW20_1_1"
			(pin input line
				(at -43.18 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 3.81)
				(name "P2.0/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 3.81)
				(name "P2.1/TA1.1")
				(number "9")
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 3.81)
				(name "P2.2/TA1.1")
				(number "10")
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 3.81)
				(name "P2.3/TA1.0")
				(number "11")
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 3.81)
				(name "P2.4/TA1.2")
				(number "12")
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 3.81)
				(name "P2.5/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 43.18 13.97 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "17")
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/TA0.0/CA1/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/TA0.1/CA2/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 3.81)
				(name "CAOUT/VREF-/VeREF-/CA3/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/VREF+/VeREF+/CA4/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 3.81)
				(name "TMS/UCB0CLK/UCA0STE/TA0.0/CA5/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/UCB0SOMI/UCB0SCL/TA0.1/CA6/A6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/CAOUT/CA7/A7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2153IPW28"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2153IPW28"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2153.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2153IPW28_0_1")
		(symbol "MSP430G2153IPW28_1_1"
			(pin input line
				(at -35.56 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "24")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 3.81)
				(name "P3.0/TA0.2")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 3.81)
				(name "P3.1/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 3.81)
				(name "P3.2/TA1.1")
				(number "13")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 3.81)
				(name "P3.3/TA1.2")
				(number "14")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 3.81)
				(name "P3.4/TA0.0")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 3.81)
				(name "P3.5/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 3.81)
				(name "P3.6/TA0.2")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 3.81)
				(name "P3.7/TA1CLK/CAOUT")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "28")
			)
			(pin input line
				(at 35.56 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "TA0CLK/ACLK/A0/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/A1/CA1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/A2/CA2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "ADC10CLK/CAOUT/VREF-/VeREF-/A3/CA3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/VREF+/VeREF+/A4/CA4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/A5/CA5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/A6/CA6/P1.6")
				(number "22")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 3.81)
				(name "TDO/TDI/CAOUT/UCB0SIMO/UCB0SDA/A7/CA7/P1.7")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 -3.81 180)
				(length 3.81)
				(name "TA1.0/P2.0")
				(number "10")
			)
			(pin bidirectional line
				(at 35.56 -6.35 180)
				(length 3.81)
				(name "TA1.1/P2.1")
				(number "11")
			)
			(pin bidirectional line
				(at 35.56 -8.89 180)
				(length 3.81)
				(name "TA1.1/P2.2")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 -11.43 180)
				(length 3.81)
				(name "TA1.0/P2.3")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 -13.97 180)
				(length 3.81)
				(name "TA1.2/P2.4")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 -16.51 180)
				(length 3.81)
				(name "TA1.2/P2.5")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 -19.05 180)
				(length 3.81)
				(name "TA0.1/XIN/P2.6")
				(number "27")
			)
			(pin bidirectional line
				(at 35.56 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2153IRHB32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2153IRHB32"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2153.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2153IRHB32_0_1")
		(symbol "MSP430G2153IRHB32_1_1"
			(pin input line
				(at -35.56 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "23")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 3.81)
				(name "P3.0/TA0.2")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 3.81)
				(name "P3.1/TA1.0")
				(number "6")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 3.81)
				(name "P3.2/TA1.1")
				(number "12")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 3.81)
				(name "P3.3/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 3.81)
				(name "P3.4/TA0.0")
				(number "14")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 3.81)
				(name "P3.5/TA0.1")
				(number "18")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 3.81)
				(name "P3.6/TA0.2")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 3.81)
				(name "P3.7/TA1CLK/CAOUT")
				(number "20")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "29")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "27")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "30")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "28")
			)
			(pin input line
				(at 35.56 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "TA0CLK/ACLK/A0/CA0/P1.0")
				(number "31")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/A1/CA1/P1.1")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/A2/CA2/P1.2")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "ADC10CLK/CAOUT/VREF-/VeREF-/A3/CA3/P1.3")
				(number "3")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/VREF+/VeREF+/A4/CA4/P1.4")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/A5/CA5/P1.5")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/A6/CA6/P1.6")
				(number "21")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 3.81)
				(name "TDO/TDI/CAOUT/UCB0SIMO/UCB0SDA/A7/CA7/P1.7")
				(number "22")
			)
			(pin bidirectional line
				(at 35.56 -3.81 180)
				(length 3.81)
				(name "TA1.0/P2.0")
				(number "9")
			)
			(pin bidirectional line
				(at 35.56 -6.35 180)
				(length 3.81)
				(name "TA1.1/P2.1")
				(number "10")
			)
			(pin bidirectional line
				(at 35.56 -8.89 180)
				(length 3.81)
				(name "TA1.1/P2.2")
				(number "11")
			)
			(pin bidirectional line
				(at 35.56 -11.43 180)
				(length 3.81)
				(name "TA1.0/P2.3")
				(number "15")
			)
			(pin bidirectional line
				(at 35.56 -13.97 180)
				(length 3.81)
				(name "TA1.2/P2.4")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 -16.51 180)
				(length 3.81)
				(name "TA1.2/P2.5")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 -19.05 180)
				(length 3.81)
				(name "TA0.1/XIN/P2.6")
				(number "26")
			)
			(pin bidirectional line
				(at 35.56 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2203IN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 17.78 0)
		)
		(property "Value" "MSP430G2203IN20"
			(at 21.59 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -27.94 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2203.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2203IN20_0_1")
		(symbol "MSP430G2203IN20_1_1"
			(pin input line
				(at -33.02 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P2.0/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P2.1/TA1.1")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P2.2/TA1.1")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "P2.3/TA1.0")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "P2.4/TA1.2")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "P2.5/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 33.02 13.97 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2203IPW20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 17.78 0)
		)
		(property "Value" "MSP430G2203IPW20"
			(at 21.59 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -26.67 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2203.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2203IPW20_0_1")
		(symbol "MSP430G2203IPW20_1_1"
			(pin input line
				(at -33.02 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P2.0/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P2.1/TA1.1")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P2.2/TA1.1")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "P2.3/TA1.0")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "P2.4/TA1.2")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "P2.5/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 33.02 13.97 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2203IPW28"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2203IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2203.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2203IPW28_0_1")
		(symbol "MSP430G2203IPW28_1_1"
			(pin input line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "P3.0/TA0.2")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "P3.1/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "P3.2/TA1.1")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "P3.3/TA1.2")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P3.4/TA0.0")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P3.5/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P3.6/TA0.2")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "P3.7/TA1CLK")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "28")
			)
			(pin input line
				(at 33.02 21.59 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/P1.6")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/P1.7")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA1.0/P2.0")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -6.35 180)
				(length 3.81)
				(name "TA1.1/P2.1")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -8.89 180)
				(length 3.81)
				(name "TA1.1/P2.2")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 -11.43 180)
				(length 3.81)
				(name "TA1.0/P2.3")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 -13.97 180)
				(length 3.81)
				(name "TA1.2/P2.4")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 -16.51 180)
				(length 3.81)
				(name "TA1.2/P2.5")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 3.81)
				(name "TA0.1/XIN/P2.6")
				(number "27")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2203IRHB32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2203IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2203.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2203IRHB32_0_1")
		(symbol "MSP430G2203IRHB32_1_1"
			(pin input line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "P3.0/TA0.2")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "P3.1/TA1.0")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "P3.2/TA1.1")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "P3.3/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P3.4/TA0.0")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P3.5/TA0.1")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P3.6/TA0.2")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "P3.7/TA1CLK")
				(number "20")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "29")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "27")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "30")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "28")
			)
			(pin input line
				(at 33.02 21.59 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/P1.1")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/P1.2")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "P1.3")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/P1.4")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/P1.5")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/P1.6")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/P1.7")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA1.0/P2.0")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -6.35 180)
				(length 3.81)
				(name "TA1.1/P2.1")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -8.89 180)
				(length 3.81)
				(name "TA1.1/P2.2")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -11.43 180)
				(length 3.81)
				(name "TA1.0/P2.3")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -13.97 180)
				(length 3.81)
				(name "TA1.2/P2.4")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 -16.51 180)
				(length 3.81)
				(name "TA1.2/P2.5")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 3.81)
				(name "TA0.1/XIN/P2.6")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2210ID"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 12.7 0)
		)
		(property "Value" "MSP430G2210ID"
			(at 10.16 -12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -15.24 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2210.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2210ID_0_1")
		(symbol "MSP430G2210ID_1_1"
			(pin input line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "17")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "TA0.1/CA2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "TA0.0/CA5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "TA0.1/CA6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "CAOUT/CA7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2213IN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2213IN20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -38.1 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2213.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2213IN20_0_1")
		(symbol "MSP430G2213IN20_1_1"
			(pin input line
				(at -43.18 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 3.81)
				(name "P2.0/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 3.81)
				(name "P2.1/TA1.1")
				(number "9")
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 3.81)
				(name "P2.2/TA1.1")
				(number "10")
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 3.81)
				(name "P2.3/TA1.0")
				(number "11")
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 3.81)
				(name "P2.4/TA1.2")
				(number "12")
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 3.81)
				(name "P2.5/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 43.18 13.97 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "17")
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 3.81)
				(name "UCA0RXD/UCA0SOMI/TA0.0/CA1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 3.81)
				(name "UCA0TXD/UCA0SIMO/TA0.1/CA2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 3.81)
				(name "CAOUT/CA3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/CA4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 3.81)
				(name "TMS/UCB0CLK/UCA0STE/TA0.0/CA5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/UCB0SOMI/UCB0SCL/TA0.1/CA6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/CAOUT/CA7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2213IPW28"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2213IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2213.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2213IPW28_0_1")
		(symbol "MSP430G2213IPW28_1_1"
			(pin input line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "P3.0/TA0.2")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "P3.1/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "P3.2/TA1.1")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "P3.3/TA1.2")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "P3.4/TA0.0")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "P3.5/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "P3.6/TA0.2")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "P3.7/TA1CLK/CAOUT")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "28")
			)
			(pin input line
				(at 33.02 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/CA1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/CA2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "CAOUT/CA3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/CA4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/CA5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/CA6/P1.6")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TDO/TDI/CAOUT/UCB0SIMO/UCB0SDA/CA7/P1.7")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA1.0/P2.0")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -6.35 180)
				(length 3.81)
				(name "TA1.1/P2.1")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -8.89 180)
				(length 3.81)
				(name "TA1.1/P2.2")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 -11.43 180)
				(length 3.81)
				(name "TA1.0/P2.3")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 -13.97 180)
				(length 3.81)
				(name "TA1.2/P2.4")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 -16.51 180)
				(length 3.81)
				(name "TA1.2/P2.5")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 3.81)
				(name "TA0.1/XIN/P2.6")
				(number "27")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2213IRHB32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2213IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2213.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2213IRHB32_0_1")
		(symbol "MSP430G2213IRHB32_1_1"
			(pin input line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "P3.0/TA0.2")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "P3.1/TA1.0")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "P3.2/TA1.1")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "P3.3/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "P3.4/TA0.0")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "P3.5/TA0.1")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "P3.6/TA0.2")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "P3.7/TA1CLK/CAOUT")
				(number "20")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "29")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "27")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "30")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "28")
			)
			(pin input line
				(at 33.02 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/P1.0")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/CA1/P1.1")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/CA2/P1.2")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "CAOUT/CA3/P1.3")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/CA4/P1.4")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/CA5/P1.5")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/CA6/P1.6")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TDO/TDI/CAOUT/UCB0SIMO/UCB0SDA/CA7/P1.7")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA1.0/P2.0")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -6.35 180)
				(length 3.81)
				(name "TA1.1/P2.1")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -8.89 180)
				(length 3.81)
				(name "TA1.1/P2.2")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -11.43 180)
				(length 3.81)
				(name "TA1.0/P2.3")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -13.97 180)
				(length 3.81)
				(name "TA1.2/P2.4")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 -16.51 180)
				(length 3.81)
				(name "TA1.2/P2.5")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 3.81)
				(name "TA0.1/XIN/P2.6")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2230ID"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 12.7 0)
		)
		(property "Value" "MSP430G2230ID"
			(at 12.7 -12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -17.78 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2230.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2230ID_0_1")
		(symbol "MSP430G2230ID_1_1"
			(pin input line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "6")
			)
			(pin input line
				(at -22.86 0 0)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "DVSS")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TA0.1/A2/P1.2")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "TA0.0/SCLK/A5/P1.5")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "TA0.1/SDO/SCL/A6/P1.6")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "SDI/SDA/A7/P1.7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2233IN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 17.78 0)
		)
		(property "Value" "MSP430G2233IN20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -30.48 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2233.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "2kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2233IN20_0_1")
		(symbol "MSP430G2233IN20_1_1"
			(pin input line
				(at -38.1 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "P2.0/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "P2.1/TA1.1")
				(number "9")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "P2.2/TA1.1")
				(number "10")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "P2.3/TA1.0")
				(number "11")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "P2.4/TA1.2")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "P2.5/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 1.27 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 1.27 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 38.1 13.97 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "17")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/VREF+/VeREF+/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/A6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/A7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2233IPW20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 17.78 0)
		)
		(property "Value" "MSP430G2233IPW20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -30.48 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2233.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2233IPW20_0_1")
		(symbol "MSP430G2233IPW20_1_1"
			(pin input line
				(at -38.1 11.43 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "P2.0/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "P2.1/TA1.1")
				(number "9")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "P2.2/TA1.1")
				(number "10")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "P2.3/TA1.0")
				(number "11")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "P2.4/TA1.2")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "P2.5/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 3.81)
				(name "P2.6/XIN/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "P2.7/XOUT")
				(number "18")
			)
			(pin power_in line
				(at 1.27 20.32 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 1.27 -19.05 90)
				(length 3.81)
				(name "DVSS")
				(number "20")
			)
			(pin input line
				(at 38.1 13.97 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "17")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/VREF+/VeREF+/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/A6/P1.6")
				(number "14")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/A7/P1.7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2233IPW28"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2233IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2233.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2233IPW28_0_1")
		(symbol "MSP430G2233IPW28_1_1"
			(pin input line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "P3.0/TA0.2")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "P3.1/TA1.0")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "P3.2/TA1.1")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "P3.3/TA1.2")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "P3.4/TA0.0")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "P3.5/TA0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "P3.6/TA0.2")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "P3.7/TA1CLK")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "28")
			)
			(pin input line
				(at 33.02 21.59 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/A0/P1.0")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/A1/P1.1")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/A2/P1.2")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/VREF+/VeREF+/A4/P1.4")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/A5/P1.5")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/A6/P1.6")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/A7/P1.7")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA1.0/P2.0")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -6.35 180)
				(length 3.81)
				(name "TA1.1/P2.1")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -8.89 180)
				(length 3.81)
				(name "TA1.1/P2.2")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 -11.43 180)
				(length 3.81)
				(name "TA1.0/P2.3")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 -13.97 180)
				(length 3.81)
				(name "TA1.2/P2.4")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 -16.51 180)
				(length 3.81)
				(name "TA1.2/P2.5")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 3.81)
				(name "TA0.1/XIN/P2.6")
				(number "27")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2233IRHB32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2233IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2233.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2233IRHB32_0_1")
		(symbol "MSP430G2233IRHB32_1_1"
			(pin input line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "P3.0/TA0.2")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "P3.1/TA1.0")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "P3.2/TA1.1")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "P3.3/TA1.2")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "P3.4/TA0.0")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "P3.5/TA0.1")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "P3.6/TA0.2")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "P3.7/TA1CLK")
				(number "20")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "29")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "27")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "30")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "28")
			)
			(pin input line
				(at 33.02 21.59 180)
				(length 3.81)
				(name "TEST/SBWTCK")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TA0CLK/ACLK/CA0/A0/P1.0")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "TA0.0/UCA0RXD/UCA0SOMI/A1/P1.1")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "TA0.1/UCA0TXD/UCA0SIMO/A2/P1.2")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "ADC10CLK/VREF-/VeREF-/A3/P1.3")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/UCB0STE/UCA0CLK/VREF+/VeREF+/A4/P1.4")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/UCB0CLK/UCA0STE/A5/P1.5")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA0.1/UCB0SOMI/UCB0SCL/A6/P1.6")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TDO/TDI/UCB0SIMO/UCB0SDA/A7/P1.7")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA1.0/P2.0")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -6.35 180)
				(length 3.81)
				(name "TA1.1/P2.1")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -8.89 180)
				(length 3.81)
				(name "TA1.1/P2.2")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -11.43 180)
				(length 3.81)
				(name "TA1.0/P2.3")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -13.97 180)
				(length 3.81)
				(name "TA1.2/P2.4")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 -16.51 180)
				(length 3.81)
				(name "TA1.2/P2.5")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 3.81)
				(name "TA0.1/XIN/P2.6")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2444IDA38"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2444IDA38"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2444.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2444IDA38_0_1")
		(symbol "MSP430G2444IDA38_1_1"
			(pin input line
				(at -29.21 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "7")
			)
			(pin bidirectional line
				(at -29.21 17.78 0)
				(length 3.81)
				(name "P3.0/A5/UCB0STE/UCA0CLK")
				(number "11")
			)
			(pin bidirectional line
				(at -29.21 15.24 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "12")
			)
			(pin bidirectional line
				(at -29.21 12.7 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "13")
			)
			(pin bidirectional line
				(at -29.21 10.16 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "14")
			)
			(pin bidirectional line
				(at -29.21 7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "25")
			)
			(pin bidirectional line
				(at -29.21 5.08 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "26")
			)
			(pin bidirectional line
				(at -29.21 2.54 0)
				(length 3.81)
				(name "P3.6/A6")
				(number "27")
			)
			(pin bidirectional line
				(at -29.21 0 0)
				(length 3.81)
				(name "P3.7/A7")
				(number "28")
			)
			(pin bidirectional line
				(at -29.21 -3.81 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "17")
			)
			(pin bidirectional line
				(at -29.21 -6.35 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "18")
			)
			(pin bidirectional line
				(at -29.21 -8.89 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "19")
			)
			(pin bidirectional line
				(at -29.21 -11.43 0)
				(length 3.81)
				(name "P4.3/A12/TB0")
				(number "20")
			)
			(pin bidirectional line
				(at -29.21 -13.97 0)
				(length 3.81)
				(name "P4.4/A13/TB1")
				(number "21")
			)
			(pin bidirectional line
				(at -29.21 -16.51 0)
				(length 3.81)
				(name "P4.5/A14/TB2")
				(number "22")
			)
			(pin bidirectional line
				(at -29.21 -19.05 0)
				(length 3.81)
				(name "P4.6/A15/TBOUTH")
				(number "23")
			)
			(pin bidirectional line
				(at -29.21 -21.59 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "24")
			)
			(pin power_in line
				(at -3.81 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "16")
			)
			(pin power_in line
				(at -3.81 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "15")
			)
			(pin power_in line
				(at 3.81 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "2")
			)
			(pin power_in line
				(at 3.81 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "4")
			)
			(pin input line
				(at 29.21 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 29.21 17.78 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "31")
			)
			(pin bidirectional line
				(at 29.21 15.24 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "32")
			)
			(pin bidirectional line
				(at 29.21 12.7 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "33")
			)
			(pin bidirectional line
				(at 29.21 10.16 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "34")
			)
			(pin bidirectional line
				(at 29.21 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/P1.4")
				(number "35")
			)
			(pin bidirectional line
				(at 29.21 5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "36")
			)
			(pin bidirectional line
				(at 29.21 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "37")
			)
			(pin bidirectional line
				(at 29.21 0 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "38")
			)
			(pin bidirectional line
				(at 29.21 -3.81 180)
				(length 3.81)
				(name "ACLK/A0/P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at 29.21 -6.35 180)
				(length 3.81)
				(name "TAINCLK/SMCLK/A1/P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at 29.21 -8.89 180)
				(length 3.81)
				(name "TA0/A2/P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at 29.21 -11.43 180)
				(length 3.81)
				(name "TA1/VREF-/VeREF-/A3/P2.3")
				(number "29")
			)
			(pin bidirectional line
				(at 29.21 -13.97 180)
				(length 3.81)
				(name "TA2/VREF+/VeREF+/A4/P2.4")
				(number "30")
			)
			(pin bidirectional line
				(at 29.21 -16.51 180)
				(length 3.81)
				(name "Rosc/P2.5")
				(number "3")
			)
			(pin bidirectional line
				(at 29.21 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "6")
			)
			(pin bidirectional line
				(at 29.21 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2444IRHA40"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2444IRHA40"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2444.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
		(symbol "MSP430G2444IRHA40_0_1")
		(symbol "MSP430G2444IRHA40_1_1"
			(pin input line
				(at -29.21 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "5")
			)
			(pin bidirectional line
				(at -29.21 17.78 0)
				(length 3.81)
				(name "P3.0/UCB0STE/UCA0CLK/A5")
				(number "9")
			)
			(pin bidirectional line
				(at -29.21 15.24 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "10")
			)
			(pin bidirectional line
				(at -29.21 12.7 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -29.21 10.16 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "12")
			)
			(pin bidirectional line
				(at -29.21 7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "23")
			)
			(pin bidirectional line
				(at -29.21 5.08 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "24")
			)
			(pin bidirectional line
				(at -29.21 2.54 0)
				(length 3.81)
				(name "P3.6/A6")
				(number "25")
			)
			(pin bidirectional line
				(at -29.21 0 0)
				(length 3.81)
				(name "P3.7/A7")
				(number "26")
			)
			(pin bidirectional line
				(at -29.21 -3.81 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "15")
			)
			(pin bidirectional line
				(at -29.21 -6.35 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "16")
			)
			(pin bidirectional line
				(at -29.21 -8.89 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "17")
			)
			(pin bidirectional line
				(at -29.21 -11.43 0)
				(length 3.81)
				(name "P4.3/TB0/A12")
				(number "18")
			)
			(pin bidirectional line
				(at -29.21 -13.97 0)
				(length 3.81)
				(name "P4.4/TB1/A13")
				(number "19")
			)
			(pin bidirectional line
				(at -29.21 -16.51 0)
				(length 3.81)
				(name "P4.5/TB2/A14")
				(number "20")
			)
			(pin bidirectional line
				(at -29.21 -19.05 0)
				(length 3.81)
				(name "P4.6/TBOUTH/A15")
				(number "21")
			)
			(pin bidirectional line
				(at -29.21 -21.59 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "22")
			)
			(pin power_in line
				(at -3.81 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin power_in line
				(at 3.81 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "38")
			)
			(pin power_in line
				(at 3.81 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "1")
			)
			(pin power_in line
				(at 6.35 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "39")
			)
			(pin power_in line
				(at 6.35 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "4")
			)
			(pin input line
				(at 29.21 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "37")
			)
			(pin bidirectional line
				(at 29.21 17.78 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "29")
			)
			(pin bidirectional line
				(at 29.21 15.24 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "30")
			)
			(pin bidirectional line
				(at 29.21 12.7 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "31")
			)
			(pin bidirectional line
				(at 29.21 10.16 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "32")
			)
			(pin bidirectional line
				(at 29.21 7.62 180)
				(length 3.81)
				(name "SMCLK/TCK/P1.4")
				(number "33")
			)
			(pin bidirectional line
				(at 29.21 5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "34")
			)
			(pin bidirectional line
				(at 29.21 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "35")
			)
			(pin bidirectional line
				(at 29.21 0 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "36")
			)
			(pin bidirectional line
				(at 29.21 -3.81 180)
				(length 3.81)
				(name "ACLK/A0/P2.0")
				(number "6")
			)
			(pin bidirectional line
				(at 29.21 -6.35 180)
				(length 3.81)
				(name "TAINCLK/SMCLK/A1/P2.1")
				(number "7")
			)
			(pin bidirectional line
				(at 29.21 -8.89 180)
				(length 3.81)
				(name "TA0/A2/P2.2")
				(number "8")
			)
			(pin bidirectional line
				(at 29.21 -11.43 180)
				(length 3.81)
				(name "TA1/VREF-/VeREF-/A3/P2.3")
				(number "27")
			)
			(pin bidirectional line
				(at 29.21 -13.97 180)
				(length 3.81)
				(name "TA2/VREF+/VeREF+/A4/P2.4")
				(number "28")
			)
			(pin bidirectional line
				(at 29.21 -16.51 180)
				(length 3.81)
				(name "ROSC/P2.5")
				(number "40")
			)
			(pin bidirectional line
				(at 29.21 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "3")
			)
			(pin bidirectional line
				(at 29.21 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2444IYFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2444IYFF"
			(at 22.86 -25.4 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2444.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2444IYFF_0_1")
		(symbol "MSP430G2444IYFF_1_1"
			(pin input line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "B3")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "P3.0/A5/UCB0STE/UCA0CLK")
				(number "B5")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "A6")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "A7")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "B6")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "G6")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "G5")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P3.6/A6")
				(number "F4")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "P3.7/A7")
				(number "G4")
			)
			(pin bidirectional line
				(at -33.02 -3.81 0)
				(length 3.81)
				(name "P4.0/TB0")
				(number "D6")
			)
			(pin bidirectional line
				(at -33.02 -6.35 0)
				(length 3.81)
				(name "P4.1/TB1")
				(number "D7")
			)
			(pin bidirectional line
				(at -33.02 -8.89 0)
				(length 3.81)
				(name "P4.2/TB2")
				(number "E6")
			)
			(pin bidirectional line
				(at -33.02 -11.43 0)
				(length 3.81)
				(name "P4.3/A12/TB0")
				(number "E7")
			)
			(pin bidirectional line
				(at -33.02 -13.97 0)
				(length 3.81)
				(name "P4.4/A13/TB1")
				(number "F7")
			)
			(pin bidirectional line
				(at -33.02 -16.51 0)
				(length 3.81)
				(name "P4.5/A14/TB2")
				(number "F6")
			)
			(pin bidirectional line
				(at -33.02 -19.05 0)
				(length 3.81)
				(name "P4.6/A15/TBOUTH")
				(number "G7")
			)
			(pin bidirectional line
				(at -33.02 -21.59 0)
				(length 3.81)
				(name "P4.7/TBCLK")
				(number "F5")
			)
			(pin power_in line
				(at -10.16 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "C6")
			)
			(pin power_in line
				(at -7.62 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "C7")
			)
			(pin power_in line
				(at -7.62 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "B7")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "D5")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "C5")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "C1")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "A3")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "D3")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "B1")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "D4")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "B2")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "E4")
			)
			(pin power_in line
				(at 7.62 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "C3")
			)
			(pin power_in line
				(at 10.16 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "E5")
			)
			(pin power_in line
				(at 10.16 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "C4")
			)
			(pin input line
				(at 33.02 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "D1")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TACLK/ADC10CLK/P1.0")
				(number "F2")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "TA0/P1.1")
				(number "G2")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "TA1/P1.2")
				(number "E2")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "TA2/P1.3")
				(number "G1")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/P1.4")
				(number "F1")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TMS/TA0/P1.5")
				(number "E1")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "TDI/TCLK/TA1/P1.6")
				(number "E3")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TDO/TDI/TA2/P1.7")
				(number "D2")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "ACLK/A0/P2.0")
				(number "A4")
			)
			(pin bidirectional line
				(at 33.02 -6.35 180)
				(length 3.81)
				(name "TAINCLK/SMCLK/A1/P2.1")
				(number "B4")
			)
			(pin bidirectional line
				(at 33.02 -8.89 180)
				(length 3.81)
				(name "TA0/A2/P2.2")
				(number "A5")
			)
			(pin bidirectional line
				(at 33.02 -11.43 180)
				(length 3.81)
				(name "TA1/VREF-/VeREF-/A3/P2.3")
				(number "F3")
			)
			(pin bidirectional line
				(at 33.02 -13.97 180)
				(length 3.81)
				(name "TA2/VREF+/VeREF+/A4/P2.4")
				(number "G3")
			)
			(pin bidirectional line
				(at 33.02 -16.51 180)
				(length 3.81)
				(name "ROSC/P2.5")
				(number "C2")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "A2")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "A1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2755IDA38"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2755IDA38"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2755.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB Flash, 4kB RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MSP430G2755IDA38_0_1")
		(symbol "MSP430G2755IDA38_1_1"
			(pin input line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "P4.0/CA0/TB0.0")
				(number "17")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "P4.1/CA1/TB0.1")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "P4.2/CA2/TB0.2")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "P4.3/A12/CA3/TB0.0")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P4.4/A13/CA4/TB0.1")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P4.5/A14/CA5/TB0.2")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P4.6/A15/CA6/TB0OUTH")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "P4.7/CA7/TB0CLK")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 -3.81 0)
				(length 3.81)
				(name "P3.0/A5/UCB0STE/UCA0CLK")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -6.35 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -8.89 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -11.43 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 -13.97 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "25")
			)
			(pin bidirectional line
				(at -33.02 -16.51 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "26")
			)
			(pin bidirectional line
				(at -33.02 -19.05 0)
				(length 3.81)
				(name "P3.6/A6/TA1.1")
				(number "27")
			)
			(pin bidirectional line
				(at -33.02 -21.59 0)
				(length 3.81)
				(name "P3.7/A7/TA1.2")
				(number "28")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "16")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "15")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "2")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "4")
			)
			(pin input line
				(at 33.02 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "TA0CLK/ADC10CLK/P1.0")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "32")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/P1.4")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/P1.5")
				(number "36")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "TDI/TA0.1/P1.6")
				(number "37")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "TDO/TDI/TA0.2/P1.7")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 3.81)
				(name "TA1CLK/ACLK/A0/P2.0")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -6.35 180)
				(length 3.81)
				(name "TA0INCLK/SMCLK/A1/P2.1")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -8.89 180)
				(length 3.81)
				(name "TA0.0/A2/P2.2")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -11.43 180)
				(length 3.81)
				(name "TA0.1/VREF-/VeREF-/A3/P2.3")
				(number "29")
			)
			(pin bidirectional line
				(at 33.02 -13.97 180)
				(length 3.81)
				(name "TA0.2/VREF+/VeREF+/A4/P2.4")
				(number "30")
			)
			(pin bidirectional line
				(at 33.02 -16.51 180)
				(length 3.81)
				(name "TA1.0/ROSC/P2.5")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSP430G2755IRHA40"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2755IRHA40"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2755.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB Flash, 4kB RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
		(symbol "MSP430G2755IRHA40_0_1")
		(symbol "MSP430G2755IRHA40_1_1"
			(pin input line
				(at -33.02 21.59 0)
				(length 3.81)
				(name "~{RST}/NMI/SBWTDIO")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "P4.0/CA0/TB0.0")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "P4.1/CA1/TB0.1")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "P4.2/CA2/TB0.2")
				(number "17")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "P4.3/A12/CA3/TB0.0")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "P4.4/A13/CA4/TB0.1")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "P4.5/A14/CA5/TB0.2")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "P4.6/A15/CA6/TB0OUTH")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "P4.7/CA7/TB0CLK")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 -3.81 0)
				(length 3.81)
				(name "P3.0/A5/UCB0STE/UCA0CLK")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 -6.35 0)
				(length 3.81)
				(name "P3.1/UCB0SIMO/UCB0SDA")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 -8.89 0)
				(length 3.81)
				(name "P3.2/UCB0SOMI/UCB0SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -11.43 0)
				(length 3.81)
				(name "P3.3/UCB0CLK/UCA0STE")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -13.97 0)
				(length 3.81)
				(name "P3.4/UCA0TXD/UCA0SIMO")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 -16.51 0)
				(length 3.81)
				(name "P3.5/UCA0RXD/UCA0SOMI")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 -19.05 0)
				(length 3.81)
				(name "P3.6/A6/TA1.1")
				(number "25")
			)
			(pin bidirectional line
				(at -33.02 -21.59 0)
				(length 3.81)
				(name "P3.7/A6/TA1.2")
				(number "26")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "AVCC")
				(number "14")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "AVSS")
				(number "13")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "38")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "1")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "DVCC")
				(number "39")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "DVSS")
				(number "4")
			)
			(pin input line
				(at 31.75 21.59 180)
				(length 3.81)
				(name "SBWTCK/TEST")
				(number "37")
			)
			(pin bidirectional line
				(at 31.75 17.78 180)
				(length 3.81)
				(name "TA0CLK/ADC10CLK/P1.0")
				(number "29")
			)
			(pin bidirectional line
				(at 31.75 15.24 180)
				(length 3.81)
				(name "TA0.0/P1.1")
				(number "30")
			)
			(pin bidirectional line
				(at 31.75 12.7 180)
				(length 3.81)
				(name "TA0.1/P1.2")
				(number "31")
			)
			(pin bidirectional line
				(at 31.75 10.16 180)
				(length 3.81)
				(name "TA0.2/P1.3")
				(number "32")
			)
			(pin bidirectional line
				(at 31.75 7.62 180)
				(length 3.81)
				(name "TCK/SMCLK/P1.4")
				(number "33")
			)
			(pin bidirectional line
				(at 31.75 5.08 180)
				(length 3.81)
				(name "TMS/TA0.0/P1.5")
				(number "34")
			)
			(pin bidirectional line
				(at 31.75 2.54 180)
				(length 3.81)
				(name "TDI/TA0.1/P1.6")
				(number "35")
			)
			(pin bidirectional line
				(at 31.75 0 180)
				(length 3.81)
				(name "TDO/TDI/TA0.2/P1.7")
				(number "36")
			)
			(pin bidirectional line
				(at 31.75 -3.81 180)
				(length 3.81)
				(name "TA1CLK/ACLK/A0/P2.0")
				(number "6")
			)
			(pin bidirectional line
				(at 31.75 -6.35 180)
				(length 3.81)
				(name "TA0INCLK/SMCLK/A1/P2.1")
				(number "7")
			)
			(pin bidirectional line
				(at 31.75 -8.89 180)
				(length 3.81)
				(name "TA0.0/A2/P2.2")
				(number "8")
			)
			(pin bidirectional line
				(at 31.75 -11.43 180)
				(length 3.81)
				(name "TA0.1/VREF-/VeREF-/A3/P2.3")
				(number "27")
			)
			(pin bidirectional line
				(at 31.75 -13.97 180)
				(length 3.81)
				(name "TA0.2/VREF+/VeREF+/A4/P2.4")
				(number "28")
			)
			(pin bidirectional line
				(at 31.75 -16.51 180)
				(length 3.81)
				(name "TA1.0/ROSC/P2.5")
				(number "40")
			)
			(pin bidirectional line
				(at 31.75 -19.05 180)
				(length 3.81)
				(name "XIN/P2.6")
				(number "3")
			)
			(pin bidirectional line
				(at 31.75 -21.59 180)
				(length 3.81)
				(name "XOUT/P2.7")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC430F5133xRGZ"
		(extends "CC430F5137xRGZ")
		(property "Reference" "U"
			(at -11.43 34.29 0)
		)
		(property "Value" "CC430F5133xRGZ"
			(at 13.97 34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-48-1EP_7x7mm_P0.5mm_EP4.1x4.1mm_ThermalVias"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cc430f5137.pdf"
			(at -10.16 31.75 0)
		)
		(property "Description" "8KB Flash, 2KB RAM, MSP430 core with integrated CC1101 radio transceiver, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 CC430 16-bit mixed signal microcontroller CC1101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CC430F5135xRGZ"
		(extends "CC430F5137xRGZ")
		(property "Reference" "U"
			(at -11.43 34.29 0)
		)
		(property "Value" "CC430F5135xRGZ"
			(at 13.97 34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-48-1EP_7x7mm_P0.5mm_EP4.1x4.1mm_ThermalVias"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cc430f5137.pdf"
			(at -10.16 31.75 0)
		)
		(property "Description" "16KB Flash, 2KB RAM, MSP430 core with integrated CC1101 radio transceiver, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 CC430 16-bit mixed signal microcontroller CC1101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430AFE231IPW"
		(extends "MSP430AFE221IPW")
		(property "Reference" "U"
			(at -22.86 19.05 0)
		)
		(property "Value" "MSP430AFE231IPW"
			(at 15.24 -19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at -21.59 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430afe231.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430AFE232IPW"
		(extends "MSP430AFE222IPW")
		(property "Reference" "U"
			(at -22.86 19.05 0)
		)
		(property "Value" "MSP430AFE232IPW"
			(at 15.24 -19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at -21.59 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430afe232.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430AFE233IPW"
		(extends "MSP430AFE223IPW")
		(property "Reference" "U"
			(at -22.86 19.05 0)
		)
		(property "Value" "MSP430AFE233IPW"
			(at 15.24 -19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at -21.59 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430afe233.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430AFE251IPW"
		(extends "MSP430AFE221IPW")
		(property "Reference" "U"
			(at -22.86 19.05 0)
		)
		(property "Value" "MSP430AFE251IPW"
			(at 15.24 -19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at -21.59 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430afe251.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430AFE252IPW"
		(extends "MSP430AFE222IPW")
		(property "Reference" "U"
			(at -22.86 19.05 0)
		)
		(property "Value" "MSP430AFE252IPW"
			(at 15.24 -19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at -21.59 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430afe252.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430AFE253IPW"
		(extends "MSP430AFE223IPW")
		(property "Reference" "U"
			(at -22.86 19.05 0)
		)
		(property "Value" "MSP430AFE253IPW"
			(at 15.24 -19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at -21.59 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430afe253.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1111AIDGV"
		(extends "MSP430F1101AIDGV")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1111AIDGV"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1111a.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, TVSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1111AIDW"
		(extends "MSP430F1101AIDW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1111AIDW"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1111a.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, SOWB-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1111AIPW"
		(extends "MSP430F1101AIPW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1111AIPW"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1111a.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1111AIRGE"
		(extends "MSP430F1101AIRGE")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1111AIRGE"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1111a.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1121AIDGV"
		(extends "MSP430F1101AIDGV")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1121AIDGV"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1121a.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, TVSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1121AIDW"
		(extends "MSP430F1101AIDW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1121AIDW"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1121a.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, SOWB-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1121AIPW"
		(extends "MSP430F1101AIPW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1121AIPW"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1121a.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1121AIRGE"
		(extends "MSP430F1101AIRGE")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F1121AIRGE"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1121a.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1132IDW"
		(extends "MSP430F1122IDW")
		(property "Reference" "U"
			(at -17.78 15.24 0)
		)
		(property "Value" "MSP430F1132IDW"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1132.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, SOWB-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1132IPW"
		(extends "MSP430F1122IPW")
		(property "Reference" "U"
			(at -17.78 15.24 0)
		)
		(property "Value" "MSP430F1132IPW"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1132.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1132IRHB"
		(extends "MSP430F1122IRHB")
		(property "Reference" "U"
			(at -17.78 15.24 0)
		)
		(property "Value" "MSP430F1132IRHB"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1132.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1232IDW"
		(extends "MSP430F1222IDW")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F1232IDW"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1232.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, SOWB-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1232IPW"
		(extends "MSP430F1222IPW")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F1232IPW"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1232.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F1232IRHB"
		(extends "MSP430F1222IRHB")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F1232IRHB"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f1232.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F123IDW"
		(extends "MSP430F122IDW")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F123IDW"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f123.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, SOWB-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F123IPW"
		(extends "MSP430F122IPW")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F123IPW"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f123.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F123IRHB"
		(extends "MSP430F122IRHB")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "MSP430F123IRHB"
			(at 12.7 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -16.51 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f123.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2011IN"
		(extends "MSP430F2001IN")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2011IN"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2011.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2011IPW"
		(extends "MSP430F2001IPW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2011IPW"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2011.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2011IRSA"
		(extends "MSP430F2001IRSA")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2011IRSA"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2011.pdf"
			(at -20.32 13.97 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2012IN"
		(extends "MSP430F2002IN")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2012IN"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2012.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2012IPW"
		(extends "MSP430F2002IPW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2012IPW"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2012.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2012IRSA"
		(extends "MSP430F2002IRSA")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2012IRSA"
			(at 11.43 -17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -13.97 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2012.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2013IN"
		(extends "MSP430F2003IN")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2013IN"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at -15.24 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2013.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2013IPW"
		(extends "MSP430F2003IPW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2013IPW"
			(at 11.43 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2013.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2013IRSA"
		(extends "MSP430F2003IRSA")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2013IRSA"
			(at 11.43 -17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -13.97 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2013.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2111IDGV"
		(extends "MSP430F2101IDGV")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2111IDGV"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2111.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, TVSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2111IDW"
		(extends "MSP430F2101IDW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2111IDW"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2111.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, SOWB-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2111IPW"
		(extends "MSP430F2101IPW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2111IPW"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2111.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2111IRGE"
		(extends "MSP430F2101IRGE")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2111IRGE"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2111.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB + 256B Flash, 128B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2121IDGV"
		(extends "MSP430F2101IDGV")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2121IDGV"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2121.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, TVSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2121IDW"
		(extends "MSP430F2101IDW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2121IDW"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2121.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, SOWB-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2121IPW"
		(extends "MSP430F2101IPW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2121IPW"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2121.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2121IRGE"
		(extends "MSP430F2101IRGE")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2121IRGE"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2121.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 256B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2122IPW"
		(extends "MSP430F2112IPW")
		(property "Reference" "U"
			(at -20.32 25.4 0)
		)
		(property "Value" "MSP430F2122IPW"
			(at 15.24 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -19.05 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2122.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 512B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2122IRHB"
		(extends "MSP430F2112IRHB")
		(property "Reference" "U"
			(at -20.32 25.4 0)
		)
		(property "Value" "MSP430F2122IRHB"
			(at 13.97 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -19.05 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2122.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2122IRTV"
		(extends "MSP430F2112IRTV")
		(property "Reference" "U"
			(at -20.32 25.4 0)
		)
		(property "Value" "MSP430F2122IRTV"
			(at 13.97 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -19.05 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2122.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB + 256B Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2131IDGV"
		(extends "MSP430F2101IDGV")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2131IDGV"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2131.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, TVSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2131IDW"
		(extends "MSP430F2101IDW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2131IDW"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2131.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, SOWB-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2131IPW"
		(extends "MSP430F2101IPW")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2131IPW"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2131.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2131IRGE"
		(extends "MSP430F2101IRGE")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430F2131IRGE"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2131.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 256B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2132IPW"
		(extends "MSP430F2112IPW")
		(property "Reference" "U"
			(at -20.32 25.4 0)
		)
		(property "Value" "MSP430F2132IPW"
			(at 15.24 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -19.05 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2132.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2132IRHB"
		(extends "MSP430F2112IRHB")
		(property "Reference" "U"
			(at -20.32 25.4 0)
		)
		(property "Value" "MSP430F2132IRHB"
			(at 13.97 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -19.05 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2132.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2132IRTV"
		(extends "MSP430F2112IRTV")
		(property "Reference" "U"
			(at -20.32 25.4 0)
		)
		(property "Value" "MSP430F2132IRTV"
			(at 13.97 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -19.05 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2132.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB + 256B Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2252IDA"
		(extends "MSP430F2232IDA")
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2252IDA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2252.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB + 256B Flash, 512B RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2252IRHA"
		(extends "MSP430F2232IRHA")
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2252IRHA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2252.pdf"
			(at -22.86 -27.94 0)
		)
		(property "Description" "16kB + 256B Flash, 512B RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2252IYFF"
		(extends "MSP430F2232IYFF")
		(property "Reference" "U"
			(at -29.21 25.4 0)
		)
		(property "Value" "MSP430F2252IYFF"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -27.94 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2252.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB + 256B Flash, 512B RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2254IDA"
		(extends "MSP430F2234IDA")
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2254IDA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2254.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB + 256B Flash, 512B RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2254IRHA"
		(extends "MSP430F2234IRHA")
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2254IRHA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2254.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB + 256B Flash, 512B RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2254IYFF"
		(extends "MSP430F2234IYFF")
		(property "Reference" "U"
			(at -26.67 25.4 0)
		)
		(property "Value" "MSP430F2254IYFF"
			(at 26.67 -25.4 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2254.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "16kB + 256B Flash, 512B RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2272IDA"
		(extends "MSP430F2232IDA")
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2272IDA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2272.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB + 256B Flash, 1kB RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2272IRHA"
		(extends "MSP430F2232IRHA")
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2272IRHA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2272.pdf"
			(at -22.86 -27.94 0)
		)
		(property "Description" "32kB + 256B Flash, 1kB RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2272IYFF"
		(extends "MSP430F2232IYFF")
		(property "Reference" "U"
			(at -29.21 25.4 0)
		)
		(property "Value" "MSP430F2272IYFF"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -27.94 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2272.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB + 256B Flash, 1kB RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2274IDA"
		(extends "MSP430F2234IDA")
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2274IDA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2274.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB + 256B Flash, 1kB RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2274IRHA"
		(extends "MSP430F2234IRHA")
		(property "Reference" "U"
			(at -22.86 25.4 0)
		)
		(property "Value" "MSP430F2274IRHA"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -21.59 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2274.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB + 256B Flash, 1kB RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2274IYFF"
		(extends "MSP430F2234IYFF")
		(property "Reference" "U"
			(at -26.67 25.4 0)
		)
		(property "Value" "MSP430F2274IYFF"
			(at 26.67 -25.4 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2274.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "32kB + 256B Flash, 1kB RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2350IRHA"
		(extends "MSP430F2330IRHA")
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "MSP430F2350IRHA"
			(at 12.7 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -16.51 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2350.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB + 256B Flash, 2kB RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2350IYFF"
		(extends "MSP430F2330IYFF")
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "MSP430F2350IYFF"
			(at 12.7 -29.21 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -16.51 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2350.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB + 256B Flash, 2kB RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2370IRHA"
		(extends "MSP430F2330IRHA")
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "MSP430F2370IRHA"
			(at 12.7 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -16.51 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2370.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB + 256B Flash, 2kB RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F2370IYFF"
		(extends "MSP430F2330IYFF")
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "MSP430F2370IYFF"
			(at 12.7 -29.21 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -16.51 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f2370.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB + 256B Flash, 2kB RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5219IRGC"
		(extends "MSP430F5217IRGC")
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5219IRGC"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5219.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 8kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5219IYFF"
		(extends "MSP430F5217IYFF")
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5219IYFF"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-64_3.415x3.535mm_Layout8x8_P0.4mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5219.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 8kB RAM, BGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.415x3.535mm*Layout8x8*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5229IRGC"
		(extends "MSP430F5227IRGC")
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5229IRGC"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5229.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 8kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5229IYFF"
		(extends "MSP430F5227IYFF")
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5229IYFF"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-64_3.415x3.535mm_Layout8x8_P0.4mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5229.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 8kB RAM, BGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.415x3.535mm*Layout8x8*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5234IRGZ"
		(extends "MSP430F5232IRGZ")
		(property "Reference" "U"
			(at -25.4 35.56 0)
		)
		(property "Value" "MSP430F5234IRGZ"
			(at 20.32 -35.56 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -24.13 -35.56 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5234.pdf"
			(at -25.4 31.75 0)
		)
		(property "Description" "128kB Flash, 8kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5239IRGC"
		(extends "MSP430F5237IRGC")
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5239IRGC"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5239.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 8kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5244IRGZ"
		(extends "MSP430F5242IRGZ")
		(property "Reference" "U"
			(at -25.4 35.56 0)
		)
		(property "Value" "MSP430F5244IRGZ"
			(at 20.32 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -24.13 -33.02 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5244.pdf"
			(at -25.4 33.02 0)
		)
		(property "Description" "128kB Flash, 8kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5249IRGC"
		(extends "MSP430F5247IRGC")
		(property "Reference" "U"
			(at -24.13 43.18 0)
		)
		(property "Value" "MSP430F5249IRGC"
			(at 19.05 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5249.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 8kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5309IPT"
		(extends "MSP430F5308IPT")
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "MSP430F5309IPT"
			(at 16.51 -29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5309.pdf"
			(at 0 0 0)
		)
		(property "Description" "24kB Flash, 6kB RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5309IRGC"
		(extends "MSP430F5308IRGC")
		(property "Reference" "U"
			(at -27.94 43.18 0)
		)
		(property "Value" "MSP430F5309IRGC"
			(at 21.59 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -26.67 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5309.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "24kB Flash, 6kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5309IRGZ"
		(extends "MSP430F5308IRGZ")
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "MSP430F5309IRGZ"
			(at 16.51 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -20.32 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5309.pdf"
			(at 0 0 0)
		)
		(property "Description" "24kB Flash, 6kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5309IZQE"
		(extends "MSP430F5308IZQE")
		(property "Reference" "U"
			(at -27.94 46.99 0)
		)
		(property "Value" "MSP430F5309IZQE"
			(at -21.59 45.72 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-80_5.0x5.0mm_Layout9x9_P0.5mm"
			(at 26.67 45.72 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5309.pdf"
			(at 0 0 0)
		)
		(property "Description" "24kB Flash, 6kB RAM, BGA-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*5.0x5.0mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5310IPT"
		(extends "MSP430F5308IPT")
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "MSP430F5310IPT"
			(at 16.51 -29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5310.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB Flash, 6kB RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5310IRGC"
		(extends "MSP430F5308IRGC")
		(property "Reference" "U"
			(at -27.94 43.18 0)
		)
		(property "Value" "MSP430F5310IRGC"
			(at 21.59 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGC0064B_VQFN-64-1EP_9x9mm_P0.5mm_EP4.25x4.25mm"
			(at -26.67 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5310.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32kB Flash, 6kB RAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGC0064B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5310IRGZ"
		(extends "MSP430F5308IRGZ")
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "MSP430F5310IRGZ"
			(at 16.51 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -20.32 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5310.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB Flash, 6kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5310IZQE"
		(extends "MSP430F5308IZQE")
		(property "Reference" "U"
			(at -27.94 46.99 0)
		)
		(property "Value" "MSP430F5310IZQE"
			(at -21.59 45.72 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-80_5.0x5.0mm_Layout9x9_P0.5mm"
			(at 26.67 45.72 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5310.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB Flash, 6kB RAM, BGA-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*5.0x5.0mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5335IPZ"
		(extends "MSP430F5333IPZ")
		(property "Reference" "U"
			(at -29.21 60.96 0)
		)
		(property "Value" "MSP430F5335IPZ"
			(at 24.13 -63.5 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -27.94 -63.5 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5335.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "256kB Flash, 18kB RAM, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5335IZQW"
		(extends "MSP430F5333IZQW")
		(property "Reference" "U"
			(at -29.21 67.31 0)
		)
		(property "Value" "MSP430F5335IZQW"
			(at -22.86 66.04 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 66.04 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5335.pdf"
			(at 0 0 0)
		)
		(property "Description" "256kB Flash, 18kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5338IPZ"
		(extends "MSP430F5336IPZ")
		(property "Reference" "U"
			(at -29.21 60.96 0)
		)
		(property "Value" "MSP430F5338IPZ"
			(at 24.13 -63.5 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -27.94 -63.5 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5338.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "256kB Flash, 18kB RAM, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5338IZQW"
		(extends "MSP430F5336IZQW")
		(property "Reference" "U"
			(at -29.21 67.31 0)
		)
		(property "Value" "MSP430F5338IZQW"
			(at -22.86 66.04 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 66.04 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5338.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 18kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5341IRGZ"
		(extends "MSP430F5340IRGZ")
		(property "Reference" "U"
			(at -26.67 34.29 0)
		)
		(property "Value" "MSP430F5341IRGZ"
			(at 17.78 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -25.4 -34.29 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5341.pdf"
			(at 0 0 0)
		)
		(property "Description" "96kB Flash, 8kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5342IRGZ"
		(extends "MSP430F5340IRGZ")
		(property "Reference" "U"
			(at -26.67 34.29 0)
		)
		(property "Value" "MSP430F5342IRGZ"
			(at 17.78 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -25.4 -34.29 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5342.pdf"
			(at 0 0 0)
		)
		(property "Description" "128kB Flash, 10kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5359IZQW"
		(extends "MSP430F5358IZQW")
		(property "Reference" "U"
			(at -29.21 68.58 0)
		)
		(property "Value" "MSP430F5359IZQW"
			(at -22.86 67.31 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 27.94 67.31 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5359.pdf"
			(at 0 0 0)
		)
		(property "Description" "512kB Flash, 66kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5501IRGZ"
		(extends "MSP430F5500IRGZ")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "MSP430F5501IRGZ"
			(at 19.05 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5501.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "16kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5502IRGZ"
		(extends "MSP430F5500IRGZ")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "MSP430F5502IRGZ"
			(at 19.05 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5502.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "24kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5503IRGZ"
		(extends "MSP430F5500IRGZ")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "MSP430F5503IRGZ"
			(at 19.05 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5503.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "32kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5505IRGZ"
		(extends "MSP430F5504IRGZ")
		(property "Reference" "U"
			(at -21.59 29.21 0)
		)
		(property "Value" "MSP430F5505IRGZ"
			(at 20.32 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -20.32 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5505.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "16kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5506IRGZ"
		(extends "MSP430F5504IRGZ")
		(property "Reference" "U"
			(at -21.59 29.21 0)
		)
		(property "Value" "MSP430F5506IRGZ"
			(at 20.32 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -20.32 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5506.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "24kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5507IRGZ"
		(extends "MSP430F5504IRGZ")
		(property "Reference" "U"
			(at -21.59 29.21 0)
		)
		(property "Value" "MSP430F5507IRGZ"
			(at 20.32 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -20.32 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5507.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "32kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5509IRGZ"
		(extends "MSP430F5508IRGZ")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "MSP430F5509IRGZ"
			(at 19.05 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5509.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "24kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5510IRGZ"
		(extends "MSP430F5508IRGZ")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "MSP430F5510IRGZ"
			(at 19.05 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGZ0048A_VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at -21.59 -29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5510.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "32kB Flash, 4kB + 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGZ0048A*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5526IYFF"
		(extends "MSP430F5524IYFF")
		(property "Reference" "U"
			(at -25.4 43.18 0)
		)
		(property "Value" "MSP430F5526IYFF"
			(at 16.51 -43.18 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-64_3.415x3.535mm_Layout8x8_P0.4mm"
			(at -24.13 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5526.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "96kB Flash, 6kB + 2kB RAM, BGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.415x3.535mm*Layout8x8*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5528IYFF"
		(extends "MSP430F5524IYFF")
		(property "Reference" "U"
			(at -25.4 43.18 0)
		)
		(property "Value" "MSP430F5528IYFF"
			(at 16.51 -43.18 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-64_3.415x3.535mm_Layout8x8_P0.4mm"
			(at -24.13 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5528.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "128kB Flash, 8kB + 2kB RAM, BGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.415x3.535mm*Layout8x8*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5631IZQW"
		(extends "MSP430F5630IZQW")
		(property "Reference" "U"
			(at -29.21 66.04 0)
		)
		(property "Value" "MSP430F5631IZQW"
			(at -29.21 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5631.pdf"
			(at 0 0 0)
		)
		(property "Description" "192kB Flash, 16kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5632IZQW"
		(extends "MSP430F5630IZQW")
		(property "Reference" "U"
			(at -29.21 66.04 0)
		)
		(property "Value" "MSP430F5632IZQW"
			(at -29.21 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5632.pdf"
			(at 0 0 0)
		)
		(property "Description" "256kB Flash, 16kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5634IZQW"
		(extends "MSP430F5633IZQW")
		(property "Reference" "U"
			(at -29.21 66.04 0)
		)
		(property "Value" "MSP430F5634IZQW"
			(at -29.21 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5634.pdf"
			(at 0 0 0)
		)
		(property "Description" "192kB Flash, 16kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5635IZQW"
		(extends "MSP430F5633IZQW")
		(property "Reference" "U"
			(at -29.21 66.04 0)
		)
		(property "Value" "MSP430F5635IZQW"
			(at -29.21 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 26.67 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5635.pdf"
			(at 0 0 0)
		)
		(property "Description" "256kB Flash, 16kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5637IZQW"
		(extends "MSP430F5636IZQW")
		(property "Reference" "U"
			(at -29.21 66.04 0)
		)
		(property "Value" "MSP430F5637IZQW"
			(at -29.21 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 25.4 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5637.pdf"
			(at 0 0 0)
		)
		(property "Description" "192kB Flash, 16kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5638IZQW"
		(extends "MSP430F5636IZQW")
		(property "Reference" "U"
			(at -29.21 66.04 0)
		)
		(property "Value" "MSP430F5638IZQW"
			(at -29.21 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 25.4 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5638.pdf"
			(at 0 0 0)
		)
		(property "Description" "256kB Flash, 16kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430F5659IZQW"
		(extends "MSP430F5658IZQW")
		(property "Reference" "U"
			(at -30.48 66.04 0)
		)
		(property "Value" "MSP430F5659IZQW"
			(at -30.48 64.77 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-113_7x7mm_Layout12x12_P0.5mm"
			(at 27.94 64.77 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430f5659.pdf"
			(at 0 0 0)
		)
		(property "Description" "512kB Flash, 64kB + 2kB RAM, BGA-113"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroStar*Junior*BGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430FR5724IRGE"
		(extends "MSP430FR5720IRGE")
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5724IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5724.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430FR5726IRGE"
		(extends "MSP430FR5722IRGE")
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5726IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5726.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "16kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430FR5728IRGE"
		(extends "MSP430FR5720IRGE")
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5728IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5728.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430FR5730IRGE"
		(extends "MSP430FR5720IRGE")
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5730IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5730.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430FR5732IRGE"
		(extends "MSP430FR5722IRGE")
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5732IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5732.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "8kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430FR5734IRGE"
		(extends "MSP430FR5720IRGE")
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5734IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5734.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430FR5736IRGE"
		(extends "MSP430FR5722IRGE")
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5736IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5736.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "16kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430FR5738IRGE"
		(extends "MSP430FR5720IRGE")
		(property "Reference" "U"
			(at -33.02 19.05 0)
		)
		(property "Value" "MSP430FR5738IRGE"
			(at 26.67 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430fr5738.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB FRAM, 1kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2101IN14"
		(extends "MSP430G2001IN14")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2101IN14"
			(at 10.16 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at -15.24 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2101.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2101IPW14"
		(extends "MSP430G2001IPW14")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2101IPW14"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2101.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2101IRSA16"
		(extends "MSP430G2001IRSA16")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2101IRSA16"
			(at 11.43 -15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -16.51 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2101.pdf"
			(at 0 0 0)
		)
		(property "Description" "1kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2201IN14"
		(extends "MSP430G2001IN14")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2201IN14"
			(at 10.16 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at -15.24 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2201.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2201IPW14"
		(extends "MSP430G2001IPW14")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2201IPW14"
			(at 11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2201.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2201IRSA16"
		(extends "MSP430G2001IRSA16")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2201IRSA16"
			(at 11.43 -15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -16.51 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2201.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2202IN20"
		(extends "MSP430G2102IN20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2202IN20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -17.78 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2202.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2202IPW14"
		(extends "MSP430G2102IPW14")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2202IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2202.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2202IPW20"
		(extends "MSP430G2102IPW20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2202IPW20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2202.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2202IRSA16"
		(extends "MSP430G2102IRSA16")
		(property "Reference" "U"
			(at -20.32 17.78 0)
		)
		(property "Value" "MSP430G2202IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2202.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2211IN14"
		(extends "MSP430G2111IN14")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2211IN14"
			(at 12.7 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2211.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2211IPW14"
		(extends "MSP430G2111IPW14")
		(property "Reference" "U"
			(at -15.24 15.24 0)
		)
		(property "Value" "MSP430G2211IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -13.97 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2211.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2211IRSA16"
		(extends "MSP430G2111IRSA16")
		(property "Reference" "U"
			(at -21.59 17.78 0)
		)
		(property "Value" "MSP430G2211IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -20.32 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2211.pdf"
			(at -22.86 13.97 0)
		)
		(property "Description" "2kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2212IN20"
		(extends "MSP430G2112IN20")
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2212IN20"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -29.21 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2212.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2212IPW14"
		(extends "MSP430G2112IPW14")
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2212IPW14"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -27.94 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2212.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2212IPW20"
		(extends "MSP430G2112IPW20")
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2212IPW20"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -27.94 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2212.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2212IRSA16"
		(extends "MSP430G2112IRSA16")
		(property "Reference" "U"
			(at -33.02 15.24 0)
		)
		(property "Value" "MSP430G2212IRSA16"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2212.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2213IPW20"
		(extends "MSP430G2113IPW20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2213IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2213.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2221IN14"
		(extends "MSP430G2121IN14")
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2221IN14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2221.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2221IPW14"
		(extends "MSP430G2121IPW14")
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2221IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -17.78 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2221.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2221IRSA16"
		(extends "MSP430G2121IRSA16")
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2221IRSA16"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -17.78 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2221.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2231IN14"
		(extends "MSP430G2131IN14")
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2231IN14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2231.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2231IPW14"
		(extends "MSP430G2131IPW14")
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2231IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -17.78 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2231.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2231IRSA16"
		(extends "MSP430G2131IRSA16")
		(property "Reference" "U"
			(at -19.05 17.78 0)
		)
		(property "Value" "MSP430G2231IRSA16"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -17.78 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2231.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 128B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2232IN20"
		(extends "MSP430G2132IN20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2232IN20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2232.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2232IPW14"
		(extends "MSP430G2132IPW14")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2232IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2232.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2232IPW20"
		(extends "MSP430G2132IPW20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2232IPW20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2232.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2232IRSA16"
		(extends "MSP430G2132IRSA16")
		(property "Reference" "U"
			(at -20.32 17.78 0)
		)
		(property "Value" "MSP430G2232IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2232.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2252IN20"
		(extends "MSP430G2152IN20")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2252IN20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -33.02 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2252.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2252IPW14"
		(extends "MSP430G2152IPW14")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2252IPW14"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2252.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2252IPW20"
		(extends "MSP430G2152IPW20")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2252IPW20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2252.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2252IRSA16"
		(extends "MSP430G2152IRSA16")
		(property "Reference" "U"
			(at -35.56 17.78 0)
		)
		(property "Value" "MSP430G2252IRSA16"
			(at 29.21 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -34.29 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2252.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2253IN20"
		(extends "MSP430G2153IN20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2253IN20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2253.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2253IPW20"
		(extends "MSP430G2153IPW20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2253IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2253.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2253IPW28"
		(extends "MSP430G2153IPW28")
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2253IPW28"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2253.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2253IRHB32"
		(extends "MSP430G2153IRHB32")
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2253IRHB32"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2253.pdf"
			(at 0 0 0)
		)
		(property "Description" "2kB Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2302IN20"
		(extends "MSP430G2102IN20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2302IN20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -17.78 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2302.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2302IPW14"
		(extends "MSP430G2102IPW14")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2302IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2302.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2302IPW20"
		(extends "MSP430G2102IPW20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2302IPW20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2302.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2302IRSA16"
		(extends "MSP430G2102IRSA16")
		(property "Reference" "U"
			(at -20.32 17.78 0)
		)
		(property "Value" "MSP430G2302IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2302.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2303IN20"
		(extends "MSP430G2203IN20")
		(property "Reference" "U"
			(at -27.94 17.78 0)
		)
		(property "Value" "MSP430G2303IN20"
			(at 21.59 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -27.94 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2303.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2303IPW20"
		(extends "MSP430G2203IPW20")
		(property "Reference" "U"
			(at -27.94 17.78 0)
		)
		(property "Value" "MSP430G2303IPW20"
			(at 21.59 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -26.67 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2303.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2303IPW28"
		(extends "MSP430G2203IPW28")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2303IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2303.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2303IRHB32"
		(extends "MSP430G2203IRHB32")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2303IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2303.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2312IN20"
		(extends "MSP430G2112IN20")
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2312IN20"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -29.21 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2312.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2312IPW14"
		(extends "MSP430G2112IPW14")
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2312IPW14"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -27.94 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2312.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2312IPW20"
		(extends "MSP430G2112IPW20")
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2312IPW20"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -27.94 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2312.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2312IRSA16"
		(extends "MSP430G2112IRSA16")
		(property "Reference" "U"
			(at -33.02 15.24 0)
		)
		(property "Value" "MSP430G2312IRSA16"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2312.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2313IN20"
		(extends "MSP430G2213IN20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2313IN20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -38.1 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2313.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2313IPW20"
		(extends "MSP430G2113IPW20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2313IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2313.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2313IPW28"
		(extends "MSP430G2213IPW28")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2313IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2313.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2313IRHB32"
		(extends "MSP430G2213IRHB32")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2313IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2313.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2332IN20"
		(extends "MSP430G2132IN20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2332IN20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2332.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2332IPW14"
		(extends "MSP430G2132IPW14")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2332IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2332.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2332IPW20"
		(extends "MSP430G2132IPW20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2332IPW20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2332.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2332IRSA16"
		(extends "MSP430G2132IRSA16")
		(property "Reference" "U"
			(at -20.32 17.78 0)
		)
		(property "Value" "MSP430G2332IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2332.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2333IN20"
		(extends "MSP430G2233IN20")
		(property "Reference" "U"
			(at -30.48 17.78 0)
		)
		(property "Value" "MSP430G2333IN20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -30.48 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2333.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "4kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2333IPW20"
		(extends "MSP430G2233IPW20")
		(property "Reference" "U"
			(at -30.48 17.78 0)
		)
		(property "Value" "MSP430G2333IPW20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -30.48 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2333.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2333IPW28"
		(extends "MSP430G2233IPW28")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2333IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2333.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2333IRHB32"
		(extends "MSP430G2233IRHB32")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2333IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2333.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2352IN20"
		(extends "MSP430G2152IN20")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2352IN20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -33.02 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2352.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2352IPW14"
		(extends "MSP430G2152IPW14")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2352IPW14"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2352.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2352IPW20"
		(extends "MSP430G2152IPW20")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2352IPW20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2352.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2352IRSA16"
		(extends "MSP430G2152IRSA16")
		(property "Reference" "U"
			(at -35.56 17.78 0)
		)
		(property "Value" "MSP430G2352IRSA16"
			(at 29.21 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -34.29 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2352.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2353IN20"
		(extends "MSP430G2153IN20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2353IN20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2353.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2353IPW20"
		(extends "MSP430G2153IPW20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2353IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2353.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2353IPW28"
		(extends "MSP430G2153IPW28")
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2353IPW28"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2353.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2353IRHB32"
		(extends "MSP430G2153IRHB32")
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2353IRHB32"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2353.pdf"
			(at 0 0 0)
		)
		(property "Description" "4kB Flash, 256B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2402IN20"
		(extends "MSP430G2102IN20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2402IN20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -17.78 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2402.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2402IPW14"
		(extends "MSP430G2102IPW14")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2402IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2402.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2402IPW20"
		(extends "MSP430G2102IPW20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2402IPW20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2402.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2402IRSA16"
		(extends "MSP430G2102IRSA16")
		(property "Reference" "U"
			(at -20.32 17.78 0)
		)
		(property "Value" "MSP430G2402IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2402.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2403IN20"
		(extends "MSP430G2203IN20")
		(property "Reference" "U"
			(at -27.94 17.78 0)
		)
		(property "Value" "MSP430G2403IN20"
			(at 21.59 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -27.94 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2403.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2403IPW20"
		(extends "MSP430G2203IPW20")
		(property "Reference" "U"
			(at -27.94 17.78 0)
		)
		(property "Value" "MSP430G2403IPW20"
			(at 21.59 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -26.67 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2403.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2403IPW28"
		(extends "MSP430G2203IPW28")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2403IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2403.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2403IRHB32"
		(extends "MSP430G2203IRHB32")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2403IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2403.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2412IN20"
		(extends "MSP430G2112IN20")
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2412IN20"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -29.21 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2412.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2412IPW14"
		(extends "MSP430G2112IPW14")
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2412IPW14"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -27.94 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2412.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2412IPW20"
		(extends "MSP430G2112IPW20")
		(property "Reference" "U"
			(at -29.21 17.78 0)
		)
		(property "Value" "MSP430G2412IPW20"
			(at 22.86 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -27.94 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2412.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2412IRSA16"
		(extends "MSP430G2112IRSA16")
		(property "Reference" "U"
			(at -33.02 15.24 0)
		)
		(property "Value" "MSP430G2412IRSA16"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2412.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2413IN20"
		(extends "MSP430G2213IN20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2413IN20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -38.1 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2413.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2413IPW20"
		(extends "MSP430G2113IPW20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2413IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2413.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2413IPW28"
		(extends "MSP430G2213IPW28")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2413IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2413.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2413IRHB32"
		(extends "MSP430G2213IRHB32")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2413IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2413.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2432IN20"
		(extends "MSP430G2132IN20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2432IN20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2432.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2432IPW14"
		(extends "MSP430G2132IPW14")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2432IPW14"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2432.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2432IPW20"
		(extends "MSP430G2132IPW20")
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "MSP430G2432IPW20"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2432.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2432IRSA16"
		(extends "MSP430G2132IRSA16")
		(property "Reference" "U"
			(at -20.32 17.78 0)
		)
		(property "Value" "MSP430G2432IRSA16"
			(at 15.24 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -19.05 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2432.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2433IN20"
		(extends "MSP430G2233IN20")
		(property "Reference" "U"
			(at -30.48 17.78 0)
		)
		(property "Value" "MSP430G2433IN20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -30.48 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2433.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "8kB Flash, 512B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2433IPW20"
		(extends "MSP430G2233IPW20")
		(property "Reference" "U"
			(at -30.48 17.78 0)
		)
		(property "Value" "MSP430G2433IPW20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -30.48 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2433.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2433IPW28"
		(extends "MSP430G2233IPW28")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2433IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2433.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2433IRHB32"
		(extends "MSP430G2233IRHB32")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2433IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2433.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2452IN20"
		(extends "MSP430G2152IN20")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2452IN20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -33.02 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2452.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2452IPW14"
		(extends "MSP430G2152IPW14")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2452IPW14"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2452.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2452IPW20"
		(extends "MSP430G2152IPW20")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "MSP430G2452IPW20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -31.75 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2452.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2452IRSA16"
		(extends "MSP430G2152IRSA16")
		(property "Reference" "U"
			(at -35.56 17.78 0)
		)
		(property "Value" "MSP430G2452IRSA16"
			(at 29.21 -16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at -34.29 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2452.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 256B RAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2453IN20"
		(extends "MSP430G2153IN20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2453IN20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2453.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2453IPW20"
		(extends "MSP430G2153IPW20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2453IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2453.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2453IPW28"
		(extends "MSP430G2153IPW28")
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2453IPW28"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2453.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2453IRHB32"
		(extends "MSP430G2153IRHB32")
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2453IRHB32"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2453.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kB Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2513IN20"
		(extends "MSP430G2213IN20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2513IN20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -38.1 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2513.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2513IPW20"
		(extends "MSP430G2113IPW20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2513IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2513.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2513IPW28"
		(extends "MSP430G2213IPW28")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2513IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2513.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2513IRHB32"
		(extends "MSP430G2213IRHB32")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2513IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2513.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2533IN20"
		(extends "MSP430G2233IN20")
		(property "Reference" "U"
			(at -30.48 17.78 0)
		)
		(property "Value" "MSP430G2533IN20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -30.48 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2533.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "16kB Flash, 512B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2533IPW20"
		(extends "MSP430G2233IPW20")
		(property "Reference" "U"
			(at -30.48 17.78 0)
		)
		(property "Value" "MSP430G2533IPW20"
			(at 26.67 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -30.48 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2533.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "16kB Flash, 512B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2533IPW28"
		(extends "MSP430G2233IPW28")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2533IPW28"
			(at 21.59 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2533.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2533IRHB32"
		(extends "MSP430G2233IRHB32")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2533IRHB32"
			(at 20.32 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2533.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2544IDA38"
		(extends "MSP430G2444IDA38")
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2544IDA38"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2544.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB + 256B Flash, 512B RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2544IRHA40"
		(extends "MSP430G2444IRHA40")
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2544IRHA40"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2544.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB + 256B Flash, 512B RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2544IYFF"
		(extends "MSP430G2444IYFF")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2544IYFF"
			(at 22.86 -25.4 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2544.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB + 256B Flash, 512B RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2553IN20"
		(extends "MSP430G2153IN20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2553IN20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2553.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2553IPW20"
		(extends "MSP430G2153IPW20")
		(property "Reference" "U"
			(at -38.1 17.78 0)
		)
		(property "Value" "MSP430G2553IPW20"
			(at 31.75 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -36.83 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2553.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2553IPW28"
		(extends "MSP430G2153IPW28")
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2553IPW28"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2553.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2553IRHB32"
		(extends "MSP430G2153IRHB32")
		(property "Reference" "U"
			(at -30.48 25.4 0)
		)
		(property "Value" "MSP430G2553IRHB32"
			(at 24.13 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHB0032E_VQFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -29.21 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2553.pdf"
			(at 0 0 0)
		)
		(property "Description" "16kB Flash, 512B RAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2744IDA38"
		(extends "MSP430G2444IDA38")
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2744IDA38"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2744.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB + 256B Flash, 1kB RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2744IRHA40"
		(extends "MSP430G2444IRHA40")
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2744IRHA40"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2744.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB + 256B Flash, 1kB RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2744IYFF"
		(extends "MSP430G2444IYFF")
		(property "Reference" "U"
			(at -27.94 25.4 0)
		)
		(property "Value" "MSP430G2744IYFF"
			(at 22.86 -25.4 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-49_3.33x3.488mm_Layout7x7_P0.4mm"
			(at -26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2744.pdf"
			(at 0 0 0)
		)
		(property "Description" "32kB + 256B Flash, 1kB RAM, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*3.33x3.488mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2855IDA38"
		(extends "MSP430G2755IDA38")
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2855IDA38"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2855.pdf"
			(at 0 0 0)
		)
		(property "Description" "48kB Flash, 4kB RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2855IRHA40"
		(extends "MSP430G2755IRHA40")
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2855IRHA40"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2855.pdf"
			(at 0 0 0)
		)
		(property "Description" "48kB Flash, 4kB RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2955IDA38"
		(extends "MSP430G2755IDA38")
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2955IDA38"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_6.1x12.5mm_P0.65mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2955.pdf"
			(at 0 0 0)
		)
		(property "Description" "56kB Flash, 4kB RAM, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MSP430G2955IRHA40"
		(extends "MSP430G2755IRHA40")
		(property "Reference" "U"
			(at -24.13 25.4 0)
		)
		(property "Value" "MSP430G2955IRHA40"
			(at 17.78 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/msp430g2955.pdf"
			(at 0 0 0)
		)
		(property "Description" "56kB Flash, 4kB RAM, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI MSP430 16-bit mixed signal microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
)
