(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CC1312R1F3RGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 -36.83 0)
		)
		(property "Value" "CC1312R1F3RGZ"
			(at 10.16 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 0 -48.26 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cc1312r.pdf"
			(at 17.78 -15.24 0)
		)
		(property "Description" "ARM Cortex-M4 SimpleLink High-Performance Sub-1GHz Wireless MCU, 48MHz, 352KB Flash, 80KB SRAM, 8KB Cache SRAM, 1.8-3.6V, 30 GPIO, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CC1312R1F3RGZ_0_1")
		(symbol "CC1312R1F3RGZ_1_1"
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "DIO_16/JTAG_TDO")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "DIO_17/JTAG_TDI")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "JTAG_TMSC")
				(number "24")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "JTAG_TCKC")
				(number "25")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "DIO_1")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "DIO_2")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "DIO_3")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "DIO_4")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "DIO_5")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "DIO_6")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "DIO_7")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "DIO_8")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "DIO_9")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "DIO_10")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "DIO_11")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "DIO_12")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "DIO_13")
				(number "19")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "X48M_N")
				(number "46")
			)
			(pin input line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "X48M_P")
				(number "47")
			)
			(pin power_in line
				(at -15.24 38.1 270)
				(length 2.54)
				(name "VDDS")
				(number "44")
			)
			(pin power_in line
				(at -12.7 38.1 270)
				(length 2.54)
				(name "VDDS2")
				(number "13")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 2.54)
				(name "VDDS3")
				(number "22")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VDDS_DCDC")
				(number "34")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDDR")
				(number "45")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDR_RF")
				(number "48")
			)
			(pin power_out line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "DCDC_SW")
				(number "33")
			)
			(pin power_out line
				(at 15.24 38.1 270)
				(length 2.54)
				(name "DCOUPL")
				(number "23")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RF_P")
				(number "1")
			)
			(pin passive line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RF_N")
				(number "2")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RX_TX")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "DIO_14")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "DIO_15")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "DIO_18")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "DIO_19")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "DIO_20")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "DIO_21")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "DIO_22")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "DIO_23")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "DIO_24")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "DIO_25")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "DIO_26")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "DIO_27")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "DIO_28")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "DIO_29")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "DIO_30")
				(number "43")
			)
			(pin input line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "X32K_Q1")
				(number "4")
			)
			(pin input line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "X32K_Q2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
)
