(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CH32V203CxTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "CH32V203CxTx"
			(at 6.858 38.862 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -1.27 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH32V203.html"
			(at 1.27 3.81 0)
		)
		(property "Description" "The CH32V203 is an industrial-grade enhanced low-power general-purpose MCU based on 32-bit RISC-V core."
			(at 0 0 0)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CH32V203CxTx_0_0"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD_VIO")
				(number "24")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
		)
		(symbol "CH32V203CxTx_0_1")
		(symbol "CH32V203CxTx_1_0"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "~{RST}")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "OSC_IN")
				(number "5")
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "6")
				(alternate "PD1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "TAMPER-RTC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "OPA1_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "OPA1_OUT1" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "BOOT1" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "SPI1_MOSI_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "USART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN1_RX_2" bidirectional line)
				(alternate "I2C1_SCL_1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN1_TX_2" bidirectional line)
				(alternate "I2C1_SDA_1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "OPA2_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART4_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART4_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
				(alternate "USBDM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
				(alternate "USBDP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "SWDIO")
				(number "34")
				(alternate "PA13" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "SWCLK")
				(number "37")
				(alternate "PA14" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "TIM2_CH13" bidirectional line)
				(alternate "TIM2_CH1_1" bidirectional line)
				(alternate "TIM2_ETR_1" bidirectional line)
				(alternate "TIM2_ETR_3" bidirectional line)
				(alternate "USART4_RTS_1" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V203F6P6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "CH32V203F6P6"
			(at 2.54 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 3.81 0)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V203.html"
			(at 0 -6.35 0)
		)
		(property "Description" "The CH32V203 is an industrial-grade enhanced low-power general-purpose MCU based on 32-bit RISC-V core."
			(at 0 0 0)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CH32V203F6P6_0_1")
		(symbol "CH32V203F6P6_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
				(alternate "CAN1_RX_2" bidirectional line)
				(alternate "I2C1_SCL_1" bidirectional line)
				(alternate "PB8" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "OSC_IN")
				(number "2")
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "3")
				(alternate "PD1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" input line)
				(alternate "OPA1_OUT1" output line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" output line)
				(alternate "TIM3_CH4_2" bidirectional line)
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "TIM2_CH1" passive line)
				(alternate "TIM2_CH1_2" bidirectional line)
				(alternate "TIM2_ETR" passive line)
				(alternate "TIM2_ETR_2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" input line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" passive line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" input line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "USART2_TX" output line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" input line)
				(alternate "OPA1_OUT0" output line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "USART2_RX" input line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" input line)
				(alternate "OPA2_OUT1" output line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" input line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" input line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" input line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" output line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" input line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" input line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "17")
				(alternate "CAN1_RX" input line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
				(alternate "USBDM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "18")
				(alternate "CAN1_TX" output line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
				(alternate "USBDP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SWDIO")
				(number "19")
				(alternate "PA13" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SWCLK")
				(number "20")
				(alternate "PA14" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V203GxUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 24.384 0)
		)
		(property "Value" "CH32V203GxUx"
			(at 15.748 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.7x2.7mm"
			(at -33.02 -21.59 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/CH32V203DS0_PDF.html"
			(at 0 37.084 0)
		)
		(property "Description" "NanjingQinheng WCH RISC-V MCU, 32-64KB flash, 10-20KB RAM, 144 MHz, 2.4-3.6V, 24 GPIO, ADC, OpAmp, CAN, USB, QFN-28"
			(at -0.508 39.37 0)
		)
		(property "ki_keywords" "RISCV WCH MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "CH32V203GxUx_1_1"
			(pin input line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PA0")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PA1")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PA2")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PA3")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PA4")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PA5")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PA6")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PA7")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PA9")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PA10/PA11/USB_D-")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PA12/USB_D+")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PA13/SWDIO")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PA14/SWCLK")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PA15")
				(number "23")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PB3")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PB4")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PB5")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PB6")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PB7")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "BOOT0/PB8")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "OSC_IN/PD0")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "OSC_OUT/PD1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
)
