(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CH32V30xCxTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 38.1 0)
		)
		(property "Value" "CH32V30xCxTx"
			(at 5.08 38.1 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 2.54 0)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CH32V30xCxTx_0_0"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
		)
		(symbol "CH32V30xCxTx_1_0"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "~{RST}")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "OPA4_OUT0" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TIM8_ETR_1" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "OPA3_OUT0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIM9_CH1_ETR_1" bidirectional line)
				(alternate "TIM9_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIM9_CH2_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM9_CH3" bidirectional line)
				(alternate "TIM9_CH3_1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH2N_1" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_TX_3" bidirectional line)
				(alternate "USART7_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM10_CH3N_1" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART7_RX_1" bidirectional line)
				(alternate "USART1_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "OTG_FS_VBUS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "USART1_RTS_2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "OTG_FS_ID" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_CK_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "OTG_FS_DM" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "OTG_FS_DP" bidirectional line)
				(alternate "TIM10_CH1N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1_ETR_1" bidirectional line)
				(alternate "TIM2_CH1_ETR_3" bidirectional line)
				(alternate "TIM8_CH3N_1" bidirectional line)
				(alternate "UART8_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "TAMPER-RTC" bidirectional line)
				(alternate "TIM8_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "OSC32_IN" bidirectional line)
				(alternate "TIM9_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "OSC32_OUT" bidirectional line)
				(alternate "TIM10_CH4_1" bidirectional line)
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "36")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "SWDIO")
				(number "34")
				(alternate "PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "SWCLK")
				(number "37")
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "UART8_TX_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "OPA1_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TIM9_CH1N_1" bidirectional line)
				(alternate "UART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "OPA4_CH0N" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TIM9_CH2N_1" bidirectional line)
				(alternate "UART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "BOOT1" bidirectional line)
				(alternate "OPA3_CH0N" bidirectional line)
				(alternate "TIM9_CH3N_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_CH1_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH2_1" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "UART5_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_CH3_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "UART5_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH3_1" bidirectional line)
				(alternate "UART6_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM10_CH2" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_BKIN_1" bidirectional line)
				(alternate "UART6_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "OPA4_CH0P" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPA3_CH0P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "OSC_IN")
				(number "5")
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "OSC_OUT")
				(number "6")
				(alternate "PD1" bidirectional line)
			)
		)
		(symbol "CH32V30xCxTx_1_1")
		(embedded_fonts no)
	)
	(symbol "CH32V30xFxPx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 20.32 0)
		)
		(property "Value" "CH32V30xFxPx"
			(at 2.54 20.32 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 -5.08 0)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CH32V30xFxPx_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PA1/PA5")
				(number "2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "9")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1_3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "10")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2_3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC8")
				(number "11")
				(alternate "TIM3_CH3_3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PA8/PC9")
				(number "12")
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SWDIO")
				(number "13")
				(alternate "PA9/PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART1_RTS_2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SWCLK")
				(number "15")
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
				(alternate "USART8_TX_1" bidirectional line)
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD33")
				(number "14")
				(alternate "VIO" power_in line)
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PB6")
				(number "16")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PB7")
				(number "17")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PB10")
				(number "3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PB11")
				(number "4")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PB12")
				(number "5")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PB13")
				(number "6")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PB14")
				(number "7")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB15")
				(number "8")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OSC_IN")
				(number "19")
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OSC_OUT")
				(number "20")
				(alternate "PD1" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V30xRxTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 55.88 0)
		)
		(property "Value" "CH32V30xRxTx"
			(at 7.62 55.88 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 5.08 0)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CH32V30xRxTx_0_0"
			(pin power_in line
				(at -2.54 55.88 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 2.54)
				(name "VIO")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
		)
		(symbol "CH32V30xRxTx_1_0"
			(pin input line
				(at -15.24 45.72 0)
				(length 2.54)
				(name "~{RST}")
				(number "7")
			)
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "ETH_MII_CRS_WKUP" bidirectional line)
				(alternate "ETH_RGMII_RXD2" bidirectional line)
				(alternate "OPA4_OUT0" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TIM8_ETR_1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "ETH_MII_RX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD3" bidirectional line)
				(alternate "ETH_RMII_REF_CLK" bidirectional line)
				(alternate "OPA3_OUT0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "ETH_MII_MDIO" bidirectional line)
				(alternate "ETH_RGMII_GTXC" bidirectional line)
				(alternate "ETH_RMII_MDIO" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIM9_CH1_ETR_1" bidirectional line)
				(alternate "TIM9_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "ETH_MII_COL" bidirectional line)
				(alternate "ETH_RGMII_TXEN" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIM9_CH2_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM9_CH3" bidirectional line)
				(alternate "TIM9_CH3_1" bidirectional line)
				(alternate "USART2_CX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MIS" bidirectional line)
				(alternate "TIM10_CH2N_1" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART7_TX_1" bidirectional line)
				(alternate "USART1_TX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RGMII_TXD0" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM10_CH3N_1" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART7_RX_1" bidirectional line)
				(alternate "USART1_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "OTG_FS_VBUS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "USART1_RTS_2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "OTG_FS_ID" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_CK_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "OTG_FS_DM" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "OTG_FS_DP" bidirectional line)
				(alternate "TIM10_CH1N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SWDIO")
				(number "46")
				(alternate "PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SWCLK")
				(number "49")
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "UART8_TX_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1_ETR_1" bidirectional line)
				(alternate "TIM2_CH1_ETR_3" bidirectional line)
				(alternate "TIM8_CH3N_1" bidirectional line)
				(alternate "UART8_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "ETH_MII_RXD2" bidirectional line)
				(alternate "ETH_RGMII_TXD3" bidirectional line)
				(alternate "OPA1_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TIM9_CH1N_1" bidirectional line)
				(alternate "UART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "ETH_MII_RXD3" bidirectional line)
				(alternate "ETH_RGMII_125IN" bidirectional line)
				(alternate "OPA4_CH0N" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TIM9_CH2N_1" bidirectional line)
				(alternate "UART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "BOOT1" bidirectional line)
				(alternate "OPA3_CH0N" bidirectional line)
				(alternate "TIM9_CH3N_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_CH1_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH2_1" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "UART5_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_PPS_OUT" bidirectional line)
				(alternate "ETH_RMII_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_CH3_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "UART5_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DVP_D6" bidirectional line)
				(alternate "ETH_MII_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH3_1" bidirectional line)
				(alternate "UART6_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM10_CH2" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_BKIN_1" bidirectional line)
				(alternate "UART6_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "ETH_MII_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ETH_MII_TX_EN" bidirectional line)
				(alternate "ETH_RMII_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_TXD0" bidirectional line)
				(alternate "ETH_RMII_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPA4_CH0P" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_MII_TXD1" bidirectional line)
				(alternate "ETH_RMII_TXD1" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPA3_CH0P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -45.72 0)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -48.26 0)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin passive line
				(at 0 55.88 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 2.54 55.88 270)
				(length 2.54)
				(hide yes)
				(name "VIO")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "ETH_RGMII_RXC" bidirectional line)
				(alternate "TIM9_CH1N" bidirectional line)
				(alternate "UART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "ETH_MII_MDC" bidirectional line)
				(alternate "ETH_RGMII_RXCTL" bidirectional line)
				(alternate "ETH_RMII_MDC" bidirectional line)
				(alternate "TIM9_CH2N" bidirectional line)
				(alternate "UART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "ETH_MII_TXD2" bidirectional line)
				(alternate "ETH_RGMII_RXD0" bidirectional line)
				(alternate "OPA3_CH1N" bidirectional line)
				(alternate "TIM9_CH3N" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "ETH_MII_TX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD1" bidirectional line)
				(alternate "OPA4_CH1N" bidirectional line)
				(alternate "TIM10_CH3" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RGMII_TXD1" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "OPA4_CH1P" bidirectional line)
				(alternate "TIM9_CH4" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART1_CTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "ETH_MII_RXD1" bidirectional line)
				(alternate "ETH_RGMII_TXD2" bidirectional line)
				(alternate "ETH_RMII_RXD1" bidirectional line)
				(alternate "OPA3_CH1P" bidirectional line)
				(alternate "TIM9_BKIN" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
				(alternate "USART1_RTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "ETH_RXP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1_3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "ETH_RXN" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2_3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "ETH_TXP" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3_3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "ETH_TXN" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2C3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_BKIN" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "TAMPER-RTC" bidirectional line)
				(alternate "TIM8_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "OSC32_IN" bidirectional line)
				(alternate "TIM9_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "OSC32_OUT" bidirectional line)
				(alternate "TIM10_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OSC_IN")
				(number "5")
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "OSC_OUT")
				(number "6")
				(alternate "PD1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM3_ETR_2" bidirectional line)
				(alternate "TIM3_ETR_3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
		)
		(symbol "CH32V30xRxTx_1_1")
		(embedded_fonts no)
	)
	(symbol "CH32V30xVxTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 71.12 0)
		)
		(property "Value" "CH32V30xVxTx"
			(at 5.08 71.12 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 5.08 0)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CH32V30xVxTx_0_0"
			(pin bidirectional line
				(at -17.78 53.34 0)
				(length 2.54)
				(name "OSC_IN")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 48.26 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "13")
			)
			(pin input line
				(at -17.78 -55.88 0)
				(length 2.54)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -17.78 -63.5 0)
				(length 2.54)
				(name "VREF-")
				(number "20")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 2.54)
				(name "VSS")
				(number "10")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 2.54)
				(name "VIO")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 2.54)
				(name "VDDA")
				(number "22")
			)
		)
		(symbol "CH32V30xVxTx_1_0"
			(pin input line
				(at -17.78 63.5 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin input line
				(at -17.78 60.96 0)
				(length 2.54)
				(name "BOOT0")
				(number "94")
			)
			(pin no_connect line
				(at -17.78 58.42 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "ETH_MII_CRS_WKUP" bidirectional line)
				(alternate "ETH_RGMII_RXD2" bidirectional line)
				(alternate "OPA4_OUT0" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TIM8_ETR_1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "ETH_MII_RX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD3" bidirectional line)
				(alternate "ETH_RMII_REF_CLK" bidirectional line)
				(alternate "OPA3_OUT0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "ETH_MII_MDIO" bidirectional line)
				(alternate "ETH_RGMII_GTXC" bidirectional line)
				(alternate "ETH_RMII_MDIO" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIM9_CH1_ETR_1" bidirectional line)
				(alternate "TIM9_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA3")
				(number "26")
				(alternate "ETH_MII_COL" bidirectional line)
				(alternate "ETH_RGMII_TXEN" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIM9_CH2_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DVP_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM9_CH3" bidirectional line)
				(alternate "TIM9_CH3_1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "DVP_VSYNC" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "DVP_PCLK" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH2N_1" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART7_TX_1" bidirectional line)
				(alternate "USART1_TX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RGMII_TXD0" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM10_CH3N_1" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART7_RX_1" bidirectional line)
				(alternate "USART1_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA8")
				(number "67")
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA9")
				(number "68")
				(alternate "DVP_D0" bidirectional line)
				(alternate "OTG_FS_VBUS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "USART1_RTS_2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "69")
				(alternate "DVP_D1" bidirectional line)
				(alternate "OTG_FS_ID" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_CK_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "70")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "OTG_FS_DM" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA12")
				(number "71")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "OTG_FS_DP" bidirectional line)
				(alternate "TIM10_CH1N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA15")
				(number "77")
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1_ETR_1" bidirectional line)
				(alternate "TIM2_CH1_ETR_3" bidirectional line)
				(alternate "TIM8_CH3N_1" bidirectional line)
				(alternate "UART8_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SWDIO")
				(number "72")
				(alternate "PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "SWCLK")
				(number "76")
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "UART8_TX_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "ETH_MII_RXD2" bidirectional line)
				(alternate "ETH_RGMII_TXD3" bidirectional line)
				(alternate "OPA_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TIM9_CH1N_1" bidirectional line)
				(alternate "UART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "ETH_MII_RXD3" bidirectional line)
				(alternate "ETH_RGMII_125IN" bidirectional line)
				(alternate "OPA4_CH0N" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TIM9_CH2N_1" bidirectional line)
				(alternate "UART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB2")
				(number "37")
				(alternate "BOOT1" bidirectional line)
				(alternate "OPA3_CH0N" bidirectional line)
				(alternate "TIM9_CH3N_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB3")
				(number "89")
				(alternate "DVP_D5" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_CH1_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH2_1" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "UART5_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB5")
				(number "91")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_PPS_OUT" bidirectional line)
				(alternate "ETH_RMII_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_CH3_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "UART5_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB6")
				(number "92")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DVP_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB7")
				(number "93")
				(alternate "FSMC_NADV" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB8")
				(number "95")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DVP_D6" bidirectional line)
				(alternate "ETH_MII_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH3_1" bidirectional line)
				(alternate "UART6_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB9")
				(number "96")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DVP_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM10_CH2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM8_BKIN_1" bidirectional line)
				(alternate "UART6_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB10")
				(number "47")
				(alternate "ETH_MII_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB11")
				(number "48")
				(alternate "ETH_MII_TX_EN" bidirectional line)
				(alternate "ETH_RMII_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB12")
				(number "51")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_TXD0" bidirectional line)
				(alternate "ETH_RMII_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPA4_CH0P" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB13")
				(number "52")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_MII_TXD1" bidirectional line)
				(alternate "ETH_RMII_TXD1" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPA3_CH0P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PB14")
				(number "53")
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin passive line
				(at -2.54 71.12 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "28")
			)
			(pin passive line
				(at -2.54 71.12 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "75")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VIO")
				(number "100")
			)
			(pin bidirectional line
				(at 17.78 63.5 180)
				(length 2.54)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "ETH_RGMII_RXC" bidirectional line)
				(alternate "TIM9_CH1N" bidirectional line)
				(alternate "UART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 60.96 180)
				(length 2.54)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "ETH_MII_MDC" bidirectional line)
				(alternate "ETH_RGMII_RXCTL" bidirectional line)
				(alternate "ETH_RMII_MDC" bidirectional line)
				(alternate "TIM9_CH2N" bidirectional line)
				(alternate "UART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 58.42 180)
				(length 2.54)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "ETH_MII_TXD2" bidirectional line)
				(alternate "ETH_RGMII_RXD0" bidirectional line)
				(alternate "OPA3_CH1N" bidirectional line)
				(alternate "TIM9_CH3N" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 55.88 180)
				(length 2.54)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "ETH_MII_TX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD1" bidirectional line)
				(alternate "OPA4_CH1N" bidirectional line)
				(alternate "TIM10_CH3" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 53.34 180)
				(length 2.54)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RGMII_TXD1" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "OPA4_CH1P" bidirectional line)
				(alternate "TIM9_CH4" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART1_CTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "ETH_MII_RXD1" bidirectional line)
				(alternate "ETH_RGMII_TXD2" bidirectional line)
				(alternate "ETH_RMII_RXD1" bidirectional line)
				(alternate "OPA3_CH1P" bidirectional line)
				(alternate "TIM9_BKIN" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
				(alternate "USART1_RTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PC6")
				(number "63")
				(alternate "ETH_RXP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1_3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PC7")
				(number "64")
				(alternate "ETH_RXN" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2_3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PC8")
				(number "65")
				(alternate "DVP_D2" bidirectional line)
				(alternate "ETH_TXP" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3_3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PC9")
				(number "66")
				(alternate "DVP_D3" bidirectional line)
				(alternate "ETH_TXN" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PC10")
				(number "78")
				(alternate "DVP_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PC11")
				(number "79")
				(alternate "DVP_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PC12")
				(number "80")
				(alternate "DVP_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_BKIN" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PC13")
				(number "7")
				(alternate "TAMPER-RTC" bidirectional line)
				(alternate "TIM8_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PC14")
				(number "8")
				(alternate "OSC32_IN" bidirectional line)
				(alternate "TIM9_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PC15")
				(number "9")
				(alternate "OSC32_OUT" bidirectional line)
				(alternate "TIM10_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PD0")
				(number "81")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "TIM10_ETR_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PD1")
				(number "82")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "TIM10_CH1_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PD2")
				(number "83")
				(alternate "DVP_D11" bidirectional line)
				(alternate "FSMC_NADV" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM3_ETR_2" bidirectional line)
				(alternate "TIM3_ETR_3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "TIM10_CH2_2" bidirectional line)
				(alternate "USART2_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIM10_CH3_2" bidirectional line)
				(alternate "USART2_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PD6")
				(number "87")
				(alternate "DVP_D10" bidirectional line)
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM10_CH4_2" bidirectional line)
				(alternate "USART2_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PD8")
				(number "55")
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "FSMC_D13" bidirectional line)
				(alternate "TIM9_CH1N_2" bidirectional line)
				(alternate "USART3_TX_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PD9")
				(number "56")
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "TIM9_CH1_ETR_2" bidirectional line)
				(alternate "USART3_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PD10")
				(number "57")
				(alternate "ETH_MII_RXD1" bidirectional line)
				(alternate "ETH_RMII_RXD1" bidirectional line)
				(alternate "FSMC_D15" bidirectional line)
				(alternate "TIM9-CH2N_2" bidirectional line)
				(alternate "USART3_CK_2" bidirectional line)
				(alternate "USART3_CK_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PD11")
				(number "58")
				(alternate "ETH_MII_RXD2" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "TIM9_CH2_2" bidirectional line)
				(alternate "USART3_CTS_2" bidirectional line)
				(alternate "USART3_CTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PD12")
				(number "59")
				(alternate "ETH_MII_RXD3" bidirectional line)
				(alternate "FSMC_A17" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "TIM9_CH3N_2" bidirectional line)
				(alternate "USART3_RTS_2" bidirectional line)
				(alternate "USART3_RTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2_1" bidirectional line)
				(alternate "TIM9_CH3_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "TIM4_CH3_1" bidirectional line)
				(alternate "TIM9_BKIN_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PD15")
				(number "62")
				(alternate "FSMC_D1" bidirectional line)
				(alternate "TIM4_CH4_1" bidirectional line)
				(alternate "TIM9_CH4_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM4_ETR_1" bidirectional line)
				(alternate "UART4_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "UART4_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "TIM10_BKIN_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "TIM10_CH1N_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "TIM10_CH2N_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "TIM10_CH3N_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "OPA3_OUT1" bidirectional line)
				(alternate "TIM1_ETR_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -45.72 180)
				(length 2.54)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "OPA4_OUT1" bidirectional line)
				(alternate "TIM1_CH1N_3" bidirectional line)
				(alternate "UART5_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -48.26 180)
				(length 2.54)
				(name "PE9")
				(number "40")
				(alternate "FSMC_D6" bidirectional line)
				(alternate "TIM1_CH1_3" bidirectional line)
				(alternate "UART5_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -50.8 180)
				(length 2.54)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "TIM1_CH2N_3" bidirectional line)
				(alternate "UART6_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -53.34 180)
				(length 2.54)
				(name "PE11")
				(number "42")
				(alternate "FSMC_D8" bidirectional line)
				(alternate "TIM1_CH2_3" bidirectional line)
				(alternate "UART6_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -55.88 180)
				(length 2.54)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "TIM1_CH3N_3" bidirectional line)
				(alternate "UART7_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -58.42 180)
				(length 2.54)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "TIM1_CH3_3" bidirectional line)
				(alternate "UART7_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -60.96 180)
				(length 2.54)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "OPA2_OUT1" bidirectional line)
				(alternate "TIM1_CH4_3" bidirectional line)
				(alternate "UART8_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -63.5 180)
				(length 2.54)
				(name "PE15")
				(number "46")
				(alternate "FSMC_D12" bidirectional line)
				(alternate "OPA1_OUT1" bidirectional line)
				(alternate "TXM1_BKIN_3" bidirectional line)
				(alternate "UART8_RX_2" bidirectional line)
			)
		)
		(symbol "CH32V30xVxTx_1_1")
		(embedded_fonts no)
	)
	(symbol "CH32V30xWxUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 50.8 0)
		)
		(property "Value" "CH32V30xWxUx"
			(at 5.08 50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 -5.08 0)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "CH32V30xWxUx_0_0"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "BOOT0")
				(number "63")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VIO")
				(number "17")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
		)
		(symbol "CH32V30xWxUx_1_0"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "~{RST}")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "ETH_MII_CRS_WKUP" bidirectional line)
				(alternate "ETH_RGMII_RXD2" bidirectional line)
				(alternate "OPA4_OUT0" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TIM8_ETR_1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "ETH_MII_RX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD3" bidirectional line)
				(alternate "ETH_RMII_REF_CLK" bidirectional line)
				(alternate "OPA3_OUT0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "ETH_MII_MDIO" bidirectional line)
				(alternate "ETH_RGMII_GXTC" bidirectional line)
				(alternate "ETH_RMII_MDIO" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIM9_CH1_ETR_1" bidirectional line)
				(alternate "TIM9_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PA3")
				(number "19")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "ETH_MII_COL" bidirectional line)
				(alternate "ETH_RGMII_TXEN" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIM9_CH2_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM9_CH3" bidirectional line)
				(alternate "TIM9_CH3_1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH2N_1" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_TX_3" bidirectional line)
				(alternate "USART7_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RGMII_TXD0" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM10_CH3N_1" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART1_RX_3" bidirectional line)
				(alternate "USART7_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA8")
				(number "43")
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA9")
				(number "44")
				(alternate "ETH_TXN" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA10")
				(number "45")
				(alternate "OTG_FS_ID" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_CK_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PA11")
				(number "46")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "OTG_FS_DM" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PA12")
				(number "47")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "OTG_FS_DP" bidirectional line)
				(alternate "TIM10_CH1N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PA15")
				(number "53")
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1_ETR_1" bidirectional line)
				(alternate "TIM2_CH1_ETR_3" bidirectional line)
				(alternate "TIM8_CH3N_1" bidirectional line)
				(alternate "UART8_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "ETH_MII_RXD2" bidirectional line)
				(alternate "ETH_RGMII_TXD3" bidirectional line)
				(alternate "OPA1_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TIM9_CH1N_1" bidirectional line)
				(alternate "UART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "ETH_MII_RXD3" bidirectional line)
				(alternate "ETH_RGMII_125IN" bidirectional line)
				(alternate "OPA4_CH0N" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TIM9_CH2N_1" bidirectional line)
				(alternate "UART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "BOOT1" bidirectional line)
				(alternate "OPA3_CH0N" bidirectional line)
				(alternate "TIM9_CH3N_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB3")
				(number "58")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_CH1_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB4")
				(number "59")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH2_1" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "UART5_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB5")
				(number "60")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_PPS_OUT" bidirectional line)
				(alternate "ETH_RMII_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_CH3_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "UART5_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB6")
				(number "61")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB7")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB8")
				(number "64")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "ETH_MII_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH3_1" bidirectional line)
				(alternate "UART6_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB9")
				(number "65")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM10_CH2" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_BKIN_1" bidirectional line)
				(alternate "UART6_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "ETH_MII_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ETH_MII_TX_EN" bidirectional line)
				(alternate "ETH_RMII_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB12")
				(number "35")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_TXD0" bidirectional line)
				(alternate "ETH_RMII_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPA4_CH0P" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PB13")
				(number "36")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_MII_TXD1" bidirectional line)
				(alternate "ETH_RMII_TXD1" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPA3_CH0P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PB14")
				(number "37")
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PB15")
				(number "38")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin passive line
				(at -2.54 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "50")
			)
			(pin passive line
				(at -2.54 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "68")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VIO")
				(number "31")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VIO")
				(number "51")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VIO")
				(number "67")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "69")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "OSC_IN")
				(number "5")
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "OSC_OUT")
				(number "6")
				(alternate "PD1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "SWDIO")
				(number "48")
				(alternate "PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "SWCLK")
				(number "52")
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "UART8_TX_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "ETH_RGMII_RXC" bidirectional line)
				(alternate "TIM9_CH1N" bidirectional line)
				(alternate "UART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "ETH_MII_MDC" bidirectional line)
				(alternate "ETH_RGMII_RXCTL" bidirectional line)
				(alternate "ETH_RMII_MDC" bidirectional line)
				(alternate "TIM9_CH2N" bidirectional line)
				(alternate "UART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "ETH_MII_TXD2" bidirectional line)
				(alternate "ETH_RGMII_RXD0" bidirectional line)
				(alternate "OPA3_CH1N" bidirectional line)
				(alternate "TIM9_CH3N" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "ETH_MII_TX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD1" bidirectional line)
				(alternate "OPA4_CH1N" bidirectional line)
				(alternate "TIM10_CH3" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RGMII_TXD1" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "OPA4_CH1P" bidirectional line)
				(alternate "TIM9_CH4" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART1_CTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "ETH_MII_RXD1" bidirectional line)
				(alternate "ETH_RGMII_TXD2" bidirectional line)
				(alternate "ETH_RMII_RDX1" bidirectional line)
				(alternate "OPA3_CH1P" bidirectional line)
				(alternate "TIM9_BKIN" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
				(alternate "USART1_RTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC6")
				(number "39")
				(alternate "ETH_RXP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1_3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC7")
				(number "40")
				(alternate "ETH_RXN" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2_3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC8")
				(number "41")
				(alternate "ETH_TXP" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3_3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC9")
				(number "42")
				(alternate "ETH_TXN" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC10")
				(number "54")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC11")
				(number "55")
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC12")
				(number "56")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_BKIN" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "TAMPER-RTC" bidirectional line)
				(alternate "TIM8_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "OSC32_IN" bidirectional line)
				(alternate "TIM9_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "OSC32_OUT" bidirectional line)
				(alternate "TIM10_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD2")
				(number "57")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM3_ETR_2" bidirectional line)
				(alternate "TIM3_ETR_3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD8")
				(number "33")
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "TIM9_CH1N_2" bidirectional line)
				(alternate "USART3_TX_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD9")
				(number "34")
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "TIM9_CH1_ETR_2" bidirectional line)
				(alternate "USART3_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PE0")
				(number "66")
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM4_ETR_1" bidirectional line)
			)
		)
		(symbol "CH32V30xWxUx_1_1")
		(embedded_fonts no)
	)
)
