(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CH32X035G8U6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.732 29.718 0)
		)
		(property "Value" "CH32X035G8U6"
			(at 8.636 29.718 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.7x2.7mm"
			(at -0.254 3.556 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/CH32X035DS0_PDF.html"
			(at 0 3.81 0)
		)
		(property "Description" "48MHz RISC-V MCU with USB PD phy (Sink, Source, DRP), USB 2.0 Full speed phy (Host, Device), 20KB RAM, 62KB Flash, QFN-28"
			(at 1.016 3.556 0)
		)
		(property "ki_keywords" "microcontroller WCH Type-C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*28*1EP*4x4mm*P0.4mm*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "CH32X035G8U6_0_0"
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PA0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PA1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA2")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA3")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA5")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA6")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA7")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "23")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PC0")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PC3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PC10/PC17/UDP")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PC11/PC16/UDM")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC14/CC1")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC15/CC2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC18/DIO")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC19/DCK")
				(number "24")
			)
		)
		(symbol "CH32X035G8U6_1_0"
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1/PB5")
				(number "16")
			)
		)
		(symbol "CH32X035G8U6_1_1")
		(embedded_fonts no)
	)
)
