(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "24AA02-OT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "24AA02-OT"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21709J.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 2Kb, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "24AA02-OT_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "WP")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "24AA025E-OT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24AA025E-OT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MPD/ProductDocuments/DataSheets/2-Kbit-I2C-Serial-EEPROMs-+EUI-48-or-EUI-64-Node-20002124.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM with EUI-48 or EUI-64, 2Kb, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "24AA025E-OT_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "24AA025E-SN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24AA025E-SN"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MPD/ProductDocuments/DataSheets/2-Kbit-I2C-Serial-EEPROMs-+EUI-48-or-EUI-64-Node-20002124.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM with EUI-48 or EUI-64, 2Kb, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "24AA025E-SN_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "24AA02E-OT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "24AA02E-OT"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MPD/ProductDocuments/DataSheets/2-Kbit-I2C-Serial-EEPROMs-+EUI-48-or-EUI-64-Node-20002124.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM with EUI-48 or EUI-64, 2Kb, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "24AA02E-OT_1_1"
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "24AA02E-SN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "24AA02E-SN"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MPD/ProductDocuments/DataSheets/2-Kbit-I2C-Serial-EEPROMs-+EUI-48-or-EUI-64-Node-20002124.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM with EUI-48 or EUI-64, 2Kb, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "24AA02E-SN_1_1"
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "24LC16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC16"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21703d.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 16Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "24LC16_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "25CSM04xxSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U3"
			(at 1.9559 8.89 0)
		)
		(property "Value" "25CSM04xxSN"
			(at 1.9559 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MPD/ProductDocuments/DataSheets/25CSM04-4-Mbit-SPI-Serial-EEPROM-With-128-Bit-Serial-Number-and-Enhanced-Write-Protection-20005817C.pdf"
			(at 2.54 -20.32 0)
		)
		(property "Description" "4Mbit SPI Serial EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "25CSM04xxSN_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SI")
				(number "5")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "25LCxxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "25LCxxx"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21832H.pdf"
			(at 0 0 0)
		)
		(property "Description" "SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "25LCxxx_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "MOSI")
				(number "5")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "MISO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "25LCxxx-MC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "25LCxxx-MC"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21832H.pdf"
			(at 0 0 0)
		)
		(property "Description" "SPI Serial EEPROM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "25LCxxx-MC_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "MOSI")
				(number "5")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "MISO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "28C256"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "28C256"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc0006.pdf"
			(at 0 0 0)
		)
		(property "Description" "Paged Parallel EEPROM 256Kb (32K x 8), DIP-28/SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Parallel EEPROM 256Kb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "28C256_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A13")
				(number "26")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A14")
				(number "1")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "~{WE}")
				(number "27")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "~{CS}")
				(number "20")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "D0")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D1")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D2")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D3")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D4")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D5")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D6")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "93AAxxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93AAxxA"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 1.8V, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "93AAxxA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "93AAxxAT-xOT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93AAxxAT-xOT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 8-bit word, 1.8V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "93AAxxAT-xOT_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "93AAxxC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93AAxxC"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, with ORG Pin, 1.8V, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "93AAxxC_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ORG")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "93CxxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93CxxA"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 5.0V, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "93CxxA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "93CxxC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93CxxC"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, with ORG Pin, 5.0V, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "93CxxC_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ORG")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "93LCxxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93LCxxA"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 2.5V, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "93LCxxA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "93LCxxAxxOT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "93LCxxAxxOT"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 2.5V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "93LCxxAxxOT_0_1")
		(symbol "93LCxxAxxOT_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "93LCxxC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93LCxxC"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, with ORG Pin, 2.5V, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "93LCxxC_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ORG")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS01-MAHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS01-MAHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 1Kb (128x8) with Unique Serial Number, UDFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS01-MAHM_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS01-SSHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS01-SSHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 1Kb (128x8) with Unique Serial Number, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS01-SSHM_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS01-STUM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS01-STUM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 1Kb (128x8) with Unique Serial Number, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AT24CS01-STUM_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS01-XHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS01-XHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 1Kb (128x8) with Unique Serial Number, TSSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS01-XHM_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS04-MAHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS04-MAHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8766-SEEPROM-AT24CS04-08-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 4Kb (512x8) with Unique Serial Number, UDFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS04-MAHM_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS04-SSHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS04-SSHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8766-SEEPROM-AT24CS04-08-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 4Kb (512x8) with Unique Serial Number, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS04-SSHM_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS04-XHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS04-XHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8766-SEEPROM-AT24CS04-08-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 4Kb (512x8) with Unique Serial Number, TSSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS04-XHM_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS08-MAHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS08-MAHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8766-SEEPROM-AT24CS04-08-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 8Kb (1024x8) with Unique Serial Number, UDFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS08-MAHM_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS08-SSHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS08-SSHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8766-SEEPROM-AT24CS04-08-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 8Kb (1024x8) with Unique Serial Number, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS08-SSHM_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS08-XHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS08-XHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8766-SEEPROM-AT24CS04-08-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 8Kb (1024x8) with Unique Serial Number, TSSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS08-XHM_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS16-MAHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS16-MAHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8859-SEEPROM-AT24CS16-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 16Kb (2048x8) with Unique Serial Number, UDFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS16-MAHM_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS16-SSHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS16-SSHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8859-SEEPROM-AT24CS16-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 16Kb (2048x8) with Unique Serial Number, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS16-SSHM_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS16-XHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS16-XHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8859-SEEPROM-AT24CS16-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 16Kb (2048x8) with Unique Serial Number, TSSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS16-XHM_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS32-SSHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS32-SSHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8869-SEEPROM-AT24CS32-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 32Kb (4096x8) with Unique Serial Number, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS32-SSHM_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS32-XHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS32-XHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8869-SEEPROM-AT24CS32-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 32Kb (4096x8) with Unique Serial Number, TSSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS32-XHM_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS64-SSHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS64-SSHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8870-SEEPROM-AT24CS64-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 64Kb (8192x8) with Unique Serial Number, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS64-SSHM_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT24CS64-XHM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS64-XHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8870-SEEPROM-AT24CS64-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 64Kb (8192x8) with Unique Serial Number, TSSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AT24CS64-XHM_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAT24M01L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "CAT24M01L"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/CAT24M01-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1 Mb I2C CMOS Serial EEPROM, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM 1Mb I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "CAT24M01L_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAT24M01W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "CAT24M01W"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/CAT24M01-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1 Mb I2C CMOS Serial EEPROM, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM 1Mb I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CAT24M01W_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAT24M01X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "CAT24M01X"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 21.59 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/CAT24M01-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1 Mb I2C CMOS Serial EEPROM, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM 1Mb I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CAT24M01X_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAT24M01Y"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "CAT24M01Y"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 21.59 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/CAT24M01-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1 Mb I2C CMOS Serial EEPROM, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM 1Mb I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CAT24M01Y_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS2431"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DS2431"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DS2431.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "1024-bit, 1-Wire® EEPROM chip, TO-92"
			(at 0 15.24 0)
		)
		(property "ki_keywords" "1kb EEPROM memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "DS2431_1_1"
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "IO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS2431P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DS2431P"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO_J-Lead:TSOC-6_3.76x3.94mm_P1.27mm"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DS2431.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "1024-bit, 1-Wire® EEPROM chip, TSOC-6"
			(at 0 15.24 0)
		)
		(property "ki_keywords" "1kb EEPROM memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOC*"
			(at 0 0 0)
		)
		(symbol "DS2431P_1_1"
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "IO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS2431Q"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DS2431Q"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:Maxim_TDFN-6-1EP_3x3mm_P0.95mm_EP1.5x2.3mm"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DS2431.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "1024-bit, 1-Wire® EEPROM chip, TDFN"
			(at 0 15.24 0)
		)
		(property "ki_keywords" "1kb EEPROM memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maxim*TDFN?6*1EP*3x3mm*P0.95mm*EP1.5x2.3mm*"
			(at 0 0 0)
		)
		(symbol "DS2431Q_1_1"
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "IO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KM28C64A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "KM28C64A"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://tvsat.com.pl/PDF/K/km28c64_sam.pdf"
			(at 0 0 0)
		)
		(property "Description" "EEPROM 8K x 8, 5V, Not  in Production, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "samsung"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "KM28C64A_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "~{WE}")
				(number "27")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "~{CE}")
				(number "20")
			)
			(pin no_connect line
				(at -7.62 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "I/O0")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "I/O1")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "I/O2")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "I/O3")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "I/O4")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "I/O5")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "I/O6")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "I/O7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KM28C65A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "KM28C65A"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://tvsat.com.pl/PDF/K/km28c64_sam.pdf"
			(at 0 0 0)
		)
		(property "Description" "EEPROM 8K x 8, 5V, Not  in Production, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "samsung"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "KM28C65A_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin output line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "RDY/~{BSY}")
				(number "1")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "~{WE}")
				(number "27")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "~{CE}")
				(number "20")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "I/O0")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "I/O1")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "I/O2")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "I/O3")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "I/O4")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "I/O5")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "I/O6")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "I/O7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M24C02-WDW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C02-WDW"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "2Kb (256x8) I2C Serial EEPROM, 2.5-5.5V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "M24C02-WDW_0_1")
		(symbol "M24C02-WDW_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "E0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "E1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "E2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{WC}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M24C02-WMN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C02-WMN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "2Kb (256x8) I2C Serial EEPROM, 2.5-5.5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "M24C02-WMN_0_1")
		(symbol "M24C02-WMN_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "E0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "E1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "E2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{WC}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M95256-WMN6P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "M95256-WMN6P"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/9d/75/f0/3e/76/00/4c/0b/CD00103810.pdf/files/CD00103810.pdf/jcr:content/translations/en.CD00103810.pdf"
			(at 0 0 0)
		)
		(property "Description" "SPI EEPROM, 256Kb (32K x 8), No Identification Page, 2.5 to 5.5V, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "M95256-WMN6P_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{W}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{S}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Q")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M95512-Axxx-MF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "M95512-Axxx-MF"
			(at 6.35 -7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:WFDFPN-8-1EP_3x2mm_P0.5mm_EP1.25x1.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/m95512-a125.pdf"
			(at 0 0 0)
		)
		(property "Description" "Automotive 512-Kbit serial SPI bus EEPROMs with high-speed clock, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DF?N*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "M95512-Axxx-MF_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{W}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{S}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Q")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMS4C1050N"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 11.43 0)
		)
		(property "Value" "TMS4C1050N"
			(at 7.62 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.datasheets360.com/pdf/3640170882560205603"
			(at 0 0 0)
		)
		(property "Description" "Field Memory, 262264 x 4 bit, [Obsolete 1992-01]"
			(at 0 0 0)
		)
		(property "ki_keywords" "Field Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*"
			(at 0 0 0)
		)
		(symbol "TMS4C1050N_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "WE")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RSTW")
				(number "2")
			)
			(pin input clock
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SWCLK")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D0")
				(number "4")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "D1")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "D2")
				(number "6")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "D3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RE/OE")
				(number "15")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RSTR")
				(number "14")
			)
			(pin input clock
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SRCLK")
				(number "13")
			)
			(pin tri_state line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "Q0")
				(number "12")
			)
			(pin tri_state line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "Q1")
				(number "11")
			)
			(pin tri_state line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "Q2")
				(number "10")
			)
			(pin tri_state line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "Q3")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "24LC00"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC00"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21178G.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 128 Bits, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC01"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC01"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21711J.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 1Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC02"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC02"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21709c.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 2Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC04"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC04"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21708K.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 4Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC08"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC08"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21710J.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 8Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC1025"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC1025"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21941B.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 1024Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC128"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC128"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21191s.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 128Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC256"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC256"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21203m.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 256Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC32"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC32"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21072G.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 32Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC512"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC512"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21754M.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 512Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "24LC64"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "24LC64"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21189f.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 64Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "25CSM04xxMF"
		(extends "25CSM04xxSN")
		(property "Reference" "U3"
			(at 1.9559 8.89 0)
		)
		(property "Value" "25CSM04xxMF"
			(at 1.9559 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_6x5mm_P1.27mm_EP3.4x4mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MPD/ProductDocuments/DataSheets/25CSM04-4-Mbit-SPI-Serial-EEPROM-With-128-Bit-Serial-Number-and-Enhanced-Write-Protection-20005817C.pdf"
			(at 2.54 -20.32 0)
		)
		(property "Description" "4Mbit SPI Serial EEPROM, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*6x5mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "25LCxxx-MF"
		(extends "25LCxxx-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "25LCxxx-MF"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WFDFPN-8-1EP_3x2mm_P0.5mm_EP1.25x1.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/25LC512-512-Kbit-SPI-Bus-Serial-EEPROM-20002065D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SPI Serial EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WFDFPN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "93AAxxB"
		(extends "93AAxxA")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93AAxxB"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 1.8V, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "93AAxxBT-xOT"
		(extends "93AAxxAT-xOT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93AAxxBT-xOT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 16-bit word, 1.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "93CxxB"
		(extends "93CxxA")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93CxxB"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 5.0V, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "93LCxxB"
		(extends "93LCxxA")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "93LCxxB"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 2.5V, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory Microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "93LCxxBxxOT"
		(extends "93LCxxAxxOT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "93LCxxBxxOT"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial EEPROM, 93 Series, 2.5V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1K Microwire Serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS02-MAHM"
		(extends "AT24CS01-MAHM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS02-MAHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 2Kb (256x8) with Unique Serial Number, UDFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS02-SSHM"
		(extends "AT24CS01-SSHM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS02-SSHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 2Kb (256x8) with Unique Serial Number, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS02-STUM"
		(extends "AT24CS01-STUM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS02-STUM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 2Kb (256x8) with Unique Serial Number, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS02-XHM"
		(extends "AT24CS01-XHM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS02-XHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 2Kb (256x8) with Unique Serial Number, TSSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS04-STUM"
		(extends "AT24CS01-STUM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS04-STUM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8766-SEEPROM-AT24CS04-08-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 4Kb (512x8) with Unique Serial Number, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS08-STUM"
		(extends "AT24CS01-STUM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS08-STUM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8766-SEEPROM-AT24CS04-08-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 8Kb (1024x8) with Unique Serial Number, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS16-STUM"
		(extends "AT24CS01-STUM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS16-STUM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8859-SEEPROM-AT24CS16-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 16Kb (2048x8) with Unique Serial Number, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS32-MAHM"
		(extends "AT24CS01-MAHM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS32-MAHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8869-SEEPROM-AT24CS32-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 32Kb (4096x8) with Unique Serial Number, UDFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS32-STUM"
		(extends "AT24CS01-STUM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS32-STUM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8869-SEEPROM-AT24CS32-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 32Kb (4096x8) with Unique Serial Number, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AT24CS64-MAHM"
		(extends "AT24CS01-MAHM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT24CS64-MAHM"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8870-SEEPROM-AT24CS64-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Serial EEPROM, 64Kb (8192x8) with Unique Serial Number, UDFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT25xxx"
		(extends "25LCxxx")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT25xxx"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8707-SEEPROM-AT25010B-020B-040B-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microchip SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT25xxx-MA"
		(extends "25LCxxx-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AT25xxx-MA"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8707-SEEPROM-AT25010B-020B-040B-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microchip SPI Serial EEPROM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "BR25Sxxx"
		(extends "25LCxxx")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "BR25Sxxx"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.rohm.com/web/global/products/-/product/BR25G128F-3"
			(at 0 0 0)
		)
		(property "Description" "ROHM Semiconductor SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "BR25xxx-NUX"
		(extends "25LCxxx-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "BR25xxx-NUX"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.rohm.com/web/global/products/-/product/BR25G128F-3"
			(at 0 0 0)
		)
		(property "Description" "ROHM Semiconductor SPI Serial EEPROM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAT24C128"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "CAT24C128"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/CAT24C128-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "128 kb CMOS Serial EEPROM, SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C EEPROM Serial 128kb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAT24C256"
		(extends "24LC16")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "CAT24C256"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/CAT24C256-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "256 kb CMOS Serial EEPROM, DIP-8/SOIC-8/TSSOP-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C EEPROM Serial 256kb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAT250xxx"
		(extends "25LCxxx")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CAT250xxx"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/PowerSolutions/product.do?id=CAT25040"
			(at 0 0 0)
		)
		(property "Description" "ON Semiconductor SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAT250xxx-HU4"
		(extends "25LCxxx-MC")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CAT250xxx-HU4"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/PowerSolutions/product.do?id=CAT25040"
			(at 0 0 0)
		)
		(property "Description" "ON Semiconductor SPI Serial EEPROM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM memory SPI serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS28E07"
		(extends "DS2431")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DS28E07"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DS28E07.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "1024-bit, 1-Wire® EEPROM chip, TO-92"
			(at 0 15.24 0)
		)
		(property "ki_keywords" "1kb EEPROM memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "DS28E07P"
		(extends "DS2431P")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DS28E07P"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO_J-Lead:TSOC-6_3.76x3.94mm_P1.27mm"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DS28E07.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "1024-bit, 1-Wire® EEPROM chip, TSOC-6"
			(at 0 15.24 0)
		)
		(property "ki_keywords" "1kb EEPROM memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOC*"
			(at 0 0 0)
		)
	)
	(symbol "DS28E07Q"
		(extends "DS2431Q")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DS28E07Q"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:Maxim_TDFN-6-1EP_3x3mm_P0.95mm_EP1.5x2.3mm"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DS28E07.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "1024-bit, 1-Wire® EEPROM chip, TDFN"
			(at 0 15.24 0)
		)
		(property "ki_keywords" "1kb EEPROM memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maxim*TDFN?6*1EP*3x3mm*P0.95mm*EP1.5x2.3mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C01-FDW"
		(extends "M24C02-WDW")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C01-FDW"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "1Kb (128x8) I2C Serial EEPROM, 1.6-5.5V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C01-FMN"
		(extends "M24C02-WMN")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C01-FMN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "1Kb (128x8) I2C Serial EEPROM, 1.6-5.5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C01-RDW"
		(extends "M24C02-WDW")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C01-RDW"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "1Kb (128x8) I2C Serial EEPROM, 1.8-5.5V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C01-RMN"
		(extends "M24C02-WMN")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C01-RMN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "1Kb (128x8) I2C Serial EEPROM, 1.8-5.5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C01-WDW"
		(extends "M24C02-WDW")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C01-WDW"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "1Kb (128x8) I2C Serial EEPROM, 2.5-5.5V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C01-WMN"
		(extends "M24C02-WMN")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C01-WMN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "1Kb (128x8) I2C Serial EEPROM, 2.5-5.5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C02-FDW"
		(extends "M24C02-WDW")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C02-FDW"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "2Kb (256x8) I2C Serial EEPROM, 1.6-5.5V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C02-FMN"
		(extends "M24C02-WMN")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C02-FMN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "2Kb (256x8) I2C Serial EEPROM, 1.6-5.5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C02-RDW"
		(extends "M24C02-WDW")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C02-RDW"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "2Kb (256x8) I2C Serial EEPROM, 1.8-5.5V, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "M24C02-RMN"
		(extends "M24C02-WMN")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "M24C02-RMN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "2Kb (256x8) I2C Serial EEPROM, 1.8-5.5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile Non-Volatile Memory ROM ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
