(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "27C010"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 29.21 0)
		)
		(property "Value" "27C010"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc0321.pdf"
			(at 0 0 0)
		)
		(property "Description" "OTP EPROM 1 MiBit (128 Ki x 8 Bit)"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP EPROM 1MiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PLCC*"
			(at 0 0 0)
		)
		(symbol "27C010_1_1"
			(pin input line
				(at -10.16 25.4 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A14")
				(number "29")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A15")
				(number "3")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "A16")
				(number "2")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{PGM}")
				(number "31")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "VPP")
				(number "1")
			)
			(pin input line
				(at -10.16 -25.4 0)
				(length 2.54)
				(name "~{CE}")
				(number "22")
			)
			(pin input line
				(at -10.16 -27.94 0)
				(length 2.54)
				(name "~{OE}")
				(number "24")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 25.4 180)
				(length 2.54)
				(name "D0")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "D1")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D2")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D3")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D4")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D5")
				(number "19")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D6")
				(number "20")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "27C020"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "27C020"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc0570.pdf"
			(at 0 0 0)
		)
		(property "Description" "OTP EPROM 2 MiBit (256 Ki x 8 Bit)"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP EPROM 2MiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PLCC*"
			(at 0 0 0)
		)
		(symbol "27C020_1_1"
			(pin input line
				(at -10.16 27.94 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -10.16 25.4 0)
				(length 2.54)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A14")
				(number "29")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A15")
				(number "3")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A16")
				(number "2")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "A17")
				(number "30")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{PGM}")
				(number "31")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "VPP")
				(number "1")
			)
			(pin input line
				(at -10.16 -25.4 0)
				(length 2.54)
				(name "~{CE}")
				(number "22")
			)
			(pin input line
				(at -10.16 -27.94 0)
				(length 2.54)
				(name "~{OE}")
				(number "24")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 27.94 180)
				(length 2.54)
				(name "D0")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 25.4 180)
				(length 2.54)
				(name "D1")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "D2")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D3")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D4")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D5")
				(number "19")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D6")
				(number "20")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "27C040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "27C040"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc0189.pdf"
			(at 0 0 0)
		)
		(property "Description" "OTP EPROM 4 MiBit (512 Ki x 8)"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP EPROM 4MiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PLCC*"
			(at 0 0 0)
		)
		(symbol "27C040_1_1"
			(pin input line
				(at -10.16 27.94 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -10.16 25.4 0)
				(length 2.54)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A14")
				(number "29")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A15")
				(number "3")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A16")
				(number "2")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "A17")
				(number "30")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "A18")
				(number "31")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "VPP")
				(number "1")
			)
			(pin input line
				(at -10.16 -25.4 0)
				(length 2.54)
				(name "~{CE}")
				(number "22")
			)
			(pin input line
				(at -10.16 -27.94 0)
				(length 2.54)
				(name "~{OE}")
				(number "24")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 27.94 180)
				(length 2.54)
				(name "D0")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 25.4 180)
				(length 2.54)
				(name "D1")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "D2")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D3")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D4")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D5")
				(number "19")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D6")
				(number "20")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "27C080"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 31.75 0)
		)
		(property "Value" "27C080"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc0360.pdf"
			(at 0 0 0)
		)
		(property "Description" "OTP EPROM 8 MiBit (1 Mi x 8)"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP EPROM 8MiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PLCC*"
			(at 0 0 0)
		)
		(symbol "27C080_1_1"
			(pin input line
				(at -10.16 27.94 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -10.16 25.4 0)
				(length 2.54)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A14")
				(number "29")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A15")
				(number "3")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A16")
				(number "2")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "A17")
				(number "30")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "A18")
				(number "31")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "A19")
				(number "1")
			)
			(pin input line
				(at -10.16 -25.4 0)
				(length 2.54)
				(name "~{CE}")
				(number "22")
			)
			(pin input line
				(at -10.16 -27.94 0)
				(length 2.54)
				(name "~{OE}")
				(number "24")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 27.94 180)
				(length 2.54)
				(name "D0")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 25.4 180)
				(length 2.54)
				(name "D1")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "D2")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D3")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D4")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D5")
				(number "19")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D6")
				(number "20")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "27C128"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "27C128"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/11003L.pdf"
			(at 0 0 0)
		)
		(property "Description" "OTP EPROM 128 KiBit, [Obsolete 2004-01]"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP EPROM 128KiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "27C128_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A13")
				(number "26")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "~{PGM}")
				(number "27")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "VPP")
				(number "1")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{CE}")
				(number "20")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "D0")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D1")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D2")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D3")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D4")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D5")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D6")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "27C256"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "27C256"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc0014.pdf"
			(at 0 0 0)
		)
		(property "Description" "OTP EPROM 256 KiBit"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP EPROM 256 KiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "27C256_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A13")
				(number "26")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A14")
				(number "27")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "VPP")
				(number "1")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{CE}")
				(number "20")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "D0")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D1")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D2")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D3")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D4")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D5")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D6")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "27C512"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "27C512"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc0015.pdf"
			(at 0 0 0)
		)
		(property "Description" "OTP EPROM 512 KiBit"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP EPROM 512KiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "27C512_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A13")
				(number "26")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A14")
				(number "27")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "A15")
				(number "1")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{CE}")
				(number "20")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "D0")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D1")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D2")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D3")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D4")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D5")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D6")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "27C512PLCC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "27C512PLCC"
			(at 2.54 -29.21 0)
		)
		(property "Footprint" "Package_LCC:PLCC-32_11.4x14.0mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc0015.pdf"
			(at 0 0 0)
		)
		(property "Description" "OTP EPROM 512 KiBit PLCC-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP EPROM 512KiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC?32*11.4x14.0mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "27C512PLCC_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "A0")
				(number "11")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A1")
				(number "10")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A2")
				(number "9")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A4")
				(number "7")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A6")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A7")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A8")
				(number "29")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A9")
				(number "28")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "24")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "27")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "3")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A13")
				(number "30")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A14")
				(number "31")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "A15")
				(number "2")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{OE}/VPP")
				(number "25")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "~{CE}")
				(number "23")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin no_connect line
				(at 7.62 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 7.62 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 7.62 -25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin tri_state line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "O0")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "O1")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "O2")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "O3")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "O4")
				(number "19")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "O5")
				(number "20")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "O6")
				(number "21")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "O7")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "27C64"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "27C64"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11107M.pdf"
			(at 0 0 0)
		)
		(property "Description" "OTP EPROM 64 KiBit, [Obsolete 2004-01]"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP EPROM 64KiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "27C64_1_1"
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "~{PGM}")
				(number "27")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "VPP")
				(number "1")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{CE}")
				(number "20")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin tri_state line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "D0")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "D1")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "D2")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "D3")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D4")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D5")
				(number "17")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D6")
				(number "18")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "27128"
		(extends "27C128")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "27128"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://eeshop.unl.edu/pdf/27128.pdf"
			(at 0 0 0)
		)
		(property "Description" "UV Erasable EPROM 128 KiBit, [Obsolete 2000-11]"
			(at 0 0 0)
		)
		(property "ki_keywords" "Erasable OTP EPROM 128KiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "27256"
		(extends "27C256")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "27256"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/D27256-2-Intel-datasheet-17852618.pdf"
			(at 0 0 0)
		)
		(property "Description" "UV Erasable EPROM 256 KiBit, [Obsolete 2000-11]"
			(at 0 0 0)
		)
		(property "ki_keywords" "Erasable EPROM 256 KiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "27512"
		(extends "27C512")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "27512"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/120/227190_DS.pdf"
			(at 0 0 0)
		)
		(property "Description" "UV Erasable EPROM 512 KiBit, [Obsolete 2007-01]"
			(at 0 0 0)
		)
		(property "ki_keywords" "Erasable EPROM 512KiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "2764"
		(extends "27C64")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "2764"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://downloads.reactivemicro.com/Electronics/ROM/2764%20EPROM.pdf"
			(at 0 0 0)
		)
		(property "Description" "EPROM 64 KiBit, [Obsolete 2000-11]"
			(at 0 0 0)
		)
		(property "ki_keywords" "EPROM 64KiBit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
)
