(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "28F400"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 36.195 0)
		)
		(property "Value" "28F400"
			(at -5.08 34.29 0)
		)
		(property "Footprint" "Package_SO:PSOP-44_16.9x27.17mm_P1.27mm"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://download.intel.com/design/archives/flash/docs/29045101.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "PA28F400BX-T/B Flash EEProm 4-MBIT (256Kx16bits, 512Kx8bits) 5V, 12V Prog"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM FLASH 4MO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PSOP*"
			(at 0 0 0)
		)
		(symbol "28F400_0_1")
		(symbol "28F400_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 6.35)
				(name "A0")
				(number "11")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 6.35)
				(name "A1")
				(number "10")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 6.35)
				(name "A2")
				(number "9")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 6.35)
				(name "A3")
				(number "8")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 6.35)
				(name "A4")
				(number "7")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 6.35)
				(name "A5")
				(number "6")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 6.35)
				(name "A6")
				(number "5")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 6.35)
				(name "A7")
				(number "4")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 6.35)
				(name "A8")
				(number "42")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 6.35)
				(name "A9")
				(number "41")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 6.35)
				(name "A10")
				(number "40")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 6.35)
				(name "A11")
				(number "39")
			)
			(pin input line
				(at -15.24 0 0)
				(length 6.35)
				(name "A12")
				(number "38")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 6.35)
				(name "A13")
				(number "37")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 6.35)
				(name "A14")
				(number "36")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 6.35)
				(name "A15")
				(number "35")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 6.35)
				(name "A16")
				(number "34")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 6.35)
				(name "A17")
				(number "3")
			)
			(pin input inverted
				(at -15.24 -20.32 0)
				(length 6.35)
				(name "CE")
				(number "12")
			)
			(pin input inverted
				(at -15.24 -22.86 0)
				(length 6.35)
				(name "OE")
				(number "14")
			)
			(pin input inverted
				(at -15.24 -25.4 0)
				(length 6.35)
				(name "WE")
				(number "43")
			)
			(pin input inverted
				(at -15.24 -27.94 0)
				(length 6.35)
				(name "PR")
				(number "44")
			)
			(pin input inverted
				(at -15.24 -30.48 0)
				(length 6.35)
				(name "BYTE")
				(number "33")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 5.08)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 5.08)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 5.08)
				(name "VPP")
				(number "1")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "GND")
				(number "32")
			)
			(pin no_connect line
				(at 8.89 -30.48 180)
				(length 6.35)
				(hide yes)
				(name "DU")
				(number "2")
			)
			(pin tri_state line
				(at 15.24 30.48 180)
				(length 6.35)
				(name "D0")
				(number "15")
			)
			(pin tri_state line
				(at 15.24 27.94 180)
				(length 6.35)
				(name "D1")
				(number "17")
			)
			(pin tri_state line
				(at 15.24 25.4 180)
				(length 6.35)
				(name "D2")
				(number "19")
			)
			(pin tri_state line
				(at 15.24 22.86 180)
				(length 6.35)
				(name "D3")
				(number "21")
			)
			(pin tri_state line
				(at 15.24 20.32 180)
				(length 6.35)
				(name "D4")
				(number "24")
			)
			(pin tri_state line
				(at 15.24 17.78 180)
				(length 6.35)
				(name "D5")
				(number "26")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 6.35)
				(name "D6")
				(number "28")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 6.35)
				(name "D7")
				(number "30")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 6.35)
				(name "D8")
				(number "16")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 6.35)
				(name "D9")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 6.35)
				(name "D10")
				(number "20")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 6.35)
				(name "D11")
				(number "22")
			)
			(pin tri_state line
				(at 15.24 0 180)
				(length 6.35)
				(name "D12")
				(number "25")
			)
			(pin tri_state line
				(at 15.24 -2.54 180)
				(length 6.35)
				(name "D13")
				(number "27")
			)
			(pin tri_state line
				(at 15.24 -5.08 180)
				(length 6.35)
				(name "D14")
				(number "29")
			)
			(pin tri_state line
				(at 15.24 -7.62 180)
				(length 6.35)
				(name "A-1/D15")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "29F010-TSOP-SP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.858 24.13 0)
		)
		(property "Value" "29F010-TSOP-SP"
			(at 15.24 -24.13 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Flash EEProm 128Ko (TSOP 32 pack.) 5V prog"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM FLASH 128KO"
			(at 0 0 0)
		)
		(symbol "29F010-TSOP-SP_0_1")
		(symbol "29F010-TSOP-SP_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 6.35)
				(name "A0")
				(number "20")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 6.35)
				(name "A1")
				(number "19")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 6.35)
				(name "A2")
				(number "18")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 6.35)
				(name "A3")
				(number "17")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 6.35)
				(name "A4")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 6.35)
				(name "A5")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 6.35)
				(name "A6")
				(number "14")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 6.35)
				(name "A7")
				(number "13")
			)
			(pin input line
				(at -15.24 0 0)
				(length 6.35)
				(name "A8")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 6.35)
				(name "A9")
				(number "2")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 6.35)
				(name "A10")
				(number "31")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 6.35)
				(name "A11")
				(number "1")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 6.35)
				(name "A12")
				(number "12")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 6.35)
				(name "A13")
				(number "4")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 6.35)
				(name "A14")
				(number "5")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 6.35)
				(name "A15")
				(number "11")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 6.35)
				(name "A16")
				(number "10")
			)
			(pin input line
				(at 1.27 30.48 270)
				(length 7.62)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at 1.27 -30.48 90)
				(length 7.62)
				(name "GND")
				(number "24")
			)
			(pin tri_state line
				(at 15.24 20.32 180)
				(length 6.35)
				(name "D0")
				(number "21")
			)
			(pin tri_state line
				(at 15.24 17.78 180)
				(length 6.35)
				(name "D1")
				(number "22")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 6.35)
				(name "D2")
				(number "23")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 6.35)
				(name "D3")
				(number "25")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 6.35)
				(name "D4")
				(number "26")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 6.35)
				(name "D5")
				(number "27")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 6.35)
				(name "D6")
				(number "28")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 6.35)
				(name "D7")
				(number "29")
			)
			(pin input inverted
				(at 15.24 -2.54 180)
				(length 6.35)
				(name "CE")
				(number "30")
			)
			(pin input inverted
				(at 15.24 -5.08 180)
				(length 6.35)
				(name "OE")
				(number "32")
			)
			(pin input inverted
				(at 15.24 -7.62 180)
				(length 6.35)
				(name "WE")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "29W040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.858 24.13 0)
		)
		(property "Value" "29W040"
			(at 7.62 -31.75 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Flash EEProm 512PP (TSOP 32) 3,3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM FLASH 512KO"
			(at 0 0 0)
		)
		(symbol "29W040_0_1")
		(symbol "29W040_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 6.35)
				(name "A0")
				(number "20")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 6.35)
				(name "A1")
				(number "19")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 6.35)
				(name "A2")
				(number "18")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 6.35)
				(name "A3")
				(number "17")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 6.35)
				(name "A4")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 6.35)
				(name "A5")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 6.35)
				(name "A6")
				(number "14")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 6.35)
				(name "A7")
				(number "13")
			)
			(pin input line
				(at -15.24 0 0)
				(length 6.35)
				(name "A8")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 6.35)
				(name "A9")
				(number "2")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 6.35)
				(name "A10")
				(number "31")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 6.35)
				(name "A11")
				(number "1")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 6.35)
				(name "A12")
				(number "12")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 6.35)
				(name "A13")
				(number "4")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 6.35)
				(name "A14")
				(number "5")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 6.35)
				(name "A15")
				(number "11")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 6.35)
				(name "A16")
				(number "10")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 6.35)
				(name "A17")
				(number "6")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 6.35)
				(name "A18")
				(number "9")
			)
			(pin power_in line
				(at 1.27 30.48 270)
				(length 7.62)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 1.27 -36.83 90)
				(length 7.62)
				(name "GND")
				(number "24")
			)
			(pin tri_state line
				(at 15.24 20.32 180)
				(length 6.35)
				(name "D0")
				(number "21")
			)
			(pin tri_state line
				(at 15.24 17.78 180)
				(length 6.35)
				(name "D1")
				(number "22")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 6.35)
				(name "D2")
				(number "23")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 6.35)
				(name "D3")
				(number "25")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 6.35)
				(name "D4")
				(number "26")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 6.35)
				(name "D5")
				(number "27")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 6.35)
				(name "D6")
				(number "28")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 6.35)
				(name "D7")
				(number "29")
			)
			(pin input inverted
				(at 15.24 -2.54 180)
				(length 6.35)
				(name "CE")
				(number "30")
			)
			(pin input inverted
				(at 15.24 -5.08 180)
				(length 6.35)
				(name "OE")
				(number "32")
			)
			(pin input inverted
				(at 15.24 -7.62 180)
				(length 6.35)
				(name "WE")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AM29F400Bx-xxEx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.636 35.306 0)
		)
		(property "Value" "AM29F400Bx-xxEx"
			(at 10.414 35.306 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-48_18.4x12mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/380/AM29F400B_EOL_21505e8-9219.pdf"
			(at -0.508 0 0)
		)
		(property "Description" "4-Mbit (512k x 8-bit / 256k x 16-bit) CMOS 5.0 Volt-only Boot Sector Flash Memory, TSOP-48"
			(at -0.254 0 0)
		)
		(property "ki_keywords" "FLASH 4Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*18.*12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AM29F400Bx-xxEx_0_1")
		(symbol "AM29F400Bx-xxEx_1_0"
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "A11")
				(number "5")
			)
		)
		(symbol "AM29F400Bx-xxEx_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 5.08)
				(name "A0")
				(number "25")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 5.08)
				(name "A1")
				(number "24")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 5.08)
				(name "A2")
				(number "23")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 5.08)
				(name "A3")
				(number "22")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 5.08)
				(name "A4")
				(number "21")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 5.08)
				(name "A5")
				(number "20")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "A6")
				(number "19")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "A7")
				(number "18")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "A8")
				(number "8")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "A9")
				(number "7")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "A10")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 5.08)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "A13")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "A14")
				(number "2")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "A15")
				(number "1")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "A16")
				(number "48")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "A17")
				(number "17")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 5.08)
				(name "~{CE}")
				(number "26")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 5.08)
				(name "~{OE}")
				(number "28")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 5.08)
				(name "~{WE}")
				(number "11")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 5.08)
				(name "~{BYTE}")
				(number "47")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 5.08)
				(name "~{RESET}")
				(number "12")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 5.08)
				(name "VCC")
				(number "37")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "46")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -25.4 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -27.94 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin tri_state line
				(at 15.24 30.48 180)
				(length 5.08)
				(name "DQ0")
				(number "29")
			)
			(pin tri_state line
				(at 15.24 27.94 180)
				(length 5.08)
				(name "DQ1")
				(number "31")
			)
			(pin tri_state line
				(at 15.24 25.4 180)
				(length 5.08)
				(name "DQ2")
				(number "33")
			)
			(pin tri_state line
				(at 15.24 22.86 180)
				(length 5.08)
				(name "DQ3")
				(number "35")
			)
			(pin tri_state line
				(at 15.24 20.32 180)
				(length 5.08)
				(name "DQ4")
				(number "38")
			)
			(pin tri_state line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "DQ5")
				(number "40")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "DQ6")
				(number "42")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "DQ7")
				(number "44")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "DQ8")
				(number "30")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "DQ9")
				(number "32")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "DQ10")
				(number "34")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "DQ11")
				(number "36")
			)
			(pin tri_state line
				(at 15.24 0 180)
				(length 5.08)
				(name "DQ12")
				(number "39")
			)
			(pin tri_state line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "DQ13")
				(number "41")
			)
			(pin tri_state line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "DQ14")
				(number "43")
			)
			(pin tri_state line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "DQ15/A-1")
				(number "45")
			)
			(pin open_collector line
				(at 15.24 -12.7 180)
				(length 5.08)
				(name "RY/~{BY}")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AM29F400Bx-xxSx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.636 35.306 0)
		)
		(property "Value" "AM29F400Bx-xxSx"
			(at 10.414 35.306 0)
		)
		(property "Footprint" "Package_SO:SOP-44_13.3x28.2mm_P1.27mm"
			(at -0.254 0 0)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/380/AM29F400B_EOL_21505e8-9219.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Mbit (512k x 8-bit / 256k x 16-bit) CMOS 5.0 Volt-only Boot Sector Flash Memory, SOP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 4Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*13.*28.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AM29F400Bx-xxSx_0_1")
		(symbol "AM29F400Bx-xxSx_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 5.08)
				(name "A0")
				(number "11")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 5.08)
				(name "A1")
				(number "10")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 5.08)
				(name "A2")
				(number "9")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 5.08)
				(name "A3")
				(number "8")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 5.08)
				(name "A4")
				(number "7")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 5.08)
				(name "A5")
				(number "6")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "A6")
				(number "5")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "A7")
				(number "4")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "A8")
				(number "42")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "A9")
				(number "41")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "A10")
				(number "40")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "A11")
				(number "39")
			)
			(pin input line
				(at -15.24 0 0)
				(length 5.08)
				(name "A12")
				(number "38")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "A13")
				(number "37")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "A14")
				(number "36")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "A15")
				(number "35")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "A16")
				(number "34")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "A17")
				(number "3")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 5.08)
				(name "~{CE}")
				(number "12")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 5.08)
				(name "~{OE}")
				(number "14")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 5.08)
				(name "~{WE}")
				(number "43")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 5.08)
				(name "~{BYTE}")
				(number "33")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 5.08)
				(name "~{RESET}")
				(number "44")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 5.08)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "VSS")
				(number "13")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin tri_state line
				(at 15.24 30.48 180)
				(length 5.08)
				(name "DQ0")
				(number "15")
			)
			(pin tri_state line
				(at 15.24 27.94 180)
				(length 5.08)
				(name "DQ1")
				(number "17")
			)
			(pin tri_state line
				(at 15.24 25.4 180)
				(length 5.08)
				(name "DQ2")
				(number "19")
			)
			(pin tri_state line
				(at 15.24 22.86 180)
				(length 5.08)
				(name "DQ3")
				(number "21")
			)
			(pin tri_state line
				(at 15.24 20.32 180)
				(length 5.08)
				(name "DQ4")
				(number "24")
			)
			(pin tri_state line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "DQ5")
				(number "26")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "DQ6")
				(number "28")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "DQ7")
				(number "30")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "DQ8")
				(number "16")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "DQ9")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "DQ10")
				(number "20")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "DQ11")
				(number "22")
			)
			(pin tri_state line
				(at 15.24 0 180)
				(length 5.08)
				(name "DQ12")
				(number "25")
			)
			(pin tri_state line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "DQ13")
				(number "27")
			)
			(pin tri_state line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "DQ14")
				(number "29")
			)
			(pin tri_state line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "DQ15/A-1")
				(number "31")
			)
			(pin open_collector line
				(at 15.24 -12.7 180)
				(length 5.08)
				(name "RY/~{BY}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AM29PDL128G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -54.61 0)
		)
		(property "Value" "AM29PDL128G"
			(at 0 54.61 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "128 Megabit (8 M x 16-Bit/4 M x 32-Bit), Simultaneous Operation Flash Memory with VersatileIO™ Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA80_1mm_15X10"
			(at 0 0 0)
		)
		(symbol "AM29PDL128G_0_1")
		(symbol "AM29PDL128G_1_1"
			(pin input line
				(at -17.78 50.8 0)
				(length 7.62)
				(name "A0")
				(number "B4")
			)
			(pin input line
				(at -17.78 48.26 0)
				(length 7.62)
				(name "A1")
				(number "C4")
			)
			(pin input line
				(at -17.78 45.72 0)
				(length 7.62)
				(name "A2")
				(number "A3")
			)
			(pin input line
				(at -17.78 43.18 0)
				(length 7.62)
				(name "A3")
				(number "B3")
			)
			(pin input line
				(at -17.78 40.64 0)
				(length 7.62)
				(name "A4")
				(number "A2")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 7.62)
				(name "A5")
				(number "A1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 7.62)
				(name "A6")
				(number "J1")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 7.62)
				(name "A7")
				(number "J2")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 7.62)
				(name "A8")
				(number "K1")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 7.62)
				(name "A9")
				(number "K2")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 7.62)
				(name "A10")
				(number "J3")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 7.62)
				(name "A11")
				(number "K3")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 7.62)
				(name "A12")
				(number "H4")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 7.62)
				(name "A13")
				(number "J5")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 7.62)
				(name "A14")
				(number "H5")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 7.62)
				(name "A15")
				(number "K6")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 7.62)
				(name "A16")
				(number "J6")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 7.62)
				(name "A17")
				(number "K7")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "A18")
				(number "K8")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 7.62)
				(name "A19")
				(number "J7")
			)
			(pin input line
				(at -17.78 0 0)
				(length 7.62)
				(name "A20")
				(number "B6")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 7.62)
				(name "A21")
				(number "A6")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 7.62)
				(name "CE#")
				(number "B7")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 7.62)
				(name "OE#")
				(number "A8")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 7.62)
				(name "WE#")
				(number "C5")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 7.62)
				(name "WP#")
				(number "B5")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 7.62)
				(name "RST#")
				(number "E4")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 7.62)
				(name "ACC")
				(number "E5")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 7.62)
				(name "WORD#")
				(number "A7")
			)
			(pin input line
				(at -17.78 -35.56 0)
				(length 7.62)
				(name "VIO")
				(number "D2")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 7.62)
				(name "VIO")
				(number "D8")
			)
			(pin input line
				(at -17.78 -40.64 0)
				(length 7.62)
				(name "VIO")
				(number "G1")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 7.62)
				(name "VIO")
				(number "G7")
			)
			(pin power_in line
				(at -17.78 -48.26 0)
				(length 7.62)
				(name "VCC")
				(number "B2")
			)
			(pin power_in line
				(at -17.78 -50.8 0)
				(length 7.62)
				(name "VCC")
				(number "J8")
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 7.62)
				(name "DQ0")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 7.62)
				(name "DQ1")
				(number "C2")
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 7.62)
				(name "DQ2")
				(number "D1")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 7.62)
				(name "DQ3")
				(number "E2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 7.62)
				(name "DQ4")
				(number "E3")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 7.62)
				(name "DQ5")
				(number "F1")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 7.62)
				(name "DQ6")
				(number "G2")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 7.62)
				(name "DQ7")
				(number "H1")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 7.62)
				(name "DQ8")
				(number "H6")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 7.62)
				(name "DQ9")
				(number "H8")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 7.62)
				(name "DQ10")
				(number "G5")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 7.62)
				(name "DQ11")
				(number "F8")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 7.62)
				(name "DQ12")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 7.62)
				(name "DQ13")
				(number "E7")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 7.62)
				(name "DQ14")
				(number "D6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 7.62)
				(name "DQ15")
				(number "C7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 7.62)
				(name "DQ16")
				(number "C3")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 7.62)
				(name "DQ17")
				(number "C1")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 7.62)
				(name "DQ18")
				(number "D4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 7.62)
				(name "DQ19")
				(number "E1")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 7.62)
				(name "DQ20")
				(number "F3")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 7.62)
				(name "DQ21")
				(number "F2")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 7.62)
				(name "DQ22")
				(number "G3")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 7.62)
				(name "DQ23")
				(number "H2")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 7.62)
				(name "DQ24")
				(number "H7")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 7.62)
				(name "DQ25")
				(number "G6")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 7.62)
				(name "DQ26")
				(number "F7")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 7.62)
				(name "DQ27")
				(number "F6")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 7.62)
				(name "DQ28")
				(number "E8")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 7.62)
				(name "DQ29")
				(number "D5")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 7.62)
				(name "DQ30")
				(number "C8")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 7.62)
				(name "DQ31/A-1")
				(number "C6")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 7.62)
				(name "RY/BY#")
				(number "A4")
			)
			(pin power_in line
				(at 17.78 -38.1 180)
				(length 7.62)
				(name "VSS")
				(number "B8")
			)
			(pin power_in line
				(at 17.78 -40.64 180)
				(length 7.62)
				(name "VSS")
				(number "D3")
			)
			(pin power_in line
				(at 17.78 -43.18 180)
				(length 7.62)
				(name "VSS")
				(number "D7")
			)
			(pin passive line
				(at 17.78 -45.72 180)
				(length 7.62)
				(name "VSS")
				(number "G4")
			)
			(pin power_in line
				(at 17.78 -48.26 180)
				(length 7.62)
				(name "VSS")
				(number "G8")
			)
			(pin power_in line
				(at 17.78 -50.8 180)
				(length 7.62)
				(name "VSS")
				(number "H3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT25DF041x-UxN-x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "AT25DF041x-UxN-x"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-8_1.58x1.63x0.35mm_Layout3x5_P0.35x0.4mm_Ball0.25mm_Pad0.25mm_NSMD"
			(at -5.08 -15.24 0)
		)
		(property "Datasheet" "http://www.adestotech.com/wp-content/uploads/DS-AT25DF041B_040.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "4-Mbit, 1.65V Minimum SPI Serial Flash Memory with Dual-I/O, WLCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI DSPI 4Mbit 1.65V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP?8*1.58x1.63*Layout3x5*P0.35x0.4mm*Ball0.25mm*"
			(at 0 0 0)
		)
		(symbol "AT25DF041x-UxN-x_0_1")
		(symbol "AT25DF041x-UxN-x_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "A3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "E1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/IO0")
				(number "D2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/IO1")
				(number "C3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "E3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "C1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "A1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "B2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT25SF081-SSHD-X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "AT25SF081-SSHD-X"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.adestotech.com/wp-content/uploads/DS-AT25SF081_045.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Mbit, 2.5V Minimum SPI Serial Flash Memory with Dual-I/O and Quad-I/O Support, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI DSPI QSPI 8Mbit 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT25SF081-SSHD-X_0_1")
		(symbol "AT25SF081-SSHD-X_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/IO0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/IO1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/IO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/IO3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT25SF081-XMHD-X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "AT25SF081-XMHD-X"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.adestotech.com/wp-content/uploads/DS-AT25SF081_045.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Mbit, 2.5V Minimum SPI Serial Flash Memory with Dual-I/O and Quad-I/O Support, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI DSPI QSPI 8Mbit 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP?8*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AT25SF081-XMHD-X_0_1")
		(symbol "AT25SF081-XMHD-X_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/IO0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/IO1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/IO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/IO3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT25SL321-U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "AT25SL321-U"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-8_1.551x2.284mm_Layout2x4_P0.5mm"
			(at 1.27 -22.86 0)
		)
		(property "Datasheet" "https://www.adestotech.com/wp-content/uploads/AT25SL321_112.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-Mbit, 1.7V 2.5V Minimum SPI Serial Flash Memory with Dual-I/O and Quad-I/O Support, WLCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI DSPI QSPI 32Mbit 1.7V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.551x2.284mm*Layout2x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT25SL321-U_0_1")
		(symbol "AT25SL321-U_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "A2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "C1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/IO0")
				(number "D1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "IO1/SO")
				(number "B2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/IO2")
				(number "C2")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/IO3")
				(number "B1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "A1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "D2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT45DB161-JC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "AT45DB161-JC"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_LCC:PLCC-32_11.4x14.0mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc0807.pdf"
			(at 0 0 0)
		)
		(property "Description" "16Mb Serial DataFlash, 2.7V Vcc, PLCC-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Atmel DataFlash"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC?32*11.4x14.0mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT45DB161-JC_0_1")
		(symbol "AT45DB161-JC_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SI")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "28")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{WP}")
				(number "29")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SCK")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SO")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RDY/~{BUSY}")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT45DB161-RC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.636 0)
		)
		(property "Value" "AT45DB161-RC"
			(at 0.762 8.636 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_8.7x18.25mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc0807.pdf"
			(at 0 0 0)
		)
		(property "Description" "16Mb Serial DataFlash, 2.7V Vcc, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Atmel DataFlash"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?28*8.7x18.25mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT45DB161-RC_0_1")
		(symbol "AT45DB161-RC_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SI")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "24")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{WP}")
				(number "25")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SCK")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SO")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RDY/~{BUSY}")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT45DB161-TC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.636 0)
		)
		(property "Value" "AT45DB161-TC"
			(at 0.762 8.636 0)
		)
		(property "Footprint" "Package_SO:TSOP-28_11.8x8mm_P0.55mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc0807.pdf"
			(at 0 0 0)
		)
		(property "Description" "16Mb Serial DataFlash, 2.7V Vcc, TSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Atmel DataFlash"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?28*11.8x8mm*P0.55mm*"
			(at 0 0 0)
		)
		(symbol "AT45DB161-TC_0_1")
		(symbol "AT45DB161-TC_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SI")
				(number "13")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "11")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SCK")
				(number "12")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SO")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RDY/~{BUSY}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT45DB161D-SU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "AT45DB161D-SU"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 29.21 -15.24 0)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/698/doc3500-2956563.pdf"
			(at 0 0 0)
		)
		(property "Description" "16Mb Serial DataFlash, 2.5V Vcc, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adesto Flash Memory DataFlash Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT45DB161D-SU_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SI")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{WP}")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SCK")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SO")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GD25D10CT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "GD25D10CT"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.elm-tech.com/en/products/spi-flash-memory/gd25d10/gd25d10.pdf"
			(at 0 0 0)
		)
		(property "Description" "1Mbit, 3.0V Standard and Dual Serial Flash, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI DSPI QSPI 1Mbit 3.0V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "GD25D10CT_0_1")
		(symbol "GD25D10CT_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/IO0")
				(number "5")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "O1/SO")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GD25QxxxEY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.398 13.97 0)
		)
		(property "Value" "GD25QxxxEY"
			(at 7.112 13.97 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_8x6mm_P1.27mm_EP3.4x4.3mm"
			(at -0.254 -24.892 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2201241400_GigaDevice-Semicon-Beijing-GD25Q256EYIGR_C2927043.pdf"
			(at 0 -27.178 0)
		)
		(property "Description" "3.0V, Standard/Dual/Quad Serial Flash, WSON-8"
			(at 0 -29.21 0)
		)
		(property "ki_keywords" "SPI DSPI QSPI 3.0V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*8x6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "GD25QxxxEY_0_1")
		(symbol "GD25QxxxEY_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SI/IO0")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SO/IO1")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{WP}/IO2")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/~{RESET}/IO3")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS25WP256D-xM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "IS25WP256D-xM"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 1.27 15.24 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/IS25LP(WP)256D.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "256-Mbit, 1.8V SPI Serial Flash Memory with Dual-I/O and Quad-I/O Support, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI DSPI QSPI NOR 256Mbit 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IS25WP256D-xM_0_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SI/IO0")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCK")
				(number "16")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CE}")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{WP}/IO2")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/IO3")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SO/IO1")
				(number "8")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{RESET}/NC")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M25PX32-VMP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "M25PX32-VMP"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-S-8-1EP_6x5mm_P1.27mm"
			(at 20.32 2.54 0)
		)
		(property "Datasheet" "https://www.mouser.de/datasheet/2/671/M25PX32-1282938.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "32Mb, Dual I/O, 4KB Subsector Erase, 3V Serial Flash Memory with 75 MHz SPI Bus Interface, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NOR Serial Flash Embedded Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*6x5mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "M25PX32-VMP_0_1")
		(symbol "M25PX32-VMP_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{S}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DQ0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DQ1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{W}/V_{PP}")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PAD/V_{SS}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M25PX32-VMW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "M25PX32-VMW"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.mouser.de/datasheet/2/671/M25PX32-1282938.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32Mb, Dual I/O, 4KB Subsector Erase, 3V Serial Flash Memory with 75 MHz SPI Bus Interface, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NOR Serial Flash Embedded Memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "M25PX32-VMW_0_1")
		(symbol "M25PX32-VMW_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{S}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DQ0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DQ1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{W}/V_{PP}")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M29W004"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.858 27.94 0)
		)
		(property "Value" "M29W004"
			(at 7.62 -29.21 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Flash EEProm 512Ko (TSOP 40 pack.) 3,3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM FLASH 512KO"
			(at 0 0 0)
		)
		(symbol "M29W004_0_1")
		(symbol "M29W004_1_1"
			(pin input line
				(at -15.24 24.13 0)
				(length 6.35)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -15.24 21.59 0)
				(length 6.35)
				(name "A1")
				(number "20")
			)
			(pin input line
				(at -15.24 19.05 0)
				(length 6.35)
				(name "A2")
				(number "19")
			)
			(pin input line
				(at -15.24 16.51 0)
				(length 6.35)
				(name "A3")
				(number "18")
			)
			(pin input line
				(at -15.24 13.97 0)
				(length 6.35)
				(name "A4")
				(number "17")
			)
			(pin input line
				(at -15.24 11.43 0)
				(length 6.35)
				(name "A5")
				(number "16")
			)
			(pin input line
				(at -15.24 8.89 0)
				(length 6.35)
				(name "A6")
				(number "15")
			)
			(pin input line
				(at -15.24 6.35 0)
				(length 6.35)
				(name "A7")
				(number "14")
			)
			(pin input line
				(at -15.24 3.81 0)
				(length 6.35)
				(name "A8")
				(number "8")
			)
			(pin input line
				(at -15.24 1.27 0)
				(length 6.35)
				(name "A9")
				(number "7")
			)
			(pin input line
				(at -15.24 -1.27 0)
				(length 6.35)
				(name "A10")
				(number "36")
			)
			(pin input line
				(at -15.24 -3.81 0)
				(length 6.35)
				(name "A11")
				(number "6")
			)
			(pin input line
				(at -15.24 -6.35 0)
				(length 6.35)
				(name "A12")
				(number "5")
			)
			(pin input line
				(at -15.24 -8.89 0)
				(length 6.35)
				(name "A13")
				(number "4")
			)
			(pin input line
				(at -15.24 -11.43 0)
				(length 6.35)
				(name "A14")
				(number "3")
			)
			(pin input line
				(at -15.24 -13.97 0)
				(length 6.35)
				(name "A15")
				(number "2")
			)
			(pin input line
				(at -15.24 -16.51 0)
				(length 6.35)
				(name "A16")
				(number "1")
			)
			(pin input line
				(at -15.24 -19.05 0)
				(length 6.35)
				(name "A17")
				(number "40")
			)
			(pin input line
				(at -15.24 -21.59 0)
				(length 6.35)
				(name "A18")
				(number "13")
			)
			(pin power_in line
				(at -1.27 33.02 270)
				(length 6.35)
				(name "VCC")
				(number "30")
			)
			(pin power_in line
				(at -1.27 -33.02 90)
				(length 6.35)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 1.27 33.02 270)
				(length 6.35)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 1.27 -33.02 90)
				(length 6.35)
				(name "GND")
				(number "23")
			)
			(pin tri_state line
				(at 15.24 24.13 180)
				(length 6.35)
				(name "D0")
				(number "25")
			)
			(pin tri_state line
				(at 15.24 21.59 180)
				(length 6.35)
				(name "D1")
				(number "26")
			)
			(pin tri_state line
				(at 15.24 19.05 180)
				(length 6.35)
				(name "D2")
				(number "27")
			)
			(pin tri_state line
				(at 15.24 16.51 180)
				(length 6.35)
				(name "D3")
				(number "28")
			)
			(pin tri_state line
				(at 15.24 13.97 180)
				(length 6.35)
				(name "D4")
				(number "32")
			)
			(pin tri_state line
				(at 15.24 11.43 180)
				(length 6.35)
				(name "D5")
				(number "33")
			)
			(pin tri_state line
				(at 15.24 8.89 180)
				(length 6.35)
				(name "D6")
				(number "34")
			)
			(pin tri_state line
				(at 15.24 6.35 180)
				(length 6.35)
				(name "D7")
				(number "35")
			)
			(pin input inverted
				(at 15.24 1.27 180)
				(length 6.35)
				(name "CE")
				(number "22")
			)
			(pin input inverted
				(at 15.24 -1.27 180)
				(length 6.35)
				(name "OE")
				(number "24")
			)
			(pin input inverted
				(at 15.24 -3.81 180)
				(length 6.35)
				(name "WE")
				(number "9")
			)
			(pin output inverted
				(at 15.24 -11.43 180)
				(length 6.35)
				(name "Busy")
				(number "12")
			)
			(pin input inverted
				(at 15.24 -13.97 180)
				(length 6.35)
				(name "Rst/B")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M29W008"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.858 27.94 0)
		)
		(property "Value" "M29W008"
			(at 7.62 -29.21 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Flash EEProm 1MO (TSOP 40 pack.) 3,3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM FLASH 1MO"
			(at 0 0 0)
		)
		(symbol "M29W008_0_1")
		(symbol "M29W008_1_1"
			(pin input line
				(at -15.24 24.13 0)
				(length 6.35)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -15.24 21.59 0)
				(length 6.35)
				(name "A1")
				(number "20")
			)
			(pin input line
				(at -15.24 19.05 0)
				(length 6.35)
				(name "A2")
				(number "19")
			)
			(pin input line
				(at -15.24 16.51 0)
				(length 6.35)
				(name "A3")
				(number "18")
			)
			(pin input line
				(at -15.24 13.97 0)
				(length 6.35)
				(name "A4")
				(number "17")
			)
			(pin input line
				(at -15.24 11.43 0)
				(length 6.35)
				(name "A5")
				(number "16")
			)
			(pin input line
				(at -15.24 8.89 0)
				(length 6.35)
				(name "A6")
				(number "15")
			)
			(pin input line
				(at -15.24 6.35 0)
				(length 6.35)
				(name "A7")
				(number "14")
			)
			(pin input line
				(at -15.24 3.81 0)
				(length 6.35)
				(name "A8")
				(number "8")
			)
			(pin input line
				(at -15.24 1.27 0)
				(length 6.35)
				(name "A9")
				(number "7")
			)
			(pin input line
				(at -15.24 -1.27 0)
				(length 6.35)
				(name "A10")
				(number "36")
			)
			(pin input line
				(at -15.24 -3.81 0)
				(length 6.35)
				(name "A11")
				(number "6")
			)
			(pin input line
				(at -15.24 -6.35 0)
				(length 6.35)
				(name "A12")
				(number "5")
			)
			(pin input line
				(at -15.24 -8.89 0)
				(length 6.35)
				(name "A13")
				(number "4")
			)
			(pin input line
				(at -15.24 -11.43 0)
				(length 6.35)
				(name "A14")
				(number "3")
			)
			(pin input line
				(at -15.24 -13.97 0)
				(length 6.35)
				(name "A15")
				(number "2")
			)
			(pin input line
				(at -15.24 -16.51 0)
				(length 6.35)
				(name "A16")
				(number "1")
			)
			(pin input line
				(at -15.24 -19.05 0)
				(length 6.35)
				(name "A17")
				(number "40")
			)
			(pin input line
				(at -15.24 -21.59 0)
				(length 6.35)
				(name "A18")
				(number "13")
			)
			(pin input line
				(at -15.24 -24.13 0)
				(length 6.35)
				(name "A19")
				(number "37")
			)
			(pin power_in line
				(at -1.27 33.02 270)
				(length 6.35)
				(name "VCC")
				(number "30")
			)
			(pin power_in line
				(at -1.27 -33.02 90)
				(length 6.35)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 1.27 33.02 270)
				(length 6.35)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 1.27 -33.02 90)
				(length 6.35)
				(name "GND")
				(number "23")
			)
			(pin tri_state line
				(at 15.24 24.13 180)
				(length 6.35)
				(name "D0")
				(number "25")
			)
			(pin tri_state line
				(at 15.24 21.59 180)
				(length 6.35)
				(name "D1")
				(number "26")
			)
			(pin tri_state line
				(at 15.24 19.05 180)
				(length 6.35)
				(name "D2")
				(number "27")
			)
			(pin tri_state line
				(at 15.24 16.51 180)
				(length 6.35)
				(name "D3")
				(number "28")
			)
			(pin tri_state line
				(at 15.24 13.97 180)
				(length 6.35)
				(name "D4")
				(number "32")
			)
			(pin tri_state line
				(at 15.24 11.43 180)
				(length 6.35)
				(name "D5")
				(number "33")
			)
			(pin tri_state line
				(at 15.24 8.89 180)
				(length 6.35)
				(name "D6")
				(number "34")
			)
			(pin tri_state line
				(at 15.24 6.35 180)
				(length 6.35)
				(name "D7")
				(number "35")
			)
			(pin input inverted
				(at 15.24 1.27 180)
				(length 6.35)
				(name "CE")
				(number "22")
			)
			(pin input inverted
				(at 15.24 -1.27 180)
				(length 6.35)
				(name "OE")
				(number "24")
			)
			(pin input inverted
				(at 15.24 -3.81 180)
				(length 6.35)
				(name "WE")
				(number "9")
			)
			(pin output inverted
				(at 15.24 -11.43 180)
				(length 6.35)
				(name "Busy")
				(number "12")
			)
			(pin input inverted
				(at 15.24 -13.97 180)
				(length 6.35)
				(name "Rst/B")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MT25QUxxxxxx1xW7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MT25QUxxxxxx1xW7"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:W-PDFN-8-1EP_6x5mm_P1.27mm_EP3x3mm"
			(at 20.32 2.54 0)
		)
		(property "Datasheet" "https://media-www.micron.com/-/media/client/global/documents/products/data-sheet/nor-flash/serial-nor/mt25q/die-rev-a/mt25q_qljs_u_256_aba_0.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "Micron 128M/256M/512M/1G/2Gbit, 1.8V Multiple I/O Serial NOR Flash Memory, W-PDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash SPI DSPI QSPI 128Mbit 256Mbit 512Mbit 1Gbit 2Gbit 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DFN*6x5mm*P1.27mm*EP3x3mm*"
			(at 0 0 0)
		)
		(symbol "MT25QUxxxxxx1xW7_0_1")
		(symbol "MT25QUxxxxxx1xW7_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{S}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DQ0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DQ1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{W}/DQ2")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{RESET}/DQ3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MX25L3233FM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MX25L3233FM"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.macronix.com/Lists/Datasheet/Attachments/8377/MX25L3233F,%203V,%2032Mb,%20v1.1.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "32-Mbit, 3V (2.65V-3.6V) SPI Serial Flash Memory, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MX25L3233FM_0_1")
		(symbol "MX25L3233FM_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "7")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/SIO0")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/SIO1")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/SIO2")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/SIO3")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MX25L3233FZN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MX25L3233FZN"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.macronix.com/Lists/Datasheet/Attachments/8377/MX25L3233F,%203V,%2032Mb,%20v1.1.pdf"
			(at 0 -17.526 0)
		)
		(property "Description" "32-Mbit, 3V (2.65V-3.6V) SPI Serial Flash Memory, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*6x5mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MX25L3233FZN_0_1")
		(symbol "MX25L3233FZN_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/SIO0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/SIO1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/SIO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/SIO3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MX25R3235FM1xx0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MX25R3235FM1xx0"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-Mbit, Wide Range Voltage SPI Serial Flash Memory, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit 1.65V-3.6V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MX25R3235FM1xx0_0_1")
		(symbol "MX25R3235FM1xx0_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/SIO0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/SIO1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/SIO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{RESET}/SIO3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MX25R3235FM1xx1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MX25R3235FM1xx1"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.macronix.com/Lists/Datasheet/Attachments/8755/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.8.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-Mbit, Wide Range Voltage SPI Serial Flash Memory, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit 1.65V-3.6V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MX25R3235FM1xx1_0_1")
		(symbol "MX25R3235FM1xx1_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/SIO0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/SIO1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/SIO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/SIO3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MX25R3235FM2xx0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MX25R3235FM2xx0"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.macronix.com/Lists/Datasheet/Attachments/8755/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.8.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-Mbit, Wide Range Voltage SPI Serial Flash Memory, SOIC-8 (SOP-8, 208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit 1.65V-3.6V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MX25R3235FM2xx0_0_1")
		(symbol "MX25R3235FM2xx0_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/SIO0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/SIO1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/SIO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{RESET}/SIO3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MX25R3235FM2xx1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "MX25R3235FM2xx1"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.macronix.com/Lists/Datasheet/Attachments/8755/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.8.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-Mbit, Wide Range Voltage SPI Serial Flash Memory, SOIC-8 (SOP-8, 208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit 1.65V-3.6V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MX25R3235FM2xx1_0_1")
		(symbol "MX25R3235FM2xx1_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/SIO0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/SIO1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/SIO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/SIO3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MX25R3235FZNxx0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MX25R3235FZNxx0"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-Mbit, Wide Range Voltage SPI Serial Flash Memory, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit 1.65V-3.6V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*6x5mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MX25R3235FZNxx0_0_1")
		(symbol "MX25R3235FZNxx0_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/SIO0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/SIO1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/SIO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{RESET}/SIO3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MX25R3235FZNxx1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MX25R3235FZNxx1"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-Mbit, Wide Range Voltage SPI Serial Flash Memory, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit 1.65V-3.6V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*6x5mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MX25R3235FZNxx1_0_1")
		(symbol "MX25R3235FZNxx1_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/SIO0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO/SIO1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/SIO2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/SIO3")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SST25VF080B-50-4x-S2Ax"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "SST25VF080B-50-4x-S2Ax"
			(at 13.97 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005045C.pdf"
			(at -1.27 13.97 0)
		)
		(property "Description" "8-Mbit, 2.7 to 3.6V, SPI Flash Memory, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "flash memory spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SST25VF080B-50-4x-S2Ax_0_1")
		(symbol "SST25VF080B-50-4x-S2Ax_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CE}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI")
				(number "5")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "SO")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SST39SF010"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 33.02 0)
		)
		(property "Value" "SST39SF010"
			(at 0 -30.48 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25022B.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "Silicon Storage Technology (SSF) 128k x 8 Flash ROM"
			(at 0 0 0)
		)
		(property "ki_keywords" "128k flash rom"
			(at 0 0 0)
		)
		(symbol "SST39SF010_0_0"
			(pin power_in line
				(at 0 36.83 270)
				(length 5.08)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -34.29 90)
				(length 5.08)
				(name "GND")
				(number "16")
			)
		)
		(symbol "SST39SF010_0_1")
		(symbol "SST39SF010_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 5.08)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 5.08)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 5.08)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 5.08)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 5.08)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 5.08)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -15.24 0 0)
				(length 5.08)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "A14")
				(number "29")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "A15")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "A16")
				(number "2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "NC")
				(number "30")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 5.08)
				(name "NC")
				(number "1")
			)
			(pin input input_low
				(at -15.24 -20.32 0)
				(length 5.08)
				(name "PGM")
				(number "31")
			)
			(pin input input_low
				(at -15.24 -25.4 0)
				(length 5.08)
				(name "CE")
				(number "22")
			)
			(pin input input_low
				(at -15.24 -27.94 0)
				(length 5.08)
				(name "OE")
				(number "24")
			)
			(pin tri_state line
				(at 15.24 30.48 180)
				(length 5.08)
				(name "D0")
				(number "13")
			)
			(pin tri_state line
				(at 15.24 27.94 180)
				(length 5.08)
				(name "D1")
				(number "14")
			)
			(pin tri_state line
				(at 15.24 25.4 180)
				(length 5.08)
				(name "D2")
				(number "15")
			)
			(pin tri_state line
				(at 15.24 22.86 180)
				(length 5.08)
				(name "D3")
				(number "17")
			)
			(pin tri_state line
				(at 15.24 20.32 180)
				(length 5.08)
				(name "D4")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "D5")
				(number "19")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "D6")
				(number "20")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "D7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SST39SF020"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 33.02 0)
		)
		(property "Value" "SST39SF020"
			(at 0 -30.48 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25022B.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "Silicon Storage Technology (SSF) 256k x 8 Flash ROM"
			(at 0 0 0)
		)
		(property "ki_keywords" "256k flash rom"
			(at 0 0 0)
		)
		(symbol "SST39SF020_0_0"
			(pin power_in line
				(at 0 36.83 270)
				(length 5.08)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -34.29 90)
				(length 5.08)
				(name "GND")
				(number "16")
			)
		)
		(symbol "SST39SF020_0_1")
		(symbol "SST39SF020_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 5.08)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 5.08)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 5.08)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 5.08)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 5.08)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 5.08)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -15.24 0 0)
				(length 5.08)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "A14")
				(number "29")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "A15")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "A16")
				(number "2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "A17")
				(number "30")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 5.08)
				(name "NC")
				(number "1")
			)
			(pin input input_low
				(at -15.24 -20.32 0)
				(length 5.08)
				(name "PGM")
				(number "31")
			)
			(pin input input_low
				(at -15.24 -25.4 0)
				(length 5.08)
				(name "CE")
				(number "22")
			)
			(pin input input_low
				(at -15.24 -27.94 0)
				(length 5.08)
				(name "OE")
				(number "24")
			)
			(pin tri_state line
				(at 15.24 30.48 180)
				(length 5.08)
				(name "D0")
				(number "13")
			)
			(pin tri_state line
				(at 15.24 27.94 180)
				(length 5.08)
				(name "D1")
				(number "14")
			)
			(pin tri_state line
				(at 15.24 25.4 180)
				(length 5.08)
				(name "D2")
				(number "15")
			)
			(pin tri_state line
				(at 15.24 22.86 180)
				(length 5.08)
				(name "D3")
				(number "17")
			)
			(pin tri_state line
				(at 15.24 20.32 180)
				(length 5.08)
				(name "D4")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "D5")
				(number "19")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "D6")
				(number "20")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "D7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SST39SF040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 33.02 0)
		)
		(property "Value" "SST39SF040"
			(at 0 -30.48 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25022B.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "Silicon Storage Technology (SSF) 512k x 8 Flash ROM"
			(at 0 0 0)
		)
		(property "ki_keywords" "512k flash rom"
			(at 0 0 0)
		)
		(symbol "SST39SF040_0_0"
			(pin power_in line
				(at 0 36.83 270)
				(length 5.08)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -34.29 90)
				(length 5.08)
				(name "GND")
				(number "16")
			)
		)
		(symbol "SST39SF040_0_1")
		(symbol "SST39SF040_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 5.08)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 5.08)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 5.08)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 5.08)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 5.08)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 5.08)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -15.24 0 0)
				(length 5.08)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "A14")
				(number "29")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "A15")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "A16")
				(number "2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "A17")
				(number "30")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 5.08)
				(name "A18")
				(number "1")
			)
			(pin input input_low
				(at -15.24 -20.32 0)
				(length 5.08)
				(name "PGM")
				(number "31")
			)
			(pin input input_low
				(at -15.24 -25.4 0)
				(length 5.08)
				(name "CE")
				(number "22")
			)
			(pin input input_low
				(at -15.24 -27.94 0)
				(length 5.08)
				(name "OE")
				(number "24")
			)
			(pin tri_state line
				(at 15.24 30.48 180)
				(length 5.08)
				(name "D0")
				(number "13")
			)
			(pin tri_state line
				(at 15.24 27.94 180)
				(length 5.08)
				(name "D1")
				(number "14")
			)
			(pin tri_state line
				(at 15.24 25.4 180)
				(length 5.08)
				(name "D2")
				(number "15")
			)
			(pin tri_state line
				(at 15.24 22.86 180)
				(length 5.08)
				(name "D3")
				(number "17")
			)
			(pin tri_state line
				(at 15.24 20.32 180)
				(length 5.08)
				(name "D4")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "D5")
				(number "19")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "D6")
				(number "20")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "D7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "W25Q32JVSS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "W25Q32JVSS"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf"
			(at 0 0 0)
		)
		(property "Description" "32Mbit / 4MiB Serial Flash Memory, Standard/Dual/Quad SPI, 2.7-3.6V, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "flash memory SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "W25Q32JVSS_0_1")
		(symbol "W25Q32JVSS_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DI/IO_{0}")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DO/IO_{1}")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/IO_{2}")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/~{RESET}/IO_{3}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "W25Q32JVZP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "W25Q32JVZP"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4.3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32Mbit / 4MiB Serial Flash Memory, Standard/Dual/Quad SPI, 2.7-3.6V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "flash memory SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*6x5mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "W25Q32JVZP_0_1")
		(symbol "W25Q32JVZP_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DI/IO_{0}")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DO/IO_{1}")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}/IO_{2}")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}/~{RESET}/IO_{3}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "W25X20CLZP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.795 0)
		)
		(property "Value" "W25X20CLZP"
			(at 2.54 10.795 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4.3mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25x20cl_revf%2020150806.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "2Mbit / 256KiB Serial Flash memory, Standard/Dual I/O SPI, 2.3-3.6V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Memory Flash SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*8*1EP*6x5mm*"
			(at 0 0 0)
		)
		(symbol "W25X20CLZP_0_1")
		(symbol "W25X20CLZP_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DI/IO_{0}")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DO/IO_{1}")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "W25X40CLSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.668 0)
		)
		(property "Value" "W25X40CLSN"
			(at 2.54 10.668 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/W25X40CL_G%2020210505.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "4Mbit / 512KiB Serial Flash memory, Standard/Dual I/O SPI, 2.3-3.6V, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Memory Flash SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "W25X40CLSN_0_1")
		(symbol "W25X40CLSN_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DI/IO_{0}")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DO/IO_{1}")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XTSD01G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "XTSD01G"
			(at 2.54 15.24 0)
		)
		(property "Footprint" "Package_LGA:LGA-8_8x6mm_P1.27mm"
			(at 2.54 -27.94 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2005251034_XTX-XTSD08GLGEAG_C558840.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1Gbit NAND flash compliant with SD2.0 interface, 50Mhz 3.3V, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "50MHz 1Gbit NAND FLASH SD2.0 "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*8x6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "XTSD01G_0_1")
		(symbol "XTSD01G_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SD2")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SD3/~{CS}")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CMD/DI")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SD0/DO")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SD1")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AM29F400BB-90SC"
		(extends "AM29F400Bx-xxSx")
		(property "Reference" "U"
			(at -8.636 35.306 0)
		)
		(property "Value" "AM29F400BB-90SC"
			(at 10.414 35.306 0)
		)
		(property "Footprint" "Package_SO:SOP-44_13.3x28.2mm_P1.27mm"
			(at -0.254 0 0)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/380/AM29F400B_EOL_21505e8-9219.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Mbit (512k x 8-bit / 256k x 16-bit) CMOS 5.0 Volt-only Boot Sector Flash Memory, SOP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 4Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*13.*28.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT25SF081-SSHF-X"
		(extends "AT25SF081-SSHD-X")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "AT25SF081-SSHF-X"
			(at 10.16 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.adestotech.com/wp-content/uploads/DS-AT25SF081_045.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Mbit, 2.3V Minimum SPI Serial Flash Memory with Dual-I/O and Quad-I/O Support, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI DSPI QSPI 8Mbit 2.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT25SF081-XMHF-X"
		(extends "AT25SF081-XMHD-X")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "AT25SF081-XMHF-X"
			(at 10.16 10.16 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.adestotech.com/wp-content/uploads/DS-AT25SF081_045.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Mbit, 2.3V Minimum SPI Serial Flash Memory with Dual-I/O and Quad-I/O Support, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI DSPI QSPI 8Mbit 2.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP?8*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT45DB161B-RC"
		(extends "AT45DB161-RC")
		(property "Reference" "U"
			(at -6.35 8.636 0)
		)
		(property "Value" "AT45DB161B-RC"
			(at 0.762 8.636 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_8.7x18.25mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc2224.pdf"
			(at 0 0 0)
		)
		(property "Description" "16Mb Serial DataFlash, 2.7V Vcc, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Atmel DataFlash"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?28*8.7x18.25mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT45DB161B-RC-2.5"
		(extends "AT45DB161-RC")
		(property "Reference" "U"
			(at -6.35 8.636 0)
		)
		(property "Value" "AT45DB161B-RC-2.5"
			(at 0.762 8.636 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_8.7x18.25mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc2224.pdf"
			(at 0 0 0)
		)
		(property "Description" "16Mb Serial DataFlash, 2.5V Vcc, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Atmel DataFlash"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?28*8.7x18.25mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT45DB161B-TC"
		(extends "AT45DB161-TC")
		(property "Reference" "U"
			(at -6.35 8.636 0)
		)
		(property "Value" "AT45DB161B-TC"
			(at 0.762 8.636 0)
		)
		(property "Footprint" "Package_SO:TSOP-28_11.8x8mm_P0.55mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc2224.pdf"
			(at 0 0 0)
		)
		(property "Description" "16Mb Serial DataFlash, 2.7V Vcc, TSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Atmel DataFlash"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?28*11.8x8mm*P0.55mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT45DB161B-TC-2.5"
		(extends "AT45DB161-TC")
		(property "Reference" "U"
			(at -6.35 8.636 0)
		)
		(property "Value" "AT45DB161B-TC-2.5"
			(at 0.762 8.636 0)
		)
		(property "Footprint" "Package_SO:TSOP-28_11.8x8mm_P0.55mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/doc2224.pdf"
			(at 0 0 0)
		)
		(property "Description" "16Mb Serial DataFlash, 2.5V Vcc, TSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Atmel DataFlash"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?28*11.8x8mm*P0.55mm*"
			(at 0 0 0)
		)
	)
	(symbol "GD25D05CT"
		(extends "GD25D10CT")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "GD25D05CT"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.elm-tech.com/en/products/spi-flash-memory/gd25d10/gd25d10.pdf"
			(at 0 0 0)
		)
		(property "Description" "512kbit, 3.0V Standard and Dual Serial Flash, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI DSPI QSPI 512Kbit 3.0V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MX25L3233FM1"
		(extends "MX25R3235FM2xx1")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MX25L3233FM1"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.macronix.com/Lists/Datasheet/Attachments/8377/MX25L3233F,%203V,%2032Mb,%20v1.1.pdf"
			(at 0 -17.526 0)
		)
		(property "Description" "32-Mbit, 3V (2.65V-3.6V) SPI Serial Flash Memory, SOP-8 (150mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MX25L3233FM2"
		(extends "MX25R3235FM2xx1")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MX25L3233FM2"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.macronix.com/Lists/Datasheet/Attachments/8933/MX25L3233F,%203V,%2032Mb,%20v1.7.pdf"
			(at 0 -17.526 0)
		)
		(property "Description" "32-Mbit, 3V (2.65V-3.6V) SPI Serial Flash Memory, SOIC-8 (SOP-8, 208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI 32Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "W25Q128JVE"
		(extends "W25Q32JVZP")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "W25Q128JVE"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_8x6mm_P1.27mm_EP3.4x4.3mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25q128jv_dtr%20revc%2003272018%20plus.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "128Mbit / 16MiB Serial Flash Memory, Standard/Dual/Quad SPI, 2.7-3.6V, WSON-8"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "flash memory SPI QPI DTR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*8x6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "W25Q128JVP"
		(extends "W25Q32JVZP")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "W25Q128JVP"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4.3mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25q128jv_dtr%20revc%2003272018%20plus.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "128Mbit / 16MiB Serial Flash Memory, Standard/Dual/Quad SPI, 2.7-3.6V, WSON-8"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "flash memory SPI QPI DTR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*6x5mm*P1.27mm*EP3.4x4.3mm*"
			(at 0 0 0)
		)
	)
	(symbol "W25Q128JVS"
		(extends "W25Q32JVSS")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "W25Q128JVS"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25q128jv_dtr%20revc%2003272018%20plus.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "128Mbit / 16MiB Serial Flash Memory, Standard/Dual/Quad SPI, 2.7-3.6V, SOIC-8"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "flash memory SPI QPI DTR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "W25Q16JVSS"
		(extends "W25Q32JVSS")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "W25Q16JVSS"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.winbond.com/hq/support/documentation/levelOne.jsp?__locale=en&DocNo=DA00-W25Q16JV.1"
			(at 0 0 0)
		)
		(property "Description" "16Mbit / 2MiB Serial Flash Memory, Standard/Dual/Quad SPI, 2.7-3.6V, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "flash memory SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "W25X20CLSN"
		(extends "W25X40CLSN")
		(property "Reference" "U"
			(at -7.62 10.668 0)
		)
		(property "Value" "W25X20CLSN"
			(at 2.54 10.668 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25x20cl_revf%2020150806.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "2Mbit / 256KiB Serial Flash memory, Standard/Dual I/O SPI, 2.3-3.6V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Memory Flash SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "W25X40CLSS"
		(extends "W25X40CLSN")
		(property "Reference" "U"
			(at -7.62 10.668 0)
		)
		(property "Value" "W25X40CLSS"
			(at 2.54 10.668 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/W25X40CL_G%2020210505.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "4Mbit / 512KiB Serial Flash memory, Standard/Dual I/O SPI, 2.3-3.6V, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Memory Flash SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "W25X40CLSV"
		(extends "W25X40CLSN")
		(property "Reference" "U"
			(at -7.62 10.668 0)
		)
		(property "Value" "W25X40CLSV"
			(at 2.54 10.668 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/W25X40CL_G%2020210505.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "4Mbit / 512KiB Serial Flash memory, Standard/Dual I/O SPI, 2.3-3.6V, VSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Memory Flash SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "XTSD02G"
		(extends "XTSD01G")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "XTSD02G"
			(at 2.54 15.24 0)
		)
		(property "Footprint" "Package_LGA:LGA-8_8x6mm_P1.27mm"
			(at 2.54 -27.94 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2005251034_XTX-XTSD08GLGEAG_C558840.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "2Gbit NAND flash compliant with SD2.0 interface, 50Mhz 3.3V, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "50MHz 2Gbit NAND FLASH SD2.0 "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*8x6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "XTSD04G"
		(extends "XTSD01G")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "XTSD04G"
			(at 2.54 15.24 0)
		)
		(property "Footprint" "Package_LGA:LGA-8_8x6mm_P1.27mm"
			(at 2.54 -27.94 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2005251034_XTX-XTSD08GLGEAG_C558840.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "4Gbit NAND flash compliant with SD2.0 interface, 50Mhz 3.3V, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "50MHz 4Gbit NAND FLASH SD2.0 "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*8x6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "XTSD08G"
		(extends "XTSD01G")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "XTSD08G"
			(at 2.54 15.24 0)
		)
		(property "Footprint" "Package_LGA:LGA-8_8x6mm_P1.27mm"
			(at 2.54 -27.94 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2005251034_XTX-XTSD08GLGEAG_C558840.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8Gbit NAND flash compliant with SD2.0 interface, 50Mhz 3.3V, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "50MHz 8Gbit NAND FLASH SD2.0 "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*8x6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
