(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "47L04"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "47L04"
			(at 7.62 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005371C.pdf"
			(at 6.35 8.89 0)
		)
		(property "Description" "4kbit I2C serial EERAM, SRAM with EEPROM backup, 2.7-3.6V, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "4kb 3V I2C serial EERAM SRAM EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "47L04_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "HS")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VCAP")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "A2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY14B256LA-SP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "CY14B256LA-SP"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_SO:SSOP-48_7.5x15.9mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY14B256LA_256-Kbit_(32_K_8)_nvSRAM-DataSheet-v13_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ebd9bf63054"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) nvSRAM, single 3V +20% to –10% operation, 25/45ns, SSOP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM Static MEMORY 256Kbit Nonvolatile Non-Volatile"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*7.*15.*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "CY14B256LA-SP_0_0"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "48")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "13")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "36")
			)
		)
		(symbol "CY14B256LA-SP_0_1")
		(symbol "CY14B256LA-SP_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "20")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "19")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "18")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "17")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A4")
				(number "9")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A8")
				(number "43")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A9")
				(number "42")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A10")
				(number "31")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A11")
				(number "40")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A13")
				(number "44")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A14")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "47")
			)
			(pin no_connect line
				(at -7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -6.35 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "41")
			)
			(pin no_connect line
				(at -5.08 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin no_connect line
				(at -5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -3.81 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VCAP")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 5.08 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 7.62 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ0")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ1")
				(number "21")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ2")
				(number "22")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ3")
				(number "26")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ4")
				(number "27")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ5")
				(number "28")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ6")
				(number "33")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "DQ7")
				(number "29")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{CE}")
				(number "30")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{OE}")
				(number "32")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{WE}")
				(number "45")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{HSB}")
				(number "46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY14E256LA-ZS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "CY14E256LA-ZS"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-44_10.16x18.41mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY14E256LA_256-Kbit_(32_K_8)_nvSRAM-DataSheet-v12_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ebf920b33f5"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) nvSRAM, single 5V +/-10% operation, 25/45ns, TSOP-II-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM Static MEMORY 256Kbit Nonvolatile Non-Volatile Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*10.1*18*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "CY14E256LA-ZS_0_0"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "33")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "34")
			)
		)
		(symbol "CY14E256LA-ZS_0_1")
		(symbol "CY14E256LA-ZS_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "3")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A4")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A5")
				(number "16")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A6")
				(number "17")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A7")
				(number "18")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A8")
				(number "19")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A9")
				(number "20")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A10")
				(number "25")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A11")
				(number "26")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A12")
				(number "27")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A14")
				(number "29")
			)
			(pin no_connect line
				(at -7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin no_connect line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "43")
			)
			(pin no_connect line
				(at 2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at 5.08 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at 5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin no_connect line
				(at 7.62 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "41")
			)
			(pin no_connect line
				(at 7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ0")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ1")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ2")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ3")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ4")
				(number "31")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ5")
				(number "32")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ6")
				(number "35")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "DQ7")
				(number "36")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{CE}")
				(number "8")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{OE}")
				(number "37")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{WE}")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{HSB}")
				(number "44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY14U256LA-BA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "CY14U256LA-BA"
			(at 4.572 20.955 0)
		)
		(property "Footprint" "Package_BGA:Infineon_TFBGA-48_6x10mm_Layout6x8_P0.75mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY14U256LA_256-Kbit_(32_K_8)_nvSRAM-DataSheet-v03_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ec0a9c33546"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) nvSRAM, core VCC = 2.7V to 3.6V, I/O VCCQ = 1.65V to 1.95V, 35ns, TFBGA-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM Static MEMORY 256Kbit Nonvolatile Non-Volatile"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*6*10mm*Layout6x8*P0.75mm*"
			(at 0 0 0)
		)
		(symbol "CY14U256LA-BA_0_0"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "A6")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "C2")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "D1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E4")
			)
		)
		(symbol "CY14U256LA-BA_0_1")
		(symbol "CY14U256LA-BA_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "A3")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "A4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "A5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "B3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A4")
				(number "B4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A5")
				(number "C3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A6")
				(number "C4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A7")
				(number "D4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A8")
				(number "H2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A9")
				(number "H3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A10")
				(number "H4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A11")
				(number "H5")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A12")
				(number "G3")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A13")
				(number "G4")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A14")
				(number "F3")
			)
			(pin no_connect line
				(at -7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B2")
			)
			(pin no_connect line
				(at -5.08 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H6")
			)
			(pin no_connect line
				(at -5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B6")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VCAP")
				(number "E3")
			)
			(pin no_connect line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "C5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F4")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VCCQ")
				(number "D6")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VCCQ")
				(number "E1")
			)
			(pin no_connect line
				(at 2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "D3")
			)
			(pin no_connect line
				(at 5.08 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H1")
			)
			(pin no_connect line
				(at 5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F2")
			)
			(pin no_connect line
				(at 7.62 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "G6")
			)
			(pin no_connect line
				(at 7.62 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F5")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "G1")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "A1")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B1")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ0")
				(number "C1")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ1")
				(number "D2")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ2")
				(number "E2")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ3")
				(number "F1")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ4")
				(number "C6")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ5")
				(number "D5")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ6")
				(number "E5")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "DQ7")
				(number "F6")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{CE}")
				(number "B5")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{OE}")
				(number "A2")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{WE}")
				(number "G5")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{HSB}")
				(number "G2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FM16W08-SG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 17.78 0)
		)
		(property "Value" "FM16W08-SG"
			(at 1.27 17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/41731/download"
			(at 0 0 0)
		)
		(property "Description" "64Kb FRAM nonvolatile memory, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM 5V Parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?28*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FM16W08-SG_0_1")
		(symbol "FM16W08-SG_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "A12")
				(number "2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "DQ0")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "DQ1")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "DQ2")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "DQ3")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "DQ4")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "DQ5")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 3.81)
				(name "DQ6")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "DQ7")
				(number "19")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 3.81)
				(name "~{WE}")
				(number "27")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 3.81)
				(name "~{CE}")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FM18W08-SG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "FM18W08-SG"
			(at 1.27 20.32 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/136521/download"
			(at 0 0 0)
		)
		(property "Description" "256k FRAM nonvolatile memory, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM 5V Parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FM18W08-SG_0_1")
		(symbol "FM18W08-SG_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "A13")
				(number "26")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "A14")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "DQ0")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "DQ1")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "DQ2")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "DQ3")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "DQ4")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "DQ5")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "DQ6")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 3.81)
				(name "DQ7")
				(number "19")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 3.81)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "~{WE}")
				(number "27")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 3.81)
				(name "~{CE}")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FM24C64B"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "FM24C64B"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/41651/download"
			(at 0 13.97 0)
		)
		(property "Description" "64Kb serial FRAM nonvolatile Memory, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM I2C Serial 5V FRAM NVRAM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FM24C64B_0_1")
		(symbol "FM24C64B_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FM24CL16B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "FM24CL16B"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-FM24CL16B_16-Kbit_(2_K_8)_Serial_(I2C)_F-RAM-DataSheet-v13_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ec99cb241e9"
			(at -5.08 8.89 0)
		)
		(property "Description" "16Kb serial FRAM nonvolatile Memory, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM I2C Serial 3.6V FRAM NVRAM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FM24CL16B_0_1")
		(symbol "FM24CL16B_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MB85RS16"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MB85RS16"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.fujitsu.com/downloads/MICRO/fsa/pdf/products/memory/fram/MB85RS16-DS501-00014-6v0-E.pdf"
			(at -8.89 -1.27 0)
		)
		(property "Description" "FRAM memory with SPI interface, SOIC-8 SON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM SPI 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x5.05mm*P1.27mm* *SON*2x3mm*P0.50mm*"
			(at 0 0 0)
		)
		(symbol "MB85RS16_0_1")
		(symbol "MB85RS16_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SI")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SO")
				(number "2")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MR20H40"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MR20H40"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.everspin.com/file/217/download"
			(at -7.62 7.62 0)
		)
		(property "Description" "4Mb MRAM memory with SPI interface, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "MRAM SPI EEPROM 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*6x5mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MR20H40_0_1")
		(symbol "MR20H40_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SO")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SI")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STK14C88"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "STK14C88"
			(at 2.54 20.955 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.farnell.com/datasheets/5333.pdf"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) AutoStore nvSRAM, single 5V +/-10% operation, 20/25/35/45ns, DIP-32/SOIC-32/LCC-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM SRAM Static MEMORY CMOS 256Kbit Nonvolatile Non-Volatile Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W15.* *DIP*W7.* *SO*7.*20.*P1.27mm* *LCC*11.*14.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STK14C88_0_0"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
		)
		(symbol "STK14C88_0_1")
		(symbol "STK14C88_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A4")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A6")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A7")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A8")
				(number "28")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A9")
				(number "27")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A11")
				(number "26")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A12")
				(number "3")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A13")
				(number "29")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A14")
				(number "2")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VCAP")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ0")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ1")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ2")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ3")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ4")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ5")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ6")
				(number "20")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "DQ7")
				(number "21")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{E}/~{CE}")
				(number "22")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{G}/~{OE}")
				(number "25")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{W}/~{WE}")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{HSB}")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "47C04"
		(extends "47L04")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "47C04"
			(at 7.62 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005371C.pdf"
			(at 6.35 8.89 0)
		)
		(property "Description" "4kbit I2C serial EERAM, SRAM with EEPROM backup, 4.5-5.5V, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "4kb 5V I2C serial EERAM SRAM EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "47C16"
		(extends "47L04")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "47C16"
			(at 7.62 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005371C.pdf"
			(at 6.35 8.89 0)
		)
		(property "Description" "16kbit I2C serial EERAM, SRAM with EEPROM backup, 4.5-5.5V, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "16kb 5V I2C serial EERAM SRAM EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "47L16"
		(extends "47L04")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "47L16"
			(at 7.62 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005371C.pdf"
			(at 6.35 8.89 0)
		)
		(property "Description" "16kbit I2C serial EERAM, SRAM with EEPROM backup, 2.7-3.6V, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "16kb 3V I2C serial EERAM SRAM EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY14B256LA-ZS"
		(extends "CY14E256LA-ZS")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "CY14B256LA-ZS"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-44_10.16x18.41mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY14B256LA_256-Kbit_(32_K_8)_nvSRAM-DataSheet-v13_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ebd9bf63054"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) nvSRAM, single 3V +20% to –10% operation, 25/45ns, TSOP-II-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM Static MEMORY 256Kbit Nonvolatile Non-Volatile"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*10.1*18*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY14E256LA-SZ"
		(extends "STK14C88")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "CY14E256LA-SZ"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_SO:SOIC-32_7.518x20.777mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY14E256LA_256-Kbit_(32_K_8)_nvSRAM-DataSheet-v12_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ebf920b33f5"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) nvSRAM, single 5V +/-10% operation, 25/45ns, SOIC-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM Static MEMORY 256Kbit Nonvolatile Non-Volatile Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY14V256LA-BA"
		(extends "CY14U256LA-BA")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "CY14V256LA-BA"
			(at 4.572 20.955 0)
		)
		(property "Footprint" "Package_BGA:Infineon_TFBGA-48_6x10mm_Layout6x8_P0.75mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY14V256LA_256-Kbit_(32_K_x_8)_nvSRAM-DataSheet-v06_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ec03c9034c2"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) nvSRAM, core VCC = 3.0V to 3.6V, I/O VCCQ = 1.65V to 1.95V, 35ns, TFBGA-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM Static MEMORY 256Kbit Nonvolatile Non-Volatile"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BGA*6*10mm*Layout6x8*P0.75mm*"
			(at 0 0 0)
		)
	)
	(symbol "FM1608B-SG"
		(extends "FM16W08-SG")
		(property "Reference" "U"
			(at -7.62 17.78 0)
		)
		(property "Value" "FM1608B-SG"
			(at 1.27 17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/41731/download"
			(at 0 0 0)
		)
		(property "Description" "64Kb FRAM nonvolatile memory, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM 5V Parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?28*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FM1808B-SG"
		(extends "FM18W08-SG")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "FM1808B-SG"
			(at 1.27 20.32 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/136521/download"
			(at 0 0 0)
		)
		(property "Description" "256k FRAM nonvolatile memory, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM 5V Parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FM24C64C"
		(extends "FM24C64B")
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "FM24C64C"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/41651/download"
			(at -5.08 8.89 0)
		)
		(property "Description" "64Kb serial FRAM nonvolatile Memory, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM I2C Serial 5V FRAM NVRAM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MB85RS128B"
		(extends "MB85RS16")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MB85RS128B"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.fujitsu.com/downloads/MICRO/fsa/pdf/products/memory/fram/MB85RS16-DS501-00014-6v0-E.pdf"
			(at -8.89 -1.27 0)
		)
		(property "Description" "FRAM memory with SPI interface, SOIC-8 SON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM SPI 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x5.05mm*P1.27mm* *SON*2x3mm*P0.50mm*"
			(at 0 0 0)
		)
	)
	(symbol "MB85RS1MT"
		(extends "MB85RS16")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MB85RS1MT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.fujitsu.com/downloads/MICRO/fsa/pdf/products/memory/fram/MB85RS16-DS501-00014-6v0-E.pdf"
			(at -8.89 -1.27 0)
		)
		(property "Description" "FRAM memory with SPI interface, SOIC-8 SON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM SPI 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x5.05mm*P1.27mm* *SON*2x3mm*P0.50mm*"
			(at 0 0 0)
		)
	)
	(symbol "MB85RS256B"
		(extends "MB85RS16")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MB85RS256B"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.fujitsu.com/downloads/MICRO/fsa/pdf/products/memory/fram/MB85RS16-DS501-00014-6v0-E.pdf"
			(at -8.89 -1.27 0)
		)
		(property "Description" "FRAM memory with SPI interface, SOIC-8 SON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM SPI 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x5.05mm*P1.27mm* *SON*2x3mm*P0.50mm*"
			(at 0 0 0)
		)
	)
	(symbol "MB85RS2MT"
		(extends "MB85RS16")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MB85RS2MT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.fujitsu.com/downloads/MICRO/fsa/pdf/products/memory/fram/MB85RS16-DS501-00014-6v0-E.pdf"
			(at -8.89 -1.27 0)
		)
		(property "Description" "FRAM memory with SPI interface, SOIC-8 SON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM SPI 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x5.05mm*P1.27mm* *SON*2x3mm*P0.50mm*"
			(at 0 0 0)
		)
	)
	(symbol "MB85RS512T"
		(extends "MB85RS16")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MB85RS512T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.fujitsu.com/downloads/MICRO/fsa/pdf/products/memory/fram/MB85RS16-DS501-00014-6v0-E.pdf"
			(at -8.89 -1.27 0)
		)
		(property "Description" "FRAM memory with SPI interface, SOIC-8 SON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM SPI 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x5.05mm*P1.27mm* *SON*2x3mm*P0.50mm*"
			(at 0 0 0)
		)
	)
	(symbol "MB85RS64"
		(extends "MB85RS16")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MB85RS64"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.fujitsu.com/downloads/MICRO/fme/fram/datasheet-MB85RS64.pdf"
			(at -8.89 -1.27 0)
		)
		(property "Description" "FRAM memory with SPI interface, SOIC-8 SON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FRAM SPI 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x5.05mm*P1.27mm* *SON*2x3mm*P0.50mm*"
			(at 0 0 0)
		)
	)
	(symbol "MR25H40"
		(extends "MR20H40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MR25H40"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.everspin.com/file/217/download"
			(at -7.62 7.62 0)
		)
		(property "Description" "4Mb MRAM memory with SPI interface, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "MRAM SPI EEPROM 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*6x5mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STK14C88-3"
		(extends "STK14C88")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "STK14C88-3"
			(at 2.54 20.955 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.mouser.com/ds/2/100/STK14C88-3_001-50592-356490.pdf"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) AutoStore nvSRAM, single 3.3V +/-0.3V operation, 35/45ns, DIP-32/SOIC-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM SRAM Static MEMORY CMOS 256Kbit Nonvolatile Non-Volatile Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W15.* *SO*7.*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STK14C88C"
		(extends "STK14C88")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "STK14C88C"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_DIP:DIP-32_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-STK14C88C_256-Kbit_(32K_x_8)_nvSRAM-DataSheet-v02_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ee81f447111"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) nvSRAM, single 5V +/-10% operation, 35ns, DIP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "EEPROM SRAM Static MEMORY CMOS 256Kbit Nonvolatile Non-Volatile Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.*"
			(at 0 0 0)
		)
	)
	(symbol "CY14B256LA-SZ"
		(extends "CY14E256LA-SZ")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "CY14B256LA-SZ"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_SO:SOIC-32_7.518x20.777mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY14B256LA_256-Kbit_(32_K_8)_nvSRAM-DataSheet-v13_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ebd9bf63054"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) nvSRAM, single 3V +20% to –10% operation, 25/45ns, SOIC-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM Static MEMORY 256Kbit Nonvolatile Non-Volatile Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STK14C88C-3"
		(extends "STK14C88C")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "STK14C88C-3"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_DIP:DIP-32_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-STK14C88C-35C35M-DataSheet-v02_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ee829987116"
			(at 0 0 0)
		)
		(property "Description" "256-Kbit (32K x 8-bit) nvSRAM, single 3.0V +20%/-10% (industrial) / single 3.3V +/-0.3V (military), 35ns, DIP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM Static MEMORY CMOS 256Kbit Nonvolatile Non-Volatile Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.*"
			(at 0 0 0)
		)
	)
)
