(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AS4C256M16D3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 41.91 0)
		)
		(property "Value" "AS4C256M16D3"
			(at 13.97 41.91 0)
		)
		(property "Footprint" "Package_BGA:BGA-96_9.0x13.0mm_Layout2x3x16_P0.8mm"
			(at -1.27 45.72 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/ddr3/4GB-AS4C256M16D3.pdf"
			(at -1.27 68.58 0)
		)
		(property "Description" "4Gb (256Mx16 bit) Double Data Rate 3 Synchronous DRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "DDR3 DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*9.0x13.0mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AS4C256M16D3_0_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "A0")
				(number "N3")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "A1")
				(number "P7")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "A2")
				(number "P3")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "A3")
				(number "N2")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "A4")
				(number "P8")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "A5")
				(number "P2")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "A6")
				(number "R8")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "A7")
				(number "R2")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "A8")
				(number "T8")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "A9")
				(number "R3")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "A10/AP")
				(number "L7")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "A11")
				(number "R7")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "A12/~{BC}")
				(number "N7")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "A13")
				(number "T3")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "A14")
				(number "T7")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "~{RESET}")
				(number "T2")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "~{CS}")
				(number "L2")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "D9")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "G7")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "K2")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "K8")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "N1")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "N9")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "R1")
			)
			(pin passive line
				(at -2.54 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "R9")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "A9")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E1")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J2")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "M1")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "P1")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "P9")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "T1")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "T9")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDDQ")
				(number "A1")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "A8")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "C1")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "C9")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "D2")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "E9")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "F1")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "H2")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "H9")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSSQ")
				(number "B1")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "B9")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "D1")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "D8")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "E2")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "E8")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "F9")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "G1")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "G9")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VREFDQ")
				(number "H1")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "DQ0")
				(number "E3")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "DQ1")
				(number "F7")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "DQ2")
				(number "F2")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "DQ3")
				(number "F8")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "DQ4")
				(number "H3")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "DQ5")
				(number "H8")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "DQ6")
				(number "G2")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "DQ7")
				(number "H7")
			)
		)
		(symbol "AS4C256M16D3_1_1"
			(text "DDR3"
				(at -3.81 3.81 0)
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "BA0")
				(number "M2")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "BA1")
				(number "N8")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "BA2")
				(number "M3")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "CK")
				(number "J7")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{CK}")
				(number "K7")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "CKE")
				(number "K9")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "~{RAS}")
				(number "J3")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "~{CAS}")
				(number "K3")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "~{WE}")
				(number "L3")
			)
			(pin input line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "ODT")
				(number "K1")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VREFCA")
				(number "M8")
			)
			(pin no_connect line
				(at 15.24 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "J1")
			)
			(pin no_connect line
				(at 15.24 -30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "J9")
			)
			(pin no_connect line
				(at 15.24 -33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "L1")
			)
			(pin no_connect line
				(at 15.24 -35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "L9")
			)
			(pin no_connect line
				(at 15.24 -38.1 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "M7")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "DQ8")
				(number "D7")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DQ9")
				(number "C3")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DQ10")
				(number "C8")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DQ11")
				(number "C2")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DQ12")
				(number "A7")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DQ13")
				(number "A2")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DQ14")
				(number "B8")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "DQ15")
				(number "A3")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "LDM")
				(number "E7")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "UDM")
				(number "D3")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "LDQS")
				(number "F3")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "~{LDQS}")
				(number "G3")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "UDQS")
				(number "C7")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{UDQS}")
				(number "B7")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "ZQ")
				(number "L8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS4C4M16SA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "AS4C4M16SA"
			(at 7.62 34.29 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/dram/64M-AS4C4M16SA-CI_v3.0_March%202015.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "64M – (4M x 16 bit) Synchronous DRAM (SDRAM), TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDRAM Synchronous DRAM PC166 PC143 64Mb 16Mbx4 MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AS4C4M16SA_0_1")
		(symbol "AS4C4M16SA_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "BA0")
				(number "20")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "BA1")
				(number "21")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "A0")
				(number "23")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A1")
				(number "24")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A2")
				(number "25")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A3")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A4")
				(number "29")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A5")
				(number "30")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A6")
				(number "31")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A7")
				(number "32")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A8")
				(number "33")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A9")
				(number "34")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A10/AP")
				(number "22")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "35")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{CS}")
				(number "19")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CKE")
				(number "37")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "CLK")
				(number "38")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "LDQM")
				(number "15")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "UDQM")
				(number "39")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "~{WE}")
				(number "16")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{CAS}")
				(number "17")
			)
			(pin input line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{RAS}")
				(number "18")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "28")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "54")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDQ")
				(number "3")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "43")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "49")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "12")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "46")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "52")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSSQ")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC/RFU")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "DQ0")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "DQ1")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "DQ2")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "DQ3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "DQ4")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ5")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ6")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ7")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ8")
				(number "42")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ9")
				(number "44")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ10")
				(number "45")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ11")
				(number "47")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DQ12")
				(number "48")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DQ13")
				(number "50")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DQ14")
				(number "51")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DQ15")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS6C1008-xxB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS6C1008-xxB"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_BGA:Alliance_TFBGA-36_6x8mm_Layout6x8_P0.75mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/AS6C1008_Mar_2023V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit (128K X 8-bit) Low Power CMOS SRAM, single 2.7V ~ 5.5V power supply, 55ns, TFBGA-36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Static MEMORY 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TFBGA*6*8mm*Layout6x8*P0.75mm*"
			(at 0 0 0)
		)
		(symbol "AS6C1008-xxB_0_0"
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "D6")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "D1")
			)
		)
		(symbol "AS6C1008-xxB_0_1")
		(symbol "AS6C1008-xxB_1_0"
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "E1")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E6")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F3")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F4")
			)
		)
		(symbol "AS6C1008-xxB_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A0")
				(number "A1")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A1")
				(number "A2")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A2")
				(number "B2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A3")
				(number "A4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A4")
				(number "B4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A5")
				(number "C4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A6")
				(number "A5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A7")
				(number "B5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A8")
				(number "A6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A9")
				(number "H1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A10")
				(number "H2")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A11")
				(number "H3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A12")
				(number "H4")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A13")
				(number "H5")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A14")
				(number "H6")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A15")
				(number "G5")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "A16")
				(number "G4")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "C3")
			)
			(pin tri_state line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "DQ0")
				(number "B6")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ1")
				(number "C6")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ2")
				(number "F6")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ3")
				(number "G6")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ4")
				(number "B1")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ5")
				(number "C1")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ6")
				(number "F1")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ7")
				(number "G1")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS1}/~{CE1}")
				(number "G3")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CS2/CE2")
				(number "A3")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{OE}")
				(number "G2")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{WE}")
				(number "B3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS6C1008-xxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS6C1008-xxP"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_DIP:DIP-32_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/AS6C1008_Mar_2023V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit (128K X 8-bit) Low Power CMOS SRAM, single 2.7V ~ 5.5V power supply, 55ns, DIP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Static MEMORY 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "AS6C1008-xxP_0_0"
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
		)
		(symbol "AS6C1008-xxP_0_1")
		(symbol "AS6C1008-xxP_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A14")
				(number "3")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A15")
				(number "31")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "A16")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "DQ0")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ1")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ2")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ3")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ4")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ5")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ6")
				(number "20")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ7")
				(number "21")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS1}/~{CE1}")
				(number "22")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CS2/CE2")
				(number "30")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{OE}")
				(number "24")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{WE}")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS6C1008-xxT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS6C1008-xxT"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_18.4x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/AS6C1008_Mar_2023V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit (128K X 8-bit) Low Power CMOS SRAM, single 2.7V ~ 5.5V power supply, 55ns, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Static MEMORY 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*18.4*8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AS6C1008-xxT_0_0"
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "24")
			)
		)
		(symbol "AS6C1008-xxT_0_1")
		(symbol "AS6C1008-xxT_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A0")
				(number "20")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A1")
				(number "19")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A2")
				(number "18")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A3")
				(number "17")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A4")
				(number "16")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A5")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A6")
				(number "14")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A7")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A8")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A9")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A10")
				(number "31")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A11")
				(number "1")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A12")
				(number "12")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A13")
				(number "4")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A14")
				(number "11")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A15")
				(number "7")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "A16")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "DQ0")
				(number "21")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ1")
				(number "22")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ2")
				(number "23")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ3")
				(number "25")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ4")
				(number "26")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ5")
				(number "27")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ6")
				(number "28")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ7")
				(number "29")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS1}/~{CE1}")
				(number "30")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CS2/CE2")
				(number "6")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{OE}")
				(number "32")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{WE}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS6C1616"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 31.75 0)
		)
		(property "Value" "AS6C1616"
			(at 6.35 -31.75 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-48_18.4x12mm_P0.5mm"
			(at 26.67 -34.29 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/AS6C1616-TSOPI.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "1024k x 16 bit low power CMOS SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "memory SRAM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?I*18.4x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AS6C1616_0_1")
		(symbol "AS6C1616_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 5.08)
				(name "DQ15")
				(number "45")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 5.08)
				(name "DQ14")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 5.08)
				(name "DQ13")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 5.08)
				(name "DQ12")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 5.08)
				(name "DQ11")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "DQ10")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "DQ9")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "DQ8")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "DQ7")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "DQ6")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "DQ5")
				(number "40")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "DQ4")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "DQ3")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "DQ2")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "DQ1")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "DQ0")
				(number "29")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 5.08)
				(name "OE#")
				(number "28")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 5.08)
				(name "WE#")
				(number "11")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 5.08)
				(name "CE#")
				(number "26")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 5.08)
				(name "CE2")
				(number "12")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 5.08)
				(name "UB#")
				(number "14")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 5.08)
				(name "LB#")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VCC")
				(number "37")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 5.08)
				(name "VSS")
				(number "46")
			)
			(pin no_connect line
				(at 10.16 -22.86 180)
				(length 0)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -25.4 180)
				(length 0)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -27.94 180)
				(length 0)
				(hide yes)
				(name "NC")
				(number "47")
			)
			(pin input line
				(at 15.24 27.94 180)
				(length 5.08)
				(name "A19")
				(number "9")
			)
			(pin input line
				(at 15.24 25.4 180)
				(length 5.08)
				(name "A18")
				(number "16")
			)
			(pin input line
				(at 15.24 22.86 180)
				(length 5.08)
				(name "A17")
				(number "17")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 5.08)
				(name "A16")
				(number "48")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "A15")
				(number "1")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "A14")
				(number "2")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "A13")
				(number "3")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "A11")
				(number "5")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "A10")
				(number "6")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "A9")
				(number "7")
			)
			(pin input line
				(at 15.24 0 180)
				(length 5.08)
				(name "A8")
				(number "8")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "A7")
				(number "18")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "A6")
				(number "19")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "A5")
				(number "20")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "A4")
				(number "21")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 5.08)
				(name "A3")
				(number "22")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 5.08)
				(name "A2")
				(number "23")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 5.08)
				(name "A1")
				(number "24")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 5.08)
				(name "A0")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS6C4008-55PCN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.035 0)
		)
		(property "Value" "AS6C4008-55PCN"
			(at 2.54 26.035 0)
		)
		(property "Footprint" "Package_DIP:DIP-32_W15.24mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/AS6C4008.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "512K x 8 Low Power CMOS RAM, DIP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "RAM SRAM CMOS MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "AS6C4008-55PCN_0_0"
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
		)
		(symbol "AS6C4008-55PCN_0_1")
		(symbol "AS6C4008-55PCN_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A14")
				(number "3")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A15")
				(number "31")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A16")
				(number "2")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "A17")
				(number "30")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "A18")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "DQ0")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "DQ1")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ2")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ3")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ4")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ5")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ6")
				(number "20")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ7")
				(number "21")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CE#")
				(number "22")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OE#")
				(number "24")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "WE#")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY7C199"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 27.94 0)
		)
		(property "Value" "CY7C199"
			(at 3.81 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CY7C199_0_0"
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
		)
		(symbol "CY7C199_0_1")
		(symbol "CY7C199_1_1"
			(pin input line
				(at -15.24 22.86 0)
				(length 3.81)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 3.81)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "A2")
				(number "24")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "A3")
				(number "25")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "A4")
				(number "26")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "A5")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "A6")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "A8")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "A9")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "A10")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "A11")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "A12")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "A13")
				(number "9")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "A14")
				(number "10")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "~{CE}")
				(number "20")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 3.81)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 3.81)
				(name "~{WE}")
				(number "27")
			)
			(pin tri_state line
				(at 15.24 22.86 180)
				(length 3.81)
				(name "D0")
				(number "11")
			)
			(pin tri_state line
				(at 15.24 20.32 180)
				(length 3.81)
				(name "D1")
				(number "12")
			)
			(pin tri_state line
				(at 15.24 17.78 180)
				(length 3.81)
				(name "D2")
				(number "13")
			)
			(pin tri_state line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "D3")
				(number "15")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "D4")
				(number "16")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "D5")
				(number "17")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "D6")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "D7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP-PSRAM32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "ESP-PSRAM32"
			(at -1.27 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp-psram32_datasheet_en.pdf"
			(at -10.16 12.7 0)
		)
		(property "Description" "32 Mbit serial pseudo SRAM device organized as 4Mx8 bits, 1.8 VCC, SOIC8 (SOP8)"
			(at 0 0 0)
		)
		(property "ki_keywords" "32 Mbit serial pseudo SRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ESP-PSRAM32_0_1")
		(symbol "ESP-PSRAM32_1_1"
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{CE}")
				(number "1")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SIO3")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SIO2")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SI/SIO")
				(number "5")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SO/SIO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "H5AN8G8NAFR-UHC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 48.26 0)
		)
		(property "Value" "H5AN8G8NAFR-UHC"
			(at 13.97 48.26 0)
		)
		(property "Footprint" "Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm"
			(at -1.27 60.96 0)
		)
		(property "Datasheet" "https://www.skhynix.com/product/filedata/fileDownload.do?seq=7687"
			(at -1.27 68.58 0)
		)
		(property "Description" "8Gb CMOS Double Data Rate IV Synchronous RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "DDR4 DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "FBGA*7.5x11mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "H5AN8G8NAFR-UHC_0_1"
			(pin input line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "A0")
				(number "L3")
			)
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "A1")
				(number "L7")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "A2")
				(number "M3")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "A3")
				(number "K7")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "A4")
				(number "K3")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "A5")
				(number "L8")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "A6")
				(number "L2")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "A7")
				(number "M8")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "A8")
				(number "M2")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "A9")
				(number "M7")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "A10/AP")
				(number "J3")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "A11")
				(number "N2")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "A12/~{BC}")
				(number "J7")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "A13")
				(number "N8")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "A14/~{WE}")
				(number "H2")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "A15/~{CAS}")
				(number "H7")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "A16/~{RAS}")
				(number "H8")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 2.54)
				(name "A17/NC")
				(number "N7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "BG1")
				(number "J8")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "BG0")
				(number "J2")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PAR")
				(number "N3")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "BA1")
				(number "K8")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "BA0")
				(number "K2")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "NC/C2/ODT1")
				(number "F2")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "ODT")
				(number "F3")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "NC/C1/~{CS1}")
				(number "G8")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "~{CS}")
				(number "G7")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "NC/C0/CKE1")
				(number "G2")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "CKE")
				(number "G3")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "CK_t")
				(number "F7")
			)
			(pin input line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "CK_c")
				(number "F8")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "~{RESET}")
				(number "L1")
			)
			(pin input line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "TEN")
				(number "G9")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{ACT}")
				(number "H3")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin passive line
				(at -2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "C7")
			)
			(pin passive line
				(at -2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "F1")
			)
			(pin passive line
				(at -2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "F9")
			)
			(pin passive line
				(at -2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "H1")
			)
			(pin passive line
				(at -2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "J9")
			)
			(pin passive line
				(at -2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "M1")
			)
			(pin passive line
				(at -2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "N9")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDQ")
				(number "B2")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "B8")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "C1")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "C9")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "E2")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "E8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "A9")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "C8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "K1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "N1")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VPP")
				(number "B1")
			)
			(pin passive line
				(at 2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VPP")
				(number "M9")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSQ")
				(number "A2")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "A8")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "D1")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "D9")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "DQ0")
				(number "C2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "DQ1")
				(number "B7")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "DQ2")
				(number "D3")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "DQ3")
				(number "D7")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "DQ4")
				(number "D2")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "DQ5")
				(number "D8")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "DQ6")
				(number "E3")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "DQ7")
				(number "E7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DQS_t")
				(number "C3")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DQS_c")
				(number "B3")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "TDQS_t/~{DM/DBI}")
				(number "A7")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "TDQS_c")
				(number "A3")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "VREFCA")
				(number "J1")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "ZQ")
				(number "B9")
			)
			(pin open_collector line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "~{ALERT}")
				(number "L9")
			)
		)
		(symbol "H5AN8G8NAFR-UHC_1_1"
			(text "DDR4"
				(at -3.81 8.89 0)
			)
		)
		(embedded_fonts no)
	)
	(symbol "HM628128_DIP32_SOP32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "HM628128_DIP32_SOP32"
			(at 2.54 23.495 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.silicon-ark.co.uk/datasheets/hm628128-datasheet-hitachi.pdf"
			(at 0 0 0)
		)
		(property "Description" "128K-word x 8-bit High-Speed CMOS Static RAM, 70/85/100/120ns, 5V supply, DIP-32/SOP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY 1Mbit Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W15.24mm* *SOP*11.*20.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HM628128_DIP32_SOP32_0_0"
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
		)
		(symbol "HM628128_DIP32_SOP32_0_1")
		(symbol "HM628128_DIP32_SOP32_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A14")
				(number "3")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A15")
				(number "31")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "A16")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "I/O0")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "I/O1")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "I/O2")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "I/O3")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "I/O4")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "I/O5")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "I/O6")
				(number "20")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "I/O7")
				(number "21")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS1}/~{CE1}")
				(number "22")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CS2/CE2")
				(number "30")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{OE}")
				(number "24")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{WE}")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HM628128_TSOP32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "HM628128_TSOP32"
			(at 2.54 23.495 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.silicon-ark.co.uk/datasheets/hm628128-datasheet-hitachi.pdf"
			(at 0 0 0)
		)
		(property "Description" "128K-word x 8-bit High-Speed CMOS Static RAM, 70/85/100/120ns, 5V supply, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY 1Mbit Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*11.8*8*P0.5mm* *TSOP?I*18.4*8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "HM628128_TSOP32_0_0"
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "24")
			)
		)
		(symbol "HM628128_TSOP32_0_1")
		(symbol "HM628128_TSOP32_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A0")
				(number "20")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A1")
				(number "19")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A2")
				(number "18")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A3")
				(number "17")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A4")
				(number "16")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A5")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A6")
				(number "14")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A7")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A8")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A9")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A10")
				(number "31")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A11")
				(number "1")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A12")
				(number "12")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A13")
				(number "4")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A14")
				(number "11")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A15")
				(number "7")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "A16")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "I/O0")
				(number "21")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "I/O1")
				(number "22")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "I/O2")
				(number "23")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "I/O3")
				(number "25")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "I/O4")
				(number "26")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "I/O5")
				(number "27")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "I/O6")
				(number "28")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "I/O7")
				(number "29")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS1}/~{CE1}")
				(number "30")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CS2/CE2")
				(number "6")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{OE}")
				(number "32")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{WE}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HY6264AxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "HY6264AxP"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.farnell.com/datasheets/2159.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Not in Production, 8Kx8 bit Static RAM, 70/85/100/120/150ns, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "HYUNDAI SRAM CMOS MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "HY6264AxP_0_0"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
		)
		(symbol "HY6264AxP_0_1")
		(symbol "HY6264AxP_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin no_connect line
				(at 0 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "I/O0")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "I/O1")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "I/O2")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "I/O3")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "I/O4")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "I/O5")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "I/O6")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "I/O7")
				(number "19")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{CS1}")
				(number "20")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "CS2")
				(number "26")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{WE}")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IDT7006PF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "IDT7006PF"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.idt.com/document/dst/7006-data-sheet"
			(at 0 0 0)
		)
		(property "Description" "16K x 8 Dual-Port SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual-port ram"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "IDT7006PF_0_1")
		(symbol "IDT7006PF_1_1"
			(pin input line
				(at -12.7 38.1 0)
				(length 2.54)
				(name "~{CE}L")
				(number "59")
			)
			(pin input line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "~{OE}L")
				(number "62")
			)
			(pin input line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "R/~{W}L")
				(number "61")
			)
			(pin output line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "~{BUSY}L")
				(number "42")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "~{SEM}L")
				(number "60")
			)
			(pin output line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "~{INT}L")
				(number "43")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "M/~{S}")
				(number "40")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0L")
				(number "44")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1L")
				(number "45")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2L")
				(number "46")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3L")
				(number "47")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A4L")
				(number "48")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A5L")
				(number "49")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A6L")
				(number "50")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A7L")
				(number "51")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A8L")
				(number "52")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A9L")
				(number "53")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A10L")
				(number "54")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A11L")
				(number "55")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A12L")
				(number "56")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A13L")
				(number "58")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "I/O0L")
				(number "63")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "I/O1L")
				(number "64")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "I/O2L")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "I/O3L")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "I/O4L")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "I/O5L")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "I/O6L")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "I/O7L")
				(number "7")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VCC")
				(number "57")
			)
			(pin input line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "~{CE}R")
				(number "22")
			)
			(pin input line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "~{OE}R")
				(number "19")
			)
			(pin input line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "R/~{W}R")
				(number "20")
			)
			(pin output line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "~{BUSY}R")
				(number "39")
			)
			(pin input line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "~{SEM}R")
				(number "21")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "~{INT}R")
				(number "38")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "A0R")
				(number "37")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "A1R")
				(number "36")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "A2R")
				(number "35")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A3R")
				(number "34")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A4R")
				(number "33")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A5R")
				(number "32")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A6R")
				(number "31")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "A7R")
				(number "30")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A8R")
				(number "29")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A9R")
				(number "28")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A10R")
				(number "27")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "A11R")
				(number "26")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "A12R")
				(number "25")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "A13R")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "I/O0R")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "I/O1R")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "I/O2R")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "I/O3R")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "I/O4R")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "I/O5R")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "I/O6R")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "I/O7R")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IDT7027_TQ100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 57.15 0)
		)
		(property "Value" "IDT7027_TQ100"
			(at 12.7 57.15 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "IDT7027_TQ100_0_1")
		(symbol "IDT7027_TQ100_1_1"
			(pin input line
				(at -22.86 53.34 0)
				(length 7.62)
				(name "A0L")
				(number "92")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 7.62)
				(name "A1L")
				(number "93")
			)
			(pin input line
				(at -22.86 48.26 0)
				(length 7.62)
				(name "A2L")
				(number "94")
			)
			(pin input line
				(at -22.86 45.72 0)
				(length 7.62)
				(name "A3L")
				(number "95")
			)
			(pin input line
				(at -22.86 43.18 0)
				(length 7.62)
				(name "A4L")
				(number "96")
			)
			(pin input line
				(at -22.86 40.64 0)
				(length 7.62)
				(name "A5L")
				(number "97")
			)
			(pin input line
				(at -22.86 38.1 0)
				(length 7.62)
				(name "A6L")
				(number "98")
			)
			(pin input line
				(at -22.86 35.56 0)
				(length 7.62)
				(name "A7L")
				(number "99")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 7.62)
				(name "A8L")
				(number "100")
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 7.62)
				(name "A9L")
				(number "1")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 7.62)
				(name "A10L")
				(number "2")
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 7.62)
				(name "A11L")
				(number "3")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 7.62)
				(name "A12L")
				(number "4")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 7.62)
				(name "A13L")
				(number "5")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 7.62)
				(name "A14L")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 7.62)
				(name "I/O0L")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 7.62)
				(name "I/O1L")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 7.62)
				(name "I/O2L")
				(number "34")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 7.62)
				(name "I/O3L")
				(number "33")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 7.62)
				(name "I/O4L")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 7.62)
				(name "I/O5L")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "I/O6L")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "I/O7L")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "I/O8L")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 7.62)
				(name "I/O9L")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 7.62)
				(name "I/O10L")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 7.62)
				(name "I/O11L")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 7.62)
				(name "I/O12L")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 7.62)
				(name "I/O13L")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 7.62)
				(name "I/O14L")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 7.62)
				(name "I/O15L")
				(number "20")
			)
			(pin input inverted
				(at -22.86 -30.48 0)
				(length 7.62)
				(name "OEL")
				(number "17")
			)
			(pin input line
				(at -22.86 -33.02 0)
				(length 7.62)
				(name "R/WL")
				(number "16")
			)
			(pin input inverted
				(at -22.86 -35.56 0)
				(length 7.62)
				(name "SEML")
				(number "14")
			)
			(pin input line
				(at -22.86 -38.1 0)
				(length 7.62)
				(name "CE1L")
				(number "13")
			)
			(pin input inverted
				(at -22.86 -40.64 0)
				(length 7.62)
				(name "CE0L")
				(number "12")
			)
			(pin input inverted
				(at -22.86 -43.18 0)
				(length 7.62)
				(name "UBL")
				(number "11")
			)
			(pin input inverted
				(at -22.86 -45.72 0)
				(length 7.62)
				(name "LBL")
				(number "10")
			)
			(pin output inverted
				(at -22.86 -48.26 0)
				(length 7.62)
				(name "INTL")
				(number "90")
			)
			(pin bidirectional inverted
				(at -22.86 -50.8 0)
				(length 7.62)
				(name "BUSYL")
				(number "89")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "28")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "46")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "58")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "88")
			)
			(pin input line
				(at 22.86 53.34 180)
				(length 7.62)
				(name "A0R")
				(number "84")
			)
			(pin input line
				(at 22.86 50.8 180)
				(length 7.62)
				(name "A1R")
				(number "83")
			)
			(pin input line
				(at 22.86 48.26 180)
				(length 7.62)
				(name "A2R")
				(number "82")
			)
			(pin input line
				(at 22.86 45.72 180)
				(length 7.62)
				(name "A3R")
				(number "81")
			)
			(pin input line
				(at 22.86 43.18 180)
				(length 7.62)
				(name "A4R")
				(number "80")
			)
			(pin input line
				(at 22.86 40.64 180)
				(length 7.62)
				(name "A5R")
				(number "79")
			)
			(pin input line
				(at 22.86 38.1 180)
				(length 7.62)
				(name "A6R")
				(number "78")
			)
			(pin input line
				(at 22.86 35.56 180)
				(length 7.62)
				(name "A7R")
				(number "77")
			)
			(pin input line
				(at 22.86 33.02 180)
				(length 7.62)
				(name "A8R")
				(number "76")
			)
			(pin input line
				(at 22.86 30.48 180)
				(length 7.62)
				(name "A9R")
				(number "75")
			)
			(pin input line
				(at 22.86 27.94 180)
				(length 7.62)
				(name "A10R")
				(number "74")
			)
			(pin input line
				(at 22.86 25.4 180)
				(length 7.62)
				(name "A11R")
				(number "73")
			)
			(pin input line
				(at 22.86 22.86 180)
				(length 7.62)
				(name "A12R")
				(number "72")
			)
			(pin input line
				(at 22.86 20.32 180)
				(length 7.62)
				(name "A13R")
				(number "71")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 7.62)
				(name "A14R")
				(number "70")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 7.62)
				(name "I/O0R")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 7.62)
				(name "I/O1R")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 7.62)
				(name "I/O2R")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 7.62)
				(name "I/O3R")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "I/O4R")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 7.62)
				(name "I/O5R")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 7.62)
				(name "I/O6R")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 7.62)
				(name "I/O7R")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "I/O8R")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 7.62)
				(name "I/O9R")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 7.62)
				(name "I/O10R")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 7.62)
				(name "I/O11R")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 7.62)
				(name "I/O12R")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 7.62)
				(name "I/O13R")
				(number "54")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 7.62)
				(name "I/O14R")
				(number "55")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 7.62)
				(name "I/O15R")
				(number "56")
			)
			(pin input inverted
				(at 22.86 -30.48 180)
				(length 7.62)
				(name "OER")
				(number "59")
			)
			(pin input line
				(at 22.86 -33.02 180)
				(length 7.62)
				(name "R/WR")
				(number "60")
			)
			(pin input inverted
				(at 22.86 -35.56 180)
				(length 7.62)
				(name "SEMR")
				(number "62")
			)
			(pin input line
				(at 22.86 -38.1 180)
				(length 7.62)
				(name "CE1R")
				(number "63")
			)
			(pin input inverted
				(at 22.86 -40.64 180)
				(length 7.62)
				(name "CE0R")
				(number "64")
			)
			(pin input inverted
				(at 22.86 -43.18 180)
				(length 7.62)
				(name "UBR")
				(number "65")
			)
			(pin input inverted
				(at 22.86 -45.72 180)
				(length 7.62)
				(name "LBR")
				(number "66")
			)
			(pin output inverted
				(at 22.86 -48.26 180)
				(length 7.62)
				(name "INTR")
				(number "85")
			)
			(pin bidirectional inverted
				(at 22.86 -50.8 180)
				(length 7.62)
				(name "BUSYR")
				(number "86")
			)
			(pin input line
				(at 22.86 -53.34 180)
				(length 7.62)
				(name "M/S")
				(number "87")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IDT7132"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "IDT7132"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "IDT7132_0_1")
		(symbol "IDT7132_1_1"
			(pin input line
				(at -22.86 30.48 0)
				(length 7.62)
				(name "/CEL")
				(number "1")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 7.62)
				(name "R/WL")
				(number "2")
			)
			(pin output line
				(at -22.86 25.4 0)
				(length 7.62)
				(name "/BSYL")
				(number "3")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 7.62)
				(name "/OEL")
				(number "5")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 7.62)
				(name "A0L")
				(number "6")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 7.62)
				(name "A1L")
				(number "7")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 7.62)
				(name "A2L")
				(number "8")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 7.62)
				(name "A3L")
				(number "9")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 7.62)
				(name "A4L")
				(number "10")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 7.62)
				(name "A5L")
				(number "11")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 7.62)
				(name "A6L")
				(number "12")
			)
			(pin input line
				(at -22.86 0 0)
				(length 7.62)
				(name "A7L")
				(number "13")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "A8L")
				(number "14")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "A9L")
				(number "15")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "A10L")
				(number "4")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 7.62)
				(name "I/O0L")
				(number "16")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 7.62)
				(name "I/O1L")
				(number "17")
			)
			(pin input line
				(at -22.86 -17.78 0)
				(length 7.62)
				(name "I/O2L")
				(number "18")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 7.62)
				(name "I/O3L")
				(number "19")
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 7.62)
				(name "I/O4L")
				(number "20")
			)
			(pin input line
				(at -22.86 -25.4 0)
				(length 7.62)
				(name "I/O5L")
				(number "21")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 7.62)
				(name "I/O6L")
				(number "22")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 7.62)
				(name "I/O7L")
				(number "23")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "24")
			)
			(pin input line
				(at 22.86 30.48 180)
				(length 7.62)
				(name "/CER")
				(number "47")
			)
			(pin input line
				(at 22.86 27.94 180)
				(length 7.62)
				(name "R/WR")
				(number "46")
			)
			(pin output line
				(at 22.86 25.4 180)
				(length 7.62)
				(name "/BSYR")
				(number "45")
			)
			(pin input line
				(at 22.86 22.86 180)
				(length 7.62)
				(name "/OER")
				(number "43")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 7.62)
				(name "A0R")
				(number "42")
			)
			(pin input line
				(at 22.86 15.24 180)
				(length 7.62)
				(name "A1R")
				(number "41")
			)
			(pin input line
				(at 22.86 12.7 180)
				(length 7.62)
				(name "A2R")
				(number "40")
			)
			(pin input line
				(at 22.86 10.16 180)
				(length 7.62)
				(name "A3R")
				(number "39")
			)
			(pin input line
				(at 22.86 7.62 180)
				(length 7.62)
				(name "A4R")
				(number "38")
			)
			(pin input line
				(at 22.86 5.08 180)
				(length 7.62)
				(name "A5R")
				(number "37")
			)
			(pin input line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "A6R")
				(number "36")
			)
			(pin input line
				(at 22.86 0 180)
				(length 7.62)
				(name "A7R")
				(number "35")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 7.62)
				(name "A8R")
				(number "34")
			)
			(pin input line
				(at 22.86 -5.08 180)
				(length 7.62)
				(name "A9R")
				(number "33")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "A10R")
				(number "44")
			)
			(pin input line
				(at 22.86 -12.7 180)
				(length 7.62)
				(name "I/O7R")
				(number "32")
			)
			(pin input line
				(at 22.86 -15.24 180)
				(length 7.62)
				(name "I/O6R")
				(number "31")
			)
			(pin input line
				(at 22.86 -17.78 180)
				(length 7.62)
				(name "I/O5R")
				(number "30")
			)
			(pin input line
				(at 22.86 -20.32 180)
				(length 7.62)
				(name "I/O4R")
				(number "29")
			)
			(pin input line
				(at 22.86 -22.86 180)
				(length 7.62)
				(name "I/O3R")
				(number "28")
			)
			(pin input line
				(at 22.86 -25.4 180)
				(length 7.62)
				(name "I/O2R")
				(number "27")
			)
			(pin input line
				(at 22.86 -27.94 180)
				(length 7.62)
				(name "I/O1R")
				(number "26")
			)
			(pin input line
				(at 22.86 -30.48 180)
				(length 7.62)
				(name "I/O0R")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IDT71V65903S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 88.9 0)
		)
		(property "Value" "IDT71V65903S"
			(at 0 -88.9 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "165 pins BGA 3.3V high-speed 9 Megabit synchronous SRAMs 512K x 18 (or  256K x 36)"
			(at 0 0 0)
		)
		(symbol "IDT71V65903S_0_1")
		(symbol "IDT71V65903S_1_1"
			(pin input line
				(at -17.78 86.36 0)
				(length 6.35)
				(name "A0")
				(number "R6")
			)
			(pin input line
				(at -17.78 83.82 0)
				(length 6.35)
				(name "A1")
				(number "P6")
			)
			(pin input line
				(at -17.78 81.28 0)
				(length 6.35)
				(name "A2")
				(number "P4")
			)
			(pin input line
				(at -17.78 78.74 0)
				(length 6.35)
				(name "A3")
				(number "R4")
			)
			(pin input line
				(at -17.78 76.2 0)
				(length 6.35)
				(name "A4")
				(number "R3")
			)
			(pin input line
				(at -17.78 73.66 0)
				(length 6.35)
				(name "A5")
				(number "P3")
			)
			(pin input line
				(at -17.78 71.12 0)
				(length 6.35)
				(name "A6")
				(number "B2")
			)
			(pin input line
				(at -17.78 68.58 0)
				(length 6.35)
				(name "A7")
				(number "A2")
			)
			(pin input line
				(at -17.78 66.04 0)
				(length 6.35)
				(name "A8")
				(number "A10")
			)
			(pin input line
				(at -17.78 63.5 0)
				(length 6.35)
				(name "A9")
				(number "B10")
			)
			(pin input line
				(at -17.78 60.96 0)
				(length 6.35)
				(name "A10")
				(number "A11")
			)
			(pin input line
				(at -17.78 58.42 0)
				(length 6.35)
				(name "A11")
				(number "P8")
			)
			(pin input line
				(at -17.78 55.88 0)
				(length 6.35)
				(name "A12")
				(number "R8")
			)
			(pin input line
				(at -17.78 53.34 0)
				(length 6.35)
				(name "A13")
				(number "R9")
			)
			(pin input line
				(at -17.78 50.8 0)
				(length 6.35)
				(name "A14")
				(number "P9")
			)
			(pin input line
				(at -17.78 48.26 0)
				(length 6.35)
				(name "A15")
				(number "P10")
			)
			(pin input line
				(at -17.78 45.72 0)
				(length 6.35)
				(name "A16")
				(number "R10")
			)
			(pin input line
				(at -17.78 43.18 0)
				(length 6.35)
				(name "A17")
				(number "R11")
			)
			(pin input line
				(at -17.78 40.64 0)
				(length 6.35)
				(name "A18")
				(number "A9")
			)
			(pin input line
				(at -17.78 36.83 0)
				(length 6.35)
				(name "/LBO")
				(number "R1")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 6.35)
				(name "/CE1")
				(number "A3")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 6.35)
				(name "CE2")
				(number "B3")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 6.35)
				(name "/CE2")
				(number "A6")
			)
			(pin input line
				(at -17.78 24.13 0)
				(length 6.35)
				(name "R/W")
				(number "B7")
			)
			(pin input line
				(at -17.78 21.59 0)
				(length 6.35)
				(name "/CEN")
				(number "A7")
			)
			(pin input line
				(at -17.78 19.05 0)
				(length 6.35)
				(name "ADV/LD")
				(number "A8")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 6.35)
				(name "/BW2")
				(number "A4")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 6.35)
				(name "/BW1")
				(number "B5")
			)
			(pin input clock
				(at -17.78 8.89 0)
				(length 6.35)
				(name "CLK")
				(number "B6")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 6.35)
				(name "/OE")
				(number "B8")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 6.35)
				(name "ZZ")
				(number "H11")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 6.35)
				(name "VSS")
				(number "C4")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 6.35)
				(name "VSS")
				(number "N4")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 6.35)
				(name "VSS")
				(number "C5")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 6.35)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 6.35)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 6.35)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 6.35)
				(name "VSS")
				(number "G5")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 6.35)
				(name "VSS")
				(number "H5")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 6.35)
				(name "VSS")
				(number "J5")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 6.35)
				(name "VSS")
				(number "K5")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 6.35)
				(name "VSS")
				(number "L5")
			)
			(pin passive line
				(at -17.78 -30.48 0)
				(length 6.35)
				(name "VSS")
				(number "M5")
			)
			(pin passive line
				(at -17.78 -33.02 0)
				(length 6.35)
				(name "VSS")
				(number "C6")
			)
			(pin passive line
				(at -17.78 -35.56 0)
				(length 6.35)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at -17.78 -38.1 0)
				(length 6.35)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at -17.78 -40.64 0)
				(length 6.35)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at -17.78 -43.18 0)
				(length 6.35)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at -17.78 -45.72 0)
				(length 6.35)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at -17.78 -48.26 0)
				(length 6.35)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at -17.78 -50.8 0)
				(length 6.35)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at -17.78 -53.34 0)
				(length 6.35)
				(name "VSS")
				(number "L6")
			)
			(pin passive line
				(at -17.78 -55.88 0)
				(length 6.35)
				(name "VSS")
				(number "M6")
			)
			(pin passive line
				(at -17.78 -58.42 0)
				(length 6.35)
				(name "VSS")
				(number "C7")
			)
			(pin passive line
				(at -17.78 -60.96 0)
				(length 6.35)
				(name "VSS")
				(number "D7")
			)
			(pin passive line
				(at -17.78 -63.5 0)
				(length 6.35)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at -17.78 -66.04 0)
				(length 6.35)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at -17.78 -68.58 0)
				(length 6.35)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at -17.78 -71.12 0)
				(length 6.35)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at -17.78 -73.66 0)
				(length 6.35)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at -17.78 -76.2 0)
				(length 6.35)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at -17.78 -78.74 0)
				(length 6.35)
				(name "VSS")
				(number "L7")
			)
			(pin passive line
				(at -17.78 -81.28 0)
				(length 6.35)
				(name "VSS")
				(number "M7")
			)
			(pin passive line
				(at -17.78 -83.82 0)
				(length 6.35)
				(name "VSS")
				(number "C8")
			)
			(pin passive line
				(at -17.78 -86.36 0)
				(length 6.35)
				(name "VSS")
				(number "N8")
			)
			(pin bidirectional line
				(at 17.78 86.36 180)
				(length 6.35)
				(name "IO0")
				(number "M10")
			)
			(pin bidirectional line
				(at 17.78 83.82 180)
				(length 6.35)
				(name "IO1")
				(number "L10")
			)
			(pin bidirectional line
				(at 17.78 81.28 180)
				(length 6.35)
				(name "IO2")
				(number "K10")
			)
			(pin bidirectional line
				(at 17.78 78.74 180)
				(length 6.35)
				(name "IO3")
				(number "J10")
			)
			(pin bidirectional line
				(at 17.78 76.2 180)
				(length 6.35)
				(name "IO4")
				(number "G11")
			)
			(pin bidirectional line
				(at 17.78 73.66 180)
				(length 6.35)
				(name "IO5")
				(number "F11")
			)
			(pin bidirectional line
				(at 17.78 71.12 180)
				(length 6.35)
				(name "IO6")
				(number "E11")
			)
			(pin bidirectional line
				(at 17.78 68.58 180)
				(length 6.35)
				(name "IO7")
				(number "D11")
			)
			(pin bidirectional line
				(at 17.78 66.04 180)
				(length 6.35)
				(name "IO8")
				(number "D2")
			)
			(pin bidirectional line
				(at 17.78 63.5 180)
				(length 6.35)
				(name "IO9")
				(number "E2")
			)
			(pin bidirectional line
				(at 17.78 60.96 180)
				(length 6.35)
				(name "IO10")
				(number "F2")
			)
			(pin bidirectional line
				(at 17.78 58.42 180)
				(length 6.35)
				(name "IO11")
				(number "G2")
			)
			(pin bidirectional line
				(at 17.78 55.88 180)
				(length 6.35)
				(name "IO12")
				(number "J1")
			)
			(pin bidirectional line
				(at 17.78 53.34 180)
				(length 6.35)
				(name "IO13")
				(number "K1")
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 6.35)
				(name "IO14")
				(number "L1")
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 6.35)
				(name "IO15")
				(number "M1")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 6.35)
				(name "IOP1")
				(number "C11")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 6.35)
				(name "IOP2")
				(number "N1")
			)
			(pin passive line
				(at 17.78 27.94 180)
				(length 6.35)
				(name "VDDx")
				(number "H2")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 6.35)
				(name "VSSx")
				(number "H1")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 6.35)
				(name "VSSx")
				(number "N7")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 6.35)
				(name "VDDQ")
				(number "C3")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 6.35)
				(name "VDDQ")
				(number "D3")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 6.35)
				(name "VDDQ")
				(number "E3")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 6.35)
				(name "VDDQ")
				(number "F3")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 6.35)
				(name "VDDQ")
				(number "G3")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 6.35)
				(name "VDDQ")
				(number "J3")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 6.35)
				(name "VDDQ")
				(number "K3")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 6.35)
				(name "VDDQ")
				(number "L3")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 6.35)
				(name "VDDQ")
				(number "M3")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 6.35)
				(name "VDDQ")
				(number "N3")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 6.35)
				(name "VDDQ")
				(number "C9")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 6.35)
				(name "VDDQ")
				(number "D9")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 6.35)
				(name "VDDQ")
				(number "E9")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 6.35)
				(name "VDDQ")
				(number "F9")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 6.35)
				(name "VDDQ")
				(number "G9")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 6.35)
				(name "VDDQ")
				(number "J9")
			)
			(pin passive line
				(at 17.78 -27.94 180)
				(length 6.35)
				(name "VDDQ")
				(number "K9")
			)
			(pin passive line
				(at 17.78 -30.48 180)
				(length 6.35)
				(name "VDDQ")
				(number "L9")
			)
			(pin passive line
				(at 17.78 -33.02 180)
				(length 6.35)
				(name "VDDQ")
				(number "M9")
			)
			(pin power_in line
				(at 17.78 -35.56 180)
				(length 6.35)
				(name "VDDQ")
				(number "N9")
			)
			(pin passive line
				(at 17.78 -43.18 180)
				(length 6.35)
				(name "VDD")
				(number "D4")
			)
			(pin passive line
				(at 17.78 -45.72 180)
				(length 6.35)
				(name "VDD")
				(number "E4")
			)
			(pin passive line
				(at 17.78 -48.26 180)
				(length 6.35)
				(name "VDD")
				(number "F4")
			)
			(pin passive line
				(at 17.78 -50.8 180)
				(length 6.35)
				(name "VDD")
				(number "G4")
			)
			(pin passive line
				(at 17.78 -53.34 180)
				(length 6.35)
				(name "VDD")
				(number "H4")
			)
			(pin passive line
				(at 17.78 -55.88 180)
				(length 6.35)
				(name "VDD")
				(number "J4")
			)
			(pin passive line
				(at 17.78 -58.42 180)
				(length 6.35)
				(name "VDD")
				(number "K4")
			)
			(pin passive line
				(at 17.78 -60.96 180)
				(length 6.35)
				(name "VDD")
				(number "L4")
			)
			(pin passive line
				(at 17.78 -63.5 180)
				(length 6.35)
				(name "VDD")
				(number "M4")
			)
			(pin passive line
				(at 17.78 -66.04 180)
				(length 6.35)
				(name "VDD")
				(number "D8")
			)
			(pin passive line
				(at 17.78 -68.58 180)
				(length 6.35)
				(name "VDD")
				(number "E8")
			)
			(pin passive line
				(at 17.78 -71.12 180)
				(length 6.35)
				(name "VDD")
				(number "F8")
			)
			(pin passive line
				(at 17.78 -73.66 180)
				(length 6.35)
				(name "VDD")
				(number "G8")
			)
			(pin passive line
				(at 17.78 -76.2 180)
				(length 6.35)
				(name "VDD")
				(number "H8")
			)
			(pin passive line
				(at 17.78 -78.74 180)
				(length 6.35)
				(name "VDD")
				(number "J8")
			)
			(pin passive line
				(at 17.78 -81.28 180)
				(length 6.35)
				(name "VDD")
				(number "K8")
			)
			(pin passive line
				(at 17.78 -83.82 180)
				(length 6.35)
				(name "VDD")
				(number "L8")
			)
			(pin passive line
				(at 17.78 -86.36 180)
				(length 6.35)
				(name "VDD")
				(number "M8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IDT7201"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 20.32 0)
		)
		(property "Value" "IDT7201"
			(at 6.35 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "IDT7201_0_1")
		(symbol "IDT7201_1_1"
			(pin input inverted
				(at -17.78 16.51 0)
				(length 7.62)
				(name "WR")
				(number "1")
			)
			(pin input line
				(at -17.78 13.97 0)
				(length 7.62)
				(name "D0")
				(number "6")
			)
			(pin input line
				(at -17.78 11.43 0)
				(length 7.62)
				(name "D1")
				(number "5")
			)
			(pin input line
				(at -17.78 8.89 0)
				(length 7.62)
				(name "D2")
				(number "4")
			)
			(pin input line
				(at -17.78 6.35 0)
				(length 7.62)
				(name "D3")
				(number "3")
			)
			(pin input line
				(at -17.78 3.81 0)
				(length 7.62)
				(name "D4")
				(number "27")
			)
			(pin input line
				(at -17.78 1.27 0)
				(length 7.62)
				(name "D5")
				(number "26")
			)
			(pin input line
				(at -17.78 -1.27 0)
				(length 7.62)
				(name "D6")
				(number "25")
			)
			(pin input line
				(at -17.78 -3.81 0)
				(length 7.62)
				(name "D7")
				(number "24")
			)
			(pin input line
				(at -17.78 -6.35 0)
				(length 7.62)
				(name "D8")
				(number "2")
			)
			(pin input inverted
				(at -17.78 -8.89 0)
				(length 7.62)
				(name "XI")
				(number "7")
			)
			(pin input inverted
				(at -17.78 -11.43 0)
				(length 7.62)
				(name "CLR")
				(number "22")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 6.35)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 6.35)
				(name "VSS")
				(number "14")
			)
			(pin input inverted
				(at 17.78 16.51 180)
				(length 7.62)
				(name "RD")
				(number "15")
			)
			(pin tri_state line
				(at 17.78 13.97 180)
				(length 7.62)
				(name "Q0")
				(number "9")
			)
			(pin tri_state line
				(at 17.78 11.43 180)
				(length 7.62)
				(name "Q1")
				(number "10")
			)
			(pin tri_state line
				(at 17.78 8.89 180)
				(length 7.62)
				(name "Q2")
				(number "11")
			)
			(pin tri_state line
				(at 17.78 6.35 180)
				(length 7.62)
				(name "Q3")
				(number "12")
			)
			(pin tri_state line
				(at 17.78 3.81 180)
				(length 7.62)
				(name "Q4")
				(number "16")
			)
			(pin tri_state line
				(at 17.78 1.27 180)
				(length 7.62)
				(name "Q5")
				(number "17")
			)
			(pin tri_state line
				(at 17.78 -1.27 180)
				(length 7.62)
				(name "Q6")
				(number "18")
			)
			(pin tri_state line
				(at 17.78 -3.81 180)
				(length 7.62)
				(name "Q7")
				(number "19")
			)
			(pin tri_state line
				(at 17.78 -6.35 180)
				(length 7.62)
				(name "Q8")
				(number "13")
			)
			(pin output inverted
				(at 17.78 -8.89 180)
				(length 7.62)
				(name "EF")
				(number "21")
			)
			(pin input inverted
				(at 17.78 -11.43 180)
				(length 7.62)
				(name "FL")
				(number "23")
			)
			(pin input inverted
				(at 17.78 -13.97 180)
				(length 7.62)
				(name "XO")
				(number "20")
			)
			(pin output inverted
				(at 17.78 -16.51 180)
				(length 7.62)
				(name "FF")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IDT7204"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 25.4 0)
		)
		(property "Value" "IDT7204"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 30.48 0)
		)
		(property "Datasheet" "http://www.idt.com/document/7203-7208-datasheet"
			(at 0 0 0)
		)
		(property "Description" "4096x9 CMOS Asynchronous FIFO, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "asynchronous fifo memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "IDT7204_0_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "D0")
				(number "6")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "D1")
				(number "5")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "D2")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "D3")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "D4")
				(number "27")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "D5")
				(number "26")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "D6")
				(number "25")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "D7")
				(number "24")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "D8")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "~{W}")
				(number "1")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "~{FF}")
				(number "8")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "~{XI}")
				(number "7")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "~{FL}/~{RT}")
				(number "23")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "~{RS}")
				(number "22")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 3.81)
				(name "Q0")
				(number "9")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "Q1")
				(number "10")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "Q2")
				(number "11")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "Q3")
				(number "12")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "Q4")
				(number "16")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "Q5")
				(number "17")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "Q6")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "Q7")
				(number "19")
			)
			(pin output line
				(at 12.7 0 180)
				(length 3.81)
				(name "Q8")
				(number "13")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "~{R}")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "~{EF}")
				(number "21")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "~{HF}/~{XO}")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS42S16400J-xC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "IS42S16400J-xC"
			(at 8.89 34.29 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/42-45S16400J.pdf"
			(at -15.24 31.75 0)
		)
		(property "Description" "64Mb Synchronous DRAM, 1 Mb x 16 b x 4 Banks, Cu leadframe plated with matte Sn, TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "IS42S16400J-xC_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "BA0")
				(number "20")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "BA1")
				(number "21")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "A0")
				(number "23")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A1")
				(number "24")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A2")
				(number "25")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A3")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A4")
				(number "29")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A5")
				(number "30")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A6")
				(number "31")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A7")
				(number "32")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A8")
				(number "33")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A9")
				(number "34")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "22")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "35")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{CS}")
				(number "19")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CKE")
				(number "37")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "CLK")
				(number "38")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "LDQM")
				(number "15")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "UDQM")
				(number "39")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "~{WE}")
				(number "16")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{CAS}")
				(number "17")
			)
			(pin input line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{RAS}")
				(number "18")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDQ")
				(number "3")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "43")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "49")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GNDQ")
				(number "12")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GNDQ")
				(number "46")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GNDQ")
				(number "52")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GNDQ")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "DQ0")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "DQ1")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "DQ2")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "DQ3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "DQ4")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ5")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ6")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ7")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ8")
				(number "42")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ9")
				(number "44")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ10")
				(number "45")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ11")
				(number "47")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DQ12")
				(number "48")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DQ13")
				(number "50")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DQ14")
				(number "51")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DQ15")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS43LQ32256A-062BLI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 39.37 0)
		)
		(property "Value" "IS43LQ32256A-062BLI"
			(at 17.78 36.83 0)
		)
		(property "Footprint" "Package_BGA:BGA-200_10x14.5mm_Layout12x22_P0.8x0.65mm"
			(at 1.27 -48.26 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/43-46LQ32256A-AL.pdf"
			(at -2.54 -30.48 0)
		)
		(property "Description" "256Mx32 bit Low Power Double Data Rate 4 (LPDDR4) SDRAM, 1600 MHz, Industrial, BGA-200"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*10x14.5mm*Layout12x22*P0.8x0.65mm*"
			(at 0 0 0)
		)
		(symbol "IS43LQ32256A-062BLI_1_0")
		(symbol "IS43LQ32256A-062BLI_1_1"
			(pin input line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "CK_T_A")
				(number "J8")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "CK_C_A")
				(number "J9")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "CS0_A")
				(number "H4")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "CA0_A")
				(number "H2")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "CA1_A")
				(number "J2")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "CA2_A")
				(number "H9")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "CA3_A")
				(number "H10")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "CA4_A")
				(number "H11")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "CA5_A")
				(number "J11")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "CKE0_A")
				(number "J4")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "DQS0_T_A")
				(number "D3")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "DQS0_C_A")
				(number "E3")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "DQ0_A")
				(number "B2")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "DQ1_A")
				(number "C2")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "DQ2_A")
				(number "E2")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "DQ3_A")
				(number "F2")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "DQ4_A")
				(number "F4")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "DQ5_A")
				(number "E4")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "DQ6_A")
				(number "C4")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "DQ7_A")
				(number "B4")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "DMI0_A")
				(number "C3")
			)
			(pin no_connect line
				(at -15.24 22.86 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H3")
			)
			(pin no_connect line
				(at -15.24 20.32 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "K5")
			)
			(pin no_connect line
				(at -15.24 0 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "J5")
			)
			(pin no_connect line
				(at -15.24 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "K8")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 5.08)
				(name "VDD1")
				(number "F1")
			)
			(pin passive line
				(at -2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD1")
				(number "F12")
			)
			(pin passive line
				(at -2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD1")
				(number "G4")
			)
			(pin passive line
				(at -2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD1")
				(number "G9")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 5.08)
				(name "VDD2")
				(number "A4")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "A9")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "F5")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "F8")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "H1")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "H12")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "H5")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "H8")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "K1")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "K10")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "K12")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "K3")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "VSS")
				(number "A10")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C12")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C8")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D11")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E12")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J12")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K11")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K2")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K4")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 5.08)
				(name "VDDQ")
				(number "B10")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "B3")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "B5")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "B8")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "D1")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "D12")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "D5")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "D8")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "F10")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "F3")
			)
			(pin no_connect line
				(at 15.24 12.7 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "A1")
			)
			(pin no_connect line
				(at 15.24 10.16 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "A2")
			)
			(pin no_connect line
				(at 15.24 7.62 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "A11")
			)
			(pin no_connect line
				(at 15.24 5.08 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "A12")
			)
			(pin no_connect line
				(at 15.24 2.54 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "B1")
			)
			(pin no_connect line
				(at 15.24 0 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "B12")
			)
			(pin input line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "ODT_CA_A")
				(number "G2")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "DQS1_T_A")
				(number "D10")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "DQS1_C_A")
				(number "E10")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "DQ8_A")
				(number "B11")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "DQ9_A")
				(number "C11")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "DQ10_A")
				(number "E11")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "DQ11_A")
				(number "F11")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "DQ12_A")
				(number "F9")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "DQ13_A")
				(number "E9")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "DQ14_A")
				(number "C9")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "DQ15_A")
				(number "B9")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "DMI1_A")
				(number "C10")
			)
		)
		(symbol "IS43LQ32256A-062BLI_2_0")
		(symbol "IS43LQ32256A-062BLI_2_1"
			(pin input line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "CK_T_B")
				(number "P8")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "CK_C_B")
				(number "P9")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "CS0_B")
				(number "R4")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "CA0_B")
				(number "R2")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "CA1_B")
				(number "P2")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "CA2_B")
				(number "R9")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "CA3_B")
				(number "R10")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "CA4_B")
				(number "R11")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "CA5_B")
				(number "P11")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "CKE0_B")
				(number "P4")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "DQS0_T_B")
				(number "W3")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "DQS0_C_B")
				(number "V3")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "DQ0_B")
				(number "AA2")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "DQ1_B")
				(number "Y2")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "DQ2_B")
				(number "V2")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "DQ3_B")
				(number "U2")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "DQ4_B")
				(number "U4")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "DQ5_B")
				(number "V4")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "DQ6_B")
				(number "Y4")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "DQ7_B")
				(number "AA4")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "DMI0_B")
				(number "Y3")
			)
			(pin no_connect line
				(at -15.24 22.86 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "R3")
			)
			(pin no_connect line
				(at -15.24 20.32 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "N5")
			)
			(pin no_connect line
				(at -15.24 0 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "P5")
			)
			(pin no_connect line
				(at -15.24 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "N8")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 5.08)
				(name "VDD1")
				(number "T4")
			)
			(pin passive line
				(at -2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD1")
				(number "T9")
			)
			(pin passive line
				(at -2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD1")
				(number "U1")
			)
			(pin passive line
				(at -2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD1")
				(number "U12")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 5.08)
				(name "VDD2")
				(number "AB4")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "AB9")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "N1")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "N10")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "N12")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "N3")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "R1")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "R12")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "R5")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "R8")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "U5")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDD2")
				(number "U8")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "VSS")
				(number "AB10")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB8")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N11")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N2")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N4")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P10")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P12")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T10")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T12")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T8")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V12")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V8")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "W11")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "W2")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "W4")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "W9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "Y1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "Y12")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "Y5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "Y8")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 5.08)
				(name "VDDQ")
				(number "AA10")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "AA3")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "AA5")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "AA8")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "U10")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "U3")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "W1")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "W12")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "W5")
			)
			(pin passive line
				(at 2.54 38.1 270)
				(length 5.08)
				(hide yes)
				(name "VDDQ")
				(number "W8")
			)
			(pin no_connect line
				(at 15.24 22.86 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A8")
			)
			(pin no_connect line
				(at 15.24 20.32 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G11")
			)
			(pin no_connect line
				(at 15.24 12.7 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "AA1")
			)
			(pin no_connect line
				(at 15.24 10.16 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "AA12")
			)
			(pin no_connect line
				(at 15.24 7.62 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "AB1")
			)
			(pin no_connect line
				(at 15.24 5.08 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "AB2")
			)
			(pin no_connect line
				(at 15.24 2.54 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "AB11")
			)
			(pin no_connect line
				(at 15.24 0 180)
				(length 5.08)
				(hide yes)
				(name "DNU")
				(number "AB12")
			)
			(pin input line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "ODT_CA_B")
				(number "T2")
			)
			(pin input line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "RESET_N")
				(number "T11")
			)
			(pin input line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "ZQ0")
				(number "A5")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "DQS1_T_B")
				(number "W10")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "DQS1_C_B")
				(number "V10")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "DQ8_B")
				(number "AA11")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "DQ9_B")
				(number "Y11")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "DQ10_B")
				(number "V11")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "DQ11_B")
				(number "U11")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "DQ12_B")
				(number "U9")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "DQ13_B")
				(number "V9")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "DQ14_B")
				(number "Y9")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "DQ15_B")
				(number "AA9")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "DMI1_B")
				(number "Y10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS61C5128AL-10KLI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "IS61C5128AL-10KLI"
			(at 12.7 31.75 0)
		)
		(property "Footprint" "Package_SO:SOJ-36_10.16x23.495mm_P1.27mm"
			(at -12.7 29.21 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/61-64C5128AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "512K x 8 HIGH-SPEED CMOS STATIC RAM, 10ns, SOJ-36"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOJ*10.16*23.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IS61C5128AL-10KLI_0_1")
		(symbol "IS61C5128AL-10KLI_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "A5")
				(number "14")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A6")
				(number "15")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A7")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A8")
				(number "17")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A9")
				(number "18")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A10")
				(number "20")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "A11")
				(number "21")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A12")
				(number "22")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "A13")
				(number "23")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "A14")
				(number "24")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "A15")
				(number "32")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "A16")
				(number "33")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "A17")
				(number "34")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "A18")
				(number "35")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "~{CE}")
				(number "6")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "~{OE}")
				(number "31")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "~{WE}")
				(number "13")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin no_connect line
				(at 12.7 -25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 12.7 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "I/O0")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "I/O1")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "I/O2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "I/O3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "I/O4")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "I/O5")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "I/O6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "I/O7")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS61C5128AL-10TLI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "IS61C5128AL-10TLI"
			(at 12.7 31.75 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-44_10.16x18.41mm_P0.8mm"
			(at -12.7 29.21 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/61-64C5128AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "512K x 8 HIGH-SPEED CMOS STATIC RAM, 10ns, TSOP II-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*10.16*18.*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "IS61C5128AL-10TLI_0_1")
		(symbol "IS61C5128AL-10TLI_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "A0")
				(number "3")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "A3")
				(number "6")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "A4")
				(number "7")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "A5")
				(number "16")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A6")
				(number "17")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A7")
				(number "18")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A8")
				(number "19")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A9")
				(number "20")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A10")
				(number "26")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "A11")
				(number "27")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A12")
				(number "28")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "A13")
				(number "29")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "A14")
				(number "30")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "A15")
				(number "38")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "A16")
				(number "39")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "A17")
				(number "40")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "A18")
				(number "41")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "~{CE}")
				(number "8")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "~{OE}")
				(number "37")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "~{WE}")
				(number "15")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "44")
			)
			(pin no_connect line
				(at 12.7 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "43")
			)
			(pin no_connect line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin no_connect line
				(at 12.7 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at 12.7 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 12.7 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at 12.7 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at 12.7 -25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 12.7 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "I/O0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "I/O1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "I/O2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "I/O3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "I/O4")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "I/O5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "I/O6")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "I/O7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS61C5128AS-25HLI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "IS61C5128AS-25HLI"
			(at 12.7 31.75 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_11.8x8mm_P0.5mm"
			(at -12.7 29.21 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/61-64C5128AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "512K x 8 HIGH-SPEED CMOS STATIC RAM, 25ns, sTSOP I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*11.8*8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IS61C5128AS-25HLI_0_1")
		(symbol "IS61C5128AS-25HLI_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "A0")
				(number "20")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "A1")
				(number "19")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "A2")
				(number "18")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "A3")
				(number "17")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "A4")
				(number "16")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "A5")
				(number "15")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A6")
				(number "14")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A7")
				(number "13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A8")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A9")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A10")
				(number "31")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "A11")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A12")
				(number "12")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "A13")
				(number "4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "A14")
				(number "11")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "A15")
				(number "7")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "A16")
				(number "10")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "A17")
				(number "9")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "A18")
				(number "6")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "~{CE}")
				(number "30")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "~{OE}")
				(number "32")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "~{WE}")
				(number "5")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "I/O0")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "I/O1")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "I/O2")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "I/O3")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "I/O4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "I/O5")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "I/O6")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "I/O7")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS61C5128AS-25QLI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "IS61C5128AS-25QLI"
			(at 12.7 31.75 0)
		)
		(property "Footprint" "Package_SO:SOP-32_11.305x20.495mm_P1.27mm"
			(at -12.7 29.21 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/61-64C5128AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "512K x 8 HIGH-SPEED CMOS STATIC RAM, 25ns, SOP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*11.3*20.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IS61C5128AS-25QLI_0_1")
		(symbol "IS61C5128AS-25QLI_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "A14")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "A15")
				(number "31")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "A16")
				(number "2")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "A17")
				(number "1")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "A18")
				(number "30")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "~{CE}")
				(number "22")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "~{OE}")
				(number "24")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "~{WE}")
				(number "29")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "I/O0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "I/O1")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "I/O2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "I/O3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "I/O4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "I/O5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "I/O6")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "I/O7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS62C256AL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.144 21.844 0)
		)
		(property "Value" "IS62C256AL"
			(at 8.128 21.844 0)
		)
		(property "Footprint" "Package_SO:SOP-28_8.4x18.16mm_P1.27mm"
			(at -0.254 -64.008 0)
		)
		(property "Datasheet" "https://www.issi.com/WW/pdf/62-65C256AL.pdf"
			(at -0.254 -25.146 0)
		)
		(property "Description" "32Kx8 bit Low Power CMOS Static RAM, 25/45ns"
			(at 0.254 -28.194 0)
		)
		(property "ki_keywords" "SRAM MEMORY ISSI parallel-interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*8.4*18.16*P1.27*"
			(at 0 0 0)
		)
		(symbol "IS62C256AL_0_0"
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
		)
		(symbol "IS62C256AL_0_1")
		(symbol "IS62C256AL_1_0"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
		)
		(symbol "IS62C256AL_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A13")
				(number "26")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A14")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "I/O0")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "I/O1")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "I/O2")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "I/O3")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "I/O4")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "I/O5")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "I/O6")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "I/O7")
				(number "19")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{CE}")
				(number "20")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{WE}")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KM62256CLP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "KM62256CLP"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.futurlec.com/Datasheet/Memory/62256.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32Kx8 bit Low Power CMOS Static RAM, 55/70ns, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "RAM SRAM CMOS MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "KM62256CLP_0_0"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
		)
		(symbol "KM62256CLP_0_1")
		(symbol "KM62256CLP_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A13")
				(number "26")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A14")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "Q0")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "Q1")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "Q2")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "Q3")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "Q4")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "Q5")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Q6")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "Q7")
				(number "19")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{CS}")
				(number "20")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{WE}")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M48Tx2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0.254 0)
		)
		(property "Value" "M48Tx2"
			(at 0 0.254 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_18.0mmx34.29mm_W15.24mm"
			(at -1.27 0.254 0)
		)
		(property "Datasheet" "https://www.mouser.at/datasheet/2/389/m48t02-1849963.pdf"
			(at -1.27 0.254 0)
		)
		(property "Description" "5.0 V, 16 Kbit (2 Kb x 8) TIMEKEEPER® SRAM, DIP-24"
			(at -1.27 0.254 0)
		)
		(property "ki_keywords" "st M48T02 M48T12"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*18.0mmx34.29mm*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "M48Tx2_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A0")
				(number "8")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A1")
				(number "7")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "6")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A4")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A5")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A6")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A7")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A8")
				(number "23")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A9")
				(number "22")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A10")
				(number "19")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{W}")
				(number "21")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "~{E}")
				(number "18")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "~{G}")
				(number "20")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ0")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ1")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ2")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ3")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ4")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ5")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ6")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DQ7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MK4116N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "MK4116N"
			(at 5.08 13.716 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://deramp.com/downloads/mfe_archive/050-Component%20Specifications/Mostek/1980_Mostek_Memory_Data_Book_and_Designers_Guide.pdf#page=98"
			(at 0 -16.256 0)
		)
		(property "Description" "16384 x 1 bit Dynamic RAM, 150/200/250ns access time, VBB -5V, VCC 5V, VDD 12V, ±10% tolerance on all power supplies, TTL compatible inputs, DIP-16 (Epoxy/Plastic package)"
			(at 1.016 -18.288 0)
		)
		(property "ki_keywords" "DRAM NMOS 16Kbit MEMORY Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "MK4116N_0_0"
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "VBB")
				(number "1")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
		)
		(symbol "MK4116N_0_1")
		(symbol "MK4116N_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A1")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A2")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A5")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A6")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DOUT")
				(number "14")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{WRITE}")
				(number "3")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{CAS}")
				(number "15")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{RAS}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MK4164N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.256 0)
		)
		(property "Value" "MK4164N"
			(at 2.54 16.256 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -20.828 0)
		)
		(property "Datasheet" "https://deramp.com/downloads/mfe_archive/050-Component%20Specifications/Mostek/1980_Mostek_Memory_Data_Book_and_Designers_Guide.pdf#page=134"
			(at 0 -16.764 0)
		)
		(property "Description" "65536 x 1 bit Dynamic RAM, 120/150ns access time, single 5V ±10% power supply, TTL compatible inputs, DIP-16 (Epoxy/Plastic package)"
			(at 1.016 -18.796 0)
		)
		(property "ki_keywords" "DRAM NMOS 64Kbit MEMORY Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "MK4164N_0_0"
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A7")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{RFSH}")
				(number "1")
			)
		)
		(symbol "MK4164N_0_1")
		(symbol "MK4164N_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A1")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A2")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A3")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DOUT")
				(number "14")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{WRITE}")
				(number "3")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{CAS}")
				(number "15")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{RAS}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MT48LC16M16A2TG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MT48LC16M16A2TG"
			(at 8.89 34.29 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.micron.com/-/media/client/global/documents/products/data-sheet/dram/256mb_sdr.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "256M – (16M x 16 bit) Synchronous DRAM (SDRAM), TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDRAM Synchronous DRAM PC100 PC133 256Mb 16Mbx16 MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MT48LC16M16A2TG_0_1")
		(symbol "MT48LC16M16A2TG_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "BA0")
				(number "20")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "BA1")
				(number "21")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "A0")
				(number "23")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A1")
				(number "24")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A2")
				(number "25")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A3")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A4")
				(number "29")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A5")
				(number "30")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A6")
				(number "31")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A7")
				(number "32")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A8")
				(number "33")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A9")
				(number "34")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "22")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "35")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "36")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{CS}")
				(number "19")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CKE")
				(number "37")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "CLK")
				(number "38")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "DQML")
				(number "15")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "DQMH")
				(number "39")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "~{WE}")
				(number "16")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{CAS}")
				(number "17")
			)
			(pin input line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{RAS}")
				(number "18")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "28")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "54")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDQ")
				(number "3")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "43")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "49")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "12")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "46")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "52")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSSQ")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "DQ0")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "DQ1")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "DQ2")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "DQ3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "DQ4")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ5")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ6")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ7")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DQ8")
				(number "42")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DQ9")
				(number "44")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DQ10")
				(number "45")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DQ11")
				(number "47")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DQ12")
				(number "48")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DQ13")
				(number "50")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DQ14")
				(number "51")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DQ15")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MT48LC32M8A2TG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MT48LC32M8A2TG"
			(at 8.89 34.29 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.micron.com/-/media/client/global/documents/products/data-sheet/dram/256mb_sdr.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "256M – (32M x 8 bit) Synchronous DRAM (SDRAM), TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDRAM Synchronous DRAM PC100 PC133 256Mb 32Mbx8 MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MT48LC32M8A2TG_0_1")
		(symbol "MT48LC32M8A2TG_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "BA0")
				(number "20")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "BA1")
				(number "21")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "A0")
				(number "23")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A1")
				(number "24")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A2")
				(number "25")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A3")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A4")
				(number "29")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A5")
				(number "30")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A6")
				(number "31")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A7")
				(number "32")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A8")
				(number "33")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A9")
				(number "34")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "22")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "35")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "36")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{CS}")
				(number "19")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CKE")
				(number "37")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "CLK")
				(number "38")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "DQM")
				(number "39")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "~{WE}")
				(number "16")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{CAS}")
				(number "17")
			)
			(pin input line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{RAS}")
				(number "18")
			)
			(pin no_connect line
				(at -10.16 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "28")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "54")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDQ")
				(number "3")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "43")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "49")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "12")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "46")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "52")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSSQ")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "45")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "48")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "51")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "DQ0")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "DQ1")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "DQ2")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "DQ3")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "DQ4")
				(number "44")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DQ5")
				(number "47")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DQ6")
				(number "50")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DQ7")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MT48LC64M4A2TG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MT48LC64M4A2TG"
			(at 8.89 34.29 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.micron.com/-/media/client/global/documents/products/data-sheet/dram/256mb_sdr.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "256M – (64M x 4 bit) Synchronous DRAM (SDRAM), TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDRAM Synchronous DRAM PC100 PC133 256Mb 64Mbx4 MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MT48LC64M4A2TG_0_1")
		(symbol "MT48LC64M4A2TG_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "BA0")
				(number "20")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "BA1")
				(number "21")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "A0")
				(number "23")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A1")
				(number "24")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A2")
				(number "25")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A3")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A4")
				(number "29")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A5")
				(number "30")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A6")
				(number "31")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A7")
				(number "32")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A8")
				(number "33")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A9")
				(number "34")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A10")
				(number "22")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "35")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "36")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{CS}")
				(number "19")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CKE")
				(number "37")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "CLK")
				(number "38")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "DQM")
				(number "39")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "~{WE}")
				(number "16")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{CAS}")
				(number "17")
			)
			(pin input line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{RAS}")
				(number "18")
			)
			(pin no_connect line
				(at -10.16 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "28")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "54")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDQ")
				(number "3")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "43")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "49")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "12")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "46")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "52")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSSQ")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "53")
			)
			(pin no_connect line
				(at 10.16 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "47")
			)
			(pin no_connect line
				(at 10.16 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "45")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "48")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "51")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "DQ0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "DQ1")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "DQ2")
				(number "44")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "DQ3")
				(number "50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "W9812G6KH-5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "W9812G6KH-5"
			(at -10.16 -33.02 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/da00-w9812g6khc1.pdf"
			(at -10.16 31.75 0)
		)
		(property "Description" "128Mb Synchronous DRAM, 2 Mb x 16 b x 4 Banks, 200 MHz, TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "W9812G6KH-5_1_1"
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "BS0")
				(number "20")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "BS1")
				(number "21")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "A0")
				(number "23")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A1")
				(number "24")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A2")
				(number "25")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A3")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A4")
				(number "29")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A5")
				(number "30")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A6")
				(number "31")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A7")
				(number "32")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A8")
				(number "33")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A9")
				(number "34")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A10/AP")
				(number "22")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A11")
				(number "35")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "19")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "CKE")
				(number "37")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CLK")
				(number "38")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "LDQM")
				(number "15")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "UDQM")
				(number "39")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "~{WE}")
				(number "16")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "~{CAS}")
				(number "17")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{RAS}")
				(number "18")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDDQ")
				(number "3")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "43")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "49")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDDQ")
				(number "9")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "12")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "46")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSSQ")
				(number "52")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "VSSQ")
				(number "6")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 2.54 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at 2.54 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "VSS")
				(number "28")
			)
			(pin passive line
				(at 2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin passive line
				(at 2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "54")
			)
			(pin no_connect line
				(at 12.7 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 12.7 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "DQ0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "DQ1")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "DQ2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "DQ3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "DQ4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "DQ5")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "DQ6")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DQ7")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DQ8")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DQ9")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DQ10")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "DQ11")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DQ12")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DQ13")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DQ14")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DQ15")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS6C1008-xxS"
		(extends "AS6C1008-xxP")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS6C1008-xxS"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:SOP-32_11.305x20.495mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/AS6C1008_Mar_2023V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit (128K X 8-bit) Low Power CMOS SRAM, single 2.7V ~ 5.5V power supply, 55ns, SOP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Static MEMORY 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOP*11.3*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS6C1008-xxST"
		(extends "AS6C1008-xxT")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS6C1008-xxST"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_11.8x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/AS6C1008_Mar_2023V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit (128K X 8-bit) Low Power CMOS SRAM, single 2.7V ~ 5.5V power supply, 55ns, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Static MEMORY 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*11.8*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7C1024B-xxJ"
		(extends "HM628128_DIP32_SOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS7C1024B-xxJ"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:SOJ-32_10.16x20.955mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/sram/fa/AS7C1024B_March2022_v3.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 1-Mbit (128K x 8-bit) FAST Asynchronous SRAM, 10/12/15/20ns, SOJ-32 (400 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MEMORY Static 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOJ*10.1*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7C1024B-xxT"
		(extends "HM628128_TSOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS7C1024B-xxT"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_18.4x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/sram/fa/AS7C1024B_March2022_v3.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 1-Mbit (128K x 8-bit) FAST Asynchronous SRAM, 10/12/15/20ns, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MEMORY Static 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*18.4*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7C31024B-xxJ"
		(extends "HM628128_DIP32_SOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS7C31024B-xxJ"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:SOJ-32_10.16x20.955mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/sram/fa/AS7C31024B.V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 1-Mbit (128K X 8-bit) CMOS SRAM, 10/12/15/20ns, SOJ-32 (400 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Static MEMORY 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOJ*10.1*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7C31024B-xxT"
		(extends "HM628128_TSOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS7C31024B-xxT"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_18.4x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/sram/fa/AS7C31024B.V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 1-Mbit (128K X 8-bit) CMOS SRAM, 10/12/15/20ns, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "MEMORY Static 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*18.4*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY62128EV30xx-xxS"
		(extends "HM628128_DIP32_SOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "CY62128EV30xx-xxS"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:SOP-32_11.305x20.495mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY62128EV30_MoBL_1_Mbit_(128K_X_8)_Static_RAM-DataSheet-v17_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ebe867f322f"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit (128K x 8-bit) Static RAM, VCC = 2.2..3.6V, 45ns, SOIC-32 (SOP-32)"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MEMORY SRAM 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOP*11.*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY62128EV30xx-xxZ"
		(extends "HM628128_TSOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "CY62128EV30xx-xxZ"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_18.4x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY62128EV30_MoBL_1_Mbit_(128K_X_8)_Static_RAM-DataSheet-v17_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ebe867f322f"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit (128K x 8-bit) Static RAM, VCC = 2.2..3.6V, 45ns, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MEMORY SRAM 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*18.4*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY62128Exx-xxS"
		(extends "HM628128_DIP32_SOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "CY62128Exx-xxS"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:SOP-32_11.305x20.495mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY62128E_MoBL_1-Mbit_(128_K_8)_Static_RAM-DataSheet-v17_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ebe7dc7321d"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit (128K x 8-bit) Static RAM, VCC = 4.5..5.5V, 45/55ns, SOIC-32 (SOP-32)"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MEMORY SRAM 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOP*11.*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY62128Exx-xxZ"
		(extends "HM628128_TSOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "CY62128Exx-xxZ"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_18.4x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-CY62128E_MoBL_1-Mbit_(128_K_8)_Static_RAM-DataSheet-v17_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ebe7dc7321d"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit (128K x 8-bit) Static RAM, VCC = 4.5..5.5V, 45/55ns, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MEMORY SRAM 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*18.4*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY62256-70PC"
		(extends "KM62256CLP")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "CY62256-70PC"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://ecee.colorado.edu/~mcclurel/Cypress_SRAM_CY62256.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "256K (32K x 8) Static RAM, 70ns, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "RAM SRAM CMOS MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "HM62256BLP"
		(extends "KM62256CLP")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "HM62256BLP"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://web.mit.edu/6.115/www/document/62256.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32,768-word × 8-bit High Speed CMOS Static RAM, 70ns, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "RAM SRAM CMOS MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "HM628128D_DIP32_SOP32"
		(extends "HM628128_DIP32_SOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "HM628128D_DIP32_SOP32"
			(at 2.54 23.495 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.futurlec.com/Datasheet/Memory/628128.pdf"
			(at 0 0 0)
		)
		(property "Description" "128K-word x 8-bit High-Speed CMOS Static RAM, 55/70ns, 5V supply, DIP-32/SOP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY 1Mbit Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W15.24mm* *SOP*11.*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HM628128D_TSOP32"
		(extends "HM628128_TSOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "HM628128D_TSOP32"
			(at 2.54 23.495 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.futurlec.com/Datasheet/Memory/628128.pdf"
			(at 0 0 0)
		)
		(property "Description" "128K-word x 8-bit High-Speed CMOS Static RAM, 55/70ns, 5V supply, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY 1Mbit Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*11.8*8*P0.5mm* *TSOP?I*18.4*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "HY6264AxJ"
		(extends "HY6264AxP")
		(property "Reference" "U"
			(at -10.16 20.955 0)
		)
		(property "Value" "HY6264AxJ"
			(at 2.54 20.955 0)
		)
		(property "Footprint" "Package_SO:SOP-28_8.4x18.16mm_P1.27mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.farnell.com/datasheets/2159.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Not in Production, 8Kx8 bit Static RAM, 70/85/100/120/150ns, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "HYUNDAI SRAM CMOS MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOP*8.4x18.16mm*P1.27*"
			(at 0 0 0)
		)
	)
	(symbol "IDT7202"
		(extends "IDT7201")
		(property "Reference" "U"
			(at -8.89 20.32 0)
		)
		(property "Value" "IDT7202"
			(at 6.35 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "IDT7203"
		(extends "IDT7204")
		(property "Reference" "U"
			(at -8.89 25.4 0)
		)
		(property "Value" "IDT7203"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 30.48 0)
		)
		(property "Datasheet" "http://www.idt.com/document/7203-7208-datasheet"
			(at 0 0 0)
		)
		(property "Description" "2048x9 CMOS Asynchronous FIFO, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "asynchronous fifo memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IDT7205"
		(extends "IDT7204")
		(property "Reference" "U"
			(at -8.89 25.4 0)
		)
		(property "Value" "IDT7205"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 30.48 0)
		)
		(property "Datasheet" "http://www.idt.com/document/7203-7208-datasheet"
			(at 0 0 0)
		)
		(property "Description" "8192x9 CMOS Asynchronous FIFO, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "asynchronous fifo memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IDT7206"
		(extends "IDT7204")
		(property "Reference" "U"
			(at -8.89 25.4 0)
		)
		(property "Value" "IDT7206"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 30.48 0)
		)
		(property "Datasheet" "http://www.idt.com/document/7203-7208-datasheet"
			(at 0 0 0)
		)
		(property "Description" "16384x9 CMOS Asynchronous FIFO, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "asynchronous fifo memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IDT7207"
		(extends "IDT7204")
		(property "Reference" "U"
			(at -8.89 25.4 0)
		)
		(property "Value" "IDT7207"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 30.48 0)
		)
		(property "Datasheet" "http://www.idt.com/document/7203-7208-datasheet"
			(at 0 0 0)
		)
		(property "Description" "32768x9 CMOS Asynchronous FIFO, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "asynchronous fifo memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IDT7208"
		(extends "IDT7204")
		(property "Reference" "U"
			(at -8.89 25.4 0)
		)
		(property "Value" "IDT7208"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 30.48 0)
		)
		(property "Datasheet" "http://www.idt.com/document/7203-7208-datasheet"
			(at 0 0 0)
		)
		(property "Description" "65536x9 CMOS Asynchronous FIFO, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "asynchronous fifo memory"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS42S16400J-xT"
		(extends "IS42S16400J-xC")
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "IS42S16400J-xT"
			(at 8.89 34.29 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/42-45S16400J.pdf"
			(at -15.24 31.75 0)
		)
		(property "Description" "64Mb Synchronous DRAM, 1 Mb x 16 b x 4 Banks, Alloy42 leadframe plated with matte Sn, TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS43LQ32256AL-062BLI"
		(extends "IS43LQ32256A-062BLI")
		(property "Reference" "U"
			(at 7.62 39.37 0)
		)
		(property "Value" "IS43LQ32256AL-062BLI"
			(at 17.78 36.83 0)
		)
		(property "Footprint" "Package_BGA:BGA-200_10x14.5mm_Layout12x22_P0.8x0.65mm"
			(at 1.27 -48.26 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/43-46LQ32256AL-AL.pdf"
			(at -2.54 -30.48 0)
		)
		(property "Description" "256Mx32 bit Low Power Double Data Rate 4X (LPDDR4X) SDRAM, 1600 MHz, Industrial, BGA-200"
			(at 0 0 0)
		)
		(property "ki_keywords" "DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*10x14.5mm*Layout12x22*P0.8x0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS61C5128AS-25TLI"
		(extends "IS61C5128AS-25QLI")
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "IS61C5128AS-25TLI"
			(at 12.7 31.75 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-32_21.0x10.2mm_P1.27mm"
			(at -12.7 29.21 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/61-64C5128AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "512K x 8 HIGH-SPEED CMOS STATIC RAM, 25ns, TSOP II-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*21.0*10.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS64C5128AL-12CTLA3"
		(extends "IS61C5128AL-10TLI")
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "IS64C5128AL-12CTLA3"
			(at 12.7 31.75 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-44_10.16x18.41mm_P0.8mm"
			(at -12.7 29.21 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/61-64C5128AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "512K x 8 HIGH-SPEED CMOS STATIC RAM, 12ns, TSOP II-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*10.16*18.*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS64C5128AL-12KLA3"
		(extends "IS61C5128AL-10KLI")
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "IS64C5128AL-12KLA3"
			(at 12.7 31.75 0)
		)
		(property "Footprint" "Package_SO:SOJ-36_10.16x23.495mm_P1.27mm"
			(at -12.7 29.21 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/61-64C5128AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "512K x 8 HIGH-SPEED CMOS STATIC RAM, 12ns, SOJ-36"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOJ*10.16*23.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS65C256AL"
		(extends "IS62C256AL")
		(property "Reference" "U"
			(at -9.144 21.844 0)
		)
		(property "Value" "IS65C256AL"
			(at 8.128 21.844 0)
		)
		(property "Footprint" "Package_SO:SOP-28_8.4x18.16mm_P1.27mm"
			(at -0.254 -64.008 0)
		)
		(property "Datasheet" "https://www.issi.com/WW/pdf/62-65C256AL.pdf"
			(at -0.254 -25.146 0)
		)
		(property "Description" "32Kx8 bit Low Power CMOS Static RAM, 25/45ns, Automotive"
			(at 0.254 -28.194 0)
		)
		(property "ki_keywords" "SRAM MEMORY ISSI parallel-interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*8.4*18.16*P1.27*"
			(at 0 0 0)
		)
	)
	(symbol "IS6xC1024AL-xxJ"
		(extends "HM628128_DIP32_SOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "IS6xC1024AL-xxJ"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:SOJ-32_7.62x20.955mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/74798/0/0/1/IS6xC1024AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "128K x 8-bit High-Speed CMOS Static RAM, IS61C1024AL (commercial and industrial) / IS64C1024AL (automotive), VDD = 5V ±10%, 12/15ns, SOJ-32 (300 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY 1Mbit Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOJ*7.6*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS6xC1024AL-xxT"
		(extends "HM628128_TSOP32")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "IS6xC1024AL-xxT"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_18.4x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.issi.com/WW/pdf/61-64C1024AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "128K x 8-bit High-Speed CMOS Static RAM, IS61C1024AL (commercial and industrial) / IS64C1024AL (automotive), VDD = 5V ±10%, 12/15ns, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*18.4*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "M48Zx2"
		(extends "M48Tx2")
		(property "Reference" "U"
			(at 0 0.254 0)
		)
		(property "Value" "M48Zx2"
			(at 0 0.254 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_18.0mmx34.29mm_W15.24mm"
			(at 0 0.254 0)
		)
		(property "Datasheet" "https://www.mouser.at/datasheet/2/389/m48z02-1849661.pdf"
			(at 0 0.254 0)
		)
		(property "Description" "5 V, 16 kbit (2 Kb x 8) ZEROPOWER® SRAM, DIP-24"
			(at 0 0.254 0)
		)
		(property "ki_keywords" "st M48Z02 M48Z12"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*18.0mmx34.29mm*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MT48LC16M16A2P"
		(extends "MT48LC16M16A2TG")
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MT48LC16M16A2P"
			(at 8.89 34.29 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.micron.com/-/media/client/global/documents/products/data-sheet/dram/256mb_sdr.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "256M – (16M x 16 bit) Synchronous DRAM (SDRAM), TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDRAM Synchronous DRAM PC100 PC133 256Mb 16Mbx16 MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MT48LC32M8A2P"
		(extends "MT48LC32M8A2TG")
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MT48LC32M8A2P"
			(at 8.89 34.29 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.micron.com/-/media/client/global/documents/products/data-sheet/dram/256mb_sdr.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "256M – (32M x 8 bit) Synchronous DRAM (SDRAM), TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDRAM Synchronous DRAM PC100 PC133 256Mb 32Mbx8 MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MT48LC64M4A2P"
		(extends "MT48LC64M4A2TG")
		(property "Reference" "U"
			(at -8.89 34.29 0)
		)
		(property "Value" "MT48LC64M4A2P"
			(at 8.89 34.29 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.micron.com/-/media/client/global/documents/products/data-sheet/dram/256mb_sdr.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "256M – (64M x 4 bit) Synchronous DRAM (SDRAM), TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDRAM Synchronous DRAM PC100 PC133 256Mb 64Mbx4 MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "R1LP0108ESF"
		(extends "AS6C1008-xxT")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "R1LP0108ESF"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_18.4x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.renesas.com/en/document/dst/r1lp0108e-series-datasheet"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit Advanced Low Power SRAM (128K x 8-bit), operating voltage 5V, 55/70ns, TSOP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MEMORY Static 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*18.4*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "R1LP0108ESN"
		(extends "AS6C1008-xxP")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "R1LP0108ESN"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:Renesas_SOP-32_11.4x20.75mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.renesas.com/en/document/dst/r1lp0108e-series-datasheet"
			(at 0 0 0)
		)
		(property "Description" "1-Mbit Advanced Low Power SRAM (128K x 8-bit), operating voltage 5V, 55/70ns, SOP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MEMORY Static 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOP*11.4*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "W9812G6KH-6"
		(extends "W9812G6KH-5")
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "W9812G6KH-6"
			(at -10.16 -33.02 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/da00-w9812g6khc1.pdf"
			(at -10.16 31.75 0)
		)
		(property "Description" "128Mb Synchronous DRAM, 2 Mb x 16 b x 4 Banks, 166 MHz, TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "W9812G6KH-6I"
		(extends "W9812G6KH-5")
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "W9812G6KH-6I"
			(at -10.16 -33.02 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/da00-w9812g6khc1.pdf"
			(at -10.16 31.75 0)
		)
		(property "Description" "128Mb Synchronous DRAM, 2 Mb x 16 b x 4 Banks, 166 MHz, TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "W9812G6KH-75"
		(extends "W9812G6KH-5")
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "W9812G6KH-75"
			(at -10.16 -33.02 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/da00-w9812g6khc1.pdf"
			(at -10.16 31.75 0)
		)
		(property "Description" "128Mb Synchronous DRAM, 2 Mb x 16 b x 4 Banks, 133 MHz, TSOP-II-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "DRAM MEMORY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP?II*22.2x10.16mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7C1024B-xxTJ"
		(extends "AS7C1024B-xxJ")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS7C1024B-xxTJ"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:SOJ-32_7.62x20.955mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/sram/fa/AS7C1024B_March2022_v3.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 1-Mbit (128K x 8-bit) FAST Asynchronous SRAM, 10/12/15/20ns, SOJ-32 (300 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS MEMORY Static 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOJ*7.6*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7C31024B-xxST"
		(extends "AS7C31024B-xxT")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS7C31024B-xxST"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_11.8x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/sram/fa/AS7C31024B.V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 1-Mbit (128K X 8-bit) CMOS SRAM, 10/12/15/20ns, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "MEMORY Static 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*11.8*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7C31024B-xxTJ"
		(extends "AS7C31024B-xxJ")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "AS7C31024B-xxTJ"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:SOJ-32_7.62x20.955mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/sram/fa/AS7C31024B.V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 1-Mbit (128K X 8-bit) CMOS SRAM, 10/12/15/20ns, SOJ-32 (300 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Static MEMORY 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOJ*7.6*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS6xC1024AL-xxH"
		(extends "IS6xC1024AL-xxT")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "IS6xC1024AL-xxH"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:TSOP-I-32_11.8x8mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.issi.com/WW/pdf/61-64C1024AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "128K x 8-bit High-Speed CMOS Static RAM, IS61C1024AL (commercial and industrial) / IS64C1024AL (automotive), VDD = 5V ±10%, 12/15ns, TSOP-I-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY 1Mbit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOP?I*11.8*8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS6xC1024AL-xxK"
		(extends "IS6xC1024AL-xxJ")
		(property "Reference" "U"
			(at -10.16 23.495 0)
		)
		(property "Value" "IS6xC1024AL-xxK"
			(at 2.54 23.495 0)
		)
		(property "Footprint" "Package_SO:SOJ-32_10.16x20.955mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/74798/0/0/1/IS6xC1024AL.pdf"
			(at 0 0 0)
		)
		(property "Description" "128K x 8-bit High-Speed CMOS Static RAM, IS61C1024AL (commercial and industrial) / IS64C1024AL (automotive), VDD = 5V ±10%, 12/15ns, SOJ-32 (400 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SRAM MEMORY 1Mbit Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOJ*10.1*20.*P1.27mm*"
			(at 0 0 0)
		)
	)
)
