(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "XC18V01SO20"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.8392 15.24 0)
		)
		(property "Value" "XC18V01SO20"
			(at 1.27 -15.1892 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/xc18v00proms.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC18V01SO20_0_1")
		(symbol "XC18V01SO20_1_1"
			(pin input line
				(at -17.78 12.7 0)
				(length 7.62)
				(name "TMS")
				(number "5")
			)
			(pin input clock
				(at -17.78 10.16 0)
				(length 7.62)
				(name "TCK")
				(number "6")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 7.62)
				(name "TDI")
				(number "4")
			)
			(pin open_collector line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "TDO")
				(number "17")
			)
			(pin input line
				(at -17.78 1.27 0)
				(length 7.62)
				(name "OE/RESET")
				(number "8")
			)
			(pin input line
				(at -17.78 -1.27 0)
				(length 7.62)
				(name "CE")
				(number "10")
			)
			(pin output line
				(at -17.78 -3.81 0)
				(length 7.62)
				(name "CEO")
				(number "13")
			)
			(pin input clock
				(at -17.78 -6.35 0)
				(length 7.62)
				(name "CLK")
				(number "3")
			)
			(pin power_in line
				(at -17.78 -10.16 0)
				(length 7.62)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at -17.78 -12.7 0)
				(length 7.62)
				(name "VCC")
				(number "20")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 7.62)
				(name "D0")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 7.62)
				(name "D1")
				(number "16")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 7.62)
				(name "D2")
				(number "2")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 7.62)
				(name "D3")
				(number "15")
			)
			(pin open_collector line
				(at 17.78 2.54 180)
				(length 7.62)
				(name "D4/CF")
				(number "7")
			)
			(pin output line
				(at 17.78 0 180)
				(length 7.62)
				(name "D5")
				(number "14")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 7.62)
				(name "D6")
				(number "9")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 7.62)
				(name "D7")
				(number "12")
			)
			(pin power_in line
				(at 17.78 -10.16 180)
				(length 7.62)
				(name "VCCO")
				(number "19")
			)
			(pin power_in line
				(at 17.78 -12.7 180)
				(length 7.62)
				(name "GND")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XCF08P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 33.02 0)
		)
		(property "Value" "XCF08P"
			(at 0 -33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds123.pdf"
			(at 0 0 0)
		)
		(property "Description" "Platform Flash In-System PROM"
			(at 0 0 0)
		)
		(property "ki_keywords" "PROM FLASH"
			(at 0 0 0)
		)
		(symbol "XCF08P_0_1")
		(symbol "XCF08P_1_1"
			(pin input line
				(at -16.51 30.48 0)
				(length 7.62)
				(name "TCK")
				(number "H3")
			)
			(pin input line
				(at -16.51 27.94 0)
				(length 7.62)
				(name "TMS")
				(number "E2")
			)
			(pin input line
				(at -16.51 25.4 0)
				(length 7.62)
				(name "TDI")
				(number "G1")
			)
			(pin output line
				(at -16.51 22.86 0)
				(length 7.62)
				(name "TDO")
				(number "E6")
			)
			(pin input line
				(at -16.51 17.78 0)
				(length 7.62)
				(name "BUSY")
				(number "C1")
			)
			(pin input line
				(at -16.51 15.24 0)
				(length 7.62)
				(name "OE/RST")
				(number "A3")
			)
			(pin input line
				(at -16.51 10.16 0)
				(length 7.62)
				(name "REV-SEL0")
				(number "G3")
			)
			(pin input line
				(at -16.51 7.62 0)
				(length 7.62)
				(name "REV-SEL1")
				(number "G4")
			)
			(pin input line
				(at -16.51 5.08 0)
				(length 7.62)
				(name "/EN-EXT-SEL")
				(number "H4")
			)
			(pin input clock
				(at -16.51 0 0)
				(length 7.62)
				(name "CLK")
				(number "B3")
			)
			(pin input input_low
				(at -16.51 -2.54 0)
				(length 7.62)
				(name "CE")
				(number "B4")
			)
			(pin bidirectional input_low
				(at -16.51 -5.08 0)
				(length 7.62)
				(name "CF")
				(number "D1")
			)
			(pin power_in line
				(at -16.51 -10.16 0)
				(length 7.62)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -16.51 -12.7 0)
				(length 7.62)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -16.51 -15.24 0)
				(length 7.62)
				(name "GND")
				(number "B6")
			)
			(pin power_in line
				(at -16.51 -17.78 0)
				(length 7.62)
				(name "GND")
				(number "F1")
			)
			(pin power_in line
				(at -16.51 -20.32 0)
				(length 7.62)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at -16.51 -22.86 0)
				(length 7.62)
				(name "GND")
				(number "F6")
			)
			(pin power_in line
				(at -16.51 -25.4 0)
				(length 7.62)
				(name "GND")
				(number "H1")
			)
			(pin tri_state line
				(at 16.51 30.48 180)
				(length 7.62)
				(name "D0")
				(number "H6")
			)
			(pin tri_state line
				(at 16.51 27.94 180)
				(length 7.62)
				(name "D1")
				(number "H5")
			)
			(pin tri_state line
				(at 16.51 25.4 180)
				(length 7.62)
				(name "D2")
				(number "E5")
			)
			(pin tri_state line
				(at 16.51 22.86 180)
				(length 7.62)
				(name "D3")
				(number "D5")
			)
			(pin tri_state line
				(at 16.51 20.32 180)
				(length 7.62)
				(name "D4")
				(number "C5")
			)
			(pin tri_state line
				(at 16.51 17.78 180)
				(length 7.62)
				(name "D5")
				(number "B5")
			)
			(pin tri_state line
				(at 16.51 15.24 180)
				(length 7.62)
				(name "D6")
				(number "A5")
			)
			(pin tri_state line
				(at 16.51 12.7 180)
				(length 7.62)
				(name "D7")
				(number "A6")
			)
			(pin output clock
				(at 16.51 0 180)
				(length 7.62)
				(name "CLKOUT")
				(number "C2")
			)
			(pin output output_low
				(at 16.51 -2.54 180)
				(length 7.62)
				(name "CEO")
				(number "D2")
			)
			(pin power_in line
				(at 16.51 -10.16 180)
				(length 7.62)
				(name "VCCINT")
				(number "B1")
			)
			(pin power_in line
				(at 16.51 -12.7 180)
				(length 7.62)
				(name "VCCINT")
				(number "E1")
			)
			(pin power_in line
				(at 16.51 -15.24 180)
				(length 7.62)
				(name "VCCINT")
				(number "G6")
			)
			(pin power_in line
				(at 16.51 -19.05 180)
				(length 7.62)
				(name "VCCO")
				(number "B2")
			)
			(pin power_in line
				(at 16.51 -21.59 180)
				(length 7.62)
				(name "VCCO")
				(number "C6")
			)
			(pin power_in line
				(at 16.51 -24.13 180)
				(length 7.62)
				(name "VCCO")
				(number "G5")
			)
			(pin power_in line
				(at 16.51 -26.67 180)
				(length 7.62)
				(name "VCCO")
				(number "D6")
			)
			(pin power_in line
				(at 16.51 -30.48 180)
				(length 7.62)
				(name "VCCJ")
				(number "H2")
			)
		)
		(embedded_fonts no)
	)
)
