(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "Fan"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 2.54 5.08 0)
		)
		(property "Value" "Fan"
			(at 2.54 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0.254 0)
		)
		(property "Datasheet" "~"
			(at 0 0.254 0)
		)
		(property "Description" "Fan"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fan Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Fan_0_1")
		(symbol "Fan_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Fan_ALT"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 3.81 5.08 0)
		)
		(property "Value" "Fan_ALT"
			(at 3.81 2.54 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 -1.27 0)
		)
		(property "Description" "Fan without PWM or tach, alternative symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fan Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Fan_ALT_0_1")
		(symbol "Fan_ALT_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Fan_IEC-60617"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 3.81 3.81 0)
		)
		(property "Value" "Fan_IEC-60617"
			(at 3.81 2.54 0)
		)
		(property "Footprint" ""
			(at 1.27 -3.556 0)
		)
		(property "Datasheet" "~"
			(at 0 0.254 0)
		)
		(property "Description" "Fan according to IEC 60617"
			(at 0 0 0)
		)
		(property "ki_keywords" "fan motor iec 60617"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Fan_IEC-60617_0_1")
		(symbol "Fan_IEC-60617_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Fan_ISO-14617"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 3.81 3.81 0)
		)
		(property "Value" "Fan_ISO-14617"
			(at 3.81 2.54 0)
		)
		(property "Footprint" ""
			(at 1.27 -3.556 0)
		)
		(property "Datasheet" "~"
			(at 0 0.254 0)
		)
		(property "Description" "Fan 2302 according to ISO 14617"
			(at 0 0 0)
		)
		(property "ki_keywords" "fan motor iso 14617"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Fan_ISO-14617_0_1")
		(symbol "Fan_ISO-14617_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Fan_Tacho"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 2.54 2.54 0)
		)
		(property "Value" "Fan_Tacho"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 -2.286 0)
		)
		(property "Datasheet" "http://www.hardwarecanucks.com/forum/attachments/new-builds/16287d1330775095-help-chassis-power-fan-connectors-motherboard-asus_p8z68.jpg"
			(at 0 -2.286 0)
		)
		(property "Description" "Fan, tacho output, 3-pin connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fan Motor tacho"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "FanPinHeader*P2.54mm*Vertical* PinHeader*P2.54mm*Vertical* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Fan_Tacho_0_0")
		(symbol "Fan_Tacho_0_1")
		(symbol "Fan_Tacho_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "Tacho")
				(number "3")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "-")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Fan_Tacho_PWM"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 2.54 5.08 0)
		)
		(property "Value" "Fan_Tacho_PWM"
			(at 2.54 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0.254 0)
		)
		(property "Datasheet" "http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf"
			(at 0 0.254 0)
		)
		(property "Description" "Fan, tacho output, PWM input, 4-pin connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fan Motor tacho PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "FanPinHeader*P2.54mm*Vertical* PinHeader*P2.54mm*Vertical* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Fan_Tacho_PWM_0_0")
		(symbol "Fan_Tacho_PWM_0_1")
		(symbol "Fan_Tacho_PWM_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Tacho")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "PWM")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "-")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Motor_AC"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 2.54 2.54 0)
		)
		(property "Value" "Motor_AC"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 -2.286 0)
		)
		(property "Datasheet" "~"
			(at 0 -2.286 0)
		)
		(property "Description" "AC Motor"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Motor_AC_0_0")
		(symbol "Motor_AC_0_1")
		(symbol "Motor_AC_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Motor_DC"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 2.54 2.54 0)
		)
		(property "Value" "Motor_DC"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 -2.286 0)
		)
		(property "Datasheet" "~"
			(at 0 -2.286 0)
		)
		(property "Description" "DC Motor"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Motor_DC_0_0")
		(symbol "Motor_DC_0_1")
		(symbol "Motor_DC_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Motor_DC_ALT"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 2.54 2.54 0)
		)
		(property "Value" "Motor_DC_ALT"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 -2.286 0)
		)
		(property "Datasheet" "~"
			(at 0 -2.286 0)
		)
		(property "Description" "DC Motor, alternative symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Motor_DC_ALT_0_0")
		(symbol "Motor_DC_ALT_0_1")
		(symbol "Motor_DC_ALT_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Motor_Servo"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at -5.08 4.445 0)
		)
		(property "Value" "Motor_Servo"
			(at -5.08 -4.064 0)
		)
		(property "Footprint" ""
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 -4.826 0)
		)
		(property "Description" "Servo Motor (Futaba, HiTec, JR connector)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Servo Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "Motor_Servo_0_1")
		(symbol "Motor_Servo_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "PWM")
				(number "1")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Motor_Servo_AirTronics"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at -5.08 4.445 0)
		)
		(property "Value" "Motor_Servo_AirTronics"
			(at -5.08 -4.064 0)
		)
		(property "Footprint" ""
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 -4.826 0)
		)
		(property "Description" "Servo Motor (AirTronics connector)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Servo Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "Motor_Servo_AirTronics_0_1")
		(symbol "Motor_Servo_AirTronics_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "PWM")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Stepper_Motor_bipolar"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 3.81 2.54 0)
		)
		(property "Value" "Stepper_Motor_bipolar"
			(at 3.81 1.27 0)
		)
		(property "Footprint" ""
			(at 0.254 -0.254 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Application-Note-TLE8110EE_driving_UniPolarStepperMotor_V1.1.pdf?fileId=db3a30431be39b97011be5d0aa0a00b0"
			(at 0.254 -0.254 0)
		)
		(property "Description" "4-wire bipolar stepper motor"
			(at 0 0 0)
		)
		(property "ki_keywords" "bipolar stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm*Vertical* TerminalBlock* Motor*"
			(at 0 0 0)
		)
		(symbol "Stepper_Motor_bipolar_0_0")
		(symbol "Stepper_Motor_bipolar_0_1")
		(symbol "Stepper_Motor_bipolar_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Stepper_Motor_unipolar_5pin"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 3.81 2.54 0)
		)
		(property "Value" "Stepper_Motor_unipolar_5pin"
			(at 3.81 1.27 0)
		)
		(property "Footprint" ""
			(at 0.254 -0.254 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Application-Note-TLE8110EE_driving_UniPolarStepperMotor_V1.1.pdf?fileId=db3a30431be39b97011be5d0aa0a00b0"
			(at 0.254 -0.254 0)
		)
		(property "Description" "5-wire unipolar stepper motor"
			(at 0 0 0)
		)
		(property "ki_keywords" "unipolar stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Stepper_Motor_unipolar_5pin_0_0")
		(symbol "Stepper_Motor_unipolar_5pin_0_1")
		(symbol "Stepper_Motor_unipolar_5pin_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Stepper_Motor_unipolar_6pin"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 3.81 2.54 0)
		)
		(property "Value" "Stepper_Motor_unipolar_6pin"
			(at 3.81 1.27 0)
		)
		(property "Footprint" ""
			(at 0.254 -0.254 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Application-Note-TLE8110EE_driving_UniPolarStepperMotor_V1.1.pdf?fileId=db3a30431be39b97011be5d0aa0a00b0"
			(at 0.254 -0.254 0)
		)
		(property "Description" "6-wire unipolar stepper motor"
			(at 0 0 0)
		)
		(property "ki_keywords" "unipolar stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
			(at 0 0 0)
		)
		(symbol "Stepper_Motor_unipolar_6pin_0_0")
		(symbol "Stepper_Motor_unipolar_6pin_0_1")
		(symbol "Stepper_Motor_unipolar_6pin_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Fan_3pin"
		(extends "Fan_Tacho")
		(property "Reference" "M"
			(at 2.54 2.54 0)
		)
		(property "Value" "Fan_3pin"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 -2.286 0)
		)
		(property "Datasheet" "http://www.hardwarecanucks.com/forum/attachments/new-builds/16287d1330775095-help-chassis-power-fan-connectors-motherboard-asus_p8z68.jpg"
			(at 0 -2.286 0)
		)
		(property "Description" "Fan, tacho output, 3-pin connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fan Motor tacho"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "FanPinHeader*P2.54mm*Vertical* PinHeader*P2.54mm*Vertical* TerminalBlock*"
			(at 0 0 0)
		)
	)
	(symbol "Fan_4pin"
		(extends "Fan_Tacho_PWM")
		(property "Reference" "M"
			(at 2.54 5.08 0)
		)
		(property "Value" "Fan_4pin"
			(at 2.54 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0.254 0)
		)
		(property "Datasheet" "http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf"
			(at 0 0.254 0)
		)
		(property "Description" "Fan, tacho output, PWM input, 4-pin connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fan Motor tacho PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "FanPinHeader*P2.54mm*Vertical* PinHeader*P2.54mm*Vertical* TerminalBlock*"
			(at 0 0 0)
		)
	)
	(symbol "Fan_CPU_4pin"
		(extends "Fan_Tacho_PWM")
		(property "Reference" "M"
			(at 2.54 5.08 0)
		)
		(property "Value" "Fan_CPU_4pin"
			(at 2.54 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0.254 0)
		)
		(property "Datasheet" "http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf"
			(at 0 0.254 0)
		)
		(property "Description" "CPU Fan, tacho output, PWM input, 4-pin connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fan Motor tacho PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "FanPinHeader*P2.54mm*Vertical* PinHeader*P2.54mm*Vertical* TerminalBlock*"
			(at 0 0 0)
		)
	)
	(symbol "Fan_PC_Chassis"
		(extends "Fan_Tacho")
		(property "Reference" "M"
			(at 2.54 2.54 0)
		)
		(property "Value" "Fan_PC_Chassis"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 -2.286 0)
		)
		(property "Datasheet" "http://www.hardwarecanucks.com/forum/attachments/new-builds/16287d1330775095-help-chassis-power-fan-connectors-motherboard-asus_p8z68.jpg"
			(at 0 -2.286 0)
		)
		(property "Description" "PC chassis fan, tacho output, 3-pin connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fan Motor tacho"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "FanPinHeader*P2.54mm*Vertical* PinHeader*P2.54mm*Vertical* TerminalBlock*"
			(at 0 0 0)
		)
	)
	(symbol "Motor_Servo_Futaba_J"
		(extends "Motor_Servo")
		(property "Reference" "M"
			(at -5.08 4.445 0)
		)
		(property "Value" "Motor_Servo_Futaba_J"
			(at -5.08 -4.064 0)
		)
		(property "Footprint" ""
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 -4.826 0)
		)
		(property "Description" "Servo Motor (Futuba J-connector)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Servo Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "Motor_Servo_Grapner_JR"
		(extends "Motor_Servo")
		(property "Reference" "M"
			(at -5.08 4.445 0)
		)
		(property "Value" "Motor_Servo_Grapner_JR"
			(at -5.08 -4.064 0)
		)
		(property "Footprint" ""
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 -4.826 0)
		)
		(property "Description" "Servo Motor (Graupner JR connector)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Servo Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "Motor_Servo_Hitec"
		(extends "Motor_Servo")
		(property "Reference" "M"
			(at -5.08 4.445 0)
		)
		(property "Value" "Motor_Servo_Hitec"
			(at -5.08 -4.064 0)
		)
		(property "Footprint" ""
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 -4.826 0)
		)
		(property "Description" "Servo Motor (HiTec connector)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Servo Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "Motor_Servo_JR"
		(extends "Motor_Servo")
		(property "Reference" "M"
			(at -5.08 4.445 0)
		)
		(property "Value" "Motor_Servo_JR"
			(at -5.08 -4.064 0)
		)
		(property "Footprint" ""
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 -4.826 0)
		)
		(property "Description" "Servo Motor (JR connector)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Servo Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "Motor_Servo_Robbe"
		(extends "Motor_Servo")
		(property "Reference" "M"
			(at -5.08 4.445 0)
		)
		(property "Value" "Motor_Servo_Robbe"
			(at -5.08 -4.064 0)
		)
		(property "Footprint" ""
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 -4.826 0)
		)
		(property "Description" "Servo Motor (Robbe connector)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Servo Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*P2.54mm*"
			(at 0 0 0)
		)
	)
)
