(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "5P49V6965"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -11.43 29.21 0)
		)
		(property "Value" "5P49V6965"
			(at 13.97 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.8x2.8mm"
			(at -1.27 -27.94 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/5p49v6965-datasheet"
			(at -11.43 29.21 0)
		)
		(property "Description" "Programmable Clock Generator, I2C interface, 1kHz-350MHz, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low-noise PLL Reference Clock"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "5P49V6965_0_1")
		(symbol "5P49V6965_1_1"
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "XOUT")
				(number "3")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "XIN/REF")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CLKIN")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CLKINB")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CLKSEL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SEL1/SDA")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SEL0/SCL")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SD/OE")
				(number "7")
			)
			(pin power_in line
				(at -7.62 30.48 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VDDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDDO0")
				(number "23")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDDO1")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDO2")
				(number "18")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "VDDO3")
				(number "15")
			)
			(pin power_in line
				(at 7.62 30.48 270)
				(length 2.54)
				(name "VDDO4")
				(number "10")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT1")
				(number "20")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT1B")
				(number "19")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "17")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT2B")
				(number "16")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT3B")
				(number "13")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT4")
				(number "11")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUT4B")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "OUT0_SEL_I2CB")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ABLNO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -8.89 6.35 0)
		)
		(property "Value" "ABLNO"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Abracon_ABLNO"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://abracon.com/Precisiontiming/ABLNO.pdf"
			(at -5.08 2.54 0)
		)
		(property "Description" "LVCMOS Ultra Low Phase Noise XO / VCXO, Abracon ABLNO"
			(at 0 0 0)
		)
		(property "ki_keywords" "XO VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*Abracon*ABLNO*"
			(at 0 0 0)
		)
		(symbol "ABLNO_0_1")
		(symbol "ABLNO_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Vctrl")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RFout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACO-xxxMHz-A"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "ACO-xxxMHz-A"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.conwin.com/datasheets/cx/cx030.pdf"
			(at -6.985 3.175 0)
		)
		(property "Description" "HCMOS Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
		(symbol "ACO-xxxMHz-A_0_1")
		(symbol "ACO-xxxMHz-A_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "Tri-State")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ASCO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -7.62 6.35 0)
		)
		(property "Value" "ASCO"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Abracon_ASCO-4Pin_1.6x1.2mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "https://abracon.com/Oscillators/ASCO.pdf"
			(at -5.715 3.175 0)
		)
		(property "Description" "Crystal Clock Oscillator, Abracon ASCO"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*Abracon*ASCO*1.6x1.2mm*"
			(at 0 0 0)
		)
		(symbol "ASCO_0_1")
		(symbol "ASCO_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Tri-State")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ASDMB-xxxMHz"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "ASDMB-xxxMHz"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Abracon_ASDMB-4Pin_2.5x2.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://abracon.com/Oscillators/ASDMB.pdf"
			(at 7.62 11.43 0)
		)
		(property "Description" "1.8-3.3V SMD Ultra Miniature Crystal Clock Oscillator, Abracon"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.8-3.3V SMD Ultra Miniature Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Abracon*ASDMB*2.5x2.0mm*"
			(at 0 0 0)
		)
		(symbol "ASDMB-xxxMHz_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Standby")
				(number "1")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Out")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ASE-xxxMHz"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "ASE-xxxMHz"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "http://www.abracon.com/Oscillators/ASV.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "3.3V CMOS SMD Crystal Clock Oscillator, Abracon"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V CMOS SMD Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Abracon*ASE*3.2x2.5mm*"
			(at 0 0 0)
		)
		(symbol "ASE-xxxMHz_0_1")
		(symbol "ASE-xxxMHz_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ASV-xxxMHz"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "ASV-xxxMHz"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Abracon_ASV-4Pin_7.0x5.1mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "http://www.abracon.com/Oscillators/ASV.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "3.3V HCMOS SMD Crystal Clock Oscillator, Abracon"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V HCMOS SMD Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Abracon*ASV*7.0x5.1mm*"
			(at 0 0 0)
		)
		(symbol "ASV-xxxMHz_0_1")
		(symbol "ASV-xxxMHz_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CFPS-72"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "CFPS-72"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IQD_IQXO70-4Pin_7.5x5.0mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.iqdfrequencyproducts.com/products/details/cfps-72-14-01.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "500kHz-100MHz 5V Crystal Oscillator, IQD CFPS-72"
			(at 0 0 0)
		)
		(property "ki_keywords" "XO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*IQD*IQXO70*7.5x5.0mm*"
			(at 0 0 0)
		)
		(symbol "CFPS-72_0_1")
		(symbol "CFPS-72_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "+Vs")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Output")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CVCO55xx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -7.62 6.35 0)
		)
		(property "Value" "CVCO55xx"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CK605_LandPatternPL-012"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.crystek.com/home/vco/cvco55.aspx"
			(at -5.08 2.54 0)
		)
		(property "Description" "Voltage Controlled Oscillator, Crystek, 0.50\" SQ SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCXO VCO Crystek"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CK605*"
			(at 0 0 0)
		)
		(symbol "CVCO55xx_0_0"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
		)
		(symbol "CVCO55xx_0_1")
		(symbol "CVCO55xx_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "Vtune")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RFout")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CXO_DIP14"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "CXO_DIP14"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
		(symbol "CXO_DIP14_0_1")
		(symbol "CXO_DIP14_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CXO_DIP8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "CXO_DIP8"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-8"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Clock Oscillator, DIP8-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*8*"
			(at 0 0 0)
		)
		(symbol "CXO_DIP8_0_1")
		(symbol "CXO_DIP8_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DFA-S11"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "DFA-S11"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Fordahl_DFAS11-4Pin_7.0x5.0mm"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "http://www.metatech.com.hk/product/fordahl/pdf/2002%20TCXO%20Page%2043-58.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Temperature compensated Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature compensated Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Fordahl*DFAS11*7.0x5.0mm*"
			(at 0 0 0)
		)
		(symbol "DFA-S11_0_1")
		(symbol "DFA-S11_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "Vctrl")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DFA-S15"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "DFA-S15"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Fordahl_DFAS15-4Pin_5.0x3.2mm"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "http://www.metatech.com.hk/product/fordahl/pdf/2002%20TCXO%20Page%2043-58.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Temperature compensated Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature compensated Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Fordahl*DFAS15*5.0x3.2mm*"
			(at 0 0 0)
		)
		(symbol "DFA-S15_0_1")
		(symbol "DFA-S15_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "Vctrl")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DFA-S2"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "DFA-S2"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Fordahl_DFAS2-4Pin_7.3x5.1mm"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "http://www.metatech.com.hk/product/fordahl/pdf/2002%20TCXO%20Page%2043-58.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Temperature compensated Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature compensated Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Fordahl*DFAS2*7.3x5.1mm*"
			(at 0 0 0)
		)
		(symbol "DFA-S2_0_1")
		(symbol "DFA-S2_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "Vctrl")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DFA-S3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "DFA-S3"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Fordahl_DFAS3-4Pin_9.1x7.2mm"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "http://www.metatech.com.hk/product/fordahl/pdf/2002%20TCXO%20Page%2043-58.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Temperature compensated Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature compensated Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Fordahl*DFAS3*9.1x7.2mm*"
			(at 0 0 0)
		)
		(symbol "DFA-S3_0_1")
		(symbol "DFA-S3_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "Vctrl")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DGOF5S3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "DGOF5S3"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.conwin.com/datasheets/cx/cx030.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "HCMOS Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
		(symbol "DGOF5S3_0_1")
		(symbol "DGOF5S3_1_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ECS-2520MV-xxx-xx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "ECS-2520MV-xxx-xx"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_ECS_2520MV-xxx-xx-4Pin_2.5x2.0mm"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://www.ecsxtal.com/store/pdf/ECS-2520MV.pdf"
			(at -4.445 3.175 0)
		)
		(property "Description" "HCMOS Crystal Clock Oscillator, 2.5x2.0 mm SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator ECS SMD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*ECS*2520MV*2.5x2.0mm*"
			(at 0 0 0)
		)
		(symbol "ECS-2520MV-xxx-xx_0_1")
		(symbol "ECS-2520MV-xxx-xx_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Tri-State")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT5HN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 1.27 11.43 0)
		)
		(property "Value" "FT5HN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Fox_FT5H_5.0x3.2mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://foxonline.com/wp-content/uploads/pdfs/T5HN_T5HV.pdf"
			(at 1.27 -19.05 0)
		)
		(property "Description" "HCMOS temperature compensated oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "TXCO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Fox*FT5H*5.0x3.2mm*"
			(at 0 0 0)
		)
		(symbol "FT5HN_0_1")
		(symbol "FT5HN_1_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT5HV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 5.08 11.43 0)
		)
		(property "Value" "FT5HV"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Fox_FT5H_5.0x3.2mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://foxonline.com/wp-content/uploads/pdfs/T5HN_T5HV.pdf"
			(at 0 0 0)
		)
		(property "Description" "HCMOS temperature compensated voltage controlled oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "TXCO VCTCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Fox*FT5H*5.0x3.2mm*"
			(at 0 0 0)
		)
		(symbol "FT5HV_0_1")
		(symbol "FT5HV_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IQXO-70"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "IQXO-70"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IQD_IQXO70-4Pin_7.5x5.0mm"
			(at 17.145 -8.255 0)
		)
		(property "Datasheet" "http://www.iqdfrequencyproducts.com/products/details/iqxo-70-11-30.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Clock Oscillator, SMD package 7.5x5.0mm²"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*IQD*IQXO70*7.5x5.0mm*"
			(at 0 0 0)
		)
		(symbol "IQXO-70_0_1")
		(symbol "IQXO-70_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E/B")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "JTOS-50"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -7.62 6.35 0)
		)
		(property "Value" "JTOS-50"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_BK377_LandPatternPL-005"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/JTOS-50+.pdf"
			(at -5.08 2.54 0)
		)
		(property "Description" "Voltage Controlled Oscillator, 25 to 47 MHz, Mini-Circuits BK377"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*BK377*"
			(at 0 0 0)
		)
		(symbol "JTOS-50_0_1")
		(symbol "JTOS-50_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Vtune")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RFout")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KC2520Z"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 2.54 12.7 0)
		)
		(property "Value" "KC2520Z"
			(at 6.35 10.16 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Kyocera_KC2520Z-4Pin_2.5x2.0mm"
			(at 3.81 3.81 0)
		)
		(property "Datasheet" "https://global.kyocera.com/prdct/electro/product/pdf/clock_z_xz_e.pdf"
			(at 3.81 3.81 0)
		)
		(property "Description" "1.8432MHz ~ 125MHz Crystal Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "xo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Kyocera*KC2520Z*2.5x2.0mm*"
			(at 0 0 0)
		)
		(symbol "KC2520Z_0_1")
		(symbol "KC2520Z_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "INH")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KT2520K-T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -4.064 6.096 0)
		)
		(property "Value" "KT2520K-T"
			(at 4.318 6.096 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Kyocera_2520-6Pin_2.5x2.0mm"
			(at -2.54 -2.54 0)
		)
		(property "Datasheet" "https://global.kyocera.com/prdct/electro/product/pdf/kt2520_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-60MHz Temperature Compensated Crystal Oscillator, Kyocera 2520"
			(at 0 0 0)
		)
		(property "ki_keywords" "tcxo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Kyocera*2.5x2.0mm*"
			(at 0 0 0)
		)
		(symbol "KT2520K-T_0_1")
		(symbol "KT2520K-T_1_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6905xS5-80"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC6905xS5-80"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6905xfa.pdf"
			(at 7.62 11.43 0)
		)
		(property "Description" "2.7-5.5V 80MHz Precision Fixed Frequency Silicon Oscillator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "oscillator fixed frequency divider silicon"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?5*"
			(at 0 0 0)
		)
		(symbol "LTC6905xS5-80_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "OE")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DIV")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX7375AXR805"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -2.54 6.35 0)
		)
		(property "Value" "MAX7375AXR805"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7375.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Silicon Clock Oscillator 8MHz, SC-70-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Silicon Clock Oscillator 8MHz 8000kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "MAX7375AXR805_0_1")
		(symbol "MAX7375AXR805_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "CLOCK")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MV267"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -7.62 6.35 0)
		)
		(property "Value" "MV267"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_OCXO_Morion_MV267"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.morion.com.ru/catalog_pdf/MV267.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "5/10 MHz Low Phase-Noise Precision OCXO, Morion MV267"
			(at 0 0 0)
		)
		(property "ki_keywords" "OCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*OCXO*Morion*MV267*"
			(at 0 0 0)
		)
		(symbol "MV267_0_1")
		(symbol "MV267_1_1"
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Uref")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Uin")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Us")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RF")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MV317"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -7.62 6.35 0)
		)
		(property "Value" "MV317"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_OCXO_Morion_MV317"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.morion-us.com/catalog_pdf/mv317.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "60, 80, 100, 120 & 122.76 MHz OCXO, Morion MV317"
			(at 0 0 0)
		)
		(property "ki_keywords" "OCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*OCXO*Morion*MV317*"
			(at 0 0 0)
		)
		(symbol "MV317_0_1")
		(symbol "MV317_1_1"
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Uref")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Uin")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Us")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RF")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NB3N502"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 2.54 15.24 0)
		)
		(property "Value" "NB3N502"
			(at 2.54 12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -19.05 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NB3N502-D.PDF"
			(at 1.27 -21.59 0)
		)
		(property "Description" "3.3V / 5.0V 14 MHz to 190 MHz PLL Clock Multiplier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "oscillator clock multiplier PLL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NB3N502_0_1")
		(symbol "NB3N502_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "X1/CLK")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "X2")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S0")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S1")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "REF")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CLKOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NB3N511"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 2.54 15.24 0)
		)
		(property "Value" "NB3N511"
			(at 2.54 12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -19.05 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NB3N511-D.PDF"
			(at 1.27 -21.59 0)
		)
		(property "Description" "3.3V / 5.0V 14 MHz to 200 MHz PLL Clock Multiplier, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "oscillator clock multiplier PLL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NB3N511_0_1")
		(symbol "NB3N511_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "X1/ICLK")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "X2")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "S0")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S1")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OE")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "CLKOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OCXO-14"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "OCXO-14"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.petermann-technik.de/fileadmin/petermann/pdf/crystal-oscillators/OCXO-14_PETERMANN-TECHNIK.pdf"
			(at -7.62 2.54 0)
		)
		(property "Description" "Voltage-Controlled Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
		(symbol "OCXO-14_0_1")
		(symbol "OCXO-14_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "Vcontrol")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OH300"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -7.62 6.35 0)
		)
		(property "Value" "OH300"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_OCXO_ConnorWinfield_OH300"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.conwin.com/datasheets/cx/cx282.pdf"
			(at -5.08 2.54 0)
		)
		(property "Description" "100MHz Sinewave output OCXO, low phase-noise, high stability, Connor-Winfield OH300"
			(at 0 0 0)
		)
		(property "ki_keywords" "OCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*OH300*"
			(at 0 0 0)
		)
		(symbol "OH300_0_1")
		(symbol "OH300_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Vcontrol")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-210SED"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-210SED"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG210-4Pin_2.5x2.0mm"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-210SED"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Oscillator Low Profile / High Stability SPXO"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG210*2.5x2.0mm*"
			(at 0 0 0)
		)
		(symbol "SG-210SED_0_1")
		(symbol "SG-210SED_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-210STF"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-210STF"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG210-4Pin_2.5x2.0mm"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-210STF"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Crystal Oscillator SPXO"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG210*2.5x2.0mm*"
			(at 0 0 0)
		)
		(symbol "SG-210STF_0_1")
		(symbol "SG-210STF_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{ST}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-3030CM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 -6.35 0)
		)
		(property "Value" "SG-3030CM"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG3030CM"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-3030CM"
			(at -2.54 0 0)
		)
		(property "Description" "32.768kHz Crystal Oscillator (SPXO)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG3030CM*"
			(at 0 0 0)
		)
		(symbol "SG-3030CM_0_1")
		(symbol "SG-3030CM_1_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VIO")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-5032CAN"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-5032CAN"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG5032CAN&lang=en"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator 1 to 75 MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002LB*5.0x3.2mm*"
			(at 0 0 0)
		)
		(symbol "SG-5032CAN_0_1")
		(symbol "SG-5032CAN_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{ST}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-7050CAN"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-7050CAN"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002CA-4Pin_7.0x5.0mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG7050CAN&lang=en"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator 1 to 75 MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002CA*7.0x5.0mm*"
			(at 0 0 0)
		)
		(symbol "SG-7050CAN_0_1")
		(symbol "SG-7050CAN_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{ST}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-8002CA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-8002CA"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002CA-4Pin_7.0x5.0mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator 1 to 125 MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002CA*7.0x5.0mm*"
			(at 0 0 0)
		)
		(symbol "SG-8002CA_0_1")
		(symbol "SG-8002CA_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-8002CE"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-8002CE"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002CE-4Pin_3.2x2.5mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002CE*3.2x2.5mm*"
			(at 0 0 0)
		)
		(symbol "SG-8002CE_0_1")
		(symbol "SG-8002CE_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-8002DB"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-8002DB"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SeikoEpson_SG-8002DB"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG-8002DB&lang=en"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Clock Oscillator, DIP14-style plastic package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SeikoEpson*SG?8002DB*"
			(at 0 0 0)
		)
		(symbol "SG-8002DB_0_1")
		(symbol "SG-8002DB_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "14")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-8002DC"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-8002DC"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SeikoEpson_SG-8002DC"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Clock Oscillator, DIP8-style plastic package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SeikoEpson*SG?8002DC*"
			(at 0 0 0)
		)
		(symbol "SG-8002DC_0_1")
		(symbol "SG-8002DC_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-8002JA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-8002JA"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002JA-4Pin_14.0x8.7mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002JA*14.0x8.7mm*"
			(at 0 0 0)
		)
		(symbol "SG-8002JA_0_1")
		(symbol "SG-8002JA_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-8002JC"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-8002JC"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002JC-4Pin_10.5x5.0mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002JC*10.5x5.0mm*"
			(at 0 0 0)
		)
		(symbol "SG-8002JC_0_1")
		(symbol "SG-8002JC_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-8002LB"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-8002LB"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG-8002LB&lang=en"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator 1 to 125 MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002LB*5.0x3.2mm*"
			(at 0 0 0)
		)
		(symbol "SG-8002LB_0_1")
		(symbol "SG-8002LB_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si512A_2.5x3.2mm"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -7.62 8.89 0)
		)
		(property "Value" "Si512A_2.5x3.2mm"
			(at 2.54 -8.89 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Silicon_Labs_LGA-6_2.5x3.2mm_P1.25mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si512-13.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Dual frequency crystal oscillator (XO) 100 kHz to 250 MHz, Single-ended CMOS output"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual frequency crystal oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Silicon*Labs*LGA*2.5x3.2mm*P1.25mm*"
			(at 0 0 0)
		)
		(symbol "Si512A_2.5x3.2mm_0_1")
		(symbol "Si512A_2.5x3.2mm_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "FS")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OE")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CLK")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si513A_2.5x3.2mm"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 8.89 0)
		)
		(property "Value" "Si513A_2.5x3.2mm"
			(at 2.54 -8.89 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Silicon_Labs_LGA-6_2.5x3.2mm_P1.25mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si512-13.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Dual frequency crystal oscillator (XO) 100 kHz to 250 MHz, Single-ended CMOS output"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual frequency crystal oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*Silicon*Labs*LGA*2.5x3.2mm*P1.25mm*"
			(at 0 0 0)
		)
		(symbol "Si513A_2.5x3.2mm_0_1")
		(symbol "Si513A_2.5x3.2mm_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FS")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CLK")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si5351A-B-GM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -12.7 21.59 0)
		)
		(property "Value" "Si5351A-B-GM"
			(at -13.97 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Programmable Any-Frequency CMOS Clock Generator, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Synth Oscillator I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "Si5351A-B-GM_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "XA")
				(number "1")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "XB")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A0")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "OEB")
				(number "7")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SSEN")
				(number "6")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDDOA")
				(number "11")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDDOB")
				(number "10")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDOC")
				(number "18")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VDDOD")
				(number "14")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "CLK0")
				(number "13")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "CLK1")
				(number "12")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "CLK2")
				(number "9")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CLK3")
				(number "8")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "CLK4")
				(number "19")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CLK5")
				(number "17")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "CLK6")
				(number "16")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "CLK7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si5351A-B-GT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -8.89 11.43 0)
		)
		(property "Value" "Si5351A-B-GT"
			(at -12.7 -12.7 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf"
			(at -8.89 -2.54 0)
		)
		(property "Description" "I2C Programmable Any-Frequency CMOS Clock Generator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Synth Oscillator I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "Si5351A-B-GT_0_1")
		(symbol "Si5351A-B-GT_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "XA")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "XB")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDDO")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CLK0")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CLK1")
				(number "9")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CLK2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si5351B-B-GM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -12.7 21.59 0)
		)
		(property "Value" "Si5351B-B-GM"
			(at -13.97 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Programmable Any-Frequency CMOS Clock Generator + VCXO, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Synth Oscillator I2C VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "Si5351B-B-GM_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "XA")
				(number "1")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "XB")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VC")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "OEB")
				(number "7")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SSEN")
				(number "6")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDDOA")
				(number "11")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDDOB")
				(number "10")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDOC")
				(number "18")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VDDOD")
				(number "14")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "CLK0")
				(number "13")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "CLK1")
				(number "12")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "CLK2")
				(number "9")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CLK3")
				(number "8")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "CLK4")
				(number "19")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CLK5")
				(number "17")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "CLK6")
				(number "16")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "CLK7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si5351C-B-GM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -12.7 21.59 0)
		)
		(property "Value" "Si5351C-B-GM"
			(at -13.97 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Programmable Any-Frequency CMOS Clock Generator, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS Synth Oscillator I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "Si5351C-B-GM_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "XA")
				(number "1")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "XB")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CLKIN")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "INTR")
				(number "3")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "OEB")
				(number "7")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDDOA")
				(number "11")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDDOB")
				(number "10")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDOC")
				(number "18")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VDDOD")
				(number "14")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "CLK0")
				(number "13")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "CLK1")
				(number "12")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "CLK2")
				(number "9")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CLK3")
				(number "8")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "CLK4")
				(number "19")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CLK5")
				(number "17")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "CLK6")
				(number "16")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "CLK7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si570"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -8.89 8.89 0)
		)
		(property "Value" "Si570"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SI570_SI571_Standard"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.silabs.com/Support%20Documents/TechnicalDocs/si570.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "10 MHZ TO 1.4 GHZ I2C PROGRAMMABLE XO/VCXO"
			(at 0 0 0)
		)
		(property "ki_keywords" "10 MHZ TO 1.4 GHZ I2C PROGRAMMABLE XO/VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SI570*SI571*"
			(at 0 0 0)
		)
		(symbol "Si570_0_1")
		(symbol "Si570_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "OE")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vcc")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CLK+")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CLK-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si571"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -10.16 10.16 0)
		)
		(property "Value" "Si571"
			(at 8.89 -10.16 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SI570_SI571_Standard"
			(at -13.97 15.24 0)
		)
		(property "Datasheet" "http://www.silabs.com/Support%20Documents/TechnicalDocs/si570.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "10 MHZ TO 1.4 GHZ I2C PROGRAMMABLE XO/VCXO"
			(at 0 0 0)
		)
		(property "ki_keywords" "10 MHZ TO 1.4 GHZ I2C PROGRAMMABLE XO/VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SI570*SI571*"
			(at 0 0 0)
		)
		(symbol "Si571_0_1")
		(symbol "Si571_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "Vc")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "OE")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "SCL")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "Vcc")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "CLK+")
				(number "4")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "CLK-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiT8008xx-7x-xxE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-7x-xxE"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_2.0x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 2.0x1.6mm (with output enable pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*2.0x1.6mm*"
			(at 0 0 0)
		)
		(symbol "SiT8008xx-7x-xxE_0_1")
		(symbol "SiT8008xx-7x-xxE_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiT8008xx-7x-xxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-7x-xxN"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_2.0x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 2.0x1.6mm (with NC pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*2.0x1.6mm*"
			(at 0 0 0)
		)
		(symbol "SiT8008xx-7x-xxN_0_1")
		(symbol "SiT8008xx-7x-xxN_1_1"
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiT8008xx-7x-xxS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-7x-xxS"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_2.0x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 2.0x1.6mm (with standby pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*2.0x1.6mm*"
			(at 0 0 0)
		)
		(symbol "SiT8008xx-7x-xxS_0_1")
		(symbol "SiT8008xx-7x-xxS_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{ST}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiT9365xx-xBx-xxE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "SiT9365xx-xBx-xxE"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiTime_PQFD-6L_3.2x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/datasheet/SiT9365"
			(at -10.16 17.78 0)
		)
		(property "Description" "SiTime Standard Frequency Ultra-low Jitter Differential Oscillator, 25-325MHz, PQFD-6, 3.2x2.5mm (with enable pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS LVPECL HCSL differential MEMS oscillatior"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFD*3.2x2.5mm*"
			(at 0 0 0)
		)
		(symbol "SiT9365xx-xBx-xxE_0_1")
		(symbol "SiT9365xx-xBx-xxE_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OE")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT+")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiT9365xx-xBx-xxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "SiT9365xx-xBx-xxN"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiTime_PQFD-6L_3.2x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/datasheet/SiT9365"
			(at -10.16 17.78 0)
		)
		(property "Description" "SiTime Standard Frequency Ultra-low Jitter Differential Oscillator, 25-325MHz, PQFD-6, 3.2x2.5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS LVPECL HCSL differential MEMS oscillatior"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFD*3.2x2.5mm*"
			(at 0 0 0)
		)
		(symbol "SiT9365xx-xBx-xxN_0_1")
		(symbol "SiT9365xx-xBx-xxN_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT+")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCXO3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 8.255 11.43 0)
		)
		(property "Value" "TCXO3"
			(at 8.255 8.89 0)
		)
		(property "Footprint" ""
			(at -13.97 6.35 0)
		)
		(property "Datasheet" "http://www.hcelectronics.cz/PDF/TCXO3_A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Temperature compensated crystal oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature compensated crystal oscillator"
			(at 0 0 0)
		)
		(symbol "TCXO3_0_1")
		(symbol "TCXO3_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "Vctrl")
				(number "18")
			)
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -10.16 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -7.62 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -7.62 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "URef")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin no_connect line
				(at -2.54 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+5V")
				(number "15")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin no_connect line
				(at 2.54 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "23")
			)
			(pin no_connect line
				(at 5.08 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at 7.62 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FREQ")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TG2520SMN-xx.xxxxxxMhz-xxxxNM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "TG2520SMN-xx.xxxxxxMhz-xxxxNM"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_TG2520SMN-xxx-xxxxxx-4Pin_2.5x2.0mm"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=app_TG2520SMN&lang=en"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Oscillator Low Profile / High Stability TCXO"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*TG2520*2.5x2.0mm*"
			(at 0 0 0)
		)
		(symbol "TG2520SMN-xx.xxxxxxMhz-xxxxNM_0_1")
		(symbol "TG2520SMN-xx.xxxxxxMhz-xxxxNM_1_1"
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXC-7C"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "TXC-7C"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_TXC_7C-4Pin_5.0x3.2mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "http://www.txccorp.com/download/products/osc/7C_o.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS SMD Crystal Clock Oscillator, TXC"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS SMD Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*TXC*7C*5.0x3.2mm*"
			(at 0 0 0)
		)
		(symbol "TXC-7C_0_1")
		(symbol "TXC-7C_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VC-81"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "VC-81"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-8"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.scsiglobal.com/Hosonic/Documents/SCSI-VC-81&83.pdf"
			(at -7.62 2.54 0)
		)
		(property "Description" "Voltage-Controlled Crystal Clock Oscillator, DIP8-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*8*"
			(at 0 0 0)
		)
		(symbol "VC-81_0_1")
		(symbol "VC-81_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "Vcontrol")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XO32"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "XO32"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_EuroQuartz_XO32-4Pin_3.2x2.5mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/B400/XO32.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "HCMOS Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*EuroQuartz*XO32*3.2x2.5mm*"
			(at 0 0 0)
		)
		(symbol "XO32_0_1")
		(symbol "XO32_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XO53"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "XO53"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_EuroQuartz_XO53-4Pin_5.0x3.2mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/B400/XO53.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Low Power Consumption Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*EuroQuartz*XO53*5.0x3.2mm*"
			(at 0 0 0)
		)
		(symbol "XO53_0_1")
		(symbol "XO53_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XO91"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "XO91"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_EuroQuartz_XO91-4Pin_7.0x5.0mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/B400/XO91.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "HCMOS Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*EuroQuartz*XO91*7.0x5.0mm*"
			(at 0 0 0)
		)
		(symbol "XO91_0_1")
		(symbol "XO91_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XUX51"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUX51"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JS6-6_5.0x3.2mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 1.8V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JS6*"
			(at 0 0 0)
		)
		(symbol "XUX51_0_1")
		(symbol "XUX51_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "E/D")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XUX71"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUX71"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JU6-6_7.0x5.0mm_P2.54mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 1.8V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JU6*"
			(at 0 0 0)
		)
		(symbol "XUX71_0_1")
		(symbol "XUX71_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "E/D")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XUY51"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUY51"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JS6-6_5.0x3.2mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP HCMOS 1.8V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JS6*"
			(at 0 0 0)
		)
		(symbol "XUY51_0_1")
		(symbol "XUY51_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "E/D")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XUY71"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUY71"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JU6-6_7.0x5.0mm_P2.54mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP HCMOS 1.8V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JU6*"
			(at 0 0 0)
		)
		(symbol "XUY71_0_1")
		(symbol "XUY71_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "E/D")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACO-xxxMHz"
		(extends "DGOF5S3")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "ACO-xxxMHz"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.conwin.com/datasheets/cx/cx030.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "HCMOS Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
	)
	(symbol "GTXO-14T"
		(extends "CXO_DIP14")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "GTXO-14T"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.golledge.com/pdf/products/tcxos/gtxo14.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
	)
	(symbol "GTXO-14V"
		(extends "OCXO-14")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "GTXO-14V"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.golledge.com/pdf/products/tcxos/gtxo14.pdf"
			(at -7.62 2.54 0)
		)
		(property "Description" "Voltage-Controlled Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
	)
	(symbol "GTXO-S14T"
		(extends "DGOF5S3")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "GTXO-S14T"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.golledge.com/pdf/products/tcxos/gtxos14.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "3.3 & 5V Stratum 3 Sinewave TCXO, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
	)
	(symbol "GTXO-S14V"
		(extends "OCXO-14")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "GTXO-S14V"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.golledge.com/pdf/products/tcxos/gtxos14.pdf"
			(at -7.62 2.54 0)
		)
		(property "Description" "3.3 & 5V Stratum 3 Sinewave TCXO, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
	)
	(symbol "JTOS-25"
		(extends "JTOS-50")
		(property "Reference" "Y"
			(at -7.62 6.35 0)
		)
		(property "Value" "JTOS-25"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_BK377_LandPatternPL-005"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/JTOS-25+.pdf"
			(at -5.08 2.54 0)
		)
		(property "Description" "Voltage Controlled Oscillator, 12.5 to 25 MHz, Mini-Circuits BK377"
			(at 0 0 0)
		)
		(property "ki_keywords" "VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*BK377*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6905xS5-100"
		(extends "LTC6905xS5-80")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC6905xS5-100"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6905xfa.pdf"
			(at 7.62 11.43 0)
		)
		(property "Description" "2.7-5.5V 100MHz Precision Fixed Frequency Silicon Oscillator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "oscillator fixed frequency divider silicon"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6905xS5-133"
		(extends "LTC6905xS5-80")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC6905xS5-133"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6905xfa.pdf"
			(at 7.62 11.43 0)
		)
		(property "Description" "2.7-5.5V 133MHz Precision Fixed Frequency Silicon Oscillator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "oscillator fixed frequency divider silicon"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6905xS5-96"
		(extends "LTC6905xS5-80")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC6905xS5-96"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6905xfa.pdf"
			(at 7.62 11.43 0)
		)
		(property "Description" "2.7-5.5V 96MHz Precision Fixed Frequency Silicon Oscillator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "oscillator fixed frequency divider silicon"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "MAX7375AXR105"
		(extends "MAX7375AXR805")
		(property "Reference" "Y"
			(at -2.54 6.35 0)
		)
		(property "Value" "MAX7375AXR105"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7375.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Silicon Clock Oscillator 1MHz, SC-70-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Silicon Clock Oscillator 1MHz 1000kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MAX7375AXR185"
		(extends "MAX7375AXR805")
		(property "Reference" "Y"
			(at -2.54 6.35 0)
		)
		(property "Value" "MAX7375AXR185"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7375.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Silicon Clock Oscillator 1.84MHz, SC-70-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Silicon Clock Oscillator 1,84MHz 1840kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MAX7375AXR365"
		(extends "MAX7375AXR805")
		(property "Reference" "Y"
			(at -2.54 6.35 0)
		)
		(property "Value" "MAX7375AXR365"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7375.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Silicon Clock Oscillator 3.58MHz, SC-70-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Silicon Clock Oscillator 3.58MHz 3580kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MAX7375AXR375"
		(extends "MAX7375AXR805")
		(property "Reference" "Y"
			(at -2.54 6.35 0)
		)
		(property "Value" "MAX7375AXR375"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7375.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Silicon Clock Oscillator 3.69MHz, SC-70-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Silicon Clock Oscillator 3.69MHz 3690kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MAX7375AXR405"
		(extends "MAX7375AXR805")
		(property "Reference" "Y"
			(at -2.54 6.35 0)
		)
		(property "Value" "MAX7375AXR405"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7375.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Silicon Clock Oscillator 4MHz, SC-70-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Silicon Clock Oscillator 4MHz 4000kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MAX7375AXR425"
		(extends "MAX7375AXR805")
		(property "Reference" "Y"
			(at -2.54 6.35 0)
		)
		(property "Value" "MAX7375AXR425"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 27.94 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7375.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Silicon Clock Oscillator 4.19MHz, SC-70-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Silicon Clock Oscillator 4.19MHz 4190kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "SG-210SCD"
		(extends "SG-210SED")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-210SCD"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG210-4Pin_2.5x2.0mm"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-210SED"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Oscillator Low Profile / High Stability SPXO"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG210*2.5x2.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SG-210SDD"
		(extends "SG-210SED")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-210SDD"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG210-4Pin_2.5x2.0mm"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-210SED"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Oscillator Low Profile / High Stability SPXO"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG210*2.5x2.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SG-211"
		(extends "SG-210STF")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-211"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG210-4Pin_2.5x2.0mm"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-211SEE"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Crystal Oscillator SPXO"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG210*2.5x2.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SG-5032CBN"
		(extends "SG-5032CAN")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-5032CBN"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG5032CBN&lang=en"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator 80 to 170 MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002LB*5.0x3.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "SG-5032CCN"
		(extends "SG-8002LB")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-5032CCN"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG5032CCN&lang=en"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator 2.5 to 50 MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002LB*5.0x3.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "SG-51"
		(extends "SG-8002DB")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-51"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SeikoEpson_SG-8002DB"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-51P"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Crystal Clock Oscillator, DIP14-style plastic package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SeikoEpson*SG?8002DB*"
			(at 0 0 0)
		)
	)
	(symbol "SG-531"
		(extends "SG-8002DC")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-531"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SeikoEpson_SG-8002DC"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-51P"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Crystal Clock Oscillator, DIP8-style plastic package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SeikoEpson*SG?8002DC*"
			(at 0 0 0)
		)
	)
	(symbol "SG-615"
		(extends "SG-8002JA")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-615"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002JA-4Pin_14.0x8.7mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-51P"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002JA*14.0x8.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "SG-7050CBN"
		(extends "SG-7050CAN")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-7050CBN"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002CA-4Pin_7.0x5.0mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG7050CBN&lang=en"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator 80 to 170 MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002CA*7.0x5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SG-7050CCN"
		(extends "SG-8002CA")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "SG-7050CCN"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002CA-4Pin_7.0x5.0mm"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG7050CAN&lang=en"
			(at -2.54 0 0)
		)
		(property "Description" "CMOS Clock Oscillator 2.5 to 50 MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002CA*7.0x5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-1x-xxE"
		(extends "SiT8008xx-7x-xxE")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-1x-xxE"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_2.5x2.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 2.5x2.0mm (with output enable pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*2.5x2.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-1x-xxN"
		(extends "SiT8008xx-7x-xxN")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-1x-xxN"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_2.5x2.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 2.5x2.0mm (with NC pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*2.5x2.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-1x-xxS"
		(extends "SiT8008xx-7x-xxS")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-1x-xxS"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_2.5x2.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 2.5x2.0mm (with standby pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*2.5x2.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-2x-xxE"
		(extends "SiT8008xx-7x-xxE")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-2x-xxE"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_3.2x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 3.2x2.5mm (with output enable pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*3.2x2.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-2x-xxN"
		(extends "SiT8008xx-7x-xxN")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-2x-xxN"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_3.2x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 3.2x2.5mm (with NC pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*3.2x2.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-2x-xxS"
		(extends "SiT8008xx-7x-xxS")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-2x-xxS"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_3.2x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 3.2x2.5mm (with standby pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*3.2x2.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-3x-xxE"
		(extends "SiT8008xx-7x-xxE")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-3x-xxE"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_5.0x3.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 5.0x3.2mm (with output enable pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*5.0x3.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-3x-xxN"
		(extends "SiT8008xx-7x-xxN")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-3x-xxN"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_5.0x3.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 5.0x3.2mm (with NC pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*5.0x3.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-3x-xxS"
		(extends "SiT8008xx-7x-xxS")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-3x-xxS"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_5.0x3.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 5.0x3.2mm (with standby pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*5.0x3.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-8x-xxE"
		(extends "SiT8008xx-7x-xxE")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-8x-xxE"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_7.0x5.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 7.0x5.0mm (with output enable pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*7.0x5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-8x-xxN"
		(extends "SiT8008xx-7x-xxN")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-8x-xxN"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_7.0x5.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 7.0x5.0mm (with NC pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*7.0x5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT8008xx-8x-xxS"
		(extends "SiT8008xx-7x-xxS")
		(property "Reference" "Y"
			(at 4.064 8.89 0)
		)
		(property "Value" "SiT8008xx-8x-xxS"
			(at 12.446 6.858 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiT_PQFN-4Pin_7.0x5.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/support/resource-library/datasheets/sit8008-datasheet"
			(at 0 0 0)
		)
		(property "Description" "SiTime Low Power Mems programmable oscillator, 1MHz to 110MHz, PQFN-4, 7.0x5.0mm (with standby pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFN*7.0x5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT9366xx-xBx-xxE"
		(extends "SiT9365xx-xBx-xxE")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "SiT9366xx-xBx-xxE"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiTime_PQFD-6L_3.2x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/datasheet/SiT9366"
			(at -10.16 17.78 0)
		)
		(property "Description" "SiTime Standard Frequency Ultra-low Jitter Differential Oscillator, 1 MHz and 220MHz, PQFD-6, 3.2x2.5mm (with enable pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS LVPECL HCSL differential MEMS oscillatior"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFD*3.2x2.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT9366xx-xBx-xxN"
		(extends "SiT9365xx-xBx-xxN")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "SiT9366xx-xBx-xxN"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiTime_PQFD-6L_3.2x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/datasheet/SiT9366"
			(at -10.16 17.78 0)
		)
		(property "Description" "SiTime Standard Frequency Ultra-low Jitter Differential Oscillator, 1 MHz and 220MHz, PQFD-6, 3.2x2.5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS LVPECL HCSL differential MEMS oscillatior"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFD*3.2x2.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT9367xx-xBx-xxE"
		(extends "SiT9365xx-xBx-xxE")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "SiT9367xx-xBx-xxE"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiTime_PQFD-6L_3.2x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/datasheet/SiT9367"
			(at -10.16 17.78 0)
		)
		(property "Description" "SiTime Standard Frequency Ultra-low Jitter Differential Oscillator, 220.000001-725MHz, PQFD-6, 3.2x2.5mm (with enable pin)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS LVPECL HCSL differential MEMS oscillatior"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFD*3.2x2.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SiT9367xx-xBx-xxN"
		(extends "SiT9365xx-xBx-xxN")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "SiT9367xx-xBx-xxN"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_SiTime_PQFD-6L_3.2x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sitime.com/datasheet/SiT9367"
			(at -10.16 17.78 0)
		)
		(property "Description" "SiTime Standard Frequency Ultra-low Jitter Differential Oscillator, 220.000001-725MHz, PQFD-6, 3.2x2.5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS LVPECL HCSL differential MEMS oscillatior"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFD*3.2x2.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCXO-14"
		(extends "DGOF5S3")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "TCXO-14"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.golledge.com/pdf/products/tcxos/gtxos14.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Temperature Compensated Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
	)
	(symbol "TFT660"
		(extends "CXO_DIP8")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "TFT660"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-8"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Clock Oscillator, DIP8-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*8*"
			(at 0 0 0)
		)
	)
	(symbol "TFT680"
		(extends "CXO_DIP14")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "TFT680"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
	)
	(symbol "VC-83"
		(extends "VC-81")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "VC-83"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-8"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.scsiglobal.com/Hosonic/Documents/SCSI-VC-81&83.pdf"
			(at -7.62 2.54 0)
		)
		(property "Description" "Voltage-Controlled Crystal Clock Oscillator, DIP8-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*8*"
			(at 0 0 0)
		)
	)
	(symbol "VTCXO-14"
		(extends "OCXO-14")
		(property "Reference" "Y"
			(at -5.08 6.35 0)
		)
		(property "Value" "VTCXO-14"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_DIP-14"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "http://www.golledge.com/pdf/products/tcxos/gtxos14.pdf"
			(at -7.62 2.54 0)
		)
		(property "Description" "Voltage-Controlled Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Crystal Clock Oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*DIP*14*"
			(at 0 0 0)
		)
	)
	(symbol "XUX52"
		(extends "XUX51")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUX52"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JS6-6_5.0x3.2mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 2.5V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JS6*"
			(at 0 0 0)
		)
	)
	(symbol "XUX53"
		(extends "XUX51")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUX53"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JS6-6_5.0x3.2mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 3.3V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JS6*"
			(at 0 0 0)
		)
	)
	(symbol "XUX72"
		(extends "XUX71")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUX72"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JU6-6_7.0x5.0mm_P2.54mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 2.5V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JU6*"
			(at 0 0 0)
		)
	)
	(symbol "XUX73"
		(extends "XUX71")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUX73"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JU6-6_7.0x5.0mm_P2.54mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 3.3V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JU6*"
			(at 0 0 0)
		)
	)
	(symbol "XUY52"
		(extends "XUY51")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUY52"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JS6-6_5.0x3.2mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 2.5V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JS6*"
			(at 0 0 0)
		)
	)
	(symbol "XUY53"
		(extends "XUY51")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUY53"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JS6-6_5.0x3.2mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 3.3V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JS6*"
			(at 0 0 0)
		)
	)
	(symbol "XUY72"
		(extends "XUY71")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUY72"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JU6-6_7.0x5.0mm_P2.54mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 2.5V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JU6*"
			(at 0 0 0)
		)
	)
	(symbol "XUY73"
		(extends "XUY71")
		(property "Reference" "Y"
			(at -6.35 6.35 0)
		)
		(property "Value" "XUY73"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_IDT_JU6-6_7.0x5.0mm_P2.54mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/xu-family-low-phase-noise-quartz-based-pll-oscillators-datasheet"
			(at -10.16 17.78 0)
		)
		(property "Description" "Low phase noise, quartz-based PLL oscillator, 0.016-1500 MHz, complementary output"
			(at 0 0 0)
		)
		(property "ki_keywords" "OTP XHCMOS 3.3V VCXO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Oscillator*JU6*"
			(at 0 0 0)
		)
	)
)
