(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD5254"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "AD5254"
			(at 1.27 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5253_5254.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Digital potentiometer, 256 position, 4 output, I2C interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD5254_0_1")
		(symbol "AD5254_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{WP}")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "AD0")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AD1")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "A0")
				(number "3")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "W0")
				(number "1")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "B0")
				(number "2")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A1")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "W1")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "A2")
				(number "11")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "W2")
				(number "13")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B2")
				(number "12")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "A3")
				(number "17")
			)
			(pin passive line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "W3")
				(number "19")
			)
			(pin passive line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "B3")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5272BCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AD5272BCP"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-WD-10-1EP_3x3mm_P0.5mm_EP1.64x2.38mm"
			(at 33.02 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5272_5274.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital potentiometer, 1024 position, 1% Resistor Tolerance, I2C interface, LFCSP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD5272BCP_0_1")
		(symbol "AD5272BCP_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ADDR")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "W")
				(number "3")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "EXT_CAP")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5272BRM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AD5272BRM"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 19.05 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5272_5274.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital potentiometer, 1024 position, 1% Resistor Tolerance, I2C interface, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD5272BRM_0_1")
		(symbol "AD5272BRM_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ADDR")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "W")
				(number "3")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "EXT_CAP")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5280"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "AD5280"
			(at 5.588 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5280_5282.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "Digital potentiometer, 256 position, single output, I2C interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD5280_0_1")
		(symbol "AD5280_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "AD0")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "AD1")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VLOG")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "11")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "W")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "O1")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "O2")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5282"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.414 13.97 0)
		)
		(property "Value" "AD5282"
			(at 0.762 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5280_5282.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Digital potentiometer, 256 position, dual output, I2C interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD5282_0_1")
		(symbol "AD5282_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "AD0")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "AD1")
				(number "10")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VLOG")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "W1")
				(number "3")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "B1")
				(number "4")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "A2")
				(number "16")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "W2")
				(number "15")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "B2")
				(number "14")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "O1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5290"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.906 8.89 0)
		)
		(property "Value" "AD5290"
			(at 2.794 9.144 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5290.pdf"
			(at 0 27.94 0)
		)
		(property "Description" "Digital Potentiometer, 256 steps, SPI interface, +30V/±15V supply, MSOP-10"
			(at 0 25.4 0)
		)
		(property "ki_keywords" "analog-devices "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD5290_0_1")
		(symbol "AD5290_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDI")
				(number "7")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDO")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CLK")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "V_{SS}")
				(number "3")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "W")
				(number "10")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5293"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.986 11.43 0)
		)
		(property "Value" "AD5293"
			(at 7.874 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5293.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital potentiometer 1024 pos (SPI), TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "R POT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD5293_0_1")
		(symbol "AD5293_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SDI")
				(number "10")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SDO")
				(number "13")
			)
			(pin input clock
				(at -17.78 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "11")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "12")
			)
			(pin open_collector output_low
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "RDY")
				(number "14")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "EXT_CAP")
				(number "7")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "Vlog")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "Vdd+")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "Vss-")
				(number "2")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "RH")
				(number "3")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 2.54)
				(name "RW")
				(number "4")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "RL")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1267_DIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "DS1267_DIP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 19.05 -11.43 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1267.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Dual Digital Potentiometer, Serial, 256 Steps, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Digital Potentiometer Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DS1267_DIP_0_1")
		(symbol "DS1267_DIP_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "DQ")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{Reset}")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "6")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SOUT")
				(number "13")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "COUT")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "VB")
				(number "1")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "H0")
				(number "11")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "W0")
				(number "12")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "L0")
				(number "10")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "H1")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "W1")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "L1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1267_SOIC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "DS1267_SOIC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 27.94 -11.43 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1267.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Dual Digital Potentiometer, Serial, 256 Steps, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Digital Potentiometer Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS1267_SOIC_0_1")
		(symbol "DS1267_SOIC_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "DQ")
				(number "9")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{Reset}")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "7")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SOUT")
				(number "14")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "COUT")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "VB")
				(number "1")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "H0")
				(number "12")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "W0")
				(number "13")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "L0")
				(number "11")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "H1")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "W1")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "L1")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1267_TSSOP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "DS1267_TSSOP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 27.94 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1267.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Dual Digital Potentiometer, Serial, 256 Steps, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Digital Potentiometer Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*0.65mm*"
			(at 0 0 0)
		)
		(symbol "DS1267_TSSOP_0_1")
		(symbol "DS1267_TSSOP_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "DQ")
				(number "11")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{Reset}")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "7")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SOUT")
				(number "17")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "COUT")
				(number "13")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "VB")
				(number "1")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "H0")
				(number "15")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "W0")
				(number "16")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "L0")
				(number "14")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "H1")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "W1")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "L1")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1882E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "DS1882E"
			(at 5.08 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 5.08 -16.51 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1882.pdf"
			(at -10.16 -2.54 0)
		)
		(property "Description" "Dual Log Audio Digital Potentiometer, 64 positions, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DS1882E_0_1")
		(symbol "DS1882E_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "13")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{CE}")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A2")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "H0")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "W0")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "L0")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "H1")
				(number "10")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "W1")
				(number "11")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "L1")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5436"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "MAX5436"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX5436-MAX5439.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Drift Digital Potentiometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer resistor variable"
			(at 0 0 0)
		)
		(symbol "MAX5436_0_1")
		(symbol "MAX5436_1_1"
			(pin input clock
				(at -12.7 2.54 0)
				(length 5.08)
				(name "SCLK")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "Din")
				(number "2")
			)
			(pin input inverted
				(at -12.7 -3.81 0)
				(length 5.08)
				(name "CS")
				(number "3")
			)
			(pin power_in line
				(at -2.54 8.89 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -8.89 90)
				(length 2.54)
				(name "Gnd")
				(number "4")
			)
			(pin power_in line
				(at 2.54 8.89 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -8.89 90)
				(length 2.54)
				(name "V-")
				(number "5")
			)
			(pin passive line
				(at 12.7 3.81 180)
				(length 5.08)
				(name "H")
				(number "7")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "W")
				(number "8")
			)
			(pin passive line
				(at 12.7 -3.81 180)
				(length 5.08)
				(name "L")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4011-xxxxMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4011-xxxxMS"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21978c.pdf, MSOP-8"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Volatile Digital Potentiometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP4011-xxxxMS_0_1")
		(symbol "MCP4011-xxxxMS_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "U/~{D}")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "W")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4011-xxxxSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4011-xxxxSN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21978c.pdf, SOIC-8"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Volatile Digital Potentiometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP4011-xxxxSN_0_1")
		(symbol "MCP4011-xxxxSN_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "U/~{D}")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "W")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4012-xxxxCH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4012-xxxxCH"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21978c.pdf, SOT-23-6"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Volatile Digital Potentiometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP4012-xxxxCH_0_1")
		(symbol "MCP4012-xxxxCH_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "U/~{D}")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "W")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4013-xxxxCH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4013-xxxxCH"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21978c.pdf, SOT-23-6"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Volatile Digital Potentiometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP4013-xxxxCH_0_1")
		(symbol "MCP4013-xxxxCH_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "U/~{D}")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "W")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4014-xxxxOT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4014-xxxxOT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21978c.pdf, SOT-23-5"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Volatile Digital Potentiometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP4014-xxxxOT_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "U/~{D}")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "W")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4017-xxxxLT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4017-xxxxLT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22147a.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 128-Step Volatile I2C Digital Potentiometer, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TWI pot rheostat"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "MCP4017-xxxxLT_0_0"
			(text "A"
				(at 3.81 6.35 0)
			)
		)
		(symbol "MCP4017-xxxxLT_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "W")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4018-xxxxLT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4018-xxxxLT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22147a.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 128-Step Volatile I2C Digital Potentiometer, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TWI pot"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "MCP4018-xxxxLT_0_1")
		(symbol "MCP4018-xxxxLT_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "W")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4019-xxxxLT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4019-xxxxLT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22147a.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 128-Step Volatile I2C Digital Potentiometer, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "TWI pot rheostat"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "MCP4019-xxxxLT_0_0"
			(text "A"
				(at 3.81 6.35 0)
			)
		)
		(symbol "MCP4019-xxxxLT_0_1")
		(symbol "MCP4019-xxxxLT_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "W")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP41010"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP41010"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11195c.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Digital Potentiometer, SPI interface, 256 taps, 10 kohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "R POT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP41010_0_1")
		(symbol "MCP41010_1_1"
			(pin passive clock
				(at -10.16 2.54 0)
				(length 3.81)
				(name "SCK")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "SI")
				(number "3")
			)
			(pin input input_low
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "~{CS}")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "PA0")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 3.81)
				(name "PW0")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "PB0")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4131-xxxx-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "MCP4131-xxxx-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22060b.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Single Digital Potentiometer, SPI interface, 129 taps, 5/10/50/100 kohm, volatile memory"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "digipot RAM 7-bit 7bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP4131-xxxx-P_0_0"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input clock
				(at -12.7 0 0)
				(length 2.54)
				(name "SCK")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDI/SDO")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P0A")
				(number "5")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "P0W")
				(number "6")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P0B")
				(number "7")
			)
		)
		(symbol "MCP4131-xxxx-P_0_1")
		(symbol "MCP4131-xxxx-P_1_1")
		(embedded_fonts no)
	)
	(symbol "MCP4132-xxxx-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "MCP4132-xxxx-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22060b.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Single Digital Rheostat, SPI interface, 129 taps, 5/10/50/100 kohm, volatile memory"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "potentiometer digipot RAM 7-bit 7bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP4132-xxxx-P_0_0"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input clock
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCK")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
		)
		(symbol "MCP4132-xxxx-P_0_1")
		(symbol "MCP4132-xxxx-P_1_0"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDI")
				(number "3")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SDO")
				(number "7")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P0B")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "P0W")
				(number "5")
			)
		)
		(symbol "MCP4132-xxxx-P_1_1")
		(embedded_fonts no)
	)
	(symbol "MCP42010"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MCP42010"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11195c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual Digital Potentiometer, SPI interface, 256 taps, 10 kohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "R POT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP42010_0_1")
		(symbol "MCP42010_1_1"
			(pin input clock
				(at -12.7 7.62 0)
				(length 5.08)
				(name "SCK")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "SI")
				(number "3")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "SO")
				(number "13")
			)
			(pin input input_low
				(at -12.7 0 0)
				(length 5.08)
				(name "~{CS}")
				(number "1")
			)
			(pin input input_low
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{RS}")
				(number "11")
			)
			(pin input input_low
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~{SHDN}")
				(number "12")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "PA0")
				(number "8")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "PW0")
				(number "9")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "PB0")
				(number "10")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "PA1")
				(number "7")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "PW1")
				(number "6")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "PB1")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4251-xxxx-ML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.508 18.288 0)
		)
		(property "Value" "MCP4251-xxxx-ML"
			(at -0.508 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.5x2.5mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22060b.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "Dual 8 Bit Digital Pot, SPI, Volatile Memory, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP4251-xxxx-ML_0_1")
		(symbol "MCP4251-xxxx-ML_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "16")
			)
			(pin input clock
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDO")
				(number "14")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "13")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{WP}")
				(number "12")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0A")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P0W")
				(number "9")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P0B")
				(number "10")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P1A")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P1W")
				(number "6")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P1B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4251-xxxx-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.508 18.288 0)
		)
		(property "Value" "MCP4251-xxxx-P"
			(at -0.508 20.32 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22060b.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "Dual 8 Bit Digital Pot, SPI, Volatile Memory, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP4251-xxxx-P_0_1")
		(symbol "MCP4251-xxxx-P_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input clock
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "3")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDO")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "12")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{WP}")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0A")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P0W")
				(number "9")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P0B")
				(number "10")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P1A")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P1W")
				(number "6")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P1B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4251-xxxx-SL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.508 18.288 0)
		)
		(property "Value" "MCP4251-xxxx-SL"
			(at -0.508 20.32 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22060b.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "Dual 8 Bit Digital Pot, SPI, Volatile Memory, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP4251-xxxx-SL_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input clock
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "3")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDO")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "12")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{WP}")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0A")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P0W")
				(number "9")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P0B")
				(number "10")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P1A")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P1W")
				(number "6")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P1B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4251-xxxx-ST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.508 18.288 0)
		)
		(property "Value" "MCP4251-xxxx-ST"
			(at -0.508 20.32 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22060b.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "Dual 8 Bit Digital Pot, SPI, Volatile Memory, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP4251-xxxx-ST_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin input clock
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "3")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDO")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "12")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{WP}")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0A")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P0W")
				(number "9")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P0B")
				(number "10")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P1A")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P1W")
				(number "6")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P1B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP4431-xxxx-ST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "MCP4431-xxxx-ST"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22267A_MCP4431.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "Quad 7 Bit Digital Potentiometer, I²C, Volatile Memory, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer DigiPot"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP4431-xxxx-ST_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "P0B")
				(number "13")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "P0W")
				(number "12")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "P0A")
				(number "11")
			)
		)
		(symbol "MCP4431-xxxx-ST_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "P1B")
				(number "8")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "P1W")
				(number "9")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "P1A")
				(number "10")
			)
		)
		(symbol "MCP4431-xxxx-ST_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "P2B")
				(number "18")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "P2W")
				(number "19")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "P2A")
				(number "20")
			)
		)
		(symbol "MCP4431-xxxx-ST_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "P3B")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "P3W")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "P3A")
				(number "1")
			)
		)
		(symbol "MCP4431-xxxx-ST_5_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "HVC/A0")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "16")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP45HV51-MQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "MCP45HV51-MQ"
			(at 11.43 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm"
			(at 40.64 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005304A.pdf"
			(at -13.97 11.43 0)
		)
		(property "Description" "7/8-bit single +36V (±18V) digital pot, I2C serial interface, volatile memory, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Potentiometer pot digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP45HV51-MQ_0_1")
		(symbol "MCP45HV51-MQ_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "~{WLAT}")
				(number "6")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin passive line
				(at -12.7 -15.24 90)
				(length 2.54)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at -10.16 -15.24 90)
				(length 2.54)
				(name "NC")
				(number "9")
			)
			(pin passive line
				(at -7.62 -15.24 90)
				(length 2.54)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VL")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V+")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "V-")
				(number "12")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "NC")
				(number "17")
			)
			(pin passive line
				(at 7.62 -15.24 90)
				(length 2.54)
				(name "NC")
				(number "18")
			)
			(pin passive line
				(at 10.16 -15.24 90)
				(length 2.54)
				(name "NC")
				(number "19")
			)
			(pin passive line
				(at 12.7 -15.24 90)
				(length 2.54)
				(name "NC")
				(number "20")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "P0A")
				(number "15")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 2.54)
				(name "P0W")
				(number "14")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "P0B")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP45HV51-ST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "MCP45HV51-ST"
			(at 11.43 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 27.94 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005304A.pdf"
			(at -13.97 11.43 0)
		)
		(property "Description" "7/8-bit single +36V (±18V) digital pot, I2C serial interface, volatile memory, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Potentiometer pot digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP45HV51-ST_0_1")
		(symbol "MCP45HV51-ST_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "~{WLAT}")
				(number "6")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "8")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VL")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V+")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "V-")
				(number "10")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "P0A")
				(number "13")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 2.54)
				(name "P0W")
				(number "12")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "P0B")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPL0401A-10-Q1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TPL0401A-10-Q1"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpl0401a-10-q1.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "128-TAPS Single-Channel Digital Potentiometer, I2C Interface, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PDSO*G*"
			(at 0 0 0)
		)
		(symbol "TPL0401A-10-Q1_0_1")
		(symbol "TPL0401A-10-Q1_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "H")
				(number "6")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "W")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "X9118"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 12.7 0)
		)
		(property "Value" "X9118"
			(at 2.54 12.7 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/x911/x9118.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "100k Digital Potentiometer, 1024 steps, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "X9118_0_0"
			(pin input clock
				(at -12.7 7.62 0)
				(length 3.81)
				(name "SCL")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "A0")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "A1")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "7")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "V+")
				(number "1")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "V-")
				(number "8")
			)
		)
		(symbol "X9118_0_1")
		(symbol "X9118_1_1"
			(pin input input_low
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "~{WP}")
				(number "5")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "RH0")
				(number "12")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "RW0")
				(number "11")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "RL0")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "X9250"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 22.86 0)
		)
		(property "Value" "X9250"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.intersil.com/content/dam/Intersil/documents/x925/x9250.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 100k Digital Potentiometer, 256 steps, TSSOP-24/SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "potentiometer resistor variable digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm* TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "X9250_0_0"
			(pin input clock
				(at -12.7 15.24 0)
				(length 3.81)
				(name "SCL")
				(number "23")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "SIN")
				(number "13")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "A1")
				(number "14")
			)
			(pin input input_low
				(at -12.7 2.54 0)
				(length 3.81)
				(name "~{CS}")
				(number "11")
			)
			(pin input input_low
				(at -12.7 0 0)
				(length 3.81)
				(name "~{HOLD}")
				(number "24")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "V-")
				(number "19")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "18")
			)
		)
		(symbol "X9250_0_1")
		(symbol "X9250_1_1"
			(pin output line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "SOUT")
				(number "1")
			)
			(pin input input_low
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "~{WP}")
				(number "12")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "RH0")
				(number "9")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "RW0")
				(number "10")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "RL0")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "RH1")
				(number "16")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "RW1")
				(number "17")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "RL1")
				(number "15")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "RH2")
				(number "21")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "RW2")
				(number "20")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "RL2")
				(number "22")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "RH3")
				(number "4")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 3.81)
				(name "RW3")
				(number "3")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 3.81)
				(name "RL3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "X9258"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 22.86 0)
		)
		(property "Value" "X9258"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/x925/x9258.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 50k Digital Potentiometer, 256 steps, TSSOP-24/SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "potentiometer resistor variable digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm* TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "X9258_0_0"
			(pin input clock
				(at -12.7 17.78 0)
				(length 3.81)
				(name "SCL")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "SDA")
				(number "13")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "A1")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "A2")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "A3")
				(number "24")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "V-")
				(number "19")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "18")
			)
		)
		(symbol "X9258_0_1")
		(symbol "X9258_1_1"
			(pin input input_low
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "~{WP}")
				(number "12")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "RH0")
				(number "9")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "RW0")
				(number "10")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "RL0")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "RH1")
				(number "16")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "RW1")
				(number "17")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "RL1")
				(number "15")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "RH2")
				(number "21")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "RW2")
				(number "20")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "RL2")
				(number "22")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "RH3")
				(number "4")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 3.81)
				(name "RW3")
				(number "3")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 3.81)
				(name "RL3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD5253"
		(extends "AD5254")
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "AD5253"
			(at 1.27 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5253_5254.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Digital potentiometer, 64 position, 4 output, I2C interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5274BCP"
		(extends "AD5272BCP")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AD5274BCP"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-WD-10-1EP_3x3mm_P0.5mm_EP1.64x2.38mm"
			(at 33.02 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5272_5274.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital potentiometer, 256 position, 1% Resistor Tolerance, I2C interface, LFCSP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AD5274BRM"
		(extends "AD5272BRM")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AD5274BRM"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 19.05 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD5272_5274.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital potentiometer, 256 position, 1% Resistor Tolerance, I2C interface, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5438"
		(extends "MAX5436")
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "MAX5438"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX5436-MAX5439.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Drift Digital Potentiometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital potentiometer resistor variable"
			(at 0 0 0)
		)
	)
	(symbol "MCP4021-xxxxMS"
		(extends "MCP4011-xxxxMS")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4021-xxxxMS"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21945e.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Digital Potentiometer with WiperLock™ Technology, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4021-xxxxSN"
		(extends "MCP4011-xxxxSN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4021-xxxxSN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21945e.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Digital Potentiometer with WiperLock™ Technology, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4022-xxxxCH"
		(extends "MCP4012-xxxxCH")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4022-xxxxCH"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21945e.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Digital Potentiometer with WiperLock™ Technology, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4023-xxxxCH"
		(extends "MCP4013-xxxxCH")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4023-xxxxCH"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21945e.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Digital Potentiometer with WiperLock™ Technology, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4024-xxxxOT"
		(extends "MCP4014-xxxxOT")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP4024-xxxxOT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21945e.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Low-Cost 64-Step Digital Potentiometer with WiperLock™ Technology, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer Up Down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP41050"
		(extends "MCP41010")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP41050"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11195c.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Digital Potentiometer, SPI interface, 256 taps, 50 kohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "R POT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP41100"
		(extends "MCP41010")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP41100"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11195c.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Digital Potentiometer, SPI interface, 256 taps, 100 kohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "R POT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4141-xxxx-P"
		(extends "MCP4131-xxxx-P")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "MCP4141-xxxx-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22059b.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Single Digital Potentiometer, SPI interface, 129 taps, 5/10/50/100 kohm, non-volatile memory"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "digipot EE 7-bit 7bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4142-xxxx-P"
		(extends "MCP4132-xxxx-P")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "MCP4142-xxxx-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22059b.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Single Digital Rheostat, SPI interface, 129 taps, 5/10/50/100 kohm, non-volatile memory"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "potentiometer digipot EE 7-bit 7bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4151-xxxx-P"
		(extends "MCP4131-xxxx-P")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "MCP4151-xxxx-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22060b.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Single Digital Potentiometer, SPI interface, 257 taps, 5/10/50/100 kohm, volatile memory"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "digipot RAM 8-bit 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4152-xxxx-P"
		(extends "MCP4132-xxxx-P")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "MCP4152-xxxx-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22060b.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Single Digital Rheostat, SPI interface, 257 taps, 5/10/50/100 kohm, volatile memory"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "potentiometer digipot RAM 8-bit 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4161-xxxx-P"
		(extends "MCP4131-xxxx-P")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "MCP4161-xxxx-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22059b.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Single Digital Potentiometer, SPI interface, 257 taps, 5/10/50/100 kohm, non-volatile memory"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "digipot EE 8-bit 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4162-xxxx-P"
		(extends "MCP4132-xxxx-P")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "MCP4162-xxxx-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/22059b.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Single Digital Rheostat, SPI interface, 257 taps, 5/10/50/100 kohm, non-volatile memory"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "potentiometer digipot EE 8-bit 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP42050"
		(extends "MCP42010")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MCP42050"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11195c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual Digital Potentiometer, SPI interface, 256 taps, 50 kohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "R POT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP42100"
		(extends "MCP42010")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MCP42100"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11195c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual Digital Potentiometer, SPI interface, 256 taps, 100 kohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "R POT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4441-xxxx-ST"
		(extends "MCP4431-xxxx-ST")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "MCP4441-xxxx-ST"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 3.4798 -4.9276 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22267A_MCP4431.pdf"
			(at 3.4798 -7.4676 0)
		)
		(property "Description" "Quad 7 Bit Digital Potentiometer, I²C, Nonvolatile Memory, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer DigiPot"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4451-xxxx-ST"
		(extends "MCP4431-xxxx-ST")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "MCP4451-xxxx-ST"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 3.4798 -4.9276 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22267A_MCP4431.pdf"
			(at 3.4798 -7.4676 0)
		)
		(property "Description" "Quad 8 Bit Digital Potentiometer, I²C, Volatile Memory, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer DigiPot"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP4461-xxxx-ST"
		(extends "MCP4431-xxxx-ST")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "MCP4461-xxxx-ST"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 3.4798 -4.9276 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22267A_MCP4431.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad 8 Bit Digital Potentiometer, I²C, Nonvolatile Memory, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer DigiPot"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP45HV31-MQ"
		(extends "MCP45HV51-MQ")
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "MCP45HV31-MQ"
			(at 11.43 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm"
			(at 40.64 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005304A.pdf"
			(at -13.97 11.43 0)
		)
		(property "Description" "7/8-bit single +36V (±18V) digital pot, I2C serial interface, volatile memory, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Potentiometer pot digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP45HV31-ST"
		(extends "MCP45HV51-ST")
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "MCP45HV31-ST"
			(at 11.43 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 27.94 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005304A.pdf"
			(at -13.97 11.43 0)
		)
		(property "Description" "7/8-bit single +36V (±18V) digital pot, I2C serial interface, volatile memory, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Potentiometer pot digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPL0401B-10-Q1"
		(extends "TPL0401A-10-Q1")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TPL0401B-10-Q1"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpl0401a-10-q1.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "128-TAPS Single-Channel Digital Potentiometer, I2C Interface, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Pot Potentiometer I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PDSO*G*"
			(at 0 0 0)
		)
	)
)
