(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AAT4610BIGV-1-T1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -6.35 0)
		)
		(property "Value" "AAT4610BIGV-1-T1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/201937A.pdf"
			(at -1.27 7.62 0)
		)
		(property "Description" "Current Limited Load Switch, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AAT4610BIGV-1-T1_0_1")
		(symbol "AAT4610BIGV-1-T1_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ON")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SET")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AAT4610BIGV-T1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -6.35 0)
		)
		(property "Value" "AAT4610BIGV-T1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/201937A.pdf"
			(at -1.27 7.62 0)
		)
		(property "Description" "Current Limited Load Switch, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active Low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AAT4610BIGV-T1_0_1")
		(symbol "AAT4610BIGV-T1_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{ON}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SET")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AAT4616IGV-1-T1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -6.35 0)
		)
		(property "Value" "AAT4616IGV-1-T1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/AAT4616_201940E.pdf"
			(at -1.27 7.62 0)
		)
		(property "Description" "Adjustable Current Limited Load Switch, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AAT4616IGV-1-T1_0_1")
		(symbol "AAT4616IGV-1-T1_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ON")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SET")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AAT4616IGV-T1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -6.35 0)
		)
		(property "Value" "AAT4616IGV-T1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/AAT4616_201940E.pdf"
			(at -1.27 7.62 0)
		)
		(property "Description" "Adjustable Current Limited Load Switch, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active Low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AAT4616IGV-T1_0_1")
		(symbol "AAT4616IGV-T1_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{ON}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SET")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM1270ACPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 -15.24 0)
		)
		(property "Value" "ADM1270ACPZ"
			(at 2.54 -15.24 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.5x1.5mm"
			(at 3.81 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM1270.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "High Voltage Input Protection Device"
			(at 1.27 0 0)
		)
		(property "ki_keywords" "high-voltage mosfet-driver hot-swap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LFCSP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADM1270ACPZ_0_1")
		(symbol "ADM1270ACPZ_1_0"
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
		)
		(symbol "ADM1270ACPZ_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "UV")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "OV")
				(number "4")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "RPFG")
				(number "16")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VCAP")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ENABLE")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ISET")
				(number "2")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin input line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "SENSE-")
				(number "14")
			)
			(pin output line
				(at 7.62 15.24 270)
				(length 2.54)
				(name "GATE")
				(number "13")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FLB")
				(number "11")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB_PG")
				(number "10")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "TIMER")
				(number "8")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TIMER_OFF")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PWRGD")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM1270ARQZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 -15.24 0)
		)
		(property "Value" "ADM1270ARQZ"
			(at 2.54 -15.24 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 3.81 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM1270.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "High Voltage Input Protection Device"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-voltage mosfet-driver hot-swap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ADM1270ARQZ_0_1")
		(symbol "ADM1270ARQZ_1_0"
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
		)
		(symbol "ADM1270ARQZ_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "UV")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "OV")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "RPFG")
				(number "2")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VCAP")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ENABLE")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ISET")
				(number "4")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "SENSE-")
				(number "16")
			)
			(pin output line
				(at 7.62 15.24 270)
				(length 2.54)
				(name "GATE")
				(number "15")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FLB")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB_PG")
				(number "12")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "TIMER")
				(number "10")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TIMER_OFF")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PWRGD")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2161W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP2161W"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2161.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active Low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP2161W_0_1")
		(symbol "AP2161W_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FLG}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2171W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP2171W"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2161.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP2171W_0_1")
		(symbol "AP2171W_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FLG}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP22913CN4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.255 0)
		)
		(property "Value" "AP22913CN4"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.89x0.89mm_Layout2x2_P0.5mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22913.pdf"
			(at 0 0 0)
		)
		(property "Description" "Slew rate controlled load switch, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lead control switch slew rate"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.89x0.89mm*Layout2x2*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AP22913CN4_0_1")
		(symbol "AP22913CN4_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "A2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ON")
				(number "B2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "B1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "A1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS1041R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS1041R"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-AUIPS1041-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aae14a0524c63"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power Low Side Switch, 39V, 4.5A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "low side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "AUIPS1041R_0_1")
		(symbol "AUIPS1041R_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS1042G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS1042G"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-AUIPS1041-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aae14a0524c63"
			(at 0 0 0)
		)
		(property "Description" "Dual Channel Intelligent Power Low Side Switch, 39V, 4.5A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual low side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AUIPS1042G_0_1")
		(symbol "AUIPS1042G_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN1")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "D1")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "D1")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "S1")
				(number "1")
			)
		)
		(symbol "AUIPS1042G_2_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN2")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "D2")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "D2")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "S2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS1051L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS1051L"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips1051.pdf?fileId=5546d462533600a4015355a4710712fc"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power Low Side Switch, 39V, 2.8A, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "low side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "AUIPS1051L_0_1")
		(symbol "AUIPS1051L_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS6011R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS6011R"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips6011.pdf?fileId=5546d462533600a4015355a787bf1309"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power High Side Switch, 39V, 60A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "AUIPS6011R_0_1")
		(symbol "AUIPS6011R_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "DG")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS6041G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS6041G"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips6041.pdf?fileId=5546d462533600a4015355a7a0251315"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power High Side Switch, 39V, 7A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AUIPS6041G_0_1")
		(symbol "AUIPS6041G_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "DG")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "6")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "8")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS6044G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS6044G"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips6044g.pdf?fileId=5546d462533600a4015355a7a8e4131a"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power High Side Switch, 39V, 7A, SOIC-28W"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AUIPS6044G_0_1")
		(symbol "AUIPS6044G_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "DG1")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "28")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT1")
				(number "25")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT1")
				(number "26")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT1")
				(number "27")
			)
		)
		(symbol "AUIPS6044G_2_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN2")
				(number "6")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "DG2")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND2")
				(number "7")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT2")
				(number "22")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT2")
				(number "23")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT2")
				(number "24")
			)
		)
		(symbol "AUIPS6044G_3_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN3")
				(number "9")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "DG3")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND3")
				(number "8")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT3")
				(number "19")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT3")
				(number "20")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT3")
				(number "21")
			)
		)
		(symbol "AUIPS6044G_4_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN4")
				(number "12")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "DG4")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND4")
				(number "13")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT4")
				(number "16")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT4")
				(number "17")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT4")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS7081S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS7081S"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips7081.pdf?fileId=5546d462533600a4015355a7b8d5131e"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power High Side Switch, 70V, 5A, D2PAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "AUIPS7081S_0_1")
		(symbol "AUIPS7081S_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "DG")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS7111S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS7111S"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips7111s.pdf?fileId=5546d462533600a4015355a7c94e1326"
			(at 0 0 0)
		)
		(property "Description" "Current Sense High Side Switch, 65V, 30A, D2PAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "AUIPS7111S_0_1")
		(symbol "AUIPS7111S_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "IFB")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS7121R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS7121R"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/auips7121.pdf?fileId=5546d462533600a4015355a7d1721328"
			(at 0 0 0)
		)
		(property "Description" "Current Sense High Side Switch, 65V, 50A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "AUIPS7121R_0_1")
		(symbol "AUIPS7121R_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "IFB")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS7142G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS7142G"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips7142g.pdf?fileId=5546d462533600a4015355a7ef451330"
			(at 0 0 0)
		)
		(property "Description" "Dual Channels Current Sense High Side Switch, 65V, 20A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AUIPS7142G_0_1")
		(symbol "AUIPS7142G_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "IFB1")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "8")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "9")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT1")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT1")
				(number "14")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT1")
				(number "15")
			)
		)
		(symbol "AUIPS7142G_2_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "IFB2")
				(number "6")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT2")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT2")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT2")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS71451G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS71451G"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips71451g.pdf?fileId=5546d462533600a4015355a7f7461332"
			(at 0 0 0)
		)
		(property "Description" "Current Sense High Side Switch, 65V, 4A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AUIPS71451G_0_1")
		(symbol "AUIPS71451G_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "IFB")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "6")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "8")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIPS7221R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "AUIPS7221R"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips7221r.pdf?fileId=5546d462533600a4015355a80e761338"
			(at 0 0 0)
		)
		(property "Description" "PWM Intelligent Power High Side Switch, 75V, 25A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "AUIPS7221R_0_1")
		(symbol "AUIPS7221R_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "Cb")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AUIR33402S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "AUIR33402S"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auir33402s.pdf?fileId=5546d462533600a4015355a88074135c"
			(at 0 0 0)
		)
		(property "Description" "Protected High Side Switch, 18V, 33A, D2PAK-7L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin4*"
			(at 0 0 0)
		)
		(symbol "AUIR33402S_0_1")
		(symbol "AUIR33402S_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "IFB")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_out line
				(at 0 -7.62 90)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "Cb")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD2222G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.826 -6.35 0)
		)
		(property "Value" "BD2222G"
			(at 0 6.604 0)
		)
		(property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm"
			(at 0 -20.828 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/power_switch/bd2242g-e.pdf"
			(at 0.254 -18.796 0)
		)
		(property "Description" "Adjustable current limit high side switch IC, active-high enable, 2.8..5.5V, 0.2..1.7A, 89mOhm Ron, TSOP-6"
			(at 0 -16.764 0)
		)
		(property "ki_keywords" "USB power-distribution ROHM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*6*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "BD2222G_0_0"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
		)
		(symbol "BD2222G_1_0"
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "ILIM")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{OC}")
				(number "4")
			)
		)
		(symbol "BD2222G_1_1")
		(embedded_fonts no)
	)
	(symbol "BD2243G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.826 -6.35 0)
		)
		(property "Value" "BD2243G"
			(at 0 6.604 0)
		)
		(property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm"
			(at 0 -20.828 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/power_switch/bd2242g-e.pdf"
			(at 0.254 -18.796 0)
		)
		(property "Description" "Adjustable current limit high side switch IC, active-low enable, output discharge, 2.8..5.5V, 0.2..1.7A, 89mOhm Ron, TSOP-6"
			(at 0 -16.764 0)
		)
		(property "ki_keywords" "USB power-distribution ROHM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*6*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "BD2243G_0_0"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
		)
		(symbol "BD2243G_1_0"
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "3")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "ILIM")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{OC}")
				(number "4")
			)
		)
		(symbol "BD2243G_1_1")
		(embedded_fonts no)
	)
	(symbol "BD48ExxG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "BD48ExxG"
			(at -5.08 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.rohm.de/datasheet/BD4830FVE/bd48xxg-e"
			(at 0 -15.24 0)
		)
		(property "Description" "Standard CMOS Voltage Detector IC, Open Drain Output, SSOP5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage detector open drain SSOP5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT-23*5*"
			(at 0 0 0)
		)
		(symbol "BD48ExxG_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD48KxxG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "BD48KxxG"
			(at -5.08 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.rohm.de/datasheet/BD4830FVE/bd48xxg-e"
			(at 0 -15.24 0)
		)
		(property "Description" "Standard CMOS Voltage Detector IC, Open Drain Output, SSOP3(1pin GND)"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage detector open drain SSOP3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT-23*"
			(at 0 0 0)
		)
		(symbol "BD48KxxG_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD48LxxG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "BD48LxxG"
			(at -5.08 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.rohm.de/datasheet/BD4830FVE/bd48xxg-e"
			(at 0 -15.24 0)
		)
		(property "Description" "Standard CMOS Voltage Detector IC, Open Drain Output, SSOP3(3pin GND)"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage detector open drain SSOP3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT-23*"
			(at 0 0 0)
		)
		(symbol "BD48LxxG_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD48xxFVE"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "BD48xxFVE"
			(at -5.08 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:VSOF5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.rohm.de/datasheet/BD4830FVE/bd48xxg-e"
			(at 0 -15.24 0)
		)
		(property "Description" "Standard CMOS Voltage Detector IC, Open Drain Output, VSOF5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage detector open drain VSOF5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSOF*5*"
			(at 0 0 0)
		)
		(symbol "BD48xxFVE_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24230RGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "BQ24230RGT"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 2.54 -32.385 0)
		)
		(property "Datasheet" "http://www.ti.com/cn/lit/ds/symlink/bq24230.pdf"
			(at -6.35 19.05 0)
		)
		(property "Description" "USB-Friendly Lithium-Ion Battery Charger And Power-Path Management IC, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lithium-ion battery charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BQ24230RGT_0_1")
		(symbol "BQ24230RGT_1_1"
			(pin power_in line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN")
				(number "13")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "ILIM")
				(number "12")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "ISET")
				(number "16")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "TMR")
				(number "14")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN2")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN1")
				(number "6")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "TS")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "BAT")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "BAT")
				(number "3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_out line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "CHG")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PGOOD")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CE")
				(number "4")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "TD")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTN8982TA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 6.35 5.715 0)
		)
		(property "Value" "BTN8982TA"
			(at 6.35 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at -5.08 11.43 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTN8982TA-DS-v01_00-EN.pdf?fileId=db3a30433fa9412f013fbe32289b7c17"
			(at -1.27 0.254 0)
		)
		(property "Description" "High Current PN Half Bridge, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge for motor drive applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*TabPin8*"
			(at 0 0 0)
		)
		(symbol "BTN8982TA_0_1")
		(symbol "BTN8982TA_1_0"
			(text "Ctrl"
				(at -2.54 0 900)
			)
		)
		(symbol "BTN8982TA_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "INH")
				(number "3")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IS")
				(number "6")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "SR")
				(number "5")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTS40K2-1EJC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS40K2-1EJC"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-8-43"
			(at -20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS40K2-1EJC-DS-v01_00-EN.pdf?fileId=5546d462518ffd85015254ee4e601f99"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 200mOhm, 1.5A, 36V, DSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*DSO*43*"
			(at 0 0 0)
		)
		(symbol "BTS40K2-1EJC_0_1")
		(symbol "BTS40K2-1EJC_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DEN")
				(number "3")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IS")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VS")
				(number "9")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTS462TATMA1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "BTS462TATMA1"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS462T-DS-v01_01-EN.pdf?fileId=5546d4625a888733015aa9b0294035f6"
			(at 0 -22.86 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 100mOhm, 3.5A, 34V, TO-252-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power load switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "BTS462TATMA1_0_0"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vbb")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTS50010-1TAD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS50010-1TAD"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin4"
			(at 21.59 -7.62 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS50010-1TAD-DS-v01_00-EN.pdf?fileId=5546d462576f34750157c38810ca55cd"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 1mOhm, 40A, 18V, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "BTS50010 PROFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*TabPin4*"
			(at 0 0 0)
		)
		(symbol "BTS50010-1TAD_0_1")
		(symbol "BTS50010-1TAD_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IS")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vbb")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTS50055-1TMA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS50055-1TMA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin4"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS50055-1TMA-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa9b00de935ed"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 6mOhm, 70A, 34V, TO220-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "BTS50055 PROFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*TabPin4*"
			(at 0 0 0)
		)
		(symbol "BTS50055-1TMA_0_1")
		(symbol "BTS50055-1TMA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IS")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vbb")
				(number "4")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTS50080-1TEA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS50080-1TEA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS50080-1TEA-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa435f2d2115b"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 16mOhm, 10A, 30V, TO252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
		(symbol "BTS50080-1TEA_0_1")
		(symbol "BTS50080-1TEA_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IS")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vbb")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTS7004-1EPP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "BTS7004-1EPP"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-TSDSO-14-22"
			(at -22.86 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS7004-1EPP-DS-v01_00-EN.pdf?fileId=5546d4626102d35a016147550a725555"
			(at 0 -12.7 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, One Channel, 12V, 15A, Rds(on) 4.4mΩ, PG-TSDSO-14-22"
			(at 0 0 0)
		)
		(property "ki_keywords" "BTS7004"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*TSDSO*22*"
			(at 0 0 0)
		)
		(symbol "BTS7004-1EPP_0_1")
		(symbol "BTS7004-1EPP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DEN")
				(number "3")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IS")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VS")
				(number "15")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "10")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "13")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "14")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTS724G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "BTS724G"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SO:Infineon_SOIC-20W_7.6x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS724G-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa3a2f1030ff1"
			(at -1.905 2.54 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, 4 Channel, RON 90mOhm, IL(NOM) 3.3A, Vbb 5.5...40V, standby current 9 µA (Tj = -40...25°C), SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "High_Side_Switch ESD CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*7.6*12.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BTS724G_0_1")
		(symbol "BTS724G_1_1"
			(pin open_collector line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "ST1/2")
				(number "4")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "ST3/4")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN3")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN4")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1/2")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VBB")
				(number "1")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "10")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "11")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "15")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "16")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "19")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "20")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND3/4")
				(number "6")
			)
			(pin open_emitter line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "18")
			)
			(pin open_emitter line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "17")
			)
			(pin open_emitter line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "14")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT4")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAP002DG"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP002DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 825V, <=500nF, 1.5MOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CAP002DG_0_1")
		(symbol "CAP002DG_1_1"
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1210"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "DS1210"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1210.pdf"
			(at -2.54 -2.54 0)
		)
		(property "Description" "Nonvolatile Controller, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Nonvolatile, RAM, Controller, Battery, Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DS1210_0_1")
		(symbol "DS1210_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VBAT1")
				(number "2")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VBAT2")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "TOL")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{CE}")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCCI")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VCCO")
				(number "1")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{CEO}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPC23102"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 9.398 22.352 0)
		)
		(property "Value" "EPC23102"
			(at 9.144 19.558 0)
		)
		(property "Footprint" "Package_DFN_QFN:EPC_QFN-13-3EP_3.5x5mm_P0.5mm"
			(at 0 43.18 0)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC23102_datasheet.pdf"
			(at 0 38.1 0)
		)
		(property "Description" "GaN Half-Bridge Power-Stage with Integrated Gate-Drivers, 80 V, 35 A, EPC_QFN-13-3EP"
			(at -0.254 47.244 0)
		)
		(property "ki_keywords" "smart fast switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EPC?QFN*3EP*3.5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EPC23102_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "RDRV")
				(number "6")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SD")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "HSIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "LSIN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDRV")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "AGND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "PGND")
				(number "8")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VBOOT")
				(number "13")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RBOOT")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VPHASE")
				(number "11")
			)
			(pin power_out line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SW")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FPF2000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FPF2000"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FPF2001-D.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Single power-distribution switcher, current limit = 50mA, blanking time = 10 ms, auto-restart time = 80 ms, ON Pin Polarity = HIGH, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "FPF2000_0_1")
		(symbol "FPF2000_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ON")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FLAGB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HF81"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "HF81"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.monolithicpower.com/DesktopModules/DocumentManage/API/Document/getDocument?id=142"
			(at 0 0 0)
		)
		(property "Description" "X capacitor bleeder, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "X capacitor discharge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HF81_0_1")
		(symbol "HF81_1_1"
			(pin no_connect line
				(at -2.54 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "L1")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "L1")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "L2")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "L2")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA3221"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "INA3221"
			(at 5.08 17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 0 27.94 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina3221.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "Triple-Channel High-Side Shunt and Bus Voltage Monitor with I2C and SMBUS Compatible Interface, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shunt and Bus voltage monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGV0016A*"
			(at 0 0 0)
		)
		(symbol "INA3221_0_1")
		(symbol "INA3221_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN+1")
				(number "12")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN-1")
				(number "11")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN+2")
				(number "15")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN-2")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN+3")
				(number "2")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN-3")
				(number "1")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VS")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VPU")
				(number "16")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PV")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "CRITICAL")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "WARNING")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "TC")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A0")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPS6011PBF"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS6011PBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6011pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 60A, Intelligent Power Switch High Side, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "IPS6011PBF_0_0"
			(text "CTRL"
				(at -1.651 0 0)
			)
		)
		(symbol "IPS6011PBF_0_1")
		(symbol "IPS6011PBF_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "DG")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 5.08 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin output line
				(at 5.08 -7.62 90)
				(length 3.81)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPS6011RPBF"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 8.255 1.905 0)
		)
		(property "Value" "IPS6011RPBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 8.255 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6011pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 60A, Intelligent Power Switch High Side, D-PAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "IPS6011RPBF_0_0"
			(text "CTRL"
				(at -1.651 0 0)
			)
		)
		(symbol "IPS6011RPBF_0_1")
		(symbol "IPS6011RPBF_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "DG")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 5.08 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin output line
				(at 5.08 -7.62 90)
				(length 3.81)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPS6011SPBF"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS6011SPBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6011pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 60A, Intelligent Power Switch High Side, D2-PAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "IPS6011SPBF_0_0"
			(text "CTRL"
				(at -1.524 0 0)
			)
		)
		(symbol "IPS6011SPBF_0_1")
		(symbol "IPS6011SPBF_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "DG")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 5.08 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin output line
				(at 5.08 -7.62 90)
				(length 3.81)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPS6041GPBF"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 9.525 2.54 0)
		)
		(property "Value" "IPS6041GPBF"
			(at 9.525 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 9.525 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6041pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 5A, Intelligent Power Switch High Side, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IPS6041GPBF_0_0"
			(text "CTRL"
				(at -1.651 0 0)
			)
		)
		(symbol "IPS6041GPBF_0_1")
		(symbol "IPS6041GPBF_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "DG")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin power_in line
				(at 5.08 7.62 270)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 5.08 -7.62 90)
				(length 3.81)
				(name "OUT")
				(number "4")
			)
			(pin power_in line
				(at 7.62 7.62 270)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPS7091GPBF"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 10.16 2.54 0)
		)
		(property "Value" "IPS7091GPBF"
			(at 10.16 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 10.16 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips7091.pdf"
			(at 0 0 0)
		)
		(property "Description" "70V, 5A, Intelligent Power Switch High Side, D2-PAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IPS7091GPBF_0_0"
			(text "CTRL"
				(at -1.651 0 0)
			)
		)
		(symbol "IPS7091GPBF_0_1")
		(symbol "IPS7091GPBF_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "DG")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 3.81)
				(name "~")
				(number "6")
			)
			(pin power_in line
				(at 5.08 7.62 270)
				(length 3.81)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 5.08 -7.62 90)
				(length 3.81)
				(name "OUT")
				(number "4")
			)
			(pin power_in line
				(at 7.62 7.62 270)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPS7091PBF"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS7091PBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips7091.pdf"
			(at 0 0 0)
		)
		(property "Description" "70V, 5A, Intelligent Power Switch High Side, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "IPS7091PBF_0_0"
			(text "CTRL"
				(at -1.651 0 0)
			)
		)
		(symbol "IPS7091PBF_0_1")
		(symbol "IPS7091PBF_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "DG")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 5.08 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin output line
				(at 5.08 -7.62 90)
				(length 3.81)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPS7091SPBF"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS7091SPBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips7091.pdf"
			(at 0 0 0)
		)
		(property "Description" "70V, 5A, Intelligent Power Switch High Side, D2-PAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "IPS7091SPBF_0_0"
			(text "CTRL"
				(at -1.651 0 0)
			)
		)
		(symbol "IPS7091SPBF_0_1")
		(symbol "IPS7091SPBF_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "DG")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 5.08 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin output line
				(at 5.08 -7.62 90)
				(length 3.81)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS25751L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "IRS25751L"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs25751lpbf.pdf?fileId=5546d462533600a40153567b31da2837"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Start-Up IC, 480V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "start up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "IRS25751L_0_1")
		(symbol "IRS25751L_1_1"
			(pin power_out line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VTH")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "ENN")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "COM")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ITS5215"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 0 12.7 0)
		)
		(property "Value" "ITS5215"
			(at 0 -10.16 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-12-9_ThermalVias"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-ITS5215L-DS-v01_01-en.pdf?fileId=db3a304412b407950112b428dba73e98"
			(at -1.905 0 0)
		)
		(property "Description" "Smart Dual Channel High Side Powertrain Switch (90mOhm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "High_Side_Switch Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PG?DSO*"
			(at 0 0 0)
		)
		(symbol "ITS5215_0_1")
		(symbol "ITS5215_1_1"
			(pin open_collector line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "ST1")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "IN1")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 5.08)
				(name "ST2")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "IN2")
				(number "4")
			)
			(pin power_in line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VBB")
				(number "12")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VBB")
				(number "13")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 5.08)
				(name "VBB")
				(number "6")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 5.08)
				(name "OUT1")
				(number "10")
			)
			(pin open_emitter line
				(at 10.16 -7.62 180)
				(length 5.08)
				(name "OUT2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5050-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "LM5050-1"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5050-1-q1.pdf"
			(at 27.94 -1.27 0)
		)
		(property "Description" "High side OR-ing FET controller, 5V to 75V operation, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "positive high-side or-ing ideal-diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LM5050-1_0_1")
		(symbol "LM5050-1_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "OFF")
				(number "3")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "VS")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5050-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "LM5050-2"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5050-2.pdf"
			(at 27.94 -1.27 0)
		)
		(property "Description" "High side OR-ing FET controller, 6V to 75V operation, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "positive high-side or-ing ideal-diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LM5050-2_0_1")
		(symbol "LM5050-2_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "OFF")
				(number "3")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{FGD}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5051"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM5051"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5051.pdf"
			(at 10.16 -1.27 0)
		)
		(property "Description" "Low side OR-ing FET controller, -6V to -100V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative low-side or-ing ideal-diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM5051_0_1")
		(symbol "LM5051_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "OFF")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{FGD}")
				(number "4")
			)
			(pin input line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "INN")
				(number "6")
			)
			(pin output line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "INP")
				(number "7")
			)
			(pin power_in line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Line")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5060"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -11.43 0)
		)
		(property "Value" "LM5060"
			(at 1.27 -11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 5.08 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5060.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "High side protection controller, +5.5V to +65V operation, VSSOP-10 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-voltage mosfet-driver hot-swap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM5060_0_1")
		(symbol "LM5060_1_0"
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
		)
		(symbol "LM5060_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "UVLO")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OVP")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "SENSE")
				(number "1")
			)
			(pin output line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "10")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "OUT")
				(number "9")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "TIMER")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{PGD}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM50672NPAR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM50672NPAR"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5067.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative Hot Swap / Inrush Current Controller with Power Limiting, SOIC-14W"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-voltage mosfet-driver hot-swap Texas Instruments"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM50672NPAR_0_1")
		(symbol "LM50672NPAR_1_0"
			(pin power_in line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "VEE")
				(number "6")
			)
		)
		(symbol "LM50672NPAR_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "UVLO")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "OVLO")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "TIMER")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PWR")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "SENSE")
				(number "9")
			)
			(pin output line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "GATE")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "PGD")
				(number "14")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5067MM-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5067MM-1"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5067.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative Hot Swap / Inrush Current Controller with Power Limiting, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-voltage mosfet-driver hot-swap Texas Instruments LM5067MM-1/NOPB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM5067MM-1_0_1")
		(symbol "LM5067MM-1_1_0"
			(pin power_in line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "VEE")
				(number "5")
			)
		)
		(symbol "LM5067MM-1_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "UVLO")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "OVLO")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "TIMER")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PWR")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "SENSE")
				(number "7")
			)
			(pin output line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "PGD")
				(number "10")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM66100DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.096 0)
		)
		(property "Value" "LM66100DCK"
			(at 0.254 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm66100.pdf"
			(at 0 -1.016 0)
		)
		(property "Description" "Ideal Diode With Input Polarity Protection 1.5 - 5.5V  Input Voltage, 1.5A Output Current, Ron 141 mOhm, SC-70-6"
			(at 0 -18.034 0)
		)
		(property "ki_keywords" "Texas Instruments"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "LM66100DCK_0_1")
		(symbol "LM66100DCK_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{CE}")
				(number "3")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "ST")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM74700"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.525 -8.89 0)
		)
		(property "Value" "LM74700"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at -9.525 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/LM74700-Q1"
			(at -9.525 -8.89 0)
		)
		(property "Description" "Low Iq reverse battery protection ideal diode controller, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM74700_0_1")
		(symbol "LM74700_1_1"
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VCAP")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at -7.62 10.16 270)
				(length 2.54)
				(name "ANODE")
				(number "6")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "CATHODE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMG3410"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 6.35 5.08 0)
		)
		(property "Value" "LMG3410"
			(at 6.35 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RWH0032A_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/snosd10c/snosd10c.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "600-V 12-A Integrated GaN Power Stage, RWH0032A"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RWH0032A*"
			(at 0 0 0)
		)
		(symbol "LMG3410_0_1")
		(symbol "LMG3410_1_0"
			(text "GaN Driver"
				(at 0 -1.27 900)
			)
		)
		(symbol "LMG3410_1_1"
			(pin output line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "32")
			)
			(pin power_out line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "LDO5V")
				(number "25")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{LPM}")
				(number "29")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IN")
				(number "31")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "RDRV")
				(number "30")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "BBSW")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -12.7 0)
				(length 2.54)
				(name "VNEG")
				(number "26")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "27")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "18")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "19")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "23")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "24")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMG5200"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 6.35 5.08 0)
		)
		(property "Value" "LMG5200"
			(at 6.35 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_MOF0009A"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmg5200.pdf"
			(at 0 0 0)
		)
		(property "Description" "80-V, 10-A GaN Half-Bridge Power Stage, MOF0009A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MOF0009A*"
			(at 0 0 0)
		)
		(symbol "LMG5200_0_1")
		(symbol "LMG5200_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "HB")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "HS")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HI")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LI")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "7")
			)
			(pin passive line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1641-1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 -11.43 0)
		)
		(property "Value" "LT1641-1"
			(at 3.81 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/164112fc.pdf"
			(at 6.35 -12.7 0)
		)
		(property "Description" "High voltage hot swap controller, +9V to +80V, with latching feature, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-voltage hot-swap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1641-1_0_1")
		(symbol "LT1641-1_1_0"
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(symbol "LT1641-1_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ON")
				(number "1")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "TIMER")
				(number "5")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "Vcc")
				(number "8")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "Sense")
				(number "7")
			)
			(pin output line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PWRGD")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT4230xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT4230xDD"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4320fb.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Ideal Diode Bridge Controller, DC to 60Hz, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode bridge replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT4230xDD_0_1")
		(symbol "LT4230xDD_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "TG1")
				(number "7")
			)
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN1")
				(number "8")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "BG2")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "OUTP")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "OUTN")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "OUTN")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "TG2")
				(number "2")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "IN2")
				(number "1")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "BG1")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT4231xUF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "LT4231xUF"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4321f.pdf"
			(at -1.27 15.24 0)
		)
		(property "Description" "PoE Ideal Diode Bridge Controller, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTPoE++ dual diode bridge replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT4231xUF_0_1")
		(symbol "LT4231xUF_1_1"
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "TG36")
				(number "1")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "TG12")
				(number "16")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN12")
				(number "15")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN36")
				(number "2")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "BG12")
				(number "14")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "BG36")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "OUTP")
				(number "12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "OUTN")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "OUTN")
				(number "9")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{EN}")
				(number "10")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "TG45")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "TG78")
				(number "5")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IN45")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IN78")
				(number "6")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "BG78")
				(number "7")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "BG45")
				(number "8")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "EN")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4242xUHF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.684 32.004 0)
		)
		(property "Value" "LTC4242xUHF"
			(at 8.128 32.004 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-38-1EP_5x7mm_P0.5mm_EP3.15x5.15mm"
			(at 0 -38.608 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4242f.pdf"
			(at 0 -36.576 0)
		)
		(property "Description" "Dual Slot Hot Swap Controller for PCI Express, WQFN-38"
			(at 0 -34.544 0)
		)
		(property "ki_keywords" "Power-Controller PCIe"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WQFN*5x7mm*P0.5mm*EP3.15x5.15mm*"
			(at 0 0 0)
		)
		(symbol "LTC4242xUHF_0_1")
		(symbol "LTC4242xUHF_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "AUXIN1")
				(number "6")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "AUXIN2")
				(number "8")
			)
			(pin open_collector line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "~{FAULT1}")
				(number "35")
			)
			(pin open_collector line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{FAULT2}")
				(number "17")
			)
			(pin open_collector line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{PGOOD1}")
				(number "33")
			)
			(pin open_collector line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{PGOOD2}")
				(number "19")
			)
			(pin open_collector line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{AUXFAULT1}")
				(number "34")
			)
			(pin open_collector line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{AUXFAULT2}")
				(number "18")
			)
			(pin open_collector line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "~{AUXPGOOD1}")
				(number "32")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{AUXPGOOD2}")
				(number "20")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{EN1}")
				(number "36")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{EN2}")
				(number "16")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "AUXON1")
				(number "1")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "AUXON2")
				(number "13")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "ON1")
				(number "38")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "ON2")
				(number "14")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "FON1")
				(number "37")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "FON2")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "EPAD")
				(number "39")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "26")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "AUXOUT1")
				(number "27")
			)
			(pin open_collector line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "3V_OUT1")
				(number "2")
			)
			(pin power_in line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "3V_IN1")
				(number "5")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "3V_SENSE1")
				(number "4")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "3V_GATE1")
				(number "3")
			)
			(pin open_collector line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "12V_OUT1")
				(number "28")
			)
			(pin power_in line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "12V_IN1")
				(number "31")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "12V_SENSE1")
				(number "30")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "12V_GATE1")
				(number "29")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "AUXOUT2")
				(number "25")
			)
			(pin open_collector line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "3V_OUT2")
				(number "12")
			)
			(pin power_in line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "3V_IN2")
				(number "9")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "3V_SENSE2")
				(number "10")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "3V_GATE2")
				(number "11")
			)
			(pin open_collector line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "12V_OUT2")
				(number "24")
			)
			(pin power_in line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "12V_IN2")
				(number "21")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "12V_SENSE2")
				(number "22")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "12V_GATE2")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4357DCB"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "LTC4357DCB"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm"
			(at 6.35 -3.81 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4357fd.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Ideal diode controller, 9-80V operation, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4357DCB_0_1")
		(symbol "LTC4357DCB_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "7")
			)
			(pin power_in line
				(at 7.62 0 180)
				(length 2.54)
				(name "Vdd")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4357MS8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "LTC4357MS8"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 6.35 -3.81 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4357fd.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Ideal diode controller, 9-80V operation, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC4357MS8_0_1")
		(symbol "LTC4357MS8_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin output line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 7.62 0 180)
				(length 2.54)
				(name "Vdd")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4359-DCB"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "LTC4359-DCB"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm"
			(at 6.35 -3.81 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc4359.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Ideal diode controller with reverse input protection, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing reverse-protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4359-DCB_0_1")
		(symbol "LTC4359-DCB_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin input line
				(at 0 10.16 270)
				(length 2.54)
				(name "SRC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "6")
			)
			(pin output line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "Pad")
				(number "7")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4359-MS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "LTC4359-MS8"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 6.35 -3.81 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc4359.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Ideal diode controller with reverse input protection, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing reverse-protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC4359-MS8_0_1")
		(symbol "LTC4359-MS8_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at 0 10.16 270)
				(length 2.54)
				(name "SRC")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "Vss")
				(number "6")
			)
			(pin output line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "1")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4364CDE"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LTC4364CDE"
			(at 5.08 -11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4mm_P0.5mm_EP1.7x3.3mm"
			(at 5.08 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf"
			(at -11.43 8.89 0)
		)
		(property "Description" "Surge stopper with ideal diode, UV and OV protection, -40V to +80V, 0°C to +40°C, DFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing reverse-protection undervoltage overvoltage surge-stopper"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4364CDE_0_1")
		(symbol "LTC4364CDE_1_1"
			(pin power_in line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "UV")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OV")
				(number "9")
			)
			(pin output line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin input line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "TMR")
				(number "13")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "SOURCE")
				(number "4")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "DGATE")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin input line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "FB")
				(number "14")
			)
			(pin open_collector line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "ENOUT")
				(number "12")
			)
			(pin open_collector line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{FLT}")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4364CMS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LTC4364CMS"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-16_3x4.039mm_P0.5mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf"
			(at -11.43 8.89 0)
		)
		(property "Description" "Surge stopper with ideal diode, UV and OV protection, -40V to +80V, 0°C to +40°C, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing reverse-protection undervoltage overvoltage surge-stopper"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4364CMS_0_1")
		(symbol "LTC4364CMS_1_1"
			(pin power_in line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "UV")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OV")
				(number "11")
			)
			(pin output line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "HGATE")
				(number "6")
			)
			(pin input line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "TMR")
				(number "15")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "SOURCE")
				(number "5")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "DGATE")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin input line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "FB")
				(number "16")
			)
			(pin open_collector line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "ENOUT")
				(number "14")
			)
			(pin open_collector line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{FLT}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4364CS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LTC4364CS"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 5.08 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf"
			(at -11.43 8.89 0)
		)
		(property "Description" "Surge stopper with ideal diode, UV and OV protection -40V to +80V, 0°C to +40°C, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing reverse-protection undervoltage overvoltage surge-stopper"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC4364CS_0_1")
		(symbol "LTC4364CS_1_1"
			(pin power_in line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "UV")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OV")
				(number "11")
			)
			(pin output line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "HGATE")
				(number "6")
			)
			(pin input line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "TMR")
				(number "15")
			)
			(pin input line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "SOURCE")
				(number "5")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "DGATE")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin input line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "FB")
				(number "16")
			)
			(pin open_collector line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "ENOUT")
				(number "14")
			)
			(pin open_collector line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{FLT}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4365DDB"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4365DDB"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x3mm_P0.5mm_EP0.61x2.2mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4365fa.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "UV, OV and Reverse Supply Protection Controller, 50/60Hz noise rejection, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage undervoltage reverse-polarity protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4365DDB_0_1")
		(symbol "LTC4365DDB_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "Vin")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "UV")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OV")
				(number "2")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4365TS8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4365TS8"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
			(at -7.62 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4365fa.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "UV, OV and Reverse Supply Protection Controller, 50/60Hz noise rejection, TSOT23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage undervoltage reverse-polarity protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC4365TS8_0_1")
		(symbol "LTC4365TS8_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "UV")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OV")
				(number "3")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vout")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4365xTS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LTC4365xTS8"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4365fa.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "UV, OV and Reverse Supply Protection Controller, 50Hz/60Hz noise rejection, TSOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage undervoltage reverse-polarity protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC4365xTS8_0_1")
		(symbol "LTC4365xTS8_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "UV")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OV")
				(number "3")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4370xDE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "LTC4370xDE"
			(at 7.62 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-16-1EP_3x4mm_P0.45mm_EP1.7x3.3mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4370f.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "OR Controller Current Sharing Controller N-Channel 2:1, DFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing current sharing load balancing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x4mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "LTC4370xDE_0_1")
		(symbol "LTC4370xDE_1_1"
			(pin passive line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "RANGE")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{EN1}")
				(number "16")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "FETON1")
				(number "9")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CPO1")
				(number "11")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VIN1")
				(number "13")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "GATE1")
				(number "12")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "OUT1")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "COMP")
				(number "3")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{EN2}")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FETON2")
				(number "8")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "CPO2")
				(number "6")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VIN2")
				(number "4")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "GATE2")
				(number "5")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4370xMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "LTC4370xMS"
			(at 7.62 19.05 0)
		)
		(property "Footprint" "Package_SO:MSOP-16_3x4.039mm_P0.5mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4370f.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "OR Controller Current Sharing Controller N-Channel 2:1, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing current sharing load balancing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4370xMS_1_1"
			(pin passive line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "RANGE")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{EN1}")
				(number "16")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "FETON1")
				(number "9")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CPO1")
				(number "11")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VIN1")
				(number "13")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "GATE1")
				(number "12")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "OUT1")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "COMP")
				(number "3")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{EN2}")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FETON2")
				(number "8")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "CPO2")
				(number "6")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VIN2")
				(number "4")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "GATE2")
				(number "5")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4412xS6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LTC4412xS6"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4412fb.pdf"
			(at 53.34 -5.08 0)
		)
		(property "Description" "Low Loss PowerPath Controller, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC4412xS6_0_1")
		(symbol "LTC4412xS6_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CTL")
				(number "3")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "STAT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4417CGN"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "LTC4417CGN"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4417f.pdf"
			(at 17.78 -29.21 0)
		)
		(property "Description" "Prioritized PowerPath Controller, Selects Highest Priority Supply from Three Inputs, SSOP"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch power FET sequence"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP-24*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "LTC4417CGN_0_1")
		(symbol "LTC4417CGN_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "V1")
				(number "24")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "UV1")
				(number "4")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "OV1")
				(number "5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "V2")
				(number "23")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "UV2")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "OV2")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "V3")
				(number "22")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "UV3")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OV3")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "2")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "HYS")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "G1")
				(number "20")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "VS1")
				(number "21")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "G2")
				(number "18")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VS2")
				(number "19")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "G3")
				(number "16")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VS3")
				(number "17")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{VALID1}")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{VALID2}")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{VALID3}")
				(number "12")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "CAS")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4417CUF"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "LTC4417CUF"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4417f.pdf"
			(at 17.78 -29.21 0)
		)
		(property "Description" "Prioritized PowerPath Controller, Selects Highest Priority Supply from Three Inputs, QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch power FET sequence"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4417CUF_0_1")
		(symbol "LTC4417CUF_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "V1")
				(number "21")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "UV1")
				(number "1")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "OV1")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "V2")
				(number "20")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "UV2")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "OV2")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "V3")
				(number "19")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "UV3")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OV3")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "23")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "EN")
				(number "22")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "HYS")
				(number "24")
			)
			(pin power_in line
				(at -5.08 -25.4 90)
				(length 2.54)
				(name "PAD")
				(number "25")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "G1")
				(number "17")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "VS1")
				(number "18")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "G2")
				(number "15")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VS2")
				(number "16")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "G3")
				(number "13")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VS3")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{VALID1}")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{VALID2}")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{VALID3}")
				(number "9")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "CAS")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX14919xUP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "MAX14919xUP"
			(at 10.16 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.15x3.35mm"
			(at 0 29.21 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max14919-max14919a.pdf"
			(at 0 26.67 0)
		)
		(property "Description" "Industrial-Protected Quad-Channel Low-Side Switch, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "low side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX14919xUP_0_1")
		(symbol "MAX14919xUP_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "18")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN2")
				(number "17")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN3")
				(number "15")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN4")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "INRUSH")
				(number "1")
			)
			(pin open_collector line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "13")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "RCLIM")
				(number "11")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VL")
				(number "10")
			)
			(pin power_out line
				(at 0 15.24 270)
				(length 2.54)
				(name "V5")
				(number "19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT4")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "REV")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX8586"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MAX8586"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX8586.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "Single 1.2A USB Current Limiting Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-channel USB current limiting power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN?8?1EP*3x3mm*P0.65mm*EP1.55x2.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX8586_0_1")
		(symbol "MAX8586_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SEL")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ON")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ENRESET")
				(number "8")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ISET")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX9611"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 11.43 0)
		)
		(property "Value" "MAX9611"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max9611-max9612.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "High-Side, Current-Sense Amplifiers with 12-Bit ADC and Op Amp/Comparator, 0V to 60V Input Common-Mode Voltage Range, 2.7V to 5.5V Power-Supply Range, Compatible with 1.8V and 3.3V Logic, Noninverting Output, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "high common-mode voltage range inrush-current-limiter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX9611_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RS+")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "RS-")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SET")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{CC}")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "A0")
				(number "9")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "A1")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2007YM6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC2007YM6"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC20XX-Fixed-and-Adjustable-Current-Limiting-Power-Distribution-Switches-DS20006486B.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "5.5V, 2.1A, Adjustable Current Limiting Power Distribution Switch, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "current limiting power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MIC2007YM6_0_1")
		(symbol "MIC2007YM6_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CSLEW")
				(number "5")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ILIM")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2025-1YM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC2025-1YM"
			(at 13.97 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MIC2025-2075-Single-Channel-Power-Distribution-Switch-DS20006030A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-channel, high side, power distribution switch, 2.7V-5.5V, Active High Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MIC2025-1YM_0_1")
		(symbol "MIC2025-1YM_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FLG")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2025-1YMM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC2025-1YMM"
			(at 15.24 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 19.05 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MIC2025-2075-Single-Channel-Power-Distribution-Switch-DS20006030A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-channel, high side, power distribution switch, 2.7V-5.5V, Active High Output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MIC2025-1YMM_0_1")
		(symbol "MIC2025-1YMM_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FLG")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2026-1BN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MIC2026-1BN"
			(at 12.7 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2026.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-channel, high side, power distribution switch, 2.7V-5.5V, Active High Output, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MIC2026-1BN_0_1")
		(symbol "MIC2026-1BN_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "ENA")
				(number "1")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "FLGA")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ENB")
				(number "4")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FLGB")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "8")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2090-1YM5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 6.35 0)
		)
		(property "Value" "MIC2090-1YM5"
			(at 0.254 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -19.304 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC2090-1-Current-Limiting-Power-Distribution-Switches-DS20006611A.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Single-channel, high side, power distribution switch, 790mOhm Ron, auto-retry, 1.8V-5.5V, 50 mA, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution current limit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MIC2090-1YM5_0_1")
		(symbol "MIC2090-1YM5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FAULT")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2544-2YM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MIC2544-2YM"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -25.4 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20005725B.pdf"
			(at 5.08 -22.86 0)
		)
		(property "Description" "Programmable Current Sense High Side Switch, 2.7-5.5V, 1.5A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*"
			(at 0 0 0)
		)
		(symbol "MIC2544-2YM_0_0"
			(text "LOGIC"
				(at -0.635 4.445 0)
			)
			(text "CHARGE"
				(at -0.635 2.54 0)
			)
			(text "PUMP"
				(at -0.635 0.635 0)
			)
		)
		(symbol "MIC2544-2YM_0_1")
		(symbol "MIC2544-2YM_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "FLG")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ILIM")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "8")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IN")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NIS5420MTxTXG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NIS5420MTxTXG"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-10-1EP_3x3mm_P0.5mm_EP1.8x2.5mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/nis5420-d.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "ON Semi, +12V Electronic Fuse, 4.6A, WDFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V efuse resettable fuse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NIS5420MTxTXG_0_1")
		(symbol "NIS5420MTxTXG_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{CC}")
				(number "11")
			)
			(pin tri_state line
				(at -12.7 0 0)
				(length 2.54)
				(name "Enable/Fault")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "dV/dt")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "Source")
				(number "10")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "Source")
				(number "6")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "Source")
				(number "7")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "Source")
				(number "8")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "Source")
				(number "9")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "I_{Limit}")
				(number "4")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "I_{SENSE}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NPC45560-H"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "NPC45560-H"
			(at 13.97 -11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm"
			(at 0 13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP45560-D.PDF"
			(at 0 13.97 0)
		)
		(property "Description" "Controlled load switch with low Ron, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "load switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP?3x3mm?P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NPC45560-H_0_1")
		(symbol "NPC45560-H_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SR")
				(number "5")
			)
			(pin power_in line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PG")
				(number "6")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "12")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "11")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOUT")
				(number "10")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "9")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "8")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "BLEED")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PD70224"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "PD70224"
			(at 10.16 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microsemi_QFN-40-32-2EP_6x8mm_P0.5mm"
			(at 0.635 0 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/131677-pd70224-data-sheet"
			(at 0.635 3.81 0)
		)
		(property "Description" "Ideal Dual Diode Bridge, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ideal diode bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microsemi*QFN*6x8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PD70224_0_1")
		(symbol "PD70224_1_1"
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN1A")
				(number "15")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "IN1A")
				(number "16")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "IN1A")
				(number "27")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "IN1A")
				(number "28")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN1B")
				(number "20")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "IN1B")
				(number "21")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "IN1B")
				(number "22")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "IN1B")
				(number "23")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SUPP_SA")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "WA_EN")
				(number "29")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SUPP_SB")
				(number "14")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN2A")
				(number "11")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IN2A")
				(number "12")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IN2A")
				(number "31")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IN2A")
				(number "32")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IN2B")
				(number "4")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "IN2B")
				(number "5")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "IN2B")
				(number "6")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "IN2B")
				(number "7")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "24")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "25")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "26")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "33")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "18")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "19")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "34")
			)
			(pin power_in line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RT9701"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "RT9701"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.richtek.com/Products/Power%20Switch/RT9701?sc_lang=en"
			(at 0 0 0)
		)
		(property "Description" "100 milliohm power distribution switch, SOT-25"
			(at 0 0 0)
		)
		(property "ki_keywords" "power distribution switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "RT9701_0_1")
		(symbol "RT9701_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VIN/EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RT9742AGJ5F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "RT9742AGJ5F"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.richtek.com/assets/product_file/RT9742/DS9742-10.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "3A, Discharge, Active High EN, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "RT9742AGJ5F_0_1")
		(symbol "RT9742AGJ5F_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FLG}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RT9742BGJ5F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "RT9742BGJ5F"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.richtek.com/assets/product_file/RT9742/DS9742-10.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "3A, Discharge, Active Low EN, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "RT9742BGJ5F_0_1")
		(symbol "RT9742BGJ5F_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FLG}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN6505ADBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "SN6505ADBV"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn6505b.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Low Noise, 1A, Transformer Drivers for Isolated Power Supplies, 160 kHz, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Transformer Drivers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SN6505ADBV_0_1")
		(symbol "SN6505ADBV_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "D1")
				(number "1")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "D2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN6507DGQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 10.16 0)
		)
		(property "Value" "SN6507DGQ"
			(at 6.35 -10.16 0)
		)
		(property "Footprint" "Package_SO:HVSSOP-10-1EP_3x3mm_P0.5mm_EP1.57x1.88mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn6507.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low Noise, 0.5A, spread spectrum 36V Push-Pull-Transformer Drivers for Isolated Power Supplies, HVSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Transformer Drivers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SN6507DGQ_0_1")
		(symbol "SN6507DGQ_1_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "SS/ILIM")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SR")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DC")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
		)
		(symbol "SN6507DGQ_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW1")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SW2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM6600"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 15.24 0)
		)
		(property "Value" "STM6600"
			(at -2.54 12.7 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-12_2x3mm_P0.5mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/stm6600.pdf"
			(at -10.16 15.24 0)
		)
		(property "Description" "Smart push-button on/off controller, power-on lockout, Low Power, 1.6-5.5V, TDFN12"
			(at 0 0 0)
		)
		(property "ki_keywords" "push-button-controller low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM6600_0_1")
		(symbol "STM6600_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "~{SR}")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "~{PB}")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "C_SRD")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "PS_HOLD")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "Vcc")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin open_collector line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "~{INT}")
				(number "11")
			)
			(pin open_collector line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "~{RST}")
				(number "10")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "~{EN}/EN")
				(number "9")
			)
			(pin open_collector line
				(at 15.24 0 180)
				(length 3.81)
				(name "~{PB}_OUT")
				(number "8")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "~{VCC}_LO")
				(number "7")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "Vref")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiP32431DR3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "SiP32431DR3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vishay.com.hk/docs/66597/sip32431.pdf"
			(at 0 0 0)
		)
		(property "Description" "10 pA, Ultra Low Leakage and Quiescent Current, Load Switch with Reverse Blocking, High Enable, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Load switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "SiP32431DR3_0_1")
		(symbol "SiP32431DR3_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "ON")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiP32432DR3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "SiP32432DR3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vishay.com.hk/docs/66597/sip32431.pdf"
			(at 0 0 0)
		)
		(property "Description" "10 pA, Ultra Low Leakage and Quiescent Current, Load Switch with Reverse Blocking, Low Enable, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Load switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "SiP32432DR3_0_1")
		(symbol "SiP32432DR3_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{ON}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEA1708T"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 1.27 0)
		)
		(property "Value" "TEA1708T"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TEA1708TDS.pdf"
			(at 0 0 0)
		)
		(property "Description" "GreenChip X capacitor discharge IC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "X capacitor discharge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TEA1708T_0_1")
		(symbol "TEA1708T_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "TMR1")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "TMR2")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "HV1")
				(number "8")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "HV2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLE8102SG"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 0 12.7 0)
		)
		(property "Value" "TLE8102SG"
			(at 0 -10.16 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-12-11_ThermalVias"
			(at 0 -15.621 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-TLE8102SG-DS-v01_05-en.pdf?fileId=db3a304319c6f18c0119c8384bf90042"
			(at -1.27 -2.54 0)
		)
		(property "Description" "Smart Dual Channel Powertrain Switch 2x8A (max 360mOhm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low_Side_Switch Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PG?DSO*"
			(at 0 0 0)
		)
		(symbol "TLE8102SG_0_1")
		(symbol "TLE8102SG_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "IN1")
				(number "7")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "IN2")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "~{CS}")
				(number "8")
			)
			(pin input clock
				(at -10.16 0 0)
				(length 5.08)
				(name "SCLK")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "MOSI")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "MISO/ST2")
				(number "11")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "ISx/ST1/Fault")
				(number "4")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 5.08)
				(name "VDD")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 5.08)
				(name "OUT1")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "OUT2")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLE8104E"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 0 17.78 0)
		)
		(property "Value" "TLE8104E"
			(at 0 -15.24 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-20-30_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-TLE8104E-DS-v01_04-en.pdf?fileId=db3a304318f3fe2901190401cfda7f25"
			(at -1.905 -7.62 0)
		)
		(property "Description" "Smart Quad Channel Powertrain Switch 4x3A (In=1A, Ilim=3A, Ron=320mOhm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low_Side_Switch Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PG?DSO*"
			(at 0 0 0)
		)
		(symbol "TLE8104E_0_1")
		(symbol "TLE8104E_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "IN1")
				(number "9")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "IN2")
				(number "2")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "IN3")
				(number "19")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "IN4")
				(number "12")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PRG")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 5.08)
				(name "~{RST}")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "~{CS}")
				(number "6")
			)
			(pin input clock
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "SCLK")
				(number "16")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "MOSI")
				(number "17")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "MISO")
				(number "15")
			)
			(pin power_in line
				(at 10.16 15.24 180)
				(length 5.08)
				(name "VS")
				(number "4")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 5.08)
				(name "~{FAULT}")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 5.08)
				(name "OUT1")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "OUT2")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 5.08)
				(name "OUT3")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "OUT4")
				(number "18")
			)
			(pin power_in line
				(at 10.16 -12.7 180)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2041B"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.795 0)
		)
		(property "Value" "TPS2041B"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2041.pdf"
			(at -1.27 7.62 0)
		)
		(property "Description" "Single power-distribution switcher"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS2041B_0_1")
		(symbol "TPS2041B_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~{OC}")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{EN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IN")
				(number "5")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 5.08)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2042D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.795 0)
		)
		(property "Value" "TPS2042D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2042.pdf"
			(at -1.27 7.62 0)
		)
		(property "Description" "Dual power-distribution switcher"
			(at 0 0 0)
		)
		(property "ki_keywords" "2-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS2042D_0_1")
		(symbol "TPS2042D_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~{OC1}")
				(number "8")
			)
			(pin open_collector line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{OC2}")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{EN1}")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~{EN2}")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IN1")
				(number "2")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 5.08)
				(name "OUT1")
				(number "7")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "OUT2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2044D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.795 0)
		)
		(property "Value" "TPS2044D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2044.pdf"
			(at -1.27 7.62 0)
		)
		(property "Description" "Quad power-distribution switcher"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "4-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS2044D_0_1")
		(symbol "TPS2044D_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~{OC1}")
				(number "16")
			)
			(pin open_collector line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{OC2}")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{EN1}")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~{EN2}")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IN1")
				(number "2")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 5.08)
				(name "OUT1")
				(number "15")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "OUT2")
				(number "14")
			)
		)
		(symbol "TPS2044D_2_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~{OC3}")
				(number "12")
			)
			(pin open_collector line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{OC4}")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{EN3}")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "~{EN4}")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IN2")
				(number "6")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 5.08)
				(name "OUT3")
				(number "11")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "OUT4")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2051CDBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "TPS2051CDBV"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2051c.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "0.5A Current limited power switch, single channel, output discharge, reverse blocking, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS2051CDBV_0_1")
		(symbol "TPS2051CDBV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FLT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2054D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.795 0)
		)
		(property "Value" "TPS2054D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2044.pdf"
			(at -1.27 7.62 0)
		)
		(property "Description" "Quad power-distribution switcher"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "4-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS2054D_0_1")
		(symbol "TPS2054D_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~{OC1}")
				(number "16")
			)
			(pin open_collector line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{OC2}")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "EN1")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "EN2")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IN1")
				(number "2")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "OUT1")
				(number "15")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "OUT2")
				(number "14")
			)
		)
		(symbol "TPS2054D_2_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "~{OC3}")
				(number "12")
			)
			(pin open_collector line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{OC4}")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "EN3")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "EN4")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IN2")
				(number "6")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "OUT3")
				(number "11")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "OUT4")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2116DRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 9.144 0)
		)
		(property "Value" "TPS2116DRL"
			(at 0.508 -8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-583-8"
			(at 0 -22.352 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2116.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "2 Channnels Power Mux with Manual and Priority Switchover, 1.6-5.5V Input Voltage, 2.5A Output Current, Ron 40 mOhm, SOT-583-8"
			(at 0 -1.016 0)
		)
		(property "ki_keywords" "Texas-Instruments power-mux switchover"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?5?3*"
			(at 0 0 0)
		)
		(symbol "TPS2116DRL_0_1")
		(symbol "TPS2116DRL_1_0"
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "7")
			)
		)
		(symbol "TPS2116DRL_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN1")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PR1")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MODE")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VIN2")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ST")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS22810DRV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS22810DRV"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps22810.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.7-18V, 79mohms On-Resistance Load Switch With Thermal Protection, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "load switch thermal protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS22810DRV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "QOD")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS22917DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS22917DBV"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps22917.pdf"
			(at 1.27 -17.78 0)
		)
		(property "Description" "1V to 5.5V, 2A, 80mΩ Ultra-Low Leakage Load Switch, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-side power distribution switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS22917DBV_0_1")
		(symbol "TPS22917DBV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "CT")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ON")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "QOD")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS22929D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TPS22929D"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps22929d.pdf"
			(at -2.54 11.43 0)
		)
		(property "Description" "High side, power distribution switch, 1.4V-5.5V, 1.8A, SOT23-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-side power distribution switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS22929D_0_1")
		(symbol "TPS22929D_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ON")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS22993"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "TPS22993"
			(at 10.16 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_S-PWQFN-N20"
			(at 33.02 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps22993"
			(at -2.54 11.43 0)
		)
		(property "Description" "Quad Channel Load Switch with GPIO and I2C Control, Bias voltage: 4.5V-17.2V, Input voltage: 1.0V-3.6V, Max 1.2A per channel, WQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad channel power distribution/load switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PWQFN*"
			(at 0 0 0)
		)
		(symbol "TPS22993_0_1")
		(symbol "TPS22993_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "ON1")
				(number "10")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "ON2")
				(number "9")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "ON3")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "ON4")
				(number "7")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN1")
				(number "4")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN2")
				(number "2")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "VIN3")
				(number "14")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIN4")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SDA")
				(number "19")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SCL")
				(number "17")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "ADD1")
				(number "6")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "ADD2")
				(number "16")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "ADD3")
				(number "20")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VBIAS")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT1")
				(number "5")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOUT2")
				(number "1")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOUT3")
				(number "15")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VOUT4")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2412D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "TPS2412D"
			(at 5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 53.34 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2412.pdf"
			(at 53.34 -5.08 0)
		)
		(property "Description" "N+1 and ORing Power Rail Controller, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS2412D_0_1")
		(symbol "TPS2412D_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "BYP")
				(number "8")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin power_in line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "RSET")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2419D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "TPS2419D"
			(at 5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 53.34 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2419.pdf"
			(at 53.34 -5.08 0)
		)
		(property "Description" "N+1 and ORing Power Rail Controller with Enable, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS2419D_0_1")
		(symbol "TPS2419D_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "BYP")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "RSET")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2592xx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS2592xx"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm_ThermalVias"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps25925.pdf"
			(at -10.16 10.16 0)
		)
		(property "Description" "5V/12V eFuse Protection Switch (VSON-10)"
			(at 0 0 0)
		)
		(property "ki_keywords" "efuse protection switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS2592xx_0_1")
		(symbol "TPS2592xx_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "7")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "ILIM")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "dV/dT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS26630RGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TPS26630RGE"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
			(at -10.16 20.32 0)
		)
		(property "Description" "60V, 6A Power Limiting, Surge Protection Industrial eFuse, Adjustable Overvoltage cut-off, Active Current Limiting, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "efuse protection switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024H*"
			(at 0 0 0)
		)
		(symbol "TPS26630RGE_0_1")
		(symbol "TPS26630RGE_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "B_GATE")
				(number "3")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DRV")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "UVLO")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "OVP")
				(number "7")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "12")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "MODE")
				(number "11")
			)
			(pin no_connect line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "IN_SYS")
				(number "5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT")
				(number "17")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "18")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PGTH")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{FLT}")
				(number "14")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PGOOD")
				(number "16")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IMON")
				(number "13")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "ILIM")
				(number "10")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "dVdT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS26631PWP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TPS26631PWP"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.96x2.96mm_ThermalVias"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
			(at -10.16 20.32 0)
		)
		(property "Description" "60V, 6A Power Limiting, Surge Protection Industrial eFuse, Adjustable Overvoltage cut-off, Active Current Limiting with Pulse current support, HTTSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "efuse protection switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS26631PWP_0_1")
		(symbol "TPS26631PWP_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "B_GATE")
				(number "4")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DRV")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "UVLO")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "OVP")
				(number "8")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "13")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "MODE")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "IN_SYS")
				(number "6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT")
				(number "18")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "19")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "20")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PGTH")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{FLT}")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PGOOD")
				(number "17")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IMON")
				(number "14")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "ILIM")
				(number "11")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "dVdT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS26632RGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TPS26632RGE"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
			(at -10.16 20.32 0)
		)
		(property "Description" "60V, 6A Power Limiting, Surge Protection Industrial eFuse, 35V fixed Overvoltage clamp, Active Current Limiting, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "efuse protection switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024H*"
			(at 0 0 0)
		)
		(symbol "TPS26632RGE_0_1")
		(symbol "TPS26632RGE_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "B_GATE")
				(number "3")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DRV")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "UVLO")
				(number "6")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "12")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "MODE")
				(number "11")
			)
			(pin no_connect line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "IN_SYS")
				(number "5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT")
				(number "17")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "18")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PGTH")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{FLT}")
				(number "14")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PGOOD")
				(number "16")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IMON")
				(number "13")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PLIM")
				(number "7")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "ILIM")
				(number "10")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "dVdT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS26633PWP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TPS26633PWP"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.96x2.96mm_ThermalVias"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
			(at -10.16 20.32 0)
		)
		(property "Description" "60V, 6A Power Limiting, Surge Protection Industrial eFuse, 35V fixed Overvoltage clamp, Active Current Limiting with Pulse current support, HTTSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "efuse protection switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS26633PWP_0_1")
		(symbol "TPS26633PWP_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "B_GATE")
				(number "4")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DRV")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "UVLO")
				(number "7")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "13")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "MODE")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "IN_SYS")
				(number "6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT")
				(number "18")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "19")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "20")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PGTH")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{FLT}")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PGOOD")
				(number "17")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IMON")
				(number "14")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PLIM")
				(number "8")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "ILIM")
				(number "11")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "dVdT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSM102"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSM102"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tsm102.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Dual Operational Amplifier and Dual Comparator and 1% Voltage Reference, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp comparator reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TSM102_1_0"
			(text "COMP"
				(at 0 0 0)
			)
		)
		(symbol "TSM102_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "TSM102_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "TSM102_3_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "11")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(symbol "TSM102_4_0"
			(text "COMP"
				(at 0 0 0)
			)
		)
		(symbol "TSM102_4_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "14")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "15")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
		)
		(symbol "TSM102_5_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "V-")
				(number "13")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSM103W"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSM103W"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tsm103w.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Dual Operational Amplifier and 2.5V 1% Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TSM103W_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(symbol "TSM103W_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "TSM103W_2_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC39002D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "UCC39002D"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/slus495i/slus495i.pdf"
			(at 0 0 0)
		)
		(property "Description" "Advanced 8-Pin Load-Share Controller, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "load share controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UCC39002D_0_1")
		(symbol "UCC39002D_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CS+")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EAO")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "CS-")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "CSO")
				(number "8")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP22804AW5"
		(extends "AP2171W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22804AW5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22804_14.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 2.5A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP22804BW5"
		(extends "AP2161W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22804BW5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22804_14.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 2.5A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active Low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP22814AW5"
		(extends "AP2171W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22814AW5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22804_14.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 3A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP22814BW5"
		(extends "AP2161W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22814BW5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22804_14.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 3A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active Low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP22816AKEWT"
		(extends "AP2171W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22816AKEWT"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22816_17_18.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 1A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP22816BKEWT"
		(extends "AP2161W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22816BKEWT"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22816_17_18.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 1A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active Low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP22817AKEWT"
		(extends "AP2171W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22817AKEWT"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22816_17_18.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 1.5A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP22817BKEWT"
		(extends "AP2161W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22817BKEWT"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22816_17_18.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 1.5A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active Low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP22818AKEWT"
		(extends "AP2171W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22818AKEWT"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22816_17_18.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 2.0A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP22818BKEWT"
		(extends "AP2161W")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "AP22818BKEWT"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22816_17_18.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Current limited 2A power switch, single channel, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active Low"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS1052G"
		(extends "AUIPS1042G")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS1052G"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips1051.pdf?fileId=5546d462533600a4015355a4710712fc"
			(at 0 0 0)
		)
		(property "Description" "Dual Channel Intelligent Power Low Side Switch, 39V, 2.8A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual low side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS2031R"
		(extends "AUIPS1041R")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS2031R"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-AUIPS2031R-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aae1488334c5c"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power Low Side Switch, 68V, 10A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "low side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS2041L"
		(extends "AUIPS1051L")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS2041L"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-AUIPS2041-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aae147a9d4c57"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power Low Side Switch, 68V, 5A, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "low side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS2051L"
		(extends "AUIPS1051L")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS2051L"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-AUIPS2052G-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aae0b6fb04c51"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power Low Side Switch, 70V, 1.8A, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "low side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS2052G"
		(extends "AUIPS1042G")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS2052G"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-AUIPS2052G-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aae0b6fb04c51"
			(at 0 0 0)
		)
		(property "Description" "Dual Channel Intelligent Power Low Side Switch, 70V, 1.8A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual low side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS6031R"
		(extends "AUIPS6011R")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS6031R"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips6031.pdf?fileId=5546d462533600a4015355a797f51311"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power High Side Switch, 39V, 16A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS7081R"
		(extends "AUIPS6011R")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS7081R"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips7081.pdf?fileId=5546d462533600a4015355a7b8d5131e"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power High Side Switch, 70V, 5A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS7091G"
		(extends "AUIPS6041G")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS7091G"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips7091.pdf?fileId=5546d462533600a4015355a7c0d21322"
			(at 0 0 0)
		)
		(property "Description" "Intelligent Power High Side Switch, 70V, 5A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS7125R"
		(extends "AUIPS7121R")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS7125R"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips7125.pdf?fileId=5546d462533600a4015355a7d96a132a"
			(at 0 0 0)
		)
		(property "Description" "Current Sense High Side Switch, 65V, 50A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS7141R"
		(extends "AUIPS7121R")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS7141R"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips7141.pdf?fileId=5546d462533600a4015355a7e126132c"
			(at 0 0 0)
		)
		(property "Description" "Current Sense High Side Switch, 65V, 20A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS7145R"
		(extends "AUIPS7121R")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIPS7145R"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auips7145r.pdf?fileId=5546d462533600a4015355a7ff1a1334"
			(at 0 0 0)
		)
		(property "Description" "Current Sense High Side Switch, 65V, 20A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "AUIPS72211R"
		(extends "AUIPS7221R")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "AUIPS72211R"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-AUIPS72211R-DS-v01_10-EN.pdf?fileId=5546d4625a888733015aad6673cb4beb"
			(at 0 0 0)
		)
		(property "Description" "Low EMI PWM Intelligent Power High Side Switch, 75V, 20A, DPAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "AUIR3313S"
		(extends "AUIPS7111S")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIR3313S"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auir3313.pdf?fileId=5546d462533600a4015355a83e2d1347"
			(at 0 0 0)
		)
		(property "Description" "Programmable Current Sense High Side Switch, 32V, 90A, D2PAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AUIR3314S"
		(extends "AUIPS7111S")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIR3314S"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auir3314.pdf?fileId=5546d462533600a4015355a846b8134a"
			(at 0 0 0)
		)
		(property "Description" "Programmable Current Sense High Side Switch, 32V, 58A, D2PAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AUIR3315S"
		(extends "AUIPS7111S")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIR3315S"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auir3315.pdf?fileId=5546d462533600a4015355a84eda134d"
			(at 0 0 0)
		)
		(property "Description" "Programmable Current Sense High Side Switch, 32V, 30A, D2PAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AUIR3316S"
		(extends "AUIPS7111S")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIR3316S"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auir3316.pdf?fileId=5546d462533600a4015355a856f41350"
			(at 0 0 0)
		)
		(property "Description" "Low EMI Current Sense High Side Switch, 26V, 90A, D2PAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AUIR3320S"
		(extends "AUIPS7111S")
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "AUIR3320S"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/auir3320s.pdf?fileId=5546d462533600a4015355a867d01356"
			(at 0 0 0)
		)
		(property "Description" "Low EMI Current Sense High Side Switch, 26V, 55A, D2PAK-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "high side switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "BD2242G"
		(extends "BD2222G")
		(property "Reference" "U"
			(at -4.826 -6.35 0)
		)
		(property "Value" "BD2242G"
			(at 0 6.604 0)
		)
		(property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm"
			(at 0 -20.828 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/power_switch/bd2242g-e.pdf"
			(at 0.254 -18.796 0)
		)
		(property "Description" "Adjustable current limit high side switch IC, 2.8..5.5V, output discharge, active-high enable, 0.2..1.7A, 89mOhm Ron, TSOP-6"
			(at 0 -16.764 0)
		)
		(property "ki_keywords" "USB power-distribution ROHM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*6*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD49ExxG"
		(extends "BD48ExxG")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "BD49ExxG"
			(at -5.08 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.rohm.de/datasheet/BD4830FVE/bd48xxg-e"
			(at 0 -15.24 0)
		)
		(property "Description" "Standard CMOS Voltage Detector IC, CMOS Output, SSOP5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage detector cmos SSOP5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT-23*5*"
			(at 0 0 0)
		)
	)
	(symbol "BD49KxxG"
		(extends "BD48KxxG")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "BD49KxxG"
			(at -5.08 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.rohm.de/datasheet/BD4830FVE/bd48xxg-e"
			(at 0 -15.24 0)
		)
		(property "Description" "Standard CMOS Voltage Detector IC, CMOS Output, SSOP3(1pin GND)"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage detector cmos SSOP3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT-23*"
			(at 0 0 0)
		)
	)
	(symbol "BD49LxxG"
		(extends "BD48LxxG")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "BD49LxxG"
			(at -5.08 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.rohm.de/datasheet/BD4830FVE/bd48xxg-e"
			(at 0 -15.24 0)
		)
		(property "Description" "Standard CMOS Voltage Detector IC, CMOS Output, SSOP3(3pin GND)"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage detector cmos SSOP3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT-23*"
			(at 0 0 0)
		)
	)
	(symbol "BD49xxFVE"
		(extends "BD48xxFVE")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "BD49xxFVE"
			(at -5.08 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:VSOF5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.rohm.de/datasheet/BD4830FVE/bd48xxg-e"
			(at 0 -15.24 0)
		)
		(property "Description" "Standard CMOS Voltage Detector IC, CMOS Output, VSOF5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage detector cmos VSOF5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSOF*5*"
			(at 0 0 0)
		)
	)
	(symbol "BTS443P"
		(extends "BTS50080-1TEA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS443P"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS443P-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa9afbc5035d5"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 16mOhm, 7.6A, 36V, TO252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "BTS50055-1TMC"
		(extends "BTS50055-1TMA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS50055-1TMC"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin4"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS50055-1TMC-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa9b0007235e9"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 6mOhm, 17A, 34V, TO220-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "BTS50055 PROFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*TabPin4*"
			(at 0 0 0)
		)
	)
	(symbol "BTS50080-1TEB"
		(extends "BTS50080-1TEA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS50080-1TEB"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS50080-1TEB-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa435e5601157"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 16mOhm, 10A, 30V, TO252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "BTS50080-1TMA"
		(extends "BTS50055-1TMA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS50080-1TMA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin4"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS50080-1TMA-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa435d7fe1153"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 16mOhm, 9.5A, 38V, TO220-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "BTS50080 PROFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*TabPin4*"
			(at 0 0 0)
		)
	)
	(symbol "BTS50080-1TMC"
		(extends "BTS50055-1TMA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS50080-1TMC"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin4"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS50080_1TMC-DS-v01_00-en.pdf?fileId=db3a3043266237920126992737c951ee"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 16mOhm, 9.5A, 38V, TO220-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "BTS50080 PROFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*TabPin4*"
			(at 0 0 0)
		)
	)
	(symbol "BTS50085-1TMA"
		(extends "BTS50055-1TMA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS50085-1TMA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin4"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS50085-1TMA-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa435bccd114b"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 9mOhm, 11.1A, 58V, TO220-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "BTS50085 PROFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*TabPin4*"
			(at 0 0 0)
		)
	)
	(symbol "BTS5012SDA"
		(extends "BTS50080-1TEA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS5012SDA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS5012SDA-DS-v01_01-en.pdf?fileId=db3a30431d8a6b3c011db95c6eba237d"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 24mOhm, 6.5A, 20V, TO252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "BTS5014SDA"
		(extends "BTS50080-1TEA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS5014SDA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS5014SDA-DS-v01_01-EN.pdf?fileId=5546d4625a888733015aa42c708e1142"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 28mOhm, 6A, 20V, TO252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "BTS5016SDA"
		(extends "BTS50080-1TEA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS5016SDA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS5016SDA-DS-v01_01-EN.pdf?fileId=5546d4625a888733015aa41a6c38112d"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 32mOhm, 5.5A, 20V, TO252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "BTS5030-1EJA"
		(extends "BTS40K2-1EJC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS5030-1EJA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-8-43"
			(at -20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS5030-1EJA-DS-v02_20-EN.pdf?fileId=5546d46259d9a4bf015a84f3e686758a"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 30mOhm, 5A, 28V, DSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*DSO*43*"
			(at 0 0 0)
		)
	)
	(symbol "BTS5045-1EJA"
		(extends "BTS40K2-1EJC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS5045-1EJA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-8-43"
			(at -20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS5045-1EJA-DS-v02_02-EN.pdf?fileId=5546d4625a888733015aa411125b1069"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 45mOhm, 4A, 28V, DSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*DSO*43*"
			(at 0 0 0)
		)
	)
	(symbol "BTS5090-1EJA"
		(extends "BTS40K2-1EJC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS5090-1EJA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-8-43"
			(at -20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS5090-1EJA-DS-v02_02-EN.pdf?fileId=5546d4625a888733015aa410fc371059"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 90mOhm, 3A, 28V, DSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*DSO*43*"
			(at 0 0 0)
		)
	)
	(symbol "BTS5200-1EJA"
		(extends "BTS40K2-1EJC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS5200-1EJA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-8-43"
			(at -20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS5200-1EJA-DS-v01_00-EN.pdf?fileId=5546d46250cc1fdf0151636cd945402e"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 200mOhm, 1.5A, 28V, DSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*DSO*43*"
			(at 0 0 0)
		)
	)
	(symbol "BTS6133D"
		(extends "BTS50080-1TEA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS6133D"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS6133D-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa3e3286f102a"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 10mOhm, 8A, 38V, TO-252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "BTS6142D"
		(extends "BTS50080-1TEA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS6142D"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS6142D-DS-v01_01-EN.pdf?fileId=5546d4625a888733015aa3da1e0e1026"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 12mOhm, 7A, 24V, TO252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "BTS6143D"
		(extends "BTS50080-1TEA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS6143D"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS6143D-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa3da10821022"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 10mOhm, 8A, 38V, TO252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "BTS6163D"
		(extends "BTS50080-1TEA")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS6163D"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTS6163D-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa3da01a1101e"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 20mOhm, 5.5A, 62V, TO252-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "BTS6200-1EJA"
		(extends "BTS40K2-1EJC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "BTS6200-1EJA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-8-43"
			(at -20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BTT6200-1EJA-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa3756ec20fcc"
			(at 0 -10.16 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, Single, 200mOhm, 1.5A, 36V, DSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "infineon power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*DSO*43*"
			(at 0 0 0)
		)
	)
	(symbol "BTS711L1"
		(extends "BTS724G")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "BTS711L1"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SO:Infineon_SOIC-20W_7.6x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS711L1-DS-v01_03-EN.pdf?fileId=5546d4625a888733015aa3bea285100c"
			(at -1.905 2.54 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, 4 Channel, RON 200mOhm, IL(NOM) 1.9A, Vbb 5.0...34V, standby current 28 µA (Tj = 25°C), SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "High_Side_Switch ESD CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*7.6*12.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BTS712N1"
		(extends "BTS724G")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "BTS712N1"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SO:Infineon_SOIC-20W_7.6x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS712N1-DS-v01_03-EN.pdf?fileId=5546d4625a888733015aa3be77471000"
			(at -1.905 2.54 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, 4 Channel, RON 200mOhm, IL(NOM) 1.9A, Vbb 5.0...34V, standby current 180 µA (Tj = 25°C), SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "High_Side_Switch ESD CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*7.6*12.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BTS716G"
		(extends "BTS724G")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "BTS716G"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SO:Infineon_SOIC-20W_7.6x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS716G-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa3be86601004"
			(at -1.905 2.54 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, 4 Channel, RON 140mOhm, IL(NOM) 2.6A, Vbb 5.5...40V, standby current 9 µA (Tj = -40...25°C), undervoltage switch off 4.5V, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "High_Side_Switch ESD CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*7.6*12.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BTS721L1"
		(extends "BTS724G")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "BTS721L1"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SO:Infineon_SOIC-20W_7.6x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS721L1-DS-v01_03-EN.pdf?fileId=5546d4625a888733015aa3ac546f0ff9"
			(at -1.905 2.54 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, 4 Channel, RON 100mOhm, IL(NOM) 2.9A, Vbb 5.0...34V, standby current 28 µA (Tj = 25°C), SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "High_Side_Switch ESD CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*7.6*12.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP003DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP003DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 825V, <=750nF, 1.02MOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP004DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP004DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 825V, <=1uF, 780kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP005DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP005DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 825V, <=1.5uF, 480kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP006DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP006DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 825V, <=2uF, 360kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP007DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP007DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 825V, <=2.5uF, 300kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP008DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP008DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 825V, <=3.5uF, 200kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger 825V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP009DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP009DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 825V, <=5uF, 150kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP012DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP012DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 1000V, <=500nF, 1.5MOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP013DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP013DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 1000V, <=750nF, 1.02MOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP014DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP014DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 1000V, <=1uF, 780kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP015DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP015DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 1000V, <=1.5uF, 480kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP016DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP016DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 1000V, <=2uF, 360kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP017DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP017DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 1000V, <=2.5uF, 300kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP018DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP018DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 1000V, <=3.5uF, 200kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP019DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP019DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Automatic Capacitor Discarger, 1000V, <=5uF, 150kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP200DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP200DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/capzero-2_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Zero Loss Automatic Capacitor Discharge IC, 1000V, 100nF-6uF, 7.5M-142kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CAP300DG"
		(extends "CAP002DG")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "CAP300DG"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product_document/data_sheet/capzero-3_family_datasheet.pdf"
			(at 1.016 0 0)
		)
		(property "Description" "CapZero Zero Loss Automatic Capacitor Discharge IC, 1000V, 100nF-6uF, >=54kOhm, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automatic Capacitor Discarger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "EPC23103"
		(extends "EPC23102")
		(property "Reference" "U"
			(at 9.652 24.638 0)
		)
		(property "Value" "EPC23103"
			(at 9.652 22.098 0)
		)
		(property "Footprint" "Package_DFN_QFN:EPC_QFN-13-3EP_3.5x5mm_P0.5mm"
			(at 0 43.18 0)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC23103_datasheet.pdf"
			(at 0 38.1 0)
		)
		(property "Description" "GaN Half-Bridge Power-Stage with Integrated Gate-Drivers, 80 V, 25 A, EPC_QFN-13-3EP"
			(at -0.254 47.244 0)
		)
		(property "ki_keywords" "smart fast switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EPC?QFN*3EP*3.5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "EPC23104"
		(extends "EPC23102")
		(property "Reference" "U"
			(at 9.398 24.892 0)
		)
		(property "Value" "EPC23104"
			(at 9.144 22.098 0)
		)
		(property "Footprint" "Package_DFN_QFN:EPC_QFN-13-3EP_3.5x5mm_P0.5mm"
			(at 0 43.18 0)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC23104_datasheet.pdf"
			(at 0 38.1 0)
		)
		(property "Description" "GaN Half-Bridge Power-Stage with Integrated Gate-Drivers, 80 V, 15 A, EPC_QFN-13-3EP"
			(at -0.254 47.244 0)
		)
		(property "ki_keywords" "smart fast switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EPC?QFN*3EP*3.5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "FPF2001"
		(extends "FPF2000")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FPF2001"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FPF2001-D.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Single power-distribution switcher, current limit = 50mA, blanking time = 10 ms, auto-restart time = 80 ms, ON Pin Polarity = LOW, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "FPF2002"
		(extends "FPF2000")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FPF2002"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FPF2001-D.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Single power-distribution switcher, current limit = 50mA, blanking time = 10 ms, w/o auto-restart, ON Pin Polarity = HIGH, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "FPF2003"
		(extends "FPF2000")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FPF2003"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FPF2001-D.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Single power-distribution switcher, current limit = 50mA, blanking time = 0 ms, w/o auto-restart, ON Pin Polarity = HIGH, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "FPF2004"
		(extends "FPF2000")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FPF2004"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FPF2001-D.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Single power-distribution switcher, current limit = 100mA, blanking time = 10 ms, auto-restart time = 80 ms, ON Pin Polarity = HIGH, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "FPF2005"
		(extends "FPF2000")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FPF2005"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FPF2001-D.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Single power-distribution switcher, current limit = 100mA, blanking time = 10 ms, auto-restart time = 80 ms, ON Pin Polarity = LOW, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "FPF2006"
		(extends "FPF2000")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FPF2006"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FPF2001-D.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Single power-distribution switcher, current limit = 100mA, blanking time = 10 ms, w/o auto-restart, ON Pin Polarity = HIGH, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "FPF2007"
		(extends "FPF2000")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FPF2007"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 22.86 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FPF2001-D.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Single power-distribution switcher, current limit = 100mA, blanking time = 0 ms, w/o auto-restart, ON Pin Polarity = HIGH, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "1-chanel power-distribution USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "IPS6021PBF"
		(extends "IPS6011PBF")
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS6021PBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6021pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 32A, Intelligent Power Switch High Side, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IPS6021RPBF"
		(extends "IPS6011RPBF")
		(property "Reference" "Q"
			(at 8.255 1.905 0)
		)
		(property "Value" "IPS6021RPBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 8.255 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6021pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 32A, Intelligent Power Switch High Side, D-PAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "IPS6021SPBF"
		(extends "IPS6011SPBF")
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS6021SPBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6021pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 32A, Intelligent Power Switch High Side, D2-PAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "IPS6031PBF"
		(extends "IPS6011PBF")
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS6031PBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6031pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 16A, Intelligent Power Switch High Side, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IPS6031RPBF"
		(extends "IPS6011RPBF")
		(property "Reference" "Q"
			(at 8.255 1.905 0)
		)
		(property "Value" "IPS6031RPBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 8.255 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6031pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 16A, Intelligent Power Switch High Side, D-PAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "IPS6031SPBF"
		(extends "IPS6011SPBF")
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS6031SPBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6031pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 16A, Intelligent Power Switch High Side, D2-PAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "IPS6041PBF"
		(extends "IPS6011PBF")
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS6041PBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6041pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 5A, Intelligent Power Switch High Side, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IPS6041RPBF"
		(extends "IPS6011RPBF")
		(property "Reference" "Q"
			(at 8.255 1.905 0)
		)
		(property "Value" "IPS6041RPBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 8.255 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6041pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 5A, Intelligent Power Switch High Side, DPAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "IPS6041SPBF"
		(extends "IPS6011SPBF")
		(property "Reference" "Q"
			(at 8.255 2.54 0)
		)
		(property "Value" "IPS6041SPBF"
			(at 8.255 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 8.255 -2.54 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/ips6041pbf.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 5A, Intelligent Power Switch High Side, D2PAK 5pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Intelligent Power Switch High Side MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM5067MM-2"
		(extends "LM5067MM-1")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5067MM-2"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5067.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative Hot Swap / Inrush Current Controller with Power Limiting, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-voltage mosfet-driver hot-swap Texas Instruments LM5067MM-2/NOPB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM5067MMX-2"
		(extends "LM5067MM-1")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5067MMX-2"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5067.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative Hot Swap / Inrush Current Controller with Power Limiting, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-voltage mosfet-driver hot-swap Texas Instruments LM5067MM-1/NOPB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM5067MWX-1"
		(extends "LM50672NPAR")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5067MWX-1"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5067.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative Hot Swap / Inrush Current Controller with Power Limiting, SOIC-14W"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-voltage mosfet-driver hot-swap Texas Instruments LM5067MWX-1/NOPB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1641-2"
		(extends "LT1641-1")
		(property "Reference" "U"
			(at -5.08 -11.43 0)
		)
		(property "Value" "LT1641-2"
			(at 3.81 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/164112fc.pdf"
			(at 6.35 -12.7 0)
		)
		(property "Description" "High voltage hot swap controller, +9V to +80V operation, with auto-retry feature"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-voltage hot-swap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT4320xDD-1"
		(extends "LT4230xDD")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT4320xDD-1"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4320fb.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "Ideal Diode Bridge Controller, DC to 600Hz, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode bridge replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4364HDE"
		(extends "LTC4364CDE")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LTC4364HDE"
			(at 5.08 -11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4mm_P0.5mm_EP1.7x3.3mm"
			(at 5.08 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf"
			(at -11.43 8.89 0)
		)
		(property "Description" "Surge stopper with ideal diode, UV and OV protection -40V to +80V, -40°C to +125°C, DFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "surge overvoltage undervoltage reverse-polarity protection diode ORing MOSFET driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4364HMS"
		(extends "LTC4364CMS")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LTC4364HMS"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-16_3x4.039mm_P0.5mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf"
			(at -11.43 8.89 0)
		)
		(property "Description" "Surge stopper with ideal diode, UV and OV protection -40V to +80V, -40°C to +125°C, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "surge overvoltage undervoltage reverse-polarity protection diode ORing MOSFET driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4364HS"
		(extends "LTC4364CS")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LTC4364HS"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 5.08 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf"
			(at -11.43 8.89 0)
		)
		(property "Description" "Surge stopper with ideal diode, UV and OV protection -40V to +80V, -40°C to +125°C, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "surge overvoltage undervoltage reverse-polarity protection diode ORing MOSFET driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4364IDE"
		(extends "LTC4364CDE")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LTC4364IDE"
			(at 5.08 -11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4mm_P0.5mm_EP1.7x3.3mm"
			(at 5.08 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf"
			(at -11.43 8.89 0)
		)
		(property "Description" "Surge stopper with ideal diode, UV and OV protection -40V to +80V, -40°C to +85°C, DFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "surge overvoltage undervoltage reverse-polarity protection diode ORing MOSFET driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4364IMS"
		(extends "LTC4364CMS")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LTC4364IMS"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-16_3x4.039mm_P0.5mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf"
			(at -11.43 8.89 0)
		)
		(property "Description" "Surge stopper with ideal diode, UV and OV protection -40V to +80V, -40°C to +85°C, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "surge overvoltage undervoltage reverse-polarity protection diode ORing MOSFET driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4364IS"
		(extends "LTC4364CS")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LTC4364IS"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 5.08 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf"
			(at -11.43 8.89 0)
		)
		(property "Description" "Surge stopper with ideal diode, UV and OV protection -40V to +80V, -40°C to +85°C, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "surge overvoltage undervoltage reverse-polarity protection diode ORing MOSFET driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4365DDB-1"
		(extends "LTC4365DDB")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4365DDB-1"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x3mm_P0.5mm_EP0.61x2.2mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4365fa.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "UV, OV and Reverse Supply Protection Controller, 1ms fault recovery, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage undervoltage reverse-polarity protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4365TS8-1"
		(extends "LTC4365TS8")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4365TS8-1"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
			(at -7.62 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4365fa.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "UV, OV and Reverse Supply Protection Controller, 1ms fault recovery, TSOT23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage undervoltage reverse-polarity protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4417HGN"
		(extends "LTC4417CGN")
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "LTC4417HGN"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4417f.pdf"
			(at 17.78 -29.21 0)
		)
		(property "Description" "Prioritized PowerPath Controller, Selects Highest Priority Supply from Three Inputs, –40°C to 125°C, SSOP"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch power FET sequence"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP-24*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4417HUF"
		(extends "LTC4417CUF")
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "LTC4417HUF"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4417f.pdf"
			(at 17.78 -29.21 0)
		)
		(property "Description" "Prioritized PowerPath Controller, Selects Highest Priority Supply from Three Inputs, –40°C to 125°C, QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch power FET sequence"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4417IGN"
		(extends "LTC4417CGN")
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "LTC4417IGN"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4417f.pdf"
			(at 17.78 -29.21 0)
		)
		(property "Description" "Prioritized PowerPath Controller, Selects Highest Priority Supply from Three Inputs, –40°C to 85°C, SSOP"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch power FET sequence"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP-24*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4417IUF"
		(extends "LTC4417CUF")
		(property "Reference" "U"
			(at 0 26.035 0)
		)
		(property "Value" "LTC4417IUF"
			(at 0 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4417f.pdf"
			(at 17.78 -29.21 0)
		)
		(property "Description" "Prioritized PowerPath Controller, Selects Highest Priority Supply from Three Inputs, –40°C to 85°C, QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch power FET sequence"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX9612"
		(extends "MAX9611")
		(property "Reference" "U"
			(at -6.985 11.43 0)
		)
		(property "Value" "MAX9612"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max9611-max9612.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "High-Side, Current-Sense Amplifiers with 12-Bit ADC and Op Amp/Comparator, 0V to 60V Input Common-Mode Voltage Range, 2.7V to 5.5V Power-Supply Range, Compatible with 1.8V and 3.3V Logic, Inverting Output, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "high common-mode voltage range inrush-current-limiter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2008YM6"
		(extends "MIC2007YM6")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC2008YM6"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC20XX-Fixed-and-Adjustable-Current-Limiting-Power-Distribution-Switches-DS20006486B.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "5.5V, 2.1A, Adjustable Current Limiting Power Distribution Switch, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "current limiting power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2017YM6"
		(extends "MIC2007YM6")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC2017YM6"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC20XX-Fixed-and-Adjustable-Current-Limiting-Power-Distribution-Switches-DS20006486B.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "5.5V, 2.1A, Adjustable Current Limiting Power Distribution Switch, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "current limiting power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2018YM6"
		(extends "MIC2007YM6")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC2018YM6"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC20XX-Fixed-and-Adjustable-Current-Limiting-Power-Distribution-Switches-DS20006486B.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "5.5V, 2.1A, Adjustable Current Limiting Power Distribution Switch, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "current limiting power switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2025-2YM"
		(extends "MIC2025-1YM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC2025-2YM"
			(at 13.97 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MIC2025-2075-Single-Channel-Power-Distribution-Switch-DS20006030A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-channel, high side, power distribution switch, 2.7V-5.5V, Active Low Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2025-2YMM"
		(extends "MIC2025-1YMM")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC2025-2YMM"
			(at 15.24 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 19.05 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MIC2025-2075-Single-Channel-Power-Distribution-Switch-DS20006030A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-channel, high side, power distribution switch, 2.7V-5.5V, Active Low Output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2026-1xM"
		(extends "MIC2026-1BN")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MIC2026-1xM"
			(at 12.7 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC2026-MIC2076-Dual-Channel-Power-Distribution-Switch-DS20006443A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-channel, high side, power distribution switch, 2.7V-5.5V, Active High Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2026-2BN"
		(extends "MIC2026-1BN")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MIC2026-2BN"
			(at 12.7 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2026.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-channel, high side, power distribution switch, 2.7V-5.5V, Active Low Output, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2026-2xM"
		(extends "MIC2026-1BN")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MIC2026-2xM"
			(at 12.7 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC2026-MIC2076-Dual-Channel-Power-Distribution-Switch-DS20006443A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-channel, high side, power distribution switch, 2.7V-5.5V, Active Low Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2090-2YM5"
		(extends "MIC2090-1YM5")
		(property "Reference" "U"
			(at -7.874 6.35 0)
		)
		(property "Value" "MIC2090-2YM5"
			(at 0.254 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -19.304 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC2090-1-Current-Limiting-Power-Distribution-Switches-DS20006611A.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Single-channel, high side, power distribution switch, 790mOhm Ron, latch-off on current limit, 1.8V-5.5V, 50 mA, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution current limit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2091-1YM5"
		(extends "MIC2090-1YM5")
		(property "Reference" "U"
			(at -7.874 6.35 0)
		)
		(property "Value" "MIC2091-1YM5"
			(at 0.254 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -19.304 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC2090-1-Current-Limiting-Power-Distribution-Switches-DS20006611A.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Single-channel, high side, power distribution switch, 790mOhm Ron, auto-retry feature, 1.8V-5.5V, 100 mA, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution current limit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2091-2YM5"
		(extends "MIC2090-1YM5")
		(property "Reference" "U"
			(at -7.874 6.35 0)
		)
		(property "Value" "MIC2091-2YM5"
			(at 0.254 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -19.304 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC2090-1-Current-Limiting-Power-Distribution-Switches-DS20006611A.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Single-channel, high side, power distribution switch, 790mOhm Ron, latch-off on current limit, 1.8V-5.5V, 100 mA, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet distribution current limit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2587-1"
		(extends "LT1641-1")
		(property "Reference" "U"
			(at -5.08 -11.43 0)
		)
		(property "Value" "MIC2587-1"
			(at 3.81 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2587-87r.pdf"
			(at 6.35 -12.7 0)
		)
		(property "Description" "Positive high voltage hot swap controller +10V to +80V with latched operation"
			(at 0 0 0)
		)
		(property "ki_keywords" "power switch FET driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2587R-1"
		(extends "LT1641-1")
		(property "Reference" "U"
			(at -5.08 -11.43 0)
		)
		(property "Value" "MIC2587R-1"
			(at 3.81 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2587-87r.pdf"
			(at 6.35 -12.7 0)
		)
		(property "Description" "Positive high voltage hot swap controller +10V to +80V with auto-retry operation"
			(at 0 0 0)
		)
		(property "ki_keywords" "power switch FET driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NPC45560-L"
		(extends "NPC45560-H")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "NPC45560-L"
			(at 13.97 -11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm"
			(at 0 13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP45560-D.PDF"
			(at 0 13.97 0)
		)
		(property "Description" "Controlled load switch with low Ron, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "load switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DFN*12*"
			(at 0 0 0)
		)
	)
	(symbol "RT9742ANGJ5F"
		(extends "RT9742AGJ5F")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "RT9742ANGJ5F"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.richtek.com/assets/product_file/RT9742/DS9742-10.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "3A, Active High EN, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "RT9742BNGJ5F"
		(extends "RT9742BGJ5F")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "RT9742BNGJ5F"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.richtek.com/assets/product_file/RT9742/DS9742-10.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "3A, Active Low EN, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SN6505BDBV"
		(extends "SN6505ADBV")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "SN6505BDBV"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn6505b.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Low Noise, 1A, Transformer Drivers for Isolated Power Supplies, 420 kHz, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Transformer Drivers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "STM6601"
		(extends "STM6600")
		(property "Reference" "U"
			(at -2.54 15.24 0)
		)
		(property "Value" "STM6601"
			(at -2.54 12.7 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-12_2x3mm_P0.5mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/stm6600.pdf"
			(at -10.16 15.24 0)
		)
		(property "Description" "Smart push-button on/off controller, power-on lockout, Low Power, 1.6-5.5V, TDFN12"
			(at 0 0 0)
		)
		(property "ki_keywords" "push-button-controller low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS2065CDBV"
		(extends "TPS2051CDBV")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "TPS2065CDBV"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2051c.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "1A Current limited power switch, single channel, output discharge, reverse blocking, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS2065CDBVx-2"
		(extends "TPS2051CDBV")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "TPS2065CDBVx-2"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2051c.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "1A Current limited power switch, single channel, reverse blocking, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS2069CDBV"
		(extends "TPS2051CDBV")
		(property "Reference" "U"
			(at -7.62 -6.35 0)
		)
		(property "Value" "TPS2069CDBV"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2051c.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "1.5A Current limited power switch, single channel, output discharge, reverse blocking, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Limit USB Active High"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS2412PW"
		(extends "TPS2412D")
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "TPS2412PW"
			(at 5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 53.34 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2412.pdf"
			(at 53.34 -5.08 0)
		)
		(property "Description" "N+1 and ORing Power Rail Controller, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS2419PW"
		(extends "TPS2419D")
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "TPS2419PW"
			(at 5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 53.34 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2419.pdf"
			(at 53.34 -5.08 0)
		)
		(property "Description" "N+1 and ORing Power Rail Controller with Enable, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ideal-diode or-ing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS26631RGE"
		(extends "TPS26630RGE")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TPS26631RGE"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
			(at -10.16 20.32 0)
		)
		(property "Description" "60V, 6A Power Limiting, Surge Protection Industrial eFuse, Adjustable Overvoltage cut-off, Active Current Limiting with Pulse current support, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "efuse protection switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024H*"
			(at 0 0 0)
		)
	)
	(symbol "TPS26633RGE"
		(extends "TPS26632RGE")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TPS26633RGE"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
			(at -10.16 20.32 0)
		)
		(property "Description" "60V, 6A Power Limiting, Surge Protection Industrial eFuse, 35V fixed Overvoltage clamp, Active Current Limiting with Pulse current support, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "efuse protection switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024H*"
			(at 0 0 0)
		)
	)
	(symbol "TPS26635RGE"
		(extends "TPS26632RGE")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TPS26635RGE"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
			(at -10.16 20.32 0)
		)
		(property "Description" "60V, 6A Power Limiting, Surge Protection Industrial eFuse, 39V fixed Overvoltage clamp, Active Current Limiting with Pulse current support, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "efuse protection switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024H*"
			(at 0 0 0)
		)
	)
	(symbol "TPS26636PWP"
		(extends "TPS26633PWP")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "TPS26636PWP"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.96x2.96mm_ThermalVias"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
			(at -10.16 20.32 0)
		)
		(property "Description" "60V, 6A Power Limiting, Surge Protection Industrial eFuse, 35V fixed Overvoltage clamp, Active Current Limiting with Pulse current support, HTTSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "efuse protection switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSM102A"
		(extends "TSM102")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSM102A"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tsm102.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Dual Operational Amplifier and Dual Comparator and 0.4% Voltage Reference, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp comparator reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSM103WA"
		(extends "TSM103W")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TSM103WA"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/tsm103w.pdf"
			(at 1.27 5.08 0)
		)
		(property "Description" "Dual Operational Amplifier and 2.5V 0.4% Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual opamp reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BTS716GB"
		(extends "BTS716G")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "BTS716GB"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SO:Infineon_SOIC-20W_7.6x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS716GB-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa3be94e21008"
			(at -1.905 2.54 0)
		)
		(property "Description" "Smart High-Side Power Switch, PROFET, 4 Channel, RON 140mOhm, IL(NOM) 2.6A, Vbb 5.5...40V, standby current 9 µA (Tj = -40...25°C), undervoltage switch off 3.2V, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "High_Side_Switch ESD CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*7.6*12.*P1.27mm*"
			(at 0 0 0)
		)
	)
)
