(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CDNBS08-SLVU2.8-4"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 1.27 11.43 0)
		)
		(property "Value" "CDNBS08-SLVU2.8-4"
			(at -8.89 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.bourns.com/pdfs/CDNBS08-SLVU28-4.pdf"
			(at 1.27 -17.78 0)
		)
		(property "Description" "Quad bidirectional transil, Suppressor for ESD protection, 5V Standoff, 4 Channels, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CDNBS08-SLVU2.8-4_0_1")
		(symbol "CDNBS08-SLVU2.8-4_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "TVS1")
				(number "5")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "TVS2")
				(number "6")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "TVS1")
				(number "7")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "TVS2")
				(number "8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "TVS2")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "TVS1")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "TVS2")
				(number "2")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "TVS1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CM1213A-01SO"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "CM1213A-01SO"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 1.27 -4.318 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/CM1213A-D.PDF"
			(at -1.905 2.032 90)
		)
		(property "Description" "Single Channel ESD Protection Array"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD Protection diodes transient suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "CM1213A-01SO_0_1")
		(symbol "CM1213A-01SO_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "VP")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "CH1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "VN")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CM1624"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 17.78 0)
		)
		(property "Value" "CM1624"
			(at 5.08 17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:OnSemi_UDFN-16-1EP_1.35x3.3mm_P0.4mm_EP0.4x2.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/cm1624-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMC interface, EMI filter, TVS, Line termination, UDFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "microsd protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*UDFN*1EP*1.35x3.3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "CM1624_0_1")
		(symbol "CM1624_1_1"
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "CLK")
				(number "14")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CMD")
				(number "11")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "Data0")
				(number "15")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Data1")
				(number "16")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "Data2")
				(number "9")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Data3")
				(number "10")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ESD1")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SDData2")
				(number "8")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SDData3")
				(number "7")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDCMD")
				(number "6")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SDCLK")
				(number "3")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SDData0")
				(number "2")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SDData1")
				(number "1")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ESD1")
				(number "4")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "ESD3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D3V3X8U9LP3810"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -2.54 -3.81 0)
		)
		(property "Value" "D3V3X8U9LP3810"
			(at 2.54 -3.81 0)
		)
		(property "Footprint" "Package_DFN_QFN:Diodes_UDFN3810-9_TYPE_B"
			(at 25.146 -9.652 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/D3V3X8U9LP3810.pdf"
			(at 34.29 -7.366 0)
		)
		(property "Description" "3V3 Reverse Working, 8 channel low capacitance 0.45pF, TVS diode array, 5.5-7V Breakdown, U-DFN3810-9"
			(at 2.286 -11.43 0)
		)
		(property "ki_keywords" "ESD protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes?UDFN3810?9?TYPE_B*"
			(at 0 0 0)
		)
		(symbol "D3V3X8U9LP3810_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
		)
		(symbol "D3V3X8U9LP3810_0_1")
		(symbol "D3V3X8U9LP3810_1_1"
			(pin passive line
				(at -7.62 5.08 270)
				(length 2.54)
				(name "Line-1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "Line-3")
				(number "2")
			)
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "Line-6")
				(number "4")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "Line-8")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "Line-7")
				(number "6")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "Line-5")
				(number "7")
			)
			(pin passive line
				(at 7.62 5.08 270)
				(length 2.54)
				(name "Line-4")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 270)
				(length 2.54)
				(name "Line-2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D3V3XA4B10LP"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.635 8.89 0)
		)
		(property "Value" "D3V3XA4B10LP"
			(at 8.89 -10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
			(at -24.13 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/D3V3XA4B10LP.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Channel Low Capacitance TVS Diode Array, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection TVS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes*UDFN*1.0x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "D3V3XA4B10LP_0_0")
		(symbol "D3V3XA4B10LP_0_1")
		(symbol "D3V3XA4B10LP_1_1"
			(pin free line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin free line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "VSS")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "8")
			)
			(pin free line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin free line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "NC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ECMF02-2AMX6"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "ECMF02-2AMX6"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UQFN-6L_1.5x1.7mm_P0.5mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ecmf02-2amx6.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Single Pair Common Mode Filter with ESD Protection, UQFN-6L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Common Mode ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?UQFN*L?1.5x1.7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ECMF02-2AMX6_0_1"
			(text "D+"
				(at 0 3.556 0)
			)
			(text "D-"
				(at 0 -1.27 0)
			)
		)
		(symbol "ECMF02-2AMX6_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D+_in")
				(number "1")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "D-_in")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin free line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D+_out")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "D-_out")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EMI2121MTTAG"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "EMI2121MTTAG"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_2x2.2mm_P0.5mm_EP0.80x0.54"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/EMI2121MT-D.PDF"
			(at -7.62 -2.54 0)
		)
		(property "Description" "Single Pair Common Mode Filter with ESD Protection, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Common Mode ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*2x2.2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EMI2121MTTAG_0_1")
		(symbol "EMI2121MTTAG_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "In_1-")
				(number "2")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "In_1+")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Out_1-")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "Out_1+")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EMI8132"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "EMI8132"
			(at 8.89 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:OnSemi_XDFN-10_1.35x2.2mm_P0.4mm"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/emi8132-d.pdf"
			(at 0 -26.67 0)
		)
		(property "Description" "On Semi, Dual Pair Common Mode Filter with ESD Protection, 3.3V working voltage, XDFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Common Mode ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*XDFN*1.35x2.2mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "EMI8132_0_1")
		(symbol "EMI8132_1_1"
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "In_1+")
				(number "1")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "In_1-")
				(number "2")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "In_1+")
				(number "4")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "In_1-")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "Out_1+")
				(number "10")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "Out_1+")
				(number "9")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "Out_1+")
				(number "7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "Out_1+")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESD224DQA"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.635 8.255 0)
		)
		(property "Value" "ESD224DQA"
			(at 8.89 -8.255 0)
		)
		(property "Footprint" "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
			(at -0.635 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/esd224.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "4-Channel Low Capacitance TVS Diode Array, USON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection TVS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes*UDFN*1.0x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ESD224DQA_0_0")
		(symbol "ESD224DQA_0_1")
		(symbol "ESD224DQA_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESDA6V1-5SC6"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -5.08 -3.81 0)
		)
		(property "Value" "ESDA6V1-5SC6"
			(at 2.54 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/esda6v1-5sc6.pdf"
			(at 0 0 90)
		)
		(property "Description" "Quintuple bidirectional transil, Suppressor for ESD protection, 6V1 Breakdown, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ESDA6V1-5SC6_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(symbol "ESDA6V1-5SC6_0_1")
		(symbol "ESDA6V1-5SC6_1_1"
			(pin passive line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "IO1")
				(number "1")
			)
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "IO2")
				(number "3")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "IO3")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "IO4")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "IO5")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESDA6V1BC6"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -2.54 -6.35 0)
		)
		(property "Value" "ESDA6V1BC6"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/21/07/21/e3/a8/df/42/a2/CD00001906.pdf/files/CD00001906.pdf/jcr:content/translations/en.CD00001906.pdf"
			(at 0 0 90)
		)
		(property "Description" "Quad bidirectional transil, Suppressor for ESD protection, 5V Standoff, 4 Channels, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ESDA6V1BC6_0_0"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "COM")
				(number "2")
			)
		)
		(symbol "ESDA6V1BC6_0_1")
		(symbol "ESDA6V1BC6_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "TVS1")
				(number "1")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "TVS2")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "5")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "TVS3")
				(number "4")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "TVS4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IP3319CX6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "IP3319CX6"
			(at -10.16 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-6_1.4x1.0mm_P0.4mm"
			(at 0.635 6.35 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP3319CX6.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Single channel common mode filter with integrated ESD protection network"
			(at 0 0 0)
		)
		(property "ki_keywords" "common mode filter ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.4x1.0mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "IP3319CX6_0_1")
		(symbol "IP3319CX6_1_1"
			(pin passive line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "D+_IN")
				(number "A2")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 5.08)
				(name "D-_IN")
				(number "B2")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "ID")
				(number "C2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "D+_OUT")
				(number "A1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 5.08)
				(name "D-_OUT")
				(number "B1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IP4234CZ6"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "IP4234CZ6"
			(at 2.794 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SC-74-6_1.55x2.9mm_P0.95mm"
			(at 0 -15.748 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4234CZ6.pdf"
			(at 0 -20.066 0)
		)
		(property "Description" "ESD Protection, 2 channel, USB 2.0 to IEC 61000-4-2 level 4, 5.5V, SOT457 (SC-74-6)"
			(at 0 -18.034 0)
		)
		(property "ki_keywords" "USB ESD protection "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SC?74?6*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "IP4234CZ6_0_0")
		(symbol "IP4234CZ6_0_1")
		(symbol "IP4234CZ6_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "VP")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VN")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IP4252CZ12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 11.43 0)
		)
		(property "Value" "IP4252CZ12"
			(at 3.175 12.065 0)
		)
		(property "Footprint" "Package_SON:Nexperia_HUSON-12_USON-12-1EP_1.35x2.5mm_P0.4mm_EP0.4x2mm"
			(at 0 -14.605 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4251_52_53_54-TTL.pdf"
			(at 0 -17.145 0)
		)
		(property "Description" "6 channel EMI filters with integrated ESD protection, 12 pF, 40 Ohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HUSON*1.35x2.5*EP0.4x2*"
			(at 0 0 0)
		)
		(symbol "IP4252CZ12_0_1")
		(symbol "IP4252CZ12_1_1"
			(pin passive line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "CH1")
				(number "1")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "CH2")
				(number "2")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "CH3")
				(number "3")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 2.54)
				(name "CH4")
				(number "4")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "CH5")
				(number "5")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "CH6")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "CH1")
				(number "12")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "CH2")
				(number "11")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "CH3")
				(number "10")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 2.54)
				(name "CH4")
				(number "9")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CH5")
				(number "8")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "CH6")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IP4252CZ16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 13.97 0)
		)
		(property "Value" "IP4252CZ16"
			(at 3.175 14.605 0)
		)
		(property "Footprint" "Package_SON:Nexperia_HUSON-16_USON-16-1EP_1.35x3.3mm_P0.4mm_EP0.4x2.8mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4251_52_53_54-TTL.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "8 channel EMI filters with integrated ESD protection,  12 pF, 40 Ohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HUSON*1.35x3.3*EP0.4x2.8*"
			(at 0 0 0)
		)
		(symbol "IP4252CZ16_0_1")
		(symbol "IP4252CZ16_1_1"
			(pin passive line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "CH1")
				(number "1")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "CH2")
				(number "2")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "CH3")
				(number "3")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "CH4")
				(number "4")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 2.54)
				(name "CH5")
				(number "5")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "CH6")
				(number "6")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "CH7")
				(number "7")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "CH8")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "CH1")
				(number "16")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "CH2")
				(number "15")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "CH3")
				(number "14")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "CH4")
				(number "13")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 2.54)
				(name "CH5")
				(number "12")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CH6")
				(number "11")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "CH7")
				(number "10")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CH8")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IP4252CZ8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 6.35 0)
		)
		(property "Value" "IP4252CZ8"
			(at 3.175 6.985 0)
		)
		(property "Footprint" "Package_SON:Nexperia_HUSON-8_USON-8-1EP_1.35x1.7mm_P0.4mm_EP0.4x1.2mm"
			(at 0 -13.335 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4251_52_53_54-TTL.pdf"
			(at 0 -16.51 0)
		)
		(property "Description" "4 channel EMI filters with integrated ESD protection, 12 pF, 40 Ohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HUSON*1.35x1.7*EP0.4x1.2*"
			(at 0 0 0)
		)
		(symbol "IP4252CZ8_0_1")
		(symbol "IP4252CZ8_1_1"
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "CH1")
				(number "1")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 2.54)
				(name "CH2")
				(number "2")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "CH3")
				(number "3")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "CH4")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "CH1")
				(number "8")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 2.54)
				(name "CH2")
				(number "7")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CH3")
				(number "6")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "CH4")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP349MN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP349MN"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x1.6mm_P0.5mm_EP1.15x1.3mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp349-d.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "28V Positive Overvoltage Protection Controller, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NCP349MN_0_1")
		(symbol "NCP349MN_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FLAG}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP361MU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP361MU"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp361-d.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "USB Positive Overvoltage Protection Controller with Internal PMOS FET and Overcurrent Protection, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage protection USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "NCP361MU_0_1")
		(symbol "NCP361MU_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FLAG}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP361SN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP361SN"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_SO:TSOP-5_1.65x3.05mm_P0.95mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp361-d.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "USB Positive Overvoltage Protection Controller with Internal PMOS FET and Overcurrent Protection, TSOP-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage protection USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*1.65x3.05*P0.95*"
			(at 0 0 0)
		)
		(symbol "NCP361SN_0_1")
		(symbol "NCP361SN_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FLAG}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NUF4401MN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.145 8.89 0)
		)
		(property "Value" "NUF4401MN"
			(at 7.62 9.525 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.6x1.2mm"
			(at -1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NUF4401MN-D.PDF"
			(at 3.81 -16.51 0)
		)
		(property "Description" "4 channel EMI filters with integrated ESD protection, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NUF4401MN_0_1")
		(symbol "NUF4401MN_1_1"
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "IN3")
				(number "3")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "IN4")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "OUT1")
				(number "8")
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "OUT3")
				(number "6")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "OUT4")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NUP2105L"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.715 2.54 0)
		)
		(property "Value" "NUP2105L"
			(at 5.715 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.715 -1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub_link/Collateral/NUP2105L-D.PDF"
			(at 3.175 3.175 0)
		)
		(property "Description" "Dual Line CAN Bus Protector, 24Vrwm"
			(at 0 0 0)
		)
		(property "ki_keywords" "can esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "NUP2105L_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(symbol "NUP2105L_0_1")
		(symbol "NUP2105L_1_1"
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NUP2202"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.334 -2.54 0)
		)
		(property "Value" "NUP2202"
			(at 6.35 1.27 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 2.032 1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/nup2202w1-d.pdf"
			(at 2.032 1.905 0)
		)
		(property "Description" "Transient voltage suppressor designed to protect high speed data lines from ESD, EFT, and lightning"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD Protection diodes  transient suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "NUP2202_0_1")
		(symbol "NUP2202_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NUP4202"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 -2.54 0)
		)
		(property "Value" "NUP4202"
			(at 6.35 1.27 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NUP4202W1-D.PDF"
			(at 1.27 1.905 0)
		)
		(property "Description" "Transient voltage suppressor designed to protect high speed data lines from ESD, EFT, and lightning"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD Protection diodes  transient suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "NUP4202_0_1")
		(symbol "NUP4202_1_1"
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCMF3USB3S"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "PCMF3USB3S"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_CSP:Nexperia_WLCSP-15_2.37x1.17mm_Layout6x3_P0.4mmP0.8mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PCMFXUSB3S_SER.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Common-mode EMI filter for differential channels with integrated ESD protection"
			(at 0 0 0)
		)
		(property "ki_keywords" "Common Mode ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*WLCSP*2.37x1.17mm*Layout6x3*P0.4mmP0.8mm*"
			(at 0 0 0)
		)
		(symbol "PCMF3USB3S_0_1")
		(symbol "PCMF3USB3S_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "CH1_IN+")
				(number "A1")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "CH1_IN-")
				(number "A2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND_CH1")
				(number "B1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "CH1_OUT+")
				(number "C1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "CH1_OUT-")
				(number "C2")
			)
		)
		(symbol "PCMF3USB3S_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "CH2_IN+")
				(number "A3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "CH2_IN-")
				(number "A4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND_CH2")
				(number "B2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "CH2_OUT+")
				(number "C3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "CH2_OUT-")
				(number "C4")
			)
		)
		(symbol "PCMF3USB3S_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "CH3_IN+")
				(number "A5")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "CH3_IN-")
				(number "A6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND_CH3")
				(number "B3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "CH3_OUT+")
				(number "C5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "CH3_OUT-")
				(number "C6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PESD3V3L4UF"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD3V3L4UF"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-886"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL4UF_G_W.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional quadruple ESD protection diode array, 3.3V, Common Anode, SOT-886"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?886*"
			(at 0 0 0)
		)
		(symbol "PESD3V3L4UF_0_1")
		(symbol "PESD3V3L4UF_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K1")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "5")
			)
		)
		(symbol "PESD3V3L4UF_2_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K2")
				(number "3")
			)
		)
		(symbol "PESD3V3L4UF_3_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K3")
				(number "4")
			)
		)
		(symbol "PESD3V3L4UF_4_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PESD3V3L4UG"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD3V3L4UG"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL4UF_G_W.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional quadruple ESD protection diode array, 3.3V, Common Anode, SOT-353"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "PESD3V3L4UG_0_1")
		(symbol "PESD3V3L4UG_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K1")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "PESD3V3L4UG_2_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K2")
				(number "3")
			)
		)
		(symbol "PESD3V3L4UG_3_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K3")
				(number "4")
			)
		)
		(symbol "PESD3V3L4UG_4_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K4")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PESD3V3L4UW"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD3V3L4UW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-665"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL4UF_G_W.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional quadruple ESD protection diode array, 3.3V, Common Anode, SOT-665"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?665*"
			(at 0 0 0)
		)
		(symbol "PESD3V3L4UW_0_1")
		(symbol "PESD3V3L4UW_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K1")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "PESD3V3L4UW_2_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K2")
				(number "3")
			)
		)
		(symbol "PESD3V3L4UW_3_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K3")
				(number "4")
			)
		)
		(symbol "PESD3V3L4UW_4_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K4")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PESD3V3L5UF"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD3V3L5UF"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-886"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL5UF_V_Y.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional fivefold ESD protection diode array, 3.3V, Common Anode, SOT-886"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?886*"
			(at 0 0 0)
		)
		(symbol "PESD3V3L5UF_0_1")
		(symbol "PESD3V3L5UF_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K1")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "PESD3V3L5UF_2_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K2")
				(number "3")
			)
		)
		(symbol "PESD3V3L5UF_3_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K3")
				(number "4")
			)
		)
		(symbol "PESD3V3L5UF_4_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K4")
				(number "5")
			)
		)
		(symbol "PESD3V3L5UF_5_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K5")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PESD3V3L5UV"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD3V3L5UV"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-666"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL5UF_V_Y.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional fivefold ESD protection diode array, 3.3V, Common Anode, SOT-666"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?666*"
			(at 0 0 0)
		)
		(symbol "PESD3V3L5UV_0_1")
		(symbol "PESD3V3L5UV_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K1")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "PESD3V3L5UV_2_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K2")
				(number "3")
			)
		)
		(symbol "PESD3V3L5UV_3_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K3")
				(number "4")
			)
		)
		(symbol "PESD3V3L5UV_4_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K4")
				(number "5")
			)
		)
		(symbol "PESD3V3L5UV_5_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K5")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PESD3V3L5UY"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD3V3L5UY"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL5UF_V_Y.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional fivefold ESD protection diode array, 3.3V, Common Anode, SOT-363"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "PESD3V3L5UY_0_1")
		(symbol "PESD3V3L5UY_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K1")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "PESD3V3L5UY_2_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K2")
				(number "3")
			)
		)
		(symbol "PESD3V3L5UY_3_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K3")
				(number "4")
			)
		)
		(symbol "PESD3V3L5UY_4_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K4")
				(number "5")
			)
		)
		(symbol "PESD3V3L5UY_5_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "K5")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PRTR5V0U2X"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.794 8.636 0)
		)
		(property "Value" "PRTR5V0U2X"
			(at 8.128 -9.398 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 1.524 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PRTR5V0U2X.pdf"
			(at 1.524 0 0)
		)
		(property "Description" "Ultra low capacitance double rail-to-rail ESD protection diode, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?143*"
			(at 0 0 0)
		)
		(symbol "PRTR5V0U2X_0_1")
		(symbol "PRTR5V0U2X_1_1"
			(pin passive line
				(at -12.7 0 0)
				(length 5.08)
				(name "I/O1")
				(number "2")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "I/O2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RCLAMP0502B"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "RCLAMP0502B"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-416"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.semtech.com/products/circuit-protection/low-capacitance/rclamp0502b"
			(at 1.27 2.54 0)
		)
		(property "Description" "Low capacitance unidirectional dual ESD protection diode, SC-75"
			(at 0 0 0)
		)
		(property "ki_keywords" "tvs unidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?416*"
			(at 0 0 0)
		)
		(symbol "RCLAMP0502B_0_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(symbol "RCLAMP0502B_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "K1")
				(number "1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "K2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RCLAMP3328P"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 13.97 2.54 0)
		)
		(property "Value" "RCLAMP3328P"
			(at 13.97 0.635 0)
		)
		(property "Footprint" "Package_DFN_QFN:UDFN-9_1.0x3.8mm_P0.5mm"
			(at 13.97 -1.27 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Semtech%20PDFs/RCLAMP3328P.pdf"
			(at 4.445 0.635 0)
		)
		(property "Description" "Low Capacitance TVS Diode Array, 3.3V Standoff, 8 Channels, UDFN-9"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UDFN*1.0x3.8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "RCLAMP3328P_0_0"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(symbol "RCLAMP3328P_0_1")
		(symbol "RCLAMP3328P_1_1"
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "K1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "K2")
				(number "2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "K3")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "K4")
				(number "5")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "K5")
				(number "6")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "K6")
				(number "7")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "K7")
				(number "8")
			)
			(pin passive line
				(at 10.16 7.62 270)
				(length 2.54)
				(name "K8")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65220"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.715 0)
		)
		(property "Value" "SN65220"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 8.89 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65220.pdf"
			(at 0 3.81 0)
		)
		(property "Description" "USB port transient suppressors"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SN65220_0_1")
		(symbol "SN65220_1_1"
			(pin passive line
				(at -15.24 0 0)
				(length 5.08)
				(name "A")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 5.08)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN75240"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.715 0)
		)
		(property "Value" "SN75240"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 3.81 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65220.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "USB port transient suppressors"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "USB suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm* TSSOP*4.4x3mm*0.65mm*"
			(at 0 0 0)
		)
		(symbol "SN75240_0_0")
		(symbol "SN75240_0_1")
		(symbol "SN75240_1_1"
			(pin passive line
				(at -12.7 0 0)
				(length 5.08)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "B")
				(number "6")
			)
		)
		(symbol "SN75240_2_1"
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "C")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 12.7 0 180)
				(length 5.08)
				(name "D")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SP0502BAHT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.715 2.54 0)
		)
		(property "Value" "SP0502BAHT"
			(at 5.715 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.715 -1.27 0)
		)
		(property "Datasheet" "http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "TVS Diode Array, 5.5V Standoff, 2 Channels, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SP0502BAHT_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(symbol "SP0502BAHT_0_1")
		(symbol "SP0502BAHT_1_1"
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SP0502BAJT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.715 2.54 0)
		)
		(property "Value" "SP0502BAJT"
			(at 5.715 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.715 -1.27 0)
		)
		(property "Datasheet" "http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "TVS Diode Array, 5.5V Standoff, 2 Channels, SC-70 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
		(symbol "SP0502BAJT_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(symbol "SP0502BAJT_0_1")
		(symbol "SP0502BAJT_1_1"
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SP0503BAHT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.715 2.54 0)
		)
		(property "Value" "SP0503BAHT"
			(at 5.715 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 5.715 -1.27 0)
		)
		(property "Datasheet" "http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "TVS Diode Array, 5.5V Standoff, 3 Channels, SOT-143 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?143*"
			(at 0 0 0)
		)
		(symbol "SP0503BAHT_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(symbol "SP0503BAHT_0_1")
		(symbol "SP0503BAHT_1_1"
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SP0504BAHT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 7.62 2.54 0)
		)
		(property "Value" "SP0504BAHT"
			(at 7.62 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "TVS Diode Array, 5.5V Standoff, 4 Channels, SOT-23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SP0504BAHT_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "SP0504BAHT_0_1")
		(symbol "SP0504BAHT_1_1"
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "4")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "K")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SP0504BAJT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 7.62 2.54 0)
		)
		(property "Value" "SP0504BAJT"
			(at 7.62 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "TVS Diode Array, 5.5V Standoff, 4 Channels, SC-70-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "SP0504BAJT_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "SP0504BAJT_0_1")
		(symbol "SP0504BAJT_1_1"
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "4")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "K")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SP0505BAHT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 7.62 2.54 0)
		)
		(property "Value" "SP0505BAHT"
			(at 7.62 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "TVS Diode Array, 5.5V Standoff, 5 Channels, SOT-23-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SP0505BAHT_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "SP0505BAHT_0_1")
		(symbol "SP0505BAHT_1_1"
			(pin passive line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "K")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "K")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SP0505BAJT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 7.62 2.54 0)
		)
		(property "Value" "SP0505BAJT"
			(at 7.62 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "TVS Diode Array, 5.5V Standoff, 5 Channels, SC-70-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "SP0505BAJT_0_0"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "SP0505BAJT_0_1")
		(symbol "SP0505BAJT_1_1"
			(pin passive line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "K")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "K")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SRV05-4"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "SRV05-4"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 17.78 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/SRV05-4-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "ESD Protection Diodes with Low Clamping Voltage, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection diodes"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SRV05-4_0_0")
		(symbol "SRV05-4_0_1")
		(symbol "SRV05-4_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "IO1")
				(number "1")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "IO2")
				(number "3")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(name "VP")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VN")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "IO3")
				(number "4")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "IO4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TBU-CA-025-050-WH"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-025-050-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 250V 50mA 13.3ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
		(symbol "TBU-CA-025-050-WH_0_1")
		(symbol "TBU-CA-025-050-WH_1_1"
			(pin no_connect line
				(at -1.27 2.54 270)
				(length 1.27)
				(hide yes)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD1E05U06DPY"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 3.175 0)
		)
		(property "Value" "TPD1E05U06DPY"
			(at 1.27 3.175 0)
		)
		(property "Footprint" "Package_SON:Texas_DPY0002A_0.6x1mm_P0.65mm"
			(at 2.54 -4.445 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpd1e05u06.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1-Channel ESD Protection for Super-Speed USB 3.0 Interface, X1SON-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection USB 3.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DPY0002A*"
			(at 0 0 0)
		)
		(symbol "TPD1E05U06DPY_0_1")
		(symbol "TPD1E05U06DPY_1_1"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "I/O")
				(number "1")
			)
			(pin power_in line
				(at 5.08 0 180)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD2E2U06DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPD2E2U06DCK"
			(at 0.508 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at -20.32 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2e2u06.pdf"
			(at -5.08 5.08 0)
		)
		(property "Description" "Dual-Channel High-Speed ESD Protection, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "TPD2E2U06DCK_0_1")
		(symbol "TPD2E2U06DCK_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD2E2U06DRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPD2E2U06DRL"
			(at 0.508 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at -20.32 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2e2u06.pdf"
			(at -5.08 5.08 0)
		)
		(property "Description" "Dual-Channel High-Speed ESD Protection, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
		(symbol "TPD2E2U06DRL_0_1")
		(symbol "TPD2E2U06DRL_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "NC")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD2EUSB30"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TPD2EUSB30"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_DRT-3"
			(at -19.05 -7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2eusb30a.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel ESD Protection for Super-Speed USB 3.0 Interface, DRT-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection USB 3.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRT*"
			(at 0 0 0)
		)
		(symbol "TPD2EUSB30_0_1")
		(symbol "TPD2EUSB30_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 5.08)
				(name "D+")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 5.08)
				(name "D-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD2S017"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "TPD2S017"
			(at 2.54 -8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at -19.05 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2s017.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel Ultra-Low Clamp Voltage ESD Solution With Series-Resistor Isolation, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPD2S017_0_1")
		(symbol "TPD2S017_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "CH1In")
				(number "3")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "CH2Int")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "CH1Out")
				(number "1")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "CH2Out")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD3E001DRLR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPD3E001DRLR"
			(at 8.89 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at -17.78 -7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd3e001.pdf"
			(at -5.08 6.35 0)
		)
		(property "Description" "TPD3E001 Low-Capacitance 3-Channel ESD-Protection for High-Speed Data Interfaces"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD-Protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
		(symbol "TPD3E001DRLR_0_1")
		(symbol "TPD3E001DRLR_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IO1")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "IO2")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IO3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD3F303DPV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.145 8.89 0)
		)
		(property "Value" "TPD3F303DPV"
			(at 7.62 9.525 0)
		)
		(property "Footprint" "Package_SON:Texas_R-PUSON-N8_USON-8-1EP_1.6x2.1mm_P0.5mm_EP0.4x1.7mm"
			(at -1.27 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tpd3f303"
			(at 3.81 -12.7 0)
		)
		(property "Description" "3 channel EMI filters with integrated ESD protection for SIM Card Interface, USON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*USON*1EP*1.6x2.1mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPD3F303DPV_0_1")
		(symbol "TPD3F303DPV_1_1"
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "DATA1_IN")
				(number "8")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "CLK_IN")
				(number "7")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "DATA2_IN")
				(number "6")
			)
			(pin no_connect line
				(at -17.78 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "DATA1_OUT")
				(number "1")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "CLK_OUT")
				(number "2")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "DATA2_OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD3S014"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPD3S014"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd3s014.pdf"
			(at -5.08 6.35 0)
		)
		(property "Description" "Current Limit Switch and D+/D– ESD Protection for USB Host Port, 0.5A, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD-Protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPD3S014_0_1")
		(symbol "TPD3S014_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "D1")
				(number "5")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "D2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD4E02B04DQA"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 -11.43 0)
		)
		(property "Value" "TPD4E02B04DQA"
			(at 7.62 1.905 0)
		)
		(property "Footprint" "Package_SON:USON-10_2.5x1.0mm_P0.5mm"
			(at 7.62 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "4-Channel ESD Protection Diode for USB Type-C and HDMI 2.0, USON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection USB HDMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USON*2.5x1.0mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPD4E02B04DQA_0_0"
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "G")
				(number "3")
			)
		)
		(symbol "TPD4E02B04DQA_0_1")
		(symbol "TPD4E02B04DQA_1_1"
			(pin passive line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "IO1")
				(number "1")
			)
			(pin free line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "IO2")
				(number "2")
			)
			(pin free line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "NC")
				(number "9")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IO3")
				(number "4")
			)
			(pin free line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "IO4")
				(number "5")
			)
			(pin free line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "G")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD4EUSB30"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.635 8.89 0)
		)
		(property "Value" "TPD4EUSB30"
			(at 8.89 -10.16 0)
		)
		(property "Footprint" "Package_SON:USON-10_2.5x1.0mm_P0.5mm"
			(at -24.13 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2eusb30a.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-Channel ESD Protection for Super-Speed USB 3.0 Interface, USON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection USB 3.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USON*2.5x1.0mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPD4EUSB30_0_0")
		(symbol "TPD4EUSB30_0_1")
		(symbol "TPD4EUSB30_1_1"
			(pin free line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "D1+")
				(number "1")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "D1-")
				(number "2")
			)
			(pin free line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin free line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "D2+")
				(number "4")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "D2-")
				(number "5")
			)
			(pin free line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "NC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD4S014"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.24 0)
		)
		(property "Value" "TPD4S014"
			(at 0 12.7 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PWSON-N10"
			(at 22.86 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd4s014.pdf"
			(at 27.94 -17.78 0)
		)
		(property "Description" "USB Charger Port Protection Including ESD Protection for All Lines and Overvoltage Protection on VBUS"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB  Port Protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Package?SON:Texas?S?PWSON?N10*"
			(at 0 0 0)
		)
		(symbol "TPD4S014_0_1")
		(symbol "TPD4S014_1_1"
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "VBUS")
				(number "10")
			)
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VBUS")
				(number "9")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "3")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ID")
				(number "5")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D-")
				(number "6")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D+")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "11")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VBUSOUT")
				(number "1")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VBUSOUT")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{ACK}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD4S1394"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 11.43 0)
		)
		(property "Value" "TPD4S1394"
			(at 1.27 -12.7 0)
		)
		(property "Footprint" "Package_SON:X2SON-8_1.4x1mm_P0.35mm"
			(at -24.13 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd4s1394.pdf"
			(at -2.54 -1.27 0)
		)
		(property "Description" "Firewire ESD Clamp With Live-Insertion Detection Circuit, X2SON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "firewire ESD clamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "X2SON*1.4x1mm*P0.35mm*"
			(at 0 0 0)
		)
		(symbol "TPD4S1394_0_1")
		(symbol "TPD4S1394_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D1+")
				(number "7")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D1-")
				(number "8")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D2+")
				(number "5")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D2-")
				(number "6")
			)
			(pin passive line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCLMP")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "FWPWR_EN")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD6E05U06RVZ"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 6.35 0)
		)
		(property "Value" "TPD6E05U06RVZ"
			(at 22.86 7.62 0)
		)
		(property "Footprint" "Package_SON:Texas_R-PUSON-N14"
			(at 15.24 -6.985 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpd1e05u06.pdf"
			(at 15.24 -8.89 0)
		)
		(property "Description" "6-Channel ESD Protection for Super-Speed USB 3.0 Interface, USON-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection USB 3.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PUSON*14*"
			(at 0 0 0)
		)
		(symbol "TPD6E05U06RVZ_0_1")
		(symbol "TPD6E05U06RVZ_1_1"
			(pin passive line
				(at -12.7 10.16 270)
				(length 5.08)
				(name "D1+")
				(number "14")
			)
			(pin free line
				(at -12.7 -10.16 90)
				(length 5.08)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at -7.62 10.16 270)
				(length 5.08)
				(name "D1-")
				(number "13")
			)
			(pin free line
				(at -7.62 -10.16 90)
				(length 5.08)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at -2.54 10.16 270)
				(length 5.08)
				(name "D2+")
				(number "12")
			)
			(pin free line
				(at -2.54 -10.16 90)
				(length 5.08)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 5.08)
				(name "D2-")
				(number "11")
			)
			(pin free line
				(at 2.54 -10.16 90)
				(length 5.08)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 5.08)
				(name "D3+")
				(number "9")
			)
			(pin free line
				(at 7.62 -10.16 90)
				(length 5.08)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 12.7 10.16 270)
				(length 5.08)
				(name "D3-")
				(number "8")
			)
			(pin free line
				(at 12.7 -10.16 90)
				(length 5.08)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 22.86 0 180)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 22.86 0 180)
				(length 5.08)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD6F003"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.145 11.43 0)
		)
		(property "Value" "TPD6F003"
			(at 7.62 12.065 0)
		)
		(property "Footprint" "Package_SON:Texas_R-PWSON-N12_EP0.4x2mm"
			(at -1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd6f003.pdf"
			(at 3.81 -16.51 0)
		)
		(property "Description" "6 channel EMI filters with integrated ESD protection"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI, ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WSON*EP0.4x2mm*"
			(at 0 0 0)
		)
		(symbol "TPD6F003_0_1")
		(symbol "TPD6F003_1_1"
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "Ch1_In")
				(number "1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "Ch2_In")
				(number "2")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "Ch3_In")
				(number "3")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "Ch4_In")
				(number "4")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "Ch5_In")
				(number "5")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "Ch6_In")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "Ch1_Out")
				(number "12")
			)
			(pin passive line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "Ch2_Out")
				(number "11")
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "Ch3_Out")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "Ch4_Out")
				(number "9")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "Ch5_Out")
				(number "8")
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "Ch6_Out")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD6S300A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "TPD6S300A"
			(at 7.62 -15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm_ThermalVias"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpd6s300a.pdf"
			(at 0 -27.94 0)
		)
		(property "Description" "USB Type-C Port Protector: Short-to-VBUS Overvoltage and IEC ESD Protection, WQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-C ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TPD6S300A_0_1")
		(symbol "TPD6S300A_1_1"
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "C_CC1")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "C_CC2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RPD_G1")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RPD_G2")
				(number "6")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "D1")
				(number "20")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D2")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "C_SBU1")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "C_SBU2")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VPWR")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{FLT}")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CC1")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CC2")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SBU1")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SBU2")
				(number "14")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "VBIAS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD8F003"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.635 13.97 0)
		)
		(property "Value" "TPD8F003"
			(at 1.27 -14.605 0)
		)
		(property "Footprint" "Package_SON:WSON-16_3.3x1.35_P0.4mm"
			(at -25.4 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd6f003.pdf"
			(at 3.81 -13.97 0)
		)
		(property "Description" "8 channel EMI filters with integrated ESD protection"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI, ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*3.3x1.35*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TPD8F003_0_0"
			(text "8.5pF"
				(at -1.778 8.636 0)
			)
			(text "100"
				(at 0 10.16 0)
			)
			(text "8.5pF"
				(at 1.778 8.636 0)
			)
		)
		(symbol "TPD8F003_0_1")
		(symbol "TPD8F003_1_1"
			(pin passive line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "Ch1_In")
				(number "1")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "Ch2_In")
				(number "2")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "Ch3_In")
				(number "3")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "Ch4_In")
				(number "4")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "Ch5_In")
				(number "5")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "Ch6_In")
				(number "6")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "Ch7_In")
				(number "7")
			)
			(pin passive line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "Ch8_In")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "Ch1_Out")
				(number "16")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "Ch2_Out")
				(number "15")
			)
			(pin passive line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "Ch3_Out")
				(number "14")
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "Ch4_Out")
				(number "13")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "Ch5_Out")
				(number "12")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "Ch6_Out")
				(number "11")
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "Ch7_Out")
				(number "10")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "Ch8_Out")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TVS0500DRV"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 1.27 0)
		)
		(property "Value" "TVS0500DRV"
			(at 2.54 -1.27 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tvs0500.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Flat-Clamp Surge Protection Device. 5Vrwm, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI, ESD, TVS protection transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*EP1x1.6mm*"
			(at 0 0 0)
		)
		(symbol "TVS0500DRV_0_0"
			(text "Det &"
				(at -8.255 0.635 0)
			)
			(text "Drv"
				(at -8.255 -1.27 0)
			)
		)
		(symbol "TVS0500DRV_0_1")
		(symbol "TVS0500DRV_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "5")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB6B1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "USB6B1"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/3e/ec/b2/54/b2/76/47/90/CD00001361.pdf/files/CD00001361.pdf/jcr:content/translations/en.CD00001361.pdf"
			(at -24.13 -2.54 0)
		)
		(property "Description" "5V Data line protection"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "USB6B1_0_1")
		(symbol "USB6B1_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "I/O1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "I/O2")
				(number "3")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VBUS")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "I/O1")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "I/O2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USBLC6-2P6"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 5.715 0)
		)
		(property "Value" "USBLC6-2P6"
			(at 0.635 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-666"
			(at 1.016 -6.731 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/usblc6-2.pdf"
			(at 1.016 -8.636 0)
		)
		(property "Description" "Very low capacitance ESD protection diode, 2 data-line, SOT-666"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb ethernet video"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?666*"
			(at 0 0 0)
		)
		(symbol "USBLC6-2P6_0_0")
		(symbol "USBLC6-2P6_0_1")
		(symbol "USBLC6-2P6_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "I/O1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "I/O2")
				(number "3")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "VBUS")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "I/O1")
				(number "6")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "I/O2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USBLC6-4SC6"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 9.525 0)
		)
		(property "Value" "USBLC6-4SC6"
			(at 1.27 6.985 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/usblc6-4.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Very low capacitance ESD protection diode, 4 data-line, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb ethernet sim card video"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "USBLC6-4SC6_0_0")
		(symbol "USBLC6-4SC6_0_1")
		(symbol "USBLC6-4SC6_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "I/O1")
				(number "1")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "I/O2")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "I/O3")
				(number "4")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "I/O4")
				(number "6")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "VBUS")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WE-TVS-82400102"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "WE-TVS-82400102"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/82400102.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Low Capacitance TVS Diode Array, 2 Channels, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD Protection TVS High-speed USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "WE-TVS-82400102_0_1")
		(symbol "WE-TVS-82400102_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZEN056V130A24LS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN056V130A24LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 5.6V, 1.30A, 24V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
		(symbol "ZEN056V130A24LS_0_1")
		(symbol "ZEN056V130A24LS_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CDSOT236-0504C"
		(extends "SRV05-4")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "CDSOT236-0504C"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 17.78 -11.43 0)
		)
		(property "Datasheet" "https://www.bourns.com/docs/product-datasheets/cdsot236-0504c.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low capacitance ESD diode / steering Diode Array, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection diodes"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DT1240A-08LP3810"
		(extends "RCLAMP3328P")
		(property "Reference" "D"
			(at 13.97 2.54 0)
		)
		(property "Value" "DT1240A-08LP3810"
			(at 13.97 0.635 0)
		)
		(property "Footprint" "Package_DFN_QFN:UDFN-9_1.0x3.8mm_P0.5mm"
			(at 13.97 -1.27 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DT1240A-08LP3810.pdf"
			(at 4.445 0.635 0)
		)
		(property "Description" "Low Capacitance TVS Diode Array, 3.3V Standoff, 8 Channels, UDFN-9"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UDFN*1.0x3.8mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ECMF04-4HSWM10"
		(extends "EMI8132")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "ECMF04-4HSWM10"
			(at 8.89 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:UDFN-10_1.35x2.6mm_P0.5mm"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://www.st.com/content/ccc/resource/technical/document/datasheet/fa/13/38/f2/70/5b/46/46/DM00109760.pdf/files/DM00109760.pdf/jcr:content/translations/en.DM00109760.pdf"
			(at 0 -26.67 0)
		)
		(property "Description" "Dual Pair Common Mode Filter with 8KV/16KV ESD Protection, 3V working voltage, STMicroelectronics, UDFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Common Mode ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*UDFN*1.35x2.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ESDA14V2SC5"
		(extends "SP0504BAHT")
		(property "Reference" "D"
			(at 7.62 2.54 0)
		)
		(property "Value" "ESDA14V2SC5"
			(at 7.62 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/esda5v3sc6.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "Quad TVS Diode Array, 14.2V Standoff, 4 Channels, 400W, ±30kV, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ESDA5V3L"
		(extends "SP0502BAHT")
		(property "Reference" "D"
			(at 5.715 2.54 0)
		)
		(property "Value" "ESDA5V3L"
			(at 5.715 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-3"
			(at -15.24 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/esdal.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "TVS Diode Array, 5.5V Standoff, 2 Channels, SOT23"
			(at 0 -12.7 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ESDA5V3SC5"
		(extends "SP0504BAHT")
		(property "Reference" "D"
			(at 7.62 2.54 0)
		)
		(property "Value" "ESDA5V3SC5"
			(at 7.62 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/esda5v3sc6.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "Quad TVS Diode Array, 5.3V Standoff, 4 Channels, 400W, ±30kV, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ESDA6V1SC5"
		(extends "SP0504BAHT")
		(property "Reference" "D"
			(at 7.62 2.54 0)
		)
		(property "Value" "ESDA6V1SC5"
			(at 7.62 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/esda5v3sc6.pdf"
			(at 3.175 3.175 0)
		)
		(property "Description" "Quad TVS Diode Array, 6.1V Standoff, 4 Channels, 400W, ±30kV, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ESDLC5V0PB8"
		(extends "RCLAMP3328P")
		(property "Reference" "D"
			(at 13.97 2.54 0)
		)
		(property "Value" "ESDLC5V0PB8"
			(at 13.97 0.635 0)
		)
		(property "Footprint" "Package_DFN_QFN:UDFN-9_1.0x3.8mm_P0.5mm"
			(at 13.97 -1.27 0)
		)
		(property "Datasheet" "https://www.mccsemi.com/pdf/Products/ESDLC5V0PB8(DFN3810-9)-A.pdf"
			(at 4.445 0.635 0)
		)
		(property "Description" "TVS Diode Array, 5.0V Standoff, 8 Channels, UDFN-9"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UDFN*1.0x3.8mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "IP4251CZ8-4-TTL"
		(extends "NUF4401MN")
		(property "Reference" "U"
			(at -17.78 8.89 0)
		)
		(property "Value" "IP4251CZ8-4-TTL"
			(at 0 9.525 0)
		)
		(property "Footprint" "Package_SON:Nexperia_HUSON-8_USON-8-1EP_1.35x1.7mm_P0.4mm_EP0.4x1.2mm"
			(at -1.27 -6.35 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4251_52_53_54-TTL.pdf"
			(at 3.81 -16.51 0)
		)
		(property "Description" "4 channel EMI filters with integrated ESD protection, 100ohm series resistance, 5pF on each side, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HUSON*1EP*1.35x1.7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "IP4252CZ8-4-TTL"
		(extends "NUF4401MN")
		(property "Reference" "U"
			(at -17.145 8.89 0)
		)
		(property "Value" "IP4252CZ8-4-TTL"
			(at 0 9.525 0)
		)
		(property "Footprint" "Package_SON:Nexperia_HUSON-8_USON-8-1EP_1.35x1.7mm_P0.4mm_EP0.4x1.2mm"
			(at -1.27 -6.35 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4251_52_53_54-TTL.pdf"
			(at 3.81 -16.51 0)
		)
		(property "Description" "4 channel EMI filters with integrated ESD protection, 40ohm series resistance, 6pF on each side, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HUSON*1EP*1.35x1.7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "IP4253CZ8-4-TTL"
		(extends "NUF4401MN")
		(property "Reference" "U"
			(at -17.145 8.89 0)
		)
		(property "Value" "IP4253CZ8-4-TTL"
			(at 0 9.525 0)
		)
		(property "Footprint" "Package_SON:Nexperia_HUSON-8_USON-8-1EP_1.35x1.7mm_P0.4mm_EP0.4x1.2mm"
			(at -1.27 -6.35 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4251_52_53_54-TTL.pdf"
			(at 3.81 -16.51 0)
		)
		(property "Description" "4 channel EMI filters with integrated ESD protection, 200ohm series resistance, 15pF on each side, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HUSON*1EP*1.35x1.7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "IP4254CZ8-4-TTL"
		(extends "NUF4401MN")
		(property "Reference" "U"
			(at -17.145 8.89 0)
		)
		(property "Value" "IP4254CZ8-4-TTL"
			(at 0 9.525 0)
		)
		(property "Footprint" "Package_SON:Nexperia_HUSON-8_USON-8-1EP_1.35x1.7mm_P0.4mm_EP0.4x1.2mm"
			(at -1.27 -6.35 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4251_52_53_54-TTL.pdf"
			(at 3.81 -16.51 0)
		)
		(property "Description" "4 channel EMI filters with integrated ESD protection, 100ohm series resistance, 15pF on each side, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI ESD protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HUSON*1EP*1.35x1.7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP349MNAE"
		(extends "NCP349MN")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP349MNAE"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x1.6mm_P0.5mm_EP1.15x1.3mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp349-d.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "28V Positive Overvoltage Protection Controller, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP349MNAM"
		(extends "NCP349MN")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP349MNAM"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x1.6mm_P0.5mm_EP1.15x1.3mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp349-d.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "28V Positive Overvoltage Protection Controller, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP349MNBG"
		(extends "NCP349MN")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP349MNBG"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x1.6mm_P0.5mm_EP1.15x1.3mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp349-d.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "28V Positive Overvoltage Protection Controller, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP349MNBK"
		(extends "NCP349MN")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP349MNBK"
			(at 7.62 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x1.6mm_P0.5mm_EP1.15x1.3mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp349-d.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "28V Positive Overvoltage Protection Controller, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "overvoltage protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PESD5V0L4UF"
		(extends "PESD3V3L4UF")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD5V0L4UF"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-886"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL4UF_G_W.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional quadruple ESD protection diode array, 5.0V, Common Anode, SOT-886"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?886*"
			(at 0 0 0)
		)
	)
	(symbol "PESD5V0L4UG"
		(extends "PESD3V3L4UG")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD5V0L4UG"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL4UF_G_W.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional quadruple ESD protection diode array, 5.0V, Common Anode, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "PESD5V0L4UW"
		(extends "PESD3V3L4UW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD5V0L4UW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-665"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL4UF_G_W.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional quadruple ESD protection diode array, 5.0V, Common Anode, SOT-665"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?665*"
			(at 0 0 0)
		)
	)
	(symbol "PESD5V0L5UF"
		(extends "PESD3V3L5UF")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD5V0L5UF"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-886"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL5UF_V_Y.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional fivefold ESD protection diode array, 5.0V, Common Anode, SOT-886"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?886*"
			(at 0 0 0)
		)
	)
	(symbol "PESD5V0L5UV"
		(extends "PESD3V3L5UV")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD5V0L5UV"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-666"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL5UF_V_Y.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional fivefold ESD protection diode array, 5.0V, Common Anode, SOT-666"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?666*"
			(at 0 0 0)
		)
	)
	(symbol "PESD5V0L5UY"
		(extends "PESD3V3L5UY")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PESD5V0L5UY"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESDXL5UF_V_Y.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Low capacitance unidirectional fivefold ESD protection diode array, 5.0V, Common Anode, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "RCLAMP0502BA"
		(extends "RCLAMP0502B")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "RCLAMP0502BA"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-416"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.semtech.com/products/circuit-protection/low-capacitance/rclamp0502ba"
			(at 1.27 2.54 0)
		)
		(property "Description" "Low capacitance unidirectional dual ESD protection diode, SC-75"
			(at 0 0 0)
		)
		(property "ki_keywords" "tvs unidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?416*"
			(at 0 0 0)
		)
	)
	(symbol "RCLAMP0582B"
		(extends "RCLAMP0502B")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "RCLAMP0582B"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-416"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.semtech.com/products/circuit-protection/low-capacitance/rclamp0582b"
			(at 1.27 2.54 0)
		)
		(property "Description" "Low capacitance unidirectional dual ESD protection diode, SC-75"
			(at 0 0 0)
		)
		(property "ki_keywords" "tvs unidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?416*"
			(at 0 0 0)
		)
	)
	(symbol "SN65240"
		(extends "SN75240")
		(property "Reference" "U"
			(at 0 5.715 0)
		)
		(property "Value" "SN65240"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 3.81 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65220.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "USB port transient suppressors"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm* TSSOP*4.4x3mm*0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SP7538P"
		(extends "RCLAMP3328P")
		(property "Reference" "D"
			(at 13.97 2.54 0)
		)
		(property "Value" "SP7538P"
			(at 13.97 0.635 0)
		)
		(property "Footprint" "Package_DFN_QFN:UDFN-9_1.0x3.8mm_P0.5mm"
			(at 13.97 -1.27 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sp7538p_datasheet.pdf.pdf"
			(at 4.445 0.635 0)
		)
		(property "Description" "Low Capacitance TVS Diode Array, 5.0V Standoff, 8 Channels, UDFN-9"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UDFN*1.0x3.8mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SZNUP2105L"
		(extends "NUP2105L")
		(property "Reference" "D"
			(at 5.715 2.54 0)
		)
		(property "Value" "SZNUP2105L"
			(at 5.715 0.635 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.715 -1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub_link/Collateral/NUP2105L-D.PDF"
			(at 3.175 3.175 0)
		)
		(property "Description" "Dual Line CAN Bus Protector, 24Vrwm, Automotive Grade"
			(at 0 0 0)
		)
		(property "ki_keywords" "can esd protection suppression transient automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-025-100-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-025-100-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 250V 100mA 7.1ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-025-200-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-025-200-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 250V 200mA 4.2ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-025-300-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-025-300-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 250V 300mA 3.2ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-025-500-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-025-500-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 250V 500mA 2.6ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-040-050-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-040-050-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 400V 50mA 14.3ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-040-100-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-040-100-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 400V 100mA 8.1ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-040-200-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-040-200-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 400V 200mA 5.2ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-040-300-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-040-300-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 400V 300mA 4.3ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-040-500-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-040-500-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 400V 500mA 3.6ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-050-050-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-050-050-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 500V 50mA 15.7ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-050-100-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-050-100-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 500V 100mA 9.5ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-050-200-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-050-200-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 500V 200mA 6.6ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-050-300-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-050-300-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 500V 300mA 5.6ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-050-500-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-050-500-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 500V 500mA 5.0ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-065-050-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-065-050-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 650V 50mA 17.7ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-065-100-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-065-100-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 650V 100mA 11.5ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-065-200-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-065-200-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 650V 200mA 8.6ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-065-300-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-065-300-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 650V 300mA 7.6ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-065-500-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-065-500-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 650V 500mA 7.0ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-085-050-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-085-050-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 850V 50mA 21.4ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-085-100-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-085-100-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 850V 100mA 15.2ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-085-200-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-085-200-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 850V 200mA 12.3ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-085-300-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-085-300-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 850V 300mA 11.3ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TBU-CA-085-500-WH"
		(extends "TBU-CA-025-050-WH")
		(property "Reference" "F"
			(at -2.54 0 90)
		)
		(property "Value" "TBU-CA-085-500-WH"
			(at 2.54 0 90)
		)
		(property "Footprint" "Fuse:Fuse_Bourns_TBU-CA"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "Description" "low capacitance single bidirectional high-speed protection, 850V 500mA 10.7ohm, https://www.bourns.com/data/global/pdfs/TBU-CA.pdf"
			(at 0 0 0)
		)
		(property "ki_keywords" "high speed bidirectional protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Bourns*TBU?CA*"
			(at 0 0 0)
		)
	)
	(symbol "TPD1E05U06DYA"
		(extends "TPD1E05U06DPY")
		(property "Reference" "U"
			(at -2.54 3.175 0)
		)
		(property "Value" "TPD1E05U06DYA"
			(at 1.27 3.175 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 2.54 -4.445 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpd1e05u06.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1-Channel ESD Protection for Super-Speed USB 3.0 Interface, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection USB 3.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOD*523*"
			(at 0 0 0)
		)
	)
	(symbol "TPD2EUSB30A"
		(extends "TPD2EUSB30")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "TPD2EUSB30A"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_DRT-3"
			(at -19.05 -7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2eusb30a.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Channel ESD Protection for Super-Speed USB 3.0 Interface, DRT-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection USB 3.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRT*"
			(at 0 0 0)
		)
	)
	(symbol "TPD3S044"
		(extends "TPD3S014")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPD3S044"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd3s014.pdf"
			(at -5.08 6.35 0)
		)
		(property "Description" "Current Limit Switch and D+/D– ESD Protection for USB Host Port, 1.5A, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD-Protection"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPD4E05U06DQA"
		(extends "TPD4EUSB30")
		(property "Reference" "U"
			(at -0.635 8.89 0)
		)
		(property "Value" "TPD4E05U06DQA"
			(at 1.905 -10.16 0)
		)
		(property "Footprint" "Package_SON:USON-10_2.5x1.0mm_P0.5mm"
			(at 1.905 -12.065 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpd4e05u06.pdf"
			(at 1.905 -13.97 0)
		)
		(property "Description" "4-Channel ESD Protection for Super-Speed USB 3.0 Interface, USON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD protection USB 3.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USON*2.5x1.0mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TVS1400DRV"
		(extends "TVS0500DRV")
		(property "Reference" "U"
			(at 2.54 1.27 0)
		)
		(property "Value" "TVS1400DRV"
			(at 2.54 -1.27 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tvs1400.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Flat-Clamp Surge Protection Device. 14Vrwm, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI, ESD, TVS protection transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*EP1x1.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "TVS1800DRV"
		(extends "TVS0500DRV")
		(property "Reference" "U"
			(at 2.54 1.27 0)
		)
		(property "Value" "TVS1800DRV"
			(at 2.54 -1.27 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tvs1800.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Flat-Clamp Surge Protection Device. 18Vrwm, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI, ESD, TVS protection transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*EP1x1.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "TVS2200DRV"
		(extends "TVS0500DRV")
		(property "Reference" "U"
			(at 2.54 1.27 0)
		)
		(property "Value" "TVS2200DRV"
			(at 2.54 -1.27 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tvs2200.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Flat-Clamp Surge Protection Device. 22Vrwm, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI, ESD, TVS protection transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*EP1x1.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "TVS2700DRV"
		(extends "TVS0500DRV")
		(property "Reference" "U"
			(at 2.54 1.27 0)
		)
		(property "Value" "TVS2700DRV"
			(at 2.54 -1.27 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tvs2700.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Flat-Clamp Surge Protection Device. 27Vrwm, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI, ESD, TVS protection transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*EP1x1.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "TVS3300DRV"
		(extends "TVS0500DRV")
		(property "Reference" "U"
			(at 2.54 1.27 0)
		)
		(property "Value" "TVS3300DRV"
			(at 2.54 -1.27 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tvs3300.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Flat-Clamp Surge Protection Device. 33Vrwm, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI, ESD, TVS protection transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*EP1x1.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "USBLC6-2SC6"
		(extends "USBLC6-2P6")
		(property "Reference" "U"
			(at 0.635 5.715 0)
		)
		(property "Value" "USBLC6-2SC6"
			(at 0.635 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/usblc6-2.pdf"
			(at 1.27 -8.255 0)
		)
		(property "Description" "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb ethernet video"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "WE-TVS-824014881"
		(extends "RCLAMP3328P")
		(property "Reference" "D"
			(at 13.97 2.54 0)
		)
		(property "Value" "WE-TVS-824014881"
			(at 13.97 0.635 0)
		)
		(property "Footprint" "Package_DFN_QFN:UDFN-9_1.0x3.8mm_P0.5mm"
			(at 13.97 -1.27 0)
		)
		(property "Datasheet" "https://eu.mouser.com/datasheet/2/445/824014881-1724976.pdf"
			(at 4.445 0.635 0)
		)
		(property "Description" "Obsolete, EOL, TVS Diode Array, 1.2V Standoff, 8 Channels, UDFN-9"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb esd protection suppression transient"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UDFN*1.0x3.8mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "WE-TVS-824015043"
		(extends "USBLC6-4SC6")
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "WE-TVS-824015043"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/824015043.pdf"
			(at 1.27 -10.16 0)
		)
		(property "Description" "Low Capacitance TVS Diode Array, 2 Channels, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESD Protection TVS High-speed USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN056V075A48LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN056V075A48LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 5.6V, 0.75A, 48V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN056V115A24LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN056V115A24LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 5.6V, 1.15A, 24V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN056V230A16LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN056V230A16LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 5.6V, 2.30A, 16V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN059V130A24LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN059V130A24LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 5.9V, 1.30A, 24V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN065V130A24LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN065V130A24LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 6.5V, 1.30A, 24V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN065V230A16LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN065V230A16LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 6.5V, 2.30A, 16V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN098V130A24LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN098V130A24LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 9.8V, 1.30A, 24V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN098V230A16LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN098V230A16LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 9.8V, 2.30A, 16V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN132V075A48LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN132V075A48LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 13.2V, 0.75A, 48V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN132V130A24LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN132V130A24LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 13.2V, 1.30A, 24V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN132V230A16LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN132V230A16LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 13.2V, 2.30A, 16V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
	(symbol "ZEN164V130A24LS"
		(extends "ZEN056V130A24LS")
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ZEN164V130A24LS"
			(at 0 7.62 0)
		)
		(property "Footprint" "Diode_SMD:Littelfuse_PolyZen-LS"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Polymer Protected Zener Diode, 16.4V, 1.30A, 24V, LS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Polymer zener"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Littelfuse*PolyZen*LS*"
			(at 0 0 0)
		)
	)
)
