(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DIO705"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 -6.35 0)
		)
		(property "Value" "DIO705"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://dioo.com/uploads/product/20210528/dae33bc3e6c4b6e07ca730d55ecc4c48.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microprocessor Reset (active-low) circuit with manual reset and watchdog, 4.65Vnom threshold, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DIO705_0_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PFI")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{MR}")
				(number "1")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{WDO}")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{PFO}")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "WDI")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
		)
		(symbol "DIO705_1_1")
		(embedded_fonts no)
	)
	(symbol "LM3880"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "LM3880"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 16.51 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3880.pdf"
			(at 0 0 0)
		)
		(property "Description" "Simple Power Sequencer, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Sequencer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM3880_0_1")
		(symbol "LM3880_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FLAG1")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "FLAG2")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FLAG3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM809"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "LM809"
			(at 5.08 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 7.62 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm809.pdf"
			(at 7.62 2.54 0)
		)
		(property "Description" "Microprocessor Reset (active-low) Circuit, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "reset supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM809_0_1")
		(symbol "LM809_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM810"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "LM810"
			(at 5.08 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 7.62 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm809.pdf"
			(at 7.62 2.54 0)
		)
		(property "Description" "Microprocessor Reset (active-high) Circuit, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "reset supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM810_0_1")
		(symbol "LM810_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "RESET")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX16050xTI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 31.75 0)
		)
		(property "Value" "MAX16050xTI"
			(at 7.62 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX16050-MAX16051.pdf"
			(at 0 0 0)
		)
		(property "Description" "5 Voltage Monitor/Sequencer with Reverse-Sequencing Capability, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "power sequencing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX16050xTI_0_1")
		(symbol "MAX16050xTI_1_1"
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "~{EN_HOLD}")
				(number "14")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "22")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SEQ1")
				(number "25")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "SEQ2")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SEQ3")
				(number "27")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SET1")
				(number "18")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DISC1")
				(number "16")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SET2")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DISC2")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SET3")
				(number "8")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DISC3")
				(number "10")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SET4")
				(number "5")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "DISC4")
				(number "7")
			)
			(pin passive line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "TIMEOUT")
				(number "24")
			)
			(pin passive line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "DELAY")
				(number "23")
			)
			(pin passive line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "ABP")
				(number "3")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin open_collector line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "REM")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "~{OV_OUT}")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT2")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT3")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT4")
				(number "6")
			)
			(pin power_out line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "CP_OUT")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX16051xTI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 31.75 0)
		)
		(property "Value" "MAX16051xTI"
			(at 8.89 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX16050-MAX16051.pdf"
			(at 0 0 0)
		)
		(property "Description" "6 Voltage Monitor/Sequencer with Reverse-Sequencing Capability, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "power sequencing"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX16051xTI_0_1")
		(symbol "MAX16051xTI_1_1"
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "~{EN_HOLD}")
				(number "14")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "22")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "SET1")
				(number "18")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DISC1")
				(number "16")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SET2")
				(number "11")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DISC2")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SET3")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DISC3")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SET4")
				(number "5")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DISC4")
				(number "7")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SET5")
				(number "27")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "DISC5")
				(number "25")
			)
			(pin passive line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "TIMEOUT")
				(number "24")
			)
			(pin passive line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "DELAY")
				(number "23")
			)
			(pin passive line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "ABP")
				(number "3")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin open_collector line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "REM")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "~{OV_OUT}")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "OUT1")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT3")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT4")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT5")
				(number "26")
			)
			(pin power_out line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "CP_OUT")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6355"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 8.89 0)
		)
		(property "Value" "MAX6355"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6351-MAX6360.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Voltage μP Supervisory Circuits, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX6355_0_1")
		(symbol "MAX6355_1_1"
			(pin power_in line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "VCC1")
				(number "6")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "RSTIN")
				(number "5")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "~{MR}")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "VCC2")
				(number "4")
			)
			(pin open_collector line
				(at 17.78 0 180)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6369"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.556 13.462 0)
		)
		(property "Value" "MAX6369"
			(at -6.604 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 16.51 -11.43 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf"
			(at 3.81 12.7 0)
		)
		(property "Description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "watchdog supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX6369_0_1")
		(symbol "MAX6369_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "WDI")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SET0")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SET1")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SET2")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{WDO}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6370"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.556 13.462 0)
		)
		(property "Value" "MAX6370"
			(at -6.604 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 16.51 -11.43 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf"
			(at 3.81 12.7 0)
		)
		(property "Description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "watchdog supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX6370_0_1")
		(symbol "MAX6370_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "WDI")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SET0")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SET1")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SET2")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{WDO}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX690xPA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.144 9.144 0)
		)
		(property "Value" "MAX690xPA"
			(at 2.032 9.144 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0.508 -12.192 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max690-max695.pdf"
			(at 0.508 -8.128 0)
		)
		(property "Description" "Microprocessor Supervisory Circuit, Battery-Backup Power Switching, Power-Fail Comparator, VCC 4.75...5.5V, VBATT 2.0...4.25V, Reset Voltage Threshold 4.65V, Reset Timeout Delay 50ms, Watchdog Timeout 1.6s, DIP-8"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "Supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX690xPA_0_1")
		(symbol "MAX690xPA_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "WDI")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PFI")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBATT")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{PFO}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX691xPE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 13.97 0)
		)
		(property "Value" "MAX691xPE"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX690-MAX695.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microprocessor Supervisory Circuit, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX691xPE_0_1")
		(symbol "MAX691xPE_1_1"
			(pin input line
				(at -19.05 6.35 0)
				(length 2.54)
				(name "PFI")
				(number "9")
			)
			(pin input line
				(at -19.05 3.81 0)
				(length 2.54)
				(name "OSC_IN")
				(number "7")
			)
			(pin input line
				(at -19.05 1.27 0)
				(length 2.54)
				(name "OSC_SEL")
				(number "8")
			)
			(pin input line
				(at -19.05 -2.54 0)
				(length 2.54)
				(name "WDI")
				(number "11")
			)
			(pin power_in line
				(at -19.05 -6.35 0)
				(length 2.54)
				(name "VBATT")
				(number "1")
			)
			(pin input line
				(at -19.05 -10.16 0)
				(length 2.54)
				(name "~{CE_IN}")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 19.05 7.62 180)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin output line
				(at 19.05 5.08 180)
				(length 2.54)
				(name "RESET")
				(number "16")
			)
			(pin output line
				(at 19.05 2.54 180)
				(length 2.54)
				(name "~{PFO}")
				(number "10")
			)
			(pin output line
				(at 19.05 0 180)
				(length 2.54)
				(name "~{LOW_LINE}")
				(number "6")
			)
			(pin output line
				(at 19.05 -2.54 180)
				(length 2.54)
				(name "~{WDO}")
				(number "14")
			)
			(pin output line
				(at 19.05 -5.08 180)
				(length 2.54)
				(name "BATT_ON")
				(number "5")
			)
			(pin power_out line
				(at 19.05 -7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin output line
				(at 19.05 -10.16 180)
				(length 2.54)
				(name "~{CE_OUT}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX691xWE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 13.97 0)
		)
		(property "Value" "MAX691xWE"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX690-MAX695.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microprocessor Supervisory Circuit, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX691xWE_0_1")
		(symbol "MAX691xWE_1_1"
			(pin input line
				(at -19.05 6.35 0)
				(length 2.54)
				(name "PFI")
				(number "9")
			)
			(pin input line
				(at -19.05 3.81 0)
				(length 2.54)
				(name "OSC_IN")
				(number "7")
			)
			(pin input line
				(at -19.05 1.27 0)
				(length 2.54)
				(name "OSC_SEL")
				(number "8")
			)
			(pin input line
				(at -19.05 -2.54 0)
				(length 2.54)
				(name "WDI")
				(number "11")
			)
			(pin power_in line
				(at -19.05 -6.35 0)
				(length 2.54)
				(name "VBATT")
				(number "1")
			)
			(pin input line
				(at -19.05 -10.16 0)
				(length 2.54)
				(name "~{CE_IN}")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 19.05 7.62 180)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin output line
				(at 19.05 5.08 180)
				(length 2.54)
				(name "RESET")
				(number "16")
			)
			(pin output line
				(at 19.05 2.54 180)
				(length 2.54)
				(name "~{PFO}")
				(number "10")
			)
			(pin output line
				(at 19.05 0 180)
				(length 2.54)
				(name "~{LOW_LINE}")
				(number "6")
			)
			(pin output line
				(at 19.05 -2.54 180)
				(length 2.54)
				(name "~{WDO}")
				(number "14")
			)
			(pin output line
				(at 19.05 -5.08 180)
				(length 2.54)
				(name "BATT_ON")
				(number "5")
			)
			(pin power_out line
				(at 19.05 -7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin output line
				(at 19.05 -10.16 180)
				(length 2.54)
				(name "~{CE_OUT}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX805LCSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.144 9.144 0)
		)
		(property "Value" "MAX805LCSA"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.508 -12.192 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX690A-MAX805L.pdf"
			(at 0.508 -8.128 0)
		)
		(property "Description" "Microprocessor Supervisory Circuit, Battery-Backup Power Switching, Power-Fail Comparator, VCC / VBATT 1.1...5.5V, Reset Threshold 4.65V, Reset Pulse Width 200ms, Watchdog Timeout 1.60s, Reset active-high, SOIC-8"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "Supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX805LCSA_0_1")
		(symbol "MAX805LCSA_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "WDI")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PFI")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBATT")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "RESET")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{PFO}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC34064D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "MC34064D"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Undervoltage Sensing Circuit, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC34064D_0_1")
		(symbol "MC34064D_1_1"
			(pin input line
				(at -8.89 1.27 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin no_connect line
				(at -6.35 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -6.35 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 6.35 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin open_collector line
				(at 8.89 1.27 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC34064DM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "MC34064DM"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Undervoltage Sensing Circuit, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC34064DM_0_1")
		(symbol "MC34064DM_1_1"
			(pin input line
				(at -8.89 1.27 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin no_connect line
				(at -6.35 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -6.35 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 6.35 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin open_collector line
				(at 8.89 1.27 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC34064P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MC34064P"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Undervoltage Sensing Circuit, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92L?Inline*"
			(at 0 0 0)
		)
		(symbol "MC34064P_0_1")
		(symbol "MC34064P_1_1"
			(pin input line
				(at -8.89 1.27 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin open_collector line
				(at 8.89 1.27 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC34064SN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MC34064SN"
			(at 6.35 5.08 0)
		)
		(property "Footprint" "Package_SO:TSOP-5_1.65x3.05mm_P0.95mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Undervoltage Sensing Circuit, TSOP-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "MC34064SN_0_1")
		(symbol "MC34064SN_1_1"
			(pin input line
				(at -8.89 1.27 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 0 -6.35 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 2.54 3.81 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin open_collector line
				(at 8.89 1.27 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP100-270D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP100-270D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 2.70V threshold, active low output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
		(symbol "MCP100-270D_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP101-270D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP101-270D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 2.70V threshold, active high output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
		(symbol "MCP101-270D_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "RST")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP120-xxxDxTO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP120-xxxDxTO"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
		(symbol "MCP120-xxxDxTO_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
		)
		(symbol "MCP120-xxxDxTO_1_1"
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP120-xxxGxTO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP120-xxxGxTO"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
		(symbol "MCP120-xxxGxTO_0_1")
		(symbol "MCP120-xxxGxTO_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{RST}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP120-xxxHxTO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP120-xxxHxTO"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
		(symbol "MCP120-xxxHxTO_0_1")
		(symbol "MCP120-xxxHxTO_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{RST}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP120-xxxxSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP120-xxxxSN"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP120-xxxxSN_0_1")
		(symbol "MCP120-xxxxSN_1_1"
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP120-xxxxTT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP120-xxxxTT"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 15.24 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP120-xxxxTT_0_1")
		(symbol "MCP120-xxxxTT_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP130-xxxFxTO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP130-xxxFxTO"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit pull-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
		(symbol "MCP130-xxxFxTO_0_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
		)
		(symbol "MCP130-xxxFxTO_1_1"
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{RST}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC811LUY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC811LUY"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 4.63V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
		(symbol "MIC811LUY_0_1")
		(symbol "MIC811LUY_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{MR}")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCM809"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TCM809"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21661E.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, active low output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC?70*"
			(at 0 0 0)
		)
		(symbol "TCM809_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCM810"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TCM810"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21661E.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, active high output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* *SC?70*"
			(at 0 0 0)
		)
		(symbol "TCM810_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "RESET")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL7702A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TL7702A"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Supply-Voltage Supervisors, 2.53V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TL7702A_0_1")
		(symbol "TL7702A_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{RESIN}")
				(number "2")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CT")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "RESET")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "REF")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL7705AxPS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TL7705AxPS"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x6.2mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Supply-Voltage Supervisors, 4.55V, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x6.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TL7705AxPS_0_1")
		(symbol "TL7705AxPS_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{RESIN}")
				(number "2")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CT")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "RESET")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "REF")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS3430WDRC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 4.064 -11.43 0)
		)
		(property "Value" "TPS3430WDRC"
			(at 11.176 -13.462 0)
		)
		(property "Footprint" "Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm"
			(at 0 -18.288 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TPS3430"
			(at 0 -20.828 0)
		)
		(property "Description" "Window watchdog timer with programmable reset delay"
			(at -0.508 -15.748 0)
		)
		(property "ki_keywords" "watchdog supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSON*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS3430WDRC_0_1")
		(symbol "TPS3430WDRC_1_0"
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDD2")
				(number "10")
			)
		)
		(symbol "TPS3430WDRC_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "WDI")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CRST")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "CWD")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SET0")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SET1")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{WDO}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS3702"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS3702"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps3702.pdf"
			(at -10.16 10.16 0)
		)
		(property "Description" "High-Accuracy, Overvoltage and Undervoltage Monitor, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "protection overvoltage unvervoltage monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS3702_0_1")
		(symbol "TPS3702_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SENSE")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SET")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OV")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "UV")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS3808DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TPS3808DBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps3808.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Low-Quiescent-Current, Programmable-Delay Supervisory Circuit, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "supply voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS3808DBV_0_1")
		(symbol "TPS3808DBV_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SENSE")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{MR}")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CT")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS3831"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "TPS3831"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SON:Texas_X2SON-4_1x1mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/sbvs193d/sbvs193d.pdf"
			(at 0 0 0)
		)
		(property "Description" "150-nA, Ultralow Power, Supply Voltage Monitor, X2SON-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "supply voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*X2SON*1x1mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS3831_0_1")
		(symbol "TPS3831_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{MR}")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "TP")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS3839DBZ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "TPS3839DBZ"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/sbvs193d/sbvs193d.pdf"
			(at 0 0 0)
		)
		(property "Description" "150-nA, Ultralow Power, Supply Voltage Monitor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "supply voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS3839DBZ_0_1")
		(symbol "TPS3839DBZ_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS3839DQN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "TPS3839DQN"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SON:Texas_X2SON-4_1x1mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/sbvs193d/sbvs193d.pdf"
			(at 0 0 0)
		)
		(property "Description" "150-nA, Ultralow Power, Supply Voltage Monitor, X2SON-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "supply voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*X2SON*1x1mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS3839DQN_0_1")
		(symbol "TPS3839DQN_1_1"
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "TP")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAT811JTBI-GT3"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CAT811JTBI-GT3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 4.00V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "CAT811LTBI-GT3"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CAT811LTBI-GT3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 4.63V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "CAT811MTBI-GT3"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CAT811MTBI-GT3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 4.38V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "CAT811RTBI-GT3"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CAT811RTBI-GT3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 2.63V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "CAT811STBI-GT3"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CAT811STBI-GT3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 2.93V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "CAT811TTBI-GT3"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CAT811TTBI-GT3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 3.08V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "CAT811ZTBI-GT3"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CAT811ZTBI-GT3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/CAT811-D.PDF"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 2.32V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "DIO706"
		(extends "DIO705")
		(property "Reference" "U"
			(at -7.112 -8.89 0)
		)
		(property "Value" "DIO706"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://dioo.com/uploads/product/20210528/dae33bc3e6c4b6e07ca730d55ecc4c48.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microprocessor Reset (active-low) circuit with manual reset and watchdog, 4.4Vnom threshold, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DIO706J"
		(extends "DIO705")
		(property "Reference" "U"
			(at -7.112 -8.89 0)
		)
		(property "Value" "DIO706J"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://dioo.com/uploads/product/20210528/dae33bc3e6c4b6e07ca730d55ecc4c48.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microprocessor Reset (active-low) circuit with manual reset and watchdog, 4.0Vnom threshold, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DIO706R"
		(extends "DIO705")
		(property "Reference" "U"
			(at -7.112 -8.89 0)
		)
		(property "Value" "DIO706R"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://dioo.com/uploads/product/20210528/dae33bc3e6c4b6e07ca730d55ecc4c48.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microprocessor Reset (active-low) circuit with manual reset and watchdog, 2.63Vnom threshold, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DIO706S"
		(extends "DIO705")
		(property "Reference" "U"
			(at -7.112 -8.89 0)
		)
		(property "Value" "DIO706S"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://dioo.com/uploads/product/20210528/dae33bc3e6c4b6e07ca730d55ecc4c48.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microprocessor Reset (active-low) circuit with manual reset and watchdog, 2.93Vnom threshold, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DIO706T"
		(extends "DIO705")
		(property "Reference" "U"
			(at -7.112 -8.89 0)
		)
		(property "Value" "DIO706T"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://dioo.com/uploads/product/20210528/dae33bc3e6c4b6e07ca730d55ecc4c48.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microprocessor Reset (active-low) circuit with manual reset and watchdog, 3.08Vnom threshold, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6371"
		(extends "MAX6369")
		(property "Reference" "U"
			(at -3.556 13.462 0)
		)
		(property "Value" "MAX6371"
			(at -6.604 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 16.51 -11.43 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf"
			(at 3.81 12.7 0)
		)
		(property "Description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "watchdog supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6372"
		(extends "MAX6370")
		(property "Reference" "U"
			(at -3.556 13.462 0)
		)
		(property "Value" "MAX6372"
			(at -6.604 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 16.51 -11.43 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf"
			(at 3.81 12.7 0)
		)
		(property "Description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "watchdog supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6373"
		(extends "MAX6369")
		(property "Reference" "U"
			(at -3.556 13.462 0)
		)
		(property "Value" "MAX6373"
			(at -6.604 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 16.51 -11.43 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf"
			(at 3.81 12.7 0)
		)
		(property "Description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "watchdog supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6374"
		(extends "MAX6370")
		(property "Reference" "U"
			(at -3.556 13.462 0)
		)
		(property "Value" "MAX6374"
			(at -6.604 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 16.51 -11.43 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6369-MAX6374.pdf"
			(at 3.81 12.7 0)
		)
		(property "Description" "Precision Pin-Selectable Watchdog Timer, 200us to 60s, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "watchdog supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX690ACSA"
		(extends "MAX690xPA")
		(property "Reference" "U"
			(at -9.144 9.144 0)
		)
		(property "Value" "MAX690ACSA"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.508 -12.192 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX690A-MAX805L.pdf"
			(at 0.508 -8.128 0)
		)
		(property "Description" "Microprocessor Supervisory Circuit, Battery-Backup Power Switching, Power-Fail Comparator, VCC / VBATT 1.0...5.5V, Reset Threshold 4.65V, Reset Pulse Width 200ms, Watchdog Timeout 1.60s, SOIC-8"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "Supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX692xPA"
		(extends "MAX690xPA")
		(property "Reference" "U"
			(at -9.144 9.144 0)
		)
		(property "Value" "MAX692xPA"
			(at 2.032 9.144 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0.508 -12.192 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max690-max695.pdf"
			(at 0.508 -8.128 0)
		)
		(property "Description" "Microprocessor Supervisory Circuit, Battery-Backup Power Switching, Power-Fail Comparator, VCC 4.5...5.5V, VBATT 2.0...4.0V, Reset Voltage Threshold 4.4V, Reset Timeout Delay 50ms, Watchdog Timeout 1.6s, DIP-8"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "Supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX694xPA"
		(extends "MAX690xPA")
		(property "Reference" "U"
			(at -9.144 9.144 0)
		)
		(property "Value" "MAX694xPA"
			(at 2.032 9.144 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0.508 -12.192 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max690-max695.pdf"
			(at 0.508 -8.128 0)
		)
		(property "Description" "Microprocessor Supervisory Circuit, Battery-Backup Power Switching, Power-Fail Comparator, VCC 4.75...5.5V, VBATT 2.0...4.25V, Reset Voltage Threshold 4.65V, Reset Timeout Delay 200ms, Watchdog Timeout 1.6s, DIP-8"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "Supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX811LEUS-T"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX811LEUS-T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 4.63V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "MAX811MEUS-T"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX811MEUS-T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 4.38V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "MAX811REUS-T"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX811REUS-T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 2.63V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "MAX811SEUS-T"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX811SEUS-T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 2.93V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "MAX811TEUS-T"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX811TEUS-T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 3.08V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "MCP100-300D"
		(extends "MCP100-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP100-300D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 3.00V threshold, active low output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP100-315D"
		(extends "MCP100-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP100-315D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 3.15V threshold, active low output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP100-450D"
		(extends "MCP100-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP100-450D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 4.50V threshold, active low output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP100-460D"
		(extends "MCP100-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP100-460D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 4.60V threshold, active low output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP100-475D"
		(extends "MCP100-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP100-475D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 4.75V threshold, active low output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP100-485D"
		(extends "MCP100-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP100-485D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 4.85V threshold, active low output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP101-300D"
		(extends "MCP101-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP101-300D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 3.00V threshold, active high output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP101-315D"
		(extends "MCP101-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP101-315D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 3.15V threshold, active high output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP101-450D"
		(extends "MCP101-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP101-450D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 4.50V threshold, active high output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP101-460D"
		(extends "MCP101-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP101-460D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 4.60V threshold, active high output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP101-475D"
		(extends "MCP101-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP101-475D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 4.75V threshold, active high output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP101-485D"
		(extends "MCP101-270D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MCP101-485D"
			(at -1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11187f.pdf"
			(at -7.62 6.35 0)
		)
		(property "Description" "Microcontroller reset monitor, 4.85V threshold, active high output"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisor reset push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP130-xxxDxTO"
		(extends "MCP120-xxxDxTO")
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP130-xxxDxTO"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit pull-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "MCP130-xxxHxTO"
		(extends "MCP120-xxxHxTO")
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP130-xxxHxTO"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit pull-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "MCP130-xxxxSN"
		(extends "MCP120-xxxxSN")
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP130-xxxxSN"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit pull-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP130-xxxxTT"
		(extends "MCP120-xxxxTT")
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "MCP130-xxxxTT"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 15.24 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/11184d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller supervisory circuit with internal 5 kΩ pull-up, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "supervisory circuit pull-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC811JUY"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC811JUY"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 4.00V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "MIC811MUY"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC811MUY"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 4.38V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "MIC811RUY"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC811RUY"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 2.63V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "MIC811SUY"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC811SUY"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 2.93V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "MIC811TUY"
		(extends "MIC811LUY")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC811TUY"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic811.pdf"
			(at -8.89 -17.78 0)
		)
		(property "Description" "Power supply supervisor, Manual reset, Threshold 3.08V, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Supervisor Reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
	)
	(symbol "TL7702B"
		(extends "TL7702A")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TL7702B"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Supply-Voltage Supervisors, 2.53V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL7705A"
		(extends "TL7702A")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TL7705A"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Supply-Voltage Supervisors, 4.55V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL7705B"
		(extends "TL7702A")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TL7705B"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Supply-Voltage Supervisors, 4.55V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL7709A"
		(extends "TL7702A")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TL7709A"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Supply-Voltage Supervisors, 7.6V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL7712A"
		(extends "TL7702A")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TL7712A"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Supply-Voltage Supervisors, 10.8V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL7715A"
		(extends "TL7702A")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TL7715A"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Supply-Voltage Supervisors, 13.5V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL7733B"
		(extends "TL7702A")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TL7733B"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tl7705b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Supply-Voltage Supervisors, 3.08V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV810EA29DBZ"
		(extends "TCM810")
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "TLV810EA29DBZ"
			(at 10.16 12.7 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv803e.pdf"
			(at 0 0 0)
		)
		(property "Description" "push-pull, active-high, 200mS reset delay, 2.93V threshold voltage, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage supervisor low power small size"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX692ACSA"
		(extends "MAX690ACSA")
		(property "Reference" "U"
			(at -9.144 9.144 0)
		)
		(property "Value" "MAX692ACSA"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.508 -12.192 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX690A-MAX805L.pdf"
			(at 0.508 -8.128 0)
		)
		(property "Description" "Microprocessor Supervisory Circuit, Battery-Backup Power Switching, Power-Fail Comparator, VCC / VBATT 1.0...5.5V, Reset Threshold 4.40V, Reset Pulse Width 200ms, Watchdog Timeout 1.60s, SOIC-8"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "Supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX802LCSA"
		(extends "MAX690ACSA")
		(property "Reference" "U"
			(at -9.144 9.144 0)
		)
		(property "Value" "MAX802LCSA"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.508 -12.192 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX690A-MAX805L.pdf"
			(at 0.508 -8.128 0)
		)
		(property "Description" "Microprocessor Supervisory Circuit, Battery-Backup Power Switching, Power-Fail Comparator accuracy ±2%, VCC / VBATT 1.0...5.5V, Reset Threshold 4.65V, Reset Pulse Width 200ms, Watchdog Timeout 1.60s, SOIC-8"
			(at 0 -10.16 0)
		)
		(property "ki_keywords" "Supervisor wdg"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
	)
)
