(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "0900PC15J0013"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 8.89 0)
		)
		(property "Value" "0900PC15J0013"
			(at 5.715 8.89 0)
		)
		(property "Footprint" "RF_Converter:Balun_Johanson_0900PC15J0013"
			(at 4.445 -10.16 0)
		)
		(property "Datasheet" "https://www.johansontechnology.com/datasheets/0900PC15J0013/0900PC15J0013.pdf"
			(at 0 0 0)
		)
		(property "Description" "868/915MHz Impedance Matched, Multi-Function, Integrated Ceramic Passive Component for Texas Instruments CC112x, CC117x & CC12xx Chipsets"
			(at 0 0 0)
		)
		(property "ki_keywords" "CC1120 CC1121 CC1125 CC1175 CC1200 CC1201 balun"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Balun*Johanson*0900PC15J0013*"
			(at 0 0 0)
		)
		(symbol "0900PC15J0013_0_1")
		(symbol "0900PC15J0013_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LNA_P")
				(number "2")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "LNA_N")
				(number "1")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "TRX")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PA")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ANT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADC-10-1R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "ADC-10-1R"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_LandPatternPL-094"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADC-10-1R.pdf"
			(at 5.08 -8.89 0)
		)
		(property "Description" "Directional Coupler, 5 to 900 MHz, 10 dB Coupling, 50 Ohm, Mini-Circuits CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Directional Coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADC-10-1R_0_1")
		(symbol "ADC-10-1R_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 6.35 0 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "OUT")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "CPL")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADCH-80"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at -7.62 6.35 0)
		)
		(property "Value" "ADCH-80"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADCH-80+.pdf"
			(at 0 0 0)
		)
		(property "Description" "50-10000MHz, RF Choke, Mini-Circuits CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "bias filter DC choke"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADCH-80_0_1")
		(symbol "ADCH-80_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "RF&DC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "DC")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADCH-80A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at -7.62 6.35 0)
		)
		(property "Value" "ADCH-80A"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADCH-80A+.pdf"
			(at 0 0 0)
		)
		(property "Description" "50-10000MHz, RF Choke, Mini-Circuits CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "bias filter DC choke"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADCH-80A_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "RF&DC")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "DC")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADL5904"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "ADL5904"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADL5904.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "DC to 6 GHz, 45 dB TruPwr Detector with Envelope Threshold Detection, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "RMS power detector log decibel dB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADL5904_0_1")
		(symbol "ADL5904_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "ENBL")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RST")
				(number "15")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN-")
				(number "16")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RFIN")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CRMS")
				(number "9")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DECL")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VPOS")
				(number "5")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VPOS")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "8")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "Q")
				(number "12")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{Q}")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VCAL")
				(number "3")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VRMS")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP-2-1W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "ADP-2-1W"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD636_LandPatternPL-035"
			(at -3.81 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADP-2-1W.pdf"
			(at -1.27 -8.89 0)
		)
		(property "Description" "Power splitter combiner, 1 to 650 MHz, 2 way 0-degree, 50 ohm, Mini-Circuits CD636"
			(at 0 0 0)
		)
		(property "ki_keywords" "splitter combiner"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD636*"
			(at 0 0 0)
		)
		(symbol "ADP-2-1W_0_1")
		(symbol "ADP-2-1W_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 5.08)
				(name "SUM")
				(number "1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 5.08)
				(name "PORT1")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 5.08)
				(name "PORT2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMK-2-13"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "AMK-2-13"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_LandPatternPL-052"
			(at -6.35 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/AMK-2-13+.pdf"
			(at -3.81 -6.35 0)
		)
		(property "Description" "2x Frequency Multiplier, output 20 to 1000 MHz, 50 Ohm, Mini-Circuits CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "frequency multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "AMK-2-13_0_0"
			(text "2x"
				(at 0 3.81 0)
			)
		)
		(symbol "AMK-2-13_0_1")
		(symbol "AMK-2-13_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "F_IN")
				(number "3")
			)
			(pin no_connect line
				(at -6.35 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "2F_OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AX5043"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "AX5043"
			(at 8.89 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm"
			(at 53.34 36.83 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/AX5043-D.PDF"
			(at 34.29 34.29 0)
		)
		(property "Description" "Advanced High Performance ASK and FSK Narrow-band Transceiver for 27 - 1050 MHz Range"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF, transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?28*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AX5043_1_0")
		(symbol "AX5043_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "CLK16N")
				(number "27")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "CLK16P")
				(number "28")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "GPADC1")
				(number "25")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "GPADC2")
				(number "26")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "15")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "MISO")
				(number "16")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "MOSI")
				(number "17")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SEL")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "FILT")
				(number "8")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "L2")
				(number "9")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "L1")
				(number "10")
			)
			(pin no_connect line
				(at -5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD_IO")
				(number "23")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDD_ANA")
				(number "1")
			)
			(pin no_connect line
				(at 2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin power_out line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VDD_ANA")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "ANTSEL")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PWRAMP")
				(number "20")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IRQ")
				(number "19")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "ANTP1")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "ANTN")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ANTP")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SYSCLK")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "DCLK")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "DATA")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC1000"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "CC1000"
			(at -24.13 15.24 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 8.89 15.24 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/cc1000.pdf"
			(at -1.27 2.54 0)
		)
		(property "Description" "Single Chip Low Power RF Transceiver, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power RF Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CC1000_0_1")
		(symbol "CC1000_1_1"
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "PDATA")
				(number "26")
			)
			(pin input clock
				(at -27.94 7.62 0)
				(length 3.81)
				(name "PCLK")
				(number "25")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "PALE")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "DIO")
				(number "23")
			)
			(pin output clock
				(at -27.94 0 0)
				(length 3.81)
				(name "DCLK")
				(number "24")
			)
			(pin passive line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RSSI/IF")
				(number "28")
			)
			(pin passive line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "XOSC_Q1")
				(number "18")
			)
			(pin passive line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "XOSC_Q2")
				(number "17")
			)
			(pin power_in line
				(at -10.16 -17.78 90)
				(length 3.81)
				(name "DGND")
				(number "20")
			)
			(pin power_in line
				(at -7.62 17.78 270)
				(length 3.81)
				(name "DVDD")
				(number "21")
			)
			(pin power_in line
				(at -7.62 -17.78 90)
				(length 3.81)
				(name "DGND")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "AGND")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "AVDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "AGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "AVDD")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "AGND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 3.81)
				(name "AVDD")
				(number "9")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 3.81)
				(name "AGND")
				(number "8")
			)
			(pin power_in line
				(at 7.62 17.78 270)
				(length 3.81)
				(name "AVDD")
				(number "15")
			)
			(pin power_in line
				(at 7.62 -17.78 90)
				(length 3.81)
				(name "AGND")
				(number "14")
			)
			(pin power_in line
				(at 10.16 -17.78 90)
				(length 3.81)
				(name "AGND")
				(number "16")
			)
			(pin power_in line
				(at 12.7 -17.78 90)
				(length 3.81)
				(name "AGND")
				(number "19")
			)
			(pin passive line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "RF_IN")
				(number "3")
			)
			(pin passive line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "RF_OUT")
				(number "4")
			)
			(pin passive line
				(at 27.94 0 180)
				(length 3.81)
				(name "L1")
				(number "10")
			)
			(pin passive line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "L2")
				(number "11")
			)
			(pin passive line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "CHP_OUT")
				(number "12")
			)
			(pin passive line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "R_BIAS")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC1200"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "CC1200"
			(at -10.16 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 15.24 29.21 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cc1200.pdf"
			(at -12.7 29.21 0)
		)
		(property "Description" "Low-Power, High-Performance RF Transceiver, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Tx Rx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CC1200_0_1")
		(symbol "CC1200_1_1"
			(pin input line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "~{RESET}")
				(number "2")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "~{CS}")
				(number "11")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "SCLK")
				(number "8")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "SI")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "SO(GPIO1)")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "GPIO0")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "GPIO2")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "GPIO3")
				(number "3")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "XOSC_Q1")
				(number "30")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "XOSC_Q2")
				(number "31")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "EXT_XOSC")
				(number "32")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "RBIAS")
				(number "14")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "LPF0")
				(number "23")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "LPF1")
				(number "24")
			)
			(pin power_in line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "GND_EP")
				(number "33")
			)
			(pin power_in line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "DVDD")
				(number "5")
			)
			(pin power_in line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "DVDD")
				(number "12")
			)
			(pin power_in line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "VDD_GUARD")
				(number "1")
			)
			(pin power_in line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "AVDD_IF")
				(number "13")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "AVDD_RF")
				(number "15")
			)
			(pin power_in line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "AVDD_PFD_CHP")
				(number "25")
			)
			(pin power_in line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "AVDD_XOSC")
				(number "28")
			)
			(pin power_in line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "AVDD_SYNTH1")
				(number "22")
			)
			(pin power_in line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "AVDD_SYNTH2")
				(number "27")
			)
			(pin power_out line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "DCPL")
				(number "6")
			)
			(pin power_out line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "DCPL_VCO")
				(number "21")
			)
			(pin power_out line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "DCPL_PFD_CHP")
				(number "26")
			)
			(pin power_out line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "DCPL_XOSC")
				(number "29")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "LNA_P")
				(number "19")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "LNA_N")
				(number "20")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "TRX_SW")
				(number "18")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "PA")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC2500"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 13.97 0)
		)
		(property "Value" "CC2500"
			(at 13.97 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGP0020H_VQFN-20-1EP_4x4mm_P0.5mm_EP2.4x2.4mm"
			(at 1.27 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cc2500.pdf"
			(at 5.08 15.24 0)
		)
		(property "Description" "Single Chip Low Power RF Transceiver, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power RF Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGP0020H*"
			(at 0 0 0)
		)
		(symbol "CC2500_0_1")
		(symbol "CC2500_1_1"
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "SO(GDO1)")
				(number "2")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "7")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "SI")
				(number "20")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "XOSC_Q1")
				(number "8")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "XOSC_Q2")
				(number "10")
			)
			(pin passive line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RBIAS")
				(number "17")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "DVDD")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD_GUARD")
				(number "18")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 2.54 15.24 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "11")
			)
			(pin passive line
				(at 2.54 15.24 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "14")
			)
			(pin passive line
				(at 2.54 15.24 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "15")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "AVDD")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "GDO2")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GDO0(ATEST)")
				(number "6")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "RF_P")
				(number "12")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RF_N")
				(number "13")
			)
			(pin power_out line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "DCOUPL")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC4759J5020AHF-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DC4759J5020AHF-1"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:Anaren_0805_2012Metric-6"
			(at 1.27 0 0)
		)
		(property "Datasheet" "https://cdn.anaren.com/product-documents/Xinger/DirectionalCouplers/DC4759J5020AHF/DC4759J5020AHF_DataSheet(Rev_E).pdf"
			(at 0.254 0 0)
		)
		(property "Description" "4.7-5.9GHz 20dB Directional Coupler, Configuration 1, Anaren 0805"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Anaren*0805*2012Metric*"
			(at 0 0 0)
		)
		(symbol "DC4759J5020AHF-1_0_1")
		(symbol "DC4759J5020AHF-1_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Input")
				(number "6")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Isolated")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Direct")
				(number "1")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Coupled")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC4759J5020AHF-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DC4759J5020AHF-2"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:Anaren_0805_2012Metric-6"
			(at 1.27 0 0)
		)
		(property "Datasheet" "https://cdn.anaren.com/product-documents/Xinger/DirectionalCouplers/DC4759J5020AHF/DC4759J5020AHF_DataSheet(Rev_E).pdf"
			(at 0.254 0 0)
		)
		(property "Description" "4.7-5.9GHz 20dB Directional Coupler, Configuration 2, Anaren 0805"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Anaren*0805*2012Metric*"
			(at 0 0 0)
		)
		(symbol "DC4759J5020AHF-2_0_1")
		(symbol "DC4759J5020AHF-2_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Input")
				(number "1")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Isolated")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Direct")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Coupled")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DW1000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 34.29 0)
		)
		(property "Value" "DW1000"
			(at 16.51 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.decawave.com/wp-content/uploads/2020/04/DW1000_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra Wideband transceiver, 6.8Mbps data rates, 3.5GHz to 6.5GHz, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Wideband UWB transceiver IEEE802.15.4-2011 Decawave Qorvo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "DW1000_0_1")
		(symbol "DW1000_1_1"
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "GPIO0/RXOKLED")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "GPIO1/SFDLED")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "GPIO2/RXLED")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "GPIO3/TXLED")
				(number "35")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "GPIO4/EXTPA")
				(number "34")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "GPIO5/EXTTXE/SPIPOL")
				(number "33")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "GPIO6/EXTRXE/SPIPHA")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "SYNC/GPIO7")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "IRQ/GPIO8")
				(number "45")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "SPICLK")
				(number "41")
			)
			(pin output line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "SPIMISO")
				(number "40")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "SPIMOSI")
				(number "39")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "~{SPICS}")
				(number "24")
			)
			(pin input line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "FORCEON")
				(number "22")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "WAKEUP")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "~{RST}")
				(number "27")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "EXTCLK/XTAL1")
				(number "3")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "XTAL2")
				(number "4")
			)
			(pin power_in line
				(at -15.24 35.56 270)
				(length 2.54)
				(name "VDDLDOD")
				(number "26")
			)
			(pin power_in line
				(at -10.16 35.56 270)
				(length 2.54)
				(name "VDDIOA")
				(number "28")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 2.54)
				(name "VDDAON")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSSIO")
				(number "32")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSIO")
				(number "43")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDPA1")
				(number "18")
			)
			(pin no_connect line
				(at 0 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 0 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 0 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VDDPA2")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 7.62 35.56 270)
				(length 2.54)
				(name "VDDLNA")
				(number "15")
			)
			(pin power_in line
				(at 12.7 35.56 270)
				(length 2.54)
				(name "VDDLDOA")
				(number "48")
			)
			(pin power_in line
				(at 17.78 35.56 270)
				(length 2.54)
				(name "VDDBATT")
				(number "47")
			)
			(pin output line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "EXTON")
				(number "21")
			)
			(pin power_out line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "VDDREG")
				(number "20")
			)
			(pin power_out line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "VDDDIG")
				(number "44")
			)
			(pin power_out line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "VDDIO")
				(number "31")
			)
			(pin power_out line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "VDDIO")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "RF_P")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "RF_N")
				(number "17")
			)
			(pin power_out line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "VDDCLK")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "CLKTUNE")
				(number "8")
			)
			(pin power_out line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "VDDVCO")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "VCOTUNE")
				(number "12")
			)
			(pin power_out line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "VDDSYN")
				(number "10")
			)
			(pin power_out line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "VDDIF")
				(number "7")
			)
			(pin power_out line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "VDDMS")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "VREF")
				(number "5")
			)
			(pin input line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "TESTMODE")
				(number "46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "F115"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "F115"
			(at -8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2205181716_Synoxo-F115_C3010244.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Synoxo 300-450MHz ASK/OOK Transmitter, +10dBm, 10kbps, Sleep/Wake Function, 1.8-3.6V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synoxo SYN115 RF Transmitter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT-23-6*"
			(at 0 0 0)
		)
		(symbol "F115_0_0"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ASK")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "XTLIN")
				(number "5")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "XTLOUT")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PAOUT")
				(number "1")
			)
		)
		(symbol "F115_1_1")
		(embedded_fonts no)
	)
	(symbol "HMC394LP4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "HMC394LP4"
			(at 11.43 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.8x2.8mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/hmc394.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "GaAs HBT Programmable 5-bit Counter, DC - 2.2 GHz, QFN-24-1EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "counter prescaler programmable frequency divider"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "HMC394LP4_0_1")
		(symbol "HMC394LP4_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{IN}")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT")
				(number "16")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{OUT}")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HMC431"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "HMC431"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.8x2.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/hmc431.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.5-6.1GHz VCO, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "vco rf"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "HMC431_0_1")
		(symbol "HMC431_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VTUNE")
				(number "22")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RFOUT")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LAT-3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "LAT-3"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_MMM168_LandPatternPL-225"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LAT-3+.pdf"
			(at 0 0.635 0)
		)
		(property "Description" "Attenuator, 3dB, 0.5W, DC to 2500 MHz, 50 Ohm, Mini-Circuits MMM168"
			(at 0 0 0)
		)
		(property "ki_keywords" "attenuator rf"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*MMM168*"
			(at 0 0 0)
		)
		(symbol "LAT-3_0_1")
		(symbol "LAT-3_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "IN")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LRPS-2-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "LRPS-2-1"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_QQQ130_LandPattern_PL-236_ClockwisePinNumbering"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LRPS-2-1.pdf"
			(at -1.27 -8.89 0)
		)
		(property "Description" "Power Splitter/Combiner, 5 to 500 MHz, 50 Ohm"
			(at 0 0 0)
		)
		(property "ki_keywords" "power splitter combiner"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*QQQ130*"
			(at 0 0 0)
		)
		(symbol "LRPS-2-1_0_1")
		(symbol "LRPS-2-1_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 5.08)
				(name "SUM")
				(number "6")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 5.08)
				(name "PORT1")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 5.08)
				(name "PORT2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC5507ES6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.858 6.35 0)
		)
		(property "Value" "LTC5507ES6"
			(at 6.604 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at -0.508 -25.146 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/5507f.pdf"
			(at 0.254 -22.098 0)
		)
		(property "Description" "100kHz to 1GHz RF Power Detector, 2.7..6V supply, TSOT-23-6"
			(at 0.508 -19.05 0)
		)
		(property "ki_keywords" "analog linear"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*6*"
			(at 0 0 0)
		)
		(symbol "LTC5507ES6_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PCAP")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RF_{IN}")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAADSS0008"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAADSS0008"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 0 0)
		)
		(property "Datasheet" "http://cdn.macom.com/datasheets/maadss0008.pdf"
			(at 1.778 -2.413 0)
		)
		(property "Description" "0-2GHz, 15dB step attenuator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*5*"
			(at 0 0 0)
		)
		(symbol "MAADSS0008_0_1")
		(symbol "MAADSS0008_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RF1")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V1")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V2")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "RF2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAAVSS0004"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MAAVSS0004"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/MAAVSS0004.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-2GHz, 35dB, Voltage Variable Absorptive Attenuator, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "VVA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAAVSS0004_0_1")
		(symbol "MAAVSS0004_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "RF1")
				(number "14")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "VC")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "RF2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC12080"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "MC12080"
			(at 5.08 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC12080-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1.1 GHz Prescaler, divide by 10 20 40 80, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "prescaler frequency divider"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC12080_0_1")
		(symbol "MC12080_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "~{IN}")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "SW1")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "SW2")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 3.81)
				(name "SW3")
				(number "7")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC12093D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "MC12093D"
			(at 5.08 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC12093-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "/2, /4, /8, 1.1 GHz Low Power Prescaler with Stand‐By Mode, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "prescaler frequency divider"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC12093D_0_1")
		(symbol "MC12093D_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "~{IN}")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "SB")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "SW1")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 3.81)
				(name "SW2")
				(number "3")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MICRF112YMM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MICRF112YMM"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MICRF112.pdf"
			(at -7.62 1.27 0)
		)
		(property "Description" "ASK/FSK Transmitter, 1.8-3.6V, 300-450MHz, +10dBm, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ask fsk ism transmitter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MICRF112YMM_0_1")
		(symbol "MICRF112YMM_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "FSK")
				(number "6")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "ASK")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "XTLIN")
				(number "2")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "XTLOUT")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "XTAL_MOD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "VSSPA")
				(number "8")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PAOUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MICRF220AYQS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MICRF220AYQS"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/micrf220.pdf"
			(at 8.89 19.05 0)
		)
		(property "Description" "ASK Receiver 3.0-3.6V, 300-450MHz, -110dBm, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "ask receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MICRF220AYQS_0_1")
		(symbol "MICRF220AYQS_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "ANT")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RO1")
				(number "1")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO2")
				(number "16")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CTH")
				(number "12")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CAGC")
				(number "13")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SQ")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GNDRF")
				(number "2")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GNDRF")
				(number "4")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "DO")
				(number "10")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RSSI")
				(number "14")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SEL0")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SEL1")
				(number "11")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{SHDN}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MRF89XA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U2"
			(at -8.89 24.13 0)
		)
		(property "Value" "MRF89XA"
			(at 6.35 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70000622D.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Ultra Low-Power, Integrated ISM Band Sub-GHz Transceiver, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Tx Rx"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MRF89XA_0_1")
		(symbol "MRF89XA_1_1"
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "RFIO")
				(number "31")
			)
			(pin power_out line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PARS")
				(number "29")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PLLN")
				(number "6")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PLLP")
				(number "7")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "OSC1")
				(number "10")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "OSC2")
				(number "11")
			)
			(pin power_out line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VCORS")
				(number "3")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VCOTN")
				(number "4")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "VCOTP")
				(number "5")
			)
			(pin power_out line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "AVRS")
				(number "27")
			)
			(pin power_out line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "DVRS")
				(number "28")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "V_{DD}")
				(number "26")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{CSDAT}")
				(number "15")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{CSCON}")
				(number "14")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SCK")
				(number "18")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SDI")
				(number "17")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDO")
				(number "16")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IRQ0")
				(number "21")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "IRQ1")
				(number "22")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PLOCK")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DATA")
				(number "20")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CLKOUT")
				(number "19")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "RST/TEST8")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NRF24L01"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "NRF24L01"
			(at 5.08 17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 20.32 0)
		)
		(property "Datasheet" "http://www.nordicsemi.com/eng/content/download/2730/34105/file/nRF24L01_Product_Specification_v2_0.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Ultra low power 2.4GHz RF Transceiver, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power RF Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4*0.5mm*"
			(at 0 0 0)
		)
		(symbol "NRF24L01_0_1")
		(symbol "NRF24L01_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "MOSI")
				(number "4")
			)
			(pin output line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "MISO")
				(number "5")
			)
			(pin input clock
				(at -15.24 7.62 0)
				(length 3.81)
				(name "SCK")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "CSN")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "CE")
				(number "1")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "IRQ")
				(number "6")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "IREF")
				(number "16")
			)
			(pin power_out line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "DVDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "VDD_PA")
				(number "11")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "ANT1")
				(number "12")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "ANT2")
				(number "13")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "XC1")
				(number "10")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "XC2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NRF24L01_Breakout"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 12.7 0)
		)
		(property "Value" "NRF24L01_Breakout"
			(at 3.81 12.7 0)
		)
		(property "Footprint" "RF_Module:nRF24L01_Breakout"
			(at 3.81 15.24 0)
		)
		(property "Datasheet" "http://www.nordicsemi.com/eng/content/download/2730/34105/file/nRF24L01_Product_Specification_v2_0.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Ultra low power 2.4GHz RF Transceiver, Carrier PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power RF Transceiver breakout carrier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "nRF24L01*Breakout*"
			(at 0 0 0)
		)
		(symbol "NRF24L01_Breakout_0_1")
		(symbol "NRF24L01_Breakout_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "MOSI")
				(number "6")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "MISO")
				(number "7")
			)
			(pin input clock
				(at -12.7 2.54 0)
				(length 3.81)
				(name "SCK")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "~{CSN}")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "CE")
				(number "3")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IRQ")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAT1220-C-0DB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-0DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 0dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
		(symbol "PAT1220-C-0DB_0_1"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "PAT1220-C-0DB_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PD4859J5050S2HF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PD4859J5050S2HF"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "RF_Converter:Anaren_0805_2012Metric-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://cdn.anaren.com/product-documents/Xinger/PowerDividers/PD4859J5050S2HF/PD4859J5050S2HF_DataSheet(Rev_D).pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "4.8-5.9GHz Wilkinson Power Divider, Anaren 0805"
			(at 0 0 0)
		)
		(property "ki_keywords" "rf power divider wilkinson"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Anaren*0805*2012Metric*"
			(at 0 0 0)
		)
		(symbol "PD4859J5050S2HF_0_1")
		(symbol "PD4859J5050S2HF_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Input")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Output1")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Output2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RMK-3-451"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "RMK-3-451"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_TT1224_LandPatternPL-258_ClockwisePinNumbering"
			(at -6.35 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/RMK-3-451+.pdf"
			(at -3.81 -6.35 0)
		)
		(property "Description" "3x Frequency Multiplier, output 300 to 450 MHz, 50 Ohm, Mini-Circuits TT1224"
			(at 0 0 0)
		)
		(property "ki_keywords" "frequency multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*TT1224*"
			(at 0 0 0)
		)
		(symbol "RMK-3-451_0_0"
			(text "3x"
				(at 0 3.81 0)
			)
		)
		(symbol "RMK-3-451_0_1")
		(symbol "RMK-3-451_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "F_IN")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "3F_OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RMK-5-51"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "RMK-5-51"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_TT1224_LandPatternPL-258_ClockwisePinNumbering"
			(at -6.35 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/RMK-5-51+.pdf"
			(at -3.81 -6.35 0)
		)
		(property "Description" "5x Frequency Multiplier, Output 37.5 to 52.5 MHz, 50 Ohm, Mini-Circuits TT1224"
			(at 0 0 0)
		)
		(property "ki_keywords" "frequency multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*TT1224*"
			(at 0 0 0)
		)
		(symbol "RMK-5-51_0_0"
			(text "5x"
				(at 0 3.81 0)
			)
		)
		(symbol "RMK-5-51_0_1")
		(symbol "RMK-5-51_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "F_IN")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "5F_OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SE5004L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "SE5004L"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/SkyWorks/Documents/Products/601-700/SE5004L_202393B.pdf"
			(at 0 0 0)
		)
		(property "Description" "5 GHz, 26dBm Power Amplifier with Power Detector, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Power Amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SE5004L_0_1")
		(symbol "SE5004L_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SP1")
				(number "6")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SP2")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "VREF")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RFIN")
				(number "3")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 2.54)
				(name "VCC1")
				(number "20")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC2")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC2")
				(number "19")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VCC3")
				(number "9")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 2.54)
				(name "VCC3")
				(number "18")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "DET")
				(number "10")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "RFOUT")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SX1231IMLTRT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "SX1231IMLTRT"
			(at 8.89 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.25x3.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/44000000MDkO/lWPNMeJClEs8Zvyu7AlDlKSyZqhYdVpQzFLVfUp.EXs"
			(at 0 0 0)
		)
		(property "Description" "Low Power Integrated UHF Transceiver, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "UHF Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SX1231IMLTRT_0_1")
		(symbol "SX1231IMLTRT_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SCK")
				(number "15")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "MISO")
				(number "16")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "MOSI")
				(number "17")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "NSS")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DIO0")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIO1/DCLK")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DIO2/DATA")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DIO3")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DIO4")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "DIO5")
				(number "12")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "RESET")
				(number "6")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VBAT1")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VBAT2")
				(number "13")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA_BOOST")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "RFIO")
				(number "21")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "RXTX")
				(number "19")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "XTA")
				(number "4")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "XTB")
				(number "5")
			)
			(pin power_out line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "VR_ANA")
				(number "2")
			)
			(pin power_out line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "VR_DIG")
				(number "3")
			)
			(pin power_out line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SX1262IMLTRT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 24.13 0)
		)
		(property "Value" "SX1262IMLTRT"
			(at 13.97 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 1.27 -31.75 0)
		)
		(property "Datasheet" "https://semtech.file.force.com/sfc/dist/version/download/?oid=00DE0000000JelG&ids=0682R00000IjPWSQA3&d=%2Fa%2F2R000000Un7F%2FyT.fKdAr9ZAo3cJLc4F2cBdUsMftpT2vsOICP7NmvMo"
			(at 1.27 -29.21 0)
		)
		(property "Description" "150 MHz to 960 MHz Low Power Long Range Transceiver, 22dBm output power, spreading factor from 5 to 12, LoRA, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "low-power lora transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SX1262IMLTRT_0_1")
		(symbol "SX1262IMLTRT_1_1"
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "XTA")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "XTB")
				(number "4")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIO1")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIO2")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIO3")
				(number "6")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SCK")
				(number "18")
			)
			(pin tri_state inverted
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "MISO")
				(number "16")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "MOSI")
				(number "17")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "NSS")
				(number "19")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VDD_IN")
				(number "1")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VBAT")
				(number "10")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VBAT_IO")
				(number "11")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "VREG")
				(number "7")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "DCC_SW")
				(number "9")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VR_PA")
				(number "24")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "RFO")
				(number "23")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RFI_N")
				(number "22")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RFI_P")
				(number "21")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "BUSY")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SX1272"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 24.13 0)
		)
		(property "Value" "SX1272"
			(at 13.97 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.8x4.8mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/440000001NCE/v_VBhk1IolDgxwwnOpcS_vTFxPfSEPQbuneK3mWsXlU"
			(at 0 -5.08 0)
		)
		(property "Description" "860 MHz to 1020 MHz Low Power Long Range Transceiver, spreading factor from 6 to 12, LoRA, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "low-power lora transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SX1272_0_1")
		(symbol "SX1272_1_1"
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "XTA")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "XTB")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIO0")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIO1")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIO2")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIO3")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIO4")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DIO5")
				(number "14")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SCK")
				(number "17")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "MISO")
				(number "18")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "MOSI")
				(number "19")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "NSS")
				(number "20")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VBAT1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VBAT2")
				(number "15")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VR_ANA")
				(number "2")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VR_DIG")
				(number "3")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 12.7 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA_BOOST")
				(number "27")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VR_PA")
				(number "28")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "RFO")
				(number "24")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RFI")
				(number "25")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RXTX")
				(number "23")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "RF_MOD")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SX1276"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 24.13 0)
		)
		(property "Value" "SX1276"
			(at 13.97 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.8x4.8mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/2R0000001Rbr/6EfVZUorrpoKFfvaF_Fkpgp5kzjiNyiAbqcpqh9qSjE"
			(at 0 -5.08 0)
		)
		(property "Description" "137 MHz to 1020 MHz Low Power Long Range Transceiver, spreading factor from 6 to 12, LoRA, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "low-power lora transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SX1276_0_1")
		(symbol "SX1276_1_1"
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "XTA")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "XTB")
				(number "6")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIO0")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIO1")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIO2")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIO3")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIO4")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DIO5")
				(number "13")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SCK")
				(number "16")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "MISO")
				(number "17")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "MOSI")
				(number "18")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "NSS")
				(number "19")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VBAT_ANA")
				(number "3")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VBAT_DIG")
				(number "14")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VBAT_RF")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VR_ANA")
				(number "2")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VR_DIG")
				(number "4")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA_BOOST")
				(number "27")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VR_PA")
				(number "25")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "RFO_LF")
				(number "28")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RFI_LF")
				(number "1")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RFO_HF")
				(number "22")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "RFI_HF")
				(number "21")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RXTX/RF_MOD")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SX1278"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 24.13 0)
		)
		(property "Value" "SX1278"
			(at 13.97 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.8x4.8mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/2R0000001Rbr/6EfVZUorrpoKFfvaF_Fkpgp5kzjiNyiAbqcpqh9qSjE"
			(at 0 -5.08 0)
		)
		(property "Description" "137 MHz to 525 MHz Low Power Long Range Transceiver, spreading factor from 6 to 12, LoRA, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "low-power lora transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SX1278_0_1")
		(symbol "SX1278_1_1"
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "XTA")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "XTB")
				(number "6")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIO0")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIO1")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIO2")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIO3")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIO4")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DIO5")
				(number "13")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SCK")
				(number "16")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "MISO")
				(number "17")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "MOSI")
				(number "18")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "NSS")
				(number "19")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VBAT_ANA")
				(number "3")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VBAT_DIG")
				(number "14")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VBAT_RF")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VR_ANA")
				(number "2")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VR_DIG")
				(number "4")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA_BOOST")
				(number "27")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VR_PA")
				(number "25")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "RFO_LF")
				(number "28")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RFI_LF")
				(number "1")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RXTX/RF_MOD")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SYPD-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "SYPD-2"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_TTT167_LandPatternPL-079"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/SYPD-2.pdf"
			(at 5.08 -7.62 0)
		)
		(property "Description" "Phase Detector, 10 to 200 MHz, 50 Ohm, Mini-Cicuits TTT167"
			(at 0 0 0)
		)
		(property "ki_keywords" "phase detector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*TTT167*"
			(at 0 0 0)
		)
		(symbol "SYPD-2_0_1")
		(symbol "SYPD-2_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 5.08)
				(name "RF1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 0 -10.16 90)
				(length 5.08)
				(name "DC")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 5.08)
				(name "RF2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si4460"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "Si4460"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias"
			(at 0 30.48 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si4464-63-61-60.pdf"
			(at -7.62 -2.54 0)
		)
		(property "Description" "High-Performance, Low-Current Sub-GHz Transceiver, +13dBm, Major bands 142-1050 MHz, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver sub-ghz radio ism"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "Si4460_0_1")
		(symbol "Si4460_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SDN")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "XIN")
				(number "17")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "XOUT")
				(number "16")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SDI")
				(number "14")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SDO")
				(number "13")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "~{SEL}")
				(number "15")
			)
			(pin open_collector line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "TX")
				(number "4")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "TXRAMP")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "RXp")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "RXn")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GPIO0")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GPIO1")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GPIO2")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "GPIO3")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCP-2-10X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "TCP-2-10X"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_DB1627"
			(at -3.81 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/TCP-2-10X+.pdf"
			(at -1.27 -8.89 0)
		)
		(property "Description" "Power splitter combiner, 5 to 1000 MHz, 2 way 0-degree, 50 ohm, Mini-Circuits DB1627"
			(at 0 0 0)
		)
		(property "ki_keywords" "splitter combiner"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*DB1627*"
			(at 0 0 0)
		)
		(symbol "TCP-2-10X_0_1")
		(symbol "TCP-2-10X_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 3.81)
				(hide yes)
				(name "CON")
				(number "2")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "CON")
				(number "5")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 5.08)
				(name "SUM")
				(number "6")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 5.08)
				(name "PORT1")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 5.08)
				(name "PORT2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "F113"
		(extends "F115")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "F113"
			(at -8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2205181716_Synoxo-F115_C3010244.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Synoxo 300-450MHz ASK/OOK Transmitter, +10dBm, 10kbps, 1.8-3.6V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synoxo SYN113 RF Transmitter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT-23-6*"
			(at 0 0 0)
		)
	)
	(symbol "F117"
		(extends "F115")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "F117"
			(at -8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2205181716_Synoxo-F115_C3010244.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Synoxo 300-450MHz ASK/OOK Transmitter, +13dBm, 10kbps, Sleep/Wake Function, 1.8-3.6V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synoxo SYN117 RF Transmitter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT-23-6*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-10DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-10DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 10dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-1DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-1DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 1dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-2DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-2DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 2dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-3DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-3DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 3dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-4DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-4DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 4dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-5DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-5DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 5dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-6DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-6DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 6dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-7DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-7DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 7dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-8DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-8DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 8dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "PAT1220-C-9DB"
		(extends "PAT1220-C-0DB")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PAT1220-C-9DB"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "RF_Converter:RF_Attenuator_Susumu_PAT1220"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.susumu.co.jp/common/pdf/n_catalog_partition16_en.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "10GHz RF Attenuator, 50ohm Matched Impedance, 9dB Attenuation, PAT1220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF attenuator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Attenuator*Susumu*PAT1220*"
			(at 0 0 0)
		)
	)
	(symbol "SX1261IMLTRT"
		(extends "SX1262IMLTRT")
		(property "Reference" "U"
			(at 13.97 24.13 0)
		)
		(property "Value" "SX1261IMLTRT"
			(at 13.97 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 1.27 -31.75 0)
		)
		(property "Datasheet" "https://semtech.file.force.com/sfc/dist/version/download/?oid=00DE0000000JelG&ids=0682R00000IjPWSQA3&d=%2Fa%2F2R000000Un7F%2FyT.fKdAr9ZAo3cJLc4F2cBdUsMftpT2vsOICP7NmvMo"
			(at 1.27 -29.21 0)
		)
		(property "Description" "150 MHz to 960 MHz Low Power Long Range Transceiver, 14dBm output power, spreading factor from 5 to 12, LoRA, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "low-power lora transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SX1273"
		(extends "SX1272")
		(property "Reference" "U"
			(at 13.97 24.13 0)
		)
		(property "Value" "SX1273"
			(at 13.97 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.8x4.8mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/440000001NCE/v_VBhk1IolDgxwwnOpcS_vTFxPfSEPQbuneK3mWsXlU"
			(at 0 -5.08 0)
		)
		(property "Description" "860 MHz to 1020 MHz Low Power Long Range Transceiver, spreading factor from 6 to 9, LoRA, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "low-power lora transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SX1277"
		(extends "SX1276")
		(property "Reference" "U"
			(at 13.97 24.13 0)
		)
		(property "Value" "SX1277"
			(at 13.97 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.8x4.8mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/2R0000001Rbr/6EfVZUorrpoKFfvaF_Fkpgp5kzjiNyiAbqcpqh9qSjE"
			(at 0 -5.08 0)
		)
		(property "Description" "137 MHz to 525 MHz Low Power Long Range Transceiver, spreading factor from 6 to 12, LoRA, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "low-power lora transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SX1279"
		(extends "SX1276")
		(property "Reference" "U"
			(at 13.97 24.13 0)
		)
		(property "Value" "SX1279"
			(at 13.97 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.8x4.8mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/2R0000001Rbr/6EfVZUorrpoKFfvaF_Fkpgp5kzjiNyiAbqcpqh9qSjE"
			(at 0 -5.08 0)
		)
		(property "Description" "137 MHz to 960 MHz Low Power Long Range Transceiver, spreading factor from 6 to 12, LoRA, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "low-power lora transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SYPD-1"
		(extends "SYPD-2")
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "SYPD-1"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_TTT167_LandPatternPL-079"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/SYPD-1+.pdf"
			(at 5.08 -7.62 0)
		)
		(property "Description" "Phase Detector, 1 to 100 MHz, 50 Ohm, Mini-Cicuits TTT167"
			(at 0 0 0)
		)
		(property "ki_keywords" "Phase Detector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*TTT167*"
			(at 0 0 0)
		)
	)
	(symbol "SYPD-52"
		(extends "SYPD-2")
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "SYPD-52"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_TTT167_LandPatternPL-079"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/SYPD-52+.pdf"
			(at 5.08 -7.62 0)
		)
		(property "Description" "Phase Detector, 400 to 500 MHz, 50 Ohm, Mini-Cicuits TTT167"
			(at 0 0 0)
		)
		(property "ki_keywords" "Phase Detector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*TTT167*"
			(at 0 0 0)
		)
	)
	(symbol "Si4461"
		(extends "Si4460")
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "Si4461"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias"
			(at 0 30.48 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si4464-63-61-60.pdf"
			(at -7.62 -2.54 0)
		)
		(property "Description" "High-Performance, Low-Current Sub-GHz Transceiver, +16dBm, Major bands 142-1050 MHz, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver sub-ghz radio ism"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si4463"
		(extends "Si4460")
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "Si4463"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias"
			(at 0 30.48 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si4464-63-61-60.pdf"
			(at -7.62 -2.54 0)
		)
		(property "Description" "High-Performance, Low-Current Sub-GHz Transceiver, +20dBm, Major bands 142-1050 MHz, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver sub-ghz radio ism"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si4464"
		(extends "Si4460")
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "Si4464"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias"
			(at 0 30.48 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si4464-63-61-60.pdf"
			(at -7.62 -2.54 0)
		)
		(property "Description" "High-Performance, Low-Current Sub-GHz Transceiver, +20dBm, Banded 119-960 MHz, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver sub-ghz radio ism"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "nRF24L01P"
		(extends "NRF24L01")
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "nRF24L01P"
			(at 5.08 17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 5.08 20.32 0)
		)
		(property "Datasheet" "http://www.nordicsemi.com/eng/content/download/2726/34069/file/nRF24L01P_Product_Specification_1_0.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "nRF24L01+, Ultra low power 2.4GHz RF Transceiver, QFN20 4x4mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power RF Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4*0.5mm*"
			(at 0 0 0)
		)
	)
)
