(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "LA1185"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 12.7 0)
		)
		(property "Value" "LA1185"
			(at -7.62 -12.7 0)
		)
		(property "Footprint" "Package_SIP:SIP-9_22.3x3mm_P2.54mm"
			(at 22.86 -12.7 0)
		)
		(property "Datasheet" "https://www.alldatasheet.com/datasheet-pdf/pdf/39974/SANYO/LA1185.html"
			(at 0 5.08 0)
		)
		(property "Description" "FM receiver front-end IC for radio-cassette recorder, music center applications, SIP-9"
			(at 0 0 0)
		)
		(property "ki_keywords" "FM mixer receiver amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP*22.3x3mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "LA1185_0_1")
		(symbol "LA1185_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RF_IN")
				(number "1")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RF_BYPASS")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "MIX_IN")
				(number "4")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OSC_MON")
				(number "7")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OSC")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RF_OUT")
				(number "3")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "MIX_OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCS3142"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 22.86 0)
		)
		(property "Value" "MCS3142"
			(at -5.08 20.32 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 3.81 -17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001747A.pdf"
			(at 3.81 -16.51 0)
		)
		(property "Description" "Microchip KEELOQ classic / ultimate encoder - keyfob IC sending button state, serial and authentiation as PWM/manchester encoded AM/FM signal in ISM bands"
			(at 0 0 0)
		)
		(property "ki_keywords" "KEELOQ classic ultimate keyless entry keyfob ISM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm?P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCS3142_0_1")
		(symbol "MCS3142_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "SW0")
				(number "19")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "SW1")
				(number "18")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "SW2")
				(number "17")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "SW3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "PGD")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "PGC")
				(number "5")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "SOSCO")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "SOSCI")
				(number "2")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "XTAL")
				(number "13")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "11")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "7")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "~{LED}")
				(number "16")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "RF_OUT")
				(number "10")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "CTRL_OUT")
				(number "14")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "CTRL_IN")
				(number "9")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "DATA_OUT")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "DATA_IN")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SA605D"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.606 24.13 0)
		)
		(property "Value" "SA605D"
			(at 12.954 24.13 0)
		)
		(property "Footprint" "Package_SO:SO-20_12.8x7.5mm_P1.27mm"
			(at 22.86 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SA605.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "High performance monolithic low-power FM IF system, SO-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "High performance monolithic low-power FM IF system"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*12.8x7.5mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SA605D_0_0"
			(text "MIX"
				(at -6.35 17.907 0)
			)
			(text "MUTE"
				(at -1.397 -34.29 0)
			)
			(text "Switch"
				(at -1.397 -36.322 0)
			)
			(text "IF"
				(at -1.27 -0.635 0)
			)
			(text "amp"
				(at -1.27 -1.524 0)
			)
			(text "Lim"
				(at -1.27 -16.51 0)
			)
			(text "QUAD"
				(at -1.27 -24.13 0)
			)
			(text "Detect"
				(at -1.27 -25.781 0)
			)
			(text "OSC"
				(at 3.175 12.065 0)
			)
			(text "RSSI"
				(at 7.62 -12.7 0)
			)
		)
		(symbol "SA605D_0_1")
		(symbol "SA605D_1_1"
			(pin input line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "RF_IN")
				(number "1")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "RF_BYPASS")
				(number "2")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "IF_AMP_DECOUPL")
				(number "19")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "IF_AMP_IN")
				(number "18")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "IF_AMP_DECOUPL")
				(number "17")
			)
			(pin input line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "LIMITER_IN")
				(number "14")
			)
			(pin input line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "LIMITER_DECOUPL")
				(number "13")
			)
			(pin input line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "LIMITER_DECOUPL")
				(number "12")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "QUADRATURE_IN")
				(number "10")
			)
			(pin input line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "MUTE_INPUT")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "MIXER_OUT")
				(number "20")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "OSC_OUT")
				(number "3")
			)
			(pin input line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "OSC_IN")
				(number "4")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "IF_AMP_OUT")
				(number "16")
			)
			(pin output line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "RSSI_OUT")
				(number "7")
			)
			(pin output line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "LIMITER_OUT")
				(number "11")
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "UNMUTED_AUD_OUTP")
				(number "9")
			)
			(pin output line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "MUTED_AUD_OUTP")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SA636DK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 31.75 0)
		)
		(property "Value" "SA636DK"
			(at 13.97 31.75 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SA636.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-voltage, high performance, monolithic FM IF system with high-speed RSSI, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low-voltage, monolithic, FM, IF, RSSI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SA636DK_0_0"
			(text "E"
				(at -11.43 10.16 0)
			)
			(text "B"
				(at -11.43 5.08 0)
			)
			(text "OSC"
				(at -7.62 7.62 0)
			)
			(text "+"
				(at -6.985 -24.13 0)
			)
			(text "RSSI"
				(at -1.27 -2.54 0)
			)
		)
		(symbol "SA636DK_0_1")
		(symbol "SA636DK_1_0")
		(symbol "SA636DK_1_1"
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "RF_IN")
				(number "1")
			)
			(pin passive line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "RF_IN_DECOUPL")
				(number "2")
			)
			(pin output line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "OSC_OUT")
				(number "3")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "OSC_IN")
				(number "4")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "RSSI_FEEDBACK")
				(number "6")
			)
			(pin output line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "RSSI_OUT")
				(number "7")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "POWER_DOWN_CTRL")
				(number "8")
			)
			(pin output line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "DATA_OUT")
				(number "9")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "QUADRATURE_IN")
				(number "10")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "MIXER_OUT")
				(number "20")
			)
			(pin passive line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "IF_AMP_DECOUPL")
				(number "19")
			)
			(pin input line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "IF_AMP_IN")
				(number "18")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "IF_AMP_DECOUPL")
				(number "17")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "IF_AMP_OUT")
				(number "16")
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "LIMITER_IN")
				(number "14")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "LIMITER_DECOUPL")
				(number "13")
			)
			(pin passive line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "LIMITER_DECOUPL")
				(number "12")
			)
			(pin output line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "LIMITER_OUT")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si4362"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 19.685 0)
		)
		(property "Value" "Si4362"
			(at -5.08 17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 8.89 -17.78 0)
		)
		(property "Datasheet" "http://www.silabs.com/Support%20Documents/TechnicalDocs/Si4362.pdf"
			(at 1.27 -25.4 0)
		)
		(property "Description" "EZRadioPRO Low Current Receiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "radio receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "Si4362_0_1")
		(symbol "Si4362_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "SDN")
				(number "1")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "RXp")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "RXn")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "XIN")
				(number "17")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "XOUT")
				(number "16")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "18")
			)
			(pin no_connect line
				(at 2.54 -16.51 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 -16.51 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 -16.51 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "GPIO0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "GPIO1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "GPIO2")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "GPIO3")
				(number "20")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "~{SEL}")
				(number "15")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "SDI")
				(number "14")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "SDO")
				(number "13")
			)
			(pin input clock
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "SCLK")
				(number "12")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "~{IRQ}")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si4735-D60-GU"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 19.685 0)
		)
		(property "Value" "Si4735-D60-GU"
			(at -5.08 17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 6.35 -17.78 0)
		)
		(property "Datasheet" "http://www.silabs.com/Support%20Documents/TechnicalDocs/Si4730-31-34-35-D60.pdf"
			(at 1.27 -25.4 0)
		)
		(property "Description" "AM/FM/SW/LW Broadcast Radio Receiver with RDS/RBDS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Broadcast AM FM SW LW Radio Receiver RDS RBDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "Si4735-D60-GU_0_1")
		(symbol "Si4735-D60-GU_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "~{RST}")
				(number "15")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "~{SEN}")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "SDIO")
				(number "18")
			)
			(pin input clock
				(at -15.24 2.54 0)
				(length 3.81)
				(name "SCLK")
				(number "17")
			)
			(pin input clock
				(at -15.24 0 0)
				(length 3.81)
				(name "RCLK")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "GPO3/[DCLK]")
				(number "3")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "GPO2/[~{INT}]")
				(number "4")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "GPO1")
				(number "5")
			)
			(pin no_connect line
				(at -11.43 -12.7 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 -16.51 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "VD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "VA")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin no_connect line
				(at 5.08 -16.51 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 11.43 -12.7 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "DBYP")
				(number "22")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "DOUT")
				(number "1")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "ROUT/[DOUT]")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "LOUT/[DFS]")
				(number "24")
			)
			(pin input line
				(at 15.24 0 180)
				(length 3.81)
				(name "DFS")
				(number "2")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "AMI")
				(number "12")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "FMI")
				(number "8")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "RFGND")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZETA-433-SO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "ZETA-433-SO"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at -8.89 6.35 0)
		)
		(property "Datasheet" "https://www.rfsolutions.co.uk/downloads/1456219226DS-ZETA.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "FM ZETA TRANSCEIVER MODULE, OPTIMISED FOR 433MHZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF TRANSCEIVER MODULE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZETA?433?SO?SMD* ZETA?433?SO?THT*"
			(at 0 0 0)
		)
		(symbol "ZETA-433-SO_0_1")
		(symbol "ZETA-433-SO_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ANT")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDN")
				(number "3")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SEL")
				(number "12")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDO")
				(number "11")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDI")
				(number "10")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GPIO1")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SA605DK"
		(extends "SA605D")
		(property "Reference" "U"
			(at -22.606 24.13 0)
		)
		(property "Value" "SA605DK"
			(at 12.954 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_4.4x6.5mm_P0.65mm"
			(at 24.13 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SA605.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "High performance monolithic low-power FM IF system, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "High performance monolithic low-power FM IF system"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si4730-D60-GU"
		(extends "Si4735-D60-GU")
		(property "Reference" "U"
			(at -5.08 19.685 0)
		)
		(property "Value" "Si4730-D60-GU"
			(at -5.08 17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 6.35 -17.78 0)
		)
		(property "Datasheet" "http://www.silabs.com/Support%20Documents/TechnicalDocs/Si4730-31-34-35-D60.pdf"
			(at 1.27 -25.4 0)
		)
		(property "Description" "AM/FM Broadcast Radio Receiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "Broadcast AM FM Radio Receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si4731-D60-GU"
		(extends "Si4735-D60-GU")
		(property "Reference" "U"
			(at -5.08 19.685 0)
		)
		(property "Value" "Si4731-D60-GU"
			(at -5.08 17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 6.35 -17.78 0)
		)
		(property "Datasheet" "http://www.silabs.com/Support%20Documents/TechnicalDocs/Si4730-31-34-35-D60.pdf"
			(at 1.27 -25.4 0)
		)
		(property "Description" "AM/FM Broadcast Radio Receiver with RDS/RBDS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Broadcast AM FM Radio Receiver RDS RBDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si4734-D60-GU"
		(extends "Si4735-D60-GU")
		(property "Reference" "U"
			(at -5.08 19.685 0)
		)
		(property "Value" "Si4734-D60-GU"
			(at -5.08 17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 6.35 -17.78 0)
		)
		(property "Datasheet" "http://www.silabs.com/Support%20Documents/TechnicalDocs/Si4730-31-34-35-D60.pdf"
			(at 1.27 -25.4 0)
		)
		(property "Description" "AM/FM/SW/LW Broadcast Radio Receiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "Broadcast AM FM SW LW Radio Receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ZETA-868-SO"
		(extends "ZETA-433-SO")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "ZETA-868-SO"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at -8.89 6.35 0)
		)
		(property "Datasheet" "https://www.rfsolutions.co.uk/downloads/1456219226DS-ZETA.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "FM ZETA TRANSCEIVER MODULE, OPTIMISED FOR 868MHZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF TRANSCEIVER MODULE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZETA?433?SO?SMD* ZETA?433?SO?THT*"
			(at 0 0 0)
		)
	)
	(symbol "ZETA-915-SO"
		(extends "ZETA-433-SO")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "ZETA-915-SO"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at -8.89 6.35 0)
		)
		(property "Datasheet" "https://www.rfsolutions.co.uk/downloads/1456219226DS-ZETA.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "FM ZETA TRANSCEIVER MODULE, OPTIMISED FOR 915MHZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF TRANSCEIVER MODULE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZETA?433?SO?SMD* ZETA?433?SO?THT*"
			(at 0 0 0)
		)
	)
)
