(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD8313xRM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "AD8313xRM"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8313.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "100 MHz to 2.5 GHz, 80 dB Logarithmic Detector / Controller, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF LOG POWER DETECTOR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD8313xRM_0_1")
		(symbol "AD8313xRM_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "INHI")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INLO")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PWDN")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VPOS")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COMM")
				(number "6")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VPOS")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "8")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSET")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADL5542"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADL5542"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_CSP:Analog_LFCSP-8-1EP_3x3mm_P0.5mm_EP1.53x1.85mm"
			(at 3.81 11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADL5542.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-6000MHz RF/IF +20dB gain block, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*LFCSP*1EP*3x3mm*P0.5mm*EP1.53x1.85mm*"
			(at 0 0 0)
		)
		(symbol "ADL5542_0_1")
		(symbol "ADL5542_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "CB")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BGA2866"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2866"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2866.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +24.3dB @ 2150MHz, 5V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
		(symbol "BGA2866_0_1")
		(symbol "BGA2866_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "Vcc")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "G")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CMX901"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "CMX901"
			(at 10.16 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm_ThermalVias"
			(at -2.54 20.32 0)
		)
		(property "Datasheet" "https://www.cmlmicro.com/wp-content/uploads/2017/10/CMX901_ds.pdf"
			(at -2.54 22.86 0)
		)
		(property "Description" "Broadband Efficient RF Power Amplifier"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF POWER AMPLIFIER BROADBAND"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*28*1EP*5x5mm*P0.5mm*EP3.35x3.35mm*"
			(at 0 0 0)
		)
		(symbol "CMX901_0_0"
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
		)
		(symbol "CMX901_0_1")
		(symbol "CMX901_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "RFIN")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(hide yes)
				(name "RFIN")
				(number "5")
			)
			(pin input line
				(at -7.62 -10.16 90)
				(length 2.54)
				(name "VGS1")
				(number "8")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "VGS2")
				(number "28")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD2")
				(number "26")
			)
			(pin input line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "VGS3")
				(number "24")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VA")
				(number "14")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "RFOUT")
				(number "16")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "RFOUT")
				(number "17")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "RFOUT")
				(number "18")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "RFOUT")
				(number "19")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "RFOUT")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HMC1099PM5E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "HMC1099PM5E"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/HMC1099PM5E.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "10 W (40 dBm), 0.01 GHz to 1.1 GHz, GaN Power Amplifier, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "HMC1099PM5E_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX2679"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "MAX2679"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_BGA:WLP-4_0.83x0.83mm_P0.4mm"
			(at -2.54 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX2679-MAX2679B.pdf"
			(at 0 0 0)
		)
		(property "Description" "GPS/GNSS Ultra-Low Current Low-Noise Amplifier, +19dB @ 1.57GHz, WLP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLP*0.83x0.83mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX2679_0_1")
		(symbol "MAX2679_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "Vcc")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "G")
				(number "B2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MMZ09332BT1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 13.97 0)
		)
		(property "Value" "MMZ09332BT1"
			(at 8.89 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.5mm_EP1.6x1.6mm_ThermalVias"
			(at -10.16 24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MMZ09332B.pdf"
			(at -10.16 20.32 0)
		)
		(property "Description" "High Efficiency/Linearity Amplifier high linearity broadband amplifier, QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MMZ09332BT1_0_1")
		(symbol "MMZ09332BT1_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VBA2")
				(number "12")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VBA1")
				(number "1")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "RF_IN")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "POWER_DOWN")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VBIAS")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCC1")
				(number "11")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VCC2/RFOUT")
				(number "9")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VCC2/RFOUT")
				(number "8")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VCC2/RFOUT")
				(number "7")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PDET")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "QPL9547"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.16 0)
		)
		(property "Value" "QPL9547"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.6mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.qorvo.com/products/d/da007268"
			(at -1.27 0 0)
		)
		(property "Description" "100-6000MHz RF/IF +19.5dB gain block, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "QPL9547_0_1")
		(symbol "QPL9547_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "Vb")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~{EN}")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SGL0622Z"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "SGL0622Z"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.6x1.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.qorvo.com/products/d/da001879"
			(at 0 0 0)
		)
		(property "Description" "5 MHz to 4000 MHz, Low-Noise SiGe HBT MMIC Amplifier, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "rf gain block"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SGL0622Z_0_0"
			(pin passive line
				(at -2.54 -7.62 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "9")
			)
		)
		(symbol "SGL0622Z_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SKY65404"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 2.54 0)
		)
		(property "Value" "SKY65404"
			(at 10.16 -2.54 0)
		)
		(property "Footprint" "RF:Skyworks_SKY65404-31"
			(at 3.81 0 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/SKY65404_31_201512K.pdf"
			(at 6.35 2.54 0)
		)
		(property "Description" "4.9-5.9GHz, 13dB Low-Noise Amplifier, QFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LNA low noise amplifier RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Skyworks*SKY65404*"
			(at 0 0 0)
		)
		(symbol "SKY65404_0_1")
		(symbol "SKY65404_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "RFIN")
				(number "3")
			)
			(pin input line
				(at 0 7.62 270)
				(length 3.81)
				(name "VENABLE")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 1.27)
				(name "EP")
				(number "7")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 5.08)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RFOUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPF5189Z"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "SPF5189Z"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "www.qorvo.com/products/d/da001910"
			(at 0 0 0)
		)
		(property "Description" "50MHz to 4000MHz, GaAs pHEMT low noise MMIC amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "SPF5189Z_0_1")
		(symbol "SPF5189Z_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TRF37A73"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 2.54 0)
		)
		(property "Value" "TRF37A73"
			(at 11.43 -2.54 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/trf37a73.pdf"
			(at 12.7 -10.16 0)
		)
		(property "Description" "6GHz, 12dB RF Gain Block, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "gain block RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TRF37A73_1_1"
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "RFIN")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 3.81)
				(name "PWDN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 5.08)
				(name "VCC")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RFOUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADL5541"
		(extends "ADL5542")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "ADL5541"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_CSP:Analog_LFCSP-8-1EP_3x3mm_P0.5mm_EP1.53x1.85mm"
			(at 3.81 11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADL5541.pdf"
			(at 0 0 0)
		)
		(property "Description" "20-6000MHz RF/IF +15dB gain block, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*LFCSP*1EP*3x3mm*P0.5mm*EP1.53x1.85mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADL5610"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "ADL5610"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADL5610.pdf"
			(at 0 0 0)
		)
		(property "Description" "30-6000MHz RF/IF +18.4dB gain block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2800"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2800"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2800.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +20.2dB @ 2150MHz, 3.3V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2801"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2801"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2801.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +23dB @ 2120MHz, 3.3V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2803"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2803"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2803.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +23.6dB @ 950MHz, 3V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2815"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2815"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2815.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +24.7dB @ 2150MHz, 3.3V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2817"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2817"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2817.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +24.4dB @ 2150MHz, 3.3V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2818"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2818"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2818.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +30dB @ 2150MHz, 3.3V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2850"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2850"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2850.pdf"
			(at 0 0 0)
		)
		(property "Description" "MIC wideband amplifier, DC-2.2GHz, +24dB @ 950MHz, 5V, SOT-363-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2851"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2851"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2851.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +24.8dB @ 950MHz, 5V, SOT-363-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2865"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2865"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2865.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +32.2dB @ 950MHz, 5V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2867"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2867"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2867.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +26.4dB @ 2150MHz, 5V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2869"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2869"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2869.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +31.7dB @ 950MHz, 5V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2870"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2870"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2870.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +31.1dB @ 500MHz, 2.5V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "BGA2874"
		(extends "BGA2866")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "BGA2874"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BGA2874.pdf"
			(at 0 0 0)
		)
		(property "Description" "MMIC wideband amplifier, DC-2.2GHz, +31dB @ 750MHz, 2.5V, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-1"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-1"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-1+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-8000MHz +11.8dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-19"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-19"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-19+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-7000MHz +11.6dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-2"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-2"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-2+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-8000MHz +14.8dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-21"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-21"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-21+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-8000MHz +13.1dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-24"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-24"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-24+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-6000MHz +16.6dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-29"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-29"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-29+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-7000MHz +19.7dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-3"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-3"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-3+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-3000MHz +19.1dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-33"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-33"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-33+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +17.5dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-39"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-39"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-39+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-7000MHz +19.7dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-4"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-4"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-4+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +13.5dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-49"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-49"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-49+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-5000MHz +13.6dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-4F"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-4F"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-4F+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +13.4dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-5"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-5"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-5+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +17.5dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-51"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-51"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-51+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +16.1dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-51F"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-51F"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-51F+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +15.9dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-52"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-52"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-52+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-2000MHz +17.8dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-55"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-55"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-55+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +18.5dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-59"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-59"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-59+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-5000MHz +18.3dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-5F"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-5F"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-5F+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +17.4dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-6"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-6"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-6+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +11.3dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-6F"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-6F"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-6F+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-4000MHz +11.6dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-74"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-74"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-74+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-1000MHz +21.8dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-84"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-84"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-84+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-6000MHz +16.7dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GALI-S66"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GALI-S66"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GALI-S66+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-3000MHz +18.2dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GVA-123"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GVA-123"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GVA-123+.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-12000MHz +16.9dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GVA-60"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GVA-60"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GVA-60+.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-5000MHz +19.8dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GVA-62"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GVA-62"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GVA-62+.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-6000MHz +15.4dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GVA-63"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GVA-63"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GVA-63+.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-6000MHz +20dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GVA-81"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GVA-81"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GVA-81+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-6000MHz +10dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GVA-82"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GVA-82"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GVA-82+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-7000MHz +13.8dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GVA-83"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GVA-83"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GVA-83+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-7000MHz +17.1dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GVA-84"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GVA-84"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GVA-84+.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC-7000MHz +16dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "GVA-93"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "GVA-93"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/GVA-93+.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-9000MHz +16.9dB Gain Block, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "HMC8500PM5E"
		(extends "HMC1099PM5E")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "HMC8500PM5E"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/HMC8500PM5E.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "10 W (40 dBm), 0.01 GHz to 2.8 GHz, GaN Power Amplifier, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX2679B"
		(extends "MAX2679")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "MAX2679B"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "Package_BGA:WLP-4_0.83x0.83mm_P0.4mm"
			(at -2.54 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX2679-MAX2679B.pdf"
			(at 0 0 0)
		)
		(property "Description" "GPS/GNSS Ultra-Low Current Low-Noise Amplifier, +16.5dB @ 1.57GHz, WLP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF GAIN BLOCK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLP*0.83x0.83mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "PGA-102"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PGA-102"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-102+.pdf"
			(at 0 0 0)
		)
		(property "Description" "50-6000MHz +15.9dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PGA-1021"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PGA-1021"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-1021+.pdf"
			(at 0 0 0)
		)
		(property "Description" "50-6000MHz +15.1dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PGA-103"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PGA-103"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-103+.pdf"
			(at 0 0 0)
		)
		(property "Description" "50-4000MHz +11dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PGA-105"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PGA-105"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-105+.pdf"
			(at 0 0 0)
		)
		(property "Description" "40-2600MHz +15.1dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PGA-106-75"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PGA-106-75"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-106-75+.pdf"
			(at 0 0 0)
		)
		(property "Description" "50-1500MHz +16.9dB CATV Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PGA-106R-75"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PGA-106R-75"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-106R-75+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5-250MHz +17.9dB CATV Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PGA-122-75"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PGA-122-75"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-122-75+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5-1500MHz +15.5dB CATV Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PGA-32-75"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PGA-32-75"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-32-75+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5-300MHz +15.6dB CATV Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PHA-1"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PHA-1"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PHA-1+.pdf"
			(at 0 0 0)
		)
		(property "Description" "50-6000MHz +13.5dB Linear Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PHA-101"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PHA-101"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PHA-101+.pdf"
			(at 0 0 0)
		)
		(property "Description" "50-1500MHz +15.2dB Linear Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PHA-13HLN"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PHA-13HLN"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PHA-13HLN+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-1000MHz +22.7dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PHA-13LN"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PHA-13LN"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PHA-13LN+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-1000MHz +22.4dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PHA-1H"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PHA-1H"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PHA-1H+.pdf"
			(at 0 0 0)
		)
		(property "Description" "50-6000MHz +13.8dB Linear Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PHA-23HLN"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PHA-23HLN"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PHA-23HLN+.pdf"
			(at 0 0 0)
		)
		(property "Description" "30-2000MHz +21.3dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "PHA-23LN"
		(extends "SPF5189Z")
		(property "Reference" "U"
			(at -1.27 7.62 0)
		)
		(property "Value" "PHA-23LN"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PHA-23LN+.pdf"
			(at 0 0 0)
		)
		(property "Description" "30-2000MHz +21dB Low Noise Amplifier, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF amplifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
)
