(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "BL652"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "BL652"
			(at 0 -1.27 0)
		)
		(property "Footprint" "RF_Module:Laird_BL652"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "http://cdn.lairdtech.com/home/brandworld/files/Datasheet%20-%20BL652.pdf"
			(at 0 -33.02 0)
		)
		(property "Description" "Bluetooth module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth Nordic nRF52"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Laird*BL652*"
			(at 0 0 0)
		)
		(symbol "BL652_0_1")
		(symbol "BL652_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "SIO_00")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "SIO_01")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "SIO_02/AIN0")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "SIO_03/AIN1")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "SIO_04/AIN2")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "SIO_05/AIN3")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "SIO_06")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "SIO_07")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "SIO_08")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "SIO_09/NFC1")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "SIO_10/NFC2")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "SIO_11")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "SIO_12")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "SIO_13")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "SIO_14")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "SIO_15")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "SIO_16")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "SIO_17")
				(number "30")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 5.08 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "SWDCLK")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "SWDIO")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "SIO_31/AIN7")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "SIO_30/AIN6")
				(number "33")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "SIO_29/AIN5")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "SIO_28/AIN4")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "SIO_27")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "SIO_26")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "SIO_25")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "SIO_24")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "SIO_23")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "SIO_22")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "SIO_21")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "SIO_20")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "SIO_19")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "SIO_18")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BM78SPPS5MC2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "BM78SPPS5MC2"
			(at 1.27 -29.21 0)
		)
		(property "Footprint" "RF_Module:BM78SPPS5XC2"
			(at 16.51 29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001380C.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bluetooth Dual-Mode, UART, Class 2"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth BLE BT GAP SPP SDP RFCOMM L2CAP GATT ATT SMP L2CAP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BM78SPPS5XC2*"
			(at 0 0 0)
		)
		(symbol "BM78SPPS5MC2_0_1")
		(symbol "BM78SPPS5MC2_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "SW_BTN")
				(number "5")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "WAKE_UP")
				(number "9")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "EAN")
				(number "20")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{RST}")
				(number "21")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "HCI_RXD")
				(number "22")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "HCI_TXD")
				(number "23")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "P2_0")
				(number "18")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P2_4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P3_1")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P3_2")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P3_3")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "P3_4")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "P3_6")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "P3_7")
				(number "29")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "BAT_IN")
				(number "4")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDD_IO")
				(number "7")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "LDO18_O")
				(number "8")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "LDO33_O")
				(number "6")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PMULDO_O")
				(number "10")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "LED1")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P0_0")
				(number "17")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P0_4")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P0_5")
				(number "16")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "SCL/P1_2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "SDA/P1_3")
				(number "14")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P1_5")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "P1_7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTM112"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 29.21 0)
		)
		(property "Value" "BTM112"
			(at -15.24 26.67 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sparkfun.com/datasheets/Wireless/Bluetooth/BTM112_wATcommands.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bluetooth SPP Module, UART, Class 2"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth BT SPP Module"
			(at 0 0 0)
		)
		(symbol "BTM112_0_1")
		(symbol "BTM112_1_1"
			(pin input line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "RESET")
				(number "6")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PCM_IN")
				(number "20")
			)
			(pin output line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PCM_OUT")
				(number "18")
			)
			(pin bidirectional clock
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PCM_CLK")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PCM_SYNC")
				(number "19")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "SPI_MISO")
				(number "7")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "SPI_MOSI")
				(number "10")
			)
			(pin input clock
				(at -20.32 0 0)
				(length 5.08)
				(name "SPI_CLK")
				(number "9")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "~{SPI_CSB}")
				(number "8")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "UART_RX")
				(number "14")
			)
			(pin output line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "UART_TX")
				(number "12")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "~{UART_RTS}")
				(number "13")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "~{UART_CTS}")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "USB_D+")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "USB_D-")
				(number "23")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "RF")
				(number "33")
			)
			(pin power_in line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "AIO0")
				(number "4")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "AIO1")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PIO0")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PIO1")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PIO2")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PIO3")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "BTN/PIO4")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PIO5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "CONN/PIO6")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "~{LINK}/PIO7")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PIO8")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PIO9")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "PIO10")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PIO11")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTM222"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 29.21 0)
		)
		(property "Value" "BTM222"
			(at -20.32 26.67 0)
		)
		(property "Footprint" ""
			(at -22.86 26.67 0)
		)
		(property "Datasheet" "https://www.tme.eu/de/Document/b90358c53cd65c9b10d2914f55812666/btm222_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bluetooth SPP Module, UART, Class 1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth BT SPP Module"
			(at 0 0 0)
		)
		(symbol "BTM222_0_1")
		(symbol "BTM222_1_1"
			(pin input line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "~{RESET}")
				(number "16")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PCM_IN")
				(number "23")
			)
			(pin output line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PCM_OUT")
				(number "24")
			)
			(pin bidirectional clock
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PCM_CLK")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PCM_SYNC")
				(number "22")
			)
			(pin output line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "SPI_MISO")
				(number "34")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "SPI_MOSI")
				(number "31")
			)
			(pin input clock
				(at -25.4 0 0)
				(length 5.08)
				(name "SPI_CLK")
				(number "33")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "~{SPI_CSB}")
				(number "32")
			)
			(pin input line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "UART_RX")
				(number "26")
			)
			(pin output line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "UART_TX")
				(number "27")
			)
			(pin output line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "UART_RTS")
				(number "28")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "UART_CTS")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "USB_D+")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "USB_D-")
				(number "21")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at -5.08 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 5.08)
				(name "PVCC")
				(number "2")
			)
			(pin power_in line
				(at 5.08 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "RF")
				(number "37")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "GND")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "AIO0/SLEEPCLK")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "AIO1")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PIO0/RXEN")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PIO1/TXEN")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PIO2/USB_PU/CLK_REQ_OUT")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PIO3/USB_WKUP/CLK_REQ_IN")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PIO4/USB_ON/BT_PRIOR")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PIO5/USB_DETACH/BT_ACT")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PIO6/CLK_REQ/WAN_ACT")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PIO7")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PIO8")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PIO9")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PIO10")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PIO11")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MOD-nRF8001"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "MOD-nRF8001"
			(at 7.62 -12.7 0)
		)
		(property "Footprint" "RF_Module:MOD-nRF8001"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.olimex.com/Products/Modules/RF/MOD-nRF8001/"
			(at 1.27 0 0)
		)
		(property "Description" "Bluetooth Low Energy module based on nRF8001 chipset"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth Low Energy nRF8001"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MOD?nRF8001*"
			(at 0 0 0)
		)
		(symbol "MOD-nRF8001_0_1")
		(symbol "MOD-nRF8001_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "RST")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "RXD")
				(number "4")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "TXD")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "3V3")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "ACTIVE")
				(number "11")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "RDYN")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 3.81)
				(name "MISO")
				(number "9")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "MOSI")
				(number "8")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "REQN")
				(number "7")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "SCK")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Microchip_BM83"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 39.37 0)
		)
		(property "Value" "Microchip_BM83"
			(at 5.08 -39.37 0)
		)
		(property "Footprint" "RF_Module:Microchip_BM83"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/WSG/ProductDocuments/DataSheets/70005402E.pdf"
			(at 0 -54.61 0)
		)
		(property "Description" "Microchip BM23 Bluetooth 5.0 Audio Stereo Module, dual-mode, Audio Profiles, 32x15mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "HFP HSP A2DP SPP AVRCP PBAP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip?BM83*"
			(at 0 0 0)
		)
		(symbol "Microchip_BM83_0_1")
		(symbol "Microchip_BM83_1_1"
			(pin input line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "~{RST}")
				(number "43")
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "DR1")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "RFS1")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "SCLK1")
				(number "3")
			)
			(pin output line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "DT1")
				(number "4")
			)
			(pin output line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "MCLK1")
				(number "5")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "MICP1")
				(number "14")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "MICN1")
				(number "13")
			)
			(pin passive line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "MICBIAS")
				(number "15")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "MICP2")
				(number "10")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "MICN2")
				(number "9")
			)
			(pin output line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "DMIC_CLK")
				(number "17")
			)
			(pin output line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "DMIC1_R")
				(number "18")
			)
			(pin output line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "DMIC1_L")
				(number "19")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "AIR")
				(number "11")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "AIL")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "DP")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "DM")
				(number "36")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PWR(MFB)")
				(number "26")
			)
			(pin input line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "SK1_AMB_DET")
				(number "27")
			)
			(pin input line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "SK2_KEY_AD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 5.08)
				(name "ADAP_IN")
				(number "22")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 5.08)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 5.08)
				(name "BAT_IN")
				(number "23")
			)
			(pin no_connect line
				(at 17.78 -33.02 180)
				(length 5.08)
				(hide yes)
				(name "VDD_IO")
				(number "25")
			)
			(pin output line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "AOHPR")
				(number "6")
			)
			(pin output line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "AOHPM")
				(number "7")
			)
			(pin output line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "AOHPL")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "P0_0/UART_TX_IND")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "P0_1")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "P0_2")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "P0_3")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "P0_5")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "P0_6")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "P0_7")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "P1_2/TDI_CPU/SCL")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "P1_3/TCK_CPU/SDA")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "P1_6/PWM1")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "P2_3")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "P2_6")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "P2_7")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "P3_2")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "P3_4/UART_RTS")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "P3_7/UART_CTS")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "P8_5/UART_TXD")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "P8_6/UART_RXD")
				(number "29")
			)
			(pin power_out line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "SYS_PWR")
				(number "24")
			)
			(pin input line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "LED1")
				(number "32")
			)
			(pin input line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "LED2")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RFD77101"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 35.56 0)
		)
		(property "Value" "RFD77101"
			(at -7.62 33.02 0)
		)
		(property "Footprint" "RF_Module:RFDigital_RFD77101"
			(at 16.51 31.75 0)
		)
		(property "Datasheet" "https://www.simblee.com/Simblee%20RFD77101%20Datasheet%20v1.0.pdf"
			(at 0 -38.1 0)
		)
		(property "Description" "Simblee Bluetooth Smart Module with ARM Cortex-M0 and integrated antenna"
			(at 0 0 0)
		)
		(property "ki_keywords" "Simblee ARM Cortex-M0 Bluetooth antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RFDigital*RFD77101*"
			(at 0 0 0)
		)
		(symbol "RFD77101_0_1")
		(symbol "RFD77101_1_1"
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "RESET/SWDIO")
				(number "8")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "FACTORY/SWDCLK")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "P0.00/AREF0")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "P0.01/AIN2")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "P0.02/AIN3")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "P0.03/AIN4")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "P0.04/AIN5")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "P0.05/AIN6")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "P0.06/AREF1/AIN7")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "P0.07")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "P0.08")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "P0.09")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "P0.10")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "P0.11")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "P0.12")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "P0.13")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "P0.14")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "P0.15")
				(number "15")
			)
			(pin power_in line
				(at -12.7 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at -7.62 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "43")
			)
			(pin power_in line
				(at 7.62 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "44")
			)
			(pin power_in line
				(at 10.16 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "45")
			)
			(pin no_connect line
				(at 15.24 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 15.24 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 15.24 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "P0.30")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "P0.29")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "P0.28")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "P0.25")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "P0.24")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "P0.23")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "P0.22")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "P0.21")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "P0.20")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "P0.19")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "P0.18")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "P0.17")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "P0.16")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RN42"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "RN42"
			(at 11.43 24.13 0)
		)
		(property "Footprint" "RF_Module:RN42"
			(at -1.27 21.59 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/rn-42-ds-v2.32r.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "Class 2 Bluetooth Module with on-board antenna"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RN42*"
			(at 0 0 0)
		)
		(symbol "RN42_0_1")
		(symbol "RN42_1_1"
			(pin power_in line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SPI_MOSI")
				(number "2")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "GPIO6")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "GPIO7")
				(number "4")
			)
			(pin input inverted
				(at -17.78 7.62 0)
				(length 2.54)
				(name "RESET")
				(number "5")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SPI_CLK")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PCM_CLK")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PCM_SYNC")
				(number "8")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PCM_IN")
				(number "9")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PCM_OUT")
				(number "10")
			)
			(pin power_in line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at -12.7 -22.86 90)
				(length 2.54)
				(name "SHIELD")
				(number "36")
			)
			(pin input line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "AIO1")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin bidirectional line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GPIO11")
				(number "34")
			)
			(pin bidirectional line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "GPIO10")
				(number "33")
			)
			(pin bidirectional line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "GPIO9")
				(number "32")
			)
			(pin output line
				(at 7.62 -22.86 90)
				(length 2.54)
				(name "GPIO8")
				(number "31")
			)
			(pin power_in line
				(at 10.16 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "28")
			)
			(pin input line
				(at 12.7 -22.86 90)
				(length 2.54)
				(name "AIO0")
				(number "30")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "SPI_MISO")
				(number "24")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SPI_CSB")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "GPIO4")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GPIO5")
				(number "21")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GPIO3")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "USB_D-")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "USB_D+")
				(number "17")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "UART_CTS")
				(number "16")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "UART_RTS")
				(number "15")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "UART_TX")
				(number "14")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "UART_RX")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RN42N"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "RN42N"
			(at 12.7 26.67 0)
		)
		(property "Footprint" "RF_Module:RN42N"
			(at -5.08 17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/rn-42-ds-v2.32r.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Class 2 Bluetooth Module without antenna"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RN42N*"
			(at 0 0 0)
		)
		(symbol "RN42N_0_1")
		(symbol "RN42N_1_1"
			(pin power_in line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SPI_MOSI")
				(number "2")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "GPIO6")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "GPIO7")
				(number "4")
			)
			(pin input inverted
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RESET")
				(number "5")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SPI_CLK")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PCM_CLK")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PCM_SYNC")
				(number "8")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PCM_IN")
				(number "9")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PCM_OUT")
				(number "10")
			)
			(pin power_in line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at -12.7 -25.4 90)
				(length 2.54)
				(name "SHIELD")
				(number "36")
			)
			(pin input line
				(at -5.08 -25.4 90)
				(length 2.54)
				(name "AIO1")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin bidirectional line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GPIO11")
				(number "34")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin bidirectional line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "GPIO10")
				(number "33")
			)
			(pin bidirectional line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "RF_ANT")
				(number "26")
			)
			(pin bidirectional line
				(at 5.08 -25.4 90)
				(length 2.54)
				(name "GPIO9")
				(number "32")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 2.54)
				(name "GND")
				(number "25")
			)
			(pin output line
				(at 7.62 -25.4 90)
				(length 2.54)
				(name "GPIO8")
				(number "31")
			)
			(pin power_in line
				(at 10.16 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "28")
			)
			(pin input line
				(at 12.7 -25.4 90)
				(length 2.54)
				(name "AIO0")
				(number "30")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SPI_MISO")
				(number "24")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SPI_CSB")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GPIO4")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GPIO5")
				(number "21")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "GPIO3")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "GPIO2")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "USB_D-")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "USB_D+")
				(number "17")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "UART_CTS")
				(number "16")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "UART_RTS")
				(number "15")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "UART_TX")
				(number "14")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "UART_RX")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RN4871"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "RN4871"
			(at 11.43 -15.24 0)
		)
		(property "Footprint" "RF_Module:Microchip_RN4871"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/50002489A.pdf"
			(at -12.7 13.97 0)
		)
		(property "Description" "Bluetooth Low Energy 4.2 Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth Low Energy 4.2 Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF*Module:Microchip*RN4871*"
			(at 0 0 0)
		)
		(symbol "RN4871_0_1")
		(symbol "RN4871_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "UART_RX")
				(number "7")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "UART_TX")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "P3_6")
				(number "9")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "RST")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "P0_0")
				(number "11")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "P2_0")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VBAT")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "BT_RF")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "P1_2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "P1_3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "P1_7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "P1_6")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "P0_2")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "P2_7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPBTLE-RF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 12.7 0)
		)
		(property "Value" "SPBTLE-RF"
			(at -13.97 10.16 0)
		)
		(property "Footprint" "RF_Module:ST_SPBTLE"
			(at 12.7 -13.97 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/spbtle-rf.pdf"
			(at -13.97 10.16 0)
		)
		(property "Description" "Very Low Power network processor module for BLE v4.1, Hub capabilities"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE bluetooth module low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*SPBTLE*"
			(at 0 0 0)
		)
		(symbol "SPBTLE-RF_0_1")
		(symbol "SPBTLE-RF_1_1"
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "~{BT_RESET}")
				(number "11")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "NC/EXT_LPCLK")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "NC/GPIO2")
				(number "2")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "NC/ANA_TEST")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "SPI_IRQ")
				(number "4")
			)
			(pin input clock
				(at 20.32 0 180)
				(length 3.81)
				(name "SPI_CLK")
				(number "7")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SPI_MISO")
				(number "8")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "SPI_MOSI")
				(number "9")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "SPI_~{CS}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF8001"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -1.27 0)
		)
		(property "Value" "nRF8001"
			(at 0 1.27 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.nordicsemi.com/eng/nordic/content_download/2981/38488/file/nRF8001_PS_v1.3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "BLE LE Connectivity IC, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE, bluetooth"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "nRF8001_0_1")
		(symbol "nRF8001_1_1"
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "DEC1")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "DEC2")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "XL2")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "XL1")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "ACTIVE")
				(number "6")
			)
			(pin output line
				(at -20.32 0 0)
				(length 3.81)
				(name "TXD")
				(number "7")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RXD")
				(number "10")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "SCK")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "REQN")
				(number "12")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "MOSI")
				(number "13")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "MISO")
				(number "14")
			)
			(pin power_in line
				(at -7.62 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "AVDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "AVDD")
				(number "26")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 3.81)
				(name "AVDD")
				(number "29")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 3.81)
				(name "EP")
				(number "33")
			)
			(pin no_connect line
				(at 15.24 -10.16 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "DCC")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "XC1")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "XC2")
				(number "27")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "IREF")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "ANT2")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "ANT1")
				(number "21")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "VDD_PA")
				(number "20")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RESET")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "RDYN")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BM78SPPS5NC2"
		(extends "BM78SPPS5MC2")
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "BM78SPPS5NC2"
			(at 1.27 -29.21 0)
		)
		(property "Footprint" "RF_Module:BM78SPPS5XC2"
			(at 16.51 29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001380C.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bluetooth Dual-Mode, UART, Class 2"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth BLE BT GAP SPP SDP RFCOMM L2CAP GATT ATT SMP L2CAP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BM78SPPS5XC2*"
			(at 0 0 0)
		)
	)
	(symbol "SPBTLE-RF0"
		(extends "SPBTLE-RF")
		(property "Reference" "U"
			(at -13.97 12.7 0)
		)
		(property "Value" "SPBTLE-RF0"
			(at -13.97 10.16 0)
		)
		(property "Footprint" "RF_Module:ST_SPBTLE"
			(at 12.7 -13.97 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/spbtle-rf0.pdf"
			(at -13.97 10.16 0)
		)
		(property "Description" "Very Low Power network processor module for BLE v4.1"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE bluetooth module low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*SPBTLE*"
			(at 0 0 0)
		)
	)
)
