(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "L70-R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "L70-R"
			(at 10.16 13.97 0)
		)
		(property "Footprint" "RF_GPS:Quectel_L70-R"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "https://www.quectel.com/product/gps-only-l70-r"
			(at 0 -30.48 0)
		)
		(property "Description" "Quectel GPS Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "quectel GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel*L70*R*"
			(at 0 0 0)
		)
		(symbol "L70-R_0_1")
		(symbol "L70-R_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ANTON")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RF_IN")
				(number "11")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RESERVED")
				(number "16")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RESERVED")
				(number "17")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RESERVED")
				(number "18")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_out line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC_RF")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_BCKP")
				(number "6")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TXD1")
				(number "2")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RXD1")
				(number "3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "STANDBY")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "1PPS")
				(number "4")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L80-R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "L80-R"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "RF_GPS:Quectel_L80-R"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.quectel.com/UploadImage/Downlad/Quectel_L80-R_Hardware_Design_V1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quectel GPS Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "quectel GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel*L80*R*"
			(at 0 0 0)
		)
		(symbol "L80-R_0_1")
		(symbol "L80-R_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RESERVED")
				(number "7")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "RESERVED")
				(number "8")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RESERVED")
				(number "11")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "V_BCKP")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TXD1")
				(number "2")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RXD1")
				(number "1")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "1PPS")
				(number "6")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LEA-M8F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 29.21 0)
		)
		(property "Value" "LEA-M8F"
			(at 13.97 29.21 0)
		)
		(property "Footprint" "RF_GPS:ublox_LEA"
			(at 10.16 -29.21 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/products/documents/LEA-M8F_DataSheet_%28UBX-14001772%29.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module LEA M8, VCC 3V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*LEA*"
			(at 0 0 0)
		)
		(symbol "LEA-M8F_0_1")
		(symbol "LEA-M8F_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "USB_DM")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "USB_DP")
				(number "26")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "TxD1/SPI_MISO")
				(number "3")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "RxD1/SPI_MOSI")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SDA2/~{SPI_CS}")
				(number "1")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SCL2/SPI_CLK")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SDA_DAC")
				(number "22")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "SCL_DAC")
				(number "23")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "FREQ_PHASE_IN1")
				(number "21")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "FREQ_PHASE_IN0")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "TIMEPULSE/TP2/~{SAFEBOOT}")
				(number "28")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "12")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "D_SEL")
				(number "5")
			)
			(pin power_in line
				(at -7.62 30.48 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "V_BCKP")
				(number "11")
			)
			(pin power_out line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VCC_OUT")
				(number "8")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD_USB")
				(number "24")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "V_ANT")
				(number "19")
			)
			(pin power_out line
				(at 7.62 30.48 270)
				(length 2.54)
				(name "VCC_RF")
				(number "18")
			)
			(pin no_connect line
				(at 15.24 2.54 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "20")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "16")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "REF_FREQ_OUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LEA-M8S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "LEA-M8S"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "RF_GPS:ublox_LEA"
			(at 10.16 -24.13 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/LEA-M8S-FW3_DataSheet_%28UBX-16010205%29.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "GNSS Module LEA M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*LEA*"
			(at 0 0 0)
		)
		(symbol "LEA-M8S_0_1")
		(symbol "LEA-M8S_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "USB_DM")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "USB_DP")
				(number "26")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "EXTINT1")
				(number "20")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "EXTINT0")
				(number "27")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "12")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "V_BCKP")
				(number "11")
			)
			(pin power_out line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VCC_OUT")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD_USB")
				(number "24")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "V_ANT")
				(number "19")
			)
			(pin power_out line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "VCC_RF")
				(number "18")
			)
			(pin no_connect line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "5")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "9")
			)
			(pin no_connect line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "21")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "22")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "23")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "16")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LEA-M8T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "LEA-M8T"
			(at 13.97 24.13 0)
		)
		(property "Footprint" "RF_GPS:ublox_LEA"
			(at 10.16 -24.13 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/documents/NEO-LEA-M8T-FW3_DataSheet_UBX-15025193.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module LEA M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*LEA*"
			(at 0 0 0)
		)
		(symbol "LEA-M8T_0_1")
		(symbol "LEA-M8T_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "USB_DM")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "USB_DP")
				(number "26")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "TXD/SPI_MISO")
				(number "3")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RXD/SPI_MOSI")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "SDA/~{SPI_CS}")
				(number "1")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SCL/SPI_CLK")
				(number "2")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "EXTINT1")
				(number "20")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "EXTINT0")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "TP2/~{SAFEBOOT}")
				(number "12")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "D_SEL")
				(number "5")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "V_BCKP")
				(number "11")
			)
			(pin power_out line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VCC_OUT")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD_USB")
				(number "24")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "V_ANT")
				(number "19")
			)
			(pin power_out line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "VCC_RF")
				(number "18")
			)
			(pin no_connect line
				(at 15.24 10.16 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "9")
			)
			(pin no_connect line
				(at 15.24 7.62 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "21")
			)
			(pin no_connect line
				(at 15.24 5.08 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "22")
			)
			(pin no_connect line
				(at 15.24 2.54 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "23")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "16")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX-8C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "MAX-8C"
			(at 11.43 16.51 0)
		)
		(property "Footprint" "RF_GPS:ublox_MAX"
			(at 10.16 -16.51 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/MAX-8_DataSheet_%28UBX-16000093%29.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module MAX M8, VCC 1.65V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*MAX*"
			(at 0 0 0)
		)
		(symbol "MAX-8C_0_1")
		(symbol "MAX-8C_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RXD")
				(number "3")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TXD")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SCL")
				(number "17")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "EXTINT")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "18")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCC_IO")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_BCKP")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_out line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VCC_RF")
				(number "14")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "LNA_EN")
				(number "13")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "11")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX-M10S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "MAX-M10S"
			(at 11.43 16.51 0)
		)
		(property "Footprint" "RF_GPS:ublox_MAX"
			(at 10.16 -16.51 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/MAX-M10S_DataSheet_UBX-20035208.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module MAX M10, VCC 1.65V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox?MAX*"
			(at 0 0 0)
		)
		(symbol "MAX-M10S_0_1")
		(symbol "MAX-M10S_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RXD")
				(number "3")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TXD")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SCL")
				(number "17")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "EXTINT")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "18")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "VIO_SEL")
				(number "15")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCC_IO")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_BCKP")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_out line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VCC_RF")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "LNA_EN")
				(number "13")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "11")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX-M8W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "MAX-M8W"
			(at 12.7 16.51 0)
		)
		(property "Footprint" "RF_GPS:ublox_MAX"
			(at 10.16 -16.51 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/MAX-M8-FW3_DataSheet_%28UBX-15031506%29.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module MAX M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*MAX*"
			(at 0 0 0)
		)
		(symbol "MAX-M8W_0_1")
		(symbol "MAX-M8W_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RXD")
				(number "3")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TXD")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SCL")
				(number "17")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "EXTINT")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "18")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCC_IO")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_BCKP")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "V_ANT")
				(number "15")
			)
			(pin power_out line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VCC_RF")
				(number "14")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "13")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "11")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NEO-M8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "NEO-M8M"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "RF_GPS:ublox_NEO"
			(at 10.16 -21.59 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/NEO-M8-FW3_DataSheet_UBX-15031086.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module NEO M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*NEO*"
			(at 0 0 0)
		)
		(symbol "NEO-M8M_0_1")
		(symbol "NEO-M8M_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "USB_DM")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "USB_DP")
				(number "6")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "TXD/SPI_MISO")
				(number "20")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RXD/SPI_MOSI")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "SDA/~{SPI_CS}")
				(number "18")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SCL/SPI_CLK")
				(number "19")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "EXTINT")
				(number "4")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "1")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "D_SEL")
				(number "2")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "V_BCKP")
				(number "22")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD_USB")
				(number "7")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin power_out line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VCC_RF")
				(number "9")
			)
			(pin no_connect line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "14")
			)
			(pin no_connect line
				(at 15.24 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "15")
			)
			(pin no_connect line
				(at 15.24 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "16")
			)
			(pin no_connect line
				(at 15.24 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "17")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "11")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NEO-M8N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "NEO-M8N"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "RF_GPS:ublox_NEO"
			(at 10.16 -21.59 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/NEO-M8-FW3_DataSheet_UBX-15031086.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module NEO M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*NEO*"
			(at 0 0 0)
		)
		(symbol "NEO-M8N_0_1")
		(symbol "NEO-M8N_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "USB_DM")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "USB_DP")
				(number "6")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "TXD/SPI_MISO")
				(number "20")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RXD/SPI_MOSI")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "SDA/~{SPI_CS}")
				(number "18")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SCL/SPI_CLK")
				(number "19")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "EXTINT")
				(number "4")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "1")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "D_SEL")
				(number "2")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "V_BCKP")
				(number "22")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD_USB")
				(number "7")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin power_out line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VCC_RF")
				(number "9")
			)
			(pin no_connect line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "15")
			)
			(pin no_connect line
				(at 15.24 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "16")
			)
			(pin no_connect line
				(at 15.24 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "17")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "LNA_EN")
				(number "14")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "11")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NEO-M8P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "NEO-M8P"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "RF_GPS:ublox_NEO"
			(at 10.16 -21.59 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/NEO-M8P_DataSheet_UBX-15016656.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS RTK Module NEO M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS RTK module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*NEO*"
			(at 0 0 0)
		)
		(symbol "NEO-M8P_0_1")
		(symbol "NEO-M8P_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "USB_DM")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "USB_DP")
				(number "6")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "TXD/SPI_MISO")
				(number "20")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RXD/SPI_MOSI")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "SDA/~{SPI_CS}")
				(number "18")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SCL/SPI_CLK")
				(number "19")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "EXTINT")
				(number "4")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "1")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "D_SEL")
				(number "2")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "V_BCKP")
				(number "22")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD_USB")
				(number "7")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin power_out line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VCC_RF")
				(number "9")
			)
			(pin no_connect line
				(at 15.24 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "17")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "LNA_EN")
				(number "14")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "11")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "3")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "RTK_STAT")
				(number "15")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GEOFENCE_STAT")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NEO-M8T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "NEO-M8T"
			(at 11.43 24.13 0)
		)
		(property "Footprint" "RF_GPS:ublox_NEO"
			(at 10.16 -24.13 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/documents/NEO-LEA-M8T-FW3_DataSheet_UBX-15025193.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module NEO M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*NEO*"
			(at 0 0 0)
		)
		(symbol "NEO-M8T_0_1")
		(symbol "NEO-M8T_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "USB_DM")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "USB_DP")
				(number "6")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "TXD/SPI_MISO")
				(number "20")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "RXD/SPI_MOSI")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SDA/~{SPI_CS}")
				(number "18")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "SCL/SPI_CLK")
				(number "19")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "EXTINT1")
				(number "15")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "EXTINT0")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "TP2/~{SAFEBOOT}")
				(number "1")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "D_SEL")
				(number "2")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "V_BCKP")
				(number "22")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD_USB")
				(number "7")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VCC_RF")
				(number "9")
			)
			(pin no_connect line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "16")
			)
			(pin no_connect line
				(at 15.24 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "17")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "LNA_EN")
				(number "14")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RF_IN")
				(number "11")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RXM-GPS-RM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "RXM-GPS-RM"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "RF_GPS:Linx_RXM-GPS"
			(at 12.7 -13.97 0)
		)
		(property "Datasheet" "https://linxtechnologies.com/wp/wp-content/uploads/rxm-gps-rm.pdf"
			(at 7.62 -7.62 0)
		)
		(property "Description" "Module GPS Low Power, 14mA tracking, 22 channels"
			(at 0 0 0)
		)
		(property "ki_keywords" "gps low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linx*RXM?GPS*"
			(at 0 0 0)
		)
		(symbol "RXM-GPS-RM_0_1")
		(symbol "RXM-GPS-RM_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RFIN")
				(number "19")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RX")
				(number "5")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "TX")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VBCKUP")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "1PPS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SAM-M8Q"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "SAM-M8Q"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "RF_GPS:ublox_SAM-M8Q"
			(at 12.7 -11.43 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/SAM-M8Q_DataSheet_%28UBX-16012619%29.pdf"
			(at 0 0 0)
		)
		(property "Description" "GPS ublox M8 variant"
			(at 0 0 0)
		)
		(property "ki_keywords" "gps module with antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*SAM?M8Q*"
			(at 0 0 0)
		)
		(symbol "SAM-M8Q_0_1")
		(symbol "SAM-M8Q_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EXTINT")
				(number "19")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "TIMEPULSE")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "18")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC_IO")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "V_BCKP")
				(number "3")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RXD")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "TXD")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SCL")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SIM28ML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "SIM28ML"
			(at 11.43 13.97 0)
		)
		(property "Footprint" "RF_GPS:SIM28ML"
			(at 0 0 0)
		)
		(property "Datasheet" "https://simcom.ee/documents/SIM28ML/SIM28ML_Hardware%20Design_V1.01.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standalone GPS/A-GPS receiver module, built-in LNA, -165dBm sensitivity, 2.8-4.3V, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "GPS A-GPS receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIM28ML*"
			(at 0 0 0)
		)
		(symbol "SIM28ML_0_1")
		(symbol "SIM28ML_1_1"
			(pin output line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "TXD0")
				(number "2")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RXD0")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "TXD1/SDA")
				(number "16")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "RXD1/SCL")
				(number "17")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "EXTINT")
				(number "5")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "Vcc")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_BACKUP")
				(number "6")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_out line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "Vcc_RF")
				(number "14")
			)
			(pin no_connect line
				(at 15.24 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 15.24 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin power_out line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "ANTON")
				(number "13")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "RF_IN")
				(number "11")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "TIMEMARK")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZED-F9P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "ZED-F9P"
			(at 11.43 26.67 0)
		)
		(property "Footprint" "RF_GPS:ublox_ZED"
			(at 0 -39.37 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/ZED-F9P-04B_DataSheet_UBX-21044850.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module ZED F9, VCC 2.7V to 3.6V, LGA-54"
			(at 0 0 0)
		)
		(property "ki_keywords" "u-blox GNSS multi-band RTK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*ZED*"
			(at 0 0 0)
		)
		(symbol "ZED-F9P_0_1")
		(symbol "ZED-F9P_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "USB_DM")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "USB_DP")
				(number "40")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "TXD/SPI_MISO")
				(number "42")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "RXD/SPI_MOSI")
				(number "43")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "TXD2")
				(number "27")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "RXD2")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SDA/~{SPI_CS}")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "SCL/SPI_CLK")
				(number "45")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "EXTINT")
				(number "51")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "50")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "49")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "D_SEL")
				(number "47")
			)
			(pin no_connect line
				(at -15.24 22.86 0)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "8")
			)
			(pin no_connect line
				(at -15.24 15.24 0)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "9")
			)
			(pin no_connect line
				(at -15.24 7.62 0)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "10")
			)
			(pin no_connect line
				(at -15.24 0 0)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "11")
			)
			(pin no_connect line
				(at -15.24 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "13")
			)
			(pin no_connect line
				(at -15.24 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "15")
			)
			(pin no_connect line
				(at -7.62 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "16")
			)
			(pin passive line
				(at -5.08 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "33")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "34")
			)
			(pin no_connect line
				(at -5.08 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "17")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "V_BCKP")
				(number "36")
			)
			(pin no_connect line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "18")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "V_USB")
				(number "38")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin no_connect line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "21")
			)
			(pin power_out line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VCC_RF")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "22")
			)
			(pin no_connect line
				(at 7.62 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "23")
			)
			(pin no_connect line
				(at 15.24 22.86 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "54")
			)
			(pin no_connect line
				(at 15.24 20.32 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "52")
			)
			(pin no_connect line
				(at 15.24 17.78 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "35")
			)
			(pin no_connect line
				(at 15.24 7.62 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "31")
			)
			(pin no_connect line
				(at 15.24 2.54 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "30")
			)
			(pin no_connect line
				(at 15.24 0 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "29")
			)
			(pin no_connect line
				(at 15.24 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "28")
			)
			(pin no_connect line
				(at 15.24 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "25")
			)
			(pin no_connect line
				(at 15.24 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "24")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "ANT_OFF")
				(number "5")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "ANT_DETECT")
				(number "4")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "~{ANT_SHORT}")
				(number "6")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "RF_IN")
				(number "2")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "53")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "RTK_STAT")
				(number "20")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "GEOFENCE_STAT")
				(number "19")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "TX_READY")
				(number "46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZOE-M8G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 39.37 0)
		)
		(property "Value" "ZOE-M8G"
			(at -19.05 36.83 0)
		)
		(property "Footprint" "RF_GPS:ublox_ZOE_M8"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/ZOE-M8_HIM_UBX-16030136.pdf"
			(at 0 0 0)
		)
		(property "Description" "ultra small GNSS  module IC, SiP"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox gnss sip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*ZOE*M8*"
			(at 0 0 0)
		)
		(symbol "ZOE-M8G_1_1"
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "SQI_D0")
				(number "D1")
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "SQI_D1")
				(number "C1")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "SQI_D2")
				(number "E3")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "SQI_D3")
				(number "F3")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "~{SQI_CS}")
				(number "D3")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "SQI_CLK")
				(number "E1")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "RXD/SPI_MOSI")
				(number "J4")
			)
			(pin output line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "TXD/SPI_MISO")
				(number "J5")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "SDA/~{SPI_CS}")
				(number "A2")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "SCL/SPI_CLK")
				(number "B1")
			)
			(pin input line
				(at -22.86 0 0)
				(length 2.54)
				(name "~{RESET}")
				(number "J6")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "RF_IN")
				(number "A4")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PIO13/EXTINT")
				(number "G4")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PIO14")
				(number "F6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PIO15")
				(number "C6")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "D_SEL")
				(number "D4")
			)
			(pin input line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "C4")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "RTC_I")
				(number "J7")
			)
			(pin output line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "RTC_O")
				(number "J8")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "J1")
			)
			(pin passive line
				(at -7.62 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "J2")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "V_BCKP")
				(number "H9")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "J3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "G1")
			)
			(pin no_connect line
				(at 20.32 0 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "A6")
			)
			(pin no_connect line
				(at 20.32 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "E9")
			)
			(pin no_connect line
				(at 20.32 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "F1")
			)
			(pin no_connect line
				(at 20.32 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "F4")
			)
			(pin no_connect line
				(at 20.32 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "F9")
			)
			(pin no_connect line
				(at 20.32 -25.4 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "G5")
			)
			(pin no_connect line
				(at 20.32 -30.48 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "G9")
			)
			(pin output line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "C3")
			)
			(pin output line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "LNA_EN")
				(number "C5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZOE-M8Q"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 39.37 0)
		)
		(property "Value" "ZOE-M8Q"
			(at -19.05 36.83 0)
		)
		(property "Footprint" "RF_GPS:ublox_ZOE_M8"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/ZOE-M8_HIM_UBX-16030136.pdf"
			(at 0 0 0)
		)
		(property "Description" "ultra small GNSS  module IC, SiP"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox gnss sip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*ZOE*M8*"
			(at 0 0 0)
		)
		(symbol "ZOE-M8Q_1_1"
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "SQI_D0")
				(number "D1")
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "SQI_D1")
				(number "C1")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "SQI_D2")
				(number "E3")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "SQI_D3")
				(number "F3")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "~{SQI_CS}")
				(number "D3")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "SQI_CLK")
				(number "E1")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "RXD/SPI_MOSI")
				(number "J4")
			)
			(pin output line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "TXD/SPI_MISO")
				(number "J5")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "SDA/~{SPI_CS}")
				(number "A2")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "SCL/SPI_CLK")
				(number "B1")
			)
			(pin input line
				(at -22.86 0 0)
				(length 2.54)
				(name "~{RESET}")
				(number "J6")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "RF_IN")
				(number "A4")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PIO13/EXTINT")
				(number "G4")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PIO14")
				(number "F6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PIO15")
				(number "C6")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "D_SEL")
				(number "D4")
			)
			(pin input line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "~{SAFEBOOT}")
				(number "C4")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "RTC_I")
				(number "J7")
			)
			(pin output line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "RTC_O")
				(number "J8")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "J1")
			)
			(pin passive line
				(at -7.62 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "J2")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "V_BCKP")
				(number "H9")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D9")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "J3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "J9")
			)
			(pin power_out line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "V_DCDC_OUT")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "V_CORE")
				(number "G1")
			)
			(pin no_connect line
				(at 20.32 0 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "A6")
			)
			(pin no_connect line
				(at 20.32 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "E9")
			)
			(pin no_connect line
				(at 20.32 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "F1")
			)
			(pin no_connect line
				(at 20.32 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "F4")
			)
			(pin no_connect line
				(at 20.32 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "F9")
			)
			(pin no_connect line
				(at 20.32 -25.4 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "G5")
			)
			(pin no_connect line
				(at 20.32 -30.48 180)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "G9")
			)
			(pin output line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "TIMEPULSE")
				(number "C3")
			)
			(pin output line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "LNA_EN")
				(number "C5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX-8Q"
		(extends "MAX-8C")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "MAX-8Q"
			(at 11.43 16.51 0)
		)
		(property "Footprint" "RF_GPS:ublox_MAX"
			(at 10.16 -16.51 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/MAX-8_DataSheet_%28UBX-16000093%29.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*MAX*"
			(at 0 0 0)
		)
	)
	(symbol "MAX-M8C"
		(extends "MAX-8C")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "MAX-M8C"
			(at 11.43 16.51 0)
		)
		(property "Footprint" "RF_GPS:ublox_MAX"
			(at 10.16 -16.51 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/MAX-M8-FW3_DataSheet_%28UBX-15031506%29.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module MAX M8, VCC 1.65V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*MAX*"
			(at 0 0 0)
		)
	)
	(symbol "MAX-M8Q"
		(extends "MAX-8C")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "MAX-M8Q"
			(at 11.43 16.51 0)
		)
		(property "Footprint" "RF_GPS:ublox_MAX"
			(at 10.16 -16.51 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/MAX-M8-FW3_DataSheet_%28UBX-15031506%29.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module MAX M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*MAX*"
			(at 0 0 0)
		)
	)
	(symbol "NEO-8Q"
		(extends "NEO-M8N")
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "NEO-8Q"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "RF_GPS:ublox_NEO"
			(at 10.16 -21.59 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/documents/NEO-8Q_DataSheet_UBX-15031913.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module NEO 8, VCC 1.65V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*NEO*"
			(at 0 0 0)
		)
	)
	(symbol "NEO-M8Q"
		(extends "NEO-M8N")
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "NEO-M8Q"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "RF_GPS:ublox_NEO"
			(at 10.16 -21.59 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/NEO-M8-FW3_DataSheet_UBX-15031086.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module NEO M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*NEO*"
			(at 0 0 0)
		)
	)
	(symbol "NEO-M9N"
		(extends "NEO-M8N")
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "NEO-M9N"
			(at 11.43 21.59 0)
		)
		(property "Footprint" "RF_GPS:ublox_NEO"
			(at 10.16 -21.59 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/NEO-M9N-00B_DataSheet_UBX-19014285.pdf"
			(at 0 0 0)
		)
		(property "Description" "GNSS Module NEO M8, VCC 2.7V to 3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ublox GPS GNSS module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*NEO*"
			(at 0 0 0)
		)
	)
	(symbol "RXM-GPS-FM"
		(extends "RXM-GPS-RM")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "RXM-GPS-FM"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "RF_GPS:Linx_RXM-GPS"
			(at 12.7 -13.97 0)
		)
		(property "Datasheet" "https://linxtechnologies.com/wp/wp-content/uploads/rxm-gps-fm.pdf"
			(at 7.62 -7.62 0)
		)
		(property "Description" "Module GPS Low Power, 14mA tracking, 22 channels"
			(at 0 0 0)
		)
		(property "ki_keywords" "gps low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linx*RXM?GPS*"
			(at 0 0 0)
		)
	)
)
