(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "BC66"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "BC66"
			(at 10.16 26.67 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BC66"
			(at 13.97 -26.67 0)
		)
		(property "Datasheet" "https://www.quectel.com/UploadImage/Downlad/Quectel_BC66_Hardware_Design_V1.1.pdf"
			(at 43.18 -25.4 0)
		)
		(property "Description" "Quectel NB-IoT Global, AT Command Set"
			(at 0 0 0)
		)
		(property "ki_keywords" "NB-IoT Data SMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel*BC66*"
			(at 0 0 0)
		)
		(symbol "BC66_0_1")
		(symbol "BC66_1_1"
			(pin output line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "RI")
				(number "20")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "RXD")
				(number "18")
			)
			(pin output line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "TXD")
				(number "17")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RXD_AUX")
				(number "28")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TXD_AUX")
				(number "29")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RXD_DBG")
				(number "38")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "TXD_DBG")
				(number "39")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PWRKEY")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PSM_EINT")
				(number "19")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "ADC0")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 22.86 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "8")
			)
			(pin no_connect line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "21")
			)
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "22")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "23")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "25")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "51")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "26")
			)
			(pin no_connect line
				(at -12.7 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "30")
			)
			(pin no_connect line
				(at -10.16 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "31")
			)
			(pin no_connect line
				(at -7.62 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "32")
			)
			(pin no_connect line
				(at -5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "33")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VBAT_BB")
				(number "42")
			)
			(pin no_connect line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "44")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VBAT_RF")
				(number "43")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin power_out line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD_EXT")
				(number "24")
			)
			(pin no_connect line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "54")
			)
			(pin no_connect line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "58")
			)
			(pin no_connect line
				(at 5.08 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "45")
			)
			(pin no_connect line
				(at 7.62 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "46")
			)
			(pin no_connect line
				(at 10.16 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "47")
			)
			(pin no_connect line
				(at 12.7 22.86 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "57")
			)
			(pin no_connect line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "55")
			)
			(pin no_connect line
				(at 12.7 15.24 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "56")
			)
			(pin no_connect line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "53")
			)
			(pin no_connect line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "52")
			)
			(pin no_connect line
				(at 12.7 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "50")
			)
			(pin no_connect line
				(at 12.7 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "49")
			)
			(pin no_connect line
				(at 12.7 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "48")
			)
			(pin passive line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "RF_ANT")
				(number "35")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SIM_VDD")
				(number "14")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SIM_RST")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SIM_DATA")
				(number "11")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SIM_CLK")
				(number "13")
			)
			(pin power_out line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SIM_GND")
				(number "10")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "SPI_MISO")
				(number "3")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SPI_MOSI")
				(number "4")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SPI_SCLK")
				(number "5")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SPI_CS")
				(number "6")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "NETLIGHT")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BC95"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "BC95"
			(at 10.16 16.51 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BC95"
			(at 11.43 -16.51 0)
		)
		(property "Datasheet" "https://www.quectel.com/UploadImage/Downlad/Quectel_BC95_Hardware_Design_V1.3.pdf"
			(at 0 0 0)
		)
		(property "Description" "NB-IoT, GSM Quad-Band Communication Module, GPRS, Audio Engine, AT Command Set"
			(at 0 0 0)
		)
		(property "ki_keywords" "NB-IoT GSM GPRS Quad-Band SMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel?BC95*"
			(at 0 0 0)
		)
		(symbol "BC95_0_1")
		(symbol "BC95_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RESET")
				(number "15")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RI")
				(number "34")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "30")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "29")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "NETLIGHT")
				(number "18")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DBG_TXD")
				(number "20")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DBG_RXD")
				(number "19")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "ADC")
				(number "21")
			)
			(pin power_out line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDD_EXT")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "66")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "83")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "92")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "93")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "94")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "USIM_GND")
				(number "42")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VBAT")
				(number "45")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VBAT")
				(number "46")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RF_ANT")
				(number "53")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 2.54)
				(name "USIM_VDD")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "USIM_DATA")
				(number "40")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "USIM_CLK")
				(number "41")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "USIM_RST")
				(number "39")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BG95-M1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.526 52.324 0)
		)
		(property "Value" "BG95-M1"
			(at 15.24 52.324 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BG95"
			(at 0 -53.594 0)
		)
		(property "Datasheet" "https://images.quectel.com/python/sites/2/2023/05/Quectel_BG95_Series_QuecOpen_Hardware_Design_V1.3.pdf"
			(at -1.27 33.02 0)
		)
		(property "Description" "NB-IoT, Cat M1 Communication Module, AT Command Set"
			(at -1.27 33.02 0)
		)
		(property "ki_keywords" "NB-IoT Cat M1 GNSS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel?BG95*"
			(at 0 0 0)
		)
		(symbol "BG95-M1_0_1")
		(symbol "BG95-M1_1_1"
			(pin input line
				(at -20.32 48.26 0)
				(length 2.54)
				(name "~{RESET}")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PWRKEY")
				(number "15")
			)
			(pin input line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "USB_BOOT")
				(number "75")
			)
			(pin input line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "MAIN_DTR")
				(number "30")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "MAIN_RXD")
				(number "34")
			)
			(pin output line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "MAIN_TXD")
				(number "35")
			)
			(pin output line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "MAIN_CTS")
				(number "36")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "MAIN_RTS")
				(number "37")
			)
			(pin output line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "MAIN_DCD")
				(number "38")
			)
			(pin output line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "MAIN_RI")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "USB_DP")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "USB_DM")
				(number "10")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PON_TRIG")
				(number "96")
			)
			(pin output line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PSM_IND")
				(number "1")
			)
			(pin output line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "STATUS")
				(number "20")
			)
			(pin output line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "NET_STATUS")
				(number "21")
			)
			(pin input line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "ADC0")
				(number "24")
			)
			(pin input line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "ADC1")
				(number "2")
			)
			(pin no_connect line
				(at -17.78 7.62 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "11")
			)
			(pin no_connect line
				(at -17.78 5.08 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "12")
			)
			(pin no_connect line
				(at -17.78 2.54 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "13")
			)
			(pin no_connect line
				(at -17.78 0 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "14")
			)
			(pin no_connect line
				(at -17.78 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "16")
			)
			(pin no_connect line
				(at -17.78 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "51")
			)
			(pin no_connect line
				(at -17.78 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "57")
			)
			(pin no_connect line
				(at -17.78 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "63")
			)
			(pin no_connect line
				(at -17.78 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "76")
			)
			(pin no_connect line
				(at -17.78 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "77")
			)
			(pin no_connect line
				(at -17.78 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "78")
			)
			(pin no_connect line
				(at -17.78 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "92")
			)
			(pin no_connect line
				(at -17.78 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "93")
			)
			(pin no_connect line
				(at -17.78 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "94")
			)
			(pin no_connect line
				(at -17.78 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "95")
			)
			(pin no_connect line
				(at -7.62 50.8 270)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "98")
			)
			(pin no_connect line
				(at -5.08 50.8 270)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "97")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 2.54)
				(name "VBAT_BB")
				(number "32")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 2.54)
				(hide yes)
				(name "VBAT_BB")
				(number "33")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 2.54)
				(name "VBAT_RF")
				(number "52")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 2.54)
				(hide yes)
				(name "VBAT_RF")
				(number "53")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "100")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "101")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "102")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "58")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "68")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "90")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 2.54)
				(name "USIM_GND")
				(number "47")
			)
			(pin no_connect line
				(at 7.62 50.8 270)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "99")
			)
			(pin no_connect line
				(at 17.78 43.18 180)
				(length 2.54)
				(hide yes)
				(name "ANT_WIFI")
				(number "56")
			)
			(pin passive line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "ANT_GNSS")
				(number "49")
			)
			(pin passive line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "ANT_MAIN")
				(number "60")
			)
			(pin power_out line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "VDD_EXT")
				(number "29")
			)
			(pin output line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "GRFC2")
				(number "84")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "GRFC1")
				(number "83")
			)
			(pin power_out line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "USIM_VDD")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "USIM_DATA")
				(number "45")
			)
			(pin output clock
				(at 20.32 17.78 180)
				(length 2.54)
				(name "USIM_CLK")
				(number "46")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "USIM_RST")
				(number "44")
			)
			(pin input line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "USIM_DET")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GPIO1")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "GPIO3")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "GPIO4")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "GPIO5")
				(number "18")
				(alternate "I2C1_SCL" open_collector line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "GPIO6")
				(number "19")
				(alternate "I2C1_SDA" open_collector line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "GPIO7")
				(number "22")
				(alternate "UART1_RXD" input line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "GPIO8")
				(number "23")
				(alternate "UART1_TXD" output line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "GPIO9")
				(number "25")
				(alternate "~{SPI1_CS}" output line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "GPIO10")
				(number "26")
				(alternate "SPI1_CLK" output line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "GPIO11")
				(number "27")
				(alternate "SPI1_MOSI" output line)
				(alternate "UART3_TXD" output line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "GPIO12")
				(number "28")
				(alternate "SPI1_MISO" input line)
				(alternate "UART3_RXD" input line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "GPIO13")
				(number "40")
				(alternate "SPI2_CLK" output line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "GPIO14")
				(number "41")
				(alternate "~{SPI2_CS}" output line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "GPIO15")
				(number "64")
				(alternate "SPI2_MOSI" output line)
				(alternate "UART2_TXD" output line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "GPIO16")
				(number "65")
				(alternate "SPI2_MISO" input line)
				(alternate "UART2_RXD" input line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 2.54)
				(name "GPIO17")
				(number "66")
				(alternate "PWM" output line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 2.54)
				(name "GPIO18")
				(number "85")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 2.54)
				(name "GPIO19")
				(number "86")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 2.54)
				(name "GPIO20")
				(number "87")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 2.54)
				(name "GPIO21")
				(number "88")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BG95-MF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.526 52.324 0)
		)
		(property "Value" "BG95-MF"
			(at 15.24 52.324 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BG95"
			(at 0 -53.594 0)
		)
		(property "Datasheet" "https://images.quectel.com/python/sites/2/2023/05/Quectel_BG95_Series_QuecOpen_Hardware_Design_V1.3.pdf"
			(at -1.27 33.02 0)
		)
		(property "Description" "NB-IoT, Cat M1 Cat NB2 Wifi Communication Module, AT Command Set"
			(at -1.27 33.02 0)
		)
		(property "ki_keywords" "NB-IoT Cat M1 NB2 Wifi GNSS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel?BG95*"
			(at 0 0 0)
		)
		(symbol "BG95-MF_0_1")
		(symbol "BG95-MF_1_1"
			(pin input line
				(at -20.32 48.26 0)
				(length 2.54)
				(name "~{RESET}")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PWRKEY")
				(number "15")
			)
			(pin input line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "USB_BOOT")
				(number "75")
			)
			(pin input line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "MAIN_DTR")
				(number "30")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "MAIN_RXD")
				(number "34")
			)
			(pin output line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "MAIN_TXD")
				(number "35")
			)
			(pin output line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "MAIN_CTS")
				(number "36")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "MAIN_RTS")
				(number "37")
			)
			(pin output line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "MAIN_DCD")
				(number "38")
			)
			(pin output line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "MAIN_RI")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "USB_DP")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "USB_DM")
				(number "10")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PON_TRIG")
				(number "96")
			)
			(pin output line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PSM_IND")
				(number "1")
			)
			(pin output line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "STATUS")
				(number "20")
			)
			(pin output line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "NET_STATUS")
				(number "21")
			)
			(pin input line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "ADC0")
				(number "24")
			)
			(pin input line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "ADC1")
				(number "2")
			)
			(pin no_connect line
				(at -17.78 7.62 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "11")
			)
			(pin no_connect line
				(at -17.78 5.08 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "12")
			)
			(pin no_connect line
				(at -17.78 2.54 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "13")
			)
			(pin no_connect line
				(at -17.78 0 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "14")
			)
			(pin no_connect line
				(at -17.78 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "16")
			)
			(pin no_connect line
				(at -17.78 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "51")
			)
			(pin no_connect line
				(at -17.78 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "57")
			)
			(pin no_connect line
				(at -17.78 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "63")
			)
			(pin no_connect line
				(at -17.78 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "76")
			)
			(pin no_connect line
				(at -17.78 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "77")
			)
			(pin no_connect line
				(at -17.78 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "78")
			)
			(pin no_connect line
				(at -17.78 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "92")
			)
			(pin no_connect line
				(at -17.78 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "93")
			)
			(pin no_connect line
				(at -17.78 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "94")
			)
			(pin no_connect line
				(at -17.78 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "95")
			)
			(pin no_connect line
				(at -7.62 50.8 270)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "98")
			)
			(pin no_connect line
				(at -5.08 50.8 270)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "97")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 2.54)
				(name "VBAT_BB")
				(number "32")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 2.54)
				(hide yes)
				(name "VBAT_BB")
				(number "33")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 2.54)
				(name "VBAT_RF")
				(number "52")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 2.54)
				(hide yes)
				(name "VBAT_RF")
				(number "53")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "100")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "101")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "102")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "58")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "68")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "90")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 2.54)
				(name "USIM_GND")
				(number "47")
			)
			(pin no_connect line
				(at 7.62 50.8 270)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "99")
			)
			(pin passive line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "ANT_GNSS")
				(number "49")
			)
			(pin passive line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "ANT_MAIN")
				(number "60")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "ANT_WIFI")
				(number "56")
			)
			(pin power_out line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "VDD_EXT")
				(number "29")
			)
			(pin output line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "GRFC2")
				(number "84")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "GRFC1")
				(number "83")
			)
			(pin power_out line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "USIM_VDD")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "USIM_DATA")
				(number "45")
			)
			(pin output clock
				(at 20.32 17.78 180)
				(length 2.54)
				(name "USIM_CLK")
				(number "46")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "USIM_RST")
				(number "44")
			)
			(pin input line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "USIM_DET")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GPIO1")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "GPIO3")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "GPIO4")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "GPIO5")
				(number "18")
				(alternate "I2C1_SCL" open_collector line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "GPIO6")
				(number "19")
				(alternate "I2C1_SDA" open_collector line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "GPIO7")
				(number "22")
				(alternate "UART1_RXD" input line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "GPIO8")
				(number "23")
				(alternate "UART1_TXD" output line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "GPIO9")
				(number "25")
				(alternate "~{SPI1_CS}" output line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "GPIO10")
				(number "26")
				(alternate "SPI1_CLK" output line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "GPIO11")
				(number "27")
				(alternate "SPI1_MOSI" output line)
				(alternate "UART3_TXD" output line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "GPIO12")
				(number "28")
				(alternate "SPI1_MISO" input line)
				(alternate "UART3_RXD" input line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "GPIO13")
				(number "40")
				(alternate "SPI2_CLK" output line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "GPIO14")
				(number "41")
				(alternate "~{SPI2_CS}" output line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "GPIO15")
				(number "64")
				(alternate "SPI2_MOSI" output line)
				(alternate "UART2_TXD" output line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "GPIO16")
				(number "65")
				(alternate "SPI2_MISO" input line)
				(alternate "UART2_RXD" input line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 2.54)
				(name "GPIO17")
				(number "66")
				(alternate "PWM" output line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 2.54)
				(name "GPIO18")
				(number "85")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 2.54)
				(name "GPIO19")
				(number "86")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 2.54)
				(name "GPIO20")
				(number "87")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 2.54)
				(name "GPIO21")
				(number "88")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LENA-R8001"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 33.02 0)
		)
		(property "Value" "LENA-R8001"
			(at 12.7 33.02 0)
		)
		(property "Footprint" "RF_GSM:ublox_LENA-R8_LGA-100"
			(at 16.51 -33.02 0)
		)
		(property "Datasheet" "https://content.u-blox.com/sites/default/files/documents/LENA-R8_SysIntegrManual_UBX-22015376.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Ublox HSPA GSM Quad-Band Communication Module, AT Command Set, AT Command Set, Worldwide , LGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "GSM LTE 2G 4G"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*LENA?R8*"
			(at 0 0 0)
		)
		(symbol "LENA-R8001_0_1")
		(symbol "LENA-R8001_1_1"
			(pin input line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "DTR")
				(number "9")
			)
			(pin output line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "RI")
				(number "7")
			)
			(pin output line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "DCD")
				(number "8")
			)
			(pin output line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "CTS")
				(number "11")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "RTS")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "DSR")
				(number "6")
			)
			(pin output line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "RXD")
				(number "13")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "TXD")
				(number "12")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "PWR_ON")
				(number "15")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "~{RESET}")
				(number "18")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "USB_BOOT")
				(number "33")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "VUSB_DET")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "USB_D-")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "USB_D+")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "SDA")
				(number "26")
			)
			(pin output line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "SCL")
				(number "27")
			)
			(pin no_connect line
				(at -16.51 27.94 0)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "21")
			)
			(pin no_connect line
				(at -16.51 25.4 0)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "31")
			)
			(pin no_connect line
				(at -16.51 2.54 0)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "44")
			)
			(pin no_connect line
				(at -16.51 -2.54 0)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "45")
			)
			(pin no_connect line
				(at -16.51 -7.62 0)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "46")
			)
			(pin no_connect line
				(at -16.51 -20.32 0)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "47")
			)
			(pin no_connect line
				(at -16.51 -22.86 0)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "48")
			)
			(pin power_in line
				(at -7.62 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "51")
			)
			(pin passive line
				(at -7.62 35.56 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin passive line
				(at -7.62 35.56 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 3.81)
				(name "V_BCKP")
				(number "2")
			)
			(pin power_out line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "V_INT")
				(number "4")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "58")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "66")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "68")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "76")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "77")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "78")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "83")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "84")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "86")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "87")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "88")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "90")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "92")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "93")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "94")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "95")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "96")
			)
			(pin no_connect line
				(at 2.54 31.75 270)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "99")
			)
			(pin no_connect line
				(at 5.08 31.75 270)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "100")
			)
			(pin no_connect line
				(at 16.51 -27.94 180)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "49")
			)
			(pin no_connect line
				(at 16.51 -30.48 180)
				(length 3.81)
				(hide yes)
				(name "RSVD")
				(number "62")
			)
			(pin passive line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "ANT")
				(number "56")
			)
			(pin input line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "ANT_DET")
				(number "59")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "RFCTRL1")
				(number "97")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "RFCTRL2")
				(number "98")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "SIM_CLK")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "SIM_IO")
				(number "39")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "SIM_RST")
				(number "40")
			)
			(pin power_out line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "VSIM")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "GPIO1")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "GPIO2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "GPIO3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "GPIO4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "GPIO5")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "GPIO6")
				(number "19")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "I2S_CLK")
				(number "36")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "I2S_WA")
				(number "34")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "I2S_TXD")
				(number "35")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "I2S_RXD")
				(number "37")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M95"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "M95"
			(at 12.7 29.21 0)
		)
		(property "Footprint" "RF_GSM:Quectel_M95"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.quectel.com/UploadImage/Downlad/M95_Hardware_Design_V1.3.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Quectel quad-band GSM/GPRS module in LCC package"
			(at 0 0 0)
		)
		(property "ki_keywords" "GSM GPRS AT SMS voice TCP/IP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel*M95*"
			(at 0 0 0)
		)
		(symbol "M95_0_1")
		(symbol "M95_1_1"
			(pin passive line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "RF_ANT")
				(number "39")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "~{PWRKEY}")
				(number "10")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{EMERG_OFF}")
				(number "11")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "DBG_RXD")
				(number "14")
			)
			(pin output line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DBG_TXD")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DTR")
				(number "20")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "21")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "TXD")
				(number "22")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CTS")
				(number "23")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RTS")
				(number "24")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DCD")
				(number "25")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RI")
				(number "26")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "16")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "18")
			)
			(pin no_connect line
				(at -12.7 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "41")
			)
			(pin no_connect line
				(at -12.7 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "42")
			)
			(pin power_in line
				(at -5.08 -30.48 90)
				(length 2.54)
				(name "AGND")
				(number "1")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "33")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VBAT")
				(number "34")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VRTC")
				(number "32")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin power_out line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDD_EXT")
				(number "19")
			)
			(pin input line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "MIC1P")
				(number "4")
			)
			(pin input line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "MIC1N")
				(number "5")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "MIC2P")
				(number "2")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "MIC2N")
				(number "3")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SPK1P")
				(number "7")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SPK1N")
				(number "6")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "LOUDSPKP")
				(number "9")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "LOUDSPKN")
				(number "8")
			)
			(pin power_out line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SIM_VDD")
				(number "27")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SIM_RST")
				(number "28")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "SIM_CLK")
				(number "30")
			)
			(pin power_out line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "SIM_GND")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "SIM_DATA")
				(number "29")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "STATUS")
				(number "12")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "NETLIGHT")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SARA-U201"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 26.67 0)
		)
		(property "Value" "SARA-U201"
			(at -11.43 26.67 0)
		)
		(property "Footprint" "RF_GSM:ublox_SARA_LGA-96"
			(at 17.78 -26.67 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/SARA-U2_DataSheet_(UBX-13005287).pdf"
			(at 0 0 0)
		)
		(property "Description" "Ublox HSPA GSM Quad-Band Communication Module, AT Command Set, AT Command Set, Worldwide , LGA-96"
			(at 0 0 0)
		)
		(property "ki_keywords" "GSM HSPA 2G 3G"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*SARA*"
			(at 0 0 0)
		)
		(symbol "SARA-U201_0_1")
		(symbol "SARA-U201_1_1"
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "DTR")
				(number "9")
			)
			(pin output line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "RI")
				(number "7")
			)
			(pin output line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "DCD")
				(number "8")
			)
			(pin output line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "CTS")
				(number "11")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RTS")
				(number "10")
			)
			(pin output line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DSR")
				(number "6")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RXD")
				(number "13")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "12")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "PWR_ON")
				(number "15")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "18")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "VUSB_DET")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "USB_D-")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "USB_D+")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "SDA")
				(number "26")
			)
			(pin output line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "SCL")
				(number "27")
			)
			(pin no_connect line
				(at -12.7 2.54 0)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "31")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "33")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "44")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "45")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "51")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin no_connect line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "46")
			)
			(pin power_out line
				(at 0 27.94 270)
				(length 2.54)
				(name "V_BCKP")
				(number "2")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "58")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "66")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "68")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "76")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "77")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "78")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "83")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "84")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "86")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "87")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "88")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "90")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "92")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "93")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "94")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "95")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "96")
			)
			(pin power_out line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "V_INT")
				(number "4")
			)
			(pin no_connect line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "49")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "48")
			)
			(pin no_connect line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "47")
			)
			(pin passive line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "ANT")
				(number "56")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "ANT_DET")
				(number "62")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SIM_CLK")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SIM_IO")
				(number "39")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SIM_RST")
				(number "40")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VSIM")
				(number "41")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SIM_DET")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "GPIO1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GPIO2")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GPIO3")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "GPIO4")
				(number "25")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "CODEC_CLK")
				(number "19")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "I2S_CLK")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "I2S_WA")
				(number "34")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "I2S_TXD")
				(number "35")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "I2S_RXD")
				(number "37")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SE150A4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 38.1 0)
		)
		(property "Value" "SE150A4"
			(at 13.97 -40.64 0)
		)
		(property "Footprint" "RF_GSM:Telit_SE150A4"
			(at 25.4 19.05 0)
		)
		(property "Datasheet" "https://atoma.spb.ru/sites/default/files/documents/telit_se150a4_smart_module_hardware_user_guide_r1.pdf"
			(at 25.4 21.59 0)
		)
		(property "Description" "GSM, WCDMA,LTE, multi-mode and multi-band wireless smart module, 3.4V to 4.4V power supply, 40.5 x 40.5 x 2.8mm"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "GPRS LTE WCDMA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Telit*SE150A4*"
			(at 0 0 0)
		)
		(symbol "SE150A4_1_1"
			(text "POWER"
				(at -11.176 12.192 0)
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "CHG_RED_LED")
				(number "197")
			)
			(pin output line
				(at -20.32 0 0)
				(length 3.81)
				(name "CHARGE_SEL")
				(number "127")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "VREF_BATT_THERM")
				(number "196")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "VBAT_SNS")
				(number "133")
			)
			(pin passive line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "VBAT_THERM")
				(number "134")
			)
			(pin no_connect line
				(at -16.51 10.16 0)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "187")
			)
			(pin no_connect line
				(at -16.51 7.62 0)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "190")
			)
			(pin no_connect line
				(at -16.51 5.08 0)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "191")
			)
			(pin no_connect line
				(at -16.51 -5.08 0)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "199")
			)
			(pin no_connect line
				(at -16.51 -12.7 0)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "202")
			)
			(pin passive line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VBAT_BB")
				(number "1")
			)
			(pin passive line
				(at -2.54 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VBAT_BB")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VBAT_RF")
				(number "145")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VBAT_RF")
				(number "146")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "120")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "122")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "130")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "132")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "135")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "140")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "143")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "144")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "147")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "148")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "149")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "150")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "160")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "161")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "162")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "163")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "164")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "165")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "166")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "167")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "168")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "169")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "170")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "171")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "172")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "173")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "174")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "175")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "176")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "177")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "178")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "180")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "181")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "182")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "184")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "185")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "186")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "188")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "189")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "192")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "193")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "198")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "200")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "201")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "208")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "209")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "76")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "78")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "86")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "88")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VRTC")
				(number "126")
			)
			(pin no_connect line
				(at 5.08 13.97 270)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "207")
			)
			(pin no_connect line
				(at 16.51 10.16 180)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "206")
			)
			(pin no_connect line
				(at 16.51 2.54 180)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "205")
			)
			(pin no_connect line
				(at 16.51 -7.62 180)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "204")
			)
			(pin no_connect line
				(at 16.51 -12.7 180)
				(length 3.81)
				(hide yes)
				(name "RESERVED")
				(number "203")
			)
			(pin power_out line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "LDO5_1V8")
				(number "111")
			)
			(pin power_out line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "LDO6_1V8")
				(number "125")
			)
			(pin power_out line
				(at 20.32 0 180)
				(length 3.81)
				(name "LDO10_2V85")
				(number "153")
			)
			(pin power_out line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "LDO16_2V85")
				(number "195")
			)
			(pin power_out line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "LDO17_2V85")
				(number "129")
			)
			(pin power_out line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "SMPS_S3_1V35")
				(number "151")
			)
		)
		(symbol "SE150A4_2_1"
			(text "USB"
				(at -6.35 15.24 0)
			)
			(text "UARTs"
				(at -6.35 2.54 0)
			)
			(text "SD Card"
				(at 5.715 15.24 0)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "USB_DP")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "USB_DM")
				(number "13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "USB_ID")
				(number "16")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "USB_BOOT")
				(number "46")
			)
			(pin output line
				(at -15.24 0 0)
				(length 3.81)
				(name "UART1_TXD")
				(number "34")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "UART1_RXD")
				(number "35")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "UART1_CTS")
				(number "36")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "UART1_RTS")
				(number "37")
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "UART2_TXD")
				(number "94")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "UART2_RXD")
				(number "93")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "USB_VBUS")
				(number "141")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 3.81)
				(hide yes)
				(name "USB_VBUS")
				(number "142")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "SD_LDO11")
				(number "38")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "SD_LDO12")
				(number "32")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "SD_DET")
				(number "45")
				(alternate "GPIO_67" input line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "SD_DATA0")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "SD_DATA1")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "SD_DATA2")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "SD_DATA3")
				(number "44")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "SD_CLK")
				(number "39")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "SD_CMD")
				(number "40")
			)
		)
		(symbol "SE150A4_3_1"
			(text "SIM Cards"
				(at 0 0 900)
			)
			(pin power_out line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "USIM1_VDD")
				(number "26")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "USIM1_DET")
				(number "22")
			)
			(pin output line
				(at -17.78 0 0)
				(length 3.81)
				(name "USIM1_RST")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "USIM1_DATA")
				(number "25")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "USIM1_CLK")
				(number "24")
			)
			(pin power_out line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "USIM2_VDD")
				(number "21")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "USIM2_DET")
				(number "17")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "USIM2_RST")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "USIM2_DATA")
				(number "20")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "USIM2_CLK")
				(number "19")
			)
		)
		(symbol "SE150A4_4_1"
			(text "Touch panel\ninterface"
				(at -5.08 -11.43 0)
			)
			(text "Camera \ninterface"
				(at 0 3.81 0)
			)
			(text "Display \ninterface"
				(at 5.08 -31.75 0)
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 3.81)
				(name "MIPI_CSI0_LN0_P")
				(number "66")
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "MIPI_CSI0_LN0_M")
				(number "65")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "MIPI_CSI0_LN1_P")
				(number "68")
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "MIPI_CSI0_LN1_M")
				(number "67")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "MIPI_CSI0_LN2_P")
				(number "156")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "MIPI_CSI0_LN2_M")
				(number "157")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "MIPI_CSI0_LN3_P")
				(number "159")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "MIPI_CSI0_LN3_M")
				(number "158")
			)
			(pin output line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "MIPI_CSI0_CLK_P")
				(number "64")
			)
			(pin output line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "MIPI_CSI0_CLK_M")
				(number "63")
			)
			(pin output line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "CAM0_MCLK")
				(number "74")
			)
			(pin output line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "~{CAM0_RST}")
				(number "79")
			)
			(pin output line
				(at -22.86 0 0)
				(length 3.81)
				(name "CAM0_PWDN")
				(number "80")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "TP_I2C_SDA")
				(number "48")
			)
			(pin output line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "TP_I2C_SCL")
				(number "47")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "~{TP_INT}")
				(number "30")
			)
			(pin output line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "~{TP_RST}")
				(number "31")
			)
			(pin input line
				(at 22.86 33.02 180)
				(length 3.81)
				(name "MIPI_CSI1_LN0_P")
				(number "73")
			)
			(pin input line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "MIPI_CSI1_LN0_M")
				(number "72")
			)
			(pin input line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "MIPI_CSI1_LN1_P")
				(number "154")
			)
			(pin input line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "MIPI_CSI1_LN1_M")
				(number "155")
			)
			(pin output line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "MIPI_CSI1_CLK_P")
				(number "71")
			)
			(pin output line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "MIPI_CSI1_CLK_M")
				(number "70")
			)
			(pin output line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "CAM1_MCLK")
				(number "75")
			)
			(pin output line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "~{CAM1_RST}")
				(number "81")
			)
			(pin output line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "CAM1_PWDN")
				(number "82")
			)
			(pin output line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "CAM_I2C_SCL")
				(number "83")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "CAM_I2C_SDA")
				(number "84")
			)
			(pin output line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "MIPI_DSI_LANE0P")
				(number "55")
			)
			(pin output line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "MIPI_DSI_LANE0M")
				(number "54")
			)
			(pin output line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "MIPI_DSI_LANE1P")
				(number "57")
			)
			(pin output line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "MIPI_DSI_LANE1M")
				(number "56")
			)
			(pin output line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "MIPI_DSI_LANE2P")
				(number "59")
			)
			(pin output line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "MIPI_DSI_LANE2M")
				(number "58")
			)
			(pin output line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "MIPI_DSI_LANE3P")
				(number "61")
			)
			(pin output line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "MIPI_DSI_LANE3M")
				(number "60")
			)
			(pin output line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "MIPI_DSI_CLK_P")
				(number "53")
			)
			(pin output line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "MIPI_DSI_CLK_M")
				(number "52")
			)
			(pin output line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "~{LCD_RST}")
				(number "49")
			)
			(pin output line
				(at 22.86 -33.02 180)
				(length 3.81)
				(name "PWM")
				(number "29")
			)
			(pin input line
				(at 22.86 -35.56 180)
				(length 3.81)
				(name "LCD_TE")
				(number "50")
			)
		)
		(symbol "SE150A4_5_1"
			(text "A/D\nConverter"
				(at -2.794 -13.97 0)
			)
			(text "Keypad"
				(at -2.54 16.51 0)
			)
			(text "Vibrator"
				(at -1.27 -20.32 0)
			)
			(text "Sensor\ninterface"
				(at 0 -1.524 900)
			)
			(text "GPIOs"
				(at 4.445 0 900)
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "~{KEY_VOL_UP}")
				(number "95")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "~{KEY_VOL_DOWN}")
				(number "96")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "PWRKEY")
				(number "114")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "~{RESET}")
				(number "179")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "SENSOR_I2C_SCL")
				(number "91")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "SENSOR_I2C_SDA")
				(number "92")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "~{ALSP_INT}")
				(number "107")
				(alternate "GPIO_43" input line)
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "~{MAG_INT}")
				(number "108")
				(alternate "GPIO_44" input line)
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{ACCL_INT1}")
				(number "110")
				(alternate "GPIO_42" input line)
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{ACCL_INT2}")
				(number "109")
				(alternate "GPIO_46" input line)
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "ADC")
				(number "128")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "ADC2")
				(number "183")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "~{VIB_DRV}")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "GPIO_6")
				(number "113")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "GPIO_7")
				(number "112")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "GPIO_8")
				(number "123")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "GPIO_9")
				(number "124")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "GPIO_20")
				(number "119")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "GPIO_21")
				(number "118")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "GPIO_22")
				(number "117")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "GPIO_23")
				(number "116")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "GPIO_25")
				(number "115")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "GPIO_33")
				(number "99")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "GPIO_34")
				(number "100")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "GPIO_61")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "GPIO_85")
				(number "103")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "GPIO_86")
				(number "104")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "GPIO_87")
				(number "105")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "GPIO_88")
				(number "106")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "GPIO_94")
				(number "90")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "GPIO_107")
				(number "102")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "GPIO_108")
				(number "101")
			)
		)
		(symbol "SE150A4_6_1"
			(text "Audio\ninterface"
				(at 0 1.27 0)
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "HS_DET")
				(number "139")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DMIC_CLK")
				(number "97")
				(alternate "GPIO_89" output line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DMIC_DATA")
				(number "98")
				(alternate "GPIO_90" bidirectional line)
			)
			(pin output line
				(at -17.78 0 0)
				(length 3.81)
				(name "MIC_BIAS1")
				(number "194")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "MIC_BIAS2")
				(number "210")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "MIC1P")
				(number "4")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "MIC2P")
				(number "6")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "MIC3P")
				(number "152")
			)
			(pin power_in line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "GND_MIC")
				(number "5")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "HPH_GND")
				(number "137")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "EAR_P")
				(number "8")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "EAR_N")
				(number "9")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "HPH_R")
				(number "136")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "HPH_L")
				(number "138")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "SPK_P")
				(number "10")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "SPK_N")
				(number "11")
			)
		)
		(symbol "SE150A4_7_1"
			(text "RF Interface"
				(at -6.35 0 900)
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 3.81)
				(name "ANT_TRX")
				(number "87")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "ANT_DRX")
				(number "131")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "ANT_GNSS")
				(number "121")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 3.81)
				(name "ANT-WIFI/BT")
				(number "77")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SIM7020E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "SIM7020E"
			(at 12.7 26.67 0)
		)
		(property "Footprint" "RF_GSM:SIMCom_SIM800C"
			(at 13.97 -26.67 0)
		)
		(property "Datasheet" "https://simcom.ee/documents/SIM7020/SIM7020%20Hardware%20Design_V1.02.pdf"
			(at -118.11 -59.69 0)
		)
		(property "Description" "NB-IoT B1/B3/B5/B8/B20/B28, AT Command Set"
			(at 0 0 0)
		)
		(property "ki_keywords" "NB-IoT Data SMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIMCom*SIM800C*"
			(at 0 0 0)
		)
		(symbol "SIM7020E_0_1")
		(symbol "SIM7020E_1_1"
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "UART1_DTR")
				(number "6")
			)
			(pin output line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "UART1_RI")
				(number "7")
			)
			(pin output line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "UART1_DCD")
				(number "5")
			)
			(pin output line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "UART1_CTS")
				(number "4")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "UART1_RTS")
				(number "3")
			)
			(pin output line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "UART1_TXD")
				(number "1")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "UART1_RXD")
				(number "2")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "UART2_TXD")
				(number "22")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "UART2_RXD")
				(number "23")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "~{PWRKEY}")
				(number "39")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "28")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "ADC")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "GPIO0")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "GPIO1")
				(number "29")
			)
			(pin power_out line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VDD_EXT")
				(number "40")
			)
			(pin power_out line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD_3V3")
				(number "9")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VBAT")
				(number "34")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VBAT")
				(number "35")
			)
			(pin no_connect line
				(at 17.78 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "ANT")
				(number "32")
			)
			(pin power_out line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "SIM_VDD")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "SIM_DATA")
				(number "15")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "SIM_CLK")
				(number "16")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "SIM_RST")
				(number "17")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "SIM_DET")
				(number "14")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "USB_VBUS")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "USB_DP")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "USB_DM")
				(number "26")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "STATUS")
				(number "42")
			)
			(pin output line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "NETLIGHT")
				(number "41")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RTC_GPIO0")
				(number "11")
			)
			(pin input line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RTC_EINT")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SIM800C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "SIM800C"
			(at 12.7 26.67 0)
		)
		(property "Footprint" "RF_GSM:SIMCom_SIM800C"
			(at 13.97 -26.67 0)
		)
		(property "Datasheet" "http://simcom.ee/documents/SIM800C/SIM800C_Hardware_Design_V1.05.pdf"
			(at -118.11 -59.69 0)
		)
		(property "Description" "GSM Quad-Band Communication Module, GPRS, Audio Engine, AT Command Set, Bluetooth is Optional"
			(at 0 0 0)
		)
		(property "ki_keywords" "GSM GPRS Quad-Band SMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIMCom*SIM800C*"
			(at 0 0 0)
		)
		(symbol "SIM800C_0_1")
		(symbol "SIM800C_1_1"
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "UART1_DTR")
				(number "6")
			)
			(pin output line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "UART1_RI")
				(number "7")
			)
			(pin output line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "UART1_DCD")
				(number "5")
			)
			(pin output line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "UART1_CTS")
				(number "4")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "UART1_RTS")
				(number "3")
			)
			(pin output line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "UART1_TXD")
				(number "1")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "UART1_RXD")
				(number "2")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "UART2_TXD")
				(number "22")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "UART2_RXD")
				(number "23")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "~{PWRKEY}")
				(number "39")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "ADC")
				(number "38")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "MICP")
				(number "9")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "MICN")
				(number "10")
			)
			(pin power_out line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VDD_EXT")
				(number "40")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VRTC")
				(number "28")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VBAT")
				(number "34")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VBAT")
				(number "35")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "GSM_ANT")
				(number "32")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "BT_ANT")
				(number "20")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RF_SYNC")
				(number "29")
			)
			(pin power_out line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "SIM_VDD")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "SIM_DATA")
				(number "15")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "SIM_CLK")
				(number "16")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "SIM_RST")
				(number "17")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "SIM_DET")
				(number "14")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "USB_VBUS")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "USB_DP")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "USB_DM")
				(number "26")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "STATUS")
				(number "42")
			)
			(pin output line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "NETLIGHT")
				(number "41")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "SPKP")
				(number "11")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "SPKN")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SIM900"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "SIM900"
			(at 8.89 39.37 0)
		)
		(property "Footprint" "RF_GSM:SIMCom_SIM900"
			(at 12.7 -39.37 0)
		)
		(property "Datasheet" "http://simcom.ee/documents/SIM900/SIM900_Hardware%20Design_V2.05.pdf"
			(at -50.8 33.02 0)
		)
		(property "Description" "GSM Quad-Band Communication Module, GPRS, Audio Engine, AT Command Set"
			(at 0 0 0)
		)
		(property "ki_keywords" "GSM GPRS Quad-Band SMS FAX"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIMCom*SIM900*"
			(at 0 0 0)
		)
		(symbol "SIM900_0_1")
		(symbol "SIM900_1_1"
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "~{RESET}")
				(number "16")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "DTR")
				(number "3")
			)
			(pin output line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "RI")
				(number "4")
			)
			(pin output line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "DCD")
				(number "5")
			)
			(pin output line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "CTS")
				(number "7")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "RTS")
				(number "8")
			)
			(pin output line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "TXD")
				(number "9")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "RXD")
				(number "10")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PWRKEY")
				(number "1")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DISP_CLK")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DISP_DATA")
				(number "12")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "DISP_D/C")
				(number "13")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DISP_CS")
				(number "14")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "NETLIGHT")
				(number "52")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "STATUS")
				(number "66")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "DBG_TXD")
				(number "27")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DBG_RXD")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "SDA")
				(number "37")
			)
			(pin output line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "SCL")
				(number "38")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "MIC_P")
				(number "19")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "MIC_N")
				(number "20")
			)
			(pin power_out line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD_EXT")
				(number "15")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VRTC")
				(number "26")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "58")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "55")
			)
			(pin passive line
				(at 5.08 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VBAT")
				(number "56")
			)
			(pin passive line
				(at 5.08 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VBAT")
				(number "57")
			)
			(pin no_connect line
				(at 15.24 33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 15.24 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 15.24 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 15.24 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin passive line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "RF_ANT")
				(number "60")
			)
			(pin power_out line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "SIM_VDD")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "SIM_DATA")
				(number "31")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "SIM_CLK")
				(number "32")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "SIM_RST")
				(number "33")
			)
			(pin input line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "SIM_PRESENCE")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "GPIO1/KBR4")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "GPIO2/KBR3")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GPIO3/KBR2")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GPIO4/KBR1")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "GPIO5/KBR0")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "GPIO6/KBC4")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "GPIO7/KBC3")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GPIO8/KBC2")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO9/KBC1")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO10")
				(number "51")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "GPIO11")
				(number "67")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GPIO12")
				(number "68")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "ADC")
				(number "25")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PWM1")
				(number "35")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PWM2")
				(number "36")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "SPK_P")
				(number "21")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "SPK_N")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UL865"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 43.18 0)
		)
		(property "Value" "UL865"
			(at 12.7 43.18 0)
		)
		(property "Footprint" "RF_GSM:Telit_xL865"
			(at 13.97 -53.34 0)
		)
		(property "Datasheet" "http://www.telit.com/fileadmin/user_upload/products/Downloads/3G/Telit_UL865_Hardware_User_Guide_r8.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "Telit 3G Module (GSM/GPRS/UMTS/HSPA), 3.8V, Digital voice and SMS, I2S, USB 2.0, UART, SPI. Manufacturer package"
			(at 0 0 0)
		)
		(property "ki_keywords" "gsm 3g gprs umts hspa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Telit*xL865*"
			(at 0 0 0)
		)
		(symbol "UL865_0_1")
		(symbol "UL865_1_1"
			(pin input line
				(at -22.86 38.1 0)
				(length 3.81)
				(name "~{RESET}")
				(number "47")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 3.81)
				(name "VUSB")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "USB_D-")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "USB_D+")
				(number "18")
			)
			(pin power_out line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "SIMVCC")
				(number "9")
			)
			(pin output line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "SIMRST")
				(number "10")
			)
			(pin output line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "SIMCLK")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "SIMIO")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "GPIO1/DVI_WA0")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GPIO2/JDR/DVI_RX")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "GPIO3/DVI_TX")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "GPIO4/DVI_CLK")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "GPIO5")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "GPIO6/SPI_SRDY")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "GPIO7/SPI_MRDY")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GPIO8/STAT_LED")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "SPI_CLK")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RXD_AUX/SPI_MISO")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "TXD_AUX/SPI_MOSI")
				(number "45")
			)
			(pin output line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "C109/DCD/GPO")
				(number "1")
			)
			(pin output line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "C125/RING/GPO")
				(number "2")
			)
			(pin output line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "C107/DSR/GPO")
				(number "3")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 3.81)
				(name "C108/DTR/GPI")
				(number "4")
			)
			(pin input line
				(at -22.86 -33.02 0)
				(length 3.81)
				(name "C105/RTS/GPI")
				(number "5")
			)
			(pin output line
				(at -22.86 -35.56 0)
				(length 3.81)
				(name "C106/CTS/GPO")
				(number "6")
			)
			(pin input line
				(at -22.86 -38.1 0)
				(length 3.81)
				(name "C103/TXD")
				(number "7")
			)
			(pin output line
				(at -22.86 -40.64 0)
				(length 3.81)
				(name "C104/RXD")
				(number "8")
			)
			(pin input line
				(at -22.86 -45.72 0)
				(length 3.81)
				(name "ADC_IN1")
				(number "13")
			)
			(pin input line
				(at -22.86 -48.26 0)
				(length 3.81)
				(name "ADC_IN2")
				(number "14")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "VBATT")
				(number "38")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 3.81)
				(name "AGND")
				(number "23")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "VBATT_PA")
				(number "37")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 2.54 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin no_connect line
				(at 19.05 -17.78 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at 19.05 -20.32 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at 19.05 -22.86 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at 19.05 -25.4 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at 19.05 -30.48 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at 19.05 -33.02 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin no_connect line
				(at 19.05 -35.56 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "48")
			)
			(pin power_out line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "VRTC")
				(number "30")
			)
			(pin power_out line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "V_AUX/PWRMON")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "ANTENNA")
				(number "34")
			)
			(pin output line
				(at 22.86 -48.26 180)
				(length 3.81)
				(name "DAC_OUT1")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BG95-M2"
		(extends "BG95-M1")
		(property "Reference" "U"
			(at -18.796 44.45 0)
		)
		(property "Value" "BG95-M2"
			(at 16.51 44.45 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BG95"
			(at 0 -57.404 0)
		)
		(property "Datasheet" "https://images.quectel.com/python/sites/2/2023/05/Quectel_BG95_Series_QuecOpen_Hardware_Design_V1.3.pdf"
			(at 0 27.94 0)
		)
		(property "Description" "NB-IoT, Cat M1 Cat NB2 Communication Module, AT Command Set"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "NB-IoT Cat M1 NB2 GNSS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel?BG95*"
			(at 0 0 0)
		)
	)
	(symbol "BG95-M3"
		(extends "BG95-M1")
		(property "Reference" "U"
			(at -18.796 44.45 0)
		)
		(property "Value" "BG95-M3"
			(at 16.51 44.45 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BG95"
			(at 0 -57.404 0)
		)
		(property "Datasheet" "https://images.quectel.com/python/sites/2/2023/05/Quectel_BG95_Series_QuecOpen_Hardware_Design_V1.3.pdf"
			(at 0 27.94 0)
		)
		(property "Description" "NB-IoT, Cat M1 Cat NB2 EGPRS Communication Module, AT Command Set"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "NB-IoT Cat M1 NB2 EGPRS GNSS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel?BG95*"
			(at 0 0 0)
		)
	)
	(symbol "BG95-M4"
		(extends "BG95-M1")
		(property "Reference" "U"
			(at -18.796 44.45 0)
		)
		(property "Value" "BG95-M4"
			(at 16.51 44.45 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BG95"
			(at 0 -57.404 0)
		)
		(property "Datasheet" "https://images.quectel.com/python/sites/2/2023/05/Quectel_BG95_Series_QuecOpen_Hardware_Design_V1.3.pdf"
			(at 0 27.94 0)
		)
		(property "Description" "NB-IoT, Cat M1  Cat NB2 Communication Module, AT Command Set"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "NB-IoT Cat M1 NB2 GNSS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel?BG95*"
			(at 0 0 0)
		)
	)
	(symbol "BG95-M5"
		(extends "BG95-M1")
		(property "Reference" "U"
			(at -18.796 44.45 0)
		)
		(property "Value" "BG95-M5"
			(at 16.51 44.45 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BG95"
			(at 0 -57.404 0)
		)
		(property "Datasheet" "https://images.quectel.com/python/sites/2/2023/05/Quectel_BG95_Series_QuecOpen_Hardware_Design_V1.3.pdf"
			(at 0 27.94 0)
		)
		(property "Description" "NB-IoT, Cat M1 NB2 EGPRS Communication Module, AT Command Set"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "NB-IoT Cat M1 NB2 EGPRS GNSS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel?BG95*"
			(at 0 0 0)
		)
	)
	(symbol "BG95-M6"
		(extends "BG95-M1")
		(property "Reference" "U"
			(at -18.796 44.45 0)
		)
		(property "Value" "BG95-M6"
			(at 16.51 44.45 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BG95"
			(at 0 -57.404 0)
		)
		(property "Datasheet" "https://images.quectel.com/python/sites/2/2023/05/Quectel_BG95_Series_QuecOpen_Hardware_Design_V1.3.pdf"
			(at 0 27.94 0)
		)
		(property "Description" "NB-IoT, Cat M1 Cat NB2 Communication Module, AT Command Set"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "NB-IoT Cat M1 NB2 GNSS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel?BG95*"
			(at 0 0 0)
		)
	)
	(symbol "BG95-M8"
		(extends "BG95-M1")
		(property "Reference" "U"
			(at -18.796 44.45 0)
		)
		(property "Value" "BG95-M8"
			(at 16.51 44.45 0)
		)
		(property "Footprint" "RF_GSM:Quectel_BG95"
			(at 0 -57.404 0)
		)
		(property "Datasheet" "https://images.quectel.com/python/sites/2/2023/05/Quectel_BG95_Series_QuecOpen_Hardware_Design_V1.3.pdf"
			(at 0 27.94 0)
		)
		(property "Description" "NB-IoT, Cat M1 Cat NB2 EGPRS Communication Module, AT Command Set"
			(at 0 27.94 0)
		)
		(property "ki_keywords" "NB-IoT Cat M1 NB2 EGPRS GNSS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Quectel?BG95*"
			(at 0 0 0)
		)
	)
	(symbol "SARA-U260"
		(extends "SARA-U201")
		(property "Reference" "U"
			(at 10.16 26.67 0)
		)
		(property "Value" "SARA-U260"
			(at -11.43 26.67 0)
		)
		(property "Footprint" "RF_GSM:ublox_SARA_LGA-96"
			(at 17.78 -26.67 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/SARA-U2_DataSheet_(UBX-13005287).pdf"
			(at 0 0 0)
		)
		(property "Description" "Ublox HSPA GSM Quad-Band Communication Module, AT Command Set, Designed for America, LGA-96"
			(at 0 0 0)
		)
		(property "ki_keywords" "GSM HSPA 2G 3G"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*SARA*"
			(at 0 0 0)
		)
	)
	(symbol "SARA-U270"
		(extends "SARA-U201")
		(property "Reference" "U"
			(at 10.16 26.67 0)
		)
		(property "Value" "SARA-U270"
			(at -11.43 26.67 0)
		)
		(property "Footprint" "RF_GSM:ublox_SARA_LGA-96"
			(at 17.78 -26.67 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/SARA-U2_DataSheet_(UBX-13005287).pdf"
			(at 0 0 0)
		)
		(property "Description" "Ublox HSPA GSM Quad-Band Communication Module, AT Command Set, Designed for Europe, Asia and Others, LGA-96"
			(at 0 0 0)
		)
		(property "ki_keywords" "GSM HSPA 2G 3G"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*SARA*"
			(at 0 0 0)
		)
	)
	(symbol "SARA-U280"
		(extends "SARA-U201")
		(property "Reference" "U"
			(at 10.16 26.67 0)
		)
		(property "Value" "SARA-U280"
			(at -11.43 26.67 0)
		)
		(property "Footprint" "RF_GSM:ublox_SARA_LGA-96"
			(at 17.78 -26.67 0)
		)
		(property "Datasheet" "https://www.u-blox.com/sites/default/files/SARA-U2_DataSheet_(UBX-13005287).pdf"
			(at 0 0 0)
		)
		(property "Description" "Ublox HSPA GSM Quad-Band Communication Module, AT Command Set, Designed for America, LGA-96"
			(at 0 0 0)
		)
		(property "ki_keywords" "GSM HSPA 2G 3G"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ublox*SARA*"
			(at 0 0 0)
		)
	)
	(symbol "SIM7020C"
		(extends "SIM7020E")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "SIM7020C"
			(at 12.7 26.67 0)
		)
		(property "Footprint" "RF_GSM:SIMCom_SIM800C"
			(at 13.97 -26.67 0)
		)
		(property "Datasheet" "https://simcom.ee/documents/SIM7020/SIM7020%20Hardware%20Design_V1.02.pdf"
			(at -118.11 -59.69 0)
		)
		(property "Description" "NB-IoT B1/B3/B5/B8, AT Command Set"
			(at 0 0 0)
		)
		(property "ki_keywords" "NB-IoT Data SMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIMCom*SIM800C*"
			(at 0 0 0)
		)
	)
)
