(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AST50147-xx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.525 11.43 0)
		)
		(property "Value" "AST50147-xx"
			(at 6.985 11.43 0)
		)
		(property "Footprint" "RF_Module:Astrocast_AST50147-00"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://docs.astrocast.com/dl/0532-DOC-M2M-ASTRO-Astronode_S-Datasheet.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "L-band satellite communication Astronode S module"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF module Astrocast radio Astronode "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Astrocast*AST50147*"
			(at 0 0 0)
		)
		(symbol "AST50147-xx_0_1")
		(symbol "AST50147-xx_1_1"
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "WAKEUP")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RESET")
				(number "14")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "24")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "34")
			)
			(pin no_connect line
				(at -7.62 10.16 270)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "20")
			)
			(pin no_connect line
				(at -5.08 10.16 270)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "21")
			)
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "22")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND_RF")
				(number "15")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND_RF")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND_RF")
				(number "18")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND_RF")
				(number "19")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "37")
			)
			(pin no_connect line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "26")
			)
			(pin no_connect line
				(at 5.08 10.16 270)
				(length 2.54)
				(hide yes)
				(name "RSVD")
				(number "38")
			)
			(pin no_connect line
				(at 5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "28")
			)
			(pin no_connect line
				(at 7.62 10.16 270)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "32")
			)
			(pin no_connect line
				(at 7.62 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "30")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "35")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "ANTN_RF")
				(number "17")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "EVENT_NOTIF")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "ANTN_USE")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMR21G18-MR210UA_NoRFPads"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 29.21 0)
		)
		(property "Value" "ATSAMR21G18-MR210UA_NoRFPads"
			(at 1.27 29.21 0)
		)
		(property "Footprint" "RF_Module:Atmel_ATSAMR21G18-MR210UA_NoRFPads"
			(at 2.54 0 90)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/atmel-42475-atsamr21g18-mr210ua_datasheet.pdf"
			(at 0 -38.1 0)
		)
		(property "Description" "RF Module, ATSAMR21, Zigbee 802.15.4, external antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Wireless Zigbee 802.15.4 ATSAMR21G18 AT45DB041E TECC508A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Atmel*ATSAMR21G18*MR210UA*NoRFPads*"
			(at 0 0 0)
		)
		(symbol "ATSAMR21G18-MR210UA_NoRFPads_1_1"
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "~{RST}")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "ATECC508_GPIO")
				(number "33")
			)
			(pin no_connect line
				(at -10.16 15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -10.16 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin no_connect line
				(at -10.16 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA07")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA08")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA12")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA16")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA17")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA18")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA19")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA22")
				(number "37")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA23")
				(number "36")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA24")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA25")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA28")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PA30")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PA31")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AX-SIP-SFEU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "AX-SIP-SFEU"
			(at 8.89 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:OnSemi_SIP-38-6EP-9x7mm_P0.65mm_EP1.2x1.2mm"
			(at 2.54 -24.13 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/AX-SIP-SFEU-D.PDF"
			(at -24.13 -31.75 0)
		)
		(property "Description" "Ultra low power, Sigfox or custom, system in package transceiver, 868Mhz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sigfox SIP 868Mhz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*SIP*6EP*9x7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AX-SIP-SFEU_0_1")
		(symbol "AX-SIP-SFEU_1_1"
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "UART_TX")
				(number "20")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "UART_RX")
				(number "21")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "25")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "RX_LED")
				(number "22")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "TX_LED")
				(number "23")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "CPULED")
				(number "17")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "RADIOLED")
				(number "18")
			)
			(pin no_connect line
				(at -15.24 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC24")
				(number "24")
			)
			(pin no_connect line
				(at -10.16 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD_IO")
				(number "27")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin no_connect line
				(at 5.08 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at 7.62 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 10.16 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "ANT")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "GPIO0/PA0")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "GPIO1/PA1")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GPIO2/PA2")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GPIO3/PA5")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "GPIO4/PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "GPIO5/PC1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "GPIO6/PC2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GPIO7/PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO8/PC4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO9/PB3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "GPIO10/PC5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GPIO11/PC6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "GPIO12/PA6")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "GPIO13/PA7")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "GPIO14/PC7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AX-SIP-SFEU-API"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "AX-SIP-SFEU-API"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:OnSemi_SIP-38-6EP-9x7mm_P0.65mm_EP1.2x1.2mm"
			(at 2.54 -24.13 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/AX-SIP-SFEU-D.PDF"
			(at -24.13 -31.75 0)
		)
		(property "Description" "Ultra low power, Sigfox or custom, programmable system in package, 868Mhz"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sigfox SIP 868Mhz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*SIP*6EP*9x7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AX-SIP-SFEU-API_0_1")
		(symbol "AX-SIP-SFEU-API_1_1"
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "UART_TX/PB4")
				(number "20")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "UART_RX/PB5")
				(number "21")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "25")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DBG_EN")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "DBG_DATA/PB6")
				(number "22")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DBG_CLK/PB7")
				(number "23")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "CPULED/PB0")
				(number "17")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "RADIOLED/PB1")
				(number "18")
			)
			(pin no_connect line
				(at -10.16 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD_IO")
				(number "27")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin no_connect line
				(at 5.08 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at 7.62 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 10.16 22.86 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "ANT")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "GPIO0/PA0")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "GPIO1/PA1")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GPIO2/PA2")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GPIO3/PA5")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "GPIO4/PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "GPIO5/PC1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "GPIO6/PC2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GPIO7/PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO8/PC4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO9/PB3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "GPIO10/PC5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GPIO11/PC6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "GPIO12/PA6")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "GPIO13/PA7")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "GPIO14/PC7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Ai-Thinker-Ra-01"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 17.78 0)
		)
		(property "Value" "Ai-Thinker-Ra-01"
			(at 13.97 -15.24 0)
		)
		(property "Footprint" "RF_Module:Ai-Thinker-Ra-01-LoRa"
			(at 25.4 -10.16 0)
		)
		(property "Datasheet" "http://wiki.ai-thinker.com/_media/lora/docs/c047ps01a1_ra-01_product_specification_v1.1.pdf"
			(at 2.54 17.78 0)
		)
		(property "Description" "Ai-Thinker Ra-01 410-525 MHz LoRa Module, SPI interface, external antenna"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ra-01 LoRa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Ai?Thinker?Ra?01*"
			(at 0 0 0)
		)
		(symbol "Ai-Thinker-Ra-01_0_1")
		(symbol "Ai-Thinker-Ra-01_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "MOSI")
				(number "14")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MISO")
				(number "13")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCK")
				(number "12")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{NSS}")
				(number "15")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "ANT")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "DIO0")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DIO1")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "DIO2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DIO3")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "DIO4")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "DIO5")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Ai-Thinker-Ra-02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 19.05 0)
		)
		(property "Value" "Ai-Thinker-Ra-02"
			(at 13.97 -15.24 0)
		)
		(property "Footprint" "RF_Module:Ai-Thinker-Ra-01-LoRa"
			(at 25.4 -10.16 0)
		)
		(property "Datasheet" "http://wiki.ai-thinker.com/_media/lora/docs/c048ps01a1_ra-02_product_specification_v1.1.pdf"
			(at 2.54 19.05 0)
		)
		(property "Description" "Ai-Thinker Ra-02 410-525 MHz LoRa Module, SPI interface, U.FL antenna connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ra-02 LoRa"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Ai?Thinker?Ra?01*"
			(at 0 0 0)
		)
		(symbol "Ai-Thinker-Ra-02_0_1")
		(symbol "Ai-Thinker-Ra-02_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "MOSI")
				(number "14")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MISO")
				(number "13")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCK")
				(number "12")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{NSS}")
				(number "15")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "DIO0")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DIO1")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "DIO2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DIO3")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "DIO4")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "DIO5")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CMWX1ZZABZ-078"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "CMWX1ZZABZ-078"
			(at 16.51 36.83 0)
		)
		(property "Footprint" "RF_Module:CMWX1ZZABZ"
			(at 0 0 0)
		)
		(property "Datasheet" "https://wireless.murata.com/RFM/data/type_abz.pdf"
			(at 62.23 -38.1 0)
		)
		(property "Description" "LoRa/SigFox Module, STM32L082 MCU, Murata CMWX1ZZABZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "iot lora sigfox"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CMWX1ZZABZ*"
			(at 0 0 0)
		)
		(symbol "CMWX1ZZABZ-078_0_1")
		(symbol "CMWX1ZZABZ-078_1_1"
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PA0/WKUP1")
				(number "33")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PA2/ADC2")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PA3/ADC3")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PA4/ADC4/DAC1")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PA5/ADC5/DAC2")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PA8/MCO")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PA9/USART1_TX")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PA10/USART1_RX")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PA11/USB_DM")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PA12/USB_DP")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PA13/SWDIO")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PA14/SWCLK")
				(number "42")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "~{MCU_RST}")
				(number "34")
			)
			(pin output line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "TCXO_OUT")
				(number "47")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PH0/OSC_IN")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PH1/OSC_OUT")
				(number "45")
			)
			(pin passive line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "~{STSAFE_RST}")
				(number "31")
			)
			(pin input line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "43")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD_USB")
				(number "4")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD_MCU")
				(number "5")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD_RF")
				(number "6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VREF+")
				(number "32")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD_TCXO")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PB2/LPTIM1_OUT")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB5/LPTIM1_IN1")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB6/LPTIM1_ETR")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB7/LPTIM1_IN2")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB8/I2C1_SCL")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB9/I2C1_SDA")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB12/SPI2_NSS")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB13/SPI2_SCK")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB14/SPI2_MISO")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PB15/SPI2_MOSI")
				(number "14")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "DBG_CRF1")
				(number "28")
			)
			(pin passive line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "DGB_CRF2")
				(number "30")
			)
			(pin passive line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "DBG_CRF3")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "DBG_SX1276_DIO0")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "DBG_SX1276_DIO1")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "DBG_SX1276_DIO2")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "DBG_SX1276_DI03")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "SX1276_DIO4")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "DBG_SX1276_DIO5")
				(number "11")
			)
			(pin passive line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "ANT")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D52MxxM8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "D52MxxM8"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "RF_Module:Garmin_M8-35_9.8x14.0mm_Layout6x6_P1.5mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "https://www.thisisant.com/assets/resources/D00001687_D52_Module_Datasheet.v.2.3_(Garmin).pdf"
			(at 2.54 -21.59 0)
		)
		(property "Description" "D52M Module, nRF52832 SoC, ARM Cortex-M4F, 64kB RAM, 512kB Flash, 1.7-3.6V, M8-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio ANT Bluetooth BLE D52 nRF52 Garmin Canada Dynastream Nordic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Garmin*M8*9.8x14.0mm*Layout6x6*P1.5mm*"
			(at 0 0 0)
		)
		(symbol "D52MxxM8_0_1")
		(symbol "D52MxxM8_1_1"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "SWDIO")
				(number "B1")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "SWDCLK")
				(number "C1")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "P021/RESET")
				(number "E6")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "P011")
				(number "F6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "P012")
				(number "B2")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "P013")
				(number "D3")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "P014")
				(number "D2")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "P015")
				(number "B3")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P016")
				(number "C4")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "P018")
				(number "D5")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P020")
				(number "B4")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P022")
				(number "D4")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P024")
				(number "D6")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "P025")
				(number "F1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "B5")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "B6")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "C5")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "C6")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "A2")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "A3")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "A4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "A5")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "A6")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P006")
				(number "E1")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P008")
				(number "D1")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "NFC1/P009")
				(number "C2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "NFC2/P010")
				(number "C3")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "AIN0/P002")
				(number "E5")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "AIN1/P003")
				(number "E3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "AIN2/P004")
				(number "E4")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "AIN3/P005")
				(number "E2")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "AIN4/P028")
				(number "F5")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "AIN5/P029")
				(number "F4")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "AIN6/P030")
				(number "F3")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "AIN7/P031")
				(number "F2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DWM1000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "DWM"
			(at -17.78 26.67 0)
		)
		(property "Value" "DWM1000"
			(at 15.875 26.67 0)
		)
		(property "Footprint" "RF_Module:DWM1000"
			(at 7.62 -26.67 0)
		)
		(property "Datasheet" "https://www.decawave.com/sites/default/files/resources/dwm1000-datasheet-v1.3.pdf"
			(at 7.62 -29.21 0)
		)
		(property "Description" "Ultra wide band RF module With ranging location capabilities"
			(at 0 0 0)
		)
		(property "ki_keywords" "Decawave Qorvo UWB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DWM1000*"
			(at 0 0 0)
		)
		(symbol "DWM1000_0_1")
		(symbol "DWM1000_1_1"
			(pin output line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "EXTON")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "WAKEUP")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "~{RST}")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "GPIO7")
				(number "4")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD3V3")
				(number "7")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD3V3")
				(number "6")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDAON")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "IRQ/GPIO8")
				(number "22")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "SPICLK")
				(number "20")
			)
			(pin output line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "SPIMISO")
				(number "19")
			)
			(pin input line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "SPIMOSI")
				(number "18")
			)
			(pin input line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "~{SPICS}")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "GPIO0/RXOKLED")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "GPIO1/SFDLED")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "GPIO2/RXLED")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "GPIO3/TXLED")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "GPIO4/EXTPA")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "GPIO5/EXTTXE/SPIPOL")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "GPIO6/EXTRXE/SPIHA")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DWM1001"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 27.94 0)
		)
		(property "Value" "DWM1001"
			(at -12.7 25.4 0)
		)
		(property "Footprint" "RF_Module:DecaWave_DWM1001"
			(at 17.78 -24.13 0)
		)
		(property "Datasheet" "https://www.decawave.com/sites/default/files/dwm1001_datasheet.pdf"
			(at 22.86 -20.32 0)
		)
		(property "Description" "Ultra wide band RF module With ranging location capabilities, I2C, UART, SPI, +2.8V to +3.6V VCC"
			(at 0 0 0)
		)
		(property "ki_keywords" "DWM1000  DecaWave RF ranging UWB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DWM1001*"
			(at 0 0 0)
		)
		(symbol "DWM1001_0_1")
		(symbol "DWM1001_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "BT_WAKE_UP")
				(number "32")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "~{RESET}")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "I2C_SDA")
				(number "14")
			)
			(pin output line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "I2C_SCL")
				(number "15")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "SWD_CLK")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "SWD_DIO")
				(number "3")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "UART_RX")
				(number "18")
			)
			(pin output line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "UART_TX")
				(number "20")
			)
			(pin output line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "SPIS_MISO")
				(number "26")
			)
			(pin tri_state line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "SPIS_MOSI")
				(number "27")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "SPIS_CLK")
				(number "28")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "~{SPIS_CS}")
				(number "29")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "READY")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "GPIO_0")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "GPIO_1")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "GPIO_2")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "GPIO_3")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "GPIO_8")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "GPIO_9")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "GPIO_10")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "GPIO_12")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "GPIO_13")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "GPIO_14")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "GPIO_15")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "GPIO_22")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "GPIO_23")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "GPIO_27")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "GPIO_30")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GPIO_31")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "E18-MS1-PCB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 21.59 0)
		)
		(property "Value" "E18-MS1-PCB"
			(at -2.54 19.05 0)
		)
		(property "Footprint" "RF_Module:E18-MS1-PCB"
			(at -5.08 5.08 0)
		)
		(property "Datasheet" "http://www.cdebyte.com/en/downpdf.aspx?id=122"
			(at -5.08 5.08 0)
		)
		(property "Description" "Zigbee RF Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Zigbee, RF, 802.15.4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "E18-MS1-PCB*"
			(at 0 0 0)
		)
		(symbol "E18-MS1-PCB_0_1")
		(symbol "E18-MS1-PCB_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "P0.0")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "P0.1")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "P0.2")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "P0.3")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "P0.4")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "P0.5")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "P0.6")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "P0.7")
				(number "16")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "P1.0")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "P1.1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "P1.2")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "P1.3")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "P1.4")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P1.5")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "P1.6")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P1.7")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "P2.0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "P2.1")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "P2.2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "E73-2G4M04S-52832"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "E73-2G4M04S-52832"
			(at 0 -1.27 0)
		)
		(property "Footprint" "RF_Module:E73-2G4M04S"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.cdebyte.com/en/downpdf.aspx?id=243"
			(at 0 11.43 0)
		)
		(property "Description" "nRF52832 BLE5 Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE5, BLE, nRF52832"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "E73*2G4M04S*"
			(at 0 0 0)
		)
		(symbol "E73-2G4M04S-52832_0_1")
		(symbol "E73-2G4M04S-52832_1_1"
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "P0.21/~{RESET}")
				(number "36")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "SWDCLK")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "SWDIO")
				(number "38")
			)
			(pin passive line
				(at -12.7 40.64 270)
				(length 2.54)
				(name "DEC1")
				(number "14")
			)
			(pin passive line
				(at -10.16 40.64 270)
				(length 2.54)
				(name "DEC2")
				(number "3")
			)
			(pin passive line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "DEC3")
				(number "4")
			)
			(pin passive line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "DEC4")
				(number "12")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "0")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin power_out line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "DCC")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "AIN0/P0.02")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "AIN1/P0.03")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "AIN2/P0.04")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "AIN3/P0.05")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "P0.06")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "P0.07")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "P0.08")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "NFC1/P0.09")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "NFC2/P0.10")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "P0.11")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "P0.12")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "P0.13")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "P0.14")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "P0.15")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "P0.16")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "P0.17")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "SWO/P0.18")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "P0.19")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "P0.20")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "P0.22")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "P0.23")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "P0.24")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "P0.25")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "P0.26")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "P0.27")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "AIN4/P0.28")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "AIN5/P0.29")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "AIN6/P0.30")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "AIN7/P0.31")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP-07"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "ESP-07"
			(at 12.7 19.05 0)
		)
		(property "Footprint" "RF_Module:ESP-07"
			(at 0 0 0)
		)
		(property "Datasheet" "http://wiki.ai-thinker.com/_media/esp8266/esp8266_series_modules_user_manual_v1.1.pdf"
			(at -8.89 2.54 0)
		)
		(property "Description" "802.11 b/g/n Wi-Fi Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "802.11 Wi-Fi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP?07*"
			(at 0 0 0)
		)
		(symbol "ESP-07_0_1")
		(symbol "ESP-07_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "ADC")
				(number "2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "GPIO0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "GPIO1/TXD")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "GPIO2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "GPIO3/RXD")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "GPIO4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "GPIO5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "GPIO12")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GPIO13")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GPIO14")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "GPIO15")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GPIO16")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP-12E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "ESP-12E"
			(at 12.7 19.05 0)
		)
		(property "Footprint" "RF_Module:ESP-12E"
			(at 0 0 0)
		)
		(property "Datasheet" "http://wiki.ai-thinker.com/_media/esp8266/esp8266_series_modules_user_manual_v1.1.pdf"
			(at -8.89 2.54 0)
		)
		(property "Description" "802.11 b/g/n Wi-Fi Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "802.11 Wi-Fi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP?12*"
			(at 0 0 0)
		)
		(symbol "ESP-12E_0_1")
		(symbol "ESP-12E_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "ADC")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CS0")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "MISO")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "GPIO9")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "GPIO10")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "MOSI")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SCLK")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "GPIO0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "GPIO1/TXD")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "GPIO2")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "GPIO3/RXD")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "GPIO4")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "GPIO5")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "GPIO12")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GPIO13")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GPIO14")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "GPIO15")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GPIO16")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP-WROOM-02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "ESP-WROOM-02"
			(at 10.16 13.97 0)
		)
		(property "Footprint" "RF_Module:ESP-WROOM-02"
			(at 15.24 -13.97 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/0c-esp-wroom-02_datasheet_en.pdf"
			(at 1.27 38.1 0)
		)
		(property "Description" "Wi-Fi Module, ESP8266EX SoC, 32-bit, 802.11b/g/n, WPA/WPA2, 2.7-3.6V, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio ESP Espressif"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP?WROOM?02*"
			(at 0 0 0)
		)
		(symbol "ESP-WROOM-02_0_1")
		(symbol "ESP-WROOM-02_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RST")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TOUT")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RXD")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "TXD")
				(number "12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IO0")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IO2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IO4")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IO5")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "IO12")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IO13")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO14")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "IO15")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "IO16")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-C3-DevKitM-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 16.51 0)
		)
		(property "Value" "ESP32-C3-DevKitM-1"
			(at 11.684 -16.764 0)
		)
		(property "Footprint" "RF_Module:ESP32-C3-DevKitM-1"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://docs.espressif.com/projects/esp-idf/en/latest/esp32c3/hw-reference/esp32c3/user-guide-devkitm-1.html"
			(at 0 -30.48 0)
		)
		(property "Description" "Development board featuring ESP32-C3-MINI-1 module"
			(at 0 -27.94 0)
		)
		(property "ki_keywords" "riscv wifi bluetooth ble"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*ESP32?C3?DevKitM?1*"
			(at 0 0 0)
		)
		(symbol "ESP32-C3-DevKitM-1_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "IO0")
				(number "9")
				(alternate "ADC1_CH0" passive line)
				(alternate "XTAL_32K_P" passive line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IO1")
				(number "10")
				(alternate "ADC1_CH1" passive line)
				(alternate "XTAL_32K_N" passive line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IO2")
				(number "4")
				(alternate "ADC1_CH0" passive line)
				(alternate "FSPIQ" passive line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "IO3")
				(number "5")
				(alternate "ADC1_CH3" passive line)
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RX")
				(number "28")
				(alternate "IO20" passive line)
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "TX")
				(number "29")
				(alternate "IO21" passive line)
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RST")
				(number "7")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(name "5V")
				(number "13")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "5V")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(hide yes)
				(name "3V3")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO4")
				(number "20")
				(alternate "ADC1_CH4" passive line)
				(alternate "FSPIHD" passive line)
				(alternate "MTMS" passive line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO5")
				(number "21")
				(alternate "ADC2_CH0" passive line)
				(alternate "FSPIWP" passive line)
				(alternate "MTDI" passive line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO6")
				(number "22")
				(alternate "FSPICLK" passive line)
				(alternate "MTCK" passive line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO7")
				(number "23")
				(alternate "FSPID" passive line)
				(alternate "MTDO" passive line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO8")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO9")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO10")
				(number "11")
				(alternate "FSPICS0" passive line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO18")
				(number "18")
				(alternate "USB_D-" passive line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO19")
				(number "17")
				(alternate "USB_D+" passive line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-C3-WROOM-02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.192 21.336 0)
		)
		(property "Value" "ESP32-C3-WROOM-02"
			(at 12.192 21.336 0)
		)
		(property "Footprint" "RF_Module:ESP32-C3-WROOM-02"
			(at 0 0.635 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3-wroom-02_datasheet_en.pdf"
			(at 0 0.635 0)
		)
		(property "Description" "802.11 b/g/n Wi­Fi and Bluetooth 5 module, ESP32­C3 SoC, RISC­V microprocessor, On-board antenna"
			(at 0 0.635 0)
		)
		(property "ki_keywords" "esp32 espressif WiFi Bluetooth LE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?C3*WROOM?02*"
			(at 0 0 0)
		)
		(symbol "ESP32-C3-WROOM-02_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IO0")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IO1")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "IO2")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IO3")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IO4")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "IO5")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "IO6")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "IO7")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IO8")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "IO9")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "IO10")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "IO18")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "IO19")
				(number "14")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "3V3")
				(number "1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IO20/RXD")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO21/TXD")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-C3-WROOM-02U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.192 21.336 0)
		)
		(property "Value" "ESP32-C3-WROOM-02U"
			(at 12.7 21.336 0)
		)
		(property "Footprint" "RF_Module:ESP32-C3-WROOM-02U"
			(at 0 -0.635 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3-wroom-02_datasheet_en.pdf"
			(at 0 -0.635 0)
		)
		(property "Description" "802.11 b/g/n Wi­Fi and Bluetooth 5 module, ESP32­C3 SoC, RISC­V microprocessor, On-board antenna"
			(at 0 -0.635 0)
		)
		(property "ki_keywords" "esp32 espressif WiFi Bluetooth LE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?C3*WROOM?02U*"
			(at 0 0 0)
		)
		(symbol "ESP32-C3-WROOM-02U_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IO0")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IO1")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "IO2")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IO3")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IO4")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "IO5")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "IO6")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "IO7")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IO8")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "IO9")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "IO10")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "IO18")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "IO19")
				(number "14")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "3V3")
				(number "1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IO20/RXD")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO21/TXD")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-C6-MINI-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "ESP32-C6-MINI-1"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "RF_Module:ESP32-C6-MINI-1"
			(at 17.78 -25.4 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c6-mini-1_mini-1u_datasheet_en.pdf"
			(at 0 36.83 0)
		)
		(property "Description" "RF Module, ESP32-C6 SoC, Wi-Fi 802.11b/g/n/ax, Bluetooth, BLE, Zigbee, Thread, 32-bit, 3.3V, SMD, onboard antenna"
			(at 0 39.37 0)
		)
		(property "ki_keywords" "Radio BT ESP Espressif"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?C6?MINI?1*"
			(at 0 0 0)
		)
		(symbol "ESP32-C6-MINI-1_0_1")
		(symbol "ESP32-C6-MINI-1_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "IO0")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IO1")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IO2")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "IO3")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IO4")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IO5")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "IO6")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "IO7")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "IO8")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IO9")
				(number "23")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at -12.7 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "3V3")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin no_connect line
				(at 12.7 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 12.7 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "TXD0")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "RXD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IO12")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IO13")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO14")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO15")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO18")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO19")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO20")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO21")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO22")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO23")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-S2-WROVER"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "ESP32-S2-WROVER"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "RF_Module:ESP32-S2-WROVER"
			(at 19.05 -29.21 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf"
			(at -7.62 -20.32 0)
		)
		(property "Description" "RF Module, ESP32-D0WDQ6 SoC, Wi-Fi 802.11b/g/n, 32-bit, 2.7-3.6V, onboard antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio ESP ESP32 Espressif onboard PCB antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?S2?WROVER*"
			(at 0 0 0)
		)
		(symbol "ESP32-S2-WROVER_0_1")
		(symbol "ESP32-S2-WROVER_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "EN")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "IO00")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "IO01")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "IO02")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "IO03")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IO04")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IO05")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "IO06")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IO07")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IO08")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "IO09")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "IO10")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "IO11")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IO12")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "IO13")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "IO14")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "IO15")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "IO16")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "IO17")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "IO18")
				(number "21")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin input line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IO46")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "IO45")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "RXD0")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "TXD0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO42")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IO41")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IO40")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO39")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO38")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO37")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO36")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO35")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO34")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO33")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO26")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO21")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "USB_D+")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "USB_D-")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-S3-MINI-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 29.21 0)
		)
		(property "Value" "ESP32-S3-MINI-1"
			(at 12.7 29.21 0)
		)
		(property "Footprint" "RF_Module:ESP32-S2-MINI-1"
			(at 15.24 -29.21 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s3-mini-1_mini-1u_datasheet_en.pdf"
			(at 0 40.64 0)
		)
		(property "Description" "RF Module, ESP32-S3 SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 3.3V, SMD, onboard antenna"
			(at 0 43.18 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32-S3 Espressif"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?S*MINI?1"
			(at 0 0 0)
		)
		(symbol "ESP32-S3-MINI-1_0_1")
		(symbol "ESP32-S3-MINI-1_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "EN")
				(number "45")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "IO0")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "IO1")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "IO2")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IO3")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IO4")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "IO5")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IO6")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IO7")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "IO8")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "IO9")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "IO10")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IO11")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "IO12")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "IO13")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "IO14")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "IO15")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "IO16")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "IO17")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "IO18")
				(number "22")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "3")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "58")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "TXD0")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "RXD0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "USB_D-")
				(number "23")
				(alternate "IO19" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "USB_D+")
				(number "24")
				(alternate "IO20" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IO21")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IO26")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO33")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO34")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO35")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO36")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO37")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO38")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO39")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO40")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO41")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "IO42")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "IO45")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "IO46")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "IO47")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "IO48")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-S3-WROOM-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ESP32-S3-WROOM-1"
			(at 12.7 26.67 0)
		)
		(property "Footprint" "RF_Module:ESP32-S3-WROOM-1"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s3-wroom-1_wroom-1u_datasheet_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "RF Module, ESP32-S3 SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 3.3V, onboard antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32-S3 Espressif onboard PCB antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?S3?WROOM?1*"
			(at 0 0 0)
		)
		(symbol "ESP32-S3-WROOM-1_0_0"
			(text "PSRAM"
				(at 5.08 2.54 900)
			)
		)
		(symbol "ESP32-S3-WROOM-1_0_1")
		(symbol "ESP32-S3-WROOM-1_1_1"
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "IO0")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "IO1")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IO2")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IO3")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "IO4")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IO5")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IO6")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "IO7")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "IO8")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "IO9")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IO10")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "IO11")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "IO12")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "IO13")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "IO14")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "IO15")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "IO16")
				(number "9")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "TXD0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "RXD0")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IO17")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO18")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "USB_D-")
				(number "13")
				(alternate "IO19" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "USB_D+")
				(number "14")
				(alternate "IO20" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO21")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO35")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO36")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO37")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO38")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO39")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO40")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO41")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO42")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "IO45")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "IO46")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "IO47")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "IO48")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-S3-WROOM-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 45.72 0)
		)
		(property "Value" "ESP32-S3-WROOM-2"
			(at 2.54 45.72 0)
		)
		(property "Footprint" "RF_Module:ESP32-S3-WROOM-2"
			(at 0 -60.96 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s3-wroom-2_datasheet_en.pdf"
			(at 0 -63.5 0)
		)
		(property "Description" "RF Module, 2.4 GHz, Wi­-Fi, Bluetooth, BLE, ESP32­-S3R8V"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bluetooth WiFi Wi-Fi ESP WROOM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?S3?WROOM?2*"
			(at 0 0 0)
		)
		(symbol "ESP32-S3-WROOM-2_0_1")
		(symbol "ESP32-S3-WROOM-2_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at -10.16 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at -10.16 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "IO0")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "IO1")
				(number "39")
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "IO2")
				(number "38")
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "IO3")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "IO4")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "IO5")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "IO6")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "IO7")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "IO8")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "IO9")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IO10")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IO11")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IO12")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IO13")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IO14")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IO15")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "IO16")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IO17")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO18")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "USB_D-/IO19")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "USB_D+/IO20")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "IO21")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "IO38")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "MTCK/IO39")
				(number "32")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "MTDO/IO40")
				(number "33")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "MTDI/IO41")
				(number "34")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "MTMS/IO42")
				(number "35")
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "TXD0/IO43")
				(number "37")
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "RXD0/IO44")
				(number "36")
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "IO45")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "IO46")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "IO47")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "IO48")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-WROOM-32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ESP32-WROOM-32"
			(at 1.27 34.29 0)
		)
		(property "Footprint" "RF_Module:ESP32-WROOM-32"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf"
			(at -7.62 1.27 0)
		)
		(property "Description" "RF Module, ESP32-D0WDQ6 SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif onboard PCB antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?WROOM?32*"
			(at 0 0 0)
		)
		(symbol "ESP32-WROOM-32_0_1")
		(symbol "ESP32-WROOM-32_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "SENSOR_VP")
				(number "4")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SENSOR_VN")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SDO/SD0")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SDI/SD1")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SHD/SD2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SWP/SD3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SCK/CLK")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SCS/CMD")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "IO0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "TXD0/IO1")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IO2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "RXD0/IO3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "IO4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IO5")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO12")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IO13")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IO14")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO15")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO16")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO17")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO18")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO19")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO21")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO22")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO23")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO25")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "IO26")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "IO27")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "IO32")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "IO33")
				(number "9")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "IO34")
				(number "6")
			)
			(pin input line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "IO35")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-WROOM-32E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ESP32-WROOM-32E"
			(at 1.27 34.29 0)
		)
		(property "Footprint" "RF_Module:ESP32-WROOM-32D"
			(at 16.51 -34.29 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "RF Module, ESP32-D0WD-V3 SoC, without PSRAM, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif onboard PCB antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?WROOM?32D*"
			(at 0 0 0)
		)
		(symbol "ESP32-WROOM-32E_0_1")
		(symbol "ESP32-WROOM-32E_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "SENSOR_VP")
				(number "4")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SENSOR_VN")
				(number "5")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "IO0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "TXD0/IO1")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IO2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "RXD0/IO3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "IO4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IO5")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO12")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IO13")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IO14")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO15")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO16")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO17")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO18")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO19")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO21")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO22")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO23")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO25")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "IO26")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "IO27")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "IO32")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "IO33")
				(number "9")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "IO34")
				(number "6")
			)
			(pin input line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "IO35")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-WROOM-32E-R2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ESP32-WROOM-32E-R2"
			(at 1.27 34.29 0)
		)
		(property "Footprint" "RF_Module:ESP32-WROOM-32D"
			(at 16.51 -34.29 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "RF Module, ESP32-D0WDR2-V3 SoC, with 2MB PSRAM, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif onboard PCB antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?WROOM?32D*"
			(at 0 0 0)
		)
		(symbol "ESP32-WROOM-32E-R2_0_1")
		(symbol "ESP32-WROOM-32E-R2_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "SENSOR_VP")
				(number "4")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SENSOR_VN")
				(number "5")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "IO0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "TXD0/IO1")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IO2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "RXD0/IO3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "IO4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IO5")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO12")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IO13")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IO14")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO15")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO17")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO18")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO19")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO21")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO22")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO23")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO25")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "IO26")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "IO27")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "IO32")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "IO33")
				(number "9")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "IO34")
				(number "6")
			)
			(pin input line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "IO35")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-WROOM-32U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ESP32-WROOM-32U"
			(at 1.27 34.29 0)
		)
		(property "Footprint" "RF_Module:ESP32-WROOM-32U"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32d_esp32-wroom-32u_datasheet_en.pdf"
			(at -7.62 1.27 0)
		)
		(property "Description" "RF Module, ESP32-D0WD SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, external antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif external U.FL antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?WROOM?32U*"
			(at 0 0 0)
		)
		(symbol "ESP32-WROOM-32U_0_1")
		(symbol "ESP32-WROOM-32U_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "SENSOR_VP")
				(number "4")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SENSOR_VN")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SDO/SD0")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SDI/SD1")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SHD/SD2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SWP/SD3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SCK/CLK")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SCS/CMD")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "IO0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "TXD0/IO1")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IO2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "RXD0/IO3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "IO4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IO5")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO12")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IO13")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IO14")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO15")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO16")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO17")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO18")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO19")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO21")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO22")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO23")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO25")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "IO26")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "IO27")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "IO32")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "IO33")
				(number "9")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "IO34")
				(number "6")
			)
			(pin input line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "IO35")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HT-CT62"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "HT-CT62"
			(at 10.16 17.78 0)
		)
		(property "Footprint" "RF_Module:Heltec_HT-CT62"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://resource.heltec.cn/download/HT-CT62/HT-CT62(Rev1.1).pdf"
			(at 0 0 0)
		)
		(property "Description" "LoRa/LoRaWAN node module with ESP32-C3 and SX1262"
			(at 0 0 0)
		)
		(property "ki_keywords" "LoRa WiFi ESP32 SX1262"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HT?CT62*"
			(at 0 0 0)
		)
		(symbol "HT-CT62_1_1"
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "GPIO0")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "GPIO1")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "GPIO2")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "GPIO3")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "GPIO4")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "GPIO5")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "GPIO6")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "GPIO7")
				(number "3")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "EN")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "2.4G_Ant")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "LoRa_Ant")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "GPIO8")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "GPIO9")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "GPIO10")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO18_DN")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO19_DP")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "GPIO20_RXD")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GPIO21_TXD")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Jadak_Thingmagic_M6e-Nano"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "Jadak_Thingmagic_M6e-Nano"
			(at 15.24 13.97 0)
		)
		(property "Footprint" "RF_Module:Jadak_Thingmagic_M6e-Nano"
			(at 20.32 -14.224 0)
		)
		(property "Datasheet" "https://www.jadaktech.com/product/thingmagic-m6e-nano-uhf-rain-rfid"
			(at -0.254 -19.304 0)
		)
		(property "Description" "RFID UHF module, 1 antenna port, 27dBm, edge pin connections"
			(at 0.508 -17.018 0)
		)
		(property "ki_keywords" "Jadak Thingmagic M6e Nano"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Thingmagic*M6e?Nano*"
			(at 0 0 0)
		)
		(symbol "Jadak_Thingmagic_M6e-Nano_0_1")
		(symbol "Jadak_Thingmagic_M6e-Nano_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "UART_RX")
				(number "21")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "UART_TX")
				(number "20")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "EN")
				(number "11")
			)
			(pin no_connect line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "RFU1")
				(number "22")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "RFU2")
				(number "23")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "RFU3")
				(number "24")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "RFU4")
				(number "25")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "RFU5")
				(number "26")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "Vin")
				(number "16")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "RFU6")
				(number "27")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "RFU7")
				(number "28")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "RF")
				(number "39")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GPIO1")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "GPIO3")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "GPIO4")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MDBT42Q-512K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 40.64 0)
		)
		(property "Value" "MDBT42Q-512K"
			(at 10.16 40.64 0)
		)
		(property "Footprint" "RF_Module:Raytac_MDBT42Q"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.raytac.com/download/index.php?index_id=27"
			(at 0 -2.54 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52832 module, ceramic antenna"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE ANT 2.4GHz 802.15.4 MDBT42Q"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Raytac?MDBT42Q*"
			(at 0 0 0)
		)
		(symbol "MDBT42Q-512K_0_1")
		(symbol "MDBT42Q-512K_1_1"
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "P0.00/XL1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "P0.01/XL2")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "P0.21/~{RESET}")
				(number "35")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "SWDCLK")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "SWDIO")
				(number "37")
			)
			(pin power_out line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "DEC4")
				(number "9")
			)
			(pin power_out line
				(at 0 40.64 270)
				(length 2.54)
				(name "DCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "AIN0/P0.02")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "AIN1/P0.03")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "AIN2/P0.04")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "AIN3/P0.05")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "P0.06")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "P0.07")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "P0.08")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "NFC1/P0.09")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "NFC2/P0.10")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "P0.11")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "P0.12")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "P0.13")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "TRACEDATA3/P0.14")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "TRACEDATA2/P0.15")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "TRACEDATA1/P0.16")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "P0.17")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "TRACEDATA0/P0.18")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "P0.19")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "TRACECLK/P0.20")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "P0.22")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "P0.23")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "P0.24")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "P0.25")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "P0.26")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "P0.27")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "AIN4/P0.28")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "AIN5/P0.29")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "AIN6/P0.30")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "AIN7/P0.31")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MDBT50Q-1MV2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "MDBT50Q-1MV2"
			(at 0 -2.54 0)
		)
		(property "Footprint" "RF_Module:Raytac_MDBT50Q"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.raytac.com/download/index.php?index_id=43"
			(at 0 -5.08 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE ANT ZigBee Thread 802.15.4 nRF52840 nordic MDBT50Q"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Raytac?MDBT50Q*"
			(at 0 0 0)
		)
		(symbol "MDBT50Q-1MV2_0_1")
		(symbol "MDBT50Q-1MV2_1_1"
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "SWDIO")
				(number "51")
			)
			(pin input line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "SWDCLK")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "P0.02")
				(number "11")
				(alternate "AIN0" input line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "P0.03")
				(number "9")
				(alternate "AIN1" input line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "P0.04")
				(number "20")
				(alternate "AIN2" input line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "P0.05")
				(number "21")
				(alternate "AIN3" input line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "P0.28")
				(number "13")
				(alternate "AIN4" input line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "P0.29")
				(number "10")
				(alternate "AIN5" input line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "P0.30")
				(number "14")
				(alternate "AIN6" input line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "P0.31")
				(number "12")
				(alternate "AIN7" input line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "P0.09")
				(number "52")
				(alternate "NFC1" input line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "P0.10")
				(number "54")
				(alternate "NFC2" input line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "D-")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "D+")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "P1.01")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "P1.02")
				(number "50")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "P1.03")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "P1.04")
				(number "56")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "P1.05")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "P1.06")
				(number "57")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "P1.07")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "P1.08")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "P1.10")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "P1.11")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "P1.12")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "P1.13")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "P1.14")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "P1.15")
				(number "8")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDH")
				(number "30")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VBUS")
				(number "32")
			)
			(pin power_out line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "DCCH")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "P0.00")
				(number "17")
				(alternate "XL1" input line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "P0.01")
				(number "18")
				(alternate "XL2" input line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "P0.06")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "P0.08")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "P0.13")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "P0.14")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "P0.15")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "P0.16")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "P0.17")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "P0.18")
				(number "40")
				(alternate "~{RESET}" input line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "P0.19")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "P0.20")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "P0.21")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "P0.22")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "P0.23")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "P0.24")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "P0.25")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "P0.26")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "P0.27")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "P1.00")
				(number "47")
				(alternate "TRACEDATA0" output line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "P0.12")
				(number "29")
				(alternate "TRACEDATA1" output line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "P0.11")
				(number "27")
				(alternate "TRACEDATA2" output line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "P1.09")
				(number "26")
				(alternate "TRACEDATA3" output line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "P0.07")
				(number "23")
				(alternate "TRACECLK" output line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MDBT50Q-512K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "MDBT50Q-512K"
			(at 0 -2.54 0)
		)
		(property "Footprint" "RF_Module:Raytac_MDBT50Q"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.raytac.com/download/index.php?index_id=46"
			(at 0 -5.08 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52833 module"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU, ARM, BLE, ANT, 2.4GHz, 802.15.4 MDBT50Q"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Raytac?MDBT50Q*"
			(at 0 0 0)
		)
		(symbol "MDBT50Q-512K_0_1")
		(symbol "MDBT50Q-512K_1_1"
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "SWDIO")
				(number "51")
			)
			(pin input line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "SWDCLK")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "P0.02")
				(number "11")
				(alternate "AIN0" input line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "P0.03")
				(number "9")
				(alternate "AIN1" input line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "P0.04")
				(number "20")
				(alternate "AIN2" input line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "P0.05")
				(number "21")
				(alternate "AIN3" input line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "P0.28")
				(number "13")
				(alternate "AIN4" input line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "P0.29")
				(number "10")
				(alternate "AIN5" input line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "P0.30")
				(number "14")
				(alternate "AIN6" input line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "P0.31")
				(number "12")
				(alternate "AIN7" input line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "P0.09")
				(number "52")
				(alternate "NFC1" input line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "P0.10")
				(number "54")
				(alternate "NFC2" input line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "D-")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "D+")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "P0.19")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "P0.23")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "P0.25")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "P1.01")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "P1.02")
				(number "50")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "P1.03")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "P1.04")
				(number "56")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "P1.05")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "P1.06")
				(number "57")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "P1.07")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "P1.08")
				(number "25")
			)
			(pin no_connect line
				(at -17.78 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDH")
				(number "30")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VBUS")
				(number "32")
			)
			(pin no_connect line
				(at 5.08 43.18 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin no_connect line
				(at 17.78 40.64 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "60")
			)
			(pin no_connect line
				(at 17.78 38.1 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "59")
			)
			(pin no_connect line
				(at 17.78 0 180)
				(length 2.54)
				(hide yes)
				(name "P0.19")
				(number "42")
			)
			(pin no_connect line
				(at 17.78 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "45")
			)
			(pin no_connect line
				(at 17.78 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "P0.00")
				(number "17")
				(alternate "XL1" input line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "P0.01")
				(number "18")
				(alternate "XL2" input line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "P0.06")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "P0.08")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "P0.13")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "P0.14")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "P0.15")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "P0.16")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "P0.17")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "P0.18")
				(number "40")
				(alternate "~{RESET}" input line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "P0.20")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "P0.21")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "P0.22")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "P0.24")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "P0.26")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "P0.27")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "P1.00")
				(number "47")
				(alternate "TRACEDATA0" output line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "P0.12")
				(number "29")
				(alternate "TRACEDATA1" output line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "P0.11")
				(number "27")
				(alternate "TRACEDATA2" output line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "P1.09")
				(number "26")
				(alternate "TRACEDATA3" output line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "P0.07")
				(number "23")
				(alternate "TRACECLK" output line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MM002"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 21.59 0)
		)
		(property "Value" "MM002"
			(at 24.13 21.59 0)
		)
		(property "Footprint" ""
			(at -13.97 -27.94 0)
		)
		(property "Datasheet" "http://www.nemeus.fr/resources/uploads/2015/04/MM002-xx-EU_datasheet_v0.11.pdf"
			(at -13.97 -27.94 0)
		)
		(property "Description" "NEMEUS Modem dual-mode LoRa/SIGFOX"
			(at 0 0 0)
		)
		(property "ki_keywords" "IOT LoRa SIGFOX"
			(at 0 0 0)
		)
		(symbol "MM002_0_1")
		(symbol "MM002_1_1"
			(pin input line
				(at -30.48 17.78 0)
				(length 2.54)
				(name "BOOT")
				(number "5")
			)
			(pin input line
				(at -30.48 15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 2.54)
				(name "PA14-IO/JTCK/SWCLK")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 2.54)
				(name "PA13-IO/JTMS/SWDAT")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 2.54)
				(name "PB3-IO/JTDO")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 2.54)
				(name "PA15-IO/JTDI")
				(number "10")
			)
			(pin input line
				(at -30.48 0 0)
				(length 2.54)
				(name "PB4-IO/NJTRST")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 2.54)
				(name "PA11-IO/UART1-CTS/USB-DM")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 2.54)
				(name "PA12-IO/UART1-RTS/USB-DP")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 2.54)
				(name "PB6-IO/UART1-TX")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 2.54)
				(name "PB7-IO/UART1-RX")
				(number "6")
			)
			(pin power_in line
				(at -15.24 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "27")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 2.54)
				(name "PA0-IO/ADC/UART2-CTS/WKUP")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 2.54)
				(name "PA1-IO/ADC/UART2-RTS")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 2.54)
				(name "PA2-IO/ADC/UART2-TX")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 2.54)
				(name "PA3-IO/ADC/UART2-RX")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 2.54)
				(name "PB8-IO/I2C-SCL")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 2.54)
				(name "PB9-IO/I2C-SDA")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 2.54)
				(name "PA4-IO/SPI-NSS")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 2.54)
				(name "PA5-IO/SPI-SCK")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 2.54)
				(name "PA6-IO/SPI-MISO")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 2.54)
				(name "PA7-IO/SPI-MOSI")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 2.54)
				(name "ANT")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Particle_P1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 46.99 0)
		)
		(property "Value" "Particle_P1"
			(at -24.13 49.53 0)
		)
		(property "Footprint" "RF_Module:Particle_P1"
			(at 0 0 0)
		)
		(property "Datasheet" "https://docs.particle.io/datasheets/p1-datasheet/"
			(at 0 0 0)
		)
		(property "Description" "Wi-Fi module, 1MB flash, 128KB RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "Wi-Fi module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Particle*P1*"
			(at 0 0 0)
		)
		(symbol "Particle_P1_1_1"
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "MICRO_GPIO_1/PB0")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "MICRO_GPIO_2/PB1")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "MICRO_GPIO_3/PC0")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "MICRO_GPIO_5/PC3")
				(number "43")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "MICRO_GPIO_6/PC4")
				(number "44")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "MICRO_GPIO_7/PB5")
				(number "45")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "MICRO_GPIO_8/PC7")
				(number "46")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "MICRO_GPIO_9/PC13")
				(number "47")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "MICRO_GPIO_12/PC1")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "MICRO_GPIO_13/PC2")
				(number "49")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "MICRO_GPIO_14/PC5")
				(number "50")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "MICRO_SPI1_MISO/PA6")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "MICRO_SPI1_SCK/PA5")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "MICRO_SPI1_MOSI/PA7")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "MICRO_SPI1_SS/PA4")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "MICRO_I2C1_SCL/PB6")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "MICRO_I2C1_SDA/PB7")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "MICRO_UART2_RTS/PA1")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "MICRO_UART2_CTS/PA0")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "MICRO_UART2_RXD/PA3")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "MICRO_UART2_TXD/PA2")
				(number "32")
			)
			(pin no_connect line
				(at -25.4 40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -25.4 38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -25.4 35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -25.4 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "PAD1")
				(number "74")
			)
			(pin no_connect line
				(at -25.4 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "PAD2")
				(number "75")
			)
			(pin power_in line
				(at -22.86 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -20.32 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at -17.78 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at -15.24 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at -12.7 48.26 270)
				(length 2.54)
				(name "WL_REG_ON")
				(number "7")
			)
			(pin power_in line
				(at -12.7 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at -10.16 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDD_3V3")
				(number "26")
			)
			(pin power_in line
				(at -7.62 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "28")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD_3V3")
				(number "27")
			)
			(pin power_in line
				(at -5.08 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO_3V3_WL")
				(number "5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "59")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VBAT_WL")
				(number "2")
			)
			(pin power_in line
				(at 5.08 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "66")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VBAT_WL")
				(number "3")
			)
			(pin power_in line
				(at 7.62 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "67")
			)
			(pin power_in line
				(at 10.16 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "68")
			)
			(pin power_in line
				(at 12.7 48.26 270)
				(length 2.54)
				(name "VBAT_MICRO")
				(number "38")
			)
			(pin power_in line
				(at 12.7 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 15.24 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "70")
			)
			(pin power_in line
				(at 17.78 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "71")
			)
			(pin power_in line
				(at 20.32 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "72")
			)
			(pin power_in line
				(at 22.86 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "73")
			)
			(pin no_connect line
				(at 25.4 40.64 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 25.4 38.1 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 25.4 35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "MICRO_UART1_RTS/PA12")
				(number "61")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "MICRO_UART1_CTS/PA11")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "MICRO_UART1_RXD/PA10")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "MICRO_UART1_TXD/PA9")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "MICRO_JTAG_~{TRST}/PB4")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "MICRO_JTAG_TDO/PB3")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "MICRO_JTAG_TDI/PA15")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "MICRO_JTAG_TMS/PA13")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "MICRO_JTAG_TCK/PA14")
				(number "55")
			)
			(pin input line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "WL_JTAG_TDI")
				(number "16")
			)
			(pin input line
				(at 27.94 0 180)
				(length 2.54)
				(name "WL_JTAG_TCK")
				(number "17")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "WL_JTAG_~{TRST}")
				(number "18")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "WL_JTAG_TMS")
				(number "19")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "WL_JTAG_TDO")
				(number "20")
			)
			(pin input line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "BTCX_STATUS")
				(number "56")
			)
			(pin input line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "BTCX_RF_ACTIVE")
				(number "57")
			)
			(pin output line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "BTCX_TXCONF")
				(number "58")
			)
			(pin input line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "WL_SLEEP_CLK")
				(number "60")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "TESTMODE")
				(number "33")
			)
			(pin input line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "MICRO_~{RST}")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAK4200"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 27.94 0)
		)
		(property "Value" "RAK4200"
			(at 0 25.4 0)
		)
		(property "Footprint" "RF_Module:RAK4200"
			(at 5.08 7.62 0)
		)
		(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK4200/Hardware-Specification/RAK4200_Module_Specifications_V1.4.pdf"
			(at 5.08 7.62 0)
		)
		(property "Description" "LoRa Module, STM32L071,  RAKwireless"
			(at 0 0 0)
		)
		(property "ki_keywords" "IoT, LoRa, LoRaWAN, RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RAK4200*"
			(at 0 0 0)
		)
		(symbol "RAK4200_0_1")
		(symbol "RAK4200_1_1"
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PA1/UART2_DE")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PA2/UART2_TX")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PA3/UART2_RX")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PA5/SPI_CLK")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PA6/SPI_MISO")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PA7/SPI_MOSI")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PA9/UART1_TX")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PA10/UART1_RX")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PA12/UART1_DE")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PA13/SWDIO")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PA14/SWCLK")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "~{MCU_NRESET}")
				(number "18")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "I2C_SCL/PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "I2C_SDA/PB7")
				(number "10")
			)
			(pin passive line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RF")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAK811-HF-EU868"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 31.75 0)
		)
		(property "Value" "RAK811-HF-EU868"
			(at 0 27.94 0)
		)
		(property "Footprint" "RF_Module:RAK811"
			(at -11.43 31.75 0)
		)
		(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf"
			(at -11.43 31.75 0)
		)
		(property "Description" "LoRa Module, STM32L151, EU868, RAKwireless"
			(at 0 0 0)
		)
		(property "ki_keywords" "IoT LoRa LoRaWAN RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RAK811*"
			(at 0 0 0)
		)
		(symbol "RAK811-HF-EU868_0_0"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA0")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA1")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA2")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA8")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA9/USART1_TX")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PA10/USART1_RX")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PA12")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PA13")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PA14")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PA15")
				(number "14")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "24")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "BOOT0")
				(number "17")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB4")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB5")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB8")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB9")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB10")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB11")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB12")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB14")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB15")
				(number "4")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RF_OUT")
				(number "33")
			)
		)
		(symbol "RAK811-HF-EU868_0_1")
		(embedded_fonts no)
	)
	(symbol "RAK811-LF-EU433"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 31.75 0)
		)
		(property "Value" "RAK811-LF-EU433"
			(at 0 27.94 0)
		)
		(property "Footprint" "RF_Module:RAK811"
			(at -11.43 31.75 0)
		)
		(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf"
			(at -11.43 31.75 0)
		)
		(property "Description" "LoRa Module, STM32L151, EU433, RAKwireless"
			(at 0 0 0)
		)
		(property "ki_keywords" "IoT LoRa LoRaWAN RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RAK811*"
			(at 0 0 0)
		)
		(symbol "RAK811-LF-EU433_0_0"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA0")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA1")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA2")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA3")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA9/USART1_TX")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PA10/USART1_RX")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PA11")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PA12")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PA13")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PA14")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PA15")
				(number "14")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "24")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "BOOT0")
				(number "17")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB5")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB6")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB7")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB10")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB11")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB12")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB13")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB14")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB15")
				(number "4")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RF_OUT")
				(number "33")
			)
		)
		(symbol "RAK811-LF-EU433_0_1")
		(embedded_fonts no)
	)
	(symbol "RFM69HW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 11.43 0)
		)
		(property "Value" "RFM69HW"
			(at -7.62 13.97 0)
		)
		(property "Footprint" "RF_Module:HOPERF_RFM69HW"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbb56f1fd7.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "ISM Radio Transceiver Module, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "Radio ISM Transceiver Module AES"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM69HW*"
			(at 0 0 0)
		)
		(symbol "RFM69HW_0_1")
		(symbol "RFM69HW_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCK")
				(number "12")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MISO")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MOSI")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "NSS")
				(number "15")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RESET")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "3.3V")
				(number "8")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "ANA")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DIO0")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DIO1")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DIO2")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DIO3")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DIO4")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DIO5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RFM95W-868S2"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.414 11.684 0)
		)
		(property "Value" "RFM95W-868S2"
			(at 1.524 11.43 0)
		)
		(property "Footprint" ""
			(at -83.82 41.91 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf"
			(at -83.82 41.91 0)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low power long range transceiver module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM9XW*"
			(at 0 0 0)
		)
		(symbol "RFM95W-868S2_0_1")
		(symbol "RFM95W-868S2_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCK")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MOSI")
				(number "3")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MISO")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "NSS")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RESET")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "3.3V")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "ANT")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DIO5")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DIO4")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DIO3")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DIO2")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DIO1")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "DIO0")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32WB5MMG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 59.69 0)
		)
		(property "Value" "STM32WB5MMG"
			(at 10.16 -59.69 0)
		)
		(property "Footprint" "RF_Module:ST-SiP-LGA-86-11x7.3mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb5mmg.pdf"
			(at 0 0 0)
		)
		(property "Description" "ST Microelectronics STM32WB55VG ARM Cortex Bluetooth Low Energy 5.0, Zigbee and 802.15.4 module, 1 MB Flash, 256kb RAM, Fully integrated BOM"
			(at 0 0 0)
		)
		(property "ki_keywords" "bluetooth bluetooth5 bluetooth5.0 802.15.4 zigbee module stm32 rf ARM Cortex-M3 Cortex-M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RF?Module:ST?SiP?LGA?86?11x7.3mm*"
			(at 0 0 0)
		)
		(symbol "STM32WB5MMG_1_1"
			(pin bidirectional line
				(at -12.7 45.72 0)
				(length 2.54)
				(name "PH3-BOOT0")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 43.18 0)
				(length 2.54)
				(name "PH1")
				(number "62")
			)
			(pin bidirectional line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "PH0")
				(number "61")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PE4")
				(number "42")
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PE3")
				(number "72")
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PE2")
				(number "78")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PE1")
				(number "64")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "PE0")
				(number "79")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD0")
				(number "33")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD1")
				(number "34")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD2")
				(number "68")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PD3")
				(number "70")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PD4")
				(number "73")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PD5")
				(number "80")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PD6")
				(number "81")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PD7")
				(number "67")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PD8")
				(number "75")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "74")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "77")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PD11")
				(number "82")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PD12")
				(number "66")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PD13")
				(number "65")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PD14")
				(number "63")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PD15")
				(number "76")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PC0")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PC1")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PC2")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PC3")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PC4")
				(number "49")
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PC5")
				(number "45")
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "PC6")
				(number "36")
			)
			(pin bidirectional line
				(at -12.7 -40.64 0)
				(length 2.54)
				(name "PC7")
				(number "71")
			)
			(pin bidirectional line
				(at -12.7 -43.18 0)
				(length 2.54)
				(name "PC8")
				(number "83")
			)
			(pin bidirectional line
				(at -12.7 -45.72 0)
				(length 2.54)
				(name "PC9")
				(number "69")
			)
			(pin bidirectional line
				(at -12.7 -48.26 0)
				(length 2.54)
				(name "PC10")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -50.8 0)
				(length 2.54)
				(name "PC11")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 -53.34 0)
				(length 2.54)
				(name "PC12")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 -55.88 0)
				(length 2.54)
				(name "PC13")
				(number "40")
			)
			(pin input line
				(at -5.08 60.96 270)
				(length 2.54)
				(name "VREF")
				(number "4")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 2.54)
				(name "VDDA")
				(number "6")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 2.54)
				(name "VBAT")
				(number "15")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "57")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "60")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "84")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "86")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 2.54)
				(name "VDDUSB")
				(number "32")
			)
			(pin no_connect line
				(at 10.16 -45.72 180)
				(length 2.54)
				(hide yes)
				(name "ANT_NC")
				(number "85")
			)
			(pin bidirectional line
				(at 12.7 45.72 180)
				(length 2.54)
				(name "PA0")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 43.18 180)
				(length 2.54)
				(name "PA1")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA2")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA3")
				(number "56")
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA4")
				(number "55")
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA5")
				(number "54")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA6")
				(number "53")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA7")
				(number "52")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA8")
				(number "50")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA9")
				(number "51")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA10")
				(number "28")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA11")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA13")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA14")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA15")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "44")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PB1")
				(number "43")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "39")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB8")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB9")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB10")
				(number "47")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB11")
				(number "46")
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB12")
				(number "41")
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB13")
				(number "35")
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB14")
				(number "37")
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB15")
				(number "38")
			)
			(pin passive line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "ANT_IN")
				(number "58")
			)
			(pin passive line
				(at 12.7 -43.18 180)
				(length 2.54)
				(name "RF_OUT")
				(number "59")
			)
			(pin input line
				(at 12.7 -50.8 180)
				(length 2.54)
				(name "NRST")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TD1205"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "TD1205"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "RF_Module:TD1205"
			(at 11.43 -8.89 0)
		)
		(property "Datasheet" "https://github.com/Telecom-Design/Documentation_TD_RF_Module/blob/master/TD1205%20Datasheet.pdf"
			(at -6.35 -35.56 0)
		)
		(property "Description" "High-Performance, Low-Current SIGFOX™ Gateway And GPS Receiver With Integrated Antennas"
			(at 0 0 0)
		)
		(property "ki_keywords" "IOT SIGFOX GPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TD1205*"
			(at 0 0 0)
		)
		(symbol "TD1205_0_1")
		(symbol "TD1205_1_1"
			(pin power_in line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "BAT+")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "BAT-")
				(number "1")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DB2-SWDIO")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DB3-SWCLK")
				(number "9")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{RST}")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "UART-TX")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "UART-RX")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TD1208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 19.05 0)
		)
		(property "Value" "TD1208"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "RF_Module:TD1208"
			(at 17.78 -21.59 0)
		)
		(property "Datasheet" "https://github.com/Telecom-Design/Documentation_TD_RF_Module/blob/master/TD1208%20Datasheet.pdf"
			(at -6.35 -27.94 0)
		)
		(property "Description" "High-Performance, Low-Current SIGFOX™ Gateway"
			(at 0 0 0)
		)
		(property "ki_keywords" "IOT SIGFOX"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TD1208*"
			(at 0 0 0)
		)
		(symbol "TD1208_0_1")
		(symbol "TD1208_1_1"
			(pin unspecified line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "Reserved")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DB2-SWDIO")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DB3-SWCLK")
				(number "5")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "UART-TX")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "UART-RX")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin power_in line
				(at -7.62 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "RF_GND")
				(number "23")
			)
			(pin power_in line
				(at 7.62 -22.86 90)
				(length 2.54)
				(name "RF_GND")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "USR0")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "USR1")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "USR2")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "USR3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "USR4")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "ADC0")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DAC0")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "TIM2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RF")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TR-52DA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 11.43 0)
		)
		(property "Value" "TR-52DA"
			(at 25.4 11.43 0)
		)
		(property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01"
			(at -25.4 -11.43 0)
		)
		(property "Datasheet" "https://iqrf.org/weben/downloads.php?id=213"
			(at 25.4 -13.97 0)
		)
		(property "Description" "IQRF common transceiver with PCB antenna, FSK modulation"
			(at 0 0 0)
		)
		(property "ki_keywords" "IQRF common transceiver, PCB antenna, FSK modulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*"
			(at 0 0 0)
		)
		(symbol "TR-52DA_0_1")
		(symbol "TR-52DA_1_1"
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "RA0/AN0/C12IN0")
				(number "C1")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "RC2/VOUT")
				(number "C2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "C3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "C4")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "RC5/RC7/RX/SDO")
				(number "C8")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "RC4/SDI/SDA")
				(number "C7")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "RC3/SCK/SCL")
				(number "C6")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "RA5/RB4/RC6/AN4/AN11/TX/~{SS}/C2OUT/CCP3")
				(number "C5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WEMOS_C3_mini"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 19.05 0)
		)
		(property "Value" "WEMOS_C3_mini"
			(at 1.27 -19.05 0)
		)
		(property "Footprint" "RF_Module:WEMOS_C3_mini"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "https://www.wemos.cc/en/latest/c3/c3_mini.html"
			(at 0 -26.416 0)
		)
		(property "Description" "32-bit microcontroller module with WiFi"
			(at 0.762 -23.114 0)
		)
		(property "ki_keywords" "ESP32-C3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WEMOS*C3*mini*"
			(at 0 0 0)
		)
		(symbol "WEMOS_C3_mini_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RX")
				(number "15")
				(alternate "GPIO20" bidirectional line)
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "TX")
				(number "16")
				(alternate "GPIO21" bidirectional line)
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VBus")
				(number "9")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_out line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "3V3")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D0")
				(number "5")
				(alternate "ADC1_CH0" input line)
				(alternate "XTAL_32K_P" passive line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D1")
				(number "4")
				(alternate "ADC1_CH1" input line)
				(alternate "XTAL_32K_N" passive line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D2")
				(number "3")
				(alternate "ADC1_CH2" input line)
				(alternate "FSPIQ" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D3")
				(number "2")
				(alternate "ADC1_CH3" input line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "D4")
				(number "6")
				(alternate "ADC1_CH4" input line)
				(alternate "FSPIHD" bidirectional line)
				(alternate "MTMS" input line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "D5")
				(number "7")
				(alternate "ADC2_CH0" input line)
				(alternate "FSPIWP" bidirectional line)
				(alternate "MTDI" input line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "D6")
				(number "11")
				(alternate "FSPICLK" bidirectional line)
				(alternate "MTCK" input line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "D7")
				(number "12")
				(alternate "FSPID" bidirectional line)
				(alternate "MTDO" output line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "D8")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "D10")
				(number "14")
				(alternate "FSPICS0" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "WEMOS_D1_mini"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 19.05 0)
		)
		(property "Value" "WEMOS_D1_mini"
			(at 1.27 -19.05 0)
		)
		(property "Footprint" "RF_Module:WEMOS_D1_mini_light"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "https://wiki.wemos.cc/products:d1:d1_mini#documentation"
			(at -46.99 -29.21 0)
		)
		(property "Description" "32-bit microcontroller module with WiFi"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESP8266 WiFi microcontroller ESP8266EX"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WEMOS*D1*mini*"
			(at 0 0 0)
		)
		(symbol "WEMOS_D1_mini_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RX")
				(number "15")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "TX")
				(number "16")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "5V")
				(number "9")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_out line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "3V3")
				(number "8")
			)
			(pin input line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "D0")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SCL/D1")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SDA/D2")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D3")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "D4")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SCK/D5")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "MISO/D6")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "MOSI/D7")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "CS/D8")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "iM880A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 21.59 0)
		)
		(property "Value" "iM880A"
			(at 19.05 21.59 0)
		)
		(property "Footprint" ""
			(at -5.08 -27.94 0)
		)
		(property "Datasheet" "http://www.wireless-solutions.de/images/stories/downloads/Radio%20Modules/iM880A/General_Information/iM880A_Datasheet_V1_1.pdf"
			(at -5.08 -27.94 0)
		)
		(property "Description" "IMST Long Range Radio Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "IOT LoRa"
			(at 0 0 0)
		)
		(symbol "iM880A_0_1")
		(symbol "iM880A_1_1"
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "BOOT")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "P1-IO/JTCK/SWCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "P2-IO/JTMS/SWDIO")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "P3-IO/JTDO")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "P4-IO/JTDI")
				(number "5")
			)
			(pin input line
				(at -22.86 0 0)
				(length 2.54)
				(name "~{RST}")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "P5-IO/UART-CTS")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "P6-IO/UART-RTS")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "RxD-IO/UART-RX")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "TxD-IO/UART-TX")
				(number "19")
			)
			(pin power_in line
				(at -7.62 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin no_connect line
				(at 5.08 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin no_connect line
				(at 7.62 20.32 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin power_in line
				(at 7.62 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "30")
			)
			(pin power_in line
				(at 10.16 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "P7-IO/SPI-MISO")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "P8-IO/SPI-MOSI")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "P9-IO/SPI-CLK")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "P10-IO/SPI-NSS")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "P11-IO")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "P12-IO/I2C-SCL")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "P13-IO/I2C-SDA")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "P14-IO/ADC")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "P15-IO/WKUP")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "P17-IO/ADC")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "RF")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CMWX1ZZABZ-091"
		(extends "CMWX1ZZABZ-078")
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "CMWX1ZZABZ-091"
			(at 16.51 36.83 0)
		)
		(property "Footprint" "RF_Module:CMWX1ZZABZ"
			(at 0 0 0)
		)
		(property "Datasheet" "https://wireless.murata.com/RFM/data/type_abz.pdf"
			(at 62.23 -38.1 0)
		)
		(property "Description" "LoRa/SigFox Module, STM32L072 MCU, Murata CMWX1ZZABZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "iot lora sigfox"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CMWX1ZZABZ*"
			(at 0 0 0)
		)
	)
	(symbol "DCTR-52DA"
		(extends "TR-52DA")
		(property "Reference" "U"
			(at -25.4 11.43 0)
		)
		(property "Value" "DCTR-52DA"
			(at 25.4 11.43 0)
		)
		(property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01"
			(at -25.4 -11.43 0)
		)
		(property "Datasheet" "https://iqrf.org/weben/downloads.php?id=213"
			(at 25.4 -13.97 0)
		)
		(property "Description" "IQRF data controlled transceiver with PCB antenna, FSK modulation"
			(at 0 0 0)
		)
		(property "ki_keywords" "IQRF data controlled transceiver, PCB antenna, FSK modulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*"
			(at 0 0 0)
		)
	)
	(symbol "DCTR-52DAT"
		(extends "TR-52DA")
		(property "Reference" "U"
			(at -25.4 11.43 0)
		)
		(property "Value" "DCTR-52DAT"
			(at 25.4 11.43 0)
		)
		(property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01"
			(at -25.4 -11.43 0)
		)
		(property "Datasheet" "https://iqrf.org/weben/downloads.php?id=213"
			(at 25.4 -13.97 0)
		)
		(property "Description" "IQRF data controlled transceiver with PCB antenna and thermometer, FSK modulation"
			(at 0 0 0)
		)
		(property "ki_keywords" "IQRF data controlled transceiver, PCB antenna, thermometer, FSK modulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*"
			(at 0 0 0)
		)
	)
	(symbol "DWM3000"
		(extends "DWM1000")
		(property "Reference" "DWM"
			(at 7.62 25.4 0)
		)
		(property "Value" "DWM3000"
			(at 1.27 3.81 0)
		)
		(property "Footprint" "RF_Module:DWM1000"
			(at 17.78 -25.4 0)
		)
		(property "Datasheet" "https://www.qorvo.com/products/d/da008334"
			(at 60.96 -27.94 0)
		)
		(property "Description" "Ultra wide band RF module With ranging location capabilities"
			(at 0 0 0)
		)
		(property "ki_keywords" "DWM3000 Decawave Qorvo RF ranging UWB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DWM1000*"
			(at 0 0 0)
		)
	)
	(symbol "E73-2G4M04S-52810"
		(extends "E73-2G4M04S-52832")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "E73-2G4M04S-52810"
			(at 0 -1.27 0)
		)
		(property "Footprint" "RF_Module:E73-2G4M04S"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.cdebyte.com/en/downpdf.aspx?id=243"
			(at 0 11.43 0)
		)
		(property "Description" "nRF52810 BLE5 Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE5, BLE, nRF52810"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "E73*2G4M04S*"
			(at 0 0 0)
		)
	)
	(symbol "ESP-12F"
		(extends "ESP-12E")
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "ESP-12F"
			(at 12.7 19.05 0)
		)
		(property "Footprint" "RF_Module:ESP-12E"
			(at 0 0 0)
		)
		(property "Datasheet" "http://wiki.ai-thinker.com/_media/esp8266/esp8266_series_modules_user_manual_v1.1.pdf"
			(at -8.89 2.54 0)
		)
		(property "Description" "802.11 b/g/n Wi-Fi Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "802.11 Wi-Fi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP?12*"
			(at 0 0 0)
		)
	)
	(symbol "ESP32-S2-WROVER-I"
		(extends "ESP32-S2-WROVER")
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "ESP32-S2-WROVER-I"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "RF_Module:ESP32-S2-WROVER"
			(at 19.05 -29.21 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf"
			(at -7.62 -20.32 0)
		)
		(property "Description" "RF Module, ESP32-D0WDQ6 SoC, Wi-Fi 802.11b/g/n, 32-bit, 2.7-3.6V, onboard antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio ESP ESP32 Espressif onboard PCB antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?S2?WROVER*"
			(at 0 0 0)
		)
	)
	(symbol "ESP32-S3-MINI-1U"
		(extends "ESP32-S3-MINI-1")
		(property "Reference" "U"
			(at -11.43 29.21 0)
		)
		(property "Value" "ESP32-S3-MINI-1U"
			(at 12.7 29.21 0)
		)
		(property "Footprint" "RF_Module:ESP32-S2-MINI-1U"
			(at 16.51 -29.21 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s3-mini-1_mini-1u_datasheet_en.pdf"
			(at 0 40.64 0)
		)
		(property "Description" "RF Module, ESP32-S3 SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 3.3V, SMD, external antenna"
			(at 0 43.18 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32-S3 Espressif"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?S*MINI?1U"
			(at 0 0 0)
		)
	)
	(symbol "ESP32-WROOM-32D"
		(extends "ESP32-WROOM-32")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ESP32-WROOM-32D"
			(at 1.27 34.29 0)
		)
		(property "Footprint" "RF_Module:ESP32-WROOM-32D"
			(at 16.51 -34.29 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32d_esp32-wroom-32u_datasheet_en.pdf"
			(at -7.62 1.27 0)
		)
		(property "Description" "RF Module, ESP32-D0WD SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif onboard PCB antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?WROOM?32D*"
			(at 0 0 0)
		)
	)
	(symbol "ESP32-WROOM-32UE"
		(extends "ESP32-WROOM-32E")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ESP32-WROOM-32UE"
			(at 1.27 34.29 0)
		)
		(property "Footprint" "RF_Module:ESP32-WROOM-32UE"
			(at 16.51 -34.29 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "RF Module, ESP32-D0WD-V3 SoC, without PSRAM, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, external antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif external U.FL antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?WROOM?32UE*"
			(at 0 0 0)
		)
	)
	(symbol "ESP32-WROOM-32UE-R2"
		(extends "ESP32-WROOM-32E-R2")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ESP32-WROOM-32UE-R2"
			(at 1.27 34.29 0)
		)
		(property "Footprint" "RF_Module:ESP32-WROOM-32UE"
			(at 16.51 -34.29 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "RF Module, ESP32-D0WDR2-V3 SoC, with 2MB PSRAM, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif external U.FL antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ESP32?WROOM?32UE*"
			(at 0 0 0)
		)
	)
	(symbol "MDBT50Q-P1MV2"
		(extends "MDBT50Q-1MV2")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "MDBT50Q-P1MV2"
			(at 0 -2.54 0)
		)
		(property "Footprint" "RF_Module:Raytac_MDBT50Q"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.raytac.com/download/index.php?index_id=43"
			(at 0 -5.08 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE ANT ZigBee Thread 802.15.4 nRF52840 nordic MDBT50Q"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Raytac?MDBT50Q*"
			(at 0 0 0)
		)
	)
	(symbol "MDBT50Q-P512K"
		(extends "MDBT50Q-512K")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "MDBT50Q-P512K"
			(at 0 -2.54 0)
		)
		(property "Footprint" "RF_Module:Raytac_MDBT50Q"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.raytac.com/download/index.php?index_id=46"
			(at 0 -5.08 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52833 module"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU, ARM, BLE, ANT, 2.4GHz, 802.15.4 MDBT50Q"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Raytac?MDBT50Q*"
			(at 0 0 0)
		)
	)
	(symbol "MDBT50Q-U1MV2"
		(extends "MDBT50Q-1MV2")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "MDBT50Q-U1MV2"
			(at 0 -2.54 0)
		)
		(property "Footprint" "RF_Module:Raytac_MDBT50Q"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.raytac.com/download/index.php?index_id=43"
			(at 0 -5.08 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE ANT ZigBee Thread 802.15.4 nRF52840 nordic MDBT50Q"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Raytac?MDBT50Q*"
			(at 0 0 0)
		)
	)
	(symbol "MDBT50Q-U512K"
		(extends "MDBT50Q-512K")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "MDBT50Q-U512K"
			(at 0 -2.54 0)
		)
		(property "Footprint" "RF_Module:Raytac_MDBT50Q"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.raytac.com/download/index.php?index_id=46"
			(at 0 -5.08 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52833 module"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU, ARM, BLE, ANT, 2.4GHz, 802.15.4 MDBT50Q"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Raytac?MDBT50Q*"
			(at 0 0 0)
		)
	)
	(symbol "RAK811-HF-AS923"
		(extends "RAK811-HF-EU868")
		(property "Reference" "U"
			(at 0 31.75 0)
		)
		(property "Value" "RAK811-HF-AS923"
			(at 0 27.94 0)
		)
		(property "Footprint" "RF_Module:RAK811"
			(at -11.43 31.75 0)
		)
		(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf"
			(at -11.43 31.75 0)
		)
		(property "Description" "LoRa Module, STM32L151, AS923, RAKwireless"
			(at 0 0 0)
		)
		(property "ki_keywords" "IoT LoRa LoRaWAN RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RAK811*"
			(at 0 0 0)
		)
	)
	(symbol "RAK811-HF-AU915"
		(extends "RAK811-HF-EU868")
		(property "Reference" "U"
			(at 0 31.75 0)
		)
		(property "Value" "RAK811-HF-AU915"
			(at 0 27.94 0)
		)
		(property "Footprint" "RF_Module:RAK811"
			(at -11.43 31.75 0)
		)
		(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf"
			(at -11.43 31.75 0)
		)
		(property "Description" "LoRa Module, STM32L151, AU915, RAKwireless"
			(at 0 0 0)
		)
		(property "ki_keywords" "IoT LoRa LoRaWAN RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RAK811*"
			(at 0 0 0)
		)
	)
	(symbol "RAK811-HF-IN865"
		(extends "RAK811-HF-EU868")
		(property "Reference" "U"
			(at 0 31.75 0)
		)
		(property "Value" "RAK811-HF-IN865"
			(at 0 27.94 0)
		)
		(property "Footprint" "RF_Module:RAK811"
			(at -11.43 31.75 0)
		)
		(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf"
			(at -11.43 31.75 0)
		)
		(property "Description" "LoRa Module, STM32L151, IN865, RAKwireless"
			(at 0 0 0)
		)
		(property "ki_keywords" "IoT LoRa LoRaWAN RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RAK811*"
			(at 0 0 0)
		)
	)
	(symbol "RAK811-HF-KR920"
		(extends "RAK811-HF-EU868")
		(property "Reference" "U"
			(at 0 31.75 0)
		)
		(property "Value" "RAK811-HF-KR920"
			(at 0 27.94 0)
		)
		(property "Footprint" "RF_Module:RAK811"
			(at -11.43 31.75 0)
		)
		(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf"
			(at -11.43 31.75 0)
		)
		(property "Description" "LoRa Module, STM32L151, KR920, RAKwireless"
			(at 0 0 0)
		)
		(property "ki_keywords" "IoT LoRa LoRaWAN RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RAK811*"
			(at 0 0 0)
		)
	)
	(symbol "RAK811-HF-US915"
		(extends "RAK811-HF-EU868")
		(property "Reference" "U"
			(at 0 31.75 0)
		)
		(property "Value" "RAK811-HF-US915"
			(at 0 27.94 0)
		)
		(property "Footprint" "RF_Module:RAK811"
			(at -11.43 31.75 0)
		)
		(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf"
			(at -11.43 31.75 0)
		)
		(property "Description" "LoRa Module, STM32L151, US915, RAKwireless"
			(at 0 0 0)
		)
		(property "ki_keywords" "IoT LoRa LoRaWAN RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RAK811*"
			(at 0 0 0)
		)
	)
	(symbol "RAK811-LF-CN470"
		(extends "RAK811-LF-EU433")
		(property "Reference" "U"
			(at 0 31.75 0)
		)
		(property "Value" "RAK811-LF-CN470"
			(at 0 27.94 0)
		)
		(property "Footprint" "RF_Module:RAK811"
			(at -11.43 31.75 0)
		)
		(property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf"
			(at -11.43 31.75 0)
		)
		(property "Description" "LoRa Module, STM32L151, CN470, RAKwireless"
			(at 0 0 0)
		)
		(property "ki_keywords" "IoT LoRa LoRaWAN RF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RAK811*"
			(at 0 0 0)
		)
	)
	(symbol "RFM69HCW"
		(extends "RFM95W-868S2")
		(property "Reference" "U"
			(at -10.414 11.684 0)
		)
		(property "Value" "RFM69HCW"
			(at 1.524 11.43 0)
		)
		(property "Footprint" ""
			(at -83.82 41.91 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcb8284d838.pdf"
			(at -83.82 41.91 0)
		)
		(property "Description" "Low power ISM Radio Transceiver Module, SPI interface, AES encryption, 434 or 915 MHz, up to 100mW, up to 300 kb/s, SMD-16, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "low power Radio ISM Transceiver Module AES encryption SPI HopeRF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM9XW*"
			(at 0 0 0)
		)
	)
	(symbol "RFM69W"
		(extends "RFM69HW")
		(property "Reference" "U"
			(at -3.81 11.43 0)
		)
		(property "Value" "RFM69W"
			(at -7.62 13.97 0)
		)
		(property "Footprint" "RF_Module:HOPERF_RFM69HW"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbe34756e1.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "ISM Radio Transceiver Module, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "Radio, ISM, Transceiver, Module, AES"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM69HW*"
			(at 0 0 0)
		)
	)
	(symbol "RFM95W-915S2"
		(extends "RFM95W-868S2")
		(property "Reference" "U"
			(at -10.414 11.684 0)
		)
		(property "Value" "RFM95W-915S2"
			(at 1.524 11.43 0)
		)
		(property "Footprint" ""
			(at -83.82 41.91 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf"
			(at -83.82 41.91 0)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 915 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low power long range transceiver module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM9XW*"
			(at 0 0 0)
		)
	)
	(symbol "RFM96W-315S2"
		(extends "RFM95W-868S2")
		(property "Reference" "U"
			(at -10.414 11.684 0)
		)
		(property "Value" "RFM96W-315S2"
			(at 1.524 11.43 0)
		)
		(property "Footprint" ""
			(at -83.82 41.91 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcc0ac60235.pdf"
			(at -83.82 41.91 0)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 315 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low power long range transceiver module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM9XW*"
			(at 0 0 0)
		)
	)
	(symbol "RFM96W-433S2"
		(extends "RFM95W-868S2")
		(property "Reference" "U"
			(at -10.414 11.684 0)
		)
		(property "Value" "RFM96W-433S2"
			(at 1.524 11.43 0)
		)
		(property "Footprint" ""
			(at -83.82 41.91 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcc0ac60235.pdf"
			(at -83.82 41.91 0)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 433 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low power long range transceiver module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM9XW*"
			(at 0 0 0)
		)
	)
	(symbol "RFM97W-868S2"
		(extends "RFM95W-868S2")
		(property "Reference" "U"
			(at -10.414 11.684 0)
		)
		(property "Value" "RFM97W-868S2"
			(at 1.524 11.43 0)
		)
		(property "Footprint" ""
			(at -83.82 41.91 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf"
			(at -83.82 41.91 0)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -139 dBm, SMD-16, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low power long range transceiver module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM9XW*"
			(at 0 0 0)
		)
	)
	(symbol "RFM97W-915S2"
		(extends "RFM95W-868S2")
		(property "Reference" "U"
			(at -10.414 11.684 0)
		)
		(property "Value" "RFM97W-915S2"
			(at 1.524 11.43 0)
		)
		(property "Footprint" ""
			(at -83.82 41.91 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf"
			(at -83.82 41.91 0)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 915 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -139 dBm, SMD-16, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low power long range transceiver module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM9XW*"
			(at 0 0 0)
		)
	)
	(symbol "RFM98W-315S2"
		(extends "RFM95W-868S2")
		(property "Reference" "U"
			(at -10.414 11.684 0)
		)
		(property "Value" "RFM98W-315S2"
			(at 1.524 11.43 0)
		)
		(property "Footprint" ""
			(at -83.82 41.91 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcdb5e17543.pdf"
			(at -83.82 41.91 0)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 315 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low power long range transceiver module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM9XW*"
			(at 0 0 0)
		)
	)
	(symbol "RFM98W-433S2"
		(extends "RFM95W-868S2")
		(property "Reference" "U"
			(at -10.414 11.684 0)
		)
		(property "Value" "RFM98W-433S2"
			(at 1.524 11.43 0)
		)
		(property "Footprint" ""
			(at -83.82 41.91 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcdb5e17543.pdf"
			(at -83.82 41.91 0)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 433 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low power long range transceiver module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HOPERF*RFM9XW*"
			(at 0 0 0)
		)
	)
	(symbol "TR-52DAT"
		(extends "TR-52DA")
		(property "Reference" "U"
			(at -25.4 11.43 0)
		)
		(property "Value" "TR-52DAT"
			(at 25.4 11.43 0)
		)
		(property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01"
			(at -25.4 -11.43 0)
		)
		(property "Datasheet" "https://iqrf.org/weben/downloads.php?id=213"
			(at 25.4 -13.97 0)
		)
		(property "Description" "IQRF common transceiver with PCB antenna and thermometer, FSK modulation"
			(at 0 0 0)
		)
		(property "ki_keywords" "IQRF common transceiver, PCB antenna, thermometer, FSK modulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*"
			(at 0 0 0)
		)
	)
	(symbol "TR-72DA"
		(extends "TR-52DA")
		(property "Reference" "U"
			(at -25.4 11.43 0)
		)
		(property "Value" "TR-72DA"
			(at 25.4 11.43 0)
		)
		(property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01"
			(at -25.4 -11.43 0)
		)
		(property "Datasheet" "https://iqrf.org/weben/downloads.php?id=337"
			(at 25.4 -13.97 0)
		)
		(property "Description" "IQRF transceiver with PCB antenna, GMSK modulation"
			(at 0 0 0)
		)
		(property "ki_keywords" "IQRF transceiver, PCB antenna, GMSK modulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*"
			(at 0 0 0)
		)
	)
	(symbol "TR-72DAT"
		(extends "TR-52DA")
		(property "Reference" "U"
			(at -25.4 11.43 0)
		)
		(property "Value" "TR-72DAT"
			(at 25.4 11.43 0)
		)
		(property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01"
			(at -25.4 -11.43 0)
		)
		(property "Datasheet" "https://iqrf.org/weben/downloads.php?id=337"
			(at 25.4 -13.97 0)
		)
		(property "Description" "IQRF transceiver with PCB antenna and thermometer, GMSK modulation"
			(at 0 0 0)
		)
		(property "ki_keywords" "IQRF transceiver, PCB antenna, thermometer, GMSK modulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*"
			(at 0 0 0)
		)
	)
	(symbol "iM880B"
		(extends "iM880A")
		(property "Reference" "U"
			(at -19.05 21.59 0)
		)
		(property "Value" "iM880B"
			(at 19.05 21.59 0)
		)
		(property "Footprint" ""
			(at -5.08 -27.94 0)
		)
		(property "Datasheet" "http://www.wireless-solutions.de/images/stories/downloads/Radio%20Modules/iM880B/General_Information/iM880B_Datasheet_V1_0.pdf"
			(at -5.08 -27.94 0)
		)
		(property "Description" "IMST Long Range Radio Module - LoRa Alliance Certified"
			(at 0 0 0)
		)
		(property "ki_keywords" "IOT LoRa"
			(at 0 0 0)
		)
	)
)
