(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "PN5321A3HN_C1xx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "PN5321A3HN_C1xx"
			(at 15.24 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-40-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at 38.1 -31.75 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/nxp/data-sheets/PN532_C1.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Near Field Communication (NFC) controller, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVQFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PN5321A3HN_C1xx_0_1")
		(symbol "PN5321A3HN_C1xx_1_1"
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "~{RSTPD}")
				(number "38")
			)
			(pin output line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "~{RSTOUT}")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "P70_IRQ")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "NSS/P50_SCL/HSU_RX")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "MOSI/SDA/HSU_TX")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "MISO/P71")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "SCK/P72")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "P30/UART_RX")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "P31/UART_TX")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "P32_INT0")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "P33_INT1")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "P35")
				(number "19")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "OSCIN")
				(number "14")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "OSCOUT")
				(number "15")
			)
			(pin passive line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "I0")
				(number "16")
			)
			(pin passive line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "I1")
				(number "17")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VBAT")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 2.54)
				(name "DVSS")
				(number "1")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "AVDD")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "AVSS")
				(number "11")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "41")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "TVDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "TVSS1")
				(number "3")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "PVDD")
				(number "23")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "TVSS2")
				(number "7")
			)
			(pin power_out line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "DVDD")
				(number "39")
			)
			(pin passive line
				(at 5.08 -33.02 90)
				(length 2.54)
				(name "TESTEN")
				(number "18")
			)
			(pin no_connect line
				(at 17.78 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "20")
			)
			(pin no_connect line
				(at 17.78 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "21")
			)
			(pin no_connect line
				(at 17.78 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "22")
			)
			(pin output line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "TX1")
				(number "4")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "TX2")
				(number "6")
			)
			(pin input line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RX")
				(number "10")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "LOADMOD")
				(number "2")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "VMID")
				(number "9")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "AUX1")
				(number "12")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "AUX2")
				(number "13")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "SVDD")
				(number "37")
			)
			(pin output line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "SIGOUT")
				(number "35")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "SIGIN")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "SIC_CLK/P34")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST25DV04K-IER8C3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "ST25DV04K-IER8C3"
			(at 10.795 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.36x1.46mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st25dv04k.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dynamic NFC/RFID tag IC with 4-Kbit EEPROM, UFDFPN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC Tag"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ST25DV04K-IER8C3_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GPO")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_EH")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "AC0")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "AC1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST25DV16K-JFR6D3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ST25DV16K-JFR6D3"
			(at 10.795 -8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFDFPN-12-1EP_3x3mm_P0.5mm_EP1.4x2.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st25dv04k.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dynamic NFC/RFID tag IC with 16-Kbit EEPROM, UFDFPN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC Tag"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFDFPN*3x3mm*P0.5mm*EP1.4x2.55mm*"
			(at 0 0 0)
		)
		(symbol "ST25DV16K-JFR6D3_1_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "LPD")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDCG")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "V_EH")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "GPO")
				(number "11")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "AC0")
				(number "4")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "AC1")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST25R3911B-AQW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "ST25R3911B-AQW"
			(at 10.16 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.5x3.5mm_ThermalVias"
			(at -0.762 -30.734 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st25r3911b.pdf"
			(at -0.762 -33.274 0)
		)
		(property "Description" "High performance HR reader/NFC initiator with 1.4W supporting VHBR and AAT, VFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ST25R3911B-AQW_0_1")
		(symbol "ST25R3911B-AQW_1_1"
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "MISO")
				(number "29")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "MOSI")
				(number "30")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "31")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "/SS")
				(number "32")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "IRQ")
				(number "27")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "MCU_CLK")
				(number "28")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "XTO")
				(number "4")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "XTI")
				(number "5")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "CSI")
				(number "25")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "CSO")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "VSN_A")
				(number "26")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD_IO")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "VSN_RF")
				(number "12")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "EP")
				(number "33")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "VSN_D")
				(number "6")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "21")
			)
			(pin power_out line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "VSP_D")
				(number "3")
			)
			(pin power_out line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "VSP_A")
				(number "7")
			)
			(pin power_out line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "VSP_RF")
				(number "9")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AGD")
				(number "24")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "TRIM1_0")
				(number "19")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "TRIM1_1")
				(number "17")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "TRIM1_2")
				(number "15")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "TRIM1_3")
				(number "13")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RFI1")
				(number "22")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "RFO1")
				(number "10")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "RFO2")
				(number "11")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "RFI2")
				(number "23")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "TRIM2_0")
				(number "20")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "TRIM2_1")
				(number "18")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "TRIM2_2")
				(number "16")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "TRIM2_3")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST25DV04K-JFR6D3"
		(extends "ST25DV16K-JFR6D3")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ST25DV04K-JFR6D3"
			(at 10.795 -8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFDFPN-12-1EP_3x3mm_P0.5mm_EP1.4x2.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st25dv04k.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dynamic NFC/RFID tag IC with 4-Kbit EEPROM, UFDFPN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC Tag"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFDFPN*3x3mm*P0.5mm*EP1.4x2.55mm*"
			(at 0 0 0)
		)
	)
	(symbol "ST25DV16K-IER8C3"
		(extends "ST25DV04K-IER8C3")
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "ST25DV16K-IER8C3"
			(at 10.795 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.36x1.46mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st25dv04k.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dynamic NFC/RFID tag IC with 16-Kbit EEPROM, UFDFPN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC Tag"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ST25DV64K-IER8C3"
		(extends "ST25DV04K-IER8C3")
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "ST25DV64K-IER8C3"
			(at 10.795 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.36x1.46mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st25dv04k.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dynamic NFC/RFID tag IC with 64-Kbit EEPROM, UFDFPN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC Tag"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ST25DV64K-JFR6D3"
		(extends "ST25DV16K-JFR6D3")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ST25DV64K-JFR6D3"
			(at 10.795 -8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFDFPN-12-1EP_3x3mm_P0.5mm_EP1.4x2.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st25dv04k.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dynamic NFC/RFID tag IC with 64-Kbit EEPROM, UFDFPN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC Tag"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFDFPN*3x3mm*P0.5mm*EP1.4x2.55mm*"
			(at 0 0 0)
		)
	)
	(symbol "ST25R3911B-AQF"
		(extends "ST25R3911B-AQW")
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "ST25R3911B-AQF"
			(at 10.16 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm_ThermalVias"
			(at -0.762 -30.734 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st25r3911b.pdf"
			(at -0.762 -33.274 0)
		)
		(property "Description" "High performance HR reader/NFC initiator with 1.4W supporting VHBR and AAT, QFN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
