(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "HTRC11001T"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "HTRC11001T"
			(at 2.54 17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at -13.97 15.24 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/037031.pdf"
			(at 0 0 0)
		)
		(property "Description" "HITAG RF Reader Device, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "HITAG RFID"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HTRC11001T_0_1")
		(symbol "HTRC11001T_1_1"
			(pin input clock
				(at -15.24 12.7 0)
				(length 3.81)
				(name "SCLK")
				(number "8")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "DIN")
				(number "9")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "DOUT")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "MODE")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "XTAL1")
				(number "6")
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "XTAL2")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "TX1")
				(number "4")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "TX2")
				(number "2")
			)
			(pin input line
				(at 15.24 0 180)
				(length 3.81)
				(name "RX")
				(number "14")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "CEXT")
				(number "12")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "QGND")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PN5120A0HN1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 25.4 0)
		)
		(property "Value" "PN5120A0HN1"
			(at 15.24 -25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PN512.pdf"
			(at 21.59 -13.97 0)
		)
		(property "Description" "NFC frontend.  ISO/IEC 14443A&B, MIFARE®, FeliCa and NFC Forum tag types, HVQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "PN512 RFID"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PN5120A0HN1_0_1")
		(symbol "PN5120A0HN1_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "~{NRSTPD}")
				(number "6")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "RX")
				(number "17")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "ALE")
				(number "24")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "A0")
				(number "32")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "D1")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "D2")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "D3")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "D4")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "D5")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "D6")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "D7")
				(number "31")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "PVDD")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -25.4 90)
				(length 2.54)
				(name "PVSS")
				(number "5")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "DVSS")
				(number "4")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "SVDD")
				(number "9")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "33")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "TVDD")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "TVSS")
				(number "10")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "TVSS")
				(number "14")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -25.4 90)
				(length 2.54)
				(name "AVSS")
				(number "18")
			)
			(pin power_out line
				(at 10.16 25.4 270)
				(length 2.54)
				(name "VMID")
				(number "16")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "IRQ")
				(number "23")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SIGIN")
				(number "7")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SIGOUT")
				(number "8")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "TX1")
				(number "11")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "TX2")
				(number "13")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "AUX1")
				(number "19")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "AUX2")
				(number "20")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "OSCOUT")
				(number "22")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "OSCIN")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
)
