(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADG901BCPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "ADG901BCPZ"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG901_902.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "SPST DC-4.5GHz absorbative switch, 40dB isolation at 1GHz, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPST switch CMOS LVTTL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADG901BCPZ_0_0"
			(text "50"
				(at -3.81 -0.127 900)
			)
			(text "50"
				(at 3.81 -0.127 900)
			)
		)
		(symbol "ADG901BCPZ_0_1")
		(symbol "ADG901BCPZ_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RF1")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CTRL")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RF2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG901BRMZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "ADG901BRMZ"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG901_902.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "SPST DC-4.5GHz absorbative switch, 40dB isolation at 1GHz, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPST switch CMOS LVTTL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG901BRMZ_0_0"
			(text "50"
				(at -3.81 -0.127 900)
			)
			(text "50"
				(at 3.81 -0.127 900)
			)
		)
		(symbol "ADG901BRMZ_0_1")
		(symbol "ADG901BRMZ_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RF1")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CTRL")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RF2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG902BRMZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "ADG902BRMZ"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG901_902.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "SPST DC-4.5GHz reflective switch, 40dB isolation at 1GHz, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPST switch CMOS LVTTL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG902BRMZ_0_0")
		(symbol "ADG902BRMZ_0_1")
		(symbol "ADG902BRMZ_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RF1")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CTRL")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RF2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG918BCPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "ADG918BCPZ"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG918_919.pdf"
			(at -1.27 5.08 0)
		)
		(property "Description" "SPDT DC-4GHz absorbative switch, 43dB isolation at 1GHz, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Mux SPDT switch CMOS LVTTL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADG918BCPZ_0_0"
			(text "50"
				(at 2.286 -5.715 900)
			)
			(text "50"
				(at 3.81 -5.715 900)
			)
		)
		(symbol "ADG918BCPZ_0_1")
		(symbol "ADG918BCPZ_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RFC")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "8")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "RF2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG918BRM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "ADG918BRM"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG918_919.pdf"
			(at -1.27 5.08 0)
		)
		(property "Description" "SPDT DC-4GHz absorbative switch, 43dB isolation at 1GHz, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Mux SPDT switch CMOS LVTTL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG918BRM_0_0"
			(text "50"
				(at 2.286 -5.715 900)
			)
			(text "50"
				(at 3.81 -5.715 900)
			)
		)
		(symbol "ADG918BRM_0_1")
		(symbol "ADG918BRM_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RFC")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "8")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "RF2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG919BCPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "ADG919BCPZ"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG918_919.pdf"
			(at -1.27 5.08 0)
		)
		(property "Description" "SPDT DC-4GHz reflective switch, 43dB isolation at 1GHz, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Mux SPDT switch CMOS LVTTL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADG919BCPZ_0_0")
		(symbol "ADG919BCPZ_0_1")
		(symbol "ADG919BCPZ_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RFC")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "8")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "RF2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADG919BRMZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "ADG919BRMZ"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADG918_919.pdf"
			(at -1.27 5.08 0)
		)
		(property "Description" "SPDT DC-4GHz reflective switch, 43dB isolation at 1GHz, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Mux SPDT switch CMOS LVTTL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADG919BRMZ_0_0")
		(symbol "ADG919BRMZ_0_1")
		(symbol "ADG919BRMZ_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RFC")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "8")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "RF2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS179-92LF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "AS179-92LF"
			(at 2.54 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/AS179_92LF_200176H.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "20 MHz to 4.0 GHz GaAs SPDT Switch, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "rf spdt switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
		(symbol "AS179-92LF_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "J1")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V1")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V2")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "J3")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "J2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BGS12WN6E6327"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "BGS12WN6E6327"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_LGA:Infineon_PG-TSNP-6-10_0.7x1.1mm_0.7x1.1mm_P0.4mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BGS12WN6-DataSheet-v02_05-EN.pdf?fileId=5546d4626b2d8e69016b89d2b3334727"
			(at -1.27 5.08 0)
		)
		(property "Description" "SPDT DC-9GHz switch, 45dB isolation at 960MHz, PG-TSNP-6-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Mux SPDT switch CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PG?TSNP*0.7x1.1mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "BGS12WN6E6327_0_0")
		(symbol "BGS12WN6E6327_0_1")
		(symbol "BGS12WN6E6327_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RFIN")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RF2")
				(number "1")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "RF1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HMC7992"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "HMC7992"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/HMC7992.pdf"
			(at 0 0 0)
		)
		(property "Description" "SP4T 100MHz-6GHz absorptive switch, 50 Ohm, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "rf switch sp4t absorptive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "HMC7992_0_1")
		(symbol "HMC7992_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RFC")
				(number "15")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "12")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "RF2")
				(number "9")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "RF3")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "RF4")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HMC849A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "HMC849A"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-16-1EP_4x4mm_P0.65mm_EP2.4x2.4mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/hmc849a.pdf"
			(at -13.97 31.75 0)
		)
		(property "Description" "High Isolation SPDT Non-Reflective Switch, DC-6GHz, Matched to 50 Ohm, LFCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPDT switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "HMC849A_0_0"
			(text "50"
				(at 1.651 1.016 0)
			)
			(text "50"
				(at 1.651 -1.016 0)
			)
		)
		(symbol "HMC849A_0_1")
		(symbol "HMC849A_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VCTL")
				(number "2")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "RFC")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RF1")
				(number "9")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "RF2")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KSW-2-46"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "KSW-2-46"
			(at 12.7 8.89 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/KSW-2-46+.pdf"
			(at -13.97 31.75 0)
		)
		(property "Description" "SPDT DC-4.6GHz reflective switch, 50 Ohm, XX112"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPDT switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*XX112* SOP*1EP*4.57x4.57mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "KSW-2-46_0_1")
		(symbol "KSW-2-46_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RF_IN")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CONTROL1")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CONTROL2")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RF_OUT1")
				(number "5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_OUT2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KSWA-2-46"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "KSWA-2-46"
			(at 12.7 8.89 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/KSWA-2-46+.pdf"
			(at -13.97 31.75 0)
		)
		(property "Description" "SPDT DC-4.6GHz absorbative switch, 50 Ohm, XX112"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPDT switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*XX112* SOP*1EP*4.57x4.57mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "KSWA-2-46_0_0"
			(text "50"
				(at 1.524 -4.699 900)
			)
			(text "50"
				(at 2.794 -4.699 900)
			)
		)
		(symbol "KSWA-2-46_0_1")
		(symbol "KSWA-2-46_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RF_IN")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CONTROL1")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CONTROL2")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RF_OUT1")
				(number "5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_OUT2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KSWHA-1-20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 6.35 0)
		)
		(property "Value" "KSWHA-1-20"
			(at 12.7 6.35 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/KSWHA-1-20+.pdf"
			(at -13.97 31.75 0)
		)
		(property "Description" "SPST DC-2.0GHz absorbative switch, 50 Ohm, XX112"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPST switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*XX112* SOP*1EP*4.57x4.57mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "KSWHA-1-20_0_1")
		(symbol "KSWHA-1-20_1_0"
			(text "50"
				(at 2.54 -3.683 900)
			)
			(text "50"
				(at 3.81 -3.683 900)
			)
		)
		(symbol "KSWHA-1-20_1_1"
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RF_IN")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CONTROL1")
				(number "2")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CONTROL2")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RF_OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MASWSS0136"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MASWSS0136"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/MASWSS0136.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Macom GaAs RF SPDT switch, DC-3GHz, 0.4/27dB loss/isolation, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SWITCH SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
		(symbol "MASWSS0136_0_1")
		(symbol "MASWSS0136_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RFC")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V1")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V2")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "RF2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MASWSS0178"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MASWSS0178"
			(at 3.556 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/MASWSS0178.pdf"
			(at 2.032 2.54 0)
		)
		(property "Description" "SPDT High Isolation Terminated Switch, 0.01-3.0 GHz, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF switch SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MASWSS0178_0_1")
		(symbol "MASWSS0178_1_1"
			(text "50"
				(at 3.683 3.556 0)
			)
			(text "50"
				(at 3.683 1.524 0)
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RFC")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CTL1")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CTL2")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "8")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "RF2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MASWSS0179"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MASWSS0179"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/MASWSS0179.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Macom GaAs RF SPDT switch, DC-2GHz, 0.6/22dB loss/isolation, SOT-26 (SOT-23-6)"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SWITCH SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MASWSS0179_0_1")
		(symbol "MASWSS0179_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RFC")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V1")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V2")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "RF2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSW-2-20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "MSW-2-20"
			(at 12.7 8.89 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.76x4.96mm_P1.27mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/MSW-2-20+.pdf"
			(at -13.97 31.75 0)
		)
		(property "Description" "SPDT DC-2.0GHz reflective switch, 50 Ohm, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPDT switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.76x4.96mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MSW-2-20_0_1")
		(symbol "MSW-2-20_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RF_IN")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CONTROL1")
				(number "5")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CONTROL2")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RF_OUT1")
				(number "6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_OUT2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSW2-50"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "MSW2-50"
			(at 12.7 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.51mm_EP1.45x1.45mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/MSW2-50+.pdf"
			(at -13.97 31.75 0)
		)
		(property "Description" "SPDT DC-5.0GHz reflective switch, 50 Ohm, QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPDT switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.51mm*"
			(at 0 0 0)
		)
		(symbol "MSW2-50_0_1")
		(symbol "MSW2-50_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RF_IN")
				(number "8")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CONTROL1")
				(number "1")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CONTROL2")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RF_OUT1")
				(number "11")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSWA-2-20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "MSWA-2-20"
			(at 12.7 8.89 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.76x4.96mm_P1.27mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/MSWA-2-20+.pdf"
			(at -13.97 31.75 0)
		)
		(property "Description" "SPDT DC-2.0GHz absorbative switch, 50 Ohm, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPDT switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.76x4.96mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MSWA-2-20_0_0"
			(text "50"
				(at 1.524 -4.699 900)
			)
			(text "50"
				(at 2.794 -4.699 900)
			)
		)
		(symbol "MSWA-2-20_0_1")
		(symbol "MSWA-2-20_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RF_IN")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CONTROL1")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CONTROL2")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RF_OUT1")
				(number "8")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSWA2-50"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "MSWA2-50"
			(at 12.7 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.51mm_EP1.45x1.45mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/MSWA2-50+.pdf"
			(at -13.97 31.75 0)
		)
		(property "Description" "SPDT DC-5.0GHz absorbative switch, 50 Ohm, QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SPDT switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.51mm*"
			(at 0 0 0)
		)
		(symbol "MSWA2-50_0_0"
			(text "50"
				(at 1.524 -4.699 900)
			)
			(text "50"
				(at 2.794 -4.699 900)
			)
		)
		(symbol "MSWA2-50_0_1")
		(symbol "MSWA2-50_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RF_IN")
				(number "8")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CONTROL1")
				(number "1")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CONTROL2")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RF_OUT1")
				(number "11")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "RF_OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SKY13380-350LF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "SKY13380-350LF"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/SkyWorks/Documents/Products/601-700/201486C.pdf"
			(at -1.27 -13.97 0)
		)
		(property "Description" "SP4T 20MHz-3GHz high power switch, 50 Ohm, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "rf switch sp4t"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*3x3mm*"
			(at 0 0 0)
		)
		(symbol "SKY13380-350LF_0_1")
		(symbol "SKY13380-350LF_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ANT")
				(number "11")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CTRL1")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CTRL2")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "13")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "RF2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "RF3")
				(number "8")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "RF4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SKY13575-639LF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "SKY13575-639LF"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "RF:Skyworks_SKY13575_639LF"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/SkyWorks/Documents/Products/2201-2300/SKY13575_639LF_203270D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SP4T 100MHz-6GHz absorptive switch, 50 Ohm, QFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "rf switch sp4t absorptive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SKY13575?639LF*"
			(at 0 0 0)
		)
		(symbol "SKY13575-639LF_0_1")
		(symbol "SKY13575-639LF_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RFC")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VC1")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VC2")
				(number "9")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "RF1")
				(number "14")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "RF2")
				(number "12")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "RF3")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "RF4")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MASW-007221"
		(extends "MASWSS0136")
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MASW-007221"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://cdn.macom.com/datasheets/masw-007221.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Macom GaAs RF SPDT switch, DC-3GHz, 0.56/12dB loss/isolation, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SWITCH SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MASWSS0115"
		(extends "MASWSS0136")
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MASWSS0115"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://cdn.macom.com/datasheets/maswss0115.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Macom GaAs RF SPDT switch, DC-3GHz, 0.3/22dB loss/isolation, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SWITCH SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MASWSS0143"
		(extends "MASWSS0136")
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MASWSS0143"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/MASWSS0143.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Macom GaAs RF SPDT switch, DC-3GHz, 0.4/16dB loss/isolation, IP 58dB@1GHz, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SWITCH SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MASWSS0151"
		(extends "MASWSS0136")
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MASWSS0151"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/MASWSS0151.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Macom GaAs RF SPDT switch, DC-3GHz, 0.65/21dB loss/isolation, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SWITCH SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MASWSS0166"
		(extends "MASWSS0136")
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MASWSS0166"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/MASWSS0166.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Macom GaAs RF SPDT switch, DC-3GHz, 0.3/12dB loss/isolation, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SWITCH SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MASWSS0176"
		(extends "MASWSS0136")
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MASWSS0176"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/MASWSS0176.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Macom GaAs RF SPDT switch, DC-3GHz, 0.35/21dB loss/isolation, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SWITCH SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MASWSS0192"
		(extends "MASWSS0136")
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MASWSS0192"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/MASWSS0192.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Macom GaAs RF SPDT switch, DC-3GHz, 0.33/13.5dB loss/isolation, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF SWITCH SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
)
