(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "HF-A11-SMT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "HF-A11-SMT"
			(at -15.24 19.05 0)
		)
		(property "Footprint" ""
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.hi-flying.com/index.php?route=tool/upload/download&code=190ec6c62d497905ed783d140f8e5af7a753b8ab"
			(at 0 -7.62 0)
		)
		(property "Description" "WiFi IEEE802.11b/g/n with Ethernet Module, UART, GPIO"
			(at 0 0 0)
		)
		(property "ki_keywords" "WiFi IEEE802.11 b/g/n"
			(at 0 0 0)
		)
		(symbol "HF-A11-SMT_0_1")
		(symbol "HF-A11-SMT_1_1"
			(pin output line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "UART_TXD")
				(number "4")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "UART_RXD")
				(number "5")
			)
			(pin output line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "UART_RTS")
				(number "6")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "UART_CTS")
				(number "7")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "UART1_RXD")
				(number "21")
			)
			(pin output line
				(at -20.32 0 0)
				(length 5.08)
				(name "UART1_TXD")
				(number "22")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "~{RESET}")
				(number "15")
			)
			(pin output line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "~{LINK}")
				(number "14")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "~{READY}")
				(number "16")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "~{RELOAD}")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "3.3V")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 5.08)
				(name "3.3V")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "RF")
				(number "25")
			)
			(pin power_in line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 5.08)
				(name "TX+")
				(number "8")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "TX-")
				(number "9")
			)
			(pin power_out line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "1.8VOUT")
				(number "23")
			)
			(pin passive line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "RX+")
				(number "10")
			)
			(pin passive line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "RX-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USR-C322"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 27.94 0)
		)
		(property "Value" "USR-C322"
			(at 10.16 27.94 0)
		)
		(property "Footprint" "RF_WiFi:USR-C322"
			(at -2.54 -10.16 0)
		)
		(property "Datasheet" "https://www.usriot.com/download/WIFI/USR-C322%20User%20Manual%20V2.3.pdf"
			(at -12.7 27.94 0)
		)
		(property "Description" "802.11 b/g/n Wi-Fi Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "WiFi IEEE802.11 b/g/n"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USR?C322*"
			(at 0 0 0)
		)
		(symbol "USR-C322_1_1"
			(pin output line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "UART0_TX")
				(number "19")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "UART0_RX")
				(number "20")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "UART0_CTS")
				(number "24")
			)
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "UART0_RTS")
				(number "25")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "UART1_TX")
				(number "30")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "UART1_RX")
				(number "31")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{RELOAD}")
				(number "21")
			)
			(pin open_collector line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "~{READY}")
				(number "22")
			)
			(pin open_collector line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "~{LINK}")
				(number "23")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SOP0")
				(number "7")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SOP1")
				(number "6")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "SOP2")
				(number "5")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "ANA_DC-DC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VBT_CC")
				(number "13")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD_ANA2")
				(number "14")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin no_connect line
				(at 5.08 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "43")
			)
			(pin no_connect line
				(at 7.62 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at 15.24 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 15.24 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 15.24 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 15.24 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin no_connect line
				(at 15.24 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "GPIO0")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "GPIO1")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "GPIO2")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "GPIO3")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "GPIO4")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GPIO5")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GPIO6")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "GPIO7")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "GPIO8")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "GPIO9")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GPIO10")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO11")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO12")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "GPIO13")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
)
