(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CC2520"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "CC2520"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/cc2520"
			(at 0 -6.35 0)
		)
		(property "Description" "2.4 GHz ZigBee/IEEE 802.15.4 RF transceiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.4GHz rf transceiver ZigBee 802.15.4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*28*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CC2520_0_1")
		(symbol "CC2520_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "25")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "VREG_EN")
				(number "26")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "28")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "SI")
				(number "2")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "SO")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "GPIO0")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "GPIO1")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "GPIO2")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "GPIO3")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "GPIO4")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "GPIO5")
				(number "4")
			)
			(pin passive line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "XOSC_Q1")
				(number "13")
			)
			(pin passive line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "XOSC_Q2")
				(number "12")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "AVDD1")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "AVDD2")
				(number "16")
			)
			(pin no_connect line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "AVDD3")
				(number "14")
			)
			(pin no_connect line
				(at 5.08 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "AVDD4")
				(number "22")
			)
			(pin power_in line
				(at 10.16 25.4 270)
				(length 2.54)
				(name "AVDD5")
				(number "11")
			)
			(pin power_in line
				(at 12.7 25.4 270)
				(length 2.54)
				(name "AVDD_GUARD")
				(number "24")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "RF_P")
				(number "17")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RF_N")
				(number "19")
			)
			(pin passive line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "DCOUPL")
				(number "27")
			)
			(pin passive line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RBIAS")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC13192"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 26.67 0)
		)
		(property "Value" "MC13192"
			(at 13.97 -29.21 0)
		)
		(property "Footprint" ""
			(at -10.16 -12.7 0)
		)
		(property "Datasheet" "https://www.nxp.com/products/no-longer-manufactured/2.4-ghz-low-power-transceiver-for-802.15.4:MC13192"
			(at -10.16 -12.7 0)
		)
		(property "Description" "2.4 GHz, Low Power Transceiver for 802.15.4 (Zigbee controller)"
			(at 0 0 0)
		)
		(property "ki_keywords" "ZIGBEE"
			(at 0 0 0)
		)
		(symbol "MC13192_0_1")
		(symbol "MC13192_1_1"
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "GPIO1")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "GPIO2")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "GPIO3")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "GPIO4")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "GPIO5")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "GPIO6")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "GPIO7")
				(number "25")
			)
			(pin input line
				(at -27.94 0 0)
				(length 7.62)
				(name "CEBi")
				(number "19")
			)
			(pin tri_state line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "MISOo")
				(number "18")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "MOSIi")
				(number "17")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "SPICLKi")
				(number "16")
			)
			(pin open_collector line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "IRQBo")
				(number "20")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "ATTNBi")
				(number "14")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "RXTXENi")
				(number "13")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "RSTBi")
				(number "12")
			)
			(pin output line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "CLKOo")
				(number "15")
			)
			(pin power_out line
				(at -12.7 33.02 270)
				(length 7.62)
				(name "VDDVCO")
				(number "30")
			)
			(pin power_out line
				(at -10.16 33.02 270)
				(length 7.62)
				(name "VDDD")
				(number "21")
			)
			(pin power_in line
				(at -7.62 33.02 270)
				(length 7.62)
				(name "VDDLO2")
				(number "28")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 7.62)
				(name "VDDLO1")
				(number "29")
			)
			(pin power_out line
				(at 0 33.02 270)
				(length 7.62)
				(name "VDDA")
				(number "32")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 7.62)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 7.62 33.02 270)
				(length 7.62)
				(name "VDDIN")
				(number "22")
			)
			(pin input line
				(at 10.16 33.02 270)
				(length 7.62)
				(name "VBATT")
				(number "31")
			)
			(pin input line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "RFIN-")
				(number "1")
			)
			(pin input line
				(at 25.4 12.7 180)
				(length 7.62)
				(name "RFIN+")
				(number "2")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "TINJ_P")
				(number "3")
			)
			(pin input line
				(at 25.4 0 180)
				(length 7.62)
				(name "TINJ_M")
				(number "4")
			)
			(pin open_collector line
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "PAO_P")
				(number "5")
			)
			(pin open_collector line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "PAO_M")
				(number "6")
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 7.62)
				(name "SM")
				(number "7")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "XTALin")
				(number "26")
			)
			(pin output line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "XTALout")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TWE-L-DP-W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "TWE-L-DP-W"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "https://www.mono-wireless.com/jp/products/TWE-Lite-DIP/MW-PDS-TWELITEDIP-JP.pdf"
			(at 19.05 -25.4 0)
		)
		(property "Description" "NXP JN5164/JN5169 breakout module, DIP"
			(at 0 0 0)
		)
		(property "ki_keywords" "TWELITE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*28*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "TWE-L-DP-W_1_0")
		(symbol "TWE-L-DP-W_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "DIO10/M1")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "DIO2/M2")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "DIO3/M3")
				(number "27")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DIO17/BPS")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIO12/DI1")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DIO13/DI2")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DIO11/DI3")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DIO16/DI4")
				(number "18")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "ADC1/AI1")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "DIO0/AI2")
				(number "23")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "ADC2/AI3")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DIO1/AI4")
				(number "25")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "DIO18/DO1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DIO19/DO2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DIO4/DO3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DIO9/DO4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DIO5/PWM1")
				(number "4")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DO0/PWM2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DO1/PWM3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "DIO8/PWM4")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DIO7/RX")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DIO6/TX")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DIO14/SCL")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "DIO15/SDA")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TWE-L-WX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "TWE-L-WX"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "RF_Module:MonoWireless_TWE-L-WX"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.mono-wireless.com/jp/products/TWE-LITE/MW-PDS-TWELITE-JP.pdf"
			(at 19.05 -25.4 0)
		)
		(property "Description" "NXP JN5164/JN5169 breakout module, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "TWELITE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MonoWireless?TWE*"
			(at 0 0 0)
		)
		(symbol "TWE-L-WX_1_0")
		(symbol "TWE-L-WX_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "DIO10/M1")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "DIO2/M2")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "DIO3/M3")
				(number "27")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DIO17/BPS")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIO12/DI1")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DIO13/DI2")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DIO11/DI3")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DIO16/DI4")
				(number "18")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "ADC1/AI1")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "DIO0/AI2")
				(number "24")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "ADC2/AI3")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DIO1/AI4")
				(number "25")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin no_connect line
				(at 15.24 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "DIO18/DO1")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DIO19/DO2")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DIO4/DO3")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DIO9/DO4")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DIO5/PWM1")
				(number "7")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DO0/PWM2")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DO1/PWM3")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "DIO8/PWM4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DIO7/RX")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DIO6/TX")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DIO14/SCL")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "DIO15/SDA")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XBee_SMT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.384 26.162 0)
		)
		(property "Value" "XBee_SMT"
			(at -20.828 24.384 0)
		)
		(property "Footprint" "RF_Module:Digi_XBee_SMT"
			(at 21.336 -26.924 0)
		)
		(property "Datasheet" "http://www.digi.com/resources/documentation/digidocs/pdfs/90002126.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Digi Xbee SMT RF module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digi XBee"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Digi*XBee*SMT*"
			(at 0 0 0)
		)
		(symbol "XBee_SMT_0_1")
		(symbol "XBee_SMT_1_1"
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "DIO13/UART_TX")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "DIO14/UART_RX/~{CONFIG}")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "DIO7/~{CTS}")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "DIO6/~{RTS}")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "DIO3/AD3")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "DIO2/AD2")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "DIO1/AD1")
				(number "32")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "DIO0/AD0")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "RESET/OD_OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "DIO8/SLEEP_REQUEST")
				(number "10")
			)
			(pin output line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "DIO19/SPI_~{ATTN}")
				(number "12")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "DIO18/SPI_CLK")
				(number "14")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "DIO17/SPI_~{SSEL}")
				(number "15")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "DIO16/SPI_MOSI")
				(number "16")
			)
			(pin output line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "DIO15/SPI_MISO")
				(number "17")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin input line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VREF")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "35")
			)
			(pin no_connect line
				(at 25.4 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 25.4 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 25.4 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 25.4 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at 25.4 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at 25.4 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at 25.4 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 25.4 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "DIO12")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "DIO10/RSSI/PWM0")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "DIO11/PWM1")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "DIO4")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "DIO9/ON/~{SLEEP}")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "DIO5/ASSOCIATE")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "RF")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MW-R-DP-W"
		(extends "TWE-L-DP-W")
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "MW-R-DP-W"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "https://www.mono-wireless.com/jp/products/TWE-Lite-DIP/MW-PDS-TWELITEDIP-JP.pdf"
			(at 19.05 -25.4 0)
		)
		(property "Description" "NXP JN5164/JN5169 breakout module, DIP"
			(at 0 0 0)
		)
		(property "ki_keywords" "TWELITE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*28*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MW-R-WX"
		(extends "TWE-L-WX")
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "MW-R-WX"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "RF_Module:MonoWireless_TWE-L-WX"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.mono-wireless.com/jp/products/TWE-LITE/MW-PDS-TWELITE-JP.pdf"
			(at 19.05 -25.4 0)
		)
		(property "Description" "NXP JN5164/JN5169 breakout module, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "TWELITE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MonoWireless?TWE*"
			(at 0 0 0)
		)
	)
)
