(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD586"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "AD586"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD586.pdf"
			(at -1.27 1.27 0)
		)
		(property "Description" "High Precision, 5V Reference, DIP-8, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD586_0_1")
		(symbol "AD586_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "TRIM")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "NR")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADR1399KEZ"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "ADR1399KEZ"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_LCC:Analog_LCC-8_5x5mm_P1.27mm"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr1399.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Oven-Compensated, Buried Zener, 7.05 V Voltage Reference, LCC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Zener diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*LCC?8*5x5mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADR1399KEZ_0_0"
			(text "+"
				(at -3.81 1.905 0)
			)
		)
		(symbol "ADR1399KEZ_0_1")
		(symbol "ADR1399KEZ_1_1"
			(text "-"
				(at -3.81 -1.905 0)
			)
			(text "F"
				(at 0.635 1.905 0)
			)
			(text "F"
				(at 0.635 -1.905 0)
			)
			(text "S"
				(at 3.175 1.905 0)
			)
			(text "S"
				(at 3.175 -1.905 0)
			)
			(pin power_in line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "HEATER+")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -5.08 90)
				(length 2.54)
				(name "HEATER-")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "+REFF")
				(number "6")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "-REFF")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "+REFS")
				(number "7")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "-REFS")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADR1399KHZ"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "ADR1399KHZ"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:Analog_TO-46-4_ThermalShield"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr1399.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Oven-Compensated, Buried Zener, 7.05 V Voltage Reference, TO-46-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Zener diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*TO?46*"
			(at 0 0 0)
		)
		(symbol "ADR1399KHZ_0_0"
			(text "+"
				(at -1.27 1.905 0)
			)
		)
		(symbol "ADR1399KHZ_0_1")
		(symbol "ADR1399KHZ_1_1"
			(text "-"
				(at -1.27 -1.905 0)
			)
			(pin power_in line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADR420ARMZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR420ARMZ"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr420_421_423_425.pdf"
			(at 0 3.81 0)
		)
		(property "Description" "2.048V Voltage Reference, Ultraprecision, Low Noise, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADR420ARMZ_0_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "TP")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "TP")
				(number "8")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "TRIM")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADR440ARMZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.382 0)
		)
		(property "Value" "ADR440ARMZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 20.828 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "2.048V Voltage Reference, Ultraprecision, Low Noise, MSOP-8"
			(at 32.258 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADR440ARMZ_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V_{IN}")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "TRIM")
				(number "5")
			)
		)
		(symbol "ADR440ARMZ_1_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CJ432"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "CJ432"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.cj-elec.com/txUpfile/20134181474991806.pdf"
			(at 0 0 0)
		)
		(property "Description" "Shunt Regulator, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "CJ432_0_1")
		(symbol "CJ432_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL21070DIH306Z-TK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.635 8.255 0)
		)
		(property "Value" "ISL21070DIH306Z-TK"
			(at -1.905 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 12.7 -6.35 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/fn75/fn7599.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.6V 25μA Micropower Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Reference 0.6V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ISL21070DIH306Z-TK_0_1")
		(symbol "ISL21070DIH306Z-TK_1_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "Vout")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM285D-1.2"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 3.175 0)
		)
		(property "Value" "LM285D-1.2"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1.235V Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM285D-1.2_0_1")
		(symbol "LM285D-1.2_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM285M-ADJ"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.905 3.81 0)
		)
		(property "Value" "LM285M-ADJ"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm185-adj.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM285M-ADJ_0_1")
		(symbol "LM285M-ADJ_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin input line
				(at 0 5.08 270)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM285S-1.2"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM285S-1.2"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.254 -4.064 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/185fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.235V Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM285S-1.2_0_1")
		(symbol "LM285S-1.2_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(hide yes)
				(name "K")
				(number "6")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM285Z-2.5"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM285Z-2.5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "2.5V Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
		(symbol "LM285Z-2.5_0_1")
		(symbol "LM285Z-2.5_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM285Z-ADJ"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.905 3.81 0)
		)
		(property "Value" "LM285Z-ADJ"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm185-adj.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LM285Z-ADJ_0_1")
		(symbol "LM285Z-ADJ_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at 0 5.08 270)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM329xZ"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM329xZ"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/129329fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "6.9V Precision Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LM329xZ_0_1")
		(symbol "LM329xZ_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin no_connect line
				(at 0 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM399"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 1.27 0)
		)
		(property "Value" "LM399"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:Analog_TO-46-4_ThermalShield"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/199399fc.pdf"
			(at 0 2.54 90)
		)
		(property "Description" "Precision Reference, 6.95V, Buried Zener Diode with Thermal Shielding Can, TO-46-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Zener diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*TO?46*"
			(at 0 0 0)
		)
		(symbol "LM399_0_0"
			(text "+"
				(at -1.27 3.937 0)
			)
		)
		(symbol "LM399_0_1")
		(symbol "LM399_1_1"
			(text "-"
				(at -1.27 -3.683 0)
			)
			(pin power_in line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4030-4.096"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4030-4.096"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4030.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V Ultra-High Precision Shunt Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "LM4030-4.096_0_1")
		(symbol "LM4030-4.096_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4040DBZ-2.0"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DBZ-2.0"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.048V Precision Micropower Shunt Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM4040DBZ-2.0_0_1")
		(symbol "LM4040DBZ-2.0_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin no_connect line
				(at -1.27 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4040DCK-2.0"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DCK-2.0"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.048V Precision Micropower Shunt Voltage Reference, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "LM4040DCK-2.0_0_1")
		(symbol "LM4040DCK-2.0_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin no_connect line
				(at -1.27 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 0 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 1.27 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4041LP-ADJ"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 3.81 0)
		)
		(property "Value" "LM4041LP-ADJ"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4041-n.pdf"
			(at 2.54 3.81 0)
		)
		(property "Description" "Adjustable Precision Micropower Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LM4041LP-ADJ_0_1")
		(symbol "LM4041LP-ADJ_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at 0 5.08 270)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4125AIM5-2.5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.255 0)
		)
		(property "Value" "LM4125AIM5-2.5"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4125.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V ±0.2% Precision Micropower Low Dropout Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Micropower Low Dropout Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM4125AIM5-2.5_0_1")
		(symbol "LM4125AIM5-2.5_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "Vout")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4128"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LM4128"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4128.pdf"
			(at 0 2.54 90)
		)
		(property "Description" "2.5V ±0.2% Precision Micropower Low Dropout Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Micropower Low Dropout Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM4128_0_1")
		(symbol "LM4128_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VREF")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM4132xMF-1.8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.318 6.096 0)
		)
		(property "Value" "LM4132xMF-1.8"
			(at 7.874 6.096 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4132.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Low Dropout Voltage Reference, 1.8V, ±0.05% to ±0.5%, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Low Dropout Voltage Reference 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM4132xMF-1.8_0_1")
		(symbol "LM4132xMF-1.8_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VREF")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1009xS8"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.905 3.81 0)
		)
		(property "Value" "LT1009xS8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1009.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC?8*"
			(at 0 0 0)
		)
		(symbol "LT1009xS8_0_1")
		(symbol "LT1009xS8_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin input line
				(at 0 5.08 270)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "6")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(hide yes)
				(name "K")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1019xN8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1019xN8"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1019fd.pdf"
			(at -10.16 3.81 0)
		)
		(property "Description" "Precision Reference, Ultra Low Drift, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1019xN8_0_1")
		(symbol "LT1019xN8_1_0"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "TEMP")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "7")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "TRIM")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1461AxS8-2.5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461AxS8-2.5"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.04%, 2.5V, 100mA, 3V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1461AxS8-2.5_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1634BCMS8-1.25"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634BCMS8-1.25"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.25V Micropower Precision Shunt Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP?8*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT1634BCMS8-1.25_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin input line
				(at 0 5.08 270)
				(length 2.54)
				(name "Test")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1634CCZ-1.25"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634CCZ-1.25"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.25V Micropower Precision Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LT1634CCZ-1.25_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at 0 5.08 270)
				(length 2.54)
				(name "Test")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1634xxS8-1.25"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634xxS8-1.25"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "1.25V Micropower Precision Shunt Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1634xxS8-1.25_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin input line
				(at 0 5.08 270)
				(length 2.54)
				(name "Test")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "K")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1790-1.25"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LT1790-1.25"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1790fc.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "1.25V Voltage Reference, Low Dropout, Micropower, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?6*"
			(at 0 0 0)
		)
		(symbol "LT1790-1.25_0_1")
		(symbol "LT1790-1.25_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 5.08 0 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT6657AHMS8-2.5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT6657AHMS8-2.5"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6657fd.pdf"
			(at 1.27 -8.89 0)
		)
		(property "Description" "Precision voltage reference, 40V input, 10mA output, 1.5ppm/C drift, 2.5V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT6657AHMS8-2.5_0_1")
		(symbol "LT6657AHMS8-2.5_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6035xSA25"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6035xSA25"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6035.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "2.5V, High-Supply-Voltage, Precision Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX6035xSA25_0_0"
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
		)
		(symbol "MAX6035xSA25_0_1")
		(symbol "MAX6035xSA25_1_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6070AAUT12+T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT12+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max6070-max6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.25V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX6070AAUT12+T_0_1")
		(symbol "MAX6070AAUT12+T_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FILTER")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTF")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTS")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6071AAUT12+T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071AAUT12+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max6070-max6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.25V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX6071AAUT12+T_0_1")
		(symbol "MAX6071AAUT12+T_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GNDF")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GNDS")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTF")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTS")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6100"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6100-MAX6107.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "Low-dropout high current voltage reference, 1.800V, ±0.4% accuracy, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX6100_0_1")
		(symbol "MAX6100_1_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6350"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "MAX6350"
			(at 1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at 30.48 -11.43 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6325-MAX6350.pdf"
			(at 2.54 -10.16 0)
		)
		(property "Description" "0.5ppm/°C Low-Noise +5V Voltage Reference, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX6350_0_1")
		(symbol "MAX6350_1_1"
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "NR")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "TRIM")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX874"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX874"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://pdfserv.maximintegrated.com/en/ds/MAX872-MAX874.pdf"
			(at 0 0 0)
		)
		(property "Description" "10µA Low-Dropout Precision Voltage Reference, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low-Dropout Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX874_0_1")
		(symbol "MAX874_1_1"
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "TRIM")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "IC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "IC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "COMP")
				(number "8")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Temper")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1501-10xCH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1501-10xCH"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.024V, 0.1%, 20mA, Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 1.024V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1501-10xCH_0_0"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(symbol "MCP1501-10xCH_0_1")
		(embedded_fonts no)
	)
	(symbol "MCP1501-10xRW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-10xRW"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "1.024V, 0.1%, 20mA, Precision Voltage Reference, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 1.024V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP1501-10xRW_0_0"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
		)
		(symbol "MCP1501-10xRW_0_1")
		(embedded_fonts no)
	)
	(symbol "MCP1501-10xSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-10xSN"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "1.024V, 0.1%, 20mA, Precision Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 1.024V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP1501-10xSN_0_0"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
		)
		(symbol "MCP1501-10xSN_0_1")
		(embedded_fonts no)
	)
	(symbol "MCP1525-TO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MCP1525-TO"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21653b.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
		(symbol "MCP1525-TO_0_1")
		(symbol "MCP1525-TO_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Vout")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1525-TT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.255 0)
		)
		(property "Value" "MCP1525-TT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21653b.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1525-TT_0_1")
		(symbol "MCP1525-TT_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "Vss")
				(number "3")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Vout")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF02AP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF02AP"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref02.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "5V ±15mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "REF02AP_0_1")
		(symbol "REF02AP_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "TEMP")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "TRIM")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF102AP"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.635 8.255 0)
		)
		(property "Value" "REF102AP"
			(at -1.905 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -1.27 10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref102.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "10V ±10mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "REF102AP_0_1")
		(symbol "REF102AP_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "TEMP")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "NR")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "TRIM")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF102AU"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.255 0)
		)
		(property "Value" "REF102AU"
			(at 3.175 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref02.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V ±10mV Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "REF102AU_0_1")
		(symbol "REF102AU_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "TEMP")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "NR")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "TRIM")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF191"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "REF191"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/REF19xSeries.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Precision voltage references 2.048V, DIP-8/SO-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision voltage references"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9m*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "REF191_0_1")
		(symbol "REF191_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{Sleep}")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "TP")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "TP")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF2025"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 5.08 7.62 0)
		)
		(property "Value" "REF2025"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.016 -9.906 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref2033.pdf"
			(at 1.778 -13.208 0)
		)
		(property "Description" "2.5V Low-Drift, Low-Power, Dual-Output, VREF and VREF / 2 Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "REF2025_0_1")
		(symbol "REF2025_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "Vref")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "Vbias")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF3012"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "REF3012"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3033.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "1.25V 50-ppm/°C Max, 50-μA, CMOS Voltage Reference, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "REF3012_0_1")
		(symbol "REF3012_1_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF3212AMDBVREP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "REF3212AMDBVREP"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.905 -9.525 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3240-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1.25V 100μA Micropower Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Precision Voltage Reference 1.25V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "REF3212AMDBVREP_0_1")
		(symbol "REF3212AMDBVREP_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ENABLE")
				(number "3")
			)
			(pin input line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GNDS")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GNDF")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT_F")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT_S")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF35102QDBVR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35102QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "1.024V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "REF35102QDBVR_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "NR")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF5020AD"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5020AD"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "2.048V 0.1% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 2.048V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "REF5020AD_0_1")
		(symbol "REF5020AD_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "Temp")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Trim/NR")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF5020ADGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5020ADGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.048V 0.1% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 2.048V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "REF5020ADGK_0_1")
		(symbol "REF5020ADGK_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "Temp")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Trim/NR")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF6025xDGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "REF6025xDGK"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref6025.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V 0.05% 4mA Extremely Low Noise High Precision Voltage Reference, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "low Noise precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "REF6025xDGK_0_1")
		(symbol "REF6025xDGK_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "FILT")
				(number "4")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND_S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND_F")
				(number "7")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT_S")
				(number "5")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT_F")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431D"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -2.54 0)
		)
		(property "Value" "TL431D"
			(at 0 -4.445 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 0.254 -10.668 0)
		)
		(property "Description" "Shunt Regulator, SO-8"
			(at -0.254 -8.382 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TL431D_0_1")
		(symbol "TL431D_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "8")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431DBV"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -2.54 0)
		)
		(property "Value" "TL431DBV"
			(at 0 -4.445 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at -0.508 -8.382 0)
		)
		(property "Description" "Shunt Regulator, SOT-23-5"
			(at -0.254 -10.414 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "TL431DBV_0_1")
		(symbol "TL431DBV_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "4")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "K")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431DBZ"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL431DBZ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 1.778 -9.144 0)
		)
		(property "Description" "Shunt Regulator, SOT-23"
			(at 0 -7.112 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TL431DBZ_0_1")
		(symbol "TL431DBZ_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "2")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431DCK"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL431DCK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.572 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 1.27 -8.382 0)
		)
		(property "Description" "Shunt Regulator, SC-70"
			(at -0.508 -6.35 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "TL431DCK_0_1")
		(symbol "TL431DCK_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "3")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431KTP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL431KTP"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/760499.pdf"
			(at 0.508 -6.35 0)
		)
		(property "Description" "Shunt Regulator, TO-252"
			(at 0.762 -8.89 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
		(symbol "TL431KTP_0_1")
		(symbol "TL431KTP_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "K")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431LP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL431LP"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 0.508 -7.112 0)
		)
		(property "Description" "Shunt Regulator, TO-92"
			(at 0 -8.89 0)
		)
		(property "ki_keywords" "diode device regulator shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
		(symbol "TL431LP_0_1")
		(symbol "TL431LP_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "K")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431P"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL431P"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -4.572 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 1.27 -8.382 0)
		)
		(property "Description" "Shunt Regulator, PDIP-8"
			(at 0 -6.35 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TL431P_0_1")
		(symbol "TL431P_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "8")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431PK"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL431PK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 -4.318 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 1.27 -7.874 0)
		)
		(property "Description" "Shunt Regulator, SOT-89"
			(at 0 -6.096 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*89*"
			(at 0 0 0)
		)
		(symbol "TL431PK_0_1")
		(symbol "TL431PK_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "K")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431PS"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL431PS"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -4.826 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 1.016 -7.112 0)
		)
		(property "Description" "Shunt Regulator, MSOP-8"
			(at 0 -9.144 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TL431PS_0_1")
		(symbol "TL431PS_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "8")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL431PW"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL431PW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 0 -4.318 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 1.016 -6.35 0)
		)
		(property "Description" "Shunt Regulator, TSSOP-8"
			(at 0 -8.382 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TL431PW_0_1")
		(symbol "TL431PW_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "8")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL432DBV"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL432DBV"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 0.508 -6.604 0)
		)
		(property "Description" "Shunt Regulator, SOT-23-5"
			(at 0.254 -8.636 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "TL432DBV_0_1")
		(symbol "TL432DBV_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "5")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "K")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL432DBZ"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL432DBZ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.318 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 0.762 -6.096 0)
		)
		(property "Description" "Shunt Regulator, SOT-23"
			(at 0 -7.874 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TL432DBZ_0_1")
		(symbol "TL432DBZ_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL432PK"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" "TL432PK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 -4.318 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf"
			(at 1.524 -6.096 0)
		)
		(property "Description" "Shunt Regulator, SOT-89"
			(at 0 -7.874 0)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*89*"
			(at 0 0 0)
		)
		(symbol "TL432PK_0_1")
		(symbol "TL432PK_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "REF")
				(number "3")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLE2425xD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "TLE2425xD"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tle2425.pdf"
			(at -35.56 25.4 0)
		)
		(property "Description" "Precision virtual ground, 2.5V output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rail splitter precision virtual ground 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLE2425xD_0_1")
		(symbol "TLE2425xD_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "COMMON")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLE2426xD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.414 8.89 0)
		)
		(property "Value" "TLE2426xD"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tle2426.pdf"
			(at -35.56 24.13 0)
		)
		(property "Description" "Precision virtual ground, noise reduction pin, 4V to 40V input, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rail splitter precision virtual ground"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLE2426xD_0_1")
		(symbol "TLE2426xD_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "NOISE_REDUCTION")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COMMON")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLE2426xLP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 6.35 0)
		)
		(property "Value" "TLE2426xLP"
			(at 11.43 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tle2426.pdf"
			(at -35.56 21.59 0)
		)
		(property "Description" "Precision virtual ground, 4V to 40V input, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rail splitter precision virtual ground"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "TLE2426xLP_0_1")
		(symbol "TLE2426xLP_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "COMMON")
				(number "2")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADR421ARMZ"
		(extends "ADR420ARMZ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR421ARMZ"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr420_421_423_425.pdf"
			(at 0 3.81 0)
		)
		(property "Description" "2.50V Voltage Reference, Ultraprecision, Low Noise, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.5V voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR423ARMZ"
		(extends "ADR420ARMZ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR423ARMZ"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr420_421_423_425.pdf"
			(at 0 3.81 0)
		)
		(property "Description" "3.00V Voltage Reference, Ultraprecision, Low Noise, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "3V voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR425ARMZ"
		(extends "ADR420ARMZ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR425ARMZ"
			(at 3.81 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr420_421_423_425.pdf"
			(at 0 3.81 0)
		)
		(property "Description" "5.00V Voltage Reference, Ultraprecision, Low Noise, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR440xRZ"
		(extends "ADR440ARMZ")
		(property "Reference" "U"
			(at 2.032 8.382 0)
		)
		(property "Value" "ADR440xRZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 22.352 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "2.048V Voltage Reference, Ultraprecision, Low Noise, SOIC-8"
			(at 32.258 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR441ARMZ"
		(extends "ADR440ARMZ")
		(property "Reference" "U"
			(at 1.27 8.636 0)
		)
		(property "Value" "ADR441ARMZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 21.082 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "2.5V Voltage Reference, Ultraprecision, Low Noise, MSOP-8"
			(at 30.988 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR441xRZ"
		(extends "ADR440ARMZ")
		(property "Reference" "U"
			(at 2.032 8.382 0)
		)
		(property "Value" "ADR441xRZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 22.352 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "2.5V Voltage Reference, Ultraprecision, Low Noise, SOIC-8"
			(at 30.734 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR443ARMZ"
		(extends "ADR440ARMZ")
		(property "Reference" "U"
			(at 1.27 8.382 0)
		)
		(property "Value" "ADR443ARMZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 20.828 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "3V Voltage Reference, Ultraprecision, Low Noise, MSOP-8"
			(at 29.972 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR443xRZ"
		(extends "ADR440ARMZ")
		(property "Reference" "U"
			(at 2.032 8.382 0)
		)
		(property "Value" "ADR443xRZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 22.352 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "3V Voltage Reference, Ultraprecision, Low Noise, SOIC-8"
			(at 29.972 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR444ARMZ"
		(extends "ADR440ARMZ")
		(property "Reference" "U"
			(at 1.27 8.636 0)
		)
		(property "Value" "ADR444ARMZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 21.082 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "4.096V Voltage Reference, Ultraprecision, Low Noise, MSOP-8"
			(at 32.258 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR444xRZ"
		(extends "ADR440ARMZ")
		(property "Reference" "U"
			(at 2.032 8.382 0)
		)
		(property "Value" "ADR444xRZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 22.352 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "4.096V Voltage Reference, Ultraprecision, Low Noise, SOIC-8"
			(at 32.258 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR445ARMZ"
		(extends "ADR440ARMZ")
		(property "Reference" "U"
			(at 1.27 8.382 0)
		)
		(property "Value" "ADR445ARMZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 20.828 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "5V Voltage Reference, Ultraprecision, Low Noise, MSOP-8"
			(at 29.972 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR445xRZ"
		(extends "ADR440ARMZ")
		(property "Reference" "U"
			(at 2.032 8.382 0)
		)
		(property "Value" "ADR445xRZ"
			(at 6.858 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 22.352 -14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adr440_441_443_444_445.pdf"
			(at 53.594 -11.938 0)
		)
		(property "Description" "5V Voltage Reference, Ultraprecision, Low Noise, SOIC-8"
			(at 29.718 -9.652 0)
		)
		(property "ki_keywords" "voltage reference Ultraprecision Low Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR4520"
		(extends "MAX6035xSA25")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR4520"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADR4520_4525_4530_4533_4540_4550.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "2.048V, Ultralow Noise, High Accuracy Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR4525"
		(extends "MAX6035xSA25")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR4525"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADR4520_4525_4530_4533_4540_4550.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "2.5V, Ultralow Noise, High Accuracy Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR4530"
		(extends "MAX6035xSA25")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR4530"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADR4520_4525_4530_4533_4540_4550.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "3.0V,  Ultralow Noise, High Accuracy Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR4533"
		(extends "MAX6035xSA25")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR4533"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADR4520_4525_4530_4533_4540_4550.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "3.3V,  Ultralow Noise, High Accuracy Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR4540"
		(extends "MAX6035xSA25")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR4540"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADR4520_4525_4530_4533_4540_4550.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "4.096V,  Ultralow Noise, High Accuracy Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADR4550"
		(extends "MAX6035xSA25")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "ADR4550"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADR4520_4525_4530_4533_4540_4550.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "5.0V,  Ultralow Noise, High Accuracy Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISL21070CIH320Z-TK"
		(extends "ISL21070DIH306Z-TK")
		(property "Reference" "U"
			(at -0.635 8.255 0)
		)
		(property "Value" "ISL21070CIH320Z-TK"
			(at -1.905 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 12.7 -6.35 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/fn75/fn7599.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.0V 25μA Micropower Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Reference 2.0V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ISL21070CIH325Z-TK"
		(extends "ISL21070DIH306Z-TK")
		(property "Reference" "U"
			(at -0.635 8.255 0)
		)
		(property "Value" "ISL21070CIH325Z-TK"
			(at -1.905 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 12.7 -6.35 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/fn75/fn7599.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V 25μA Micropower Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM285D-2.5"
		(extends "LM285D-1.2")
		(property "Reference" "U"
			(at 0 3.175 0)
		)
		(property "Value" "LM285D-2.5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "2.500V Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM285S-2.5"
		(extends "LM285S-1.2")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM285S-2.5"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.254 -4.064 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/185fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.500V Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM285Z-1.2"
		(extends "LM285Z-2.5")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM285Z-1.2"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1.235V Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM385BZ-1.2"
		(extends "LM285Z-2.5")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM385BZ-1.2"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1.235V Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM385BZ-2.5"
		(extends "LM285Z-2.5")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM385BZ-2.5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "2.5V Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM385D-1.2"
		(extends "LM285D-1.2")
		(property "Reference" "U"
			(at 0 3.175 0)
		)
		(property "Value" "LM385D-1.2"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1.235V Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM385D-2.5"
		(extends "LM285D-1.2")
		(property "Reference" "U"
			(at 0 3.175 0)
		)
		(property "Value" "LM385D-2.5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "2.500V Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM385M-ADJ"
		(extends "LM285M-ADJ")
		(property "Reference" "U"
			(at 1.905 3.81 0)
		)
		(property "Value" "LM385M-ADJ"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm185-adj.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM385S-1.2"
		(extends "LM285S-1.2")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM385S-1.2"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.254 -4.064 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/185fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.235V Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM385S-2.5"
		(extends "LM285S-1.2")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM385S-2.5"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.254 -4.064 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/185fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.500V Micropower Voltage Reference Diodes, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM385Z-1.2"
		(extends "LM285Z-2.5")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM385Z-1.2"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1.235V Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM385Z-2.5"
		(extends "LM285Z-2.5")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM385Z-2.5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/LM285-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "2.5V Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM385Z-ADJ"
		(extends "LM285Z-ADJ")
		(property "Reference" "U"
			(at 1.905 3.81 0)
		)
		(property "Value" "LM385Z-ADJ"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm185-adj.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LM4030-2.5"
		(extends "LM4030-4.096")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4030-2.5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4030.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.500V Ultra-High Precision Shunt Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DBZ-10"
		(extends "LM4040DBZ-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DBZ-10"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "10.00V Precision Micropower Shunt Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DBZ-2.5"
		(extends "LM4040DBZ-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DBZ-2.5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.500V Precision Micropower Shunt Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DBZ-3"
		(extends "LM4040DBZ-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DBZ-3"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.000V Precision Micropower Shunt Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DBZ-4.1"
		(extends "LM4040DBZ-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DBZ-4.1"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V Precision Micropower Shunt Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DBZ-5"
		(extends "LM4040DBZ-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DBZ-5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.000V Precision Micropower Shunt Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DBZ-8.2"
		(extends "LM4040DBZ-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DBZ-8.2"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "8.192V Precision Micropower Shunt Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DCK-10"
		(extends "LM4040DCK-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DCK-10"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "10.0V Precision Micropower Shunt Voltage Reference, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DCK-2.5"
		(extends "LM4040DCK-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DCK-2.5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.500V Precision Micropower Shunt Voltage Reference, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DCK-3"
		(extends "LM4040DCK-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DCK-3"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.000V Precision Micropower Shunt Voltage Reference, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DCK-4.1"
		(extends "LM4040DCK-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DCK-4.1"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V Precision Micropower Shunt Voltage Reference, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DCK-5"
		(extends "LM4040DCK-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DCK-5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.000V Precision Micropower Shunt Voltage Reference, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040DCK-8.2"
		(extends "LM4040DCK-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040DCK-8.2"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "8.192V Precision Micropower Shunt Voltage Reference, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040LP-2.0"
		(extends "LM285Z-2.5")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040LP-2.0"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.048V Precision Micropower Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM4125IM5-2.0"
		(extends "LM4125AIM5-2.5")
		(property "Reference" "U"
			(at 1.27 8.255 0)
		)
		(property "Value" "LM4125IM5-2.0"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4125.pdf"
			(at 0 0 0)
		)
		(property "Description" "2V ±0.5% Precision Micropower Low Dropout Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Micropower Low Dropout Voltage Reference 2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4125IM5-2.5"
		(extends "LM4125AIM5-2.5")
		(property "Reference" "U"
			(at 1.27 8.255 0)
		)
		(property "Value" "LM4125IM5-2.5"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4125.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V ±0.5% Precision Micropower Low Dropout Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Micropower Low Dropout Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4132xMF-2.0"
		(extends "LM4132xMF-1.8")
		(property "Reference" "U"
			(at -4.318 6.096 0)
		)
		(property "Value" "LM4132xMF-2.0"
			(at 7.874 6.096 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4132.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Low Dropout Voltage Reference, 2.048V, ±0.05% to ±0.5%, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Low Dropout Voltage Reference 2.048V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4132xMF-2.5"
		(extends "LM4132xMF-1.8")
		(property "Reference" "U"
			(at -4.318 6.096 0)
		)
		(property "Value" "LM4132xMF-2.5"
			(at 7.874 6.096 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4132.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Low Dropout Voltage Reference, 2.5V, ±0.05% to ±0.5%, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Low Dropout Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4132xMF-3.0"
		(extends "LM4132xMF-1.8")
		(property "Reference" "U"
			(at -4.318 6.096 0)
		)
		(property "Value" "LM4132xMF-3.0"
			(at 7.874 6.096 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4132.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Low Dropout Voltage Reference, 3.0V, ±0.05% to ±0.5%, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Low Dropout Voltage Reference 3.0V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4132xMF-3.3"
		(extends "LM4132xMF-1.8")
		(property "Reference" "U"
			(at -4.318 6.096 0)
		)
		(property "Value" "LM4132xMF-3.3"
			(at 7.874 6.096 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4132.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Low Dropout Voltage Reference, 3.3V, ±0.05% to ±0.5%, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Low Dropout Voltage Reference 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM4132xMF-4.1"
		(extends "LM4132xMF-1.8")
		(property "Reference" "U"
			(at -4.318 6.096 0)
		)
		(property "Value" "LM4132xMF-4.1"
			(at 7.874 6.096 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4132.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Low Dropout Voltage Reference, 4.096V, ±0.05% to ±0.5%, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Low Dropout Voltage Reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT1009CMS8"
		(extends "LT1009xS8")
		(property "Reference" "U"
			(at 1.905 3.81 0)
		)
		(property "Value" "LT1009CMS8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1009.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MSOP*"
			(at 0 0 0)
		)
	)
	(symbol "LT1009xZ"
		(extends "LM285Z-ADJ")
		(property "Reference" "U"
			(at 1.905 3.81 0)
		)
		(property "Value" "LT1009xZ"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1009.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Micropower Voltage Reference Diodes, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference LT1009CZ LT1009IZ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461AxS8-3"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461AxS8-3"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.04%, 3V, 100mA, 3.5V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461AxS8-3.3"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461AxS8-3.3"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.04%, 3.3V, 100mA, 3.8V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461AxS8-4"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461AxS8-4"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.04%, 4.096V, 100mA, 4.596V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461AxS8-5"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461AxS8-5"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.04%, 5V, 100mA, 5.5V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461BxS8-2.5"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461BxS8-2.5"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.06%, 2.5V, 100mA, 3V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461BxS8-3"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461BxS8-3"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.06%, 3V, 100mA, 3.5V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461BxS8-3.3"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461BxS8-3.3"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.06%, 3.3V, 100mA, 3.8V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461BxS8-4"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461BxS8-4"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.06%, 4.096V, 100mA, 4.596V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461BxS8-5"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461BxS8-5"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.06%, 5V, 100mA, 5.5V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461CxS8-2.5"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461CxS8-2.5"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.08%, 2.5V, 100mA, 3V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461CxS8-3"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461CxS8-3"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.08%, 3V, 100mA, 3.5V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461CxS8-3.3"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461CxS8-3.3"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.08%, 3.3V, 100mA, 3.8V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461CxS8-4"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461CxS8-4"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.08%, 4.096V, 100mA, 4.596V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461CxS8-5"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461CxS8-5"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.08%, 5V, 100mA, 5.5V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461DxS8-2.5"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461DxS8-2.5"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.15%, 2.5V, 100mA, 3V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461DxS8-3"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461DxS8-3"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.15%, 3V, 100mA, 3.5V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461DxS8-3.3"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461DxS8-3.3"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.15%, 3.3V, 100mA, 3.8V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461DxS8-4"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461DxS8-4"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.15%, 4.096V, 100mA, 4.596V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1461DxS8-5"
		(extends "LT1461AxS8-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1461DxS8-5"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1461.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "Voltage Reference, ±0.15%, 5V, 100mA, 5.5V-20V Vin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference precision"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1634BCMS8-2.5"
		(extends "LT1634BCMS8-1.25")
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634BCMS8-2.5"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V Micropower Precision Shunt Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP?8*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1634CCZ-2.5"
		(extends "LT1634CCZ-1.25")
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634CCZ-2.5"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V Micropower Precision Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LT1634CCZ-4.096"
		(extends "LT1634CCZ-1.25")
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634CCZ-4.096"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V Micropower Precision Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LT1634CCZ-5"
		(extends "LT1634CCZ-1.25")
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634CCZ-5"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V Micropower Precision Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LT1634xxS8-2.5"
		(extends "LT1634xxS8-1.25")
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634xxS8-2.5"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "2.5V Micropower Precision Shunt Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1634xxS8-4.096"
		(extends "LT1634xxS8-1.25")
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634xxS8-4.096"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "4.096V Micropower Precision Shunt Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1634xxS8-5"
		(extends "LT1634xxS8-1.25")
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "LT1634xxS8-5"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1634ff.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "5V Micropower Precision Shunt Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1790-2.048"
		(extends "LT1790-1.25")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LT1790-2.048"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1790fc.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "2.048V Voltage Reference, Low Dropout, Micropower, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "LT1790-2.5"
		(extends "LT1790-1.25")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LT1790-2.5"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1790fc.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "2.5V Voltage Reference, Low Dropout, Micropower, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "LT1790-3"
		(extends "LT1790-1.25")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LT1790-3"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1790fc.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "3V Voltage Reference, Low Dropout, Micropower, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "LT1790-3.3"
		(extends "LT1790-1.25")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LT1790-3.3"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1790fc.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "3.3V Voltage Reference, Low Dropout, Micropower, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "LT1790-4.096"
		(extends "LT1790-1.25")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LT1790-4.096"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1790fc.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "4.096V Voltage Reference, Low Dropout, Micropower, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "LT1790-5"
		(extends "LT1790-1.25")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LT1790-5"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1790fc.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "5V Voltage Reference, Low Dropout, Micropower, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference Micropower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "LT6657AHMS8-3"
		(extends "LT6657AHMS8-2.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT6657AHMS8-3"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6657fd.pdf"
			(at 1.27 -8.89 0)
		)
		(property "Description" "Precision voltage reference, 40V input, 10mA output, 1.5ppm/C drift, 3.0V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT6657AHMS8-4.096"
		(extends "LT6657AHMS8-2.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT6657AHMS8-4.096"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6657fd.pdf"
			(at 1.27 -8.89 0)
		)
		(property "Description" "Precision voltage reference, 40V input, 10mA output, 1.5ppm/C drift, 4.096V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT6657AHMS8-5"
		(extends "LT6657AHMS8-2.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT6657AHMS8-5"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6657fd.pdf"
			(at 1.27 -8.89 0)
		)
		(property "Description" "Precision voltage reference, 40V input, 10mA output, 1.5ppm/C drift, 5.0V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT6657BHMS8-2.5"
		(extends "LT6657AHMS8-2.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT6657BHMS8-2.5"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6657fd.pdf"
			(at 1.27 -8.89 0)
		)
		(property "Description" "Precision voltage reference, 40V input, 10mA output, 3.0ppm/C drift, 2.5V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT6657BHMS8-3"
		(extends "LT6657AHMS8-2.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT6657BHMS8-3"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6657fd.pdf"
			(at 1.27 -8.89 0)
		)
		(property "Description" "Precision voltage reference, 40V input, 10mA output, 3.0ppm/C drift, 3.0V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT6657BHMS8-4.096"
		(extends "LT6657AHMS8-2.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT6657BHMS8-4.096"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6657fd.pdf"
			(at 1.27 -8.89 0)
		)
		(property "Description" "Precision voltage reference, 40V input, 10mA output, 3ppm/C drift, 4.096V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT6657BHMS8-5"
		(extends "LT6657AHMS8-2.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT6657BHMS8-5"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6657fd.pdf"
			(at 1.27 -8.89 0)
		)
		(property "Description" "Precision voltage reference, 40V input, 10mA output, 3.0ppm/C drift, 5.0V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6001"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6001"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6001-MAX6005.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "1.250V series voltage reference, ±1% accuracy,  100ppm/°C temperature coefficient, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6002"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6002"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6001-MAX6005.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "2.5V series voltage reference, ±1% accuracy,  100ppm/°C temperature coefficient, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6003"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6003"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6001-MAX6005.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "3.0V series voltage reference, ±1% accuracy,  100ppm/°C temperature coefficient, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6004"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6004"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6001-MAX6005.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "4.096V series voltage reference, ±1% accuracy,  100ppm/°C temperature coefficient, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6005"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6005"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6001-MAX6005.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "5.0V series voltage reference, ±1% accuracy,  100ppm/°C temperature coefficient, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6035xxUR25"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6035xxUR25"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6035.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "2.5V, High-Supply-Voltage, Precision Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6035xxUR30"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6035xxUR30"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6035.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "3V, High-Supply-Voltage, Precision Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6035xxUR50"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6035xxUR50"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6035.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "5V, High-Supply-Voltage, Precision Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "vref"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT18+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT18+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max6070-max6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.8V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT18V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT18V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max6070-max6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.8V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070AAUT18/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT21+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT21+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.048V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT25+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT25+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.5V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT30+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT30+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT33+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT33+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3.3V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT33V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT33V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3.3V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070AAUT33/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT41+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT41+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 4.096V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT50+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT50+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 5V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070AAUT50V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070AAUT50V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 5V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070AAUT50/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT12+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT12+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.25V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT12V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT12V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.25V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070BAUT12/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT18+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT18+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.8V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT21+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT21+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.048V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT21V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT21V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.048V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070BAUT21/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT25+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT25+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.5V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT25V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT25V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.5V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070BAUT25/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT30+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT30+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT33+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT33+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3.3V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT33V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT33V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3.3V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070BAUT33/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT41+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT41+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 4.096V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT41V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT41V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 4.096V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070BAUT41/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT50+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT50+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 5V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070BAUT50V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070BAUT50V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 5V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070BAUT50/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070DAUT12V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070DAUT12V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.25V, ±0.2% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070DAUT12/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070DAUT25V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070DAUT25V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.5V, ±0.2% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070DAUT25/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070DAUT30V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070DAUT30V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3V, ±0.2% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070DAUT30/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6070DAUT41V+T"
		(extends "MAX6070AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6070DAUT41V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 4.096V, ±0.2% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6070DAUT41/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071AAUT18+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071AAUT18+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.8V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071AAUT21+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071AAUT21+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.048V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071AAUT25+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071AAUT25+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.5V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071AAUT30+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071AAUT30+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071AAUT30V+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071AAUT30V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6071AAUT30/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071AAUT33+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071AAUT33+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3.3V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071AAUT41+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071AAUT41+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 4.096V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071AAUT50+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071AAUT50+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 5V, ±0.04% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071BAUT12+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071BAUT12+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.25V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071BAUT18+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071BAUT18+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 1.8V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071BAUT21+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071BAUT21+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.048V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071BAUT25+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071BAUT25+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.5V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071BAUT25V+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071BAUT25V+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 2.5V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference AEC-Q100 MAX6071BAUT25/V+T"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071BAUT30+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071BAUT30+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071BAUT33+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071BAUT33+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 3.3V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071BAUT41+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071BAUT41+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 4.096V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6071BAUT50+T"
		(extends "MAX6071AAUT12+T")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MAX6071BAUT50+T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6070-MAX6071.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Noise, High-Precision Series Voltage Reference, 5V, ±0.08% initial accuracy, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6101"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6101"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6100-MAX6107.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "Low-dropout high current voltage reference, 1.250V, ±0.4% accuracy, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6102"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6102"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6100-MAX6107.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "Low-dropout high current voltage reference, 2.500V, ±0.4% accuracy, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6103"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6103"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6100-MAX6107.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "Low-dropout high current voltage reference, 3.000V, ±0.4% accuracy, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6104"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6104"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6100-MAX6107.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "Low-dropout high current voltage reference, 4.096V, ±0.4% accuracy, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6105"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6105"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6100-MAX6107.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "Low-dropout high current voltage reference, 5.000V, ±0.4% accuracy, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6106"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6106"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6100-MAX6107.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "Low-dropout high current voltage reference, 2.048V, ±0.4% accuracy, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6107"
		(extends "MAX6100")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MAX6107"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6100-MAX6107.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "Low-dropout high current voltage reference, 4.500V, ±0.4% accuracy, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6225"
		(extends "MAX6350")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "MAX6225"
			(at 1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at 30.48 -11.43 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6225-MAX6250.pdf"
			(at 2.54 -10.16 0)
		)
		(property "Description" "1ppm/°C Low-Noise Precision +2.5V Voltage Reference, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6241"
		(extends "MAX6350")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "MAX6241"
			(at 1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at 30.48 -11.43 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6225-MAX6250.pdf"
			(at 2.54 -10.16 0)
		)
		(property "Description" "1ppm/°C Low-Noise Precision +4.096V Voltage Reference, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6250"
		(extends "MAX6350")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "MAX6250"
			(at 1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at 30.48 -11.43 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6225-MAX6250.pdf"
			(at 2.54 -10.16 0)
		)
		(property "Description" "1ppm/°C Low-Noise Precision +5V Voltage Reference, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6325"
		(extends "MAX6350")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "MAX6325"
			(at 1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at 30.48 -11.43 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6325-MAX6350.pdf"
			(at 2.54 -10.16 0)
		)
		(property "Description" "0.5ppm/°C Low-Noise +2.5V Voltage Reference, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX6341"
		(extends "MAX6350")
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "MAX6341"
			(at 1.27 -8.89 0)
		)
		(property "Footprint" ""
			(at 30.48 -11.43 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX6325-MAX6350.pdf"
			(at 2.54 -10.16 0)
		)
		(property "Description" "0.5ppm/°C Low-Noise +4.096V Voltage Reference, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX872"
		(extends "MAX874")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MAX872"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://pdfserv.maximintegrated.com/en/ds/MAX872-MAX874.pdf"
			(at 0 0 0)
		)
		(property "Description" "10µA Low-Dropout Precision Voltage Reference, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low-Dropout Precision Voltage Reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-12xCH"
		(extends "MCP1501-10xCH")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1501-12xCH"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.25V, 0.1%, 20mA, Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 1.25V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-12xRW"
		(extends "MCP1501-10xRW")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-12xRW"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "1.25V, 0.1%, 20mA, Precision Voltage Reference, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 1.25V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-12xSN"
		(extends "MCP1501-10xSN")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-12xSN"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "1.25V, 0.1%, 20mA, Precision Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 1.25V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-18xCH"
		(extends "MCP1501-10xCH")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1501-18xCH"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.8V, 0.1%, 20mA, Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-18xRW"
		(extends "MCP1501-10xRW")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-18xRW"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "1.8V, 0.1%, 20mA, Precision Voltage Reference, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-18xSN"
		(extends "MCP1501-10xSN")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-18xSN"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "1.8V, 0.1%, 20mA, Precision Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-20xCH"
		(extends "MCP1501-10xCH")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1501-20xCH"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.048V, 0.1%, 20mA, Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 2.048V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-20xRW"
		(extends "MCP1501-10xRW")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-20xRW"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "2.048V, 0.1%, 20mA, Precision Voltage Reference, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 2.048V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-20xSN"
		(extends "MCP1501-10xSN")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-20xSN"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "2.048V, 0.1%, 20mA, Precision Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 2.048V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-25xCH"
		(extends "MCP1501-10xCH")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1501-25xCH"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V, 0.1%, 20mA, Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-25xRW"
		(extends "MCP1501-10xRW")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-25xRW"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "2.5V, 0.1%, 20mA, Precision Voltage Reference, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-25xSN"
		(extends "MCP1501-10xSN")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-25xSN"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "2.5V, 0.1%, 20mA, Precision Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-30xCH"
		(extends "MCP1501-10xCH")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1501-30xCH"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 0 0 0)
		)
		(property "Description" "3V, 0.1%, 20mA, Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-30xRW"
		(extends "MCP1501-10xRW")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-30xRW"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "3V, 0.1%, 20mA, Precision Voltage Reference, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-30xSN"
		(extends "MCP1501-10xSN")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-30xSN"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "3V, 0.1%, 20mA, Precision Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-33xCH"
		(extends "MCP1501-10xCH")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1501-33xCH"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 0.1%, 20mA, Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-33xRW"
		(extends "MCP1501-10xRW")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-33xRW"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "3.3V, 0.1%, 20mA, Precision Voltage Reference, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-33xSN"
		(extends "MCP1501-10xSN")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-33xSN"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "3.3V, 0.1%, 20mA, Precision Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-40xCH"
		(extends "MCP1501-10xCH")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1501-40xCH"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V, 0.1%, 20mA, Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-40xRW"
		(extends "MCP1501-10xRW")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-40xRW"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "4.096V, 0.1%, 20mA, Precision Voltage Reference, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1501-40xSN"
		(extends "MCP1501-10xSN")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1501-40xSN"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005474E.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "4.096V, 0.1%, 20mA, Precision Voltage Reference, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "precision buffered voltage reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1541-TO"
		(extends "MCP1525-TO")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "MCP1541-TO"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21653b.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1541-TT"
		(extends "MCP1525-TT")
		(property "Reference" "U"
			(at 1.27 8.255 0)
		)
		(property "Value" "MCP1541-TT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21653b.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V Voltage Reference, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF01CP"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF01CP"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "10V ±100mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF01CS"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 1.905 8.255 0)
		)
		(property "Value" "REF01CS"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "10V ±100mV Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF01EZ"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF01EZ"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "10V ±30mV Precision Voltage Reference, CERDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF01HP"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF01HP"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "10V ±50mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF01HZ"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF01HZ"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "10V ±50mV Precision Voltage Reference, CERDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02AU"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 1.905 8.255 0)
		)
		(property "Value" "REF02AU"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref02.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "5V ±15mV Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02AZ"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF02AZ"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "5V ±15mV Precision Voltage Reference, CERDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02BP"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF02BP"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref02.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "5V ±10mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02BU"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 1.905 8.255 0)
		)
		(property "Value" "REF02BU"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref02.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "5V ±10mV Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02CP"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF02CP"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "5V ±50mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02CS"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 1.905 8.255 0)
		)
		(property "Value" "REF02CS"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "5V ±50mV Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02EZ"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF02EZ"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "5V ±15mV Precision Voltage Reference, CERDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02HP"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF02HP"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "5V ±25mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02HS"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 1.905 8.255 0)
		)
		(property "Value" "REF02HS"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "5V ±25mV Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02HZ"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF02HZ"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "5V ±25mV Precision Voltage Reference, CERDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF02Z"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF02Z"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "5V ±25mV Precision Voltage Reference, CERDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF03GP"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF03GP"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 15.24 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "2.5V ±15mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF03GS"
		(extends "REF02AP")
		(property "Reference" "U"
			(at 1.905 8.255 0)
		)
		(property "Value" "REF03GS"
			(at 0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/REF01_02_03.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "2.5V ±15mV Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF102BP"
		(extends "REF102AP")
		(property "Reference" "U"
			(at -0.635 8.255 0)
		)
		(property "Value" "REF102BP"
			(at -1.905 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -1.27 10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref102.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "10V ±5mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF102BU"
		(extends "REF102AU")
		(property "Reference" "U"
			(at 0 8.255 0)
		)
		(property "Value" "REF102BU"
			(at 3.175 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref02.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V ±5mV Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF102CP"
		(extends "REF102AP")
		(property "Reference" "U"
			(at -0.635 8.255 0)
		)
		(property "Value" "REF102CP"
			(at -1.905 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -1.27 10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref102.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "10V ±2.5mV Precision Voltage Reference, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF102CU"
		(extends "REF102AU")
		(property "Reference" "U"
			(at 0 8.255 0)
		)
		(property "Value" "REF102CU"
			(at 3.175 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref02.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V ±2.5mV Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF192"
		(extends "REF191")
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "REF192"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/REF19xSeries.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Precision voltage references 2.5V, DIP-8/SO-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision voltage references"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9m*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF193"
		(extends "REF191")
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "REF193"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/REF19xSeries.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Precision voltage references 3V, DIP-8/SO-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision voltage references"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9m*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF194"
		(extends "REF191")
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "REF194"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/REF19xSeries.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Precision voltage references 4.5V, DIP-8/SO-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision voltage references"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9m*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF195"
		(extends "REF191")
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "REF195"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/REF19xSeries.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Precision voltage references 5V, DIP-8/SO-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision voltage references"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9m*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF196"
		(extends "REF191")
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "REF196"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/REF19xSeries.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Precision voltage references 3.3V, DIP-8/SO-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision voltage references"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9m*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF198"
		(extends "REF191")
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "REF198"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/REF19xSeries.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Precision voltage references 4.096V, DIP-8/SO-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision voltage references"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9m*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF2030"
		(extends "REF2025")
		(property "Reference" "U?"
			(at 5.08 7.62 0)
		)
		(property "Value" "REF2030"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.016 -9.906 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref2033.pdf"
			(at 1.778 -13.208 0)
		)
		(property "Description" "3.0V Low-Drift, Low-Power, Dual-Output, VREF and VREF / 2 Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF2033"
		(extends "REF2025")
		(property "Reference" "U?"
			(at 5.08 7.62 0)
		)
		(property "Value" "REF2033"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.016 -9.906 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref2033.pdf"
			(at 1.778 -13.208 0)
		)
		(property "Description" "3.3V Low-Drift, Low-Power, Dual-Output, VREF and VREF / 2 Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF2041"
		(extends "REF2025")
		(property "Reference" "U?"
			(at 5.08 7.62 0)
		)
		(property "Value" "REF2041"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.016 -9.906 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref2033.pdf"
			(at 1.778 -13.208 0)
		)
		(property "Description" "4.096V Low-Drift, Low-Power, Dual-Output, VREF and VREF / 2 Voltage Reference, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3020"
		(extends "REF3012")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "REF3020"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3033.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "2.048V 50-ppm/°C Max, 50-μA, CMOS Voltage Reference, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3025"
		(extends "REF3012")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "REF3025"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3033.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "2.500V 50-ppm/°C Max, 50-μA, CMOS Voltage Reference, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3030"
		(extends "REF3012")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "REF3030"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3033.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "3.0V 50-ppm/°C Max, 50-μA, CMOS Voltage Reference, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3033"
		(extends "REF3012")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "REF3033"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3033.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "3.3V 50-ppm/°C Max, 50-μA, CMOS Voltage Reference, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3040"
		(extends "REF3012")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "REF3040"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3033.pdf"
			(at 2.54 -8.89 0)
		)
		(property "Description" "4.096V 50-ppm/°C Max, 50-μA, CMOS Voltage Reference, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3220AMDBVREP"
		(extends "REF3212AMDBVREP")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "REF3220AMDBVREP"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.905 -9.525 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3240-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "2.048V 100μA Micropower Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Precision Voltage Reference 2.048V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3225AMDBVREP"
		(extends "REF3212AMDBVREP")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "REF3225AMDBVREP"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.905 -9.525 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3240-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "2.5V 100μA Micropower Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Precision Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3230AMDBVREP"
		(extends "REF3212AMDBVREP")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "REF3230AMDBVREP"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.905 -9.525 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3240-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "3V 100μA Micropower Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Precision Voltage Reference 3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3233AMDBVREP"
		(extends "REF3212AMDBVREP")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "REF3233AMDBVREP"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.905 -9.525 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3240-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "3.3V 100μA Micropower Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Precision Voltage Reference 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF3240AMDBVREP"
		(extends "REF3212AMDBVREP")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "REF3240AMDBVREP"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.905 -9.525 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref3240-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "4.096V 100μA Micropower Precision Voltage Reference, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Precision Voltage Reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35120QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35120QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "1.2V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35125QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35125QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "1.25V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35160QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35160QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "1.6V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35170QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35170QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "1.7V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35180QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35180QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "1.8V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35205QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35205QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "2.048V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35250QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35250QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "2.5V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35300QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35300QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "3.0V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35330QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35330QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "3.3V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35360QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35360QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "3.6V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35409QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35409QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "4.096V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF35500QDBVR"
		(extends "REF35102QDBVR")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "REF35500QDBVR"
			(at 8.636 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref35.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "5.0V, Ultra Low-Power, High-Precision Voltage Reference, SOT-23-6"
			(at 0 19.05 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "REF5010AD"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5010AD"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "10V 0.1% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5010ADGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5010ADGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V 0.1% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5010ID"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5010ID"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "10V 0.05% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5010IDGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5010IDGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V 0.05% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 10V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5020ID"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5020ID"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "2.048V 0.05% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 2.048V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5020IDGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5020IDGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.048V 0.05% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 2.048V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5025AD"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5025AD"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "2.5V 0.1% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5025ADGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5025ADGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V 0.1% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5025ID"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5025ID"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "2.5V 0.05% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5025IDGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5025IDGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V 0.05% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5030AD"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5030AD"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "3V 0.1% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5030ADGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5030ADGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "3V 0.1% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5030ID"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5030ID"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "3V 0.05% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5030IDGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5030IDGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "3V 0.05% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5040AD"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5040AD"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "4.096V 0.1% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5040ADGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5040ADGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V 0.1% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5040ID"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5040ID"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "4.096V 0.05% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5040IDGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5040IDGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V 0.05% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 4.096V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5045AD"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5045AD"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "4.5V 0.1% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 4.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5045ADGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5045ADGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.5V 0.1% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 4.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5045ID"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5045ID"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "4.5V 0.05% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 4.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5045IDGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5045IDGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.5V 0.05% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 4.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5050AD"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5050AD"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "5V 0.1% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5050ADGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5050ADGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 0.1% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5050ID"
		(extends "REF5020AD")
		(property "Reference" "U"
			(at -1.27 8.255 0)
		)
		(property "Value" "REF5050ID"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.905 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "5V 0.05% 10mA Low Noise Precision Voltage Reference, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF5050IDGK"
		(extends "REF5020ADGK")
		(property "Reference" "U"
			(at 0.635 8.255 0)
		)
		(property "Value" "REF5050IDGK"
			(at -0.635 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ref5030.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 0.05% 10mA Low Noise Precision Voltage Reference, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Precision Voltage Reference 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF6030xDGK"
		(extends "REF6025xDGK")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "REF6030xDGK"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref6025.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0V 0.05% 4mA Extremely Low Noise High Precision Voltage Reference, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "low Noise precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF6033xDGK"
		(extends "REF6025xDGK")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "REF6033xDGK"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref6025.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 0.05% 4mA Extremely Low Noise High Precision Voltage Reference, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "low Noise precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF6041xDGK"
		(extends "REF6025xDGK")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "REF6041xDGK"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref6025.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.1V 0.05% 4mA Extremely Low Noise High Precision Voltage Reference, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "low Noise precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF6045xDGK"
		(extends "REF6025xDGK")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "REF6045xDGK"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref6025.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.5V 0.05% 4mA Extremely Low Noise High Precision Voltage Reference, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "low Noise precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "REF6050xDGK"
		(extends "REF6025xDGK")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "REF6050xDGK"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref6025.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.0V 0.05% 4mA Extremely Low Noise High Precision Voltage Reference, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "low Noise precision voltage reference"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2425xLP"
		(extends "TLE2426xLP")
		(property "Reference" "U"
			(at -7.874 6.35 0)
		)
		(property "Value" "TLE2425xLP"
			(at 11.43 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tle2425.pdf"
			(at -35.56 21.59 0)
		)
		(property "Description" "Precision virtual ground, 2.5V output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rail splitter precision virtual ground 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "TLE2426xP"
		(extends "TLE2426xD")
		(property "Reference" "U"
			(at -10.414 8.89 0)
		)
		(property "Value" "TLE2426xP"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tle2426.pdf"
			(at -35.56 24.13 0)
		)
		(property "Description" "Precision virtual ground, noise reduction pin, 4V to 40V input, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rail splitter precision vitrual ground"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040LP-10"
		(extends "LM4040LP-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040LP-10"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "10.00V Precision Micropower Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040LP-2.5"
		(extends "LM4040LP-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040LP-2.5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.500V Precision Micropower Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040LP-3"
		(extends "LM4040LP-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040LP-3"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.000V Precision Micropower Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040LP-4.1"
		(extends "LM4040LP-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040LP-4.1"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.096V Precision Micropower Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040LP-5"
		(extends "LM4040LP-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040LP-5"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.000V Precision Micropower Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM4040LP-8.2"
		(extends "LM4040LP-2.0")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LM4040LP-8.2"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4040-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "8.192V Precision Micropower Shunt Voltage Reference, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode device voltage reference shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*"
			(at 0 0 0)
		)
	)
)
