(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ICE1PCS01"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE1PCS01"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE1PCS01-DS-v01_03-en.pdf?fileId=db3a304412b407950112b427c6f13cc7"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ICE1PCS01_0_0")
		(symbol "ICE1PCS01_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ISENSE")
				(number "3")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "ICOMP")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FREQ")
				(number "4")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VCOMP")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VSENSE")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE1PCS02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE1PCS02"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE1PCS02-DS-v01_02-en.pdf?fileId=db3a304412b407950112b427c9283ccb"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM With Input Brown-Out Protection, 65kHz, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ICE1PCS02_0_0")
		(symbol "ICE1PCS02_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VINS")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ISENSE")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ICOMP")
				(number "2")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VCOMP")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VSENSE")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE3PCS01"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "ICE3PCS01"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE3PCS01-DS-v03_00-EN.pdf?fileId=db3a304329a0f6ee0129a67ae8c02b46"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ICE3PCS01_0_0")
		(symbol "ICE3PCS01_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "BOP")
				(number "9")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VBTHL_EN")
				(number "7")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VREF")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ISENSE")
				(number "2")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ICOMP")
				(number "4")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "FREQ")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "SGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "14")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "OVP")
				(number "10")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VSENSE")
				(number "11")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GATE")
				(number "13")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BOFO")
				(number "1")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VB_OK")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE3PCS02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE3PCS02"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE3PCS02G-DS-v03_00-EN.pdf?fileId=db3a304329a0f6ee0129a67fab472b4b"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ICE3PCS02_0_0")
		(symbol "ICE3PCS02_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ISENSE")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ICOMP")
				(number "3")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "FREQ")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OVP")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VSENSE")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE3PCS03"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE3PCS03"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE3PCS03G-DS-v03_00-EN.pdf?fileId=db3a304329a0f6ee0129a683c9c92b50"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ICE3PCS03_0_0")
		(symbol "ICE3PCS03_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "BOP")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ISENSE")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ICOMP")
				(number "3")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "FREQ")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VSENSE")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR1153S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR1153S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir1153.pdf?fileId=5546d462533600a4015355c42a5b1649"
			(at 0 0 0)
		)
		(property "Description" "Fixed 22.2kHz Frequency, uPFC One Cycle Control IC With Brown-Out Protection, Continuous Conduction Mode, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "pfc controller ccm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR1153S_0_1")
		(symbol "IR1153S_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "ISNS")
				(number "3")
			)
			(pin output line
				(at -7.62 0 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "BOP")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "1")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "OVP/EN")
				(number "5")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VFB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR1155S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR1155S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir1155spbf.pdf?fileId=5546d462533600a4015355c431f9164b"
			(at 0 0 0)
		)
		(property "Description" "Programmable Frequency, One Cycle Control PFC IC, Continuous Conduction Mode, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "pfc controller ccm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR1155S_0_1")
		(symbol "IR1155S_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "ISNS")
				(number "3")
			)
			(pin output line
				(at -7.62 0 0)
				(length 2.54)
				(name "COMP")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "FREQ")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "1")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "OVP")
				(number "4")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VFB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR1161L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "IR1161L"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir1161lpbf.pdf?fileId=5546d462533600a4015355c439a5164d"
			(at 0 0 0)
		)
		(property "Description" "SmartRectifier Control IC, 500kHz, 200V, 1.0/2.5A, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "IR1161L_0_1")
		(symbol "IR1161L_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VD")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "MOT")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR1167S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR1167S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir1167aspbf.pdf?fileId=5546d462533600a4015355c45d9c1655"
			(at 0 0 0)
		)
		(property "Description" "SmartRectifier Control IC, 500kHz, 200V, 2.0/7.0A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR1167S_0_1")
		(symbol "IR1167S_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "OVT")
				(number "2")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "MOT")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VD")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "VGATE")
				(number "8")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR11688S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR11688S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir11688spbf.pdf?fileId=5546d462533600a4015355c47c70165c"
			(at 0 0 0)
		)
		(property "Description" "Dual Synchronous Rectification Control IC, 400kHz, 200V, 1.0/4.0A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR11688S_0_1")
		(symbol "IR11688S_1_1"
			(pin output line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "GATE1")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "VD1")
				(number "4")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "MOT")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "GATE2")
				(number "8")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VD2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR1168S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR1168S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir1168.pdf?fileId=5546d462533600a4015355c467fa1658"
			(at 0 0 0)
		)
		(property "Description" "Dual Smart Rectifier Driver IC, 500kHz, 200V, 1.0/4.0A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR1168S_0_1")
		(symbol "IR1168S_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "VS1")
				(number "3")
			)
			(pin output line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "GATE1")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "VD1")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VS2")
				(number "6")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "GATE2")
				(number "8")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VD2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR1169S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR1169S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir1169.pdf?fileId=5546d462533600a4015355c485c4165e"
			(at 0 0 0)
		)
		(property "Description" "Advanced SmartRectifier Control IC, 500kHz, 200V, 1.0/4.0A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR1169S_0_1")
		(symbol "IR1169S_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "2")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "MOT")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VD")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "VGATE")
				(number "8")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS2505L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 11.43 0)
		)
		(property "Value" "IRS2505L"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2505lpbf.pdf?fileId=5546d462533600a40153567ad42c2819"
			(at 0 0 0)
		)
		(property "Description" "Boost PFC and SMPS Control IC, Critical Conduction Mode, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "pfc controller crcm dcm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "IRS2505L_0_1")
		(symbol "IRS2505L_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "CMP")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "COM")
				(number "2")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VBUS")
				(number "5")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "PFC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL6551"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "ISL6551"
			(at 6.35 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.intersil.com/content/dam/Intersil/documents/isl6/isl6551.pdf"
			(at 0 0 0)
		)
		(property "Description" "ZVS Full Bridge PWM Controller, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISL6551_0_0")
		(symbol "ISL6551_1_1"
			(pin output line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "BGREF")
				(number "8")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PKILIM")
				(number "7")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "ISENSE")
				(number "6")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "LATSD")
				(number "16")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ON/OFF")
				(number "18")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EANI")
				(number "12")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EAI")
				(number "13")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EAO")
				(number "14")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CT")
				(number "2")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "RD")
				(number "3")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "R_RESDLY")
				(number "4")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "R_RA")
				(number "5")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "R_LEB")
				(number "9")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "CS_COMP")
				(number "10")
			)
			(pin passive line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "CSS")
				(number "11")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDP1")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "PGND")
				(number "25")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VDDP2")
				(number "26")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "UPPER1")
				(number "24")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "LOWER1")
				(number "22")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "UPPER2")
				(number "23")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "LOWER2")
				(number "21")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "SYNC1")
				(number "20")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SYNC2")
				(number "19")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "SHARE")
				(number "15")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DCOK")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L4981A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "L4981A"
			(at 1.27 21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l4981.pdf"
			(at 0 0 0)
		)
		(property "Description" "Power Factor Corrector, Fixed Frequency Average Current Mode, DIP-20/SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "L4981A_0_0")
		(symbol "L4981A_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "IAC")
				(number "4")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "VRMS")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SYNC")
				(number "16")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IPK")
				(number "2")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "MULT-OUT")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "P-UVLO")
				(number "15")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CA-OUT")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ISENSE")
				(number "9")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "SS")
				(number "12")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "ROSC")
				(number "17")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "COSC")
				(number "18")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "19")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "S-GND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "P-GND")
				(number "1")
			)
			(pin input line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VFEED")
				(number "14")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "VA-OUT")
				(number "13")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OVP")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LFF")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GDRV")
				(number "20")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VREF")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L4981B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "L4981B"
			(at 1.27 21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l4981.pdf"
			(at 0 0 0)
		)
		(property "Description" "Power Factor Corrector, Line Modulated Frequency Average Current Mode, DIP-20/SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "L4981B_0_0")
		(symbol "L4981B_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "IAC")
				(number "4")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "VRMS")
				(number "7")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "FREQ-MOD")
				(number "16")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IPK")
				(number "2")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "MULT-OUT")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "P-UVLO")
				(number "15")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CA-OUT")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ISENSE")
				(number "9")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "SS")
				(number "12")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "ROSC")
				(number "17")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "COSC")
				(number "18")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "19")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "S-GND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "P-GND")
				(number "1")
			)
			(pin input line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VFEED")
				(number "14")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "VA-OUT")
				(number "13")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OVP")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LFF")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GDRV")
				(number "20")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VREF")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L4984D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "L4984D"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-10_3.9x4.9mm_P1.00mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l4984d.pdf"
			(at 0 0 0)
		)
		(property "Description" "CCM PFC Controller, SSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P1.00mm*"
			(at 0 0 0)
		)
		(symbol "L4984D_0_0")
		(symbol "L4984D_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INV")
				(number "1")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "MULT")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VFF")
				(number "5")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "TIMER")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PFC_OK")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GD")
				(number "9")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L6561"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "L6561"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6561.pdf"
			(at 0 0 0)
		)
		(property "Description" "Transition Mode Power Factor Corrector, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "L6561_0_0")
		(symbol "L6561_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INV")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "MULT")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ZCD")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "GD")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L6563"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "L6563"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6563.pdf"
			(at 0 0 0)
		)
		(property "Description" "Advanced Transition-Mode PFC Controller, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "L6563_0_0")
		(symbol "L6563_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "INV")
				(number "1")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "MULT")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RUN")
				(number "10")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VFF")
				(number "5")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "TBO")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "ZCD")
				(number "11")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "GD")
				(number "13")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CS")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PWM_LATCH")
				(number "8")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PWM_STOP")
				(number "9")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PFC_OK")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L6563H"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "L6563H"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6563h.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Voltage Start-Up Transition-Mode PFC, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "L6563H_0_0")
		(symbol "L6563H_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "INV")
				(number "1")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "MULT")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RUN")
				(number "12")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VFF")
				(number "5")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "TBO")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin input line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "HVS")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "ZCD")
				(number "13")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "GD")
				(number "15")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CS")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PWM_LATCH")
				(number "8")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PWM_STOP")
				(number "11")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PFC_OK")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L6564"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "L6564"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-10_3.9x4.9mm_P1.00mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6564.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-Pin Transition-Mode PFC Controller, SSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P1.00mm*"
			(at 0 0 0)
		)
		(symbol "L6564_0_0")
		(symbol "L6564_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INV")
				(number "1")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MULT")
				(number "3")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VFF")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "ZCD")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PFC_OK")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GD")
				(number "9")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L6564H"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "L6564H"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6564h.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Voltage Start-Up Transition-Mode PFC, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "L6564H_0_0")
		(symbol "L6564H_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INV")
				(number "1")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MULT")
				(number "3")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VFF")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin input line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "HVS")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "ZCD")
				(number "11")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PFC_OK")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GD")
				(number "13")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L6598"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "L6598"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/l6598.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Voltage Resonant Controller, DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "L6598_0_0")
		(symbol "L6598_1_1"
			(pin output line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "OPOUT")
				(number "5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "OPIN-")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "OPIN+")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN1")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN2")
				(number "9")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CSS")
				(number "1")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RFSTART")
				(number "2")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CF")
				(number "3")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RFMIN")
				(number "4")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VS")
				(number "12")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VBOOT")
				(number "16")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "HVG")
				(number "15")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT")
				(number "14")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LVG")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L6599"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "L6599"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/l6599.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Voltage Resonant Controller, DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "L6599_0_0")
		(symbol "L6599_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "LINE")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DIS")
				(number "8")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "STBY")
				(number "5")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RFMIN")
				(number "4")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CSS")
				(number "1")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DELAY")
				(number "2")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CF")
				(number "3")
			)
			(pin open_collector line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PFC_STOP")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "ISEN")
				(number "6")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VBOOT")
				(number "16")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "HVG")
				(number "15")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT")
				(number "14")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LVG")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L6727"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "L6727"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6727.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Phase PWM Controller, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "L6727_0_0")
		(symbol "L6727_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "COMP/DIS/OC")
				(number "7")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "FB")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "UGATE")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "PHASE")
				(number "8")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LGATE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM25119"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "LM25119"
			(at -2.54 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm25119.pdf"
			(at 0 0 0)
		)
		(property "Description" "Wide Input Range, Dual Synchronous Buck Controller, WQFN-32"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Synchronous Buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM25119_0_1")
		(symbol "LM25119_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "FB1")
				(number "9")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "COMP1")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RAMP1")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SS1")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PGND1")
				(number "3")
			)
			(pin power_in line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "HB1")
				(number "30")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "HO1")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SW1")
				(number "32")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "LO1")
				(number "2")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CS1")
				(number "5")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CSG1")
				(number "4")
			)
		)
		(symbol "LM25119_2_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "FB2")
				(number "16")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "COMP2")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RAMP2")
				(number "19")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EN2")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SS2")
				(number "18")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC2")
				(number "24")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PGND2")
				(number "22")
			)
			(pin power_in line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "HB2")
				(number "27")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "HO2")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SW2")
				(number "25")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "LO2")
				(number "23")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CS2")
				(number "20")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CSG2")
				(number "21")
			)
		)
		(symbol "LM25119_3_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "UVLO")
				(number "28")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DEMB")
				(number "17")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VCCDIS")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "13")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RES")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "12")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "29")
			)
			(pin unspecified line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM3478MA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.525 8.89 0)
		)
		(property "Value" "LM3478MA"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 25.4 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lm3478"
			(at 0.635 12.7 0)
		)
		(property "Description" "2.97~40V Wide Input Range Boost/SEPIC/Flyback DC-DC Controller, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost flyback SEPIC DC-DC controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-8*3.9x4.9mm_P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM3478MA_0_1")
		(symbol "LM3478MA_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{IN}")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "FA/SD")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DR")
				(number "6")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "I_{SEN}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5023"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LM5023"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5023.pdf"
			(at 20.32 -1.27 0)
		)
		(property "Description" "Quasi-Resonant Current-Mode PWM Controller for Off-Line Supplies, OVP/OTP, Latched OVP, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps pwm controller ac-dc ac dc offline off-line quasi resonant quasi-resonant flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM5023_0_0"
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VSD")
				(number "2")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SS")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "QR")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CS")
				(number "5")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "COMP")
				(number "4")
			)
		)
		(symbol "LM5023_0_1")
		(embedded_fonts no)
	)
	(symbol "LT1248"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 24.13 0)
		)
		(property "Value" "LT1248"
			(at 7.62 21.59 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1248fd.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Power Factor Controller, DIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*3.9x9.9mm*P1.27mm* DIP*16*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1248_0_1")
		(symbol "LT1248_1_1"
			(pin output line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "VAOUT")
				(number "7")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VSENSE")
				(number "11")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "OVP")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IAC")
				(number "6")
			)
			(pin power_out line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "VREF")
				(number "9")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "EN/SYNC")
				(number "10")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "CSET")
				(number "14")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "RSET")
				(number "12")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SS")
				(number "13")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "MOUT")
				(number "5")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "CAOUT")
				(number "3")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "ISENSE")
				(number "4")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PKLIM")
				(number "2")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GTDR")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1249"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 16.51 0)
		)
		(property "Value" "LT1249"
			(at 6.35 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1249fbs.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Power Factor Controller, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1249_0_1")
		(symbol "LT1249_1_1"
			(pin output line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "VAOUT")
				(number "5")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VSENSE")
				(number "6")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "CAOUT")
				(number "2")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "MOUT")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "IAC")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "GTDR")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1509"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 24.13 0)
		)
		(property "Value" "LT1509"
			(at 7.62 21.59 0)
		)
		(property "Footprint" ""
			(at -3.81 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1509.pdf"
			(at -3.81 -5.08 0)
		)
		(property "Description" "Power Factor and PWM Controller, DIP-20/SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "pfc pwm controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1509_0_1")
		(symbol "LT1509_1_1"
			(pin output line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "VAOUT")
				(number "10")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VSENSE")
				(number "14")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "OVP")
				(number "11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IAC")
				(number "9")
			)
			(pin power_out line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "VREF")
				(number "12")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "CSET")
				(number "4")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RSET")
				(number "15")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "SS2")
				(number "13")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SS1")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "GND2")
				(number "2")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND1")
				(number "3")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PKLIM")
				(number "5")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "MOUT")
				(number "8")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "ISENSE")
				(number "7")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CAOUT")
				(number "6")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GTDR1")
				(number "1")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "GTDR2")
				(number "20")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RAMP")
				(number "19")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "VC")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT4295xUFD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "LT4295xUFD"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT4295.pdf"
			(at 0 24.13 0)
		)
		(property "Description" "IEEE 802.3bt PD Interface with Forward/Flyback Controller, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTPoE++ IEEE 802.3af IEEE 802.3at IEEE 802.3bt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT4295xUFD_0_1")
		(symbol "LT4295xUFD_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "FSSDLY")
				(number "12")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SWVCC")
				(number "23")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "HSSRC")
				(number "25")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "HSGATE")
				(number "26")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "VPORT")
				(number "28")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "AUX")
				(number "2")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "ROSC")
				(number "10")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SFST")
				(number "11")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RLDCMP")
				(number "15")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "22")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "8")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VIN")
				(number "24")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PG")
				(number "20")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "ISEN+")
				(number "17")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "ISEN-")
				(number "16")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SG")
				(number "18")
			)
			(pin open_collector line
				(at 15.24 0 180)
				(length 2.54)
				(name "T2P")
				(number "5")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "ITHB")
				(number "13")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "FB31")
				(number "14")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RCLASS")
				(number "4")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RCLASS++")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1624CS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LTC1624CS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1624f.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Efficiency N-Channel Switching Regulator Controller, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1624CS8_0_1")
		(symbol "LTC1624CS8_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ISENSE")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "Ith/RUN")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SET")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BOOST")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "TG")
				(number "6")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3805xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 11.43 0)
		)
		(property "Value" "LTC3805xMSE"
			(at 1.016 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Adjustable Frequency current Mode Flyback DC/DC controller, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "flyback dc-dc switcher switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*10*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC3805xMSE_0_1")
		(symbol "LTC3805xMSE_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RUN")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "Ith")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SSFLT")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "FS")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SYNC")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "GATE")
				(number "10")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OC")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Isense")
				(number "7")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3890"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "LTC3890"
			(at 15.494 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 8.89 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3890fc.pdf"
			(at 0 29.21 0)
		)
		(property "Description" "60V dual 2-phase synchronous step-down DC/DC controller, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter regulator dual-output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC3890_0_1")
		(symbol "LTC3890_1_1"
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "TG1")
				(number "26")
			)
			(pin output line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "BOOST1")
				(number "24")
			)
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SW1")
				(number "25")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "BG1")
				(number "23")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SENSE1+")
				(number "32")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SENSE1-")
				(number "1")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "VFB1")
				(number "31")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "RUN1")
				(number "7")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PGOOD1")
				(number "27")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PLLIN/MODE")
				(number "5")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "FREQ")
				(number "2")
			)
			(pin output line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "CLKOUT")
				(number "4")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "ITH1")
				(number "30")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "TRACK/SS1")
				(number "29")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "Vin")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "INTVcc")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "21")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "EXTVcc")
				(number "20")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TG2")
				(number "15")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "BOOST2")
				(number "17")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SW2")
				(number "16")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "BG2")
				(number "18")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SENSE2+")
				(number "10")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SENSE2-")
				(number "9")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "VFB2")
				(number "11")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RUN2")
				(number "8")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PGOOD2")
				(number "14")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PHASMD")
				(number "3")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "ILIM")
				(number "28")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "ITH2")
				(number "12")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "TRACK/SS2")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3890-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "LTC3890-1"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_3.9x9.9mm_P0.635mm"
			(at 8.89 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/38901fb.pdf"
			(at 0 31.75 0)
		)
		(property "Description" "60V dual 2-phase synchronous step-down DC/DC controller, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter regulator dual-output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x9.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "LTC3890-1_0_1")
		(symbol "LTC3890-1_1_1"
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "TG1")
				(number "26")
			)
			(pin output line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "BOOST1")
				(number "24")
			)
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SW1")
				(number "25")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "BG1")
				(number "23")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SENSE1+")
				(number "3")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SENSE1-")
				(number "4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "VFB1")
				(number "2")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "RUN1")
				(number "8")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PGOOD1")
				(number "27")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PLLIN/MODE")
				(number "6")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "FREQ")
				(number "5")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "ITH1")
				(number "1")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "TRACK/SS1")
				(number "28")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "Vin")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "SGND")
				(number "7")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "INTVcc")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "21")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "EXTVcc")
				(number "20")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TG2")
				(number "15")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "BOOST2")
				(number "17")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SW2")
				(number "16")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "BG2")
				(number "18")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SENSE2+")
				(number "11")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SENSE2-")
				(number "10")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "VFB2")
				(number "12")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RUN2")
				(number "9")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "ITH2")
				(number "13")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "TRACK/SS2")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3892"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "LTC3892"
			(at 15.494 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 8.89 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/38921fc.pdf"
			(at 0 29.21 0)
		)
		(property "Description" "60V dual 2-phase synchronous step-down DC/DC controller, continuous conduction, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter regulator dual-output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC3892_0_1")
		(symbol "LTC3892_1_1"
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "TG1")
				(number "26")
			)
			(pin output line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "BOOST1")
				(number "24")
			)
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SW1")
				(number "25")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "BG1")
				(number "23")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SENSE1+")
				(number "31")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SENSE1-")
				(number "32")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "VFB1")
				(number "30")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "RUN1")
				(number "6")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PGOOD1")
				(number "3")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PLLIN/MODE")
				(number "2")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "FREQ")
				(number "1")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "VPRG1")
				(number "28")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "ITH1")
				(number "29")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "TRACK/SS1")
				(number "27")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "Vin")
				(number "22")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "EXTVcc")
				(number "21")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "INTVcc")
				(number "5")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "DRVcc")
				(number "20")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TG2")
				(number "16")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "BOOST2")
				(number "18")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SW2")
				(number "17")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "BG2")
				(number "19")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SENSE2+")
				(number "10")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SENSE2-")
				(number "9")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "VFB2")
				(number "11")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RUN2")
				(number "7")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PGOOD2")
				(number "4")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DRVSET")
				(number "14")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "DRVUV")
				(number "13")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "ILIM")
				(number "8")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "ITH2")
				(number "12")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "TRACK/SS2")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3892-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "LTC3892-1"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.05x7.56mm_ThermalVias"
			(at 8.89 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/38921fc.pdf"
			(at 0 29.21 0)
		)
		(property "Description" "60V dual 2-phase synchronous step-down DC/DC controller, forced continuous conduction mode, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter regulator dual-output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*1EP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC3892-1_0_1")
		(symbol "LTC3892-1_1_1"
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "TG1")
				(number "27")
			)
			(pin output line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "BOOST1")
				(number "25")
			)
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SW1")
				(number "26")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "BG1")
				(number "24")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SENSE1+")
				(number "3")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SENSE1-")
				(number "4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "VFB1")
				(number "2")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "RUN1")
				(number "8")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PLLIN/MODE")
				(number "6")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "FREQ")
				(number "5")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "ITH1")
				(number "1")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "TRACK/SS1")
				(number "28")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "Vin")
				(number "23")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "EXTVcc")
				(number "22")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "INTVcc")
				(number "7")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "DRVcc")
				(number "21")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TG2")
				(number "17")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "BOOST2")
				(number "19")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SW2")
				(number "18")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "BG2")
				(number "20")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SENSE2+")
				(number "11")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SENSE2-")
				(number "10")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "VFB2")
				(number "12")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RUN2")
				(number "9")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DRVSET")
				(number "15")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "DRVUV")
				(number "14")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "ITH2")
				(number "13")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "TRACK/SS2")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC7810"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "LTC7810"
			(at 15.494 24.13 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48-1EP_7x7mm_P0.5mm_EP3.6x3.6mm"
			(at 8.89 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf"
			(at 0 29.21 0)
		)
		(property "Description" "150V dual 2-phase synchronous step-down DC/DC controller, LQPF-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter regulator dual-output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP?48?1EP*7x7mm*P0.5mm*EP3.6x3.6mm*"
			(at 0 0 0)
		)
		(symbol "LTC7810_0_1")
		(symbol "LTC7810_1_1"
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "TG1")
				(number "42")
			)
			(pin output line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "BOOST1")
				(number "40")
			)
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SW1")
				(number "41")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "BG1")
				(number "37")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SENSE1+")
				(number "48")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SENSE1-")
				(number "1")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "VFB1")
				(number "47")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "RUN1")
				(number "32")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "REGSD")
				(number "7")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PLLIN/SPREAD")
				(number "4")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "FREQ")
				(number "6")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "OVLO")
				(number "9")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "ITH1")
				(number "46")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "TRACK/SS1")
				(number "45")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "Vin")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "25")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "EXTVcc")
				(number "11")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "SGND")
				(number "5")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "INTVcc")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "SGND")
				(number "49")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "DRVcc")
				(number "26")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TG2")
				(number "19")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "BOOST2")
				(number "21")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SW2")
				(number "20")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "BG2")
				(number "24")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SENSE2+")
				(number "13")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SENSE2-")
				(number "12")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "VFB2")
				(number "14")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RUN2")
				(number "29")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "NDRV")
				(number "10")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DRVSET")
				(number "2")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "MODE")
				(number "8")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "ITH2")
				(number "15")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "TRACK/SS2")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1200D40"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1200D40"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1200-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Off-Line Supplies, AC-DC, 40kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NCP1200D40_0_0")
		(symbol "NCP1200D40_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HV")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DRV")
				(number "5")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1200P40"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1200P40"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1200-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Off-Line Supplies, AC-DC, 40kHz, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "NCP1200P40_0_0")
		(symbol "NCP1200P40_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HV")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DRV")
				(number "5")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1207A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "NCP1207A"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1207B.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Free Running Quasi-Resonant Operation, AC-DC, 8us min Toff, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "NCP1207A_0_0")
		(symbol "NCP1207A_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "DMG")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin input line
				(at 0 10.16 270)
				(length 2.54)
				(name "HV")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "DRV")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1207B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "NCP1207B"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-N7_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1207B.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Free Running Quasi-Resonant Operation, AC-DC, 4.5us min Toff, SOIC-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*N7*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NCP1207B_0_0")
		(symbol "NCP1207B_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "DMG")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 0 10.16 270)
				(length 2.54)
				(name "HV")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "DRV")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1280"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "NCP1280"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP1280-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Active Clamp Voltage Mode PWM Controller for Off-Line Applications, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NCP1280_0_0")
		(symbol "NCP1280_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "FF")
				(number "4")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VAUX")
				(number "16")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "VREF")
				(number "11")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "UV/OV")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DCMAX")
				(number "8")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "VEA")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "13")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CS")
				(number "5")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "TD")
				(number "12")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SS")
				(number "9")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "RT")
				(number "7")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "CSKIP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1380A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1380A"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP1380-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Quasi-Resonant Current-Mode Controller for Off-Line Supplies, OVP/OTP, Latched OCP, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NCP1380A_0_0")
		(symbol "NCP1380A_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "FAULT")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ZCD")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CT")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DRV")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1653"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1653"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP1653-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Compact, Fixed-Frequency, Continuous Conduction Mode PFC Controller, 100kHz, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PFC SMPS Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "NCP1653_0_0")
		(symbol "NCP1653_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CS")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "VCONTROL")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "FB/SD")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "DRV")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VM")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP4308AD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP4308AD"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP4308-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Synchronous Rectifier Controller, 4A/8A, 4V UVLO, GaN Capable, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NCP4308AD_0_1")
		(symbol "NCP4308AD_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MIN_TOFF")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "MIN_TON")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DRV")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP4308AMT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP4308AMT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:OnSemi_DFN-8_2x2mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP4308-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Synchronous Rectifier Controller, 4A/8A, 4V UVLO, GaN Capable, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*DFN*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NCP4308AMT_0_1")
		(symbol "NCP4308AMT_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MIN_TOFF")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "MIN_TON")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DRV")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP4308DMN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP4308DMN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.39x2.21mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP4308-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Synchronous Rectifier Controller, 4A/8A, 4V UVLO, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*4x4mm*P0.8mm*EP2.39x2.21mm*"
			(at 0 0 0)
		)
		(symbol "NCP4308DMN_0_1")
		(symbol "NCP4308DMN_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MIN_TOFF")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "MIN_TON")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DRV")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP4308QD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP4308QD"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP4308-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Synchronous Rectifier Controller, 4A/8A, 4V UVLO, Max TON, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NCP4308QD_0_1")
		(symbol "NCP4308QD_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MIN_TOFF")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "MIN_TON")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MAX_TON")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DRV")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG3525"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 19.05 0)
		)
		(property "Value" "SG3525"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/sg3525.pdf"
			(at 0 0 0)
		)
		(property "Description" "Regulating Pulse Width Modulators, NOR Logic, PDIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*3.9x9.9mm*P1.27mm* SOIC*16*7.5x10.3mm*P1.27mm* DIP*16*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SG3525_0_1")
		(symbol "SG3525_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "NI")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INV")
				(number "1")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "COMP")
				(number "9")
			)
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "REF")
				(number "16")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SD")
				(number "10")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "SYNC")
				(number "3")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSC")
				(number "4")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CT")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DISCH")
				(number "7")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VIN")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VC")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA4862"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TDA4862"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-PFC_DCMICTDA4862G-DS-v02_00-en.pdf?fileId=db3a304412b407950112b417ffae24a3"
			(at 0 0 0)
		)
		(property "Description" "Power Factor Controller IC for High Power Factor and Active Harmonic Filter, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PFC SMPS Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TDA4862_0_0")
		(symbol "TDA4862_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VAOUT")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VSENSE")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MULTIN")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "DETIN")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "GTDRV")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ISENSE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL494"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 19.05 0)
		)
		(property "Value" "TL494"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl494.pdf"
			(at 0 0 0)
		)
		(property "Description" "Pulse-Width-Modulation Control Circuits, PDIP-16/SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm* SOIC*3.9x9.9mm*P1.27mm* SOIC*5.3x10.2mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TL494_0_1")
		(symbol "TL494_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "1IN-")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "1IN+")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "2IN+")
				(number "16")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "2IN-")
				(number "15")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin power_out line
				(at -12.7 0 0)
				(length 2.54)
				(name "REF")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DTC")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OUTCTRL")
				(number "13")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "C1")
				(number "8")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "C2")
				(number "11")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "E1")
				(number "9")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "E2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2375-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 -8.89 0)
		)
		(property "Value" "TPS2375-1"
			(at 7.62 -11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps2375-1"
			(at 0 20.32 0)
		)
		(property "Description" "IEEE802.3af PoE Controller, Auto-Retry"
			(at 0 0 0)
		)
		(property "ki_keywords" "IEEE802.3af PoE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS2375-1_0_1")
		(symbol "TPS2375-1_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DET")
				(number "3")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "ILIM")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CLASS")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PG")
				(number "6")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "RTN")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UC3525"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 19.05 0)
		)
		(property "Value" "UC3525"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc2525b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Regulating Pulse Width Modulators, NOR Logic, PDIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*7.5x10.3mm*P1.27mm* DIP*16*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "UC3525_0_1")
		(symbol "UC3525_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "NI")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INV")
				(number "1")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "COMP")
				(number "9")
			)
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "REF")
				(number "16")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SD")
				(number "10")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "SYNC")
				(number "3")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSC")
				(number "4")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CT")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DISCH")
				(number "7")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VIN")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VC")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UC3842_SOIC14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3842_SOIC14"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 100% Duty Cycle, 16V/10V UVLO, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UC3842_SOIC14_0_1")
		(symbol "UC3842_SOIC14_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "COMP")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VREF")
				(number "14")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RC")
				(number "7")
			)
			(pin no_connect line
				(at -10.16 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VC")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PWRGND")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CS")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UC3842_SOIC16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3842_SOIC16"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc2843a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 100% Duty Cycle, 16V/10V UVLO, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UC3842_SOIC16_0_1")
		(symbol "UC3842_SOIC16_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "COMP")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VREF")
				(number "15")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RC")
				(number "6")
			)
			(pin no_connect line
				(at -10.16 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VC")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PWRGND")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CS")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UC3842_SOIC8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3842_SOIC8"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 100% Duty Cycle, 16V/10V UVLO, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UC3842_SOIC8_0_1")
		(symbol "UC3842_SOIC8_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "COMP")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VREF")
				(number "8")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RC")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UC3854"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "UC3854"
			(at 1.27 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3854.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Power Factor Preregulator, DIP-16/SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "PFC SMPS Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "UC3854_0_0")
		(symbol "UC3854_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "ISENSE")
				(number "4")
			)
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CAOUT")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MULTOUT")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "PKLMT")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IAC")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VRMS")
				(number "8")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "ENA")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VSENSE")
				(number "11")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VAOUT")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "GTDRV")
				(number "16")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VREF")
				(number "9")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "RSET")
				(number "12")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SS")
				(number "13")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "CT")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC24610D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "UCC24610D"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc24610.pdf"
			(at 0 0 0)
		)
		(property "Description" "GREEN Rectifier Controller Device, 600kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UCC24610D_0_1")
		(symbol "UCC24610D_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN/TOFF")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "TON")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VD")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC24610DRB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "UCC24610DRB"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_DRB0008A"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc24610.pdf"
			(at 0 0 0)
		)
		(property "Description" "GREEN Rectifier Controller Device, 600kHz, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRB*"
			(at 0 0 0)
		)
		(symbol "UCC24610DRB_0_1")
		(symbol "UCC24610DRB_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN/TOFF")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "TON")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VD")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "GATE")
				(number "5")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC24612-1DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "UCC24612-1DBV"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc24612.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Frequency Synchronous Rectifier Controller, 1MHz, Min On Time = 375ns, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "UCC24612-1DBV_0_1")
		(symbol "UCC24612-1DBV_1_1"
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "REG")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VD")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "VG")
				(number "1")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC24630DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "UCC24630DBV"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc24630.pdf"
			(at 0 0 0)
		)
		(property "Description" "Synchronous Rectifier Controller, 200kHz, CCM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "UCC24630DBV_0_1")
		(symbol "UCC24630DBV_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "VSC")
				(number "2")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "TBLK")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VPC")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DRV")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC25600"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "UCC25600"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc25600.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Performance Resonant Mode Controller, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UCC25600_0_0")
		(symbol "UCC25600_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "OC")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "RT")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "DT")
				(number "1")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "GD1")
				(number "8")
			)
			(pin output line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "GD2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC256301"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 -16.51 0)
		)
		(property "Value" "UCC256301"
			(at 2.54 -19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-14-16_3.9x9.9mm_P1.27mm"
			(at 1.27 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ucc256301.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hybrid Hysteretic LLC Resonant Controller, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UCC256301_0_1")
		(symbol "UCC256301_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "HV")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "BLK")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ISNS")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VCR")
				(number "7")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "BW")
				(number "8")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "LL/SS")
				(number "9")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_out line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "RVCC")
				(number "12")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "HB")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "HO")
				(number "15")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "16")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "LO")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC25800"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.335 0)
		)
		(property "Value" "UCC25800"
			(at 10.16 -15.24 0)
		)
		(property "Footprint" "Package_SO:HVSSOP-8-1EP_3x3mm_P0.65mm_EP1.57x1.89mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ucc25800-q1.pdf"
			(at 0 -26.67 0)
		)
		(property "Description" "Ultra-low EMI Transformer Driver for Isolated Bias Supplies, HVSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transformer driver isolated bias supply llc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVSSOP*1EP*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "UCC25800_0_1")
		(symbol "UCC25800_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SYNC")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{DIS/FLT}")
				(number "2")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "VREG")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "OC/DT")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "RT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC2891"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 21.59 0)
		)
		(property "Value" "UCC2891"
			(at 5.08 19.05 0)
		)
		(property "Footprint" ""
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc2891.pdf"
			(at -5.08 -20.32 0)
		)
		(property "Description" "SMPS Current-Mode Active Clamp PWM Controller, SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "UCC2891_0_1")
		(symbol "UCC2891_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VIN")
				(number "16")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "LINEUV")
				(number "15")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VREF")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "FB")
				(number "9")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SS/SD")
				(number "10")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RTDEL")
				(number "1")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RTON")
				(number "2")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RTOFF")
				(number "3")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "RSLOPE")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "PGND")
				(number "11")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "AUX")
				(number "12")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "CS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC2892"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 21.59 0)
		)
		(property "Value" "UCC2892"
			(at 5.08 19.05 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc2892.pdf"
			(at -5.08 -13.97 0)
		)
		(property "Description" "SMPS Current-Mode Active Clamp PWM Controller, SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "UCC2892_0_1")
		(symbol "UCC2892_1_1"
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "LINEOV")
				(number "16")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "LINEUV")
				(number "15")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VREF")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "FB")
				(number "9")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SS/SD")
				(number "10")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RTDEL")
				(number "1")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RTON")
				(number "2")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RTOFF")
				(number "3")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "RSLOPE")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "PGND")
				(number "11")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "AUX")
				(number "12")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "CS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC2897"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 21.59 0)
		)
		(property "Value" "UCC2897"
			(at 5.08 19.05 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc2897.pdf"
			(at -5.08 -13.97 0)
		)
		(property "Description" "SMPS Advanced Current-Mode Active Clamp PWM Controller, TSSOP-20/QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm* QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "UCC2897_0_1")
		(symbol "UCC2897_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "LINEOV")
				(number "19")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "LINEUV")
				(number "18")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "FB")
				(number "11")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SS/SD")
				(number "12")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RTDEL")
				(number "3")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RTON")
				(number "4")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RTOFF")
				(number "5")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "RSLOPE")
				(number "10")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "PVDD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "PGND")
				(number "13")
			)
			(pin no_connect line
				(at 12.7 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "15")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "AUX")
				(number "14")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "CS")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC3800"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3800"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3800.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power BiCMOS Current-Mode PWM Controllers, 100% Duty Cycle, 7.2V/6.9V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "UCC3800_0_1")
		(symbol "UCC3800_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "COMP")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "REF")
				(number "8")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RC")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC3808D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "UCC3808D"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3808-2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Current Mode Push-Pull PWM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UCC3808D_0_1")
		(symbol "UCC3808D_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "COMP")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CS")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RC")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC3808N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "UCC3808N"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3808-2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Current Mode Push-Pull PWM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "UCC3808N_0_1")
		(symbol "UCC3808N_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "COMP")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CS")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RC")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "1")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC3895DW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "UCC3895DW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3895.pdf"
			(at -1.27 2.54 0)
		)
		(property "Description" "BiCMOS, Advanced Phase-ShiftPWM Controller, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Phase-shift full-bridge converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UCC3895DW_0_1")
		(symbol "UCC3895DW_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "EAN")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "EAOUT")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RAMP")
				(number "3")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "REF")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "6")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CT")
				(number "7")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "8")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DELAB")
				(number "9")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DELCD")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "16")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "EAP")
				(number "20")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SS/DISB")
				(number "19")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "18")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "17")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTC")
				(number "14")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTD")
				(number "13")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CS")
				(number "12")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "ADS")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC3895N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "UCC3895N"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm_LongPads"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3895.pdf"
			(at -1.27 2.54 0)
		)
		(property "Description" "BiCMOS, Advanced Phase-ShiftPWM Controller, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Phase-shift full-bridge converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "UCC3895N_0_1")
		(symbol "UCC3895N_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "EAN")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "EAOUT")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RAMP")
				(number "3")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "REF")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "6")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CT")
				(number "7")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "8")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DELAB")
				(number "9")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DELCD")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "16")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "EAP")
				(number "20")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SS/DISB")
				(number "19")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "18")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "17")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTC")
				(number "14")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTD")
				(number "13")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CS")
				(number "12")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "ADS")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC3895PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "UCC3895PW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3895.pdf"
			(at -1.27 2.54 0)
		)
		(property "Description" "BiCMOS, Advanced Phase-ShiftPWM Controller, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Phase-shift full-bridge converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "UCC3895PW_0_1")
		(symbol "UCC3895PW_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "EAN")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "EAOUT")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RAMP")
				(number "3")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "REF")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "6")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CT")
				(number "7")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "8")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DELAB")
				(number "9")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DELCD")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "16")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "EAP")
				(number "20")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SS/DISB")
				(number "19")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "18")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "17")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTC")
				(number "14")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTD")
				(number "13")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CS")
				(number "12")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "ADS")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE2PCS01"
		(extends "ICE1PCS01")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE2PCS01"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE2PCS01-DS-v02_03-en.pdf?fileId=db3a304412b407950112b427caa43ccf"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICE2PCS02"
		(extends "ICE1PCS02")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE2PCS02"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE2PCS02-DS-v02_04-en.pdf?fileId=db3a304412b407950112b427cc3c3cdc"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM With Input Brown-Out Protection, 65kHz, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICE2PCS03"
		(extends "ICE1PCS02")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE2PCS03"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE2PCS03-DS-v02_01-en.pdf?fileId=db3a30431936bc4b01193b45457e52a1"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM With Input Brown-Out Protection, 100kHz, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICE2PCS04"
		(extends "ICE1PCS02")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE2PCS04"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE2PCS04-DS-v02_01-en.pdf?fileId=db3a30431936bc4b01193b4e467952a9"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM With Input Brown-Out Protection, 133kHz, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICE2PCS05"
		(extends "ICE1PCS01")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE2PCS05"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE2PCS05-DS-v01_02-en.pdf?fileId=db3a30431c69a49d011cdfb46a834373"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICE2PCS06"
		(extends "ICE1PCS02")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "ICE2PCS06"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ICE2PCS06-DS-v01_01-en.pdf?fileId=db3a3043327f13e3013285ff4ecb2e77"
			(at 0 0 0)
		)
		(property "Description" "Standalone PFC Controller in CCM With Input Brown-Out Protection, 65kHz, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR11662S"
		(extends "IR1167S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR11662S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir11662spbf.pdf?fileId=5546d462533600a4015355c44195164f"
			(at 0 0 0)
		)
		(property "Description" "Advanced SmartRectifier Control IC, 500kHz, 200V, 1.0/4.0A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR11672AS"
		(extends "IR1167S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR11672AS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir11672aspbf.pdf?fileId=5546d462533600a4015355c455561653"
			(at 0 0 0)
		)
		(property "Description" "Advanced SmartRectifier Control IC, 500kHz, 200V, 2.0/7.0A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR11682S"
		(extends "IR1168S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR11682S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir11682spbf.pdf?fileId=5546d462533600a4015355c47188165a"
			(at 0 0 0)
		)
		(property "Description" "Dual SmartRectifier Driver IC, 400kHz, 200V, 1.0/4.0A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L6562"
		(extends "L6561")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "L6562"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6562.pdf"
			(at 0 0 0)
		)
		(property "Description" "Transition-Mode PFC Controller, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "L6562A"
		(extends "L6561")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "L6562A"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6562a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Transition-Mode PFC Controller, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "L6562AT"
		(extends "L6561")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "L6562AT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6562at.pdf"
			(at 0 0 0)
		)
		(property "Description" "Transition-Mode PFC Controller, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "L6563A"
		(extends "L6563")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "L6563A"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6563.pdf"
			(at 0 0 0)
		)
		(property "Description" "Advanced Transition-Mode PFC Controller, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L6563S"
		(extends "L6563")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "L6563S"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6563s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Enhanced Transition-Mode PFC Controller, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L6564T"
		(extends "L6564")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "L6564T"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-10_3.9x4.9mm_P1.00mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l6564t.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-Pin Transition-Mode PFC Controller for Outdoor Applications, SSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS pfc controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P1.00mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM3478MM"
		(extends "LM3478MA")
		(property "Reference" "U"
			(at -9.525 8.89 0)
		)
		(property "Value" "LM3478MM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 25.4 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lm3478"
			(at 0.635 12.7 0)
		)
		(property "Description" "2.97~40V Wide Input Range Boost/SEPIC/Flyback DC-DC Controller, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost flyback SEPIC DC-DC controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM3478QMM"
		(extends "LM3478MA")
		(property "Reference" "U"
			(at -9.525 8.89 0)
		)
		(property "Value" "LM3478QMM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 25.4 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lm3478q-q1"
			(at 0.635 12.7 0)
		)
		(property "Description" "2.97~40V Wide Input Range Boost/SEPIC/Flyback DC-DC Controller, AEC-Q100 Qualified, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost flyback SEPIC DC-DC controller Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3892-2"
		(extends "LTC3892")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "LTC3892-2"
			(at 15.494 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 8.89 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/38921fc.pdf"
			(at 0 29.21 0)
		)
		(property "Description" "60V dual 2-phase synchronous step-down DC/DC controller, pulse-skipping, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter regulator dual-output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1200D100"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1200D100"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1200-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Off-Line Supplies, AC-DC, 100kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1200D60"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1200D60"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1200-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Off-Line Supplies, AC-DC, 60kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1200P100"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1200P100"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1200-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Off-Line Supplies, AC-DC, 100kHz, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1200P60"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1200P60"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1200-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Off-Line Supplies, AC-DC, 60kHz, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1203D100"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1203D100"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1203-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Universal Off-Line Supplies Featuring Standby and Short Circuit Protection, AC-DC, 100kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1203D40"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1203D40"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1203-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Universal Off-Line Supplies Featuring Standby and Short Circuit Protection, AC-DC, 40kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1203D60"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1203D60"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1203-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Universal Off-Line Supplies Featuring Standby and Short Circuit Protection, AC-DC, 60kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1203P100"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1203P100"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1203-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Universal Off-Line Supplies Featuring Standby and Short Circuit Protection, AC-DC, 100kHz, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1203P40"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1203P40"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1203-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Universal Off-Line Supplies Featuring Standby and Short Circuit Protection, AC-DC, 40kHz, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1203P60"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1203P60"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1203-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "PWM Current-Mode Controller for Universal Off-Line Supplies Featuring Standby and Short Circuit Protection, AC-DC, 60kHz, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217AD100"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217AD100"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 100kHz, 1ms Soft Start, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217AD133"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217AD133"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 133kHz, 1ms Soft Start, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217AD65"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217AD65"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 65kHz, 1ms Soft Start, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217AP100"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217AP100"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 100kHz, 1ms Soft Start, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217AP133"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217AP133"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 133kHz, 1ms Soft Start, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217AP65"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217AP65"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 65kHz, 1ms Soft Start, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217D100"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217D100"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 100kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217D133"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217D133"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 133kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217D65"
		(extends "NCP1200D40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217D65"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 65kHz, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217P100"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217P100"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 100kHz, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217P133"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217P133"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 133kHz, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1217P65"
		(extends "NCP1200P40")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1217P65"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1217-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Enhanced PWM Current-Mode Controller for High-Power Universal Off-Line Supplies, AC-DC, 65kHz, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1380B"
		(extends "NCP1380A")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1380B"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP1380-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Quasi-Resonant Current-Mode Controller for Off-Line Supplies, OVP/OTP, Auto-Recovery OCP, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1380C"
		(extends "NCP1380A")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1380C"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP1380-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Quasi-Resonant Current-Mode Controller for Off-Line Supplies, UVP/OVP, Latched OCP, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1380D"
		(extends "NCP1380A")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1380D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP1380-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Quasi-Resonant Current-Mode Controller for Off-Line Supplies, UVP/OVP, Auto-Recovery OCP, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1653A"
		(extends "NCP1653")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP1653A"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP1653-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Compact, Fixed-Frequency, Continuous Conduction Mode PFC Controller, 67kHz, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PFC SMPS Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP4308DD"
		(extends "NCP4308AD")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP4308DD"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP4308-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Synchronous Rectifier Controller, 4A/8A, 4V UVLO, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP4308DMT"
		(extends "NCP4308AMT")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCP4308DMT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:OnSemi_DFN-8_2x2mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP4308-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Synchronous Rectifier Controller, 4A/8A, 4V UVLO, WDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*DFN*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SG3527"
		(extends "SG3525")
		(property "Reference" "U"
			(at 3.81 19.05 0)
		)
		(property "Value" "SG3527"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_view/11120-sg1525a-sg1527a-datasheet"
			(at 0 0 0)
		)
		(property "Description" "Regulating Pulse Width Modulators, OR Logic, PDIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*3.9x9.9mm*P1.27mm* SOIC*16*7.5x10.3mm*P1.27mm* DIP*16*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TDA4863"
		(extends "TDA4862")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TDA4863"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-TDA4863-DS-v02_00-en.pdf?fileId=db3a304412b407950112b427d2d23ce8"
			(at 0 0 0)
		)
		(property "Description" "Power Factor Controller IC for High Power Factor and Low THD, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PFC SMPS Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TDA4863-2"
		(extends "TDA4862")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TDA4863-2"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-TDA4863_2-DS-v02_01-en.pdf?fileId=db3a304412b407950112b41802de24ab"
			(at 0 0 0)
		)
		(property "Description" "Power Factor Controller IC for High Power Factor and Low THD, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PFC SMPS Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3527"
		(extends "UC3525")
		(property "Reference" "U"
			(at 3.81 19.05 0)
		)
		(property "Value" "UC3527"
			(at 3.81 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc2525b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Regulating Pulse Width Modulators, OR Logic, PDIP-16/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*7.5x10.3mm*P1.27mm* DIP*16*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3842_DIP8"
		(extends "UC3842_SOIC8")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3842_DIP8"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 100% Duty Cycle, 16V/10V UVLO, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3843_DIP8"
		(extends "UC3842_SOIC8")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3843_DIP8"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 100% Duty Cycle, 8.4V/7.6V UVLO, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3843_SOIC14"
		(extends "UC3842_SOIC14")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3843_SOIC14"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 100% Duty Cycle, 8.4V/7.6V UVLO, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3843_SOIC8"
		(extends "UC3842_SOIC8")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3843_SOIC8"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 100% Duty Cycle, 8.4V/7.6V UVLO, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3844_DIP8"
		(extends "UC3842_SOIC8")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3844_DIP8"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 50% Duty Cycle, 16V/10V UVLO, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3844_SOIC14"
		(extends "UC3842_SOIC14")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3844_SOIC14"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 50% Duty Cycle, 16V/10V UVLO, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3844_SOIC8"
		(extends "UC3842_SOIC8")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3844_SOIC8"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 50% Duty Cycle, 16V/10V UVLO, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3845_DIP8"
		(extends "UC3842_SOIC8")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3845_DIP8"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 50% Duty Cycle, 8.4V/7.6V UVLO, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3845_SOIC14"
		(extends "UC3842_SOIC14")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3845_SOIC14"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 50% Duty Cycle, 8.4V/7.6V UVLO, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UC3845_SOIC8"
		(extends "UC3842_SOIC8")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UC3845_SOIC8"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uc3842.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current-Mode PWM Controllers, 50% Duty Cycle, 8.4V/7.6V UVLO, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC1895J"
		(extends "UCC3895N")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "UCC1895J"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm_LongPads"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3895.pdf"
			(at -1.27 2.54 0)
		)
		(property "Description" "BiCMOS, Advanced Phase-ShiftPWM Controller, CDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Phase-shift full-bridge converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC24612-2DBV"
		(extends "UCC24612-1DBV")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "UCC24612-2DBV"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc24612.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Frequency Synchronous Rectifier Controller, 800kHz, Min On Time = 540ns, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "UCC24636DBV"
		(extends "UCC24630DBV")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "UCC24636DBV"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc24636.pdf"
			(at 0 0 0)
		)
		(property "Description" "Synchronous Rectifier Controller, 130kHz, DCM/TM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous rectifier controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "UCC2893"
		(extends "UCC2891")
		(property "Reference" "U"
			(at 5.08 21.59 0)
		)
		(property "Value" "UCC2893"
			(at 5.08 19.05 0)
		)
		(property "Footprint" ""
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc2893.pdf"
			(at -5.08 -20.32 0)
		)
		(property "Description" "SMPS Current-Mode Active Clamp PWM Controller, SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC2894"
		(extends "UCC2892")
		(property "Reference" "U"
			(at 5.08 21.59 0)
		)
		(property "Value" "UCC2894"
			(at 5.08 19.05 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc2894.pdf"
			(at -5.08 -13.97 0)
		)
		(property "Description" "SMPS Current-Mode Active Clamp PWM Controller, SOIC-16/TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC2895DW"
		(extends "UCC3895DW")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "UCC2895DW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3895.pdf"
			(at -1.27 2.54 0)
		)
		(property "Description" "BiCMOS, Advanced Phase-ShiftPWM Controller, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Phase-shift full-bridge converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC2895N"
		(extends "UCC3895N")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "UCC2895N"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm_LongPads"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3895.pdf"
			(at -1.27 2.54 0)
		)
		(property "Description" "BiCMOS, Advanced Phase-ShiftPWM Controller, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Phase-shift full-bridge converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC2895PW"
		(extends "UCC3895PW")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "UCC2895PW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3895.pdf"
			(at -1.27 2.54 0)
		)
		(property "Description" "BiCMOS, Advanced Phase-ShiftPWM Controller, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Phase-shift full-bridge converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3801"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3801"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3800.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power BiCMOS Current-Mode PWM Controllers, 50% Duty Cycle, 9.4V/7.4V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3802"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3802"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3800.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power BiCMOS Current-Mode PWM Controllers, 100% Duty Cycle, 12.5V/8.3V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3803"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3803"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3800.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power BiCMOS Current-Mode PWM Controllers, 100% Duty Cycle, 4.1V/3.6V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3804"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3804"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3800.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power BiCMOS Current-Mode PWM Controllers, 50% Duty Cycle, 12.5V/8.3V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3805"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3805"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3800.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power BiCMOS Current-Mode PWM Controllers, 50% Duty Cycle, 4.1V/3.6V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3813-0"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3813-0"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3813-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power Economy BiCMOS Current-Mode PWM, 100% Duty Cycle, 7.2V/6.9V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3813-1"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3813-1"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3813-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power Economy BiCMOS Current-Mode PWM, 50% Duty Cycle, 9.4V/7.4V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3813-2"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3813-2"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3813-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power Economy BiCMOS Current-Mode PWM, 100% Duty Cycle, 12.5V/8.3V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3813-3"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3813-3"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3813-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power Economy BiCMOS Current-Mode PWM, 100% Duty Cycle, 4.1V/3.6V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3813-4"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3813-4"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3813-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power Economy BiCMOS Current-Mode PWM, 50% Duty Cycle, 12.5V/8.3V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC3813-5"
		(extends "UCC3800")
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "UCC3813-5"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc3813-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-Power Economy BiCMOS Current-Mode PWM, 50% Duty Cycle, 4.1V/3.6V UVLO, DIP-8/SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS PWM Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
)
