(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CAT3200"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 11.43 0)
		)
		(property "Value" "CAT3200"
			(at 7.62 -11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/cat3200-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Noise Regulated Charge Pump DC-DC Converter, 100 mA, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switched capacitor charge pump"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*"
			(at 0 0 0)
		)
		(symbol "CAT3200_0_1")
		(symbol "CAT3200_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "CPOS")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "CNEG")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "SGND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "8")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAT3200-5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 11.43 0)
		)
		(property "Value" "CAT3200-5"
			(at 6.35 -11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/cat3200-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Noise Regulated Charge Pump DC-DC Converter, 5 V, 100 mA, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "switched capacitor charge pump"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "CAT3200-5_0_1")
		(symbol "CAT3200-5_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "CPOS")
				(number "6")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "CNEG")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2665M6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM2665M6"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm2665.pdf"
			(at -46.99 31.75 0)
		)
		(property "Description" "Switched Capacitor Voltage Converter, Doubles or Splits Input Supply Voltage (2.5 V to 5.5 V or 1.8 V to 11 V), 40 mA, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "switched capacitor voltage converter doubler splitter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM2665M6_0_1")
		(symbol "LM2665M6_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CAP+")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CAP-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2775DSG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM2775DSG"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lm2775"
			(at 0 0 0)
		)
		(property "Description" "5V charge pump, 200mA, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Charge pump inductorless"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM2775DSG_0_1")
		(symbol "LM2775DSG_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PFM")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OUTDIS")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "C1+")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "C1-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2776"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM2776"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2776.pdf"
			(at -46.99 31.75 0)
		)
		(property "Description" "Switched capacitor inverter, inverts positive voltage +2.7 to +5.5V to negative, 200mA, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switched capacitor inverter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM2776_0_1")
		(symbol "LM2776_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "C1+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "C1-")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM27761"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LM27761"
			(at 3.302 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 3.81 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm27761.pdf"
			(at 63.5 -10.16 0)
		)
		(property "Description" "low-noise regulated switched-capacitor voltage inverter with 2.7V-5.5V input to -1.5 to -5V Output Voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "low-noise switched capacitor voltage converter invert"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP?2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM27761_0_1")
		(symbol "LM27761_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "C+")
				(number "8")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "C-")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VFB")
				(number "5")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CPOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM27762"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 8.89 0)
		)
		(property "Value" "LM27762"
			(at 6.096 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-12-1EP_3x2mm_P0.5mm_EP1x2.65_ThermalVias"
			(at 3.81 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm27762.pdf"
			(at 63.5 -10.16 0)
		)
		(property "Description" "Low-noise inverting charge pump with both positive and negative LDO's, with 2.7V-5.5V input to +1.5 to +5V and -1.5 to -5V Output Voltage, WSON-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low-noise inverting charge pump with both positive and negative LDO's"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP?3x2mm*P0.5mm*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "LM27762_0_1")
		(symbol "LM27762_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "PGOOD")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN-")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN+")
				(number "12")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "C+")
				(number "10")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "C-")
				(number "9")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "PAD")
				(number "13")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT+")
				(number "11")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB+")
				(number "2")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FB-")
				(number "7")
			)
			(pin power_out line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT-")
				(number "6")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "CP")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM7705"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LM7705"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm7705.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative bias generator, low-noise, 3-5.25V input, -0.232V fixed output, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switched capacitor voltage converter inverter negative bias regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM7705_0_1")
		(symbol "LM7705_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SD")
				(number "3")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "CF+")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CF-")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CRES")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMC7660"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 11.43 0)
		)
		(property "Value" "LMC7660"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at -66.04 30.48 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmc7660.pdf"
			(at -66.04 30.48 0)
		)
		(property "Description" "Voltage converter from +1.5V to +10V to +1.5V to +10V, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LMC7660_0_1")
		(symbol "LMC7660_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OSC")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "LV")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CAP+")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CAP-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1054"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 11.176 0)
		)
		(property "Value" "LT1054"
			(at 4.318 11.176 0)
		)
		(property "Footprint" ""
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1054lfh.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched-Capacitor Voltage Converter with Regulator, output current 100mA, operating range 3.5V to 15V, low loss 1.1V at 100mA, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "monolithic bipolar switched capacitor voltage converter regulator inverter doubler shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "LT1054_0_1")
		(symbol "LT1054_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "FB/SHDN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OSC")
				(number "7")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "-VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CAP+")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CAP-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1054xSW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 11.176 0)
		)
		(property "Value" "LT1054xSW"
			(at 4.318 11.176 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1054lfh.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched-Capacitor Voltage Converter with Regulator, output current 100mA, operating range 3.5V to 15V, low loss 1.1V at 100mA, SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "monolithic bipolar switched capacitor voltage converter regulator inverter doubler shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?16W*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1054xSW_0_1")
		(symbol "LT1054xSW_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "FB/SHDN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OSC")
				(number "7")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "-VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CAP+")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CAP-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1044"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LTC1044"
			(at 3.81 11.43 0)
		)
		(property "Footprint" ""
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1044.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched Capacitor Voltage Converter, 1.5V to 9V supply operation, 200uA Max No Load Supply Current at 5V, DIP-8/TO-99"
			(at 0 0 0)
		)
		(property "ki_keywords" "monolithic CMOS switched capacitor voltage converter invert double divide multiply boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* TO?99*"
			(at 0 0 0)
		)
		(symbol "LTC1044_0_1")
		(symbol "LTC1044_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "BOOST")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OSC")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "LV")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CAP+")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CAP-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1502xS8-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.144 11.684 0)
		)
		(property "Value" "LTC1502xS8-3.3"
			(at 1.524 11.684 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -24.384 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/15023f.pdf"
			(at 3.81 -20.32 0)
		)
		(property "Description" "Single Alkaline / NiCd Cell to 3.3V Regulated Charge Pump DC/DC Converter, 0.9..1.8V input, 10mA output, SOIC-8"
			(at 0.508 -22.352 0)
		)
		(property "ki_keywords" "Linear-Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.*4.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1502xS8-3.3_0_1")
		(symbol "LTC1502xS8-3.3_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "V_{IN}")
				(number "5")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "C1^{+}")
				(number "2")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "C1^{-}/~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "8")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "C3^{+}")
				(number "7")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "C3^{-}")
				(number "6")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "C2")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1503CMS8-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 11.176 0)
		)
		(property "Value" "LTC1503CMS8-2"
			(at 4.318 11.176 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1503f.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched-Capacitor Voltage Step-Down Converter, 2V output, max output current 100mA, operating range 2.4V to 6V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator inductorless"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*"
			(at 0 0 0)
		)
		(symbol "LTC1503CMS8-2_0_1")
		(symbol "LTC1503CMS8-2_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{SHDN}/SS")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "C1+")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "C1-")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C2+")
				(number "6")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "C2-")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1751"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 12.7 0)
		)
		(property "Value" "LTC1751"
			(at 5.08 12.7 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1751f.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA charge-pump, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "charge pump"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65*"
			(at 0 0 0)
		)
		(symbol "LTC1751_0_1")
		(symbol "LTC1751_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PGOOD/FB")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C+")
				(number "6")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "C-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1754"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "LTC1754"
			(at 5.08 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/175435f.pdf"
			(at 0 0 0)
		)
		(property "Description" "40mA charge-pump, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "charge pump"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC1754_0_1")
		(symbol "LTC1754_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CP+")
				(number "6")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CP-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3260xDE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 29.718 0)
		)
		(property "Value" "LTC3260xDE"
			(at 0.254 26.924 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4mm_P0.5mm_EP1.7x3.3mm"
			(at 0 -38.354 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc3260.pdf"
			(at 0.762 -44.196 0)
		)
		(property "Description" "Low Noise Dual Supply Inverting Charge Pump with both positive and negative LDO regulators, V_{IN} range 4.5V to 32V, 50 mA LDO output current, DFN-14-1EP"
			(at 0 -41.148 0)
		)
		(property "ki_keywords" "switched capacitor inverting bipolar supply charge pump positive negativ ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x4mm*P0.5mm*EP1.7x3.3mm*"
			(at 0 0 0)
		)
		(symbol "LTC3260xDE_1_1"
			(pin power_in line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "V_{IN}")
				(number "9")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "EN^{+}")
				(number "1")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "EN^{-}")
				(number "11")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "MODE")
				(number "12")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "2")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "V_{OUT}")
				(number "6")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "C^{+}")
				(number "8")
			)
			(pin passive line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "C^{-}")
				(number "7")
			)
			(pin power_out line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "LDO^{+}")
				(number "10")
			)
			(pin input line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "ADJ^{+}")
				(number "13")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "BYP^{+}")
				(number "14")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "BYP^{-}")
				(number "3")
			)
			(pin input line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "ADJ^{-}")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -22.86 180)
				(length 2.54)
				(name "LDO^{-}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3260xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 29.718 0)
		)
		(property "Value" "LTC3260xMSE"
			(at 0.254 26.924 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 0 -38.354 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc3260.pdf"
			(at 0.762 -44.196 0)
		)
		(property "Description" "Low Noise Dual Supply Inverting Charge Pump with both positive and negative LDO regulators, V_{IN} range 4.5V to 32V, 50 mA LDO output current, MSOP-16"
			(at 0 -41.148 0)
		)
		(property "ki_keywords" "switched capacitor inverting bipolar supply charge pump positive negativ ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x4.039mm*P0.5mm*EP1.651x2.845mm*"
			(at 0 0 0)
		)
		(symbol "LTC3260xMSE_1_1"
			(pin power_in line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "V_{IN}")
				(number "11")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "EN^{+}")
				(number "1")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "EN^{-}")
				(number "13")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "MODE")
				(number "14")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "2")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "V_{OUT}")
				(number "6")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "C^{+}")
				(number "10")
			)
			(pin passive line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "C^{-}")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_out line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "LDO^{+}")
				(number "12")
			)
			(pin input line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "ADJ^{+}")
				(number "15")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "BYP^{+}")
				(number "16")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "BYP^{-}")
				(number "3")
			)
			(pin input line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "ADJ^{-}")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -22.86 180)
				(length 2.54)
				(name "LDO^{-}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC660"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LTC660"
			(at 3.81 11.43 0)
		)
		(property "Footprint" ""
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/660fa.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Monolithic CMOS switched-capacitor from 1.5V to 5.5V up to 100mA, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "monolithic CMOS switched capacitor voltage converter invert double divide multiply boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "LTC660_0_1")
		(symbol "LTC660_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "BOOST")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OSC")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "LV")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CAP+")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CAP-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1044"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MAX1044"
			(at 3.81 11.43 0)
		)
		(property "Footprint" ""
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/ICL7660-MAX1044.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched-Capacitor Voltage Converter, 1.5V to 10.0V operating supply voltage, 10mA with a 0.5V output drop, SO-8/DIP-8/µMAX-8/TO-99"
			(at 0 0 0)
		)
		(property "ki_keywords" "monolithic CMOS switched capacitor voltage converter invert double divide multiply boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* MSOP*3x3mm*P0.65mm* TO?99*"
			(at 0 0 0)
		)
		(symbol "MAX1044_0_1")
		(symbol "MAX1044_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OSC")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "LV")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CAP+")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CAP-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RT9361AxE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "RT9361AxE"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://www.richtek.com/assets/product_file/RT9361A=RT9361B/DS9361AB-14.pdf"
			(at 0 0 0)
		)
		(property "Description" "Switched capacitor boost, Fixed 5V output, 110mA, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switched capacitor boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "RT9361AxE_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "CN")
				(number "4")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CP")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS60151DRV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS60151DRV"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps60151.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 140mA charge-pump, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "charge pump"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS60151DRV_0_1")
		(symbol "TPS60151DRV_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ENA")
				(number "6")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "EP")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CP+")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CP-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS60400DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "TPS60400DBV"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps60400.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Unregulated 60-mA Charge Pump Voltage Inverter with Variable Switching Frequency 50 kHz - 250 kHz, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "unregulated charge pump inverter variable switching frequency"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS60400DBV_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "C_{FLY+}")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "C_{FLY-}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS60500DGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "TPS60500DGS"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps60503.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "250mA High-Efficiency Step-Down Charge Pump Regulator, Adjustable Output Voltage, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator Step-Down Charge Pump TPS Texas Instruments Ti"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS60500DGS_0_1")
		(symbol "TPS60500DGS_1_1"
			(pin power_in line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{EN}")
				(number "1")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "C1+")
				(number "6")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "C1-")
				(number "8")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "C2+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "C2-")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "VOUT")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PG")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICL7660"
		(extends "MAX1044")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "ICL7660"
			(at 3.81 11.43 0)
		)
		(property "Footprint" ""
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/ICL7660-MAX1044.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched-Capacitor Voltage Converter, 1.5V to 10.0V operating supply voltage, 10mA with a 0.5V output drop, SO-8/DIP-8/µMAX-8/TO-99"
			(at 0 0 0)
		)
		(property "ki_keywords" "monolithic CMOS switched capacitor voltage converter invert double divide multiply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* MSOP*3x3mm*P0.65mm* TO?99*"
			(at 0 0 0)
		)
	)
	(symbol "LT1054L"
		(extends "LT1054")
		(property "Reference" "U"
			(at -6.604 11.176 0)
		)
		(property "Value" "LT1054L"
			(at 4.318 11.176 0)
		)
		(property "Footprint" ""
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1054lfh.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched-Capacitor Voltage Converter with Regulator, output current 125mA, operating range 3.5V to 15V, low loss 1.1V at 100mA, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "monolithic bipolar switched capacitor voltage converter regulator inverter doubler shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1502xMS8-3.3"
		(extends "LTC1502xS8-3.3")
		(property "Reference" "U"
			(at -9.144 11.684 0)
		)
		(property "Value" "LTC1502xMS8-3.3"
			(at 1.524 11.684 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -24.384 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/15023f.pdf"
			(at 3.81 -20.32 0)
		)
		(property "Description" "Single Alkaline / NiCd Cell to 3.3V Regulated Charge Pump DC/DC Converter, 0.9..1.8V input, 10mA output, MSOP-8"
			(at 0.508 -22.352 0)
		)
		(property "ki_keywords" "Linear-Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MSOP*3*3*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1503CMS8-1.8"
		(extends "LTC1503CMS8-2")
		(property "Reference" "U"
			(at -6.604 11.176 0)
		)
		(property "Value" "LTC1503CMS8-1.8"
			(at 4.318 11.176 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1503f.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched-Capacitor Voltage Step-Down Converter, 1.8V output, max output current 100mA, operating range 2.4V to 6V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator inductorless"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1503xS8-1.8"
		(extends "LTC1503CMS8-2")
		(property "Reference" "U"
			(at -6.604 11.176 0)
		)
		(property "Value" "LTC1503xS8-1.8"
			(at 4.318 11.176 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1503f.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched-Capacitor Voltage Step-Down Converter, 1.8V output, max output current 100mA, operating range 2.4V to 6V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator inductorless"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1503xS8-2"
		(extends "LTC1503CMS8-2")
		(property "Reference" "U"
			(at -6.604 11.176 0)
		)
		(property "Value" "LTC1503xS8-2"
			(at 4.318 11.176 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1503f.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "Switched-Capacitor Voltage Step-Down Converter, 2V output, max output current 100mA, operating range 2.4V to 6V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator inductorless"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "RT9361BxE"
		(extends "RT9361AxE")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "RT9361BxE"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 17.78 -8.89 0)
		)
		(property "Datasheet" "https://www.richtek.com/assets/product_file/RT9361A=RT9361B/DS9361AB-14.pdf"
			(at 0 0 0)
		)
		(property "Description" "Switched capacitor boost, Fixed 4.5V output, 150mA, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switched capacitor boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS60401DBV"
		(extends "TPS60400DBV")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "TPS60401DBV"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps60401.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Unregulated 60-mA Charge Pump Voltage Inverter with Fixed Switching Frequency 20 kHz, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "unregulated charge pump inverter fixed switching frequency"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS60402DBV"
		(extends "TPS60400DBV")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "TPS60402DBV"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps60401.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Unregulated 60-mA Charge Pump Voltage Inverter with Fixed Switching Frequency 50 kHz, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "unregulated charge pump inverter fixed switching frequency"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS60403DBV"
		(extends "TPS60400DBV")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "TPS60403DBV"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps60401.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Unregulated 60-mA Charge Pump Voltage Inverter with Fixed Switching Frequency 250 kHz, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "unregulated charge pump inverter fixed switching frequency"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS60501DGS"
		(extends "TPS60500DGS")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "TPS60501DGS"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps60503.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA High-Efficiency Step-Down Charge Pump Regulator, 3.3V Output Voltage, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator Step-Down Charge Pump TPS Texas Instruments Ti"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS60502DGS"
		(extends "TPS60500DGS")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "TPS60502DGS"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps60503.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA High-Efficiency Step-Down Charge Pump Regulator, 1.8V Output Voltage, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator Step-Down Charge Pump TPS Texas Instruments Ti"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS60503DGS"
		(extends "TPS60500DGS")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "TPS60503DGS"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps60503.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA High-Efficiency Step-Down Charge Pump Regulator, 1.5V Output Voltage, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator Step-Down Charge Pump TPS Texas Instruments Ti"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
