(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "171050601"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "171050601"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 0 0 0)
		)
		(property "Datasheet" "https://katalog.we-online.de/pm/datasheet/171050601.pdf"
			(at -1.27 19.05 0)
		)
		(property "Description" "MagI3C Power Module, Variable Step Down Regulator Module, 6 to 36V Input Voltage, 0.8 to 6V, 5A Output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "power module regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*TabPin8*"
			(at 0 0 0)
		)
		(symbol "171050601_0_1")
		(symbol "171050601_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SYNC")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PGND")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "7")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SS/TRK")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A4403GEU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "A4403GEU"
			(at -2.54 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/~/media/Files/Datasheets/A4403-Datasheet.ashx"
			(at -6.35 11.43 0)
		)
		(property "Description" "Valley current mode buck converter, 46V, 3A, up to 2MHz, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "A4403GEU_0_1")
		(symbol "A4403GEU_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "TON")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DIS")
				(number "10")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "SGND")
				(number "9")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "BOOT")
				(number "11")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LX")
				(number "12")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ISEN")
				(number "8")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AAT1217ICA-1.2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AAT1217ICA-1.2"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/AAT1217_202050B.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA, 2.5-5.5V, 1.2MHz, Micropower Synchronous Step-Up Converter, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator step-up adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "AAT1217ICA-1.2_0_1")
		(symbol "AAT1217ICA-1.2_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AAT1217IGU-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AAT1217IGU-3.3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/AAT1217_202050B.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA, 3.3V, 1.2MHz, Micropower Synchronous Step-Up Converter, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AAT1217IGU-3.3_0_1")
		(symbol "AAT1217IGU-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP2108AUJ-1.0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-1.0"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 1.0V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "ADP2108AUJ-1.0_0_1")
		(symbol "ADP2108AUJ-1.0_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP2302ARDZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADP2302ARDZ"
			(at -3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2302_2303.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Nonsynchronous Step-Down Regulator 2 Amp Vout Adjustable SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADP2302ARDZ_0_1")
		(symbol "ADP2302ARDZ_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PGOOD")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PADGND")
				(number "9")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BST")
				(number "1")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP2360xCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ADP2360xCP"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-WD-8-1EP_3x3mm_P0.65mm_EP1.6x2.44mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2360.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "High Efficiency Buck Regulator, Vin 60V, Vout Adjustable, 50mA, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADP2360xCP_0_1")
		(symbol "ADP2360xCP_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ITH")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP5054"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 24.13 0)
		)
		(property "Value" "ADP5054"
			(at 22.86 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 33.02 -44.45 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP5054.pdf"
			(at -27.94 17.78 0)
		)
		(property "Description" "250kHz to 2MHz, 6A/6A/2A/2A Quad Buck Regulator, -40 to +125C, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "quad regulator dcdc buck synchronizable parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADP5054_0_0"
			(text "LDO"
				(at -12.7 19.05 0)
			)
			(text "Channel 1 Buck"
				(at -1.27 10.16 0)
			)
			(text "Channel 2 Buck"
				(at -1.27 -5.08 0)
			)
			(text "Channel 3 Buck"
				(at -1.27 -15.24 0)
			)
			(text "Channel 4 Buck"
				(at -1.27 -29.21 0)
			)
		)
		(symbol "ADP5054_0_1")
		(symbol "ADP5054_1_1"
			(pin power_out line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "VREG")
				(number "45")
			)
			(pin power_out line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "VDD")
				(number "43")
			)
			(pin passive line
				(at -27.94 12.7 0)
				(length 5.08)
				(hide yes)
				(name "PVIN1")
				(number "36")
			)
			(pin passive line
				(at -27.94 12.7 0)
				(length 5.08)
				(hide yes)
				(name "PVIN1")
				(number "37")
			)
			(pin power_in line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PVIN1")
				(number "38")
			)
			(pin unspecified line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "COMP1")
				(number "40")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "EN1")
				(number "39")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "CFG12")
				(number "18")
			)
			(pin passive line
				(at -27.94 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "PVIN2")
				(number "22")
			)
			(pin passive line
				(at -27.94 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "PVIN2")
				(number "23")
			)
			(pin power_in line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PVIN2")
				(number "24")
			)
			(pin unspecified line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "COMP2")
				(number "20")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "EN2")
				(number "21")
			)
			(pin power_in line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PVIN3")
				(number "6")
			)
			(pin unspecified line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "COMP3")
				(number "47")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "EN3")
				(number "48")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "CFG34")
				(number "13")
			)
			(pin power_in line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PVIN4")
				(number "7")
			)
			(pin unspecified line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "COMP4")
				(number "15")
			)
			(pin input line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "EN4")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 5.08)
				(name "PGND")
				(number "30")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "PGND3")
				(number "2")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 5.08)
				(name "PGND3")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 5.08)
				(name "PGND4")
				(number "10")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "PGND4")
				(number "11")
			)
			(pin power_in line
				(at 5.08 -48.26 90)
				(length 5.08)
				(name "EPAD")
				(number "49")
			)
			(pin unspecified line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "SYNC/MODE")
				(number "44")
			)
			(pin unspecified line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "RT")
				(number "42")
			)
			(pin input line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "FB1")
				(number "41")
			)
			(pin power_in line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "BST1")
				(number "32")
			)
			(pin passive line
				(at 27.94 7.62 180)
				(length 5.08)
				(hide yes)
				(name "SW1")
				(number "33")
			)
			(pin passive line
				(at 27.94 7.62 180)
				(length 5.08)
				(hide yes)
				(name "SW1")
				(number "34")
			)
			(pin power_out line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "SW1")
				(number "35")
			)
			(pin output line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "DL1")
				(number "31")
			)
			(pin output line
				(at 27.94 0 180)
				(length 5.08)
				(name "DL2")
				(number "29")
			)
			(pin passive line
				(at 27.94 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "SW2")
				(number "25")
			)
			(pin passive line
				(at 27.94 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "SW2")
				(number "26")
			)
			(pin power_out line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "SW2")
				(number "27")
			)
			(pin power_in line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "BST2")
				(number "28")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "FB2")
				(number "19")
			)
			(pin power_in line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "BST3")
				(number "1")
			)
			(pin power_out line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "SW3")
				(number "4")
			)
			(pin passive line
				(at 27.94 -15.24 180)
				(length 5.08)
				(hide yes)
				(name "SW3")
				(number "5")
			)
			(pin input line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "FB3")
				(number "46")
			)
			(pin power_in line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "BST4")
				(number "12")
			)
			(pin power_out line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "SW4")
				(number "8")
			)
			(pin passive line
				(at 27.94 -30.48 180)
				(length 5.08)
				(hide yes)
				(name "SW4")
				(number "9")
			)
			(pin input line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "FB4")
				(number "16")
			)
			(pin open_collector line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PWRGD")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP5070AREZ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "ADP5070AREZ"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_SO:ETSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3x4.2mm"
			(at 1.27 -25.4 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP5070.pdf"
			(at 1.27 -27.94 0)
		)
		(property "Description" "1A/0.6A DC-to-DC Switching Regulator with Independent Positive and Negative Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage regulator switching inverter double positive negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ETSSOP*1EP?4.4x6.5mm?P0.65mm?EP3x4.2mm*"
			(at 0 0 0)
		)
		(symbol "ADP5070AREZ_0_1")
		(symbol "ADP5070AREZ_1_1"
			(pin passive line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "COMP1")
				(number "8")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "EN1")
				(number "9")
			)
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PVIN1")
				(number "17")
			)
			(pin power_in line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PVIN2")
				(number "19")
			)
			(pin power_in line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PVINSYS")
				(number "18")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VREG")
				(number "16")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "COMP2")
				(number "12")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "11")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SS")
				(number "10")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SYNC/FREQ")
				(number "4")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SLEW")
				(number "6")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "SEQ")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "15")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "21")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "INBK")
				(number "3")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SW1")
				(number "2")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "FB1")
				(number "7")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VREF")
				(number "14")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "FB2")
				(number "13")
			)
			(pin power_out line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SW2")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM6000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "ADuM6000"
			(at 0 12.7 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM6000.PDF"
			(at -12.7 7.62 0)
		)
		(property "Description" "Isolated 5 kV DC-to-DC Converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "Isolated DC-to-DC Converter 5kV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM6000_0_1")
		(symbol "ADuM6000_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin no_connect line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "RC_IN")
				(number "4")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RC_OUT")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RC_SEL")
				(number "6")
			)
			(pin power_in line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VDD1")
				(number "7")
			)
			(pin power_in line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "V_ISO")
				(number "16")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GND_ISO")
				(number "15")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "NC")
				(number "14")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "V_SEL")
				(number "13")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "V_ISO")
				(number "10")
			)
			(pin power_out line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "GND_ISO")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AOZ1280CI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -6.35 0)
		)
		(property "Value" "AOZ1280CI"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "http://aosmd.com/res/data_sheets/AOZ1280CI.pdf"
			(at -6.35 -6.35 0)
		)
		(property "Description" "1.2 A Simple Buck Regulator, 3-26V input, 1.5Mhz"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AOZ1280CI_0_1")
		(symbol "AOZ1280CI_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BST")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "LX")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AOZ6663DI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "AOZ6663DI"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:AO_AOZ666xDI_DFN-8-1EP_3x3mm_P0.65mm_EP1.25x2.7mm"
			(at 33.02 -17.78 0)
		)
		(property "Datasheet" "http://aosmd.com/res/data_sheets/AOZ6663DI.pdf"
			(at 27.94 -20.32 0)
		)
		(property "Description" "3A Buck Regulator, 4.5-18V input, 750kHz, pulse energy mode on light load, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AOZ6663DI_0_0"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "BST")
				(number "8")
			)
		)
		(symbol "AOZ6663DI_0_1")
		(symbol "AOZ6663DI_1_0"
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
		)
		(symbol "AOZ6663DI_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "COMP")
				(number "4")
			)
			(pin power_out line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VCC_CAP")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "LX")
				(number "2")
			)
			(pin power_out line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP3211K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP3211K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 17.78 -7.62 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3211.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "1.5A, Adjustable Step-Down Voltage Regulator, 1.4MHz Frequency, Vin=4.5..18V, Vout=0.81..15V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down PWM buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP3211K_0_1")
		(symbol "AP3211K_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BS")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP3402"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP3402"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3402.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.0MHz 2A Step-Down DC-DC Buck Converter, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck switching converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "AP3402_0_1")
		(symbol "AP3402_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "PG")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LX")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP3441SHE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "AP3441SHE"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.7mm"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3441-L.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "3A step-Down DC-DC 1Mhz buck converter, Input 2.7 to 5.5V, Output: 0.6 to V_{IN} , DFN-8"
			(at 0 11.43 0)
		)
		(property "ki_keywords" "Diodes"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP?2x2mm?P0.5mm?EP0.9x1.7mm*"
			(at 0 0 0)
		)
		(symbol "AP3441SHE_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "SGND")
				(number "8")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "SGND")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LX")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP62150WU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP62150WU"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP62150.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "1.5A, 1.3MHz Buck DC/DC Converter, 4.2V-18V input voltage, 0.8V-7V adjustable output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.5A 1.3MHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?6*"
			(at 0 0 0)
		)
		(symbol "AP62150WU_0_1")
		(symbol "AP62150WU_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BST")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP62150Z6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP62150Z6"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP62150.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A, 1.3MHz Buck DC/DC Converter, adjustable output voltage, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.5A 1.3MHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
		(symbol "AP62150Z6_0_1")
		(symbol "AP62150Z6_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BST")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP62300WU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP62300WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP62300_AP62301_AP62300T.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A, 750kHz Buck DC/DC Converter, PFM for light load efficiency, 4.2V-18V input voltage, 0.8V-7V adjustable output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "AP62300WU_0_1")
		(symbol "AP62300WU_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BST")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP63200WU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP63200WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP63200-AP63201-AP63203-AP63205.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 500kHz Buck DC/DC Converter, adjustable output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "2A Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "AP63200WU_0_1")
		(symbol "AP63200WU_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BST")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP6502"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "AP6502"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 16.51 -13.97 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP6502.pdf"
			(at 0 3.81 0)
		)
		(property "Description" "340kHz 18V 2A Synchronous DC/DC Buck Converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck switching converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes_SO-8EP*"
			(at 0 0 0)
		)
		(symbol "AP6502_0_1")
		(symbol "AP6502_1_1"
			(pin power_in line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin tri_state line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin output line
				(at 7.62 10.16 180)
				(length 2.54)
				(name "BST")
				(number "1")
			)
			(pin power_out line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin output line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP65111AWU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP65111AWU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP65111A.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A, 500kHz Buck DC/DC Converter, adjustable output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.5A 500kHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "AP65111AWU_0_1")
		(symbol "AP65111AWU_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BST")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APE1707H-33-HF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707H-33-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://pdf.datasheet.live/datasheets-1/advanced_power_electronics/APE1707H-12-HF.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, fixed 3.3V output voltage, TO-252-5 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin3*"
			(at 0 0 0)
		)
		(symbol "APE1707H-33-HF_0_1")
		(symbol "APE1707H-33-HF_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APE1707M-33-HF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707M-33-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://files.remont-aud.net/baza/dc_dc/data/APE1707.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, fixed 3.3V output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "APE1707M-33-HF_0_1")
		(symbol "APE1707M-33-HF_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APE1707S-33-HF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707S-33-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://pdf.datasheet.live/datasheets-1/advanced_power_electronics/APE1707S-12-HF.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, fixed 3.3V output voltage, TO-263-5 (DD-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin3*"
			(at 0 0 0)
		)
		(symbol "APE1707S-33-HF_0_1")
		(symbol "APE1707S-33-HF_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD9001F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "BD9001F"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 6.35 -8.89 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/switching_regulator/bd9778f-e.pdf"
			(at 0 0 0)
		)
		(property "Description" "48V 2A, Flexible Step-Down Switching Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC-DC Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BD9001F_0_1")
		(symbol "BD9001F_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "INV")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD9778F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "BD9778F"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 6.35 -8.89 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/switching_regulator/bd9778f-e.pdf"
			(at 0 0 0)
		)
		(property "Description" "35V 2A, Flexible Step-Down Switching Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC-DC Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BD9778F_0_1")
		(symbol "BD9778F_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PVIN")
				(number "8")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "INV")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD9778HFP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "BD9778HFP"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Rohm_HRP7"
			(at 6.35 -8.89 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/switching_regulator/bd9778f-e.pdf"
			(at 0 0 0)
		)
		(property "Description" "35V 2A, Flexible Step-Down Switching Regulator, HRP7"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC-DC Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Rohm*HRP7*"
			(at 0 0 0)
		)
		(symbol "BD9778HFP_0_1")
		(symbol "BD9778HFP_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "INV")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD9781HFP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "BD9781HFP"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Rohm_HRP7"
			(at 10.16 -8.89 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/switching_regulator/bd9778f-e.pdf"
			(at 0 0 0)
		)
		(property "Description" "35V 4A, Flexible Step-Down Switching Regulator, HRP7"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC-DC Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Rohm*HRP7*"
			(at 0 0 0)
		)
		(symbol "BD9781HFP_0_1")
		(symbol "BD9781HFP_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "RT")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EN/SYNC")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "INV")
				(number "6")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD9G341EFJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "BD9G341EFJ"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm_ThermalVias"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Rohm%20PDFs/BD9G341EFJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V-76V input voltage range 3A output current, Buck Converter, Integrated FET, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*EP*3.9x4.9mm*P1.27mm*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "BD9G341EFJ_0_1")
		(symbol "BD9G341EFJ_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 0 12.7 270)
				(length 2.54)
				(name "BST")
				(number "7")
			)
			(pin input line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "RT")
				(number "5")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "LX")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VC")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CRE1S0505DC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CRE1S0505DC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_CRE1xxxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/datasheet?/data/power/ncl/kdc_cre1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "5V to 5V 200mA DC-DC Converter with 1kV isolation, DC-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*CRE1xxxxxxDC*"
			(at 0 0 0)
		)
		(symbol "CRE1S0505DC_0_1")
		(symbol "CRE1S0505DC_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "+VIN")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "-VIN")
				(number "1")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+VOUT")
				(number "5")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "-VOUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CRE1S0505S3C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CRE1S0505S3C"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_CRE1xxxxxx3C_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://power.murata.com/datasheet?/data/power/ncl/kdc_cre1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "5V to 5V 200mA, Isolated 2W Single-Output DC-DC Converter Modules with 3kV isolation, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*CRE1xxxxxx3C*"
			(at 0 0 0)
		)
		(symbol "CRE1S0505S3C_0_1")
		(symbol "CRE1S0505S3C_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "+VIN")
				(number "2")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "-VIN")
				(number "1")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+VOUT")
				(number "4")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "-VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CRE1S0505SC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CRE1S0505SC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_CRE1xxxxxxSC_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://power.murata.com/datasheet?/data/power/ncl/kdc_cre1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "5V to 5V 200mA DC-DC Converter with 1kV isolation, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*CRE1xxxxxxSC*"
			(at 0 0 0)
		)
		(symbol "CRE1S0505SC_0_1")
		(symbol "CRE1S0505SC_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "+VIN")
				(number "2")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "-VIN")
				(number "1")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+VOUT")
				(number "4")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "-VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIO6970"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "DIO6970"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "http://www.dioo.com/uploads/product/20190313/7a4d03690a9be004035eb1035a429f24.pdf"
			(at 12.7 0 0)
		)
		(property "Description" "High-Efficiency 2A, 24V Input Synchronous Step Down Converter, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps buck boost inverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "DIO6970_0_1")
		(symbol "DIO6970_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BS")
				(number "6")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FSBH0170"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FSBH0170"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSBH0270-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Green Mode Fairchild Power Switch, 700V Vds, 1.0A Id, 15W/13W 230V/85-265V, VIN Pin, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "FSBH0170_0_1")
		(symbol "FSBH0170_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "HV")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DRAIN")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "DRAIN")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "DRAIN")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FSBH0F70A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FSBH0F70A"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSBH0270-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Green Mode Fairchild Power Switch, 700V Vds, 0.5A Id, 10W/8W 230V/85-265V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "FSBH0F70A_0_1")
		(symbol "FSBH0F70A_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "HV")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DRAIN")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "DRAIN")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "DRAIN")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FSDH321"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 6.35 0)
		)
		(property "Value" "FSDH321"
			(at 10.16 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 10.16 1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSDH321JP-D.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "17W SMPS Controller, 100kHz, AC-DC, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET 17W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "FSDH321_0_0"
			(text "CTRL"
				(at 0 0 0)
			)
		)
		(symbol "FSDH321_0_1")
		(symbol "FSDH321_1_1"
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "IPK")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "VSTR")
				(number "5")
			)
			(pin input line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FSDH321L"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 6.35 0)
		)
		(property "Value" "FSDH321L"
			(at 10.16 3.81 0)
		)
		(property "Footprint" "Package_DIP:Fairchild_LSOP-8"
			(at 10.16 1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSDH321JP-D.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "17W SMPS Controller, 100kHz, AC-DC, SMD-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET 17W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*LSOP*"
			(at 0 0 0)
		)
		(symbol "FSDH321L_0_0"
			(text "CTRL"
				(at 0 0 0)
			)
		)
		(symbol "FSDH321L_0_1")
		(symbol "FSDH321L_1_1"
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "IPK")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "VSTR")
				(number "5")
			)
			(pin input line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FSL136MRT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "FSL136MRT"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:Fairchild_TO-220F-6L"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSL136MRT-D.pdf"
			(at 1.905 0 0)
		)
		(property "Description" "67kHz SMPS Controller w/ Soft Start, max. 50W AC-DC, TO-220F-6L"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller 50W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*TO*220F*6L*"
			(at 0 0 0)
		)
		(symbol "FSL136MRT_0_0"
			(text "CTRL"
				(at 0.127 0 0)
			)
		)
		(symbol "FSL136MRT_0_1")
		(symbol "FSL136MRT_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "VST")
				(number "6")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FSQ0565RSWDTU"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "FSQ0565RSWDTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:Fairchild_TO-220F-6L"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FSQ0565RS-D.PDF"
			(at 1.905 0 0)
		)
		(property "Description" "67kHz Quasi Resonant SMPS Controller w/ Soft Start, max. 80W AC-DC, TO-220F-6L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quasi Resonant SMPS Controller 80W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*TO*220F*6L*"
			(at 0 0 0)
		)
		(symbol "FSQ0565RSWDTU_0_0"
			(text "CTRL"
				(at 0.762 0 0)
			)
		)
		(symbol "FSQ0565RSWDTU_0_1")
		(symbol "FSQ0565RSWDTU_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "SYNC")
				(number "5")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "VST")
				(number "6")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GL2576-3.3SF8DR"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-3.3SF8DR"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "3.3V 3A, 52KHz Step Down Converter, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "GL2576-3.3SF8DR_0_1")
		(symbol "GL2576-3.3SF8DR_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HT7463A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "HT7463A"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://www.holtek.com/documents/10179/116711/HT7463A_Bv160.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA High-Efficiency Step-Down DC-DC Converter, 4.5-52V input voltage, adjustable output voltage, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck regulator "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
		(symbol "HT7463A_0_1")
		(symbol "HT7463A_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CB")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL8117FRZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ISL8117FRZ"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://www.intersil.com/content/dam/Intersil/documents/isl8/isl8117.pdf"
			(at -12.7 13.97 0)
		)
		(property "Description" "Synchronous step-down PWM controller, 4.5v to 60v input, 0.6v to 54v Output Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM step down buck converter controller synchronous POL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ISL8117FRZ_0_1")
		(symbol "ISL8117FRZ_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EN")
				(number "16")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "MOD/SYNC")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PGOOD")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CLKOUT")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SS/TRK")
				(number "5")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "4")
			)
			(pin input line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "EXTBIAS")
				(number "15")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC5V")
				(number "9")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "SGND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VIN")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "7")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "BOOT")
				(number "13")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "UGATE")
				(number "12")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PHASE")
				(number "11")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "ISEN")
				(number "10")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "LGATE/OCS")
				(number "8")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL8117FVEZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ISL8117FVEZ"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://www.intersil.com/content/dam/Intersil/documents/isl8/isl8117.pdf"
			(at -12.7 13.97 0)
		)
		(property "Description" "Synchronous step-down PWM controller, 4.5v to 60v input, 0.6v to 54v Output Voltage, HTSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM step down buck converter controller synchronous POL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ISL8117FVEZ_0_1")
		(symbol "ISL8117FVEZ_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "MOD/SYNC")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PGOOD")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CLKOUT")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SS/TRK")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin input line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "EXTBIAS")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC5V")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "SGND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VIN")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "9")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "BOOT")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "UGATE")
				(number "14")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PHASE")
				(number "13")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "ISEN")
				(number "12")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "LGATE/OCS")
				(number "10")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KA5H02659RN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5H02659RN"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "100kHz SMPS Controller, AC-DC, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "KA5H02659RN_0_0"
			(text "CTRL"
				(at 0.127 0 0)
			)
		)
		(symbol "KA5H02659RN_0_1")
		(symbol "KA5H02659RN_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KA5H0265RCTU"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5H0265RCTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:ONSemi_TO-220-5L"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "100kHz SMPS Controller w/ Soft Start, AC-DC, TO-220F-5L"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*5L*"
			(at 0 0 0)
		)
		(symbol "KA5H0265RCTU_0_0"
			(text "CTRL"
				(at 0.127 0 0)
			)
		)
		(symbol "KA5H0265RCTU_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "SS")
				(number "5")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KA5H0265RCYDTU"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5H0265RCYDTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:ONSemi_TO-220-5L_Forming"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "KA5H0265RCTU, 100kHz SMPS Controller w/ Soft Start, AC-DC, TO-220F-5L(Forming)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*5L*"
			(at 0 0 0)
		)
		(symbol "KA5H0265RCYDTU_0_0"
			(text "CTRL"
				(at 0.127 0 0)
			)
		)
		(symbol "KA5H0265RCYDTU_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "SS")
				(number "5")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KA5M0265RTU"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5M0265RTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-4_Vertical"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "67kHz SMPS Controller, AC-DC, TO-220F-4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*4*"
			(at 0 0 0)
		)
		(symbol "KA5M0265RTU_0_0"
			(text "CTRL"
				(at 0.127 0 0)
			)
		)
		(symbol "KA5M0265RTU_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KA5M0265RYDTU"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5M0265RYDTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:ONSemi_TO-220F-4L_Forming"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "67kHz SMPS Controller, AC-DC, TO-220F-4L(Forming)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*4*"
			(at 0 0 0)
		)
		(symbol "KA5M0265RYDTU_0_0"
			(text "CTRL"
				(at 0.127 0 0)
			)
		)
		(symbol "KA5M0265RYDTU_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin power_in line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L4962-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.224 11.684 0)
		)
		(property "Value" "L4962-A"
			(at 10.16 11.684 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/389/cd00000076-1795191.pdf"
			(at -0.508 -24.384 0)
		)
		(property "Description" "1.5A Power Switching Regulator, 9..46V input, 5.1..40V output, 150 kHz, DIP-16"
			(at 0 -22.352 0)
		)
		(property "ki_keywords" "buck step-down dc-dc converter PowerDIP L4962/A Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.*"
			(at 0 0 0)
		)
		(symbol "L4962-A_0_0")
		(symbol "L4962-A_1_0"
			(pin power_in line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "INPUT")
				(number "7")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "FREQ_COMP")
				(number "11")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "OSCILLATOR")
				(number "14")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "SOFT_START")
				(number "15")
			)
			(pin no_connect line
				(at -15.24 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -15.24 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 15.24 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 15.24 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 15.24 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "OUTPUT")
				(number "2")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "FEEDBACK")
				(number "10")
			)
		)
		(symbol "L4962-A_1_1"
			(pin no_connect line
				(at 15.24 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L4962E-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.224 11.684 0)
		)
		(property "Value" "L4962E-A"
			(at 9.652 11.684 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-7_P2.54x5.08mm_StaggerOdd_Lead3.08mm_Vertical"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/389/cd00000076-1795191.pdf"
			(at -0.508 -24.384 0)
		)
		(property "Description" "1.5A Power Switching Regulator, 9..46V input, 5.1..40V output, 150 kHz, TO-220-7 (Heptawatt V)"
			(at 0 -22.352 0)
		)
		(property "ki_keywords" "buck step-down dc-dc converter L4962E/A Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*P2.54x5.08*StaggerOdd*Lead3.08*Vertical*"
			(at 0 0 0)
		)
		(symbol "L4962E-A_0_0")
		(symbol "L4962E-A_1_0"
			(pin power_in line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "INPUT")
				(number "1")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "FREQ_COMP")
				(number "3")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "OSCILLATOR")
				(number "5")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "SOFT_START")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "OUTPUT")
				(number "7")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "FEEDBACK")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L5973D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "L5973D"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/l5973d.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A step down switching regulator, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step down buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HSOP*EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "L5973D_0_1")
		(symbol "L5973D_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INH")
				(number "3")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L7980A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "L7980A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.3x2.3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/l7980.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "2A step down switching regulator, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step down buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HSOP*EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "L7980A_0_1")
		(symbol "L7980A_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FSW")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "COMP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD7575"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LD7575"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.leadtrend.com.tw/archive/doc/product/sheets/LD7575-DS-04b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Green-Mode PWM Controller with High-Voltage Start-Up Circuit, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LD7575_0_1")
		(symbol "LD7575_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "1")
			)
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "HV")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LGS5116B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LGS5116B"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 20.32 -12.7 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2305121704_Legend-Si-LGS5116B_C5818961.pdf"
			(at 45.72 -15.24 0)
		)
		(property "Description" "2A, 500kHz Buck DC/DC Converter, adjustable output voltage, 4.5-18V input, 0.6-12V output, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "2A Buck DC/DC Legend"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LGS5116B_0_1")
		(symbol "LGS5116B_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BST")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LGS6302B5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LGS6302B5"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2304071430_Legend-Si-LGS6302_C5123975.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A, 1.2MHz Boost DC/DC Converter, adjustable 3-60V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LGS6302B5_0_1")
		(symbol "LGS6302B5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM22676MR-ADJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LM22676MR-ADJ"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm22676.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "3A Step-Down Switching Voltage Regulater, 4.5-42V Input, Adjustable Output, 500kHz Switching Frequency, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Converter 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*"
			(at 0 0 0)
		)
		(symbol "LM22676MR-ADJ_0_1")
		(symbol "LM22676MR-ADJ_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM22678TJ-ADJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM22678TJ-ADJ"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm22678.pdf"
			(at 1.27 -2.54 0)
		)
		(property "Description" "5A Step-Down Switching Voltage Regulater, 4.5-42V Input, Adjustable Output, 500kHz Switching Frequency, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Converter 5A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "LM22678TJ-ADJ_0_1")
		(symbol "LM22678TJ-ADJ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BOOT")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM25085MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM25085MM"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm25085.pdf"
			(at 0 0 0)
		)
		(property "Description" "42V Constant On-Time PFET Buck Switching Controller, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck switching controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM25085MM_0_1")
		(symbol "LM25085MM_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "PGATE")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ISEN")
				(number "5")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM25085MY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM25085MY"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm25085.pdf"
			(at 0 0 0)
		)
		(property "Description" "42V Constant On-Time PFET Buck Switching Controller, MSOP-8-EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck switching controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM25085MY_0_1")
		(symbol "LM25085MY_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "2")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "PGATE")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ISEN")
				(number "5")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM25085SD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM25085SD"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x3mm_P0.5mm_EP1.6x2.0mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm25085.pdf"
			(at 0 0 0)
		)
		(property "Description" "42V Constant On-Time PFET Buck Switching Controller, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck switching controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.5mm*EP1.6x2.0mm*"
			(at 0 0 0)
		)
		(symbol "LM25085SD_0_1")
		(symbol "LM25085SD_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "2")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "PGATE")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ISEN")
				(number "5")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2574HVM-12"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVM-12"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 0.5A Step-Down Voltage Regulator, High Voltage Input, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM2574HVM-12_0_1")
		(symbol "LM2574HVM-12_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "SGND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "PGND")
				(number "6")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2574HVN-12"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVN-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 0.5A Step-Down Voltage Regulator, High Voltage Input, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM2574HVN-12_0_1")
		(symbol "LM2574HVN-12_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "SGND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2576HVS-12"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVS-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 3A High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "LM2576HVS-12_0_1")
		(symbol "LM2576HVS-12_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2576HVT-12"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVT-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 3A High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LM2576HVT-12_0_1")
		(symbol "LM2576HVT-12_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2594M-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594M-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3.3V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 45V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "LM2594M-3.3_0_1")
		(symbol "LM2594M-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2594N-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594N-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3.3V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 45V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM2594N-3.3_0_1")
		(symbol "LM2594N-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2595S-12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2595S-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/lm2595.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 1A Step-Down Voltage Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "LM2595S-12_0_1")
		(symbol "LM2595S-12_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2595T-12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2595T-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/lm2595.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 1A Step-Down Voltage Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LM2595T-12_0_1")
		(symbol "LM2595T-12_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2596S-12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2596S-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2596.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 3A Step-Down Voltage Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "LM2596S-12_0_1")
		(symbol "LM2596S-12_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2596T-12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2596T-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2596.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 3A 150kHz Step-Down Voltage Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LM2596T-12_0_1")
		(symbol "LM2596T-12_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ON}/OFF")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2611xMF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2611xMF"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm2611.pdf"
			(at -46.99 31.75 0)
		)
		(property "Description" "1.4MHz Cuk Converter, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "switched converter inverter PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM2611xMF_0_1")
		(symbol "LM2611xMF_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "NFB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM26480SQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "LM26480SQ"
			(at 15.24 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm26480.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual 1.5A 2MHz Buck Regulators and Dual 300mA LDOs, WQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Buck Regulator LDO 2MHz 1.5A 300mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM26480SQ_0_1")
		(symbol "LM26480SQ_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SYNC")
				(number "2")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "ENSW1")
				(number "7")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "ENSW2")
				(number "12")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "ENLDO1")
				(number "17")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "ENLDO2")
				(number "16")
			)
			(pin power_in line
				(at -7.62 22.86 270)
				(length 2.54)
				(name "VIN1")
				(number "6")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VIN2")
				(number "13")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "GND_SW1")
				(number "4")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VINLDO1")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "GND_SW2")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VINLDO2")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND_L")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "GND_C")
				(number "9")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VINLDO12")
				(number "1")
			)
			(pin passive line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin power_in line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "10")
			)
			(pin open_collector line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "~{POR}")
				(number "3")
			)
			(pin power_out line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "SW1")
				(number "5")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "FB1")
				(number "8")
			)
			(pin power_out line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "SW2")
				(number "14")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "FB2")
				(number "11")
			)
			(pin power_out line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "LDO1")
				(number "20")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "FBL1")
				(number "21")
			)
			(pin power_out line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "LDO2")
				(number "23")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "FBL2")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2672M-12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2672M-12"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2672.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 1A Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM2672M-12_0_1")
		(symbol "LM2672M-12_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SS")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "CB")
				(number "1")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VSW")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2672N-12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2672N-12"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2672.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 1A Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM2672N-12_0_1")
		(symbol "LM2672N-12_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SS")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "CB")
				(number "1")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VSW")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2674M-12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2674M-12"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2674.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 500mA Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM2674M-12_0_1")
		(symbol "LM2674M-12_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "CB")
				(number "1")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VSW")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2674N-12"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2674N-12"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2674.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 500mA Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM2674N-12_0_1")
		(symbol "LM2674N-12_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "CB")
				(number "1")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VSW")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2734Y"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2734Y"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2734.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "1A Step-Down DC-DC Regulator, Adjustable Output Voltage, 550kHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LM2734Y_0_1"
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BOOST")
				(number "1")
			)
		)
		(symbol "LM2734Y_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM3150MH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "LM3150MH"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-14-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3.1mm"
			(at 2.54 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3150.pdf"
			(at 50.8 -11.43 0)
		)
		(property "Description" "42V Wide Vin synchronous Buck controller, HTSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck step-down converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x5mm*P0.65*"
			(at 0 0 0)
		)
		(symbol "LM3150MH_0_1")
		(symbol "LM3150MH_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "RON")
				(number "7")
			)
			(pin power_out line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SS")
				(number "6")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "SGND")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "SGND")
				(number "5")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "SGND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "14")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "HG")
				(number "11")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "BST")
				(number "12")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SW")
				(number "10")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "ILIM")
				(number "8")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "LG")
				(number "13")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM3407MY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM3407MY"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm_ThermalVias"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3407.pdf"
			(at 0 0 0)
		)
		(property "Description" "LED Lighting CC Floating Buck Switching Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM3407MY_0_1")
		(symbol "LM3407MY_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DIM")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "FS")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GNDPAD")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LX")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "ISNS")
				(number "1")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM3578"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM3578"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3578a.pdf"
			(at -1.27 -1.27 0)
		)
		(property "Description" "750mA, Switching Regulator, adjustable output voltage, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "LM3578_0_1")
		(symbol "LM3578_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "E-")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "E+")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CAP")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ILIM")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin open_emitter line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "E")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5001MA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LM5001MA"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5001.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "1A, High Voltage (75V) Switch-Mode Regulator, Adjustable Output Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Voltage Switch-mode Regulator Flyback SEPIC Boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM5001MA_0_1")
		(symbol "LM5001MA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "COMP")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5006MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "LM5006MM"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5006.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA, 80V Constant On-Time Buck Switching Regulator, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Constant On-Time Buck Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM5006MM_0_1")
		(symbol "LM5006MM_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RT/SD")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "UV")
				(number "5")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "UVO")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "RTN")
				(number "4")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BST")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LG")
				(number "3")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5007MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5007MM"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5007.pdf"
			(at 0 0 0)
		)
		(property "Description" "700mA, High Voltage (80V) Step-Down Switching Regulator, Adjustable Output Voltage, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM5007MM_0_1")
		(symbol "LM5007MM_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RON/SD")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RCL")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "RTN")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BST")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5007SD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5007SD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.6x3mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5007.pdf"
			(at 0 0 0)
		)
		(property "Description" "700mA, High Voltage (80V) Step-Down Switching Regulator, Adjustable Output Voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LM5007SD_0_1")
		(symbol "LM5007SD_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RON/SD")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RCL")
				(number "3")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "RTN")
				(number "4")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BST")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5017MR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5017MR"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.71x3.4mm_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5017.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA, 100V Step-Down Switching Regulator, PowerSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM5017MR_0_1")
		(symbol "LM5017MR_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RON")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ULVO")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "RTN")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "RTNPAD")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BST")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5017SD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5017SD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP1.98x3mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5017.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA, 100V Step-Down Switching Regulator, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LM5017SD_0_1")
		(symbol "LM5017SD_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RON")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ULVO")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "RTN")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "RTNPAD")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BST")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5022MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM5022MM"
			(at -2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5022.pdf"
			(at 0 0 0)
		)
		(property "Description" "60-V Low-Side Controller for Boost and SEPIC, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost switching controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM5022MM_0_1")
		(symbol "LM5022MM_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "UVLO")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "9")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SS")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "CS")
				(number "8")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "COMP")
				(number "3")
			)
			(pin power_out line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5088-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "LM5088-1"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3mm_ThermalVias"
			(at 45.72 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5088.pdf"
			(at 57.15 -19.05 0)
		)
		(property "Description" "Wide Input Range Non-Synchronous Buck Controller, Frequency Dithering, 75V, HTSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step down buck high voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM5088-1_0_1")
		(symbol "LM5088-1_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DITH")
				(number "10")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RAMP")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SS")
				(number "3")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RT/SYNC")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "PGND")
				(number "17")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "HG")
				(number "14")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BOOT")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SW")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "CS")
				(number "12")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CSG")
				(number "11")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT")
				(number "9")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "COMP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5088-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "LM5088-2"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3mm_ThermalVias"
			(at 45.72 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5088.pdf"
			(at 57.15 -19.05 0)
		)
		(property "Description" "Wide Input Range Non-Synchronous Buck Controller, Hiccup Mode Restart, 75V, HTSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step down buck high voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM5088-2_0_1")
		(symbol "LM5088-2_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RES")
				(number "10")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RAMP")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SS")
				(number "3")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RT/SYNC")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "PGND")
				(number "17")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "HG")
				(number "14")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BOOT")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SW")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "CS")
				(number "12")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CSG")
				(number "11")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT")
				(number "9")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "COMP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5118MH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "LM5118MH"
			(at -12.7 16.51 0)
		)
		(property "Footprint" "Package_SO:Texas_PWP0020A"
			(at 17.78 16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5118.pdf"
			(at 50.8 -11.43 0)
		)
		(property "Description" "Wide Voltage Range Buck-Boost Controller, HTSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck Boost step-up step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PWP0020A*"
			(at 0 0 0)
		)
		(symbol "LM5118MH_0_1")
		(symbol "LM5118MH_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "UVLO")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "11")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SS")
				(number "7")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "RAMP")
				(number "5")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RT")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "14")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "HO")
				(number "19")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "HB")
				(number "18")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "HS")
				(number "20")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LO")
				(number "15")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CS")
				(number "12")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "CSG")
				(number "13")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "10")
			)
			(pin power_in line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VCCX")
				(number "17")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "COMP")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5161PWP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM5161PWP"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-14-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3.1mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5161.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "1A Synchronous Buck/Fly-buck Converter, 4.5V-100V input, adjustable output voltage, HTSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x5*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM5161PWP_0_1")
		(symbol "LM5161PWP_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RON")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "4")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SS")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "1")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "15")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "2")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "BST")
				(number "11")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "12")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "13")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "9")
			)
			(pin power_out line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FPWM")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5164DDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "LM5164DDA"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5164.pdf?ts=1598311864250&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FLM5164%253FHQS%253DTI-null-null-octopart-df-pf-null-wwe"
			(at -7.62 8.89 0)
		)
		(property "Description" "1A synchronous buck converter with ultra-low IQ, 6V - 100V input, adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HSOP*1EP*3.9x4.9*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM5164DDA_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RON")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "BST")
				(number "7")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PGOOD")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5165"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM5165"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5165.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "150mA Synchronous Buck Converter With Ultra-Low IQ, 3V-65V input, adjustable output voltage, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PVSON*N10*"
			(at 0 0 0)
		)
		(symbol "LM5165_0_1")
		(symbol "LM5165_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "PGOOD")
				(number "6")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "HYS")
				(number "9")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "RT")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "11")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ILIM")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5165X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM5165X"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5165.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "150mA Synchronous Buck Converter With Ultra-Low IQ, 3V-65V input, 5.0V fixed output voltage, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator fixed 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PVSON*N10*"
			(at 0 0 0)
		)
		(symbol "LM5165X_0_1")
		(symbol "LM5165X_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "PGOOD")
				(number "6")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "HYS")
				(number "9")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "RT")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ILIM")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5175PWP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "LM5175PWP"
			(at -12.7 21.59 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_ThermalVias"
			(at 17.78 21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5175.pdf"
			(at 50.8 -11.43 0)
		)
		(property "Description" "42-V wide Vin synchronous 4-switch Buck-Boost controller, HTSSOP-28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck Boost step-up step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x9.7mm*P0.65*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "LM5175PWP_0_1")
		(symbol "LM5175PWP_1_1"
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "EN/UVLO")
				(number "1")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "SS")
				(number "8")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "COMP")
				(number "9")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "MODE")
				(number "4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "RT/SYNC")
				(number "6")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 5.08)
				(name "DITH")
				(number "5")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "SLOPE")
				(number "7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "CS")
				(number "16")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "CSG")
				(number "15")
			)
			(pin power_in line
				(at -7.62 -25.4 90)
				(length 5.08)
				(name "AGND")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -25.4 90)
				(length 5.08)
				(name "PGND")
				(number "22")
			)
			(pin input line
				(at -2.54 -25.4 90)
				(length 5.08)
				(name "PowerPAD")
				(number "29")
			)
			(pin input line
				(at 2.54 25.4 270)
				(length 5.08)
				(name "VISNS")
				(number "3")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 5.08)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "VCC")
				(number "23")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "BIAS")
				(number "24")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "VOSNS")
				(number "12")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "HDRV1")
				(number "27")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "BOOT1")
				(number "26")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "SW1")
				(number "28")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "LDRV1")
				(number "25")
			)
			(pin input line
				(at 17.78 0 180)
				(length 5.08)
				(name "FB")
				(number "11")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "PGOOD")
				(number "17")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "HDRV2")
				(number "19")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "BOOT2")
				(number "20")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "SW2")
				(number "18")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "LDRV2")
				(number "21")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "ISNS(-)")
				(number "13")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "ISNS(+)")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5175RHF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "LM5175RHF"
			(at -12.7 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-28-1EP_4x5mm_P0.5mm_EP2.55x3.55mm"
			(at 17.78 21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5175.pdf"
			(at 50.8 -11.43 0)
		)
		(property "Description" "42-V wide Vin synchronous 4-switch Buck-Boost controller, QFN-28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck Boost step-up step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*4x5mm*P0.5*"
			(at 0 0 0)
		)
		(symbol "LM5175RHF_0_1")
		(symbol "LM5175RHF_1_1"
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "EN/UVLO")
				(number "26")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "SS")
				(number "5")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "COMP")
				(number "6")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "MODE")
				(number "1")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "RT/SYNC")
				(number "3")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 5.08)
				(name "DITH")
				(number "2")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "SLOPE")
				(number "4")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "CS")
				(number "13")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "CSG")
				(number "12")
			)
			(pin power_in line
				(at -7.62 -25.4 90)
				(length 5.08)
				(name "AGND")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -25.4 90)
				(length 5.08)
				(name "PGND")
				(number "19")
			)
			(pin input line
				(at -2.54 -25.4 90)
				(length 5.08)
				(name "PowerPAD")
				(number "29")
			)
			(pin input line
				(at 2.54 25.4 270)
				(length 5.08)
				(name "VISNS")
				(number "28")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 5.08)
				(name "VIN")
				(number "27")
			)
			(pin power_in line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "BIAS")
				(number "21")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "VOSNS")
				(number "9")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "HDRV1")
				(number "24")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "BOOT1")
				(number "23")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "SW1")
				(number "25")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "LDRV1")
				(number "22")
			)
			(pin input line
				(at 17.78 0 180)
				(length 5.08)
				(name "FB")
				(number "8")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "PGOOD")
				(number "14")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "HDRV2")
				(number "16")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "BOOT2")
				(number "17")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "SW2")
				(number "15")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "LDRV2")
				(number "18")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "ISNS(-)")
				(number "10")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "ISNS(+)")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMR10510XMF"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LMR10510XMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr10510.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1A, 5.5V Step-Down Voltage Regulator, 1.6MHz Frequency, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LMR10510XMF_0_1")
		(symbol "LMR10510XMF_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMR10510YSD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LMR10510YSD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr10510.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A, 5.5V Step-Down Voltage Regulator, 3MHz Frequency, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "LMR10510YSD_0_1")
		(symbol "LMR10510YSD_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VINA")
				(number "5")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIND")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMR16006YQ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "LMR16006YQ"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr16006y-q1.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "Simple Switcher Buck Regulator, Vin=4-40V, Iout=600mA, Adjustable output voltage, SOT-23-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LMR16006YQ_0_1")
		(symbol "LMR16006YQ_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CB")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMR33640ADDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33640ADDA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33640.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=4A, F=400kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
		(symbol "LMR33640ADDA_0_1")
		(symbol "LMR33640ADDA_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_out line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMR36510ADDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR36510ADDA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr36510.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=4.2-65V, Iout=1A, F=400kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous buck step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HTSOP*1EP*3.9x4.9mm*P1.27mm*EP2.95x4.9mm*Mask2.4x3.1mm*"
			(at 0 0 0)
		)
		(symbol "LMR36510ADDA_0_1")
		(symbol "LMR36510ADDA_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_out line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMR50410"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "LMR50410"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr50410.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "Simple Switcher Buck Regulator, Vin=4-36V, Iout=1A, Adjustable output voltage, SOT-23-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LMR50410_0_1")
		(symbol "LMR50410_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CB")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMR51430"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LMR51430"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmr51430.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "4.5-V to 36-V, 3-A synchronous buck converter with 40-µA IQ, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LMR51430_0_1")
		(symbol "LMR51430_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CB")
				(number "6")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMR62421XSD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LMR62421XSD"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 3.81 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr62421.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.1A, 24Vout Step-Up Voltage Regulator, 1.6MHz Frequency, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost SEPIC Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "LMR62421XSD_0_1")
		(symbol "LMR62421XSD_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "AGND")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMZ13608"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LMZ13608"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_NDY0011A"
			(at -24.13 22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/snvs710i/snvs710i.pdf"
			(at -24.13 22.86 0)
		)
		(property "Description" "8A Adjustable Step-Down DC/DC Power Module in 15x15mm, Texas NDY0011A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*NDY0011A*"
			(at 0 0 0)
		)
		(symbol "LMZ13608_0_1")
		(symbol "LMZ13608_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "AGND")
				(number "5")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "PGND")
				(number "12")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "10")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "11")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMZ23605TZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZ23605TZ"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_NDW-7_TabPin4"
			(at 20.955 -10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/lmz23605"
			(at 0 -17.78 0)
		)
		(property "Description" "5A Adjustable Step-Down DC/DC Power Module, Vin: 6-36V"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*NDW*"
			(at 0 0 0)
		)
		(symbol "LMZ23605TZ_0_1")
		(symbol "LMZ23605TZ_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SS/TRK")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "7")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMZM23601"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZM23601"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_LGA:Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm_ThermalVias"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmzm23601.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "1A Adjustable Step-Down DC/DC Power Module in 3.8x3mm, MicroSIP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*SIL*1EP*3.8x3mm*P0.6mm*"
			(at 0 0 0)
		)
		(symbol "LMZM23601_0_1")
		(symbol "LMZM23601_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "MODE/SYNC")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK302D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK302D"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 80mA Output Current, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8B*"
			(at 0 0 0)
		)
		(symbol "LNK302D_0_1")
		(symbol "LNK302D_1_1"
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin input line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "BP")
				(number "1")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK302G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK302G"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 80mA Output Current, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
		(symbol "LNK302G_0_1")
		(symbol "LNK302G_1_1"
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "BP")
				(number "3")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK302P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK302P"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 80mA Output Current, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
		(symbol "LNK302P_0_1")
		(symbol "LNK302P_1_1"
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "BP")
				(number "3")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK3202D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3202D"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN2 Family, 80mA Output Current, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
		(symbol "LNK3202D_0_1")
		(symbol "LNK3202D_1_1"
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin input line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "BP/M")
				(number "1")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK3202G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3202G"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN2 Family, 80mA Output Current, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
		(symbol "LNK3202G_0_1")
		(symbol "LNK3202G_1_1"
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin input line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "BP/M")
				(number "1")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK3202P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3202P"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN2 Family, 80mA Output Current, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
		(symbol "LNK3202P_0_1")
		(symbol "LNK3202P_1_1"
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin input line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "BP/M")
				(number "1")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK362D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK362D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk362-364.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-XT Family, 2.6W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Effi cient, Low Power Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
		(symbol "LNK362D_0_1")
		(symbol "LNK362D_1_1"
			(pin open_collector line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK362G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK362G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk362-364.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-XT Family, 2.6W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Effi cient, Low Power Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
		(symbol "LNK362G_0_1")
		(symbol "LNK362G_1_1"
			(pin open_collector line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK362P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK362P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk362-364.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-XT Family, 2.6W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Effi cient, Low Power Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
		(symbol "LNK362P_0_1")
		(symbol "LNK362P_1_1"
			(pin open_collector line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK403EG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK403EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 12W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
		(symbol "LNK403EG_0_1")
		(symbol "LNK403EG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "R")
				(number "1")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "2")
			)
			(pin input line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK403LG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK403LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 12W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
		(symbol "LNK403LG_0_1")
		(symbol "LNK403LG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "R")
				(number "1")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "2")
			)
			(pin input line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK454D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK454D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PL Family, 3W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Constant Current Control for Non-Isolated Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
		(symbol "LNK454D_0_1")
		(symbol "LNK454D_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BP")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK457K"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK457K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PL Family, 8W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Constant Current Control for Non-Isolated Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
		(symbol "LNK457K_0_1")
		(symbol "LNK457K_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "13")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "9")
			)
			(pin no_connect line
				(at -2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK457V"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK457V"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PL Family, 8W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Constant Current Control for Non-Isolated Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12B*"
			(at 0 0 0)
		)
		(symbol "LNK457V_0_1")
		(symbol "LNK457V_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "12")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "9")
			)
			(pin no_connect line
				(at -2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK562D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK562D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linklp_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-LP Family, 1.9W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Efficient Off-Line Switcher IC for Linear Transformer Replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
		(symbol "LNK562D_0_1")
		(symbol "LNK562D_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK562G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK562G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linklp_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-LP Family, 1.9W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Efficient Off-Line Switcher IC for Linear Transformer Replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
		(symbol "LNK562G_0_1")
		(symbol "LNK562G_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK562P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK562P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linklp_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-LP Family, 1.9W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Efficient Off-Line Switcher IC for Linear Transformer Replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
		(symbol "LNK562P_0_1")
		(symbol "LNK562P_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK603DG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK603DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 3.3W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
		(symbol "LNK603DG_0_1")
		(symbol "LNK603DG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP/M")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK603PG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK603PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 3.3W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
		(symbol "LNK603PG_0_1")
		(symbol "LNK603PG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP/M")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK606GG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK606GG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 6.1W Output Power, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
		(symbol "LNK606GG_0_1")
		(symbol "LNK606GG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP/M")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK623DG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK623DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkcv_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-CV Family, 6W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-line Switcher with Accurate Primary-side Constant-Voltage Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
		(symbol "LNK623DG_0_1")
		(symbol "LNK623DG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK623PG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK623PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkcv_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-CV Family, 6W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-line Switcher with Accurate Primary-side Constant-Voltage Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
		(symbol "LNK623PG_0_1")
		(symbol "LNK623PG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LNK632DG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK632DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_632DG_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 3.1W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV Switcher With CC Control for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
		(symbol "LNK632DG_0_1")
		(symbol "LNK632DG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP/M")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1073CN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1073CN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1073fa.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC/DC Converter Adjustable Output Voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1073CN_0_1")
		(symbol "LT1073CN_1_1"
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "A0")
				(number "6")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "Ilim")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at 0 -10.16 90)
				(length 2.54)
				(name "SW2")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW1")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SET")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1073CN-5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1073CN-5"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1073fa.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC/DC Converter, Fixed 5V Output Voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1073CN-5_0_1")
		(symbol "LT1073CN-5_1_1"
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "A0")
				(number "6")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "Ilim")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at 0 -10.16 90)
				(length 2.54)
				(name "SW2")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW1")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SET")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1073CS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1073CS"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1073fa.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC/DC Converter Adjustable Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "LT1073CS_0_1")
		(symbol "LT1073CS_1_1"
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "A0")
				(number "6")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "Ilim")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at 0 -10.16 90)
				(length 2.54)
				(name "SW2")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW1")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SET")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1073CS-5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1073CS-5"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1073fa.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC/DC Converter, Fixed 5V Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1073CS-5_0_1")
		(symbol "LT1073CS-5_1_1"
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "A0")
				(number "6")
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "Ilim")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at 0 -10.16 90)
				(length 2.54)
				(name "SW2")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW1")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SET")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1301"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LT1301"
			(at 7.62 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1301.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower High Efficiency 5V/12V Step-Up DC/DC Converter for Flash Memory, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "5v 12v dc converter boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1301_0_1")
		(symbol "LT1301_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SEL")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SHDN")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ILIM")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "8")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1307CMS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1307CMS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1307fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Cell Micropower 600kHz PWM DC/DC Converter, 50µA Quiescent Current, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower PWM DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT1307CMS8_0_1")
		(symbol "LT1307CMS8_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LBI")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vc")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LBO")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1307CN8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1307CN8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1307fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Cell Micropower 600kHz PWM DC/DC Converter, 50µA Quiescent Current, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower PWM DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1307CN8_0_1")
		(symbol "LT1307CN8_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LBI")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vc")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LBO")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1307CS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1307CS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1307fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Cell Micropower 600kHz PWM DC/DC Converter, 50µA Quiescent Current, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower PWM DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1307CS8_0_1")
		(symbol "LT1307CS8_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LBI")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vc")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LBO")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1372CN8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1372CN8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/13727fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A High Efficiency Switching Regulators, 500kHz, 35V Switch Voltage, Adjustable Output Voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1372CN8_0_1")
		(symbol "LT1372CN8_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S/S")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vin")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GNDS")
				(number "6")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VSW")
				(number "8")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "NFB")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VC")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1372CS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1372CS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/13727fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A High Efficiency Switching Regulators, 500kHz, 35V Switch Voltage, Adjustable Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1372CS8_0_1")
		(symbol "LT1372CS8_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S/S")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vin")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GNDS")
				(number "6")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VSW")
				(number "8")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "NFB")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VC")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1945"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LT1945"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1945fa.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "Dual Micropower DC/DC Converter with Positive and Negative Outputs, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "switched voltage converter regulator inverter double shutdown  positive negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT1945_0_1")
		(symbol "LT1945_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{SHDN1}")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SHDN2}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "PGND")
				(number "9")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "FB2")
				(number "5")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW2")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW1")
				(number "10")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "NFB1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3430"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT3430"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14-1EP_4.4x5mm_P0.65mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/34301fa.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "3A High Voltage 200kHz Step-Down Switching Regulator, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3430_0_1")
		(symbol "LT3430_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SYNC")
				(number "14")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "15")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VC")
				(number "11")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at 0 10.16 270)
				(length 2.54)
				(name "BOOST")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BIAS")
				(number "10")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3439"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LT3439"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16-1EP_4.4x5mm_P0.65mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3439fs.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "1A Slew Rate Controlled Ultralow Noise Isolated DC/DC Transformer Driver, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Isolated DC/DC Transformer Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3439_0_1")
		(symbol "LT3439_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "11")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "5")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "Ct")
				(number "6")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "Rt")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PADGND")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "COLA")
				(number "3")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "COLB")
				(number "14")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "Rsl")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3471"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 11.43 0)
		)
		(property "Value" "LT3471"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3471fb.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Dual 1.3A, 1.2MHz Boost/Inverter, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc/dc converter boost inverter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3471_0_1")
		(symbol "LT3471_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "FB1P")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "FB1N")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{SHDN}/SS1")
				(number "9")
			)
			(pin power_out line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "VREF")
				(number "3")
			)
			(pin passive line
				(at -10.16 12.7 270)
				(length 2.54)
				(name "SW1")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 10.16 12.7 270)
				(length 2.54)
				(name "SW2")
				(number "6")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "FB2P")
				(number "4")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "FB2N")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{SHDN}/SS2")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3472"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LT3472"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3472f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Boost and Inverting DC/DC Converter for CCD Bias, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC converter CCD Bias Boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3472_0_1")
		(symbol "LT3472_1_1"
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VPOS")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "FBP")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "SWP")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "SSP")
				(number "9")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "SWN")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "SSN")
				(number "7")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DN")
				(number "5")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "FBN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3483xS6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "LT3483xS6"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at -19.05 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3483fc.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Inverting Micropower DC/DC Converter with integrated schottky, 2.5V to 16V input, down to -38V output, 200mA, TSOT-23-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Inverting Converter Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT3483xS6_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V_{IN}")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3514xUFD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "LT3514xUFD"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm_ThermalVias"
			(at 39.37 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3514fa.pdf"
			(at -7.62 24.13 0)
		)
		(property "Description" "Triple Step-Down Switching Regulator with 100% Duty Cycle Operation, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "triple step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3514xUFD_0_1")
		(symbol "LT3514xUFD_1_1"
			(pin open_collector line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SW5")
				(number "24")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SKY")
				(number "25")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "16")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "PG")
				(number "23")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RUN/SS1")
				(number "13")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "RUN/SS3")
				(number "15")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RUN/SS4")
				(number "12")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "RT/SYNC")
				(number "17")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "11")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "26")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "28")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "9")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin power_out line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "SW1")
				(number "5")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DA1")
				(number "6")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "FB1")
				(number "20")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SW3")
				(number "4")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DA3")
				(number "3")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FB3")
				(number "21")
			)
			(pin power_out line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SW4")
				(number "7")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "DA4")
				(number "8")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "FB4")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3580xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LT3580xDD"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 31.75 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3580fg.pdf"
			(at -39.37 -10.16 0)
		)
		(property "Description" "Boost/Inverting DC/DC Converter with 2A Switch, Soft-Start, and Synchronization, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost inverting dc-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3580xDD_0_1")
		(symbol "LT3580xDD_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "VC")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SYNC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3580xMS8E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LT3580xMS8E"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm"
			(at 30.48 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3580fg.pdf"
			(at -39.37 -10.16 0)
		)
		(property "Description" "Boost/Inverting DC/DC Converter with 2A Switch, Soft-Start, and Synchronization, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost inverting dc-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3580xMS8E_0_1")
		(symbol "LT3580xMS8E_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "VC")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SYNC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3748xMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "LT3748xMS"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_SO:Analog_MSOP-12-16_3x4.039mm_P0.5mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt3748.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "100V Isolated Flyback Controller, MSOP-16(12)"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated flyback controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3748xMS_0_1")
		(symbol "LT3748xMS_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INTVCC")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VC")
				(number "11")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "10")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "TC")
				(number "12")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "RREF")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RFB")
				(number "16")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "GATE")
				(number "6")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SENSE")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3757EDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LT3757EDD"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3757Afe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boost, flyback, SEPIC and inverting regulator. DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost flyback SEPIC inverting DC/DC regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3757EDD_0_1")
		(symbol "LT3757EDD_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SHDN}/UVLO")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SYNC")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "3")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "VC")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GATE")
				(number "7")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SENSE")
				(number "6")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FBX")
				(number "2")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "INTVCC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3757EMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LT3757EMSE"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3757Afe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boost, flyback, SEPIC and inverting regulator. MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost flyback SEPIC inverting DC/DC regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3757EMSE_0_1")
		(symbol "LT3757EMSE_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SHDN}/UVLO")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SYNC")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RT")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "3")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "VC")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GATE")
				(number "7")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SENSE")
				(number "6")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FBX")
				(number "2")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "INTVCC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3988"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.525 27.305 0)
		)
		(property "Value" "LT3988"
			(at -3.81 24.765 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at -27.94 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3988f.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Dual 1A Switching Buck Regulator with Internal Switches"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual 60V 1A Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*16*1EP*3x4.039mm*P0.5mm*EP1.651x2.845mm*"
			(at 0 0 0)
		)
		(symbol "LT3988_0_1")
		(symbol "LT3988_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "5")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "TRACK/SS1")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "12")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "BOOST1")
				(number "3")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SW1")
				(number "2")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "DA1")
				(number "1")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "FB1")
				(number "14")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VIN1")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VIN2")
				(number "9")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "TRACK/SS2")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RT")
				(number "13")
			)
			(pin power_in line
				(at 15.24 0 180)
				(length 2.54)
				(name "BD")
				(number "4")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "BOOST2")
				(number "6")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SW2")
				(number "7")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "DA2")
				(number "8")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "FB2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT8303"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LT8303"
			(at -6.35 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/8303fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "100VIN Micropower Isolated Flyback Converter with 150V/450mA Switch, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flyback switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT8303_0_1")
		(symbol "LT8303_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "RFB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT8306"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.286 8.89 0)
		)
		(property "Value" "LT8306"
			(at -0.762 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt8306.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.5-60Vin micropower isolated flyback controller, no-optoisolator, 8V NMOS gate drive, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT8306_0_1")
		(symbol "LT8306_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{IN}")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "R_{FB}")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "3")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT8610"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LT8610"
			(at 6.858 8.636 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm_ThermalVias"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt8610.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "42V, 2.5A Synchronous Step-Down Regulator with 2.5uA Quiescent Current, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "high efficiency speed synchronous monolithic buck step-down switching regulator 42V 2.5A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*16*1EP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT8610_0_1")
		(symbol "LT8610_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "EN/UV")
				(number "4")
			)
			(pin open_collector line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PG")
				(number "15")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SYNC")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "TR/SS")
				(number "2")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BIAS")
				(number "14")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INTVcc")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "BST")
				(number "12")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "10")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "9")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT8610AC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LT8610AC"
			(at 0.762 8.636 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm_ThermalVias"
			(at -2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt8610ac-8610ac-1.pdf"
			(at 0 -16.51 0)
		)
		(property "Description" "42V, 3.5A Synchronous Step-Down Regulator with 2.5uA Quiescent Current, 0.8V Feedback Voltage, 3.0V Minimum Vin, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "high efficiency speed synchronous monolithic buck step-down switching regulator 42V 3.5A lower feedback voltage minimum vin"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*16*1EP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT8610AC_0_1")
		(symbol "LT8610AC_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "EN/UV")
				(number "4")
			)
			(pin open_collector line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PG")
				(number "15")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SYNC")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "TR/SS")
				(number "2")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "7")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BIAS")
				(number "14")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INTVcc")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "BST")
				(number "12")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "10")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "9")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT8705AxFE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.304 -29.464 0)
		)
		(property "Value" "LT8705AxFE"
			(at -0.508 5.08 0)
		)
		(property "Footprint" "Package_SO:Linear_HTSSOP-31-38-1EP_4.4x9.7mm_P0.5mm_EP2.74x4.75mm_ThermalVias"
			(at 0 -37.592 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/8705af.pdf"
			(at 0 -33.528 0)
		)
		(property "Description" "Synchronous 4-Switch Buck-Boost DC/DC Controller, 2.8..80V VIN, 1.3..80V VOUT, 100-400kHz, HTSSOP-38(31)"
			(at 0 -35.56 0)
		)
		(property "ki_keywords" "Analog-Devices Linear-Technology soft-start"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HTSSOP*1EP*4.4*9.7*P0.5mm*EP2.74x4.75mm*"
			(at 0 0 0)
		)
		(symbol "LT8705AxFE_1_1"
			(pin output line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "TG1")
				(number "26")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "CSNIN")
				(number "36")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "CSPIN")
				(number "37")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "FBIN")
				(number "8")
			)
			(pin power_in line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "38")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "MODE")
				(number "2")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "SYNC")
				(number "14")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "RT")
				(number "15")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "SS")
				(number "12")
			)
			(pin passive line
				(at -17.78 33.02 270)
				(length 2.54)
				(name "BOOST1")
				(number "28")
			)
			(pin power_out line
				(at -12.7 33.02 270)
				(length 2.54)
				(name "SW1")
				(number "24")
			)
			(pin output line
				(at -10.16 33.02 270)
				(length 2.54)
				(name "BG1")
				(number "17")
			)
			(pin input line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "CSP")
				(number "6")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin input line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "CSN")
				(number "5")
			)
			(pin output line
				(at 10.16 33.02 270)
				(length 2.54)
				(name "BG2")
				(number "19")
			)
			(pin power_out line
				(at 12.7 33.02 270)
				(length 2.54)
				(name "SW2")
				(number "22")
			)
			(pin passive line
				(at 17.78 33.02 270)
				(length 2.54)
				(name "BOOST2")
				(number "20")
			)
			(pin output line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "TG2")
				(number "21")
			)
			(pin input line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "CSPOUT")
				(number "34")
			)
			(pin input line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "CSNOUT")
				(number "32")
			)
			(pin input line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "FBOUT")
				(number "9")
			)
			(pin power_in line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "EXTVCC")
				(number "30")
			)
			(pin power_out line
				(at 22.86 0 180)
				(length 2.54)
				(name "INTVCC")
				(number "1")
			)
			(pin power_in line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "GATEVCC")
				(number "18")
			)
			(pin power_out line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "LDO33")
				(number "7")
			)
			(pin output line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "CLKOUT")
				(number "13")
			)
			(pin passive line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "IMON_IN")
				(number "3")
			)
			(pin passive line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "IMON_OUT")
				(number "10")
			)
			(pin output line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "VC")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1436A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 26.67 0)
		)
		(property "Value" "LTC1436A"
			(at 3.81 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/14367afb.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Efficiency Low Noise Synchronous Step-Down Switching Regulators, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck controller 36V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "LTC1436A_0_1")
		(symbol "LTC1436A_1_1"
			(pin open_collector line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "AUXDR")
				(number "14")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "SFB")
				(number "6")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "AUXFB")
				(number "13")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "AUXON")
				(number "12")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "LBI")
				(number "4")
			)
			(pin open_collector line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "LBO")
				(number "3")
			)
			(pin open_collector line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "POR")
				(number "24")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "VPROG")
				(number "8")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "COSC")
				(number "1")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "RUN/SS")
				(number "2")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "ITH")
				(number "5")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "EXTVCC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "SGND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "16")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "TGL")
				(number "22")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "TGS")
				(number "20")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SW")
				(number "21")
			)
			(pin power_in line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "INTVCC")
				(number "18")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "BOOST")
				(number "23")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "BG")
				(number "17")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SENSE+")
				(number "11")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "SENSE-")
				(number "10")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "VOSENSE")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1436A-PLL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 26.67 0)
		)
		(property "Value" "LTC1436A-PLL"
			(at 3.81 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/14367afb.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Efficiency Low Noise Synchronous Step-Down Switching Regulators, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck controller 36V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "LTC1436A-PLL_0_1")
		(symbol "LTC1436A-PLL_1_1"
			(pin open_collector line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "AUXDR")
				(number "13")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "SFB")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "AUXFB")
				(number "12")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "AUXON")
				(number "11")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "PLLIN")
				(number "24")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PLLLPF")
				(number "1")
			)
			(pin open_collector line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "POR")
				(number "23")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "VPROG")
				(number "7")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "COSC")
				(number "2")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "RUN/SS")
				(number "3")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "ITH")
				(number "4")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "EXTVCC")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "SGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "15")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "TGL")
				(number "21")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "TGS")
				(number "19")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SW")
				(number "20")
			)
			(pin power_in line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "INTVCC")
				(number "17")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "BOOST")
				(number "22")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "BG")
				(number "16")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SENSE+")
				(number "10")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "SENSE-")
				(number "9")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "VOSENSE")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1437A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 29.21 0)
		)
		(property "Value" "LTC1437A"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/14367afb.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Efficiency Low Noise Synchronous Step-Down Switching Regulators, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck controller 36V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC1437A_0_1")
		(symbol "LTC1437A_1_1"
			(pin open_collector line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "AUXDR")
				(number "16")
			)
			(pin passive line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "SFB")
				(number "7")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "AUXFB")
				(number "15")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "AUXON")
				(number "14")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "LBI")
				(number "5")
			)
			(pin open_collector line
				(at -15.24 0 0)
				(length 2.54)
				(name "LBO")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PLLIN")
				(number "28")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PLLLPF")
				(number "1")
			)
			(pin open_collector line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "POR")
				(number "27")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "VPROG")
				(number "9")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "COSC")
				(number "2")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "RUN/SS")
				(number "3")
			)
			(pin passive line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "ITH")
				(number "6")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "EXTVCC")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "SGND")
				(number "8")
			)
			(pin no_connect line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VIN")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "PGND")
				(number "18")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "TGL")
				(number "25")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "TGS")
				(number "23")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SW")
				(number "24")
			)
			(pin power_in line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "INTVCC")
				(number "21")
			)
			(pin power_in line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DRVCC")
				(number "20")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "BOOST")
				(number "26")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "BG")
				(number "19")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "SENSE+")
				(number "13")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "SENSE-")
				(number "12")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "VOSENSE")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1878EMS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LTC1878EMS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1878f.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "High Efficiency Monolithic Synchronous Step-Down Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC1878EMS8_0_1")
		(symbol "LTC1878EMS8_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RUN")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SYNC/MODE")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ITH")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VFB")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PLL_LPF")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3105xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LTC3105xDD"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3105fb.pdf"
			(at -35.56 5.08 0)
		)
		(property "Description" "400mA Step-Up DC/DC Converter with Maximum Power Point Control and 250mV Start-Up, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Solar MPPT Maximum Power Point Control Converter Step-Up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*3x3mm*0.5mm*EP*"
			(at 0 0 0)
		)
		(symbol "LTC3105xDD_0_0"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "MPPC")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_out line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "AUX")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SWITCH")
				(number "7")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{PGOOD}")
				(number "8")
			)
			(pin power_out line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LDO")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FBLDO")
				(number "3")
			)
		)
		(symbol "LTC3105xDD_0_1")
		(embedded_fonts no)
	)
	(symbol "LTC3105xMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LTC3105xMS"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-12_3x4.039mm_P0.65mm"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3105fb.pdf"
			(at -35.56 5.08 0)
		)
		(property "Description" "400mA Step-Up DC/DC Converter with Maximum Power Point Control and 250mV Start-Up, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Solar MPPT Maximum Power Point Control Converter Step-Up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC3105xMS_0_0"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MPPC")
				(number "5")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "AUX")
				(number "12")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin open_collector line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{PGOOD}")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SWITCH")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "11")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LDO")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FBLDO")
				(number "3")
			)
		)
		(symbol "LTC3105xMS_0_1")
		(embedded_fonts no)
	)
	(symbol "LTC3245xDE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -15.24 0)
		)
		(property "Value" "LTC3245xDE"
			(at 3.81 -17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x4mm_P0.5mm_EP1.7x3.3mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc3245.pdf"
			(at 0 -31.75 0)
		)
		(property "Description" "Wide VIN Range, Low Noise, 250mA Buck-Boost Charge Pump, DFN-12"
			(at 0 -29.21 0)
		)
		(property "ki_keywords" "widerange  lownoise buckboost chargepump"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DFN*3x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC3245xDE_0_0"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{BURST}")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SEL1")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SEL2")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "C+")
				(number "9")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "C-")
				(number "11")
			)
		)
		(symbol "LTC3245xDE_1_0"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "EP")
				(number "13")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "PGOOD")
				(number "8")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUTS/ADJ")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3406BES5-1.2"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3406BES5-1.2"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3406b12fs.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "600mA Synchronous Step-Down Regulator, 1.5MHz, Fixed 1.2V Output Voltage, Burst Mode Disabled, ThinSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC3406BES5-1.2_0_1")
		(symbol "LTC3406BES5-1.2_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "RUN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3429"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3429"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3429fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA, 500kHz Micropower Synchronous Boost Converter with Output Disconnect, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC3429_0_1")
		(symbol "LTC3429_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3442"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "LTC3442"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x4mm_P0.5mm_EP1.7x3.3mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3442fb.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Micropower Synchronous Buck-Boost DC/DC Converter with Automatic Burst Mode Operation, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Synchronous Buck-Boost DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*3x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC3442_0_1")
		(symbol "LTC3442_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{SHDN}/SS")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RLIM")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RT")
				(number "2")
			)
			(pin power_in line
				(at -7.62 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "9")
			)
			(pin power_in line
				(at -7.62 -15.24 90)
				(length 2.54)
				(name "SGND")
				(number "3")
			)
			(pin bidirectional line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "SW1")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "PADGND")
				(number "13")
			)
			(pin bidirectional line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "SW2")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "8")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FB")
				(number "12")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VC")
				(number "11")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "BURST")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3525"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3525"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3525fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "400mA Micropower Synchronous Step-Up DC/DC Converter with Output Disconnect, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70* SOT?363*"
			(at 0 0 0)
		)
		(symbol "LTC3525_0_1")
		(symbol "LTC3525_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3561EDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 11.176 0)
		)
		(property "Value" "LTC3561EDD"
			(at 1.778 11.176 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3561f.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A, 0.8V to 5V out, up to 4MHz Synchronous buck converter with internal switch, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck internal switch dc/dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*EP1.65x2.38mm*"
			(at 0 0 0)
		)
		(symbol "LTC3561EDD_0_0"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "PV_{IN}")
				(number "5")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SV_{IN}")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "I_{TH}")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SHDN/R_{T}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "SGND")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "V_{FB}")
				(number "7")
			)
		)
		(symbol "LTC3561EDD_1_0"
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
		)
		(symbol "LTC3561EDD_1_1")
		(embedded_fonts no)
	)
	(symbol "LTC3630xDHC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 11.43 0)
		)
		(property "Value" "LTC3630xDHC"
			(at 1.016 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-16-1EP_3x5mm_P0.5mm_EP1.66x4.4mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3630fd.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA High efficiency 65V synchronous step-down converter, DFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck dc-dc switcher switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*3x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC3630xDHC_0_1")
		(symbol "LTC3630xDHC_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RUN")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vprg1")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Vprg2")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "10")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "Iset")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vin")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Vfb")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FBO")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3630xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 11.43 0)
		)
		(property "Value" "LTC3630xMSE"
			(at 1.016 11.43 0)
		)
		(property "Footprint" "Package_SO:Analog_MSOP-12-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3630fd.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA High efficiency 65V synchronous step-down converter, MSOP-16(12)"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck dc-dc switcher switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*MSOP*12*16*EP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC3630xMSE_0_1")
		(symbol "LTC3630xMSE_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RUN")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vprg1")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Vprg2")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "10")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "Iset")
				(number "11")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vin")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Vfb")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FBO")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3638xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 11.43 0)
		)
		(property "Value" "LTC3638xMSE"
			(at 1.016 11.43 0)
		)
		(property "Footprint" "Package_SO:Analog_MSOP-12-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3638fa.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "250mA High efficiency 140V step-down converter, MSOP-16(12)"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck dc-dc switcher switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*MSOP*12*16*EP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC3638xMSE_0_1")
		(symbol "LTC3638xMSE_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RUN")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OVLO")
				(number "12")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VPRG1")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VPRG2")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "10")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ISET")
				(number "11")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VFB")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FBO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3886"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 3.81 0)
		)
		(property "Value" "LTC3886"
			(at 12.7 3.81 0)
		)
		(property "Footprint" "Package_DFN_QFN:Linear_UGK52_QFN-46-52"
			(at 7.62 -80.01 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTC3886-3886-1.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "60V dual output buck output with digital power system management, UKG52(46)"
			(at 0 0 0)
		)
		(property "ki_keywords" "step down switch manager I2C telemetry fault current sense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linear*UGK52*QFN*46*52*"
			(at 0 0 0)
		)
		(symbol "LTC3886_0_1")
		(symbol "LTC3886_1_1"
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "TG0")
				(number "2")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "BOOST0")
				(number "52")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "SW0")
				(number "1")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "BG0")
				(number "50")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "Isense0+")
				(number "4")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "Isense0-")
				(number "5")
			)
			(pin power_in line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "EXTVcc")
				(number "43")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "Vsense0+")
				(number "7")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "Vsense0-")
				(number "8")
			)
			(pin input line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "TSNS0")
				(number "6")
			)
			(pin input line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "ASEL0")
				(number "21")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "ASEL1")
				(number "22")
			)
			(pin input line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "SYNC")
				(number "13")
			)
			(pin input line
				(at -17.78 -53.34 0)
				(length 2.54)
				(name "WP")
				(number "28")
			)
			(pin input line
				(at -17.78 -55.88 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -58.42 0)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin output line
				(at -17.78 -60.96 0)
				(length 2.54)
				(name "~{ALERT}")
				(number "16")
			)
			(pin input line
				(at -17.78 -63.5 0)
				(length 2.54)
				(name "RUN0")
				(number "19")
			)
			(pin input line
				(at -17.78 -66.04 0)
				(length 2.54)
				(name "RUN1")
				(number "20")
			)
			(pin input line
				(at -17.78 -71.12 0)
				(length 2.54)
				(name "Ithr0")
				(number "11")
			)
			(pin input line
				(at -17.78 -73.66 0)
				(length 2.54)
				(name "Ith0")
				(number "12")
			)
			(pin power_in line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "Vin")
				(number "48")
			)
			(pin power_out line
				(at -5.08 -81.28 90)
				(length 2.54)
				(name "Vdd33")
				(number "30")
			)
			(pin power_out line
				(at 0 5.08 270)
				(length 2.54)
				(name "INTVcc")
				(number "44")
			)
			(pin power_in line
				(at 0 -81.28 90)
				(length 2.54)
				(name "GND")
				(number "53")
			)
			(pin input line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "Iin+")
				(number "47")
			)
			(pin power_out line
				(at 5.08 -81.28 90)
				(length 2.54)
				(name "Vdd25")
				(number "27")
			)
			(pin input line
				(at 7.62 5.08 270)
				(length 2.54)
				(name "Iin-")
				(number "46")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "TG1")
				(number "38")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "BOOST1")
				(number "40")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "SW1")
				(number "39")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "BG1")
				(number "42")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "Isense1+")
				(number "9")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "Isense1-")
				(number "10")
			)
			(pin input line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "Vsense1+")
				(number "35")
			)
			(pin input line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "TSNS1")
				(number "36")
			)
			(pin input line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "Vout_cfg0")
				(number "23")
			)
			(pin input line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "Vout_cfg1")
				(number "24")
			)
			(pin input line
				(at 17.78 -48.26 180)
				(length 2.54)
				(name "FREQ_CFG")
				(number "25")
			)
			(pin input line
				(at 17.78 -50.8 180)
				(length 2.54)
				(name "PHAS_CFG")
				(number "26")
			)
			(pin output line
				(at 17.78 -55.88 180)
				(length 2.54)
				(name "~{FAULT0}")
				(number "17")
			)
			(pin output line
				(at 17.78 -58.42 180)
				(length 2.54)
				(name "~{FAULT1}")
				(number "18")
			)
			(pin output line
				(at 17.78 -60.96 180)
				(length 2.54)
				(name "PGOOD0")
				(number "34")
			)
			(pin output line
				(at 17.78 -63.5 180)
				(length 2.54)
				(name "PGOOD1")
				(number "33")
			)
			(pin input line
				(at 17.78 -66.04 180)
				(length 2.54)
				(name "SHARE_CLK")
				(number "29")
			)
			(pin input line
				(at 17.78 -71.12 180)
				(length 2.54)
				(name "Ithr1")
				(number "32")
			)
			(pin input line
				(at 17.78 -73.66 180)
				(length 2.54)
				(name "Ith1")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC7138xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 11.43 0)
		)
		(property "Value" "LTC7138xMSE"
			(at 1.016 11.43 0)
		)
		(property "Footprint" "Package_SO:Analog_MSOP-12-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/7138f.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "400mA High efficiency 140V step-down converter, MSOP-16(12)"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck dc-dc switcher switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*MSOP*12*16*EP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC7138xMSE_0_1")
		(symbol "LTC7138xMSE_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RUN")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OVLO")
				(number "12")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VPRG1")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VPRG2")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "10")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ISET")
				(number "11")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "ANODE")
				(number "16")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VFB")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FBO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTM4637xV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 17.78 0)
		)
		(property "Value" "LTM4637xV"
			(at 8.89 17.78 0)
		)
		(property "Footprint" "Package_LGA:Linear_LGA-133_15.0x15.0mm_Layout12x12_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4637fc.pdf"
			(at 22.86 19.05 0)
		)
		(property "Description" "20A DC/DC µModule Step-Down Regulator, LGA-133"
			(at 0 0 0)
		)
		(property "ki_keywords" "uModule DCDC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linear*LGA*15.0x15.0mm*Layout12x12*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTM4637xV_0_1")
		(symbol "LTM4637xV_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "RUN")
				(number "A10")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "MODE_PLLIN")
				(number "A8")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "TEMP")
				(number "D10")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "TRACK/SS")
				(number "A9")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "FSET")
				(number "B12")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "COMP")
				(number "A11")
			)
			(pin no_connect line
				(at -10.16 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP1")
				(number "A12")
			)
			(pin no_connect line
				(at -7.62 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP2")
				(number "B11")
			)
			(pin no_connect line
				(at -5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP3")
				(number "C10")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "EXTVCC")
				(number "E12")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "SGND")
				(number "G11")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "SGND")
				(number "H11")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "SGND")
				(number "H12")
			)
			(pin power_out line
				(at 0 20.32 270)
				(length 3.81)
				(name "INTVCC")
				(number "A7")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 3.81)
				(hide yes)
				(name "INTVCC")
				(number "D9")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "B7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "VIN")
				(number "A1")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A2")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A3")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A4")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A5")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A6")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B1")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B2")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B3")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B4")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B5")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B6")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C1")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C2")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C3")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C4")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C5")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C6")
			)
			(pin no_connect line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP4")
				(number "C11")
			)
			(pin no_connect line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP5")
				(number "C12")
			)
			(pin no_connect line
				(at 7.62 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP6")
				(number "D11")
			)
			(pin no_connect line
				(at 10.16 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP7")
				(number "D12")
			)
			(pin open_collector line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "PGOOD")
				(number "F11")
			)
			(pin open_collector line
				(at 15.24 12.7 180)
				(length 3.81)
				(hide yes)
				(name "PGOOD")
				(number "G12")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "DIFF_OUT")
				(number "K12")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "VOUT_LCL")
				(number "L12")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 3.81)
				(name "VOUT")
				(number "J1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J10")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J3")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J8")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J9")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K10")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K11")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K3")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K8")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K9")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L10")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L11")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L3")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L8")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L9")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M10")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M11")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M3")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M8")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M9")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "VOSNS+")
				(number "J12")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "VOSNS-")
				(number "M12")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "VFB")
				(number "F12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTM4637xY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 17.78 0)
		)
		(property "Value" "LTM4637xY"
			(at 8.89 17.78 0)
		)
		(property "Footprint" "Package_BGA:Linear_BGA-133_15.0x15.0mm_Layout12x12_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4637fc.pdf"
			(at 22.86 19.05 0)
		)
		(property "Description" "20A DC/DC µModule Step-Down Regulator, BGA-133"
			(at 0 0 0)
		)
		(property "ki_keywords" "uModule DCDC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linear*BGA*15.0x15.0mm*Layout12x12*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTM4637xY_0_1")
		(symbol "LTM4637xY_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "RUN")
				(number "A10")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "MODE_PLLIN")
				(number "A8")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "TEMP")
				(number "D10")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "TRACK/SS")
				(number "A9")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "FSET")
				(number "B12")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "COMP")
				(number "A11")
			)
			(pin no_connect line
				(at -10.16 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP1")
				(number "A12")
			)
			(pin no_connect line
				(at -7.62 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP2")
				(number "B11")
			)
			(pin no_connect line
				(at -5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP3")
				(number "C10")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "EXTVCC")
				(number "E12")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "SGND")
				(number "G11")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "SGND")
				(number "H11")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "SGND")
				(number "H12")
			)
			(pin power_out line
				(at 0 20.32 270)
				(length 3.81)
				(name "INTVCC")
				(number "A7")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 3.81)
				(hide yes)
				(name "INTVCC")
				(number "D9")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "B7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G9")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H6")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "VIN")
				(number "A1")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A2")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A3")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A4")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A5")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "A6")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B1")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B2")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B3")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B4")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B5")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "B6")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C1")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C2")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C3")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C4")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C5")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 3.81)
				(hide yes)
				(name "VIN")
				(number "C6")
			)
			(pin no_connect line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP4")
				(number "C11")
			)
			(pin no_connect line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP5")
				(number "C12")
			)
			(pin no_connect line
				(at 7.62 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP6")
				(number "D11")
			)
			(pin no_connect line
				(at 10.16 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "MTP7")
				(number "D12")
			)
			(pin open_collector line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "PGOOD")
				(number "F11")
			)
			(pin open_collector line
				(at 15.24 12.7 180)
				(length 3.81)
				(hide yes)
				(name "PGOOD")
				(number "G12")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "DIFF_OUT")
				(number "K12")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "VOUT_LCL")
				(number "L12")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 3.81)
				(name "VOUT")
				(number "J1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J10")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J3")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J8")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "J9")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K10")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K11")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K3")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K8")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "K9")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L10")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L11")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L3")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L8")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "L9")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M1")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M10")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M11")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M3")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M5")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M6")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M8")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(hide yes)
				(name "VOUT")
				(number "M9")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "VOSNS+")
				(number "J12")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "VOSNS-")
				(number "M12")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "VFB")
				(number "F12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTM4638"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "LTM4638"
			(at 7.62 19.05 0)
		)
		(property "Footprint" "Package_BGA:Analog_BGA-49_6.25x6.25mm_Layout7x7_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltm4638.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog Devices 20VIN, 15A Step-Down DC/DC uModule Regulator, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "uModule Buck Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*BGA*6.25x6.25mm*Layout7x7*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LTM4638_0_1")
		(symbol "LTM4638_1_1"
			(pin power_in line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "V_{IN}")
				(number "D3")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "D4")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "E3")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "E4")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "F4")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "G4")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "RUN")
				(number "B4")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "MODE/CLKIN")
				(number "D2")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "PHMODE")
				(number "G5")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "FREQ")
				(number "E1")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "SW")
				(number "B7")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "COMPa")
				(number "D1")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "COMPb")
				(number "F1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "B2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C7")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D7")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E7")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "V_{OUT}")
				(number "A1")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT}")
				(number "A2")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT}")
				(number "A3")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT}")
				(number "A4")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT}")
				(number "A5")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT}")
				(number "F3")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT}")
				(number "G1")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT}")
				(number "G2")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT}")
				(number "G3")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "V_{OSNS}+")
				(number "B1")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "V_{OSNS}-")
				(number "C2")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "FB")
				(number "C1")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "PGOOD")
				(number "B5")
			)
			(pin output line
				(at 15.24 0 180)
				(length 3.81)
				(name "CLKOUT")
				(number "F2")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "T_{SENSE}+")
				(number "A6")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "T_{SENSE}-")
				(number "A7")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "TRACK/SS")
				(number "E2")
			)
			(pin power_out line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "INTV_{CC}")
				(number "B3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTM4668"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 24.13 0)
		)
		(property "Value" "LTM4668"
			(at 0 21.59 0)
		)
		(property "Footprint" "Package_BGA:Analog_BGA-49_6.25x6.25mm_Layout7x7_P0.8mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltm4668.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Quad DC/DC μModule Regulator with Configurable 1.2A Output Array"
			(at 0 0 0)
		)
		(property "ki_keywords" "uModule DCDC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*BGA*6.25x6.25mm*Layout7x7*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LTM4668_1_1"
			(pin power_in line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "VIN")
				(number "A4")
			)
			(pin passive line
				(at -15.24 17.78 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "B4")
			)
			(pin power_in line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VIN")
				(number "F4")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "G4")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RUN1")
				(number "C3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RUN2")
				(number "C5")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RUN3")
				(number "E5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "RUN4")
				(number "E3")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "INTVCC")
				(number "C4")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "MODE/SYNC")
				(number "E4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "A2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin power_out line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "VOUT1")
				(number "A1")
			)
			(pin passive line
				(at 15.24 17.78 180)
				(length 2.54)
				(hide yes)
				(name "VOUT1")
				(number "B1")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "FB1")
				(number "C1")
			)
			(pin open_collector line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PGOOD1")
				(number "D2")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOUT2")
				(number "A7")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VOUT2")
				(number "B7")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "FB2")
				(number "C7")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PGOOD2")
				(number "D6")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VOUT3")
				(number "F7")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT3")
				(number "G7")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "FB3")
				(number "E7")
			)
			(pin open_collector line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PGOOD3")
				(number "D7")
			)
			(pin power_out line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "VOUT4")
				(number "F1")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "VOUT4")
				(number "G1")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "FB4")
				(number "E1")
			)
			(pin open_collector line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PGOOD4")
				(number "D1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTM4671"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 50.8 0)
		)
		(property "Value" "LTM4671"
			(at 0 48.26 0)
		)
		(property "Footprint" "Package_BGA:Analog_BGA-209_9.5x16mm_Layout11x19_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTM4671.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad DC/DC uModule Regulator with Configurable Dual 0.6-3.3V/12A, Dual 0.6-5.5V/5A Output Array, 3.1-20Vin (BGA-209)"
			(at 0 0 0)
		)
		(property "ki_keywords" "uModule DCDC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*BGA*9.5x16mm*Layout11x19*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LTM4671_1_1"
			(pin passive line
				(at -20.32 43.18 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "D10")
			)
			(pin passive line
				(at -20.32 43.18 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "D11")
			)
			(pin power_in line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "V_{IN}")
				(number "D7")
			)
			(pin passive line
				(at -20.32 43.18 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "D8")
			)
			(pin passive line
				(at -20.32 43.18 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "D9")
			)
			(pin passive line
				(at -20.32 43.18 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "E8")
			)
			(pin power_in line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "V_{IN}")
				(number "H6")
			)
			(pin passive line
				(at -20.32 40.64 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "J5")
			)
			(pin passive line
				(at -20.32 40.64 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "J6")
			)
			(pin power_in line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "V_{IN}")
				(number "L5")
			)
			(pin passive line
				(at -20.32 38.1 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "L6")
			)
			(pin passive line
				(at -20.32 38.1 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "M6")
			)
			(pin power_in line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "V_{IN}")
				(number "R10")
			)
			(pin passive line
				(at -20.32 35.56 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "T10")
			)
			(pin passive line
				(at -20.32 35.56 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "T11")
			)
			(pin passive line
				(at -20.32 35.56 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "T7")
			)
			(pin passive line
				(at -20.32 35.56 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "T8")
			)
			(pin passive line
				(at -20.32 35.56 0)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "T9")
			)
			(pin power_in line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "SV_{IN0}")
				(number "E9")
			)
			(pin power_in line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "SV_{IN3}")
				(number "R9")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "RUN0")
				(number "F11")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "RUN1")
				(number "J8")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "RUN2")
				(number "L8")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "RUN3")
				(number "P7")
			)
			(pin open_collector line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "PGOOD0")
				(number "E11")
			)
			(pin open_collector line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PGOOD1")
				(number "H8")
			)
			(pin open_collector line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PGOOD2")
				(number "M8")
			)
			(pin open_collector line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PGOOD3")
				(number "R7")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "MODE/CLKIN0")
				(number "G11")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "MODE/CLKIN12")
				(number "L9")
			)
			(pin passive line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "MODE/CLKIN3")
				(number "R8")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "CLKOUT0")
				(number "E10")
			)
			(pin output line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "CLKOUT3")
				(number "P6")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "FREQ0")
				(number "F10")
			)
			(pin passive line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "FREQ12")
				(number "K10")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "FREQ3")
				(number "P8")
			)
			(pin passive line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "COMP0a")
				(number "H10")
			)
			(pin passive line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "COMP0b")
				(number "H11")
			)
			(pin passive line
				(at -20.32 -35.56 0)
				(length 3.81)
				(name "COMP1")
				(number "J11")
			)
			(pin passive line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "COMP2")
				(number "M11")
			)
			(pin passive line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "COMP3a")
				(number "N9")
			)
			(pin passive line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "COMP3b")
				(number "N8")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A10")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A9")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B10")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B8")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B9")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C10")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C8")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C9")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E3")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F2")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F3")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G2")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G3")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "J7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "J9")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K2")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K3")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "L7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "M10")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "M5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "M7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N2")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N3")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "P1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "P11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "P2")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "P3")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "P4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "P5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "R3")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "R4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "R5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "T4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "T5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "T6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U10")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U8")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U9")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V10")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V8")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V9")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "W10")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "W11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "W4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "W5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "W8")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "W9")
			)
			(pin power_out line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "V_{OUT0}")
				(number "A1")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "A2")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "A3")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "B1")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "B2")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "B3")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "C1")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "C2")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "C3")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "D1")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "D2")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "D3")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "E1")
			)
			(pin passive line
				(at 20.32 43.18 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT0}")
				(number "E2")
			)
			(pin input line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "VOSNS0^{+}")
				(number "G8")
			)
			(pin input line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "VOSNS0^{-}")
				(number "F8")
			)
			(pin input line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "FB0")
				(number "G9")
			)
			(pin power_out line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "V_{OUT1}")
				(number "H1")
			)
			(pin passive line
				(at 20.32 30.48 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT1}")
				(number "H2")
			)
			(pin passive line
				(at 20.32 30.48 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT1}")
				(number "H3")
			)
			(pin passive line
				(at 20.32 30.48 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT1}")
				(number "H4")
			)
			(pin passive line
				(at 20.32 30.48 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT1}")
				(number "J1")
			)
			(pin passive line
				(at 20.32 30.48 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT1}")
				(number "J2")
			)
			(pin passive line
				(at 20.32 30.48 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT1}")
				(number "J3")
			)
			(pin passive line
				(at 20.32 30.48 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT1}")
				(number "J4")
			)
			(pin input line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "VOSNS1")
				(number "J10")
			)
			(pin input line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "FB1")
				(number "H9")
			)
			(pin power_out line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "V_{OUT2}")
				(number "L1")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT2}")
				(number "L2")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT2}")
				(number "L3")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT2}")
				(number "L4")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT2}")
				(number "M1")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT2}")
				(number "M2")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT2}")
				(number "M3")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT2}")
				(number "M4")
			)
			(pin input line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "VOSNS2")
				(number "L10")
			)
			(pin input line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "FB2")
				(number "M9")
			)
			(pin power_out line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "V_{OUT3}")
				(number "R1")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "R2")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "T1")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "T2")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "T3")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "U1")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "U2")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "U3")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "V1")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "V2")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "V3")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "W1")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "W2")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(hide yes)
				(name "V_{OUT3}")
				(number "W3")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "VOSNS3^{+}")
				(number "N11")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "VOSNS3^{-}")
				(number "P10")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "FB3")
				(number "N10")
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "TSENSE0^{+}")
				(number "A7")
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TSENSE0^{-}")
				(number "A6")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "TMON")
				(number "K8")
			)
			(pin passive line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "TSENSE3^{+}")
				(number "W6")
			)
			(pin passive line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "TSENSE3^{-}")
				(number "W7")
			)
			(pin passive line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PHMODE0")
				(number "E6")
			)
			(pin passive line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PHMODE3")
				(number "R6")
			)
			(pin passive line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "TRACK/SS0")
				(number "F9")
			)
			(pin passive line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "TRACK/SS1")
				(number "G7")
			)
			(pin passive line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "TRACK/SS2")
				(number "N7")
			)
			(pin passive line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "TRACK/SS3")
				(number "P9")
			)
			(pin power_out line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "INTV_{CC0}")
				(number "E7")
			)
			(pin power_out line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "INTV_{CC12}")
				(number "K9")
			)
			(pin power_out line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "INTV_{CC3}")
				(number "R11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTM8049"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 22.86 0)
		)
		(property "Value" "LTM8049"
			(at 6.35 -22.86 0)
		)
		(property "Footprint" "Package_BGA:Analog_BGA-77_9x15mm_Layout7x11_P1.27mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTM8049.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Dual SEPIC or Inverting μModule DC/DC Converter, 2.6 to 20V input, 2.5V to 24V or -2.5V to -24V output, 1A @ 5V output current per converter, BGA-77 package."
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Converter Dual"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*BGA*9x15mm*Layout7x11*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTM8049_1_1"
			(pin power_in line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "V_{IN1}")
				(number "A5")
			)
			(pin passive line
				(at -12.7 17.78 0)
				(length 2.54)
				(hide yes)
				(name "V_{IN1}")
				(number "A6")
			)
			(pin passive line
				(at -12.7 17.78 0)
				(length 2.54)
				(hide yes)
				(name "V_{IN1}")
				(number "A7")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "RUN1")
				(number "B7")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "RT1")
				(number "E7")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CLKOUT1")
				(number "E6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SYNC1")
				(number "D7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SHARE1")
				(number "F3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SHARE2")
				(number "F4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SYNC2")
				(number "H7")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CLKOUT2")
				(number "G6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "RT2")
				(number "G7")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "RUN2")
				(number "K7")
			)
			(pin power_in line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "V_{IN2}")
				(number "L5")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "V_{IN2}")
				(number "L6")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "V_{IN2}")
				(number "L7")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "H3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "H4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "H5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "J3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "J4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "J5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "J6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "K3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "K4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "K5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "K6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "L3")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "L4")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "SS1")
				(number "C7")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PG1")
				(number "D6")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "V_{OUT1P}")
				(number "A1")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT1P}")
				(number "A2")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT1P}")
				(number "B1")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT1P}")
				(number "B2")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "FBX1")
				(number "C1")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "V_{OUT1N}")
				(number "C2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT1N}")
				(number "D1")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT1N}")
				(number "D2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT1N}")
				(number "E1")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT1N}")
				(number "E2")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "V_{OUT2P}")
				(number "K1")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT2P}")
				(number "K2")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT2P}")
				(number "L1")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT2P}")
				(number "L2")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "FBX2")
				(number "J1")
			)
			(pin power_out line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "V_{OUT2N}")
				(number "G1")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT2N}")
				(number "G2")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT2N}")
				(number "H1")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT2N}")
				(number "H2")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT2N}")
				(number "J2")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PG2")
				(number "H6")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "SS2")
				(number "J7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTM8063"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "LTM8063"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_BGA:Analog_BGA-28_4x6.25mm_Layout4x7_P0.8mm"
			(at 20.32 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/8063fa.pdf"
			(at 22.86 19.05 0)
		)
		(property "Description" "40VIN, 2A Silent Switcher µModule Regulator, BGA-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "uModule DCDC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*BGA*4x6.25mm*Layout4x7*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LTM8063_0_1")
		(symbol "LTM8063_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RUN")
				(number "B3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "B2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "TR/SS")
				(number "A3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RT")
				(number "C1")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "B4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E3")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "C4")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "F1")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "F2")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "F3")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "F4")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "G1")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "G2")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "G3")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "G4")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "PG")
				(number "B1")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX15062A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "MAX15062A"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8_2x2mm_P0.5mm"
			(at 0 13.97 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX15062.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "60V, 300mA, synchronous step-down dc-dc converter, 3.3V fixed output voltage, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX15062A_0_1")
		(symbol "MAX15062A_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "MODE")
				(number "5")
			)
			(pin power_out line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LX")
				(number "8")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB/Vout")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1522"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.445 6.35 0)
		)
		(property "Value" "MAX1522"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX1522-MAX1524.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Boost converter, external switch, soft-start, latch on output fault, 2.5V..5.5Vin,  SOT-23-6"
			(at 0 10.795 0)
		)
		(property "ki_keywords" "maxim analog-devices"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX1522_0_0"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "V_{CC}")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "EXT")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(symbol "MAX1522_1_1")
		(embedded_fonts no)
	)
	(symbol "MAX17501AxTB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX17501AxTB"
			(at 2.032 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-10-1EP_2x3mm_P0.5mm_EP0.9x2mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17501.pdf"
			(at -34.29 26.67 0)
		)
		(property "Description" "4.5V–60Vin, 500mA, High-Efficiency, 3.3V Synchronous Step-Down DC-DC Converter, PFM Mode, TDFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX17501AxTB_0_1")
		(symbol "MAX17501AxTB_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "3")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "6")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LX")
				(number "10")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB/VO")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX17501GxTB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX17501GxTB"
			(at 2.032 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-10-1EP_2x3mm_P0.5mm_EP0.9x2mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17501.pdf"
			(at -34.29 26.67 0)
		)
		(property "Description" "4.5V–60Vin, 500mA, High-Efficiency, Adjustable Synchronous Step-Down DC-DC Converter, 600KHz, TDFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX17501GxTB_0_1")
		(symbol "MAX17501GxTB_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "3")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "7")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "6")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LX")
				(number "10")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB/VO")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX17572"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "MAX17572"
			(at 4.572 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17572.pdf"
			(at -34.29 26.67 0)
		)
		(property "Description" "4.5V–60V, 1A, High-Efficiency, Synchronous Step-Down DC-DC Converter with Internal Compensation, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX17572_0_1")
		(symbol "MAX17572_1_1"
			(pin power_in line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RT/SYNC")
				(number "6")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "EXTVCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "13")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "BST")
				(number "10")
			)
			(pin power_out line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "LX")
				(number "11")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
			(pin open_collector line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin power_out line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX17574"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "MAX17574"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x5mm_P0.5mm_EP2.65x3.65mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17574.pdf"
			(at -35.56 15.24 0)
		)
		(property "Description" "4.5V–60V, 3A, High-Efficiency, Synchronous Step-Down DC-DC Converter with Internal Compensation, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX17574_0_1")
		(symbol "MAX17574_1_1"
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "5")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "6")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "7")
			)
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "9")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "RT")
				(number "19")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "MODE/SYNC")
				(number "15")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SS")
				(number "16")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "2")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "EXTVCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "SGND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BST")
				(number "22")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "LX")
				(number "1")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "LX")
				(number "23")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LX")
				(number "24")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "CF")
				(number "17")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "18")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{RESET}")
				(number "14")
			)
			(pin power_out line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX17620ATA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "MAX17620ATA"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17620.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "2.7-5.5V, 600mA, Synchronous Step-Down DC-DC Converter with Integrated MOSFETs, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX17620ATA_0_1")
		(symbol "MAX17620ATA_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "MODE")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "LX")
				(number "8")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOUT")
				(number "7")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PGOOD")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1771xSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 10.16 0)
		)
		(property "Value" "MAX1771xSA"
			(at 6.35 10.16 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1771.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V or Adjustable, High-Efficiency, Low IQ, Step-Up DC-DC Controller, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Step-Up Boost Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX1771xSA_0_1")
		(symbol "MAX1771xSA_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SHDN")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "REF")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "EXT")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5035AUPA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX5035AUPA"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5035.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A, High-Efficiency Step-Down DC-DC Converter, 3.3V fixed output voltage, Vin 76V, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V 1A Step-Down Converter 76V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX5035AUPA_0_1")
		(symbol "MAX5035AUPA_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "SGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BST")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "LX")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5035AUSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX5035AUSA"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5035.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A, High-Efficiency Step-Down DC-DC Converter, 3.3V fixed output voltage, Vin 76V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V 1A Step-Down Converter 76V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX5035AUSA_0_1")
		(symbol "MAX5035AUSA_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "SGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BST")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "LX")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX777L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX777L"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://kanga.gerbilator.org/ICs/MAX777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "210mA, Low voltage input, step-up DC-DC converter, 5V output voltage, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching regulator boost step-up dc-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX777L_0_1")
		(symbol "MAX777L_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ILIM")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LX")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX77827AEFD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -11.43 0)
		)
		(property "Value" "MAX77827AEFD"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Maxim_FC2QFN-14_2.5x2.5mm_P0.5mm"
			(at 0 13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX77827.pdf"
			(at 0 16.51 0)
		)
		(property "Description" "5.5V Input, 1.8A/3.1A Switch Buck-Boost, QFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck Boost Switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maxim?FC2QFN*14*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX77827AEFD_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "LX1")
				(number "8")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FPWM")
				(number "14")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SEL")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "BIAS")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "9")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "LX2")
				(number "10")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "11")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTS")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "POK")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX778L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX778L"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://kanga.gerbilator.org/ICs/MAX777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "210mA, Low voltage input, step-up DC-DC converter, 3V/3.3V output voltage, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching regulator boost step-up dc-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX778L_0_1")
		(symbol "MAX778L_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ILIM")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SEL")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LX")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX779L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX779L"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://kanga.gerbilator.org/ICs/MAX777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "210mA, Low voltage input, step-up DC-DC converter, adjustable output voltage, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching regulator boost step-up dc-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX779L_0_1")
		(symbol "MAX779L_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ILIM")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LX")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC33063AD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MC33063AD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF"
			(at 12.7 -2.54 0)
		)
		(property "Description" "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps buck boost inverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC33063AD_0_1")
		(symbol "MC33063AD_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "Vin")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "TC")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Ipk")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DC")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "SwC")
				(number "1")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SwE")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Vfb")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC33063AP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MC33063AP"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF"
			(at 12.7 -2.54 0)
		)
		(property "Description" "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps buck boost inverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MC33063AP_0_1")
		(symbol "MC33063AP_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "Vin")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "TC")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Ipk")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DC")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "SwC")
				(number "1")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SwE")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Vfb")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC33063MNTXG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MC33063MNTXG"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.5x3.6mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF"
			(at 12.7 -2.54 0)
		)
		(property "Description" "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps buck boost inverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC33063MNTXG_0_1")
		(symbol "MC33063MNTXG_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "Vin")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "TC")
				(number "3")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Ipk")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DC")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "SwC")
				(number "1")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SwE")
				(number "2")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Vfb")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP16301x-xCH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP16301x-xCH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005004D.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 4.0 to 30V Input, High Voltage Input integrated switch step-down regulator, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP16301x-xCH_0_1")
		(symbol "MCP16301x-xCH_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V_{IN}")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BOOST")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Vfb")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP16311x-xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP16311x-xMNY"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP16311-Family-Data-Sheet-DS20005255C.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "1A Output Voltage, 30V Input, integrated switch step-down regulator, PFM/PWM modulation, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP16311x-xMNY_0_1")
		(symbol "MCP16311x-xMNY_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{IN}")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V_{CC}")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOST")
				(number "7")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Vfb")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP16311x-xMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP16311x-xMS"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP16311-Family-Data-Sheet-DS20005255C.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "30V Input, 1A Output Voltage, integrated switch step-down regulator, PFM/PWM modulation, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP16311x-xMS_0_1")
		(symbol "MCP16311x-xMS_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{IN}")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V_{CC}")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOST")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Vfb")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP16331x-xCH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 8.89 0)
		)
		(property "Value" "MCP16331x-xCH"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005308C.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "High-Voltage Input Integrated Switch Step-Down Regulator, VDD +4.4V to 50V, Out +2.0V to +24V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Voltage Input Integrated Switch Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP16331x-xCH_0_1")
		(symbol "MCP16331x-xCH_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{IN}")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOST")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "V_{FB}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP16331x-xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 8.89 0)
		)
		(property "Value" "MCP16331x-xMNY"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005308C.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "High-Voltage Input Integrated Switch Step-Down Regulator, VDD +4.4V to 50V, Out +2.0V to +24V, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Voltage Input Integrated Switch Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP16331x-xMNY_0_1")
		(symbol "MCP16331x-xMNY_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{IN}")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOST")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "V_{FB}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1640x-xCHY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1640x-xCHY"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002234D.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output 2.0V-5.5V, PWM/PFM True Disconnect, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1640x-xCHY_0_1")
		(symbol "MCP1640x-xCHY_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{IN}")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "V_{FB}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1640x-xMC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1640x-xMC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002234D.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output 2.0V-5.5V, PWM/PFM True Disconnect, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP1640x-xMC_0_1")
		(symbol "MCP1640x-xMC_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{IN}")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "V_{OUT}")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "V_{FB}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1650x-xMC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1650x-xMC"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21876B.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "750 kHz Boost Controller, 3.3-100V output voltage, 5W, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP1650x-xMC_0_1")
		(symbol "MCP1650x-xMC_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V_{IN}")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
			(pin open_emitter line
				(at 10.16 0 180)
				(length 2.54)
				(name "EXT")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1651x-xMC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1651x-xMC"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21876B.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "750 kHz Boost Controller, 3.3-100V output voltage, 5W, Low Battery Detection, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP1651x-xMC_0_1")
		(symbol "MCP1651x-xMC_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V_{IN}")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "LBI")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "EXT")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{LBO}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1652x-xMC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1652x-xMC"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21876B.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "750 kHz Boost Controller, 3.3-100V output voltage, 5W, Power Good Detection, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP1652x-xMC_0_1")
		(symbol "MCP1652x-xMC_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V_{IN}")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
			(pin open_emitter line
				(at 10.16 0 180)
				(length 2.54)
				(name "EXT")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1653x-xUN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP1653x-xUN"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21876B.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "750 kHz Boost Controller, 3.3-100V output voltage, 5W, Low Battery Detection, Power Good Detection, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP1653x-xUN_0_1")
		(symbol "MCP1653x-xUN_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V_{IN}")
				(number "10")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "LBI")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "CS")
				(number "3")
			)
			(pin open_emitter line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EXT")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{LBO}")
				(number "8")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2177"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "MIC2177"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2177.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A Synchronous Buck Regulator, Adjustable Output Voltage, SO-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck Regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W?7.5x12.8mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MIC2177_0_1")
		(symbol "MIC2177_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "2")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "9")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "20")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "18")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "AUTO")
				(number "11")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Bias")
				(number "19")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "SGND")
				(number "14")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "SGND")
				(number "15")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "SGND")
				(number "16")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "SGND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "6")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "7")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "Sense")
				(number "10")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2178"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "MIC2178"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2177.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A Synchronous Buck Regulator, 4.5-16.5V Input Voltage, Adjustable Output Voltage, SO-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck Regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MIC2178_0_1")
		(symbol "MIC2178_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "2")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "9")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN")
				(number "20")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "18")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{PWM}")
				(number "10")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "BIAS")
				(number "19")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "SGND")
				(number "14")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "SGND")
				(number "15")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "SGND")
				(number "16")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "SGND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "6")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "7")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "FB")
				(number "12")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "PWRGD")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2207"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 11.43 0)
		)
		(property "Value" "MIC2207"
			(at 10.16 -11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.5mm_EP1.7x2.4mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC2207-2MHz-3A-PWM-Buck-Regulator-DS20006470A.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "3A 2MHz Non-Synchronous Buck Regulator, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "adjustable switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MIC2207_0_1")
		(symbol "MIC2207_1_1"
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "11")
			)
			(pin power_in line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "BIAS")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin open_collector line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PGOOD")
				(number "9")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "SGND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "12")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2253"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 -11.43 0)
		)
		(property "Value" "MIC2253"
			(at 7.62 -11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.5mm_EP1.6x2.5mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/MIC2253-High-Current-1MHz-High-Efficiency-Boost-Regulator-with-OVP-and-Soft-Start-DS20006070A.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.5A 1 MHz boost regulator, 2.5V to 10V input, up to 30V output, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching voltage converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*12*1EP*3x3mm*P0.5mm*EP1.6x2.5mm*"
			(at 0 0 0)
		)
		(symbol "MIC2253_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "EN")
				(number "11")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "2")
			)
			(pin power_in line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 12.7 270)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin passive line
				(at 5.08 12.7 270)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OVP")
				(number "9")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "COMP")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC2290"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC2290"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:Micrel_MLF-8-1EP_2x2mm_P0.5mm_EP0.8x1.3mm_ThermalVias"
			(at -31.75 -19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2290.pdf"
			(at 1.27 -5.08 0)
		)
		(property "Description" "1.2 Mhz PWM Boost Regulator with Internal Schotty Diode, MLF-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost switching voltage converter regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Micrel*MLF*8*2x2mm*"
			(at 0 0 0)
		)
		(symbol "MIC2290_0_1")
		(symbol "MIC2290_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "EP_GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC23050-CYML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "MIC23050-CYML"
			(at -7.62 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:Micrel_MLF-8-1EP_2x2mm_P0.5mm_EP0.6x1.2mm_ThermalVias"
			(at 15.24 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic23050.pdf"
			(at 15.24 2.54 0)
		)
		(property "Description" "4MHz PWM Buck Regulator with HyperLight Load Switching Scheme, 1.0V Fixed Output Voltage, MLF-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Micrel*MLF*8*2x2mm*"
			(at 0 0 0)
		)
		(symbol "MIC23050-CYML_0_0"
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "EP_GND")
				(number "9")
			)
		)
		(symbol "MIC23050-CYML_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "8")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SNS")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "CFF")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC4684"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC4684"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MIC4684.pdf"
			(at 1.27 -1.27 0)
		)
		(property "Description" "2A, 200kHz SuperSwitcher Buck Regulator, 4-30V Input Voltage, Adjustable Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator switching adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MIC4684_0_1")
		(symbol "MIC4684_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BS")
				(number "4")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC4690"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC4690"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic4690.pdf"
			(at 1.27 -1.27 0)
		)
		(property "Description" "1A, 500kHz SuperSwitcher Buck Regulator, 4-34V Input Voltage, Adjustable Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator switching adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MIC4690_0_1")
		(symbol "MIC4690_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SHDN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP1470"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MP1470"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/pub/media/document/MP1470_r1.02.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Efficiency, 2A, 16V, 500kHz Synchronous, Step-Down Converter, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "MP1470_0_1")
		(symbol "MP1470_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BST")
				(number "6")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP171GJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "MP171GJ"
			(at 10.16 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/pub/media/document/m/p/mp171_r1.01.pdf"
			(at 6.35 0 0)
		)
		(property "Description" "60mA Non-Isolated Off-Line Regulator, 700V Input Voltage, Adjustable Output Voltage, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator switching adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "MP171GJ_0_1")
		(symbol "MP171GJ_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DRAIN")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SOURCE")
				(number "3")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "SOURCE")
				(number "4")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP171GS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "MP171GS"
			(at 10.16 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/pub/media/document/m/p/mp171_r1.01.pdf"
			(at 7.62 2.54 0)
		)
		(property "Description" "60mA Non-Isolated Off-Line Regulator, 700V Input Voltage, Adjustable Output Voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator switching adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MP171GS_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DRAIN")
				(number "7")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SOURCE")
				(number "3")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "SOURCE")
				(number "4")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP2303ADN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.366 8.636 0)
		)
		(property "Value" "MP2303ADN"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/pub/media/document/MP2303A_r1.1.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Synchronous Rectified 3A, 28V, 360kHz Step-Down Converter, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter step down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MP2303ADN_0_1")
		(symbol "MP2303ADN_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BS")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP2303ADP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.366 8.636 0)
		)
		(property "Value" "MP2303ADP"
			(at 6.985 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/pub/media/document/MP2303A_r1.1.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Synchronous Rectified 3A, 28V, 360kHz Step-Down Converter, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter step down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MP2303ADP_0_1")
		(symbol "MP2303ADP_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BS")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPM3550EGLE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MPM3550EGLE"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_LGA:MPS_LGA-18-10EP_12x12mm_P3.3mm"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MPM3550EGLE/document_id/5102/"
			(at -3.81 -9.525 0)
		)
		(property "Description" "Synchronous Step-Down Regulator 5 Amp, 4.5V to 36V input voltage, 1.0V to 12.0V Adjustable Vout LGA-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MPS*LGA*10EP*12x12mm*P3.3mm*"
			(at 0 0 0)
		)
		(symbol "MPM3550EGLE_0_1")
		(symbol "MPM3550EGLE_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RFREQ")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PGOOD")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MT3608"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.89 0)
		)
		(property "Value" "MT3608"
			(at -3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.olimex.com/Products/Breadboarding/BB-PWR-3608/resources/MT3608.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency 1.2MHz 2A Step Up Converter, 2-24V Vin, 28V Vout, 4A current limit, 1.2MHz, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*"
			(at 0 0 0)
		)
		(symbol "MT3608_0_1")
		(symbol "MT3608_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MUN12AD01-SH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MUN12AD01-SH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Cyntec_MUN12AD01-SH"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.cyntec.com/upfile/products/download/Cyntec%20MUN12AD01-SH_Datasheet.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "DC/DC Switching Regulator, Power Module, 1A, Cyntec MUN12AD01"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Switching Regulator Power Module 1A Cyntec MUN12AD01"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?Cyntec?MUN12AD01?SH*"
			(at 0 0 0)
		)
		(symbol "MUN12AD01-SH_0_1")
		(symbol "MUN12AD01-SH_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PGOOD")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MUN12AD03-SH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MUN12AD03-SH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Cyntec_MUN12AD03-SH"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.cyntec.com/upfile/products/download/Cyntec%20MUN12AD03-SH_Datasheet.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "DC/DC Switching Regulator, Power Module, 3A, Cyntec MUN12AD03"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Switching Regulator Power Module 3A Cyntec MUN12AD03"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?Cyntec?MUN12AD03?SH*"
			(at 0 0 0)
		)
		(symbol "MUN12AD03-SH_0_1")
		(symbol "MUN12AD03-SH_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "9")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PGOOD")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NBM5100A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 -13.97 0)
		)
		(property "Value" "NBM5100A"
			(at -10.16 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DHVQFN-16-1EP_2.5x3.5mm_P0.5mm_EP1x2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/NBM5100.pdf"
			(at 0 0 0)
		)
		(property "Description" "coin cell booster charge pump DHVQFN16 SOT763"
			(at 0 0 0)
		)
		(property "ki_keywords" "charge pump"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DHVQFN*1EP*2.5x3.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NBM5100A_0_1")
		(symbol "NBM5100A_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VBT")
				(number "7")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "RDY")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "START")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ADR")
				(number "4")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "TST")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "VSSP")
				(number "12")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDHS")
				(number "9")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VDH")
				(number "14")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VDP")
				(number "15")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LX2")
				(number "11")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LX1")
				(number "13")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CAP")
				(number "10")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "BAL")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NBM7100A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 -13.97 0)
		)
		(property "Value" "NBM7100A"
			(at -10.16 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DHVQFN-16-1EP_2.5x3.5mm_P0.5mm_EP1x2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/NBM7100.pdf"
			(at 0 0 0)
		)
		(property "Description" "coin cell booster charge pump DHVQFN16 SOT763"
			(at 0 0 0)
		)
		(property "ki_keywords" "charge pump"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DHVQFN*1EP*2.5x3.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NBM7100A_0_1")
		(symbol "NBM7100A_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VBT")
				(number "7")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "RDY")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "START")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ADR")
				(number "4")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "TST")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "VSSP")
				(number "12")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDHS")
				(number "9")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VDH")
				(number "14")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VDP")
				(number "15")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LX2")
				(number "11")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LX1")
				(number "13")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CAP")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1070P065"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1070P065"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 65kHz, 22Ohm Rds(on), 250mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "NCP1070P065_0_1")
		(symbol "NCP1070P065_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "DRAIN")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1070STAT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1070STAT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 65kHz, 22Ohm Rds(on), 250mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "NCP1070STAT_0_1")
		(symbol "NCP1070STAT_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "DRAIN")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NID30S24-05"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NID30S24-05"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_MeanWell_NID30_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.meanwell.com/webapp/product/search.aspx?prod=nid30"
			(at 0 0 0)
		)
		(property "Description" "2.5A/12.5W Step Down Converter Module, fixed 5V Output Voltage, 250kHz, 20-53V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Converter Module DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*MeanWell*NID30*THT*"
			(at 0 0 0)
		)
		(symbol "NID30S24-05_0_1")
		(symbol "NID30S24-05_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "7")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "RC")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "COM")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "Vout")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "Vout")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NID60S24-05"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NID60S24-05"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_MeanWell_NID60_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.meanwell.com/78ddf876-a86c-4a52-8a41-4ee24dd9913d"
			(at 0 0 0)
		)
		(property "Description" "4A/20W Step Down Converter Module, fixed 5V Output Voltage, 250kHz, 20-53V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Converter Module DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*MeanWell*NID60*"
			(at 0 0 0)
		)
		(symbol "NID60S24-05_0_1")
		(symbol "NID60S24-05_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "7")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "RC")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "COM")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "Vout")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "Vout")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NMA0512DC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA0512DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±42mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, ±12V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
		(symbol "NMA0512DC_0_1")
		(symbol "NMA0512DC_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN+")
				(number "14")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VIN-")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT+")
				(number "9")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "0V")
				(number "8")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VOUT-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NMA0512SC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA0512SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±42mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, ±12V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
		(symbol "NMA0512SC_0_1")
		(symbol "NMA0512SC_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN+")
				(number "1")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VIN-")
				(number "2")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT+")
				(number "6")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "0V")
				(number "5")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VOUT-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NXE2S0505MC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "NXE2S0505MC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NXExSxxxxMC_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8807031898142/kdc-nxe2.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "2W 5V to 5V 400mA DC-DC Converter with 3kV isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NXExSxxxxMC*"
			(at 0 0 0)
		)
		(symbol "NXE2S0505MC_0_1")
		(symbol "NXE2S0505MC_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "+VIN")
				(number "3")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "-VIN")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+VOUT")
				(number "8")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "-VOUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM2301CAAB330"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2301CAAB330"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/PAM2301.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "800mA, Step-Down DC/DC-Converter, 3.3V Fixed Output Voltage, 1.5MHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "PAM2301CAAB330_0_1")
		(symbol "PAM2301CAAB330_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM2301CAABADJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2301CAABADJ"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/PAM2301.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "800mA, Step-Down DC/DC-Converter, Adjustable Output Voltage, 1.5MHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "PAM2301CAABADJ_0_1")
		(symbol "PAM2301CAABADJ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM2305AAB330"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305AAB330"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 3.3V Fixed Output Voltage, 1.5MHz, TSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "PAM2305AAB330_0_1")
		(symbol "PAM2305AAB330_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM2305BJE330"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305BJE330"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 3.3V Fixed Output Voltage, 1.5MHz, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAM2305BJE330_0_1")
		(symbol "PAM2305BJE330_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "10")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "11")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "12")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "14")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "15")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM2305CGF330"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305CGF330"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 3.3V Fixed Output Voltage, 1.5MHz, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PAM2305CGF330_0_1")
		(symbol "PAM2305CGF330_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAM2306AYPAA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "PAM2306AYPAA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2306.pdf"
			(at -33.02 -45.72 0)
		)
		(property "Description" "1A, Dual Step-Down DC/DC-Converter, Out1 ADJ, Out2 ADJ, 1.5MHz, W-DFN3x3"
			(at 0 0 0)
		)
		(property "ki_keywords" "STEP-DOWN Dual channel 1A Out1 ADJ, Out2 ADJ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*3x3mm?P0.45mm*"
			(at 0 0 0)
		)
		(symbol "PAM2306AYPAA_0_1")
		(symbol "PAM2306AYPAA_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN1")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN1")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN2")
				(number "1")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN2")
				(number "12")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC1")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC2")
				(number "11")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LX1")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB1")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LX2")
				(number "2")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "R-78B1.2-2.0"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78B1.2-2.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78B-2.0_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Bxx-2.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down DC/DC-Regulator, 4.75-32V input, 1.2V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78B*2.0*"
			(at 0 0 0)
		)
		(symbol "R-78B1.2-2.0_0_1")
		(symbol "R-78B1.2-2.0_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "R-78E5.0-0.5"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78E5.0-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 7-28V input, 5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
		(symbol "R-78E5.0-0.5_0_1")
		(symbol "R-78E5.0-0.5_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "R-78HB24-0.3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78HB24-0.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78HB-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78HBxx-0.5_L.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Step-Down DC/DC-Regulator, 36-72V input, 24V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78HB*0.5*"
			(at 0 0 0)
		)
		(symbol "R-78HB24-0.3_0_1")
		(symbol "R-78HB24-0.3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "R-78S3.3-0.1"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "R-78S3.3-0.1"
			(at 0 5.715 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78S-0.1_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Sxx-0.1.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA Step-Up DC/DC-Regulator, 0.65-3.15V input, 3.3V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78S*0.1*"
			(at 0 0 0)
		)
		(symbol "R-78S3.3-0.1_0_1")
		(symbol "R-78S3.3-0.1_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "4")
			)
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC4503TSK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "SC4503TSK"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "https://www.semtech.com/uploads/documents/sc4503.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.9A, 1.3MHz Step-Up DC/DC Converter, 2.5V-20V output voltage, TSOT23"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.9A 1.3MHz Step-Up DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
		(symbol "SC4503TSK_0_1")
		(symbol "SC4503TSK_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SIC437A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC437A"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/75921/sic437.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "12A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
		(symbol "SIC437A_0_1")
		(symbol "SIC437A_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "EN")
				(number "19")
			)
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "P_{GOOD}")
				(number "14")
			)
			(pin power_out line
				(at -12.7 0 0)
				(length 3.81)
				(name "V_{DD}")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "MODE1")
				(number "21")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "MODE2")
				(number "20")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "V_{IN}")
				(number "1")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "2")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "22")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "26")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "A_{GND}")
				(number "16")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "A_{GND}")
				(number "25")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "P_{GND}")
				(number "13")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "P_{GND}")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 3.81)
				(name "P_{GND}")
				(number "3")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "P_{GND}")
				(number "4")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "BOOT")
				(number "23")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "PHASE")
				(number "24")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "SW")
				(number "5")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(hide yes)
				(name "SW")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(hide yes)
				(name "SW")
				(number "7")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(hide yes)
				(name "SW")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(hide yes)
				(name "SW")
				(number "9")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "GL")
				(number "10")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(hide yes)
				(name "GL")
				(number "11")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(hide yes)
				(name "GL")
				(number "28")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "FB")
				(number "17")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "V_{OUT}")
				(number "18")
			)
			(pin power_out line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "V_{DRV}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SIC437C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC437C"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/75921/sic437.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "12A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
		(symbol "SIC437C_0_1")
		(symbol "SIC437C_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "EN")
				(number "19")
			)
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "P_{GOOD}")
				(number "14")
			)
			(pin power_in line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "V_{DRV}")
				(number "12")
			)
			(pin power_in line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "V_{DD}")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "MODE1")
				(number "21")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "MODE2")
				(number "20")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "V_{IN}")
				(number "1")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "2")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "22")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 3.81)
				(hide yes)
				(name "V_{IN}")
				(number "26")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "A_{GND}")
				(number "16")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "A_{GND}")
				(number "25")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "P_{GND}")
				(number "13")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "P_{GND}")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 3.81)
				(name "P_{GND}")
				(number "3")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "P_{GND}")
				(number "4")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "BOOT")
				(number "23")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "PHASE")
				(number "24")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "SW")
				(number "5")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(hide yes)
				(name "SW")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(hide yes)
				(name "SW")
				(number "7")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(hide yes)
				(name "SW")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(hide yes)
				(name "SW")
				(number "9")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "GL")
				(number "10")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(hide yes)
				(name "GL")
				(number "11")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(hide yes)
				(name "GL")
				(number "28")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "FB")
				(number "17")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "V_{OUT}")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST1S10PHR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 5.715 0)
		)
		(property "Value" "ST1S10PHR"
			(at -0.635 5.715 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8"
			(at 3.175 -8.89 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00169322.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A monolithic synchronous step-down regulator, Adjustable Output Voltage, 2.5-18V Input Voltage, 900kHz, PowerSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Conwerter 3A Low Voltage Input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*"
			(at 0 0 0)
		)
		(symbol "ST1S10PHR_0_1")
		(symbol "ST1S10PHR_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VINSW")
				(number "6")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "VINA")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "INH")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PADGND")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST1S10PUR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 5.715 0)
		)
		(property "Value" "ST1S10PUR"
			(at -0.635 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.5x3.6mm"
			(at 3.175 -8.89 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00169322.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A monolithic synchronous step-down regulator, Adjustable Output Voltage, 2.5-18V Input Voltage, 900kHz, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Conwerter 3A Low Voltage Input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ST1S10PUR_0_1")
		(symbol "ST1S10PUR_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VINSW")
				(number "6")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "VINA")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "INH")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PADGND")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST1S12XX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ST1S12XX"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st1s12xx.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.7A synchronous step-down regulator, Adjustable Output Voltage, 2.5-5.5V Input Voltage, 1.7MHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Converter 0.7A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "ST1S12XX_0_1")
		(symbol "ST1S12XX_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V_{IN}")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB/V_{O}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST1S14PHR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.255 8.89 0)
		)
		(property "Value" "ST1S14PHR"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8"
			(at 3.175 -8.89 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00285678.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A step-down switching regulator, Adjustable Output Voltage, 5.5-48V Input Voltage, 850kHz, PowerSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Conwerter 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*"
			(at 0 0 0)
		)
		(symbol "ST1S14PHR_0_1")
		(symbol "ST1S14PHR_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN1}")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "5")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PG")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PADGND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDN_5-0910WISM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-0910WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 4.5 to 13.2V, Output 3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
		(symbol "TDN_5-0910WISM_0_1")
		(symbol "TDN_5-0910WISM_1_1"
			(pin power_in line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "+VIN")
				(number "1")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "ON/OFF")
				(number "4")
			)
			(pin power_in line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "-VIN")
				(number "2")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "+VOUT")
				(number "7")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "-VOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL497"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TL497"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl497a.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA step up/step down/inverting switching voltage regulator, SIP-14/SOIC-14(W)"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x9.0mm*P1.27mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TL497_0_1")
		(symbol "TL497_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "Comp")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Curr_Lim")
				(number "13")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "Freq")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Inhbt")
				(number "2")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "Substrate")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "COLOUT")
				(number "10")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "Anode")
				(number "7")
			)
			(pin open_emitter line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "EMITOUT")
				(number "8")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "BASE")
				(number "11")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BaseDrv")
				(number "12")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "Cath.")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL5001"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "TL5001"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tl5001.pdf"
			(at 0 0 0)
		)
		(property "Description" "PWM Controller with wide input range, with 5% tolerance on reference. Input range 3.6-40V. Max output 50V."
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM SMPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO?8*3.9x4.9mm*P1.27mm* *DIP?8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TL5001_0_1"
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(symbol "TL5001_1_1"
			(pin output line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SCP")
				(number "5")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "DTC")
				(number "6")
			)
			(pin output line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin open_collector line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "V_{O}")
				(number "1")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "COMP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV61046ADB"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TLV61046ADB"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv61046a.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "28-V Output Voltage Boost Converter with Power Diode and Isolation Switch, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TLV61046ADB_0_1")
		(symbol "TLV61046ADB_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "VI")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV61225DC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV61225DC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv61225.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "Fixed 3.3V Output Voltage Boost Converter with Power Diode and Isolation Switch, 5uA Quiescent Current, SOT-363"
			(at 0 -22.86 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "TLV61225DC_0_1")
		(symbol "TLV61225DC_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "L")
				(number "5")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV62080DSGx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TLV62080DSGx"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 3.81 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62080.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "High-efficiency Step-down Converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WSON?8?1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TLV62080DSGx_0_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin open_collector line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "PG")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "VOS")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV62095RGTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TLV62095RGTx"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 0 19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62095.pdf"
			(at -1.27 22.86 0)
		)
		(property "Description" "High efficiency step-down converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TLV62095RGTx_0_1"
			(pin power_in line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PVIN")
				(number "11")
			)
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PVIN")
				(number "12")
			)
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "AVIN")
				(number "10")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DEF")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "9")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "CP")
				(number "7")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "CN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "15")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin power_out line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOS")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 0 180)
				(length 2.54)
				(name "PG")
				(number "4")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV62566DBVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TLV62566DBVx"
			(at 7.62 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv62565.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.7-V to 5.5-V input, PG Output, 1.5-A high efficiency step-down converter, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TLV62566DBVx_0_1")
		(symbol "TLV62566DBVx_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV62568DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV62568DBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62568.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 1A, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TLV62568DBV_0_1")
		(symbol "TLV62568DBV_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV62568DDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV62568DDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62568.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 1A, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TLV62568DDC_0_1")
		(symbol "TLV62568DDC_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV62568DRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV62568DRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62568.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 1A, SOT-563-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*563*"
			(at 0 0 0)
		)
		(symbol "TLV62568DRL_0_1")
		(symbol "TLV62568DRL_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "4")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMR_1-0511"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-0511"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, 5V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
		(symbol "TMR_1-0511_0_1")
		(symbol "TMR_1-0511_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "+VIN")
				(number "2")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "-VIN")
				(number "1")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+VOUT")
				(number "4")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "-VOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMR_1-0511SM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-0511SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, 5V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
		(symbol "TMR_1-0511SM_0_1")
		(symbol "TMR_1-0511SM_1_1"
			(pin power_in line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "+VIN")
				(number "14")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "Remote_on/off")
				(number "2")
			)
			(pin power_in line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "-VIN")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+VOUT")
				(number "8")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "-VOUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMR_1-0522"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-0522"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Dual_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "±42mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, ±12V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Dual*"
			(at 0 0 0)
		)
		(symbol "TMR_1-0522_0_1")
		(symbol "TMR_1-0522_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "+VIN")
				(number "2")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "-VIN")
				(number "1")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+VOUT")
				(number "4")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "Common")
				(number "5")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "-VOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMR_1-0522SM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "TMR_1-0522SM"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 5.08 -12.7 0)
		)
		(property "Description" "±42mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, ±12V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR-1SM*SMD*"
			(at 0 0 0)
		)
		(symbol "TMR_1-0522SM_0_1")
		(symbol "TMR_1-0522SM_1_1"
			(pin power_in line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "+VIN")
				(number "14")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "Remote_on/off")
				(number "2")
			)
			(pin power_in line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "-VIN")
				(number "1")
			)
			(pin power_out line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "+VOUT")
				(number "8")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 2.54)
				(hide yes)
				(name "Common")
				(number "6")
			)
			(pin power_out line
				(at 17.78 0 180)
				(length 2.54)
				(name "Common")
				(number "9")
			)
			(pin power_out line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "-VOUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TNY263G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY263G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 4.7W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
		(symbol "TNY263G_0_1")
		(symbol "TNY263G_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN/UV")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TNY263P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY263P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 4.7W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
		(symbol "TNY263P_0_1")
		(symbol "TNY263P_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN/UV")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TNY274G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY274G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 8.5W Output Power, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
		(symbol "TNY274G_0_1")
		(symbol "TNY274G_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN/UV")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP/M")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TNY274P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY274P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 8.5W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
		(symbol "TNY274P_0_1")
		(symbol "TNY274P_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN/UV")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP/M")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TNY284D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY284D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 8.5W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
		(symbol "TNY284D_0_1")
		(symbol "TNY284D_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN/UV")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP/M")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TNY284K"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY284K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 8.5W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
		(symbol "TNY284K_0_1")
		(symbol "TNY284K_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "13")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "9")
			)
			(pin no_connect line
				(at -2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN/UV")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP/M")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TNY284P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY284P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 8.5W Output Power, PDIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
		(symbol "TNY284P_0_1")
		(symbol "TNY284P_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN/UV")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BP/M")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP100YN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP100YN"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top100.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 20W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "TOP100YN_0_1")
		(symbol "TOP100YN_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP200YAI"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP200YAI"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top200-204214.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 12W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "TOP200YAI_0_1")
		(symbol "TOP200YAI_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP209G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP209G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top209210.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 2W Max Output Power, SMD-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8*"
			(at 0 0 0)
		)
		(symbol "TOP209G_0_1")
		(symbol "TOP209G_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP209P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP209P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top209210.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 2W Max Output Power, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TOP209P_0_1")
		(symbol "TOP209P_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP252EN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP252EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 13W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
		(symbol "TOP252EN_0_1")
		(symbol "TOP252EN_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "X")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "F")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP252GN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP252GN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 10W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
		(symbol "TOP252GN_0_1")
		(symbol "TOP252GN_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "M")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP252MN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP252MN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SDIP-10C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 10W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SDIP?10C*"
			(at 0 0 0)
		)
		(symbol "TOP252MN_0_1")
		(symbol "TOP252MN_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "9")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "X")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP252PN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP252PN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 10W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
		(symbol "TOP252PN_0_1")
		(symbol "TOP252PN_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "M")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP254YN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP254YN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:PowerIntegrations_TO-220-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 43W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations*TO?220?7C*"
			(at 0 0 0)
		)
		(symbol "TOP254YN_0_1")
		(symbol "TOP254YN_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "X")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "F")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP255LN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP255LN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 57W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
		(symbol "TOP255LN_0_1")
		(symbol "TOP255LN_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "X")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "F")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP259YN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP259YN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:PowerIntegrations_TO-220-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 171W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations*TO?220?7C*"
			(at 0 0 0)
		)
		(symbol "TOP259YN_0_1")
		(symbol "TOP259YN_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "X")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "G")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP264EG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP264EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 43W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
		(symbol "TOP264EG_0_1")
		(symbol "TOP264EG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "X")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "F")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP264KG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP264KG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 30W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
		(symbol "TOP264KG_0_1")
		(symbol "TOP264KG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "12")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "9")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "X")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "F")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOP264VG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP264VG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 43W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12*"
			(at 0 0 0)
		)
		(symbol "TOP264VG_0_1")
		(symbol "TOP264VG_1_1"
			(pin open_collector line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "12")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "S")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "9")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "X")
				(number "2")
			)
			(pin input line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "F")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TOS06-05SIL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.398 6.35 0)
		)
		(property "Value" "TOS06-05SIL"
			(at 3.556 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TOS06-05SIL_THT"
			(at -1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tos06sil.pdf"
			(at -1.27 -6.096 0)
		)
		(property "Description" "6A step-down regulator, 0.75-3.3VDC output voltage, 2.4-5.5VDC input voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated not-isolated pol dc-dc converter regulator single 6A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TOS06*05SIL*THT*"
			(at 0 0 0)
		)
		(symbol "TOS06-05SIL_0_1")
		(symbol "TOS06-05SIL_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "+Vin")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "1")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Trim")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS51363"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 19.05 0)
		)
		(property "Value" "TPS51363"
			(at 6.35 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RVE0028A_VQFN-28-1EP_3.5x4.5mm_P0.4mm_EP2.1x3.1mm"
			(at 1.27 22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps51363.pdf"
			(at 0 30.48 0)
		)
		(property "Description" "High-voltage input, synchronous converter with integrated FET, VQFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RVE0028A*"
			(at 0 0 0)
		)
		(symbol "TPS51363_0_1"
			(pin power_in line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "VIN")
				(number "15")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "16")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "17")
			)
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "V5")
				(number "18")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "28")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "TRIP")
				(number "20")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SLEW")
				(number "21")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "MODE")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NU")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NU")
				(number "27")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "PGND")
				(number "10")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "12")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "13")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "29")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin power_out line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "7")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "8")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "9")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "BST")
				(number "5")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VREF")
				(number "26")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "REFIN")
				(number "25")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "REFIN2")
				(number "24")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VSNS")
				(number "22")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GSNS")
				(number "23")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PGOOD")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS5403"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "TPS5403"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps5403.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "4.5-28V In, 3.3V Out, 1.7A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "TPS5403_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "ROSC")
				(number "3")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "LX")
				(number "8")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VSENSE")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS54061DRB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS54061DRB"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N8"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps54061.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.2A, Step Down DC-DC Converter with Low IQ, 4.5-60V Input Voltage, VSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator High Voltage Adjustable Frequency"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PVSON*"
			(at 0 0 0)
		)
		(symbol "TPS54061DRB_0_1")
		(symbol "TPS54061DRB_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RT/CLK")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "PH")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VSENSE")
				(number "5")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS5420D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS5420D"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -1.27 11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps5420.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output, 2A Step-Down Converter, 5.5V-36V Input, 500kHz Switching Frequency"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS5420D_0_1")
		(symbol "TPS5420D_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ENA")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PH")
				(number "8")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VSNS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS54233"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "TPS54233"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps54233.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "2A, Step Down DC-DC Converter with Eco-mode, 3.5-28V Input Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator High Voltage High Frequency"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
		(symbol "TPS54233_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "PH")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS54260DGQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TPS54260DGQ"
			(at 1.27 -11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP2.2x3.1mm_Mask1.83x1.89mm_ThermalVias"
			(at -2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps54260.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A, Step Down DC-DC Converter with Eco-mode, 3.5-60V Input Voltage, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS54260DGQ_0_1")
		(symbol "TPS54260DGQ_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SS/TR")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RT/CLK")
				(number "5")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "COMP")
				(number "8")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PH")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSENSE")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PWRGD")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS54302"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS54302"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps54302.pdf"
			(at -7.62 8.89 0)
		)
		(property "Description" "3A, 4.5 to 28V Input, EMI Friendly integrated switch synchronous step-down regulator, pulse-skipping, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator emi spread spectrum"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS54302_0_1")
		(symbol "TPS54302_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BOOT")
				(number "6")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS5430DDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TPS5430DDA"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8_ThermalVias"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps5430.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A, Step Down Swift Converter, Adjustable Output Voltage, 5.5-36V Input Voltage, PowerSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "TPS5430DDA_0_1")
		(symbol "TPS5430DDA_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GNDPAD")
				(number "9")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "PH")
				(number "8")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VSENSE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS54336ADDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TPS54336ADDA"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8_ThermalVias"
			(at 22.86 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps54336a.pdf"
			(at 25.4 -11.43 0)
		)
		(property "Description" "4.5V to 28V Input, 3A, Synchronous Step-Down Converter with Eco-mode(tm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "TPS54336ADDA_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "ETPAD")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "PH")
				(number "3")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VSENSE")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS54360DDA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS54360DDA"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps54360.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.5A, Step Down DC-DC Converter with Eco-mode, 4.5-60V Input Voltage, PowerSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator High Voltage High Frequency"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "TPS54360DDA_0_1")
		(symbol "TPS54360DDA_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "RT/CLK")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GNDPAD")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS54560BDDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS54560BDDA"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_R-PDSO-G8_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps54560b.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "5A, Step Down DC-DC Converter, 4.5-60V Input Voltage, Texas R-PDSO-G8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PDSO*G8*"
			(at 0 0 0)
		)
		(symbol "TPS54560BDDA_0_1")
		(symbol "TPS54560BDDA_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "6")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RT/CLK")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS560200"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TPS560200"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps560200.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "500mA, Synchronous Step-Down Converter With, Adjustable Output Voltage, 4.5-17V Input Voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS560200_0_1")
		(symbol "TPS560200_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "PH")
				(number "3")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS562200"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS562200"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps563200.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage, 4.5-17V Input Voltage, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS562200_0_1")
		(symbol "TPS562200_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "VBST")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VFB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS562202"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS562202"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps562202"
			(at 0 0 0)
		)
		(property "Description" "2A Synchronous Step-Down Voltage Regulator 580kHz, adjustable output voltage, 4.5-17V Input Voltage, 0.804V-7V Output Voltage, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
		(symbol "TPS562202_0_1")
		(symbol "TPS562202_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "VBST")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VFB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS563202S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS563202S"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps563202s.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage, 4.3-17V Input Voltage, 0.806-7V Output Voltage, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
		(symbol "TPS563202S_0_1")
		(symbol "TPS563202S_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BST")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS563300"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "TPS563300"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-583-8"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps563300.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "3.8-28V, 3A Synchronous Buck Converters with pulse frequency modulation (PFM), SOT583-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous buck converter pulse frequency modulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?583*"
			(at 0 0 0)
		)
		(symbol "TPS563300_0_1")
		(symbol "TPS563300_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "BST")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS56339DDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS56339DDC"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps56339.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.5V to 24V Input, 3-A Output Synchronous Buck Converter, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS56339DDC_0_1")
		(symbol "TPS56339DDC_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BOOT")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS56528DDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS56528DDA"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at -26.67 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps56528.pdf"
			(at -1.27 -11.43 0)
		)
		(property "Description" "5A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage 0.6-7V, 4.5-18V Input Voltage, SO-8EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
		(symbol "TPS56528DDA_0_1")
		(symbol "TPS56528DDA_1_0"
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VREG5")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PG")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
		)
		(symbol "TPS56528DDA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VBST")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VFB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS568215RNN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TPS568215RNN"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RNN0018A"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps568215.pdf"
			(at 8.89 15.24 0)
		)
		(property "Description" "4.5V-17V Input, 8A Synchronous Step-Down SWIFT Converter, Adjustable Output, 400kHz/800kHz/1.2MHz Switching Frequency, Texas VQFN-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RNN0018A*"
			(at 0 0 0)
		)
		(symbol "TPS568215RNN_0_1")
		(symbol "TPS568215RNN_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "11")
			)
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "15")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "MODE")
				(number "18")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VREG5")
				(number "17")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "12")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "3")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "8")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "7")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PGOOD")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61041DDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS61041DDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61040.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output up to 28V, 250 mA Switch Current Limit, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS61041DDC_0_1")
		(symbol "TPS61041DDC_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61041DRV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS61041DRV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61040.pdf"
			(at 3.81 8.89 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output up to 28V, 250 mA Switch Current Limit, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS61041DRV_0_1")
		(symbol "TPS61041DRV_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61085DGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "TPS61085DGK"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 22.86 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps61085.pdf"
			(at 0 0 0)
		)
		(property "Description" "Step-Up DC-DC Converter, input 2.3V to 6V , output 2.8V to 18.5, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost converter switching VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS61085DGK_0_1")
		(symbol "TPS61085DGK_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FREQ")
				(number "7")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "COMP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61089"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TPS61089"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_VQFN-RNR0011A-11"
			(at 22.86 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61089.pdf"
			(at 0 0 0)
		)
		(property "Description" "7A Boost Converters, Adjustable output voltage (PFM), input 2.7 to 12V , output 4.5 to 12.6V, VQFN-11"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 7A boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN?RNR0011A?11*"
			(at 0 0 0)
		)
		(symbol "TPS61089_0_1")
		(symbol "TPS61089_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SW")
				(number "11")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "BOOT")
				(number "10")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FSW")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VIN")
				(number "9")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "COMP")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ILIM")
				(number "8")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61090"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "TPS61090"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm_ThermalVias"
			(at -24.13 -26.67 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61090.pdf"
			(at 3.81 -29.21 0)
		)
		(property "Description" "2A Step-Up DC-DC Converter for Batteries, Isw up to 2500mA, Adjustable output voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 2A battery boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "TPS61090_0_0"
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SW")
				(number "4")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VBAT")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "11")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "LBI")
				(number "9")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "7")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin power_out line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VOUT")
				(number "15")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "16")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "LBO")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
		)
		(symbol "TPS61090_0_1")
		(embedded_fonts no)
	)
	(symbol "TPS61099DRV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS61099DRV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TPS61099"
			(at 0 2.54 0)
		)
		(property "Description" "Boost Converter, 0.7-5.5V Input Voltage, 1A Switch Current, Adjustable 1.8-5.5V Output Voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS61099DRV_0_1")
		(symbol "TPS61099DRV_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "VI")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61200DRC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TPS61200DRC"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61200.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Input Voltage Synchronous Boost Converter With 1.3A Switches, Adjustable Output Voltage, 0.3-5.5V Input Voltage, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PVSON*N10*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "TPS61200DRC_0_1")
		(symbol "TPS61200DRC_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "PS")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "UVLO")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "L")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "VAUX")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61202DSC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TPS61202DSC"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_DSC0010J_ThermalVias"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61200.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Input Voltage Synchronous Boost Converter With 1.3A Switches, Fixed 5V Output Voltage, 0.3-5.5V Input Voltage, WSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSC0010J*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "TPS61202DSC_0_1")
		(symbol "TPS61202DSC_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "PS")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "UVLO")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "L")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "VAUX")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61220DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS61220DCK"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61220.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "400 mA Step-Up Converter, Adjustable Output Voltage, 0.7-5.5V Input Voltage, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost adjustable converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PDSO*G6*"
			(at 0 0 0)
		)
		(symbol "TPS61220DCK_0_1")
		(symbol "TPS61220DCK_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "L")
				(number "5")
			)
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61230DRC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS61230DRC"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 2.54 35.56 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61232.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "High Efficiency Synchronous Step Up Converters with 5-A Switches, 2.3-5.5V Input Voltage, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost converter switching adjustable 5A-switch VSON-10"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PVSON*N10*"
			(at 0 0 0)
		)
		(symbol "TPS61230DRC_0_1")
		(symbol "TPS61230DRC_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "9")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "HYS")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61252DSG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "TPS61252DSG"
			(at 10.16 10.16 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 1.27 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61252.pdf"
			(at 0 0 0)
		)
		(property "Description" "Tiny 1.5-A Boost Converter With Adjustable Input Current Limit, 2.3-6.0V Vin, 3.0-6.5V Vout, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost converter switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS61252DSG_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ILIM")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS613221ADBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613221ADBV"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1.2A Step-Up Converter, 3.3V Output Voltage, 0.9-5.5V Input Voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS613221ADBV_0_1")
		(symbol "TPS613221ADBV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS613221ADBZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613221ADBZ"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1.2A Step-Up Converter, 3.3V Output Voltage, 0.9-5.5V Input Voltage, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS613221ADBZ_0_1")
		(symbol "TPS613221ADBZ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61322DBZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS61322DBZ"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "750mA Step-Up Converter, 2.2V Output Voltage, 0.9-5.5V Input Voltage, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS61322DBZ_0_1")
		(symbol "TPS61322DBZ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62056DGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "TPS62056DGS"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 22.86 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62056.pdf"
			(at 1.27 -1.27 0)
		)
		(property "Description" "800 mA Step-Down Converter, Adjustable Output Voltage, 0.7-6V Input Voltage, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage regulator switch mode step down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS62056DGS_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "LBI")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "10")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SW")
				(number "9")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LBO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62130"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62130"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62130.pdf"
			(at 27.94 -13.97 0)
		)
		(property "Description" "3A Step-Down Converter with DCS-Control, Adjustable Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS62130_0_1")
		(symbol "TPS62130_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "13")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SS/TR")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DEF")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FSW")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "11")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOS")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "4")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62160DGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62160DGK"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62160.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, adjustable output, 3-17V input voltage, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS62160DGK_0_1")
		(symbol "TPS62160DGK_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PG")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOS")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62170DSG"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62170DSG"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62170.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "500mA Step-Down Converter with DCS-Control, adjustable output, 3-17V input voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS62170DSG_0_1")
		(symbol "TPS62170DSG_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PG")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOS")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62177DQC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62177DQC"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-10-1EP_2x3mm_P0.5mm_EP0.84x2.4mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62177.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "500mA Step-Down Converter with Sleep Mode, fixed 3.3V Output Voltage, 4.75-28V input voltage, WSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS62177DQC_0_1")
		(symbol "TPS62177DQC_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "8")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PG")
				(number "7")
			)
			(pin passive line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOS")
				(number "10")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62200DBV"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS62200DBV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62201.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA High-Efficiency Step-Down DC-DC Converter, adjustable output voltage, 2.5-6V input voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS62200DBV_0_1")
		(symbol "TPS62200DBV_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62823DLC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62823DLC"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_VSON-HR-8_1.5x2mm_P0.5mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62823.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "3A Step-Down Converter with DCS-Control, adjustable output, 2.4-5.5V input voltage, QFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VSON*HR*1.5x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS62823DLC_0_1")
		(symbol "TPS62823DLC_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PG")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "AGND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS628436DRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS628436DRL"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62843.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "600mA Step-Down Converter with DCS-Control, ultra-low Iq, 1.8-5.5 Vin, 0.4-0.8 Vout, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
		(symbol "TPS628436DRL_0_1")
		(symbol "TPS628436DRL_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VSET")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOS")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS628436YKA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS628436YKA"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-6_0.757x1.01mm_Layout2x3_P0.35mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62843.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "600mA Step-Down Converter with DCS-Control, ultra-low Iq, 1.8-5.5 Vin, 0.4-0.8 Vout, WLCSP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*0.757x1.01mm*Layout2x3*P0.35mm*"
			(at 0 0 0)
		)
		(symbol "TPS628436YKA_0_1")
		(symbol "TPS628436YKA_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "B1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "C2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VSET")
				(number "C1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "A1")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "B2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOS")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62912"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TPS62912"
			(at 5.334 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RPU0010A_VQFN-HR-10_2x2mm_P0.5mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62912.pdf"
			(at 0 -25.654 0)
		)
		(property "Description" "2.2MHz or 1MHz, 2A, Low Noise, Low Ripple, Buck Converter with Integrated Ferrite Bead Filter Compensation, VQFN-HR"
			(at 0 -27.94 0)
		)
		(property "ki_keywords" "step-down high psrr adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Texas*RPU0010A*"
			(at 0 0 0)
		)
		(symbol "TPS62912_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN/SYNC")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "S-CONF")
				(number "10")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "NR/SS")
				(number "8")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PSNS")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "9")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62933"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "TPS62933"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-583-8"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62933.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "3.8-30V, 3A Synchronous Buck Converters with pulse frequency modulation (PFM), SOT583-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous buck converter pulse frequency modulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?583*"
			(at 0 0 0)
		)
		(symbol "TPS62933_0_1")
		(symbol "TPS62933_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "BST")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62933P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "TPS62933P"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-583-8"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62933.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "3.8-30V, 3A Synchronous Buck Converters with pulse frequency modulation (PFM) and power good, SOT583-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous buck converter pulse frequency modulation power good"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?583*"
			(at 0 0 0)
		)
		(symbol "TPS62933P_0_1")
		(symbol "TPS62933P_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin open_collector line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "PG")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "BST")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62A01DRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A01DRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a01"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 1A, Power Good, Enable, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
		(symbol "TPS62A01DRL_0_1")
		(symbol "TPS62A01DRL_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62A01PDDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A01PDDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a01"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 1A, Power Good, Enable, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?6*"
			(at 0 0 0)
		)
		(symbol "TPS62A01PDDC_0_1")
		(symbol "TPS62A01PDDC_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS62A02NDRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A02NDRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a02"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 2A, Enable, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
		(symbol "TPS62A02NDRL_0_1")
		(symbol "TPS62A02NDRL_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "2")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS63000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPS63000"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_DRC0010J_ThermalVias"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63000.pdf"
			(at -7.62 13.97 0)
		)
		(property "Description" "Buck-Boost Converter, 1.8-5.5V Input Voltage, 1.8A Switch Current, Adjustable 1.2-5.5V Output Voltage, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost adjustable converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRC0010J*"
			(at 0 0 0)
		)
		(symbol "TPS63000_0_1")
		(symbol "TPS63000_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VINA")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PS/SYNC")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "L1")
				(number "4")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "L2")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS63030DSK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPS63030DSK"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:WSON-10-1EP_2.5x2.5mm_P0.5mm_EP1.2x2mm"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63030.pdf"
			(at -7.62 13.97 0)
		)
		(property "Description" "Buck-Boost Converter, 1.8-5.5V Input Voltage, 1A Switch Current, Adjustable Output Voltage, VSON-10 (DSK0010A)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost adjustable converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2.5x2.5mm*P0.5mm*EP1.2x2mm*"
			(at 0 0 0)
		)
		(symbol "TPS63030DSK_0_1")
		(symbol "TPS63030DSK_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VINA")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PS/SYNC")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "L1")
				(number "4")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "L2")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS63060"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPS63060"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PWSON-N10_ThermalVias"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63060.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "Buck-Boost Converter, 2.5-12V Input Voltage, 2-A Switch Current, Adjustable 2.5-8V Output Voltage, S-PWSON-N10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost adjustable converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PWSON*N10*"
			(at 0 0 0)
		)
		(symbol "TPS63060_0_1")
		(symbol "TPS63060_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PS/SYNC")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "L1")
				(number "1")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "L2")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "11")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VOUT")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VAUX")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS63061"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPS63061"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PWSON-N10_ThermalVias"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63060.pdf"
			(at -1.27 -19.05 0)
		)
		(property "Description" "Buck-Boost Converter, 2.5-12V Input Voltage, 2-A Switch Current, Fixed 5V Output Voltage, S-PWSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost converter 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PWSON*N10*"
			(at 0 0 0)
		)
		(symbol "TPS63061_0_1")
		(symbol "TPS63061_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PS/SYNC")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "L1")
				(number "1")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "L2")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "11")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VOUT")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VAUX")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS63900"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPS63900"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:WSON-10-1EP_2.5x2.5mm_P0.5mm_EP1.2x2mm_ThermalVias"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps63900.pdf"
			(at -7.62 13.97 0)
		)
		(property "Description" "Buck-Boost Converter, 1.8-5.5V Input Voltage, 0.4A Switch Current, Adjustable 1.8-5V Output Voltage, WSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost adjustable converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*10*1EP*2.5x2.5*P0.5*"
			(at 0 0 0)
		)
		(symbol "TPS63900_0_1")
		(symbol "TPS63900_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SEL")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "LX1")
				(number "9")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "LX2")
				(number "7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CFG1")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CFG2")
				(number "4")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CFG3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS65130RGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.858 21.082 0)
		)
		(property "Value" "TPS65130RGE"
			(at -1.016 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps65130.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Split-Rail Converter with Dual, Positive and Negative Outputs (300mA typ, Switch Current Limit 800mA typ), 2.7-5.5V, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "split-rail switching dual positive negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS65130RGE_0_1")
		(symbol "TPS65130RGE_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "INP")
				(number "1")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(hide yes)
				(name "INP")
				(number "24")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "BSW")
				(number "7")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INN")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "INN")
				(number "6")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ENP")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PSP")
				(number "9")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ENN")
				(number "10")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PSN")
				(number "11")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "AGND")
				(number "19")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "PGND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "3")
			)
			(pin input line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "VPOS")
				(number "23")
			)
			(pin input line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "FBP")
				(number "22")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VREF")
				(number "17")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "FBN")
				(number "16")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "VNEG")
				(number "15")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTN")
				(number "13")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUTN")
				(number "14")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CN")
				(number "18")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "CP")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS82130"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 11.43 0)
		)
		(property "Value" "TPS82130"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_LGA:Texas_SIL0008D_MicroSiP-8-1EP_2.8x3mm_P0.65mm_EP1.1x1.9mm_ThermalVias"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps82130.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "17V Input 3A Step-Down Converter MicroSiP Module with Integrated Inductor, μSiL-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "17V 3A Step-down Buck Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroSiP*1EP*2.8x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS82130_0_1")
		(symbol "TPS82130_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PG")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SS/TR")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSR_1-2450"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-2450"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 5V output voltage, 5-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
		(symbol "TSR_1-2450_0_1")
		(symbol "TSR_1-2450_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VIPer22ADIP-E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "VIPer22ADIP-E"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.st.com/web/en/resource/technical/document/datasheet/CD00087939.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power OFF-line SMPS primary switcher"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "VIPer22ADIP-E_0_0"
			(text "CTRL"
				(at -0.635 0 0)
			)
		)
		(symbol "VIPer22ADIP-E_0_1")
		(symbol "VIPer22ADIP-E_1_1"
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin power_in line
				(at -7.62 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VIPer22AS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "VIPer22AS"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.st.com/web/en/resource/technical/document/datasheet/CD00087939.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power OFF-line SMPS primary switcher"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "VIPer22AS_0_0"
			(text "CTRL"
				(at -0.635 0 0)
			)
		)
		(symbol "VIPer22AS_0_1")
		(symbol "VIPer22AS_1_1"
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin power_in line
				(at -7.62 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VIPer25LN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "VIPer25LN"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00231127.pdf"
			(at 0 0 0)
		)
		(property "Description" "12W SMPS Controller, AC-DC, PDIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET 12W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PDIP*8B*"
			(at 0 0 0)
		)
		(symbol "VIPer25LN_0_0"
			(text "CTRL"
				(at -1.905 -0.127 0)
			)
		)
		(symbol "VIPer25LN_0_1")
		(symbol "VIPer25LN_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BR")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ZCD")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin input line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "FB")
				(number "4")
			)
			(pin passive line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VIPer26LD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 12.7 0)
		)
		(property "Value" "VIPer26LD"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/viper26.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V, 10-20W, 60kHz, SMPS Controller, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "VIPer26LD_0_1")
		(symbol "VIPer26LD_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "NA")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "LIM")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "DRAIN")
				(number "13")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "DRAIN")
				(number "14")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "DRAIN")
				(number "15")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DRAIN")
				(number "16")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VIPer26LN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 12.7 0)
		)
		(property "Value" "VIPer26LN"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N6_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/viper26.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V, 10-20W, 60kHz, SMPS Controller, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N6*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "VIPer26LN_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "LIM")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "DRAIN")
				(number "7")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DRAIN")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XL1509-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 6.096 0)
		)
		(property "Value" "XL1509-3.3"
			(at 5.842 6.096 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.382 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1809050422_XLSEMI-XL1509-5-0E1_C61063.pdf"
			(at 2.54 10.668 0)
		)
		(property "Description" "Buck DC/DC Converter, 2A, 3.3V Output Voltage, 4.5-40V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck DC/DC converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "XL1509-3.3_0_1")
		(symbol "XL1509-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XL4015"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at -6.35 6.35 0)
		)
		(property "Value" "XL4015"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 21.59 -7.62 0)
		)
		(property "Datasheet" "http://www.xlsemi.net/datasheet/XL4015%20datasheet-English.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 180kHz 36V Buck DC to DC Converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck DC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "XL4015_0_1")
		(symbol "XL4015_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AAT1217ICA-3.3"
		(extends "AAT1217ICA-1.2")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AAT1217ICA-3.3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/AAT1217_202050B.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA, 3.3V, 1.2MHz, Micropower Synchronous Step-Up Converter, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AAT1217ICA-5.0"
		(extends "AAT1217ICA-1.2")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AAT1217ICA-5.0"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.skyworksinc.com/uploads/documents/AAT1217_202050B.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA, 5.0V, 1.2MHz, Micropower Synchronous Step-Up Converter, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP1108AN"
		(extends "LT1073CN")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "ADP1108AN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, adjustable output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP1108AN-12"
		(extends "LT1073CN-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "ADP1108AN-12"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, 12V fixed output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP1108AN-3.3"
		(extends "LT1073CN-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "ADP1108AN-3.3"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, 3.3V fixed output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP1108AN-5"
		(extends "LT1073CN-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "ADP1108AN-5"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, 5V fixed output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP1108AR"
		(extends "LT1073CS")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "ADP1108AR"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, adjustable output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP1108AR-12"
		(extends "LT1073CS-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "ADP1108AR-12"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, 12V fixed output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP1108AR-3.3"
		(extends "LT1073CS-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "ADP1108AR-3.3"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, 3.3V fixed output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP1108AR-5"
		(extends "LT1073CS-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "ADP1108AR-5"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, 5V fixed output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-1.1"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-1.1"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 1.1V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-1.2"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-1.2"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 1.2V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-1.3"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-1.3"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 1.3V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-1.5"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-1.5"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 1.5V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-1.8"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-1.8"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 1.8V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-1.82"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-1.82"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 1.82V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-2.3"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-2.3"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 2.3V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-2.5"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-2.5"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 2.5V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-3.0"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-3.0"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 3.0V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2108AUJ-3.3"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ADP2108AUJ-3.3"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "3MHz switching bucK regulator, 600mA 3.3V output voltage,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2302ARDZ-2.5"
		(extends "ADP2302ARDZ")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADP2302ARDZ-2.5"
			(at -3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2302_2303.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Nonsynchronous Step-Down Regulator 2 Amp Vout 2.5v SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2302ARDZ-3.3"
		(extends "ADP2302ARDZ")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADP2302ARDZ-3.3"
			(at -3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2302_2303.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Nonsynchronous Step-Down Regulator 2 Amp Vout 3.3v SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2302ARDZ-5.0"
		(extends "ADP2302ARDZ")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADP2302ARDZ-5.0"
			(at -3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2302_2303.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Nonsynchronous Step-Down Regulator 2 Amp Vout 5.0v SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2303ARDZ"
		(extends "ADP2302ARDZ")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADP2303ARDZ"
			(at -3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2302_2303.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Nonsynchronous Step-Down Regulator 3 Amp Vout Adjustable SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2303ARDZ-2.5"
		(extends "ADP2302ARDZ")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADP2303ARDZ-2.5"
			(at -3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2302_2303.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Nonsynchronous Step-Down Regulator 3 Amp Vout 2.5v SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2303ARDZ-3.3"
		(extends "ADP2302ARDZ")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADP2303ARDZ-3.3"
			(at -3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2302_2303.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Nonsynchronous Step-Down Regulator 3 Amp Vout 3.3v SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2303ARDZ-5.0"
		(extends "ADP2302ARDZ")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADP2303ARDZ-5.0"
			(at -3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2302_2303.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Nonsynchronous Step-Down Regulator 3 Amp Vout 5.0v SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2360xCP-3.3"
		(extends "ADP2360xCP")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ADP2360xCP-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-WD-8-1EP_3x3mm_P0.65mm_EP1.6x2.44mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2360.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "High Efficiency Buck Regulator, Vin 60V, Vout 3.3V, 50mA, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP2360xCP-5.0"
		(extends "ADP2360xCP")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ADP2360xCP-5.0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-WD-8-1EP_3x3mm_P0.65mm_EP1.6x2.44mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2360.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "High Efficiency Buck Regulator, Vin 60V, Vout 5.0V, 50mA, LFCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP5071AREZ"
		(extends "ADP5070AREZ")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "ADP5071AREZ"
			(at 12.7 24.13 0)
		)
		(property "Footprint" "Package_SO:ETSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3x4.2mm"
			(at 1.27 -25.4 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP5071.pdf"
			(at 1.27 -27.94 0)
		)
		(property "Description" "2A/1.2A DC-to-DC Switching Regulator with Independent Positive and Negative Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage regulator switching inverter double positive negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ETSSOP*1EP?4.4x6.5mm?P0.65mm?EP3x4.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "AOZ1282CI"
		(extends "AOZ1280CI")
		(property "Reference" "U"
			(at -6.35 -6.35 0)
		)
		(property "Value" "AOZ1282CI"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "http://aosmd.com/res/data_sheets/AOZ1282CI.pdf"
			(at -6.35 -6.35 0)
		)
		(property "Description" "1.2 A Simple Buck Regulator, 4.5-36V input, 450kHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AOZ1282CI-1"
		(extends "AOZ1280CI")
		(property "Reference" "U"
			(at -6.35 -6.35 0)
		)
		(property "Value" "AOZ1282CI-1"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "http://www.aosmd.com/res/data_sheets/AOZ1282CI-1.pdf"
			(at -6.35 -6.35 0)
		)
		(property "Description" "600 mA Simple Buck Regulator, 4.5-36V input, 1MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AOZ6663DI-01"
		(extends "AOZ6663DI")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "AOZ6663DI-01"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:AO_AOZ666xDI_DFN-8-1EP_3x3mm_P0.65mm_EP1.25x2.7mm"
			(at -0.635 -11.43 0)
		)
		(property "Datasheet" "http://aosmd.com/res/data_sheets/AOZ6663DI.pdf"
			(at 2.54 -11.43 0)
		)
		(property "Description" "3A Buck Regulator, 4.5-18V input, 750kHz,  fixed frequency on light load <= 4V, pulse energy mode on light load > 4V,DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AP3012"
		(extends "SC4503TSK")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "AP3012"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3012.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA, Adjustable Step-Up Voltage Regulator, 1.5MHz Frequency, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP62250WU"
		(extends "AP62150WU")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP62250WU"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP62250.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "2.5A, 1.3MHz Buck DC/DC Converter, 4.2V-18V input voltage, 0.8V-7V adjustable output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.5A 1.3MHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "AP62250Z6"
		(extends "AP62150Z6")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP62250Z6"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP62250.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A, 1.3MHz Buck DC/DC Converter, adjustable output voltage, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.5A 1.3MHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "AP62300TWU"
		(extends "AP62300WU")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP62300TWU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP62300_AP62301_AP62300T.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A, 750kHz Buck DC/DC Converter, PFM for light load efficiency, 4.2V-18V input voltage, 0.8V-7V adjustable output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP62300Z6"
		(extends "AP62150Z6")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP62300Z6"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP62300_AP62301_AP62300T.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A, 1.3MHz Buck DC/DC Converter, adjustable output voltage, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A 1.3MHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "AP62301WU"
		(extends "AP62300WU")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP62301WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP62300_AP62301_AP62300T.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A, 750kHz Buck DC/DC Converter, 4.2V-18V input voltage, 0.8V-7V adjustable output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP63201WU"
		(extends "AP63200WU")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP63201WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP63200-AP63201-AP63203-AP63205.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 500kHz Buck DC/DC Converter, adjustable output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "2A Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP63203WU"
		(extends "AP63200WU")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP63203WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP63200-AP63201-AP63203-AP63205.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 1.1MHz Buck DC/DC Converter, fixed 3.3V output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "2A Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP63205WU"
		(extends "AP63200WU")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP63205WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP63200-AP63201-AP63203-AP63205.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 1.1MHz Buck DC/DC Converter, fixed 5.0V output voltage, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "2A Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP6503"
		(extends "AP6502")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "AP6503"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 16.51 -13.97 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP6503.pdf"
			(at 0 3.81 0)
		)
		(property "Description" "340kHz 23V 3A Synchonous DC/DC Buck Converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck switching converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes_SO-8EP*"
			(at 0 0 0)
		)
	)
	(symbol "APE1707H-12-HF"
		(extends "APE1707H-33-HF")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707H-12-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://pdf.datasheet.live/datasheets-1/advanced_power_electronics/APE1707H-12-HF.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, fixed 12.0V output voltage, TO-252-5 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "APE1707H-50-HF"
		(extends "APE1707H-33-HF")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707H-50-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://pdf.datasheet.live/datasheets-1/advanced_power_electronics/APE1707H-12-HF.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, fixed 5.0V output voltage, TO-252-5 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "APE1707H-HF"
		(extends "APE1707H-33-HF")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707H-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://pdf.datasheet.live/datasheets-1/advanced_power_electronics/APE1707H-12-HF.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, adjustable output voltage, TO-252-5 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "APE1707M-12-HF"
		(extends "APE1707M-33-HF")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707M-12-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://files.remont-aud.net/baza/dc_dc/data/APE1707.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, fixed 12.0V output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "APE1707M-50-HF"
		(extends "APE1707M-33-HF")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707M-50-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://files.remont-aud.net/baza/dc_dc/data/APE1707.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, fixed 5.0V output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "APE1707M-HF"
		(extends "APE1707M-33-HF")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707M-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://files.remont-aud.net/baza/dc_dc/data/APE1707.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, adjustable output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "APE1707S-12-HF"
		(extends "APE1707S-33-HF")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707S-12-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://pdf.datasheet.live/datasheets-1/advanced_power_electronics/APE1707S-12-HF.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, fixed 12.0V output voltage, TO-263-5 (DD-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "APE1707S-50-HF"
		(extends "APE1707S-33-HF")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707S-50-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://pdf.datasheet.live/datasheets-1/advanced_power_electronics/APE1707S-12-HF.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, fixed 5.0V output voltage, TO-263-5 (DD-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "APE1707S-HF"
		(extends "APE1707S-33-HF")
		(property "Reference" "U"
			(at -7.62 5.715 0)
		)
		(property "Value" "APE1707S-HF"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://pdf.datasheet.live/datasheets-1/advanced_power_electronics/APE1707S-12-HF.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 150KHz PWM Buck DC/DC Converter, adjustable output voltage, TO-263-5 (DD-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 2A 150KHz PWM Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "CRE1S0305S3C"
		(extends "CRE1S0505S3C")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CRE1S0305S3C"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_CRE1xxxxxx3C_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://power.murata.com/datasheet?/data/power/ncl/kdc_cre1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "3.3V to 5V 200mA, Isolated 2W Single-Output DC-DC Converter Modules with 3kV isolation, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*CRE1xxxxxx3C*"
			(at 0 0 0)
		)
	)
	(symbol "CRE1S0515SC"
		(extends "CRE1S0505SC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CRE1S0515SC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_CRE1xxxxxxSC_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://power.murata.com/datasheet?/data/power/ncl/kdc_cre1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "15V to 5V 67mA DC-DC Converter with 1kV isolation, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*CRE1xxxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "CRE1S1205SC"
		(extends "CRE1S0505SC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CRE1S1205SC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_CRE1xxxxxxSC_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://power.murata.com/datasheet?/data/power/ncl/kdc_cre1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "12V to 5V 200mA DC-DC Converter with 1kV isolation, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*CRE1xxxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "CRE1S1212SC"
		(extends "CRE1S0505SC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CRE1S1212SC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_CRE1xxxxxxSC_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://power.murata.com/datasheet?/data/power/ncl/kdc_cre1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "12V to 12V 83mA DC-DC Converter with 1kV isolation, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*CRE1xxxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "CRE1S2405SC"
		(extends "CRE1S0505SC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CRE1S2405SC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_CRE1xxxxxxSC_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://power.murata.com/datasheet?/data/power/ncl/kdc_cre1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "24V to 5V 200mA DC-DC Converter with 1kV isolation, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*CRE1xxxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "CRE1S2412SC"
		(extends "CRE1S0505SC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CRE1S2412SC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_CRE1xxxxxxSC_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://power.murata.com/datasheet?/data/power/ncl/kdc_cre1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "24V to 12V 83mA DC-DC Converter with 1kV isolation, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*CRE1xxxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "FSBH0170A"
		(extends "FSBH0F70A")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FSBH0170A"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSBH0270-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Green Mode Fairchild Power Switch, 700V Vds, 1.0A Id, 15W/13W 230V/85-265V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSBH0170W"
		(extends "FSBH0170")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FSBH0170W"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FSBH0270W-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Green Mode Fairchild Power Switch, 700V Vds, 1.0A Id, 15W/13W 230V/85-265V, VIN Pin, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSBH0270"
		(extends "FSBH0170")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FSBH0270"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSBH0270-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Green Mode Fairchild Power Switch, 700V Vds, 2.0A Id, 20W/16W 230V/85-265V, VIN Pin, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSBH0270A"
		(extends "FSBH0F70A")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FSBH0270A"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSBH0270-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Green Mode Fairchild Power Switch, 700V Vds, 2.0A Id, 20W/16W 230V/85-265V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSBH0270W"
		(extends "FSBH0170")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FSBH0270W"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FSBH0270W-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Green Mode Fairchild Power Switch, 700V Vds, 2.0A Id, 20W/16W 230V/85-265V, VIN Pin, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSBH0370"
		(extends "FSBH0170")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FSBH0370"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSBH0270-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Green Mode Fairchild Power Switch, 700V Vds, 3.0A Id, 25W/19W 230V/85-265V, VIN Pin, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSBH0F70WA"
		(extends "FSBH0F70A")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "FSBH0F70WA"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FSBH0270W-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Green Mode Fairchild Power Switch, 700V Vds, 0.5A Id, 10W/8W 230V/85-265V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSDL321"
		(extends "FSDH321")
		(property "Reference" "U"
			(at 10.16 6.35 0)
		)
		(property "Value" "FSDL321"
			(at 10.16 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 10.16 1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSDH321JP-D.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "17W SMPS Controller, 50kHz, AC-DC, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET 17W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FSDL321L"
		(extends "FSDH321L")
		(property "Reference" "U"
			(at 10.16 6.35 0)
		)
		(property "Value" "FSDL321L"
			(at 10.16 3.81 0)
		)
		(property "Footprint" "Package_DIP:Fairchild_LSOP-8"
			(at 10.16 1.27 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSDH321JP-D.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "17W SMPS Controller, 50kHz, AC-DC, SMD-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET 17W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*LSOP*"
			(at 0 0 0)
		)
	)
	(symbol "FSQ0565RQLDTU"
		(extends "FSQ0565RSWDTU")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "FSQ0565RQLDTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:Fairchild_TO-220F-6L"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FSQ0565RS-D.PDF"
			(at 1.905 0 0)
		)
		(property "Description" "67kHz Quasi Resonant SMPS Controller w/ Soft Start, max. 80W AC-DC, TO-220F-6L (Formed)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quasi Resonant SMPS Controller 80W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*TO*220F*6L*"
			(at 0 0 0)
		)
	)
	(symbol "FSQ0565RQWDTU"
		(extends "FSQ0565RSWDTU")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "FSQ0565RQWDTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:Fairchild_TO-220F-6L"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FSQ0565RS-D.PDF"
			(at 1.905 0 0)
		)
		(property "Description" "67kHz Quasi Resonant SMPS Controller w/ Soft Start, max. 80W AC-DC, TO-220F-6L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quasi Resonant SMPS Controller 80W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*TO*220F*6L*"
			(at 0 0 0)
		)
	)
	(symbol "FSQ0565RSLDTU"
		(extends "FSQ0565RSWDTU")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "FSQ0565RSLDTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:Fairchild_TO-220F-6L"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FSQ0565RS-D.PDF"
			(at 1.905 0 0)
		)
		(property "Description" "67kHz Quasi Resonant SMPS Controller w/ Soft Start, max. 80W AC-DC, TO-220F-6L (Formed)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quasi Resonant SMPS Controller 80W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*TO*220F*6L*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-12SF8DR"
		(extends "GL2576-3.3SF8DR")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-12SF8DR"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "12V 3A, 52KHz Step Down Converter, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-12TA5R"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-12TA5R"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 3A, 52KHz Step Down Converter, TO263-5 (D2-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-12TB5T"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-12TB5T"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 3A, 52KHz Step Down Converter, TO220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-15SF8DR"
		(extends "GL2576-3.3SF8DR")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-15SF8DR"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "15V 3A, 52KHz Step Down Converter, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "15V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-15TA5R"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-15TA5R"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V 3A, 52KHz Step Down Converter, TO263-5 (D2-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "15V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-15TB5T"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-15TB5T"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V 3A, 52KHz Step Down Converter, TO220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "15V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-3.3TA5R"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-3.3TA5R"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 3A, 52KHz Step Down Converter, TO263-5 (D2-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-3.3TB5T"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-3.3TB5T"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 3A, 52KHz Step Down Converter, TO220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-5.0SF8DR"
		(extends "GL2576-3.3SF8DR")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-5.0SF8DR"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "5V 3A, 52KHz Step Down Converter, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-5.0TA5R"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-5.0TA5R"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 3A, 52KHz Step Down Converter, TO263-5 (D2-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-5.0TB5T"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-5.0TB5T"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 3A, 52KHz Step Down Converter, TO220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-ASF8DR"
		(extends "GL2576-3.3SF8DR")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-ASF8DR"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "Adjustable 3A, 52KHz Step Down Converter, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-ATA5R"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-ATA5R"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable 3A, 52KHz Step Down Converter, TO263-5 (D2-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "GL2576-ATB5T"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "GL2576-ATB5T"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.dianyuan.com/bbs/u/54/437861181916300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable 3A, 52KHz Step Down Converter, TO220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 3A 52KHz Buck DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "HT7463B"
		(extends "HT7463A")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "HT7463B"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://www.holtek.com/documents/10179/116711/HT7463A_Bv160.pdf"
			(at 5.08 -16.51 0)
		)
		(property "Description" "52V/600mA, 550kHz Asynchronous Step Down Converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "600mA Buck DC/DC 52V 550kHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
	)
	(symbol "KA5H0280RTU"
		(extends "KA5M0265RTU")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5H0280RTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-4_Vertical"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "100kHz SMPS Controller, AC-DC, TO-220F-4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*4*"
			(at 0 0 0)
		)
	)
	(symbol "KA5H0280RYDTU"
		(extends "KA5M0265RYDTU")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5H0280RYDTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:ONSemi_TO-220F-4L_Forming"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "100kHz SMPS Controller, AC-DC, TO-220F-4L(Forming)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*4*"
			(at 0 0 0)
		)
	)
	(symbol "KA5L0265RTU"
		(extends "KA5M0265RTU")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5L0265RTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-4_Vertical"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "50kHz SMPS Controller, AC-DC, TO-220F-4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*4*"
			(at 0 0 0)
		)
	)
	(symbol "KA5L0265RYDTU"
		(extends "KA5M0265RYDTU")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5L0265RYDTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:ONSemi_TO-220F-4L_Forming"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "50kHz SMPS Controller, AC-DC, TO-220F-4L(Forming)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*4*"
			(at 0 0 0)
		)
	)
	(symbol "KA5M02659RN"
		(extends "KA5H02659RN")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5M02659RN"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "67kHz SMPS Controller, AC-DC, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "KA5M0280RTU"
		(extends "KA5M0265RTU")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5M0280RTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-4_Vertical"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "67kHz SMPS Controller, AC-DC, TO-220F-4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*4*"
			(at 0 0 0)
		)
	)
	(symbol "KA5M0280RYDTU"
		(extends "KA5M0265RYDTU")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "KA5M0280RYDTU"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:ONSemi_TO-220F-4L_Forming"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/KA5L0265R-D.PDF"
			(at 1.27 0 0)
		)
		(property "Description" "KA5M0280RTDTU, 67kHz SMPS Controller, AC-DC, TO-220F-4L(Forming)"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TO*220*4*"
			(at 0 0 0)
		)
	)
	(symbol "L4962EH-A"
		(extends "L4962E-A")
		(property "Reference" "U"
			(at -14.224 11.684 0)
		)
		(property "Value" "L4962EH-A"
			(at 9.144 11.684 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-7_P2.54x5.1mm_StaggerOdd_Lead8.025mm_TabDown"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/389/cd00000076-1795191.pdf"
			(at -0.508 -24.384 0)
		)
		(property "Description" "1.5A Power Switching Regulator, 9..46V input, 5.1..40V output, 150 kHz, TO-220-7 (Heptawatt H)"
			(at 0 -22.352 0)
		)
		(property "ki_keywords" "buck step-down dc-dc converter L4962EH/A Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*P2.54x5.1*StaggerOdd*Lead8.025*TabDown*"
			(at 0 0 0)
		)
	)
	(symbol "LGS5145"
		(extends "LGS5116B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LGS5145"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 20.32 -12.7 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2304071600_Legend-Si-LGS5145_C5123971.pdf"
			(at 45.72 -15.24 0)
		)
		(property "Description" "1A, 1.2MHz Buck DC/DC Converter, adjustable output voltage, 4.5..55V input, 0.8..50V output, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Legend step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM22676MR-5"
		(extends "LM22676MR-ADJ")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LM22676MR-5"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm22676.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "3A Step-Down Switching Voltage Regulater, 4.5-42V Input, 5V Output, 500kHz Switching Frequency, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Converter 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*"
			(at 0 0 0)
		)
	)
	(symbol "LM22678TJ-5"
		(extends "LM22678TJ-ADJ")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM22678TJ-5"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm22678.pdf"
			(at 1.27 -2.54 0)
		)
		(property "Description" "5A Step-Down Switching Voltage Regulater, 4.5-42V Input, 5V Output, 500kHz Switching Frequency, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Converter 5A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574HVM-15"
		(extends "LM2574HVM-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVM-15"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 15V 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574HVM-3.3"
		(extends "LM2574HVM-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVM-3.3"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574HVM-5"
		(extends "LM2574HVM-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVM-5"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574HVM-ADJ"
		(extends "LM2574HVM-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVM-ADJ"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator Adjustable 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574HVN-15"
		(extends "LM2574HVN-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVN-15"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 15V 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574HVN-3.3"
		(extends "LM2574HVN-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVN-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574HVN-5"
		(extends "LM2574HVN-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVN-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574HVN-ADJ"
		(extends "LM2574HVN-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574HVN-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator Adjustable 500mA HV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574M-12"
		(extends "LM2574HVM-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574M-12"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574M-15"
		(extends "LM2574HVM-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574M-15"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 15V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574M-3.3"
		(extends "LM2574HVM-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574M-3.3"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574M-5"
		(extends "LM2574HVM-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574M-5"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574M-ADJ"
		(extends "LM2574HVM-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574M-ADJ"
			(at -5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-14W_7.5x9mm_P1.27mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator Adjustable 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574N-12"
		(extends "LM2574HVN-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574N-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574N-15"
		(extends "LM2574HVN-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574N-15"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 15V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574N-3.3"
		(extends "LM2574HVN-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574N-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574N-5"
		(extends "LM2574HVN-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574N-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2574N-ADJ"
		(extends "LM2574HVN-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2574N-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.national.com/ds/LM/LM2574.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator Adjustable 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2575-12BT"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2575-12BT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/lm2575.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 12V 52kHz Simple 1A Buck Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck regulator Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2575-12BU"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2575-12BU"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/lm2575.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 12V 52kHz Simple 1A Buck Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck regulator Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2575-3.3BT"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2575-3.3BT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/lm2575.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 3.3V 52kHz Simple 1A Buck Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck regulator Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2575-3.3BU"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2575-3.3BU"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/lm2575.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 3.3V 52kHz Simple 1A Buck Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck regulator Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2575-5.0BT"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2575-5.0BT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/lm2575.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 5.0V 52kHz Simple 1A Buck Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck regulator Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2575-5.0BU"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2575-5.0BU"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/lm2575.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 5.0V 52kHz Simple 1A Buck Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck regulator Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2575BT-ADJ"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2575BT-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/lm2575.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable 52kHz Simple 1A Buck Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck regulator Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2575BU-ADJ"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2575BU-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/lm2575.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable 52kHz Simple 1A Buck Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck Regulator Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576HVS-15"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVS-15"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 15V 3A High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576HVS-3.3"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVS-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 3A, SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 3A High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576HVS-5"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVS-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 3A, SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 3A High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576HVS-ADJ"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVS-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3A Adjustable High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576HVT-15"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVT-15"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 15V 3A High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576HVT-3.3"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVT-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 3A High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576HVT-5"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVT-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 3A High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576HVT-ADJ"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576HVT-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3A Adjustable High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576S-12"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576S-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576S-15"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576S-15"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 15V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576S-3.3"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576S-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576S-5"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576S-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576S-ADJ"
		(extends "LM2576HVS-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576S-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3A Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576T-12"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576T-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576T-15"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576T-15"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 15V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576T-3.3"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576T-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576T-5"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576T-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2576T-ADJ"
		(extends "LM2576HVT-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2576T-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_Vertical"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2576.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3A Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2578"
		(extends "LM3578")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM2578"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3578a.pdf"
			(at -1.27 -1.27 0)
		)
		(property "Description" "750mA, Switching Regulator, adjustable output voltage, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594HVM-12"
		(extends "LM2594M-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594HVM-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "12V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 60V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594HVM-3.3"
		(extends "LM2594M-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594HVM-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3.3V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 60V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594HVM-5.0"
		(extends "LM2594M-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594HVM-5.0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "5.0V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 60V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594HVM-ADJ"
		(extends "LM2594M-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594HVM-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Adjustable Output Voltage, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 60V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594HVN-12"
		(extends "LM2594N-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594HVN-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "12V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 60V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594HVN-3.3"
		(extends "LM2594N-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594HVN-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3.3V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 60V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594HVN-5.0"
		(extends "LM2594N-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594HVN-5.0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "5.0V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 60V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594HVN-ADJ"
		(extends "LM2594N-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594HVN-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Adjustable Output Voltage, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 60V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594M-12"
		(extends "LM2594M-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594M-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "12V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 45V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594M-5.0"
		(extends "LM2594M-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594M-5.0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "5.0V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 45V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594M-ADJ"
		(extends "LM2594M-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594M-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Adjustable Output Voltage, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 45V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594N-12"
		(extends "LM2594N-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594N-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "12V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 45V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594N-5.0"
		(extends "LM2594N-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594N-5.0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "5.0V, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 45V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2594N-ADJ"
		(extends "LM2594N-3.3")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2594N-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2594.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Adjustable Output Voltage, 0.5A SIMPLE SWITCHER® Step-Down Voltage Regulator, Maximum VIN 45V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck converter regulator step-down voltage simple switcher adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2595S-3.3"
		(extends "LM2595S-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2595S-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/lm2595.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 1A Step-Down Voltage Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2595S-5"
		(extends "LM2595S-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2595S-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/lm2595.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 1A Step-Down Voltage Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2595S-ADJ"
		(extends "LM2595S-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2595S-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/lm2595.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output 1A Step-Down Voltage Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 1A Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2595T-3.3"
		(extends "LM2595T-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2595T-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/lm2595.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 1A Step-Down Voltage Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2595T-5"
		(extends "LM2595T-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2595T-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/lm2595.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 1A Step-Down Voltage Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2595T-ADJ"
		(extends "LM2595T-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2595T-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/lm2595.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output 1A Step-Down Voltage Regulator, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 1A Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2596S-3.3"
		(extends "LM2596S-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2596S-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2596.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 3A Step-Down Voltage Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2596S-5"
		(extends "LM2596S-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2596S-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2596.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 3A Step-Down Voltage Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2596S-ADJ"
		(extends "LM2596S-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2596S-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2596.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable 3A Step-Down Voltage Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator Adjustable 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2596T-3.3"
		(extends "LM2596T-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2596T-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2596.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 3A 150kHz Step-Down Voltage Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2596T-5"
		(extends "LM2596T-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2596T-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2596.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 3A 150kHz Step-Down Voltage Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2596T-ADJ"
		(extends "LM2596T-12")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "LM2596T-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2596.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable 3A 150kHz Step-Down Voltage Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator Adjustable 3A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2672M-3.3"
		(extends "LM2672M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2672M-3.3"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2672.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 1A Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2672M-5.0"
		(extends "LM2672M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2672M-5.0"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2672.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 1A Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2672M-ADJ"
		(extends "LM2672M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2672M-ADJ"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2672.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 1A Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2672N-3.3"
		(extends "LM2672N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2672N-3.3"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2672.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 1A Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2672N-5.0"
		(extends "LM2672N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2672N-5.0"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2672.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 1A Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2672N-ADJ"
		(extends "LM2672N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2672N-ADJ"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2672.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 1A Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2674M-3.3"
		(extends "LM2674M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2674M-3.3"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2674.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 500mA Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2674M-5.0"
		(extends "LM2674M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2674M-5.0"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2674.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 500mA Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2674M-ADJ"
		(extends "LM2674M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2674M-ADJ"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2674.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 500mA Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2674N-3.3"
		(extends "LM2674N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2674N-3.3"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2674.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 500mA Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2674N-5.0"
		(extends "LM2674N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2674N-5.0"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2674.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 500mA Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2674N-ADJ"
		(extends "LM2674N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2674N-ADJ"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2674.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 500mA Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2675M-12"
		(extends "LM2674M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2675M-12"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2675.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 1A Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2675M-3.3"
		(extends "LM2674M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2675M-3.3"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2675.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 1A Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2675M-5"
		(extends "LM2674M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2675M-5"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2675.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 1A Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2675M-ADJ"
		(extends "LM2674M-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2675M-ADJ"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2675.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 1A Step-Down Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2675N-12"
		(extends "LM2674N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2675N-12"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2675.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 1A Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 12V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2675N-3.3"
		(extends "LM2674N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2675N-3.3"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2675.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 1A Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 3.3V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2675N-5"
		(extends "LM2674N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2675N-5"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2675.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 1A Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator 5V 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2675N-ADJ"
		(extends "LM2674N-12")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM2675N-ADJ"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2675.pdf"
			(at 0 0 0)
		)
		(property "Description" "Adjustable Output Voltage, 1A Step-Down Voltage Regulator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Voltage Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM27313XMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LM27313XMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm27313.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1A, 28Vout Boost Voltage Regulator, 1.6MHz Frequency, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2731XMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LM2731XMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2731.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "LM27313, 1.8A, 22Vout Boost Voltage Regulator, 1.6MHz Frequency, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2731YMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LM2731YMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2731.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "LM27313, 1.8A, 22Vout Boost Voltage Regulator, 600KHz Frequency,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2733XMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LM2733XMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2733.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "LM27313, 1A, 40Vout Boost Voltage Regulator, 1.6MHz Frequency, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2733YMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LM2733YMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2733.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "LM27313, 1A, 40Vout Boost Voltage Regulator, 600KHz Frequency,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2734X"
		(extends "LM2734Y")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2734X"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2734.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "1A Step-Down DC-DC Regulator, Adjustable Output Voltage, 1.6MHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2735XMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LM2735XMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2735.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "LM27313, 2.1A, 24Vout Boost/FlybacK/SEPIC Voltage Regulator, 520kHz/1.6MHz Frequency,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost Flyback SEPIC Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2840X"
		(extends "LM2734Y")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2840X"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2842-q1.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "100mA 42V Input Step-Down DC-DC Regulator, Adjustable Output Voltage, 550kHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2840Y"
		(extends "LM2734Y")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2840Y"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2842-q1.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "100mA 42V Input Step-Down DC-DC Regulator, Adjustable Output Voltage, 1.25MHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2841X"
		(extends "LM2734Y")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2841X"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2842-q1.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "300mA 42V Input Step-Down DC-DC Regulator, Adjustable Output Voltage, 550kHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2841Y"
		(extends "LM2734Y")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2841Y"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2842-q1.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "300mA 42V Input Step-Down DC-DC Regulator, Adjustable Output Voltage, 1.25MHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2842X"
		(extends "LM2734Y")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2842X"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2842-q1.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "600mA 42V Input Step-Down DC-DC Regulator, Adjustable Output Voltage, 550kHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM2842Y"
		(extends "LM2734Y")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LM2842Y"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0.635 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2842-q1.pdf"
			(at -2.54 2.54 0)
		)
		(property "Description" "600mA 42V Input Step-Down DC-DC Regulator, Adjustable Output Voltage, 1.25MHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM3670MF"
		(extends "ADP2108AUJ-1.0")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LM3670MF"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3670.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "Miniature Step-Down DC-DC Converter for Ultralow Voltage Circuits, 2.5V < Vin < 5.5V, adjustable output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC-DC buck converter step down voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM5008MM"
		(extends "LM5007MM")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5008MM"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5008.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA, High Voltage (100V) Step-Down Switching Regulator, Adjustable Output Voltage, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM5008SD"
		(extends "LM5007SD")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5008SD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.6x3mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5008.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA, High Voltage (100V) Step-Down Switching Regulator, Adjustable Output Voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM5009MM"
		(extends "LM5007MM")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5009MM"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5009.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, High Voltage (80V) Step-Down Switching Regulator, Adjustable Output Voltage, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM5009SD"
		(extends "LM5007SD")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LM5009SD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.6x3mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5009.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA, High Voltage (80V) Step-Down Switching Regulator, Adjustable Output Voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM5165Y"
		(extends "LM5165X")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM5165Y"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5165.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "150mA Synchronous Buck Converter With Ultra-Low IQ, 3V-65V input, 3.3V fixed output voltage, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator fixed 3V3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PVSON*N10*"
			(at 0 0 0)
		)
	)
	(symbol "LM5166"
		(extends "LM5165")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM5166"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5166.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "500mA Synchronous Buck Converter With Ultra-Low IQ, 3V-65V input, adjustable output voltage, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PVSON*N10*"
			(at 0 0 0)
		)
	)
	(symbol "LM5166X"
		(extends "LM5165X")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM5166X"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5166.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "500mA Synchronous Buck Converter With Ultra-Low IQ, 3V-65V input, 5.0V fixed output voltage, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator fixed 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PVSON*N10*"
			(at 0 0 0)
		)
	)
	(symbol "LM5166Y"
		(extends "LM5165X")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LM5166Y"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5166.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "500mA Synchronous Buck Converter With Ultra-Low IQ, 3V-65V input, 3.3V fixed output voltage, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator fixed 3V3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PVSON*N10*"
			(at 0 0 0)
		)
	)
	(symbol "LM5176PWP"
		(extends "LM5175PWP")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "LM5176PWP"
			(at -12.7 21.59 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_ThermalVias"
			(at 17.78 21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5176.pdf"
			(at 50.8 -11.43 0)
		)
		(property "Description" "55-V wide Vin synchronous 4-switch Buck-Boost controller, HTSSOP-28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck Boost step-up step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x9.7mm*P0.65*ThermalVias*"
			(at 0 0 0)
		)
	)
	(symbol "LM5176RHF"
		(extends "LM5175RHF")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "LM5176RHF"
			(at -12.7 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-28-1EP_4x5mm_P0.5mm_EP2.55x3.55mm"
			(at 17.78 21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5176.pdf"
			(at 50.8 -11.43 0)
		)
		(property "Description" "55-V wide Vin synchronous 4-switch Buck-Boost controller, QFN-28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck Boost step-up step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*4x5mm*P0.5*"
			(at 0 0 0)
		)
	)
	(symbol "LMR10510YMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LMR10510YMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr10510.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1A, 5.5V Step-Down Voltage Regulator, 3MHz Frequency, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Down Buck Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMR14206"
		(extends "LMR16006YQ")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "LMR14206"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr14206.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "Simple Switcher Buck Regulator, Vin=4.5-42V, Iout=600mA, Adjustable output voltage, SOT-23-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMR16006YQ3"
		(extends "LMR16006YQ")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "LMR16006YQ3"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr16006y-q1.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "Simple Switcher Buck Regulator, Vin=4-40V, Iout=600mA, Fixed 3.3V output voltage, SOT-23-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMR16006YQ5"
		(extends "LMR16006YQ")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "LMR16006YQ5"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr16006y-q1.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "Simple Switcher Buck Regulator, Vin=4-40V, Iout=600mA, Fixed 5.0V output voltage, SOT-23-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMR33610ADDAR"
		(extends "LMR33640ADDA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33610ADDAR"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33610.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=1A, F=400kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "LMR33610BDDAR"
		(extends "LMR33640ADDA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33610BDDAR"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33610.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=1A, F=1400kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "LMR33620ADDA"
		(extends "LMR33640ADDA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33620ADDA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33620.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=2A, F=400kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "LMR33620BDDA"
		(extends "LMR33640ADDA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33620BDDA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33620.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=2A, F=1400kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "LMR33620CDDA"
		(extends "LMR33640ADDA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33620CDDA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33640.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=2A, F=2100kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "LMR33630ADDA"
		(extends "LMR33640ADDA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33630ADDA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33630.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=3A, F=400kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "LMR33630BDDA"
		(extends "LMR33640ADDA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33630BDDA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33630.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=3A, F=1400kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "LMR33630CDDA"
		(extends "LMR33640ADDA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33630CDDA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33630.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=3A, F=2100kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "LMR33640DDDA"
		(extends "LMR33640ADDA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LMR33640DDDA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr33640.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Simple Switcher Synchronous Buck Regulator, Vin=3.8-36V, Iout=4A, F=1000kHz, Adjustable output voltage, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "simple-switcher synchronous buck step-down voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HSOP*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "LMR62014XMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LMR62014XMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr62014.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1.4A, 20Vout Step-Up Voltage Regulator, 1.6MHz Frequency, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMR62421XMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LMR62421XMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr62421.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2.1A, 24Vout Boost/SEPIC Voltage Regulator, 1.6MHz Frequency, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost SEPIC Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMR64010XMF"
		(extends "LMR10510XMF")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LMR64010XMF"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmr64010.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1A, 40Vout Step-Up Voltage Regulator, 1.6MHz Frequency, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Step-Up Boost Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LMZ22003TZ"
		(extends "LMZ23605TZ")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZ22003TZ"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_NDW-7_TabPin4"
			(at 20.955 -10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/LMZ22003"
			(at 0 -17.78 0)
		)
		(property "Description" "3A Adjustable Step-Down DC/DC Power Module, Vin: 6-20V"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*NDW*"
			(at 0 0 0)
		)
	)
	(symbol "LMZ22005TZ"
		(extends "LMZ23605TZ")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZ22005TZ"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_NDW-7_TabPin4"
			(at 20.955 -10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/LMZ22005"
			(at 0 -17.78 0)
		)
		(property "Description" "5A Adjustable Step-Down DC/DC Power Module, Vin: 6-20V"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*NDW*"
			(at 0 0 0)
		)
	)
	(symbol "LMZ23603TZ"
		(extends "LMZ23605TZ")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZ23603TZ"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_NDW-7_TabPin4"
			(at 20.955 -10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/lmz23603"
			(at 0 -17.78 0)
		)
		(property "Description" "3A Adjustable Step-Down DC/DC Power Module, Vin: 6-36V"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*NDW*"
			(at 0 0 0)
		)
	)
	(symbol "LMZM23600"
		(extends "LMZM23601")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZM23600"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_LGA:Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm_ThermalVias"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmzm23600.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "0.5A Adjustable Step-Down DC/DC Power Module in 3.8x3mm, MicroSIP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*SIL*1EP*3.8x3mm*P0.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMZM23600V3"
		(extends "LMZM23601")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZM23600V3"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_LGA:Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm_ThermalVias"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmzm23600.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "0.5A 3.3V Step-Down DC/DC Power Module in 3.8x3mm, MicroSIP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*SIL*1EP*3.8x3mm*P0.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMZM23600V5"
		(extends "LMZM23601")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZM23600V5"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_LGA:Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm_ThermalVias"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmzm23600.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "0.5A 5V Step-Down DC/DC Power Module in 3.8x3mm, MicroSIP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*SIL*1EP*3.8x3mm*P0.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMZM23601V3"
		(extends "LMZM23601")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZM23601V3"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_LGA:Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm_ThermalVias"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmzm23601.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "1A 3.3V Step-Down DC/DC Power Module in 3.8x3mm, MicroSIP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*SIL*1EP*3.8x3mm*P0.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMZM23601V5"
		(extends "LMZM23601")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LMZM23601V5"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_LGA:Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm_ThermalVias"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmzm23601.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "1A 5V Step-Down DC/DC Power Module in 3.8x3mm, MicroSIP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC/DC Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*SIL*1EP*3.8x3mm*P0.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "LNK304D"
		(extends "LNK302D")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK304D"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 170mA Output Current, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK304G"
		(extends "LNK302G")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK304G"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 170mA Output Current, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK304P"
		(extends "LNK302P")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK304P"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 170mA Output Current, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK305D"
		(extends "LNK302D")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK305D"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 280mA Output Current, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK305G"
		(extends "LNK302G")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK305G"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 280mA Output Current, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK305P"
		(extends "LNK302P")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK305P"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 280mA Output Current, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK306D"
		(extends "LNK302D")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK306D"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 360mA Output Current, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK306G"
		(extends "LNK302G")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK306G"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 360mA Output Current, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK306P"
		(extends "LNK302P")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK306P"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk302_304-306.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 360mA Output Current, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK3204D"
		(extends "LNK3202D")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3204D"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN2 Family, 170mA Output Current, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK3204G"
		(extends "LNK3202G")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3204G"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN2 Family, 170mA Output Current, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK3204P"
		(extends "LNK3202P")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3204P"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN2 Family, 170mA Output Current, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK3205D"
		(extends "LNK3202D")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3205D"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 270mA Output Current, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK3205G"
		(extends "LNK3202G")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3205G"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 270mA Output Current, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK3205P"
		(extends "LNK3202P")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3205P"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN Family, 270mA Output Current, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK3206D"
		(extends "LNK3202D")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3206D"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN2 Family, 360mA Output Current, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK3206G"
		(extends "LNK3202G")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3206G"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN2 Family, 360mA Output Current, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK3206P"
		(extends "LNK3202P")
		(property "Reference" "U"
			(at 0 -6.35 0)
		)
		(property "Value" "LNK3206P"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/LinkSwitch-TN2_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-TN2 Family, 360mA Output Current, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lowest Component Count, Energy-Efficient Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK363D"
		(extends "LNK362D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK363D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk362-364.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-XT Family, 4.7W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Effi cient, Low Power Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK363G"
		(extends "LNK362G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK363G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk362-364.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-XT Family, 4.7W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Effi cient, Low Power Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK363P"
		(extends "LNK362P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK363P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk362-364.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-XT Family, 4.7W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Effi cient, Low Power Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK364D"
		(extends "LNK362D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK364D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk362-364.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-XT Family, 6W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Effi cient, Low Power Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK364G"
		(extends "LNK362G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK364G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk362-364.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-XT Family, 6W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Effi cient, Low Power Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK364P"
		(extends "LNK362P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK364P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/lnk362-364.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-XT Family, 6W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Effi cient, Low Power Off-Line Switcher IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK404EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK404EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 15W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK404LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK404LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 15W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK405EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK405EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 18W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK405LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK405LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 18W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK406EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK406EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 22W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK406LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK406LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 22W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK407EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK407EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 25W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK407LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK407LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 25W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK408EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK408EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 35W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK408LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK408LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 35W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK409EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK409EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 50W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK409LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK409LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 50W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK410EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK410EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 78W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK410LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK410LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 78W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK413EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK413EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 12W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK413LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK413LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 12W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK414EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK414EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 15W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK414LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK414LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 15W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK415EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK415EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 18W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK415LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK415LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 18W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK416EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK416EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 22W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK416LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK416LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 22W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK417EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK417EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 25W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK417LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK417LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 25W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK418EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK418EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 35W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK418LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK418LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 35W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK419EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK419EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 50W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK419LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK419LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 50W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK420EG"
		(extends "LNK403EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK420EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 78W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK420LG"
		(extends "LNK403LG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "LNK420LG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ph_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PH Family, 78W Output Power, eSIP-7F"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC, Single-Stage PFC and Primary-Side Constant Current Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "LNK456D"
		(extends "LNK454D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK456D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PL Family, 6W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Constant Current Control for Non-Isolated Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK457D"
		(extends "LNK454D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK457D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PL Family, 8W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Constant Current Control for Non-Isolated Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK458K"
		(extends "LNK457K")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK458K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PL Family, 11.5W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Constant Current Control for Non-Isolated Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK458V"
		(extends "LNK457V")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK458V"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PL Family, 8W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Constant Current Control for Non-Isolated Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK460K"
		(extends "LNK457K")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK460K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PL Family, 16W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Constant Current Control for Non-Isolated Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK460V"
		(extends "LNK457V")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK460V"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-PL Family, 8W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver IC with TRIAC Dimming, Single-Stage PFC and Constant Current Control for Non-Isolated Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK563D"
		(extends "LNK562D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK563D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linklp_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-LP Family, 2.5W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Efficient Off-Line Switcher IC for Linear Transformer Replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK563G"
		(extends "LNK562G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK563G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linklp_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-LP Family, 2.5W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Efficient Off-Line Switcher IC for Linear Transformer Replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK563P"
		(extends "LNK562P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK563P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linklp_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-LP Family, 2.5W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Efficient Off-Line Switcher IC for Linear Transformer Replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK564D"
		(extends "LNK562D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK564D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linklp_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-LP Family, 3W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Efficient Off-Line Switcher IC for Linear Transformer Replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK564G"
		(extends "LNK562G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK564G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linklp_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-LP Family, 3W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Efficient Off-Line Switcher IC for Linear Transformer Replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK564P"
		(extends "LNK562P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK564P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linklp_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-LP Family, 3W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Efficient Off-Line Switcher IC for Linear Transformer Replacement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "LNK604DG"
		(extends "LNK603DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK604DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 4.1W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK604PG"
		(extends "LNK603PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK604PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 4.1W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK605DG"
		(extends "LNK603DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK605DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 5.1W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK605PG"
		(extends "LNK603PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK605PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 5.1W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK606DG"
		(extends "LNK603DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK606DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 6.1W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK606PG"
		(extends "LNK603PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK606PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 6.1W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK613DG"
		(extends "LNK603DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK613DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 3.3W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK613PG"
		(extends "LNK603PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK613PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 3.3W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK614DG"
		(extends "LNK603DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK614DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 4.1W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK614PG"
		(extends "LNK603PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK614PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 4.1W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK615DG"
		(extends "LNK603DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK615DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 5.1W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK615PG"
		(extends "LNK603PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK615PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 5.1W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK616DG"
		(extends "LNK603DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK616DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 6.1W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK616GG"
		(extends "LNK606GG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK616GG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 6.1W Output Power, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK616PG"
		(extends "LNK603PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK616PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkswitch-ii_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-II Family, 6.1W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Accurate CV/CC Switcher for Adapters and Chargers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK624DG"
		(extends "LNK623DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK624DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkcv_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-CV Family, 6.5W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Effi cient, Off-line Switcher with Accurate Primary-side Constant-Voltage Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK624PG"
		(extends "LNK623PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK624PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkcv_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-CV Family, 6.5W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-line Switcher with Accurate Primary-side Constant-Voltage Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK625DG"
		(extends "LNK623DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK625DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkcv_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-CV Family, 8W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-line Switcher with Accurate Primary-side Constant-Voltage Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK625PG"
		(extends "LNK623PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK625PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkcv_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-CV Family, 8W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-line Switcher with Accurate Primary-side Constant-Voltage Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK626DG"
		(extends "LNK623DG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK626DG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkcv_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-CV Family, 10W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-line Switcher with Accurate Primary-side Constant-Voltage Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LNK626PG"
		(extends "LNK623PG")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "LNK626PG"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/linkcv_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "LinkSwitch-CV Family, 10W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-line Switcher with Accurate Primary-side Constant-Voltage Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "LT1073CN-12"
		(extends "LT1073CN-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1073CN-12"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1073fa.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC/DC Converter, Fixed 12V Output Voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1073CS-12"
		(extends "LT1073CS-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1073CS-12"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1073fa.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC/DC Converter, Fixed 12V Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1108CN"
		(extends "LT1073CN")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1108CN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, adjustable output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1108CN-12"
		(extends "LT1073CN-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1108CN-12"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, fixed 12V output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1108CN-5"
		(extends "LT1073CN-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1108CN-5"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, fixed 5V output voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1108CS"
		(extends "LT1073CS")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1108CS"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, adjustable output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1108CS-12"
		(extends "LT1073CS-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1108CS-12"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, fixed 12V output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1108CS-5"
		(extends "LT1073CS-5")
		(property "Reference" "U"
			(at 1.27 10.795 0)
		)
		(property "Value" "LT1108CS-5"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt1108.pdf"
			(at -5.08 15.24 0)
		)
		(property "Description" "Micropower DC-DC converter, step-up or step-down operation, 2V-30Vin, fixed 5V output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck boost converter step-down step-up"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1307BCMS8"
		(extends "LT1307CMS8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1307BCMS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1307fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Cell Micropower 600kHz PWM DC/DC Converter, 10µA Quiescent Current, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower PWM DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1307BCS8"
		(extends "LT1307CS8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1307BCS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1307fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Cell Micropower 600kHz PWM DC/DC Converter, 10µA Quiescent Current, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower PWM DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1372HVCN8"
		(extends "LT1372CN8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1372HVCN8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/13727fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A High Efficiency Switching Regulators, 500kHz, 42V Switch Voltage, Adjustable Output Voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1372HVCS8"
		(extends "LT1372CS8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1372HVCS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/13727fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A High Efficiency Switching Regulators, 500kHz, 42V Switch Voltage, Adjustable Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1373CN8"
		(extends "LT1372CN8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1373CN8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1373fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A Low Supply Current High Efficiency Switching Regulators, 250kHz, 35V Switch Voltage, Adjustable Output Voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1373CS8"
		(extends "LT1372CS8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1373CS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1373fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A Low Supply Current High Efficiency Switching Regulators, 250kHz, 35V Switch Voltage, Adjustable Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1373HVCN8"
		(extends "LT1372CN8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1373HVCN8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1373fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A Low Supply Current High Efficiency Switching Regulators, 250kHz, 42V Switch Voltage, Adjustable Output Voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1373HVCS8"
		(extends "LT1372CS8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1373HVCS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1373fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A Low Supply Current High Efficiency Switching Regulators, 250kHz, 42V Switch Voltage, Adjustable Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1377CN8"
		(extends "LT1372CN8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1377CN8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/13727fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A High Efficiency Switching Regulators, 1MHz, 35V Switch Voltage, Adjustable Output Voltage, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1377CS8"
		(extends "LT1372CS8")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT1377CS8"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/13727fbs.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "1.5A High Efficiency Switching Regulators, 1MHz, 35V Switch Voltage, Adjustable Output Voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3430-1"
		(extends "LT3430")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT3430-1"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14-1EP_4.4x5mm_P0.65mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/34301fa.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "3A High Voltage 100kHz Step-Down Switching Regulator, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3483AxS6"
		(extends "LT3483xS6")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "LT3483AxS6"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at -19.05 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3483fc.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Inverting Micropower DC/DC Converter with integrated schottky, 2.5V to 16V input, down to -38V output, 400mA, TSOT-23-6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Inverting Converter Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT3757AEDD"
		(extends "LT3757EDD")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LT3757AEDD"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3757Afe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boost, flyback, SEPIC and inverting regulator, improved load transient performance, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost flyback SEPIC inverting DC/DC regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3757AEMSE"
		(extends "LT3757EMSE")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LT3757AEMSE"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3757Afe.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boost, flyback, SEPIC and inverting regulator, improved load transient performance, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost flyback SEPIC inverting DC/DC regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT8610AC-1"
		(extends "LT8610AC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LT8610AC-1"
			(at 0.762 8.636 0)
		)
		(property "Footprint" "Package_SO:LTC_MSOP-16-1EP_3x4mm_P0.5mm_EP2.15x3.26mm"
			(at -2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/8610acfa.pdf"
			(at 0 -16.51 0)
		)
		(property "Description" "42V, 3.5A Synchronous Step-Down Regulator with 2.5uA Quiescent Current, Internal Compensation for Improved Transient, Soft-Start at Dropout and Brownout, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "high efficiency speed synchronous monolithic buck step-down switching regulator 42V 3.5A lower feedback voltage minimum vin internal compensation soft-start"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LTC*MSOP*16*1EP*3x4mm*P0.5mm*EP2.15x3.26mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3245xMSE"
		(extends "LTC3245xDE")
		(property "Reference" "U"
			(at 3.81 -15.24 0)
		)
		(property "Value" "LTC3245xMSE"
			(at 3.81 -17.78 0)
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc3245.pdf"
			(at 0 -31.75 0)
		)
		(property "Description" "Wide VIN Range, Low Noise, 250mA Buck-Boost Charge Pump, MSOP-12"
			(at 0 -29.21 0)
		)
		(property "ki_keywords" "widerange  lownoise buckboost chargepump"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MSOP*3x4.039mm*P0.65mm*EP1.651x2.845mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3406AES5"
		(extends "LTC3406BES5-1.2")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3406AES5"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3406afa.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "600mA Synchronous Step-Down Regulator, 1.5MHz, Fixed 1.2V Output Voltage, Low Ripple Burst Mode, ThinSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3406B-2ES5"
		(extends "LTC3406BES5-1.2")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3406B-2ES5"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3406b2fs.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "600mA Synchronous Step-Down Regulator, 2.25MHz, Adjustable Output Voltage,ThinSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3406ES5"
		(extends "LTC3406BES5-1.2")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3406ES5"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3406b12fs.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "600mA Synchronous Step-Down Regulator, 1.5MHz, Adjustable Output Voltage, Burst Mode, ThinSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3406ES5-1.2"
		(extends "LTC3406BES5-1.2")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3406ES5-1.2"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3406b12fs.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "600mA Synchronous Step-Down Regulator, 1.5MHz, Fixed 1.2V Output Voltage, Burst Mode, ThinSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3406ES5-1.5"
		(extends "LTC3406BES5-1.2")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3406ES5-1.5"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3406b12fs.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "600mA Synchronous Step-Down Regulator, 1.5MHz, Fixed 1.5V Output Voltage, Burst Mode, ThinSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3406ES5-1.8"
		(extends "LTC3406BES5-1.2")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3406ES5-1.8"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3406b12fs.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "600mA Synchronous Step-Down Regulator, 1.5MHz, Fixed 1.8V Output Voltage, Burst Mode, ThinSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator step-down"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3429B"
		(extends "LTC3429")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3429B"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3429fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA, 500kHz Micropower Synchronous Boost Converter with Output Disconnect, Continuous Switching at Light Loads, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3525-3"
		(extends "LTC3525")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3525-3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3525fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 3V, 400mA Micropower Synchronous Step-Up DC/DC Converter with Output Disconnect, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "fixed boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70* SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3525-3.3"
		(extends "LTC3525")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3525-3.3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3525fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 3V3, 400mA Micropower Synchronous Step-Up DC/DC Converter with Output Disconnect, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "fixed boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70* SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3525-5"
		(extends "LTC3525")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3525-5"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3525fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 5V, 400mA Micropower Synchronous Step-Up DC/DC Converter with Output Disconnect, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "fixed boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70* SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3525D-3.3"
		(extends "LTC3525")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3525D-3.3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3525d33fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 3V3, 400mA Micropower Synchronous Step-Up DC/DC Converter with Pass Through Mode, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "fixed boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70* SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3525L-3"
		(extends "LTC3525")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC3525L-3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3525laf.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 3V, 400mA Micropower Synchronous Step-Up DC/DC Converter with Output Disconnect, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "fixed boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70* SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3630AxDHC"
		(extends "LTC3630xDHC")
		(property "Reference" "U"
			(at -7.874 11.43 0)
		)
		(property "Value" "LTC3630AxDHC"
			(at 1.016 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-16-1EP_3x5mm_P0.5mm_EP1.66x4.4mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3630afc.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "High efficiency 76V 500mA synchronous step-down converter, DFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck dc-dc switcher switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*3x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3630AxMSE"
		(extends "LTC3630xMSE")
		(property "Reference" "U"
			(at -7.874 11.43 0)
		)
		(property "Value" "LTC3630AxMSE"
			(at 1.016 11.43 0)
		)
		(property "Footprint" "Package_SO:Analog_MSOP-12-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3630afc.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "High efficiency 76V 500mA synchronous step-down converter, MSOP-16(12)"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck dc-dc switcher switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*MSOP*12*16*EP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC3639xMSE"
		(extends "LTC3638xMSE")
		(property "Reference" "U"
			(at -7.874 11.43 0)
		)
		(property "Value" "LTC3639xMSE"
			(at 1.016 11.43 0)
		)
		(property "Footprint" "Package_SO:Analog_MSOP-12-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3639fd.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "100mA High efficiency 150V syncrhonous step-down converter, MSOP-16(12)"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck dc-dc switcher switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*MSOP*12*16*EP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTM4626"
		(extends "LTM4638")
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "LTM4626"
			(at 8.89 21.59 0)
		)
		(property "Footprint" "Package_BGA:Analog_BGA-49_6.25x6.25mm_Layout7x7_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltm4626.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog Devices 20VIN, 12A Step-Down DC/DC uModule Regulator, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "uModule Buck Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*BGA*6.25x6.25mm*Layout7x7*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTM4657"
		(extends "LTM4638")
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "LTM4657"
			(at 8.89 21.59 0)
		)
		(property "Footprint" "Package_BGA:Analog_BGA-49_6.25x6.25mm_Layout7x7_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltm4657.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog Devices 20VIN, 8A Step-Down DC/DC uModule Regulator, BGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "uModule Buck Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*BGA*6.25x6.25mm*Layout7x7*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTM4668A"
		(extends "LTM4668")
		(property "Reference" "U"
			(at -1.27 3.81 0)
		)
		(property "Value" "LTM4668A"
			(at -1.27 1.27 0)
		)
		(property "Footprint" "Package_BGA:Analog_BGA-49_6.25x6.25mm_Layout7x7_P0.8mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltm4668a.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Quad DC/DC μModule Regulator with Configurable 1.2A Output Array"
			(at 0 0 0)
		)
		(property "ki_keywords" "uModule DCDC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Analog*BGA*6.25x6.25mm*Layout7x7*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LV2862XDDC"
		(extends "LMR16006YQ")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "LV2862XDDC"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lv2862.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "60V, 0.6A, stepdown, DC/DC converter, 770kHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "step down DCDC converter regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LV2862YDDC"
		(extends "LMR16006YQ")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "LV2862YDDC"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lv2862.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "60V, 0.6A, stepdown, DC/DC converter, 2.1MHz"
			(at 0 0 0)
		)
		(property "ki_keywords" "step down DCDC converter regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX15062B"
		(extends "MAX15062A")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "MAX15062B"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8_2x2mm_P0.5mm"
			(at 0 13.97 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX15062.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "60V, 300mA, synchronous step-down dc-dc converter, 5.0V fixed output voltage, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX15062C"
		(extends "MAX15062A")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "MAX15062C"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8_2x2mm_P0.5mm"
			(at 0 13.97 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX15062.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "60V, 300mA, synchronous step-down dc-dc converter, adjustable output voltage, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX1523"
		(extends "MAX1522")
		(property "Reference" "U"
			(at -4.445 6.35 0)
		)
		(property "Value" "MAX1523"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 14.478 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX1522-MAX1524.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Boost converter, external switch, soft-start, retry on output fault, 2.5V..5.5Vin,  SOT-23-6"
			(at 0 2.54 0)
		)
		(property "ki_keywords" "maxim analog-devices"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX1524"
		(extends "MAX1522")
		(property "Reference" "U"
			(at -4.445 6.35 0)
		)
		(property "Value" "MAX1524"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX1522-MAX1524.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Boost converter, 1.5V startup, external switch, soft-start, bootstrapped operation, latch on output fault, 1.5V..5.5Vin,  SOT-23-6"
			(at 0 10.795 0)
		)
		(property "ki_keywords" "maxim analog-devices"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX17501BxTB"
		(extends "MAX17501AxTB")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX17501BxTB"
			(at 2.032 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-10-1EP_2x3mm_P0.5mm_EP0.9x2mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17501.pdf"
			(at -34.29 26.67 0)
		)
		(property "Description" "4.5V–60Vin, 500mA, High-Efficiency, 5V Synchronous Step-Down DC-DC Converter, PFM Mode, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX17501ExTB"
		(extends "MAX17501AxTB")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX17501ExTB"
			(at 2.032 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-10-1EP_2x3mm_P0.5mm_EP0.9x2mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17501.pdf"
			(at -34.29 26.67 0)
		)
		(property "Description" "4.5V–60Vin, 500mA, High-Efficiency, 3.3V Synchronous Step-Down DC-DC Converter, PWM Mode, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX17501FxTB"
		(extends "MAX17501AxTB")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX17501FxTB"
			(at 2.032 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-10-1EP_2x3mm_P0.5mm_EP0.9x2mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17501.pdf"
			(at -34.29 26.67 0)
		)
		(property "Description" "4.5V–60Vin, 500mA, High-Efficiency, 5V Synchronous Step-Down DC-DC Converter, PWM Mode, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX17501HxTB"
		(extends "MAX17501GxTB")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "MAX17501HxTB"
			(at 2.032 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-10-1EP_2x3mm_P0.5mm_EP0.9x2mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX17501.pdf"
			(at -34.29 26.67 0)
		)
		(property "Description" "4.5V–60Vin, 500mA, High-Efficiency, Adjustable Synchronous Step-Down DC-DC Converter, 300KHz, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-down dc-dc switching regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5035BUPA"
		(extends "MAX5035AUPA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX5035BUPA"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5035.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A, High-Efficiency Step-Down DC-DC Converter, 5V fixed output voltage, Vin 76V, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 1A Step-Down Converter 76V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5035BUSA"
		(extends "MAX5035AUSA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX5035BUSA"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5035.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A, High-Efficiency Step-Down DC-DC Converter, 5V fixed output voltage, Vin 76V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 1A Step-Down Converter 76V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5035CUPA"
		(extends "MAX5035AUPA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX5035CUPA"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5035.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A, High-Efficiency Step-Down DC-DC Converter, 12V fixed output voltage, Vin 76V, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 1A Step-Down Converter 76V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5035CUSA"
		(extends "MAX5035AUSA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX5035CUSA"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5035.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A, High-Efficiency Step-Down DC-DC Converter, 12V fixed output voltage, Vin 76V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 1A Step-Down Converter 76V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5035DUPA"
		(extends "MAX5035AUPA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX5035DUPA"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5035.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A, High-Efficiency Step-Down DC-DC Converter, adjustable output voltage, Vin 76V, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 1A Step-Down Converter 76V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5035DUSA"
		(extends "MAX5035AUSA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX5035DUSA"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5035.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A, High-Efficiency Step-Down DC-DC Converter, adjustable output voltage, Vin 76V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 1A Step-Down Converter 76V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5035EUSA"
		(extends "MAX5035AUSA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX5035EUSA"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5035.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A, High-Efficiency Step-Down DC-DC Converter, adjustable output voltage, Vin 76V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 1A Step-Down Converter 76V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC34063AD"
		(extends "MC33063AD")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MC34063AD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF"
			(at 12.7 -2.54 0)
		)
		(property "Description" "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps buck boost inverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC34063AP"
		(extends "MC33063AP")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MC34063AP"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF"
			(at 12.7 -2.54 0)
		)
		(property "Description" "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps buck boost inverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1623x-xCHY"
		(extends "MCP1640x-xCHY")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1623x-xCHY"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001420D.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low-Voltage Input Boost Regulator for PIC Microcontrollers, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1623x-xMC"
		(extends "MCP1640x-xMC")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1623x-xMC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001420D.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low-Voltage Input Boost Regulator for PIC Microcontrollers, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP16301Hx-xCH"
		(extends "MCP16301x-xCH")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MCP16301Hx-xCH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005004D.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 4.7 to 36V Input, High Voltage Input integrated switch step-down regulator, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP16312x-xMNY"
		(extends "MCP16311x-xMNY")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP16312x-xMNY"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP16311-Family-Data-Sheet-DS20005255C.pdf"
			(at -7.62 15.24 0)
		)
		(property "Description" "1A Output Voltage, 30V Input, integrated switch step-down regulator, PWM modulation, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP16312x-xMS"
		(extends "MCP16311x-xMS")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP16312x-xMS"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP16311-Family-Data-Sheet-DS20005255C.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "1A Output Voltage, 30V Input, integrated switch step-down regulator with, modulation, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1640Bx-xCHY"
		(extends "MCP1640x-xCHY")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1640Bx-xCHY"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002234D.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output 2.0V-5.5V, PWM Only True Disconnect, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1640Bx-xMC"
		(extends "MCP1640x-xMC")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1640Bx-xMC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002234D.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output 2.0V-5.5V, PWM Only True Disconnect, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1640Cx-xCHY"
		(extends "MCP1640x-xCHY")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1640Cx-xCHY"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002234D.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output 2.0V-5.5V, PWM/PFM Input to Output Bypass, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1640Cx-xMC"
		(extends "MCP1640x-xMC")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1640Cx-xMC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002234D.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output 2.0V-5.5V, PWM/PFM Input to Output Bypass, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1640Dx-xCHY"
		(extends "MCP1640x-xCHY")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1640Dx-xCHY"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002234D.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output 2.0V-5.5V, PWM Only Input to Output Bypass, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1640Dx-xMC"
		(extends "MCP1640x-xMC")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1640Dx-xMC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002234D.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output 2.0V-5.5V, PWM Only Input to Output Bypass, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2177-3.3"
		(extends "MIC2177")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "MIC2177-3.3"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2177.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A Synchronous Buck Regulator, 3.3V Fixed Output Voltage, SO-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W?7.5x12.8mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2177-5.0"
		(extends "MIC2177")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "MIC2177-5.0"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2177.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A Synchronous Buck Regulator, 5.0V Fixed Output Voltage, SO-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W?7.5x12.8mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2178-3.3"
		(extends "MIC2178")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "MIC2178-3.3"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2177.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A Synchronous Buck Regulator, 4.5-16.5V Input Voltage, 3.3V Fixed Output Voltage, SO-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC2178-5.0"
		(extends "MIC2178")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "MIC2178-5.0"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic2177.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A Synchronous Buck Regulator, 4.5-16.5V Input Voltage, 5.0V Fixed Output Voltage, SO-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC23050-4YML"
		(extends "MIC23050-CYML")
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "MIC23050-4YML"
			(at -10.16 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:Micrel_MLF-8-1EP_2x2mm_P0.5mm_EP0.6x1.2mm_ThermalVias"
			(at 5.08 1.27 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic23050.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4MHz PWM Buck Regulator with HyperLight Load Switching Scheme, 1.2V Fixed Output Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Micrel*MLF*8*2x2mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC23050-GYML"
		(extends "MIC23050-CYML")
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "MIC23050-GYML"
			(at -7.62 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:Micrel_MLF-8-1EP_2x2mm_P0.5mm_EP0.6x1.2mm_ThermalVias"
			(at 5.08 1.27 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic23050.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4MHz PWM Buck Regulator with HyperLight Load Switching Scheme, 1.8V Fixed Output Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Micrel*MLF*8*2x2mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC23050-SYML"
		(extends "MIC23050-CYML")
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "MIC23050-SYML"
			(at -7.62 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:Micrel_MLF-8-1EP_2x2mm_P0.5mm_EP0.6x1.2mm_ThermalVias"
			(at 5.08 1.27 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic23050.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4MHz PWM Buck Regulator with HyperLight Load Switching Scheme, 3.3V Fixed Output Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator switching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Micrel*MLF*8*2x2mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1070P100"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1070P100"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 100kHz, 22Ohm Rds(on), 250mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1070P130"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1070P130"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 130kHz, 22Ohm Rds(on), 250mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1070STBT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1070STBT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 100kHz, 22Ohm Rds(on), 250mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1070STCT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1070STCT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 130kHz, 22Ohm Rds(on), 250mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1071P065"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1071P065"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 65kHz, 22Ohm Rds(on), 350mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1071P100"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1071P100"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 100kHz, 22Ohm Rds(on), 350mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1071P130"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1071P130"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 130kHz, 22Ohm Rds(on), 350mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1071STAT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1071STAT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 65kHz, 22Ohm Rds(on), 350mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1071STBT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1071STBT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 100kHz, 22Ohm Rds(on), 350mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1071STCT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1071STCT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 14W/7.75W, 230V/85-265V, 130kHz, 22Ohm Rds(on), 350mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1072P065"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1072P065"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 65kHz, 11Ohm Rds(on), 250mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1072P100"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1072P100"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 100kHz, 11Ohm Rds(on), 250mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1072P130"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1072P130"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 130kHz, 11Ohm Rds(on), 250mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1072STAT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1072STAT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 65kHz, 11Ohm Rds(on), 250mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1072STBT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1072STBT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 100kHz, 11Ohm Rds(on), 250mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1072STCT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1072STCT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 130kHz, 11Ohm Rds(on), 250mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1075P065"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1075P065"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 65kHz, 11Ohm Rds(on), 450mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1075P100"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1075P100"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 100kHz, 11Ohm Rds(on), 450mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1075P130"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1075P130"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 130kHz, 11Ohm Rds(on), 450mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1075STAT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1075STAT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 65kHz, 11Ohm Rds(on), 450mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1075STBT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1075STBT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 100kHz, 11Ohm Rds(on), 450mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1075STCT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1075STCT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 19W/10W, 230V/85-265V, 130kHz, 11Ohm Rds(on), 450mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1076P065"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1076P065"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 65kHz, 4.7Ohm Rds(on), 650mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1076P100"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1076P100"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 100kHz, 4.7Ohm Rds(on), 650mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1076P130"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1076P130"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 130kHz, 4.7Ohm Rds(on), 650mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1076STAT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1076STAT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 65kHz, 4.7Ohm Rds(on), 650mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1076STBT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1076STBT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 100kHz, 4.7Ohm Rds(on), 650mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1076STCT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1076STCT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 130kHz, 4.7Ohm Rds(on), 650mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1077P065"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1077P065"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 65kHz, 4.7Ohm Rds(on), 800mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1077P100"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1077P100"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 100kHz, 4.7Ohm Rds(on), 800mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1077P130"
		(extends "NCP1070P065")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1077P130"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 130kHz, 4.7Ohm Rds(on), 800mA Ipk, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1077STAT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1077STAT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 65kHz, 4.7Ohm Rds(on), 800mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1077STBT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1077STBT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 100kHz, 4.7Ohm Rds(on), 800mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1077STCT"
		(extends "NCP1070STAT")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "NCP1077STCT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP1070-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "High-Voltage Switcher for Low Power Offline SMPS, 700V Vds, 25W/15W, 230V/85-265V, 130kHz, 4.7Ohm Rds(on), 800mA Ipk, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1529A"
		(extends "TLV62568DBV")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NCP1529A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP1529-D.PDF"
			(at -6.35 11.43 0)
		)
		(property "Description" "1.7MHz, 1A, High Efficiency, Low Ripple, Adjustable Output Voltage Step-down Converter, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV33063AVD"
		(extends "MC33063AD")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "NCV33063AVD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF"
			(at 12.7 -2.54 0)
		)
		(property "Description" "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps buck boost inverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NID30S24-12"
		(extends "NID30S24-05")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NID30S24-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_MeanWell_NID30_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.meanwell.com/webapp/product/search.aspx?prod=nid30"
			(at 0 0 0)
		)
		(property "Description" "2.5A/30W Step Down Converter Module, fixed 12V Output Voltage, 250kHz, 20-53V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Converter Module DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*MeanWell*NID30*THT*"
			(at 0 0 0)
		)
	)
	(symbol "NID30S24-15"
		(extends "NID30S24-05")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NID30S24-15"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_MeanWell_NID30_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.meanwell.com/webapp/product/search.aspx?prod=nid30"
			(at 0 0 0)
		)
		(property "Description" "2.5A/30W Step Down Converter Module, fixed 15V Output Voltage, 250kHz, 20-53V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Converter Module DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*MeanWell*NID30*THT*"
			(at 0 0 0)
		)
	)
	(symbol "NID30S48-24"
		(extends "NID30S24-05")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NID30S48-24"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_MeanWell_NID30_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.meanwell.com/webapp/product/search.aspx?prod=nid30"
			(at 0 0 0)
		)
		(property "Description" "1.25A/30W Step Down Converter Module, fixed 24V Output Voltage, 250kHz, 30-53V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Converter Module DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*MeanWell*NID30*THT*"
			(at 0 0 0)
		)
	)
	(symbol "NID60S24-12"
		(extends "NID60S24-05")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NID60S24-12"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_MeanWell_NID60_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.meanwell.com/78ddf876-a86c-4a52-8a41-4ee24dd9913d"
			(at 0 0 0)
		)
		(property "Description" "4A/48W Step Down Converter Module, fixed 12V Output Voltage, 250kHz, 20-53V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Converter Module DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*MeanWell*NID60*"
			(at 0 0 0)
		)
	)
	(symbol "NID60S24-15"
		(extends "NID60S24-05")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NID60S24-15"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_MeanWell_NID60_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.meanwell.com/78ddf876-a86c-4a52-8a41-4ee24dd9913d"
			(at 0 0 0)
		)
		(property "Description" "4A/60W Step Down Converter Module, fixed 15V Output Voltage, 250kHz, 20-53V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Converter Module DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*MeanWell*NID60*"
			(at 0 0 0)
		)
	)
	(symbol "NID60S48-24"
		(extends "NID60S24-05")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "NID60S48-24"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_MeanWell_NID60_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.meanwell.com/78ddf876-a86c-4a52-8a41-4ee24dd9913d"
			(at 0 0 0)
		)
		(property "Description" "2.5A/60W Step Down Converter Module, fixed 24V Output Voltage, 250kHz, 30-53V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Converter Module DC/DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*MeanWell*NID60*"
			(at 0 0 0)
		)
	)
	(symbol "NMA0505DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA0505DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±100mA Isolated 1W Dual output DC/DC Converter, 5V Input Voltage, ±5V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA0505SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA0505SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±100mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, ±5V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA0509DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA0509DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±55mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, ±9V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA0509SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA0509SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±55mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, ±9V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA0515DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA0515DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±33mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, ±15V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA0515SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA0515SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±33mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, ±15V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1205DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1205DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±100mA Isolated 1W Dual output DC/DC Converter Module, 12V Input Voltage, ±5V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1205SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1205SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±100mA Isolated 1W Dual output DC/DC Converter Module, 12V Input Voltage, ±5V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1209DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1209DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±55mA Isolated 1W Dual output DC/DC Converter Module, 12V Input Voltage, ±9V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1209SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1209SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±55mA Isolated 1W Dual output DC/DC Converter Module, 12V Input Voltage, ±9V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1212DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1212DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±42mA Isolated 1W Dual output DC/DC Converter Module, 12V Input Voltage, ±12V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1212SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1212SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±42mA Isolated 1W Dual output DC/DC Converter Module, 12V Input Voltage, ±12V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1215DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1215DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±33mA Isolated 1W Dual output DC/DC Converter Module, 12V Input Voltage, ±15V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1215SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1215SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±33mA Isolated 1W Dual output DC/DC Converter Module, 12V Input Voltage, ±15V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1505DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1505DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±100mA Isolated 1W Dual output DC/DC Converter Module, 15V Input Voltage, ±5V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1505SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1505SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±100mA Isolated 1W Dual output DC/DC Converter Module, 15V Input Voltage, ±5V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1512DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1512DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±42mA Isolated 1W Dual output DC/DC Converter Module, 15V Input Voltage, ±12V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1512SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1512SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±42mA Isolated 1W Dual output DC/DC Converter Module, 15V Input Voltage, ±12V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1515DC"
		(extends "NMA0512DC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1515DC"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±33mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, ±15V Output Voltage, DIP Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxDC*"
			(at 0 0 0)
		)
	)
	(symbol "NMA1515SC"
		(extends "NMA0512SC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NMA1515SC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NMAxxxxSC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://power.murata.com/data/power/ncl/kdc_nma.pdf"
			(at 0 0 0)
		)
		(property "Description" "±33mA Isolated 1W Dual output DC/DC Converter Module, 5V Input Voltage, ±15V Output Voltage, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NMAxxxxSC*"
			(at 0 0 0)
		)
	)
	(symbol "NXE1S0303MC"
		(extends "NXE2S0505MC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "NXE1S0303MC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NXExSxxxxMC_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8807031865374/kdc-nxe1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "1W 3.3V to 3.3V 303mA DC-DC Converter with 3kV isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NXExSxxxxMC*"
			(at 0 0 0)
		)
	)
	(symbol "NXE1S0305MC"
		(extends "NXE2S0505MC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "NXE1S0305MC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NXExSxxxxMC_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8807031865374/kdc-nxe1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "1W 3.3V to 5V 200mA DC-DC Converter with 3kV isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NXExSxxxxMC*"
			(at 0 0 0)
		)
	)
	(symbol "NXE1S0505MC"
		(extends "NXE2S0505MC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "NXE1S0505MC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NXExSxxxxMC_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8807031865374/kdc-nxe1.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "1W 5V to 5V 200mA DC-DC Converter with 3kV isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NXExSxxxxMC*"
			(at 0 0 0)
		)
	)
	(symbol "NXE2S1205MC"
		(extends "NXE2S0505MC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "NXE2S1205MC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NXExSxxxxMC_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8807031898142/kdc-nxe2.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "2W 12V to 5V 400mA DC-DC Converter with 3kV isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NXExSxxxxMC*"
			(at 0 0 0)
		)
	)
	(symbol "NXE2S1212MC"
		(extends "NXE2S0505MC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "NXE2S1212MC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NXExSxxxxMC_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8807031898142/kdc-nxe2.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "2W 12V to 12V 400mA DC-DC Converter with 3kV isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NXExSxxxxMC*"
			(at 0 0 0)
		)
	)
	(symbol "NXE2S1215MC"
		(extends "NXE2S0505MC")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "NXE2S1215MC"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_NXExSxxxxMC_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8807031898142/kdc-nxe2.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "2W 12V to 15V 400mA DC-DC Converter with 3kV isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*Murata*NXExSxxxxMC*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2301CAAB120"
		(extends "PAM2301CAAB330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2301CAAB120"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/PAM2301.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "800mA, Step-Down DC/DC-Converter, 1.2V Fixed Output Voltage, 1.5MHz, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305AAB120"
		(extends "PAM2305AAB330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305AAB120"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 1.2V Fixed Output Voltage, 1.5MHz, TSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305AAB150"
		(extends "PAM2305AAB330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305AAB150"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 1.5V Fixed Output Voltage, 1.5MHz, TSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305AAB180"
		(extends "PAM2305AAB330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305AAB180"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 1.8V Fixed Output Voltage, 1.5MHz, TSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305AAB250"
		(extends "PAM2305AAB330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305AAB250"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 2.5V Fixed Output Voltage, 1.5MHz, TSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305AAB280"
		(extends "PAM2305AAB330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305AAB280"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 2.8V Fixed Output Voltage, 1.5MHz, TSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305AABADJ"
		(extends "PAM2305AAB330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305AABADJ"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, Adjustable Output Voltage, 1.5MHz, TSOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305BJE120"
		(extends "PAM2305BJE330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305BJE120"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 1.2V Fixed Output Voltage, 1.5MHz, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305BJE150"
		(extends "PAM2305BJE330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305BJE150"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 1.5V Fixed Output Voltage, 1.5MHz, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305BJE180"
		(extends "PAM2305BJE330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305BJE180"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 1.8V Fixed Output Voltage, 1.5MHz, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305BJE250"
		(extends "PAM2305BJE330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305BJE250"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 2.5V Fixed Output Voltage, 1.5MHz, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305BJE280"
		(extends "PAM2305BJE330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305BJE280"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 2.8V Fixed Output Voltage, 1.5MHz, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305BJEADJ"
		(extends "PAM2305BJE330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305BJEADJ"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, Adjustable Output Voltage, 1.5MHz, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305CGF120"
		(extends "PAM2305CGF330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305CGF120"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 1.2V Fixed Output Voltage, 1.5MHz, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305CGF150"
		(extends "PAM2305CGF330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305CGF150"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 1.5V Fixed Output Voltage, 1.5MHz, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305CGF180"
		(extends "PAM2305CGF330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305CGF180"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 1.8V Fixed Output Voltage, 1.5MHz, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305CGF250"
		(extends "PAM2305CGF330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305CGF250"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 2.5V Fixed Output Voltage, 1.5MHz, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305CGF280"
		(extends "PAM2305CGF330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305CGF280"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, 2.8V Fixed Output Voltage, 1.5MHz, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2305CGFADJ"
		(extends "PAM2305CGF330")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "PAM2305CGFADJ"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2305.pdf"
			(at -6.35 -8.89 0)
		)
		(property "Description" "1A, Step-Down DC/DC-Converter, Adjustable Output Voltage, 1.5MHz, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage regulator switching buck fixed output analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2306AYPBB"
		(extends "PAM2306AYPAA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "PAM2306AYPBB"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2306.pdf"
			(at -33.02 -45.72 0)
		)
		(property "Description" "1A, Dual Step-Down DC/DC-Converter, Out1 1.2V, Out2 1.2V, 1.5MHz, W-DFN3x3"
			(at 0 0 0)
		)
		(property "ki_keywords" "STEP-DOWN Dual channel 1A Out1 1.2V, Out2 1.2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*3x3mm?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2306AYPBK"
		(extends "PAM2306AYPAA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "PAM2306AYPBK"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2306.pdf"
			(at -33.02 -45.72 0)
		)
		(property "Description" "1A, Dual Step-Down DC/DC-Converter, Out1 1.2V, Out2 3.3V, 1.5MHz, W-DFN3x3"
			(at 0 0 0)
		)
		(property "ki_keywords" "STEP-DOWN Dual channel 1A Out1 1.5V, Out2 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*3x3mm?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2306AYPCB"
		(extends "PAM2306AYPAA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "PAM2306AYPCB"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2306.pdf"
			(at -33.02 -45.72 0)
		)
		(property "Description" "1A, Dual Step-Down DC/DC-Converter, Out1 1.5V, Out2 1.2V, 1.5MHz, W-DFN3x3"
			(at 0 0 0)
		)
		(property "ki_keywords" "STEP-DOWN Dual channel 1A Out1 1.5V, Out2 1.2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*3x3mm?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2306AYPKB"
		(extends "PAM2306AYPAA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "PAM2306AYPKB"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2306.pdf"
			(at -33.02 -45.72 0)
		)
		(property "Description" "1A, Dual Step-Down DC/DC-Converter, Out1 3.3V, Out2 1.2V, 1.5MHz, W-DFN3x3"
			(at 0 0 0)
		)
		(property "ki_keywords" "STEP-DOWN Dual channel 1A Out1 3.3V, Out2 1.2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*3x3mm?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2306AYPKE"
		(extends "PAM2306AYPAA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "PAM2306AYPKE"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2306.pdf"
			(at -33.02 -45.72 0)
		)
		(property "Description" "1A, Dual Step-Down DC/DC-Converter, Out1 3.3V, Out2 1.8V, 1.5MHz, W-DFN3x3"
			(at 0 0 0)
		)
		(property "ki_keywords" "STEP-DOWN Dual channel 1A Out1 3.3V, Out2 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*3x3mm?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAM2306DYPAA"
		(extends "PAM2306AYPAA")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "PAM2306DYPAA"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
			(at 33.02 -8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM2306D.pdf"
			(at -33.02 -45.72 0)
		)
		(property "Description" "1A, Dual Step-Down DC/DC-Converter, Out1 ADJ, Out2 ADJ, 1.5MHz, W-DFN3x3"
			(at 0 0 0)
		)
		(property "ki_keywords" "STEP-DOWN Dual channel 1A Out1 ADJ, Out2 ADJ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*3x3mm?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "R-781.5-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-781.5-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 4.75-30V input, 1.5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-781.8-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-781.8-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 4.75-32V input, 1.8V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-781.8-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-781.8-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 4.75-18V input, 1.8V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-7812-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-7812-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 15-32V input, 12V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-7815-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-7815-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 18-32V input, 15V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-782.5-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-782.5-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 4.75-18V input, 2.5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-782.5-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-782.5-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 4.75-18V input, 2.5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-783.3-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-783.3-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 4.75-18V input, 3.3V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-783.3-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-783.3-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 4.75-18V input, 3.3V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-785.0-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-785.0-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 6.5-18V input, 5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-785.0-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-785.0-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 6.5-18V input, 5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-786.5-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-786.5-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78xx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 8-32V input, 6.5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78B1.5-2.0"
		(extends "R-78B1.2-2.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78B1.5-2.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78B-2.0_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Bxx-2.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down DC/DC-Regulator, 4.75-32V input, 1.5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78B*2.0*"
			(at 0 0 0)
		)
	)
	(symbol "R-78B1.8-2.0"
		(extends "R-78B1.2-2.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78B1.8-2.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78B-2.0_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Bxx-2.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down DC/DC-Regulator, 4.75-32V input, 1.8V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78B*2.0*"
			(at 0 0 0)
		)
	)
	(symbol "R-78B12-2.0"
		(extends "R-78B1.2-2.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78B12-2.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78B-2.0_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Bxx-2.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down DC/DC-Regulator, 15-32V input, 12V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78B*2.0*"
			(at 0 0 0)
		)
	)
	(symbol "R-78B15-2.0"
		(extends "R-78B1.2-2.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78B15-2.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78B-2.0_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Bxx-2.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down DC/DC-Regulator, 18-32V input, 15V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78B*2.0*"
			(at 0 0 0)
		)
	)
	(symbol "R-78B2.5-2.0"
		(extends "R-78B1.2-2.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78B2.5-2.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78B-2.0_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Bxx-2.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down DC/DC-Regulator, 4.75-32V input, 2.5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78B*2.0*"
			(at 0 0 0)
		)
	)
	(symbol "R-78B3.3-2.0"
		(extends "R-78B1.2-2.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78B3.3-2.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78B-2.0_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Bxx-2.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down DC/DC-Regulator, 4.75-32V input, 3.3V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78B*2.0*"
			(at 0 0 0)
		)
	)
	(symbol "R-78B5.0-2.0"
		(extends "R-78B1.2-2.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78B5.0-2.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78B-2.0_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Bxx-2.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down DC/DC-Regulator, 6.5-32V input, 5.0V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78B*2.0*"
			(at 0 0 0)
		)
	)
	(symbol "R-78B9.0-2.0"
		(extends "R-78B1.2-2.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78B9.0-2.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78B-2.0_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Bxx-2.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down DC/DC-Regulator, 11-32V input, 9.0V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78B*2.0*"
			(at 0 0 0)
		)
	)
	(symbol "R-78C1.8-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78C1.8-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Cxx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 5-42V input, 1.8V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78C12-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78C12-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Cxx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 15-42V input, 12V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78C15-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78C15-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Cxx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 18-42V input, 15V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78C3.3-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78C3.3-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Cxx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 6-42V input, 3.3V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78C5.0-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78C5.0-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Cxx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 7-42V input, 5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78C9.0-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78C9.0-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Cxx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 12-42V input, 9V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78E12-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78E12-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 15-28V input, 12V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78E15-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78E15-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 18-28V input, 15V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78E3.3-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78E3.3-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 6-28V input, 3.3V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78E3.3-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78E3.3-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 6-28V input, 3.3V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78E5.0-1.0"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78E5.0-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-1.0.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down DC/DC-Regulator, 7-28V input, 5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78E9.0-0.5"
		(extends "R-78E5.0-0.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78E9.0-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 12-28V input, 9V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78HB12-0.5"
		(extends "R-78HB24-0.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78HB12-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78HB-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78HBxx-0.5_L.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 17-72V input, 12V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78HB*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78HB15-0.5"
		(extends "R-78HB24-0.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78HB15-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78HB-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78HBxx-0.5_L.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 20-72V input, 15V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78HB*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78HB3.3-0.5"
		(extends "R-78HB24-0.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78HB3.3-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78HB-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78HBxx-0.5_L.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 9-72V input, 3.3V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78HB*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78HB5.0-0.5"
		(extends "R-78HB24-0.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78HB5.0-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78HB-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78HBxx-0.5_L.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 9-72V input, 5.0V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78HB*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78HB6.5-0.5"
		(extends "R-78HB24-0.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78HB6.5-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78HB-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78HBxx-0.5_L.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 9-72V input, 6.5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78HB*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "R-78HB9.0-0.5"
		(extends "R-78HB24-0.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "R-78HB9.0-0.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78HB-0.5_THT"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78HBxx-0.5_L.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Step-Down DC/DC-Regulator, 14-72V input, 9.0V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*R*78HB*0.5*"
			(at 0 0 0)
		)
	)
	(symbol "SC33063AD"
		(extends "MC33063AD")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "SC33063AD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF"
			(at 12.7 -2.54 0)
		)
		(property "Description" "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps buck boost inverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SC34063AP"
		(extends "MC33063AP")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "SC34063AP"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF"
			(at 12.7 -2.54 0)
		)
		(property "Description" "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "smps buck boost inverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SIC431A"
		(extends "SIC437A")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC431A"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/74589/sic431.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "24A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
	(symbol "SIC431C"
		(extends "SIC437C")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC431C"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/74589/sic431.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "24A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
	(symbol "SIC437B"
		(extends "SIC437A")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC437B"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/75921/sic437.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "12A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
	(symbol "SIC437D"
		(extends "SIC437C")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC437D"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/75921/sic437.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "12A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
	(symbol "SIC438A"
		(extends "SIC437A")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC438A"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/75921/sic437.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "8A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
	(symbol "SIC438C"
		(extends "SIC437C")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC438C"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/75921/sic437.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "8A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-0911WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-0911WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 4.5 to 13.2V, Output 5.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-0912WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-0912WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 4.5 to 13.2V, Output 12.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-0913WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-0913WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 4.5 to 13.2V, Output 15.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-0915WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-0915WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 4.5 to 13.2V, Output 24.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-0919WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-0919WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 4.5 to 13.2V, Output 9.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-2410WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-2410WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 9.0 to 36.0V, Output 3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-2411WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-2411WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 9.0 to 36.0V, Output 5.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-2412WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-2412WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 9.0 to 36.0V, Output 12.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-2413WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-2413WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 9.0 to 36.0V, Output 15.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-2415WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-2415WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 9.0 to 36.0V, Output 24.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-2419WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-2419WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 9.0 to 36.0V, Output 9.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5WW"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-4810WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-4810WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 18.0 to 75.0V, Output 3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-4811WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-4811WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 18.0 to 75.0V, Output 5.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-4812WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-4812WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 18.0 to 75.0V, Output 12.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-4813WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-4813WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 18.0 to 75.0V, Output 15.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-4815WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-4815WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 18.0 to 75.0V, Output 24.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TDN_5-4819WISM"
		(extends "TDN_5-0910WISM")
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "TDN_5-4819WISM"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TDN_5-xxxxWISM_SMD"
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://assets.tracopower.com/20190626081517/TDN5WISM/documents/tdn5wism-datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Input 18.0 to 75.0V, Output 9.0V"
			(at 0 0 0)
		)
		(property "ki_keywords" "dcdc traco 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter?DCDC?TRACO?TDN?5*WISM?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TL497A"
		(extends "TL497")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TL497A"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl497a.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA step up/step down switching regulator"
			(at 0 0 0)
		)
		(property "ki_keywords" "buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x9.0mm*P1.27mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TL5001A"
		(extends "TL5001")
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "TL5001A"
			(at 3.81 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tl5001a.pdf"
			(at 0 0 0)
		)
		(property "Description" "PWM Controller with wide input range, with 3% tolerance on reference. Input range 3.6-40V. Max output 50V."
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM SMPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO?8*3.9x4.9mm*P1.27mm* *DIP?8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV61070ADBV"
		(extends "MCP1640x-xCHY")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TLV61070ADBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv61070a.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Boost Converter, 2.5A switch current limit, 2.2-5.5V Output Voltage, 0.5-5.5V Input Voltage, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost adjustable converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV62084ADSGx"
		(extends "TLV62080DSGx")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TLV62084ADSGx"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 3.81 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62080.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "High-efficiency Step-down Converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WSON?8?1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV62084DSGx"
		(extends "TLV62080DSGx")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TLV62084DSGx"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 3.81 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62080.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "High-efficiency Step-down Converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "Synchronous Buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WSON?8?1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV62565DBVx"
		(extends "TLV62568DBV")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV62565DBVx"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv62565.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "2.7-V to 5.5-V input, EN Input, 1.5-A  step-down converter, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "high efficiency"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV62568ADRL"
		(extends "TLV62568DRL")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV62568ADRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tlv62568a"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter with forced PWM, Adjustable Output 0.6V-5.5V, 1A, SOT-563-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*563*"
			(at 0 0 0)
		)
	)
	(symbol "TLV62569ADRL"
		(extends "TLV62568DRL")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV62569ADRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tlv62569a"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter with forced PWM, Adjustable Output 0.6V-5.5V, 2A, SOT-563-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*563*"
			(at 0 0 0)
		)
	)
	(symbol "TLV62569DBV"
		(extends "TLV62568DBV")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV62569DBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62569.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 2A, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV62569DDC"
		(extends "TLV62568DDC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV62569DDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62569.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 2A, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV62569DRL"
		(extends "TLV62568DRL")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TLV62569DRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv62569.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 2A, SOT-563-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down Buck DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*563*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-0512"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-0512"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "83mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, 12V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-0512SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-0512SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "83mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, 12V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-0513"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-0513"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "67mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, 15V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-0513SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-0513SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "67mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, 15V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-0515"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-0515"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "42mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, 24V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-0523"
		(extends "TMR_1-0522")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-0523"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Dual_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "±33mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, ±15V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Dual*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-0523SM"
		(extends "TMR_1-0522SM")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "TMR_1-0523SM"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 5.08 -12.7 0)
		)
		(property "Description" "±33mA Regulated 1W DC/DC converter with 1.5kV isolation, 4.5V-9V input, ±15V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR-1SM*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1211"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-1211"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, 5V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1211SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-1211SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, 5V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1212"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-1212"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "83mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, 12V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1212SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-1212SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "83mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, 12V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1213"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-1213"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "67mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, 15V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1213SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-1213SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "67mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, 15V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1215"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-1215"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "42mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, 24V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1222"
		(extends "TMR_1-0522")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-1222"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Dual_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "±42mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, ±12V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Dual*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1222SM"
		(extends "TMR_1-0522SM")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "TMR_1-1222SM"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 5.08 -12.7 0)
		)
		(property "Description" "±42mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, ±12V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR-1SM*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1223"
		(extends "TMR_1-0522")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-1223"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Dual_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "±33mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, ±15V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Dual*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-1223SM"
		(extends "TMR_1-0522SM")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "TMR_1-1223SM"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 5.08 -12.7 0)
		)
		(property "Description" "±33mA Regulated 1W DC/DC converter with 1.5kV isolation, 9V-18V input, ±15V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR-1SM*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2411"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-2411"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, 5V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2411SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-2411SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, 5V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2412"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-2412"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "83mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, 12V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2412SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-2412SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "83mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, 12V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2413"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-2413"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "67mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, 15V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2413SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-2413SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "67mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, 15V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2415"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-2415"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "42mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, 24V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2422"
		(extends "TMR_1-0522")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-2422"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Dual_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "±42mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, ±12V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Dual*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2422SM"
		(extends "TMR_1-0522SM")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "TMR_1-2422SM"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 5.08 -12.7 0)
		)
		(property "Description" "±42mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, ±12V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR-1SM*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2423"
		(extends "TMR_1-0522")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-2423"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Dual_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "±33mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, ±15V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Dual*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-2423SM"
		(extends "TMR_1-0522SM")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "TMR_1-2423SM"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 5.08 -12.7 0)
		)
		(property "Description" "±33mA Regulated 1W DC/DC converter with 1.5kV isolation, 18V-36V input, ±15V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR-1SM*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4811"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-4811"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, 5V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4811SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-4811SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, 5V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4812"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-4812"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "83mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, 12V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4812SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-4812SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "83mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, 12V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4813"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-4813"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "67mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, 15V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4813SM"
		(extends "TMR_1-0511SM")
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "TMR_1-4813SM"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "67mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, 15V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1SM*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4815"
		(extends "TMR_1-0511")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-4815"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "42mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, 24V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Single*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4822"
		(extends "TMR_1-0522")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-4822"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Dual_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "±42mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, ±12V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Dual*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4822SM"
		(extends "TMR_1-0522SM")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "TMR_1-4822SM"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 5.08 -12.7 0)
		)
		(property "Description" "±42mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, ±12V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR-1SM*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4823"
		(extends "TMR_1-0522")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMR_1-4823"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Dual_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1/documents/tmr1-datasheet.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "±33mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, ±15V fixed Output Voltage, SIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR?1*Dual*"
			(at 0 0 0)
		)
	)
	(symbol "TMR_1-4823SM"
		(extends "TMR_1-0522SM")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "TMR_1-4823SM"
			(at 15.24 8.89 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TMR-1SM_SMD"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://assets.tracopower.com/TMR1SM/documents/tmr1sm-datasheet.pdf"
			(at 5.08 -12.7 0)
		)
		(property "Description" "±33mA Regulated 1W DC/DC converter with 1.5kV isolation, 36V-75V input, ±15V fixed Output Voltage, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Murata isolated isolation dc-dc converter transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TMR-1SM*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "TNY264G"
		(extends "TNY263G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY264G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 6W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY264P"
		(extends "TNY263P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY264P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 6W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY265G"
		(extends "TNY263G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY265G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 7.5W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY265P"
		(extends "TNY263P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY265P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 7.5W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY266G"
		(extends "TNY263G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY266G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 9.5W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY266P"
		(extends "TNY263P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY266P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 9.5W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY267G"
		(extends "TNY263G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY267G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 12W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY267P"
		(extends "TNY263P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY267P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 12W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY268G"
		(extends "TNY263G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY268G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 15W Output Power, SMD-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY268P"
		(extends "TNY263P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY268P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny263_268.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-II Family, 15W Output Power, DIP-8B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Enhanced, Energy Efficient, Low Power Off-line Switcher"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY275G"
		(extends "TNY274G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY275G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 11.5W Output Power, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY275P"
		(extends "TNY274P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY275P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 11.5W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY276G"
		(extends "TNY274G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY276G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 15W Output Power, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY276P"
		(extends "TNY274P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY276P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 15W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY277G"
		(extends "TNY274G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY277G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 18W Output Power, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY277P"
		(extends "TNY274P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY277P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 18W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY278G"
		(extends "TNY274G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY278G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 21.5W Output Power, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY278P"
		(extends "TNY274P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY278P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 21.5W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY279G"
		(extends "TNY274G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY279G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 25W Output Power, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY279P"
		(extends "TNY274P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY279P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 25W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY280G"
		(extends "TNY274G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY280G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 28.5W Output Power, SMD-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY280P"
		(extends "TNY274P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY280P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/tny274-280.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-III Family, 28.5W Output Power, DIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Enhanced Flexibility and Extended Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY285D"
		(extends "TNY284D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY285D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 11.5W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY285K"
		(extends "TNY284K")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY285K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 11.5W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY285P"
		(extends "TNY284P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY285P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 11.5W Output Power, PDIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY286D"
		(extends "TNY284D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY286D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 15W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY286K"
		(extends "TNY284K")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY286K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 15W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY286P"
		(extends "TNY284P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY286P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 15W Output Power, PDIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY287D"
		(extends "TNY284D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY287D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 18W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY287K"
		(extends "TNY284K")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY287K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 18W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY287P"
		(extends "TNY284P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY287P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 18W Output Power, PDIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY288D"
		(extends "TNY284D")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY288D"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_SO-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 19.5W Output Power, SO-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SO?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY288K"
		(extends "TNY284K")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY288K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 21.5W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY288P"
		(extends "TNY284P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY288P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 21.5W Output Power, PDIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY289K"
		(extends "TNY284K")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY289K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 25W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY289P"
		(extends "TNY284P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY289P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 25W Output Power, PDIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TNY290K"
		(extends "TNY284K")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY290K"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 28.5W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TNY290P"
		(extends "TNY284P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TNY290P"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-4_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TinySwitch-4 Family, 28.5W Output Power, PDIP-8C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy-Efficient, Off-Line Switcher With Line Compensated Overload Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP101YN"
		(extends "TOP100YN")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP101YN"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top100.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 35W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TOP102YN"
		(extends "TOP100YN")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP102YN"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top100.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 45W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TOP103YN"
		(extends "TOP100YN")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP103YN"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top100.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 55W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TOP104YN"
		(extends "TOP100YN")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP104YN"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top100.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 60W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TOP201YAI"
		(extends "TOP200YAI")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP201YAI"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top200-204214.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 22W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TOP202YAI"
		(extends "TOP200YAI")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP202YAI"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top200-204214.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 30W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TOP203YAI"
		(extends "TOP200YAI")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP203YAI"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top200-204214.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 35W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TOP204YAI"
		(extends "TOP200YAI")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP204YAI"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top200-204214.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 50W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TOP210G"
		(extends "TOP209G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP210G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top209210.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 5W Max Output Power, SMD-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8*"
			(at 0 0 0)
		)
	)
	(symbol "TOP210PFI"
		(extends "TOP209P")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP210PFI"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top209210.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 5W Max Output Power, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TOP214YAI"
		(extends "TOP200YAI")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TOP214YAI"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.powerint.com/sites/default/files/product-docs/top200-204214.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch Family, 42W Max Output Power, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-terminal Off-line PWM Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TOP252EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP252EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 13W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP253EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP253EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 29W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP253EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP253EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 29W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP253GN"
		(extends "TOP252GN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP253GN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 15W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP253MN"
		(extends "TOP252MN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP253MN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SDIP-10C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 15W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SDIP?10C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP253PN"
		(extends "TOP252PN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP253PN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 15W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP254EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP254EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 43W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP254EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP254EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 43W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP254GN"
		(extends "TOP252GN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP254GN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 20W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP254MN"
		(extends "TOP252MN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP254MN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SDIP-10C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 20W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SDIP?10C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP254PN"
		(extends "TOP252PN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP254PN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 20W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP255EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP255EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 57W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP255EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP255EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 57W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP255GN"
		(extends "TOP252GN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP255GN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 22W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP255MN"
		(extends "TOP252MN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP255MN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SDIP-10C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 22W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SDIP?10C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP255PN"
		(extends "TOP252PN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP255PN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 22W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP255YN"
		(extends "TOP254YN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP255YN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:PowerIntegrations_TO-220-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 57W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations*TO?220?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP256EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP256EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 86W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP256EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP256EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 86W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP256GN"
		(extends "TOP252GN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP256GN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 26W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP256LN"
		(extends "TOP255LN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP256LN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 64W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "TOP256MN"
		(extends "TOP252MN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP256MN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SDIP-10C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 26W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SDIP?10C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP256PN"
		(extends "TOP252PN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP256PN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 26W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP256YN"
		(extends "TOP254YN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP256YN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:PowerIntegrations_TO-220-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 86W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations*TO?220?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP257EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP257EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 119W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP257EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP257EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 119W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP257GN"
		(extends "TOP252GN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP257GN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 30W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP257LN"
		(extends "TOP255LN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP257LN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 78W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "TOP257MN"
		(extends "TOP252MN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP257MN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SDIP-10C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 30W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SDIP?10C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP257PN"
		(extends "TOP252PN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP257PN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 30W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP257YN"
		(extends "TOP254YN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP257YN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:PowerIntegrations_TO-220-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 119W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations*TO?220?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP258EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP258EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 148W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP258EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP258EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 148W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP258GN"
		(extends "TOP252GN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP258GN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SMD-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 35W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SMD?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP258LN"
		(extends "TOP255LN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP258LN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 92W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "TOP258MN"
		(extends "TOP252MN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP258MN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_SDIP-10C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 35W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?SDIP?10C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP258PN"
		(extends "TOP252PN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP258PN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 35W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?PDIP?8C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP258YN"
		(extends "TOP254YN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP258YN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:PowerIntegrations_TO-220-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 148W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations*TO?220?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP259EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP259EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 171W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP259EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP259EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 171W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP259LN"
		(extends "TOP255LN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP259LN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 120W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "TOP260EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP260EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 200W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP260EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP260EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 200W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP260LN"
		(extends "TOP255LN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP260LN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 140W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "TOP260YN"
		(extends "TOP259YN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP260YN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:PowerIntegrations_TO-220-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 200W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations*TO?220?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP261EG"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP261EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 254W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP261EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP261EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 254W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP261LN"
		(extends "TOP255LN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP261LN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 177W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "TOP261YN"
		(extends "TOP259YN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP261YN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:PowerIntegrations_TO-220-7C"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 254W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations*TO?220?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP262EN"
		(extends "TOP252EN")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP262EN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 254W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP262LN"
		(extends "TOP255LN")
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "TOP262LN"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7F"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-hx_family_datasheet.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "TOPSwitch-HX Family, 177W Output Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "Eco Smart Off-Line Switcher Extendend Power Range"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7F*"
			(at 0 0 0)
		)
	)
	(symbol "TOP265EG"
		(extends "TOP264EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP265EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 57W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP265KG"
		(extends "TOP264KG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP265KG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 34W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TOP265VG"
		(extends "TOP264VG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP265VG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 57W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "TOP266EG"
		(extends "TOP264EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP266EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 86W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP266KG"
		(extends "TOP264KG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP266KG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 39W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TOP266VG"
		(extends "TOP264VG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP266VG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 86W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "TOP267EG"
		(extends "TOP264EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP267EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 103W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP267KG"
		(extends "TOP264KG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP267KG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 45W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TOP267VG"
		(extends "TOP264VG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP267VG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 103W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "TOP268EG"
		(extends "TOP264EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP268EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 112W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP268KG"
		(extends "TOP264KG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP268KG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 50W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TOP268VG"
		(extends "TOP264VG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP268VG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 112W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "TOP269EG"
		(extends "TOP264EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP269EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 120W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP269KG"
		(extends "TOP264KG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP269KG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 55W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TOP269VG"
		(extends "TOP264VG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP269VG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 120W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "TOP270EG"
		(extends "TOP264EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP270EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 140W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP270KG"
		(extends "TOP264KG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP270KG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 60W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TOP270VG"
		(extends "TOP264VG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP270VG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 140W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "TOP271EG"
		(extends "TOP264EG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP271EG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SIP:PowerIntegrations_eSIP-7C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 177W Output Power, eSIP-7C"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
		)
	)
	(symbol "TOP271KG"
		(extends "TOP264KG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP271KG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:PowerIntegrations_eSOP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 66W Output Power, eSOP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSOP?12B*"
			(at 0 0 0)
		)
	)
	(symbol "TOP271VG"
		(extends "TOP264VG")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "TOP271VG"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_eDIP-12B"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "TOPSwitch-JX Family, 177W Output Power, eDIP-12B"
			(at 0 0 0)
		)
		(property "ki_keywords" "Integrated Off-Line Switcher with EcoSmart™ Technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerIntegrations?eDIP?12*"
			(at 0 0 0)
		)
	)
	(symbol "TOS06-12SIL"
		(extends "TOS06-05SIL")
		(property "Reference" "U"
			(at -9.398 6.35 0)
		)
		(property "Value" "TOS06-12SIL"
			(at 3.556 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TOS06-12SIL_THT"
			(at -1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tos06sil.pdf"
			(at -1.27 -6.096 0)
		)
		(property "Description" "6A step-down regulator, 0.75-5.0VDC output voltage, 8.3-14.0VDC input voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated not-isolated pol dc-dc converter regulator single 6A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TOS06*12SIL*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TPS54202DDC"
		(extends "TPS54302")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS54202DDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps54202.pdf"
			(at -7.62 8.89 0)
		)
		(property "Description" "2A, 4.5 to 28V Input, EMI Friendly integrated switch synchronous step-down regulator, pulse-skipping, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator emi spread spectrum"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS54260DRC"
		(extends "TPS54260DGQ")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TPS54260DRC"
			(at 1.27 -11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_DRC0010J_ThermalVias"
			(at -2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps54260.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5A, Step Down DC-DC Converter with Eco-mode, 3.5-60V Input Voltage, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRC0010J*"
			(at 0 0 0)
		)
	)
	(symbol "TPS54308"
		(extends "TPS54302")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS54308"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps54308.pdf"
			(at -7.62 8.89 0)
		)
		(property "Description" "3A, 4.5 to 28V Input, EMI Friendly integrated switch synchronous step-down regulator, continuous-conduction, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "switching buck converter power-supply voltage regulator emi spread spectrum FCCM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS5431DDA"
		(extends "TPS5430DDA")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TPS5431DDA"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8_ThermalVias"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps5430.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A, Step Down Swift Converter, Adjustable Output Voltage, 5.5-23V Input Voltage, PowerSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*ThermalVias*"
			(at 0 0 0)
		)
	)
	(symbol "TPS54340DDA"
		(extends "TPS54360DDA")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS54340DDA"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8_ThermalVias"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps54340.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.5A, Step Down DC-DC Converter with Eco-mode, 4.5-42V Input Voltage, PowerSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator High Voltage High Frequency"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*ThermalVias*"
			(at 0 0 0)
		)
	)
	(symbol "TPS562202S"
		(extends "TPS562202")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS562202S"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps562202s.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Synchronous Step-Down Voltage Regulator 580kHz, Adjustable Output Voltage, 4.5-17V Input Voltage, 0.804V-7V Output Voltage, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS562203"
		(extends "TPS562202")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS562203"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps562203.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Synchronous Step-Down Voltage Regulator 600kHz, Adjustable Output Voltage, 4.5-17V Input Voltage, 0.6V-7V Output Voltage, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS562206"
		(extends "TPS562202")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS562206"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps562203.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Synchronous Step-Down Voltage Regulator 600kHz, Adjustable Output Voltage, 4.5-17V Input Voltage, 0.6V-7V Output Voltage, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS563200"
		(extends "TPS562200")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS563200"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps563200.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage, 4.5-17V Input Voltage, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS563203"
		(extends "TPS563202S")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS563203"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps563203.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage, 4.2-17V Input Voltage, 0.6-7V Output Voltage, Eco mode, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS563206"
		(extends "TPS563202S")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS563206"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps563206.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage, 4.2-17V Input Voltage, 0.6-7V Output Voltage, FCCM mode, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS563240DDC"
		(extends "TPS562200")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS563240DDC"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/tps563240.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage, 4.5-17V Input Voltage, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS565208"
		(extends "TPS562200")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS565208"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps565208.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage, 4.5-17V Input Voltage, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61040DBV"
		(extends "TPS61041DDC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS61040DBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61040.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output up to 28V, 400 mA Switch Current Limit, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61040DDC"
		(extends "TPS61041DDC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS61040DDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps61040.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output up to 28V, 400 mA Switch Current Limit, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61040DRV"
		(extends "TPS61041DRV")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS61040DRV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps61040.pdf"
			(at 3.81 8.89 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output up to 28V, 400 mA Switch Current Limit, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61041DBV"
		(extends "TPS61041DDC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS61041DBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61040.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output up to 28V, 250 mA Switch Current Limit, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61085PW"
		(extends "TPS61085DGK")
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "TPS61085PW"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 22.86 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps61085.pdf"
			(at 0 0 0)
		)
		(property "Description" "Step-Up DC-DC Converter, input 2.3V to 6V , output 2.8V to 18.5, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost converter switching TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS610891"
		(extends "TPS61089")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TPS610891"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_VQFN-RNR0011A-11"
			(at 22.86 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61089.pdf"
			(at 0 0 0)
		)
		(property "Description" "7A Boost Converters, Adjustable output voltage (ForcedPWM), input 2.7 to 12V , output 4.5 to 12.6V, VQFN-11"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable 7A boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN?RNR0011A?11*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61091"
		(extends "TPS61090")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "TPS61091"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm_ThermalVias"
			(at -24.13 -26.67 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61090.pdf"
			(at 3.81 -29.21 0)
		)
		(property "Description" "2A Step-Up DC-DC Converter for Batteries, Isw up to 2500mA, 3.3V Output Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed 3.3V 2A battery boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61092"
		(extends "TPS61090")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "TPS61092"
			(at 1.27 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RSA_VQFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm_ThermalVias"
			(at -24.13 -26.67 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61090.pdf"
			(at 3.81 -29.21 0)
		)
		(property "Description" "2A Step-Up DC-DC Converter for Batteries, Isw up to 2500mA, 5V Output Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed 5V 2A battery boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RSA*EP2.7x2.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS610991DRV"
		(extends "TPS61099DRV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS610991DRV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TPS61099"
			(at 0 2.54 0)
		)
		(property "Description" "Boost Converter, 0.7-5.5V Input Voltage, 1A Switch Current, Fixed 1.8V Output Voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS610992DRV"
		(extends "TPS61099DRV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS610992DRV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TPS61099"
			(at 0 2.54 0)
		)
		(property "Description" "Boost Converter, 0.7-5.5V Input Voltage, 1A Switch Current, Fixed 2.5V Output Voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS610993DRV"
		(extends "TPS61099DRV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS610993DRV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TPS61099"
			(at 0 2.54 0)
		)
		(property "Description" "Boost Converter, 0.7-5.5V Input Voltage, 1A Switch Current, Fixed 3V Output Voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS610994DRV"
		(extends "TPS61099DRV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS610994DRV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TPS61099"
			(at 0 2.54 0)
		)
		(property "Description" "Boost Converter, 0.7-5.5V Input Voltage, 1A Switch Current, Fixed 3.3V Output Voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS610995DRV"
		(extends "TPS61099DRV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS610995DRV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TPS61099"
			(at 0 2.54 0)
		)
		(property "Description" "Boost Converter, 0.7-5.5V Input Voltage, 1A Switch Current, Fixed 3.6V Output Voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS610996DRV"
		(extends "TPS61099DRV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS610996DRV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TPS61099"
			(at 0 2.54 0)
		)
		(property "Description" "Boost Converter, 0.7-5.5V Input Voltage, 1A Switch Current, Fixed 4.5V Output Voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS610997DRV"
		(extends "TPS61099DRV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS610997DRV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TPS61099"
			(at 0 2.54 0)
		)
		(property "Description" "Boost Converter, 0.7-5.5V Input Voltage, 1A Switch Current, 5V Fixed Output Voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Up DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61201DRC"
		(extends "TPS61200DRC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TPS61201DRC"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61200.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Input Voltage Synchronous Boost Converter With 1.3A Switches, Fixed 5V Output Voltage, 0.3-5.5V Input Voltage, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PVSON*N10*ThermalVias*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61202DRC"
		(extends "TPS61200DRC")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TPS61202DRC"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61200.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Input Voltage Synchronous Boost Converter With 1.3A Switches, Fixed 5V Output Voltage, 0.3-5.5V Input Voltage, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "boost step-up DC/DC synchronous"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PVSON*N10*ThermalVias*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61221DCK"
		(extends "TPS61220DCK")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS61221DCK"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61220.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "400 mA Step-Up Converter, Fixed 3.3V Output Voltage, 0.7-5.5V Input Voltage, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost adjustable converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PDSO*G6*"
			(at 0 0 0)
		)
	)
	(symbol "TPS61222DCK"
		(extends "TPS61220DCK")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS61222DCK"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61220.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "400 mA Step-Up Converter, Fixed 5V Output Voltage, 0.7-5.5V Input Voltage, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost adjustable converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PDSO*G6*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613222ADBV"
		(extends "TPS613221ADBV")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613222ADBV"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1.8A Step-Up Converter, 5V Output Voltage, 0.9-5.5V Input Voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613222ADBZ"
		(extends "TPS613221ADBZ")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613222ADBZ"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1.8A Step-Up Converter, 5V Output Voltage, 0.9-5.5V Input Voltage, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613223ADBV"
		(extends "TPS613221ADBV")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613223ADBV"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "750mA Step-Up Converter, 2V Output Voltage, 0.9-5.5V Input Voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613223ADBZ"
		(extends "TPS613221ADBZ")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613223ADBZ"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "750mA Step-Up Converter, 2V Output Voltage, 0.9-5.5V Input Voltage, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613224ADBV"
		(extends "TPS613221ADBV")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613224ADBV"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "750mA Step-Up Converter, 2.5V Output Voltage, 0.9-5.5V Input Voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613224ADBZ"
		(extends "TPS613221ADBZ")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613224ADBZ"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "750mA Step-Up Converter, 2.5V Output Voltage, 0.9-5.5V Input Voltage, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613225ADBV"
		(extends "TPS613221ADBV")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613225ADBV"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1.2A Step-Up Converter, 3V Output Voltage, 0.9-5.5V Input Voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613225ADBZ"
		(extends "TPS613221ADBZ")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613225ADBZ"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1.2A Step-Up Converter, 3V Output Voltage, 0.9-5.5V Input Voltage, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613226ADBV"
		(extends "TPS613221ADBV")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613226ADBV"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1.2A Step-Up Converter, 3.6V Output Voltage, 0.9-5.5V Input Voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS613226ADBZ"
		(extends "TPS613221ADBZ")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TPS613226ADBZ"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61322.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1.2A Step-Up Converter, 3.6V Output Voltage, 0.9-5.5V Input Voltage, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62125DSG"
		(extends "TPS62170DSG")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62125DSG"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62125.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "300mA Step-Down Converter with Enable Threshold and Hysteresis, adjustable output, 3-17V input voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62130A"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62130A"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62130.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Step-Down Converter with DCS-Control, Adjustable Output Voltage, 3-17V Input Voltage, PG=LOW in Power-Down, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62131"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62131"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62130.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Step-Down Converter with DCS-Control, Fixed 1.8V Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62132"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62132"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62130.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Step-Down Converter with DCS-Control, Fixed 3.3V Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62133"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62133"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62130.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Step-Down Converter with DCS-Control, Fixed 5.0V Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62140"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62140"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62140.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down Converter with DCS-Control, Adjustable Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62140A"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62140A"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62140.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down Converter with DCS-Control, Adjustable Output Voltage, 3-17V Input Voltage, PG=LOW in Power-Down, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62141"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62141"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62140.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down Converter with DCS-Control, Fixed 1.8V Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62142"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62142"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62140.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down Converter with DCS-Control, Fixed 3.3V Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62143"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62143"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62140.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Step-Down Converter with DCS-Control, Fixed 5.0V Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62150"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62150"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62150.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, Adjustable Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62150A"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62150A"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62150.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, Adjustable Output Voltage, 3-17V Input Voltage, PG=LOW in Power-Down, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62151"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62151"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62150.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, Fixed 1.8V Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62152"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62152"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62150.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, Fixed 3.3V Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62153"
		(extends "TPS62130")
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "TPS62153"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/TPS62150.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, Fixed 5.0V Output Voltage, 3-17V Input Voltage, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dcdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62160DSG"
		(extends "TPS62170DSG")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62160DSG"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62160.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, adjustable output, 3-17V input voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62161DSG"
		(extends "TPS62170DSG")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62161DSG"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62160.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, fixed 1.8V output, 3-17V input voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62162DSG"
		(extends "TPS62170DSG")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62162DSG"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62160.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, fixed 3.3V output, 3-17V input voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62163DSG"
		(extends "TPS62170DSG")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62163DSG"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62160.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, fixed 5.0V output, 3-17V input voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62171DSG"
		(extends "TPS62170DSG")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62171DSG"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62170.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "500mA Step-Down Converter with DCS-Control, fixed 1.8V output, 3-17V input voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62172DSG"
		(extends "TPS62170DSG")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62172DSG"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62170.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "500mA Step-Down Converter with DCS-Control, fixed 3.3V output, 3-17V input voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62173DSG"
		(extends "TPS62170DSG")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62173DSG"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62170.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "500mA Step-Down Converter with DCS-Control, fixed 5.0V output, 3-17V input voltage, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62175DQC"
		(extends "TPS62177DQC")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62175DQC"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-10-1EP_2x3mm_P0.5mm_EP0.84x2.4mm_ThermalVias"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62177.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "500mA Step-Down Converter with Sleep Mode, adjustable Output Voltage, 4.75-28V input voltage, WSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*EP*2x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62201DBV"
		(extends "TPS62200DBV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS62201DBV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62201.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA High-Efficiency Step-Down DC-DC Converter, fixed 1.5V output voltage, 2.5-6V input voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62202DBV"
		(extends "TPS62200DBV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS62202DBV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62201.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA High-Efficiency Step-Down DC-DC Converter, fixed 1.8V output voltage, 2.5-6V input voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62203DBV"
		(extends "TPS62200DBV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS62203DBV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62201.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA High-Efficiency Step-Down DC-DC Converter, fixed 3.3V output voltage, 2.5-6V input voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62204DBV"
		(extends "TPS62200DBV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS62204DBV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62201.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA High-Efficiency Step-Down DC-DC Converter, fixed 1.6V output voltage, 2.5-6V input voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62205DBV"
		(extends "TPS62200DBV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS62205DBV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62201.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA High-Efficiency Step-Down DC-DC Converter, fixed 2.5V output voltage, 2.5-6V input voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62207DBV"
		(extends "TPS62200DBV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS62207DBV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62201.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA High-Efficiency Step-Down DC-DC Converter, fixed 1.2V output voltage, 2.5-6V input voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62208DBV"
		(extends "TPS62200DBV")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "TPS62208DBV"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62201.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA High-Efficiency Step-Down DC-DC Converter, fixed 1.875V output voltage, 2.5-6V input voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62821DLC"
		(extends "TPS62823DLC")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62821DLC"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_VSON-HR-8_1.5x2mm_P0.5mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62823.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "1A Step-Down Converter with DCS-Control, adjustable output, 2.4-5.5V input voltage, QFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VSON*HR*1.5x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62822DLC"
		(extends "TPS62823DLC")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS62822DLC"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_VSON-HR-8_1.5x2mm_P0.5mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps62823.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "2A Step-Down Converter with DCS-Control, adjustable output, 2.4-5.5V input voltage, QFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VSON*HR*1.5x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS628437DRL"
		(extends "TPS628436DRL")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS628437DRL"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62843.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "600mA Step-Down Converter with DCS-Control, ultra-low Iq, 1.8-5.5 Vin, 0.8-1.8 Vout, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS628437YKA"
		(extends "TPS628436YKA")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS628437YKA"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-6_0.757x1.01mm_Layout2x3_P0.35mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62843.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "600mA Step-Down Converter with DCS-Control, ultra-low Iq, 1.8-5.5 Vin, 0.8-1.8 Vout, WLCSP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*0.757x1.01mm*Layout2x3*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS628438DRL"
		(extends "TPS628436DRL")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS628438DRL"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62843.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "600mA Step-Down Converter with DCS-Control, ultra-low Iq, 1.8-5.5 Vin, 1.8-3.6 Vout, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS628438YKA"
		(extends "TPS628436YKA")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TPS628438YKA"
			(at -1.27 11.43 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-6_0.757x1.01mm_Layout2x3_P0.35mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62843.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "600mA Step-Down Converter with DCS-Control, ultra-low Iq, 1.8-5.5 Vin, 1.8-3.6 Vout, WLCSP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TI buck regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*0.757x1.01mm*Layout2x3*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62913"
		(extends "TPS62912")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TPS62913"
			(at 5.334 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RPU0010A_VQFN-HR-10_2x2mm_P0.5mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62912.pdf"
			(at 0 -25.654 0)
		)
		(property "Description" "2.2MHz or 1MHz, 3A, Low Noise, Low Ripple, Buck Converter with Integrated Ferrite Bead Filter Compensation, VQFN-HR"
			(at 0 -27.94 0)
		)
		(property "ki_keywords" "step-down high psrr adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Texas*RPU0010A*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62932"
		(extends "TPS62933")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "TPS62932"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-583-8"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62933.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "3.8-30V, 2A  Synchronous Buck Converters with pulse frequency modulation (PFM), SOT583-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous buck converter pulse frequency modulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?583*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62933F"
		(extends "TPS62933")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "TPS62933F"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-583-8"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62933.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "3.8-30V, 3A Synchronous Buck Converters with forced continuous conduction mode (FCCM), SOT583-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous buck converter forced continuous conduction mode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?583*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62933O"
		(extends "TPS62933P")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "TPS62933O"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-583-8"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62933.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "3.8-30V, 3A Synchronous Buck Converters with out of audio (OOA) mode and power good, SOT583-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "synchronous buck converter out of audio power good"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?583*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62A01ADRL"
		(extends "TPS62A01DRL")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A01ADRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a01a"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter with forced PWM, Adjustable Output 0.6V-5.5V, 1A, Power Good, Enable, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62A01APDDC"
		(extends "TPS62A01PDDC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A01APDDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a01a"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter with forced PWM, Adjustable Output 0.6V-5.5V, 1A, Power Good, Enable, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62A02ADRL"
		(extends "TPS62A01DRL")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A02ADRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a02a"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter with forced PWM, Adjustable Output 0.6V-5.5V, 2A, Power Good, Enable, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62A02APDDC"
		(extends "TPS62A01PDDC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A02APDDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a02a"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter with forced PWM, Adjustable Output 0.6V-5.5V, 2A, Power Good, Enable, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62A02DRL"
		(extends "TPS62A01DRL")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A02DRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a02"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 2A, Power Good, Enable, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62A02NADRL"
		(extends "TPS62A02NDRL")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A02NADRL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a02a"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter with forced PWM, Adjustable Output 0.6V-5.5V, 2A, Enable, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TPS62A02PDDC"
		(extends "TPS62A01PDDC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "TPS62A02PDDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps62a02"
			(at -6.35 11.43 0)
		)
		(property "Description" "High Efficiency Synchronous Buck Converter, Adjustable Output 0.6V-5.5V, 2A, Power Good, Enable, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Step-Down DC-DC Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "TPS63000-Q1"
		(extends "TPS63000")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPS63000-Q1"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_DRC0010J_ThermalVias"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63000-q1.pdf"
			(at -7.62 13.97 0)
		)
		(property "Description" "Buck-Boost Converter, 1.8-5.5V Input Voltage, 1.8A Switch Current, Adjustable 1.2-5.5V Output Voltage, Automotive, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost adjustable converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRC0010J*"
			(at 0 0 0)
		)
	)
	(symbol "TPS63001"
		(extends "TPS63000")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPS63001"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_DRC0010J_ThermalVias"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63000.pdf"
			(at -7.62 13.97 0)
		)
		(property "Description" "Buck-Boost Converter, 1.8-5.5V Input Voltage, 1.7A Switch Current, 3.3V Output Voltage, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost fixed 3.3V converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRC0010J*"
			(at 0 0 0)
		)
	)
	(symbol "TPS63002"
		(extends "TPS63000")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPS63002"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:Texas_DRC0010J_ThermalVias"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63000.pdf"
			(at -7.62 13.97 0)
		)
		(property "Description" "Buck-Boost Converter, 1.8-5.5V Input Voltage, 1.7A Switch Current, 5V Output Voltage, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost fixed 5V converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DRC0010J*"
			(at 0 0 0)
		)
	)
	(symbol "TPS63031DSK"
		(extends "TPS63030DSK")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TPS63031DSK"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_SON:WSON-10-1EP_2.5x2.5mm_P0.5mm_EP1.2x2mm"
			(at 21.59 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63031.pdf"
			(at -7.62 13.97 0)
		)
		(property "Description" "Buck-Boost Converter, 1.8-5.5V Input Voltage, 1A Switch Current, 3.3V Output Voltage, VSON-10 (DSK0010A)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost fixed 3.3V converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2.5x2.5mm*P0.5mm*EP1.2x2mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS65131RGE"
		(extends "TPS65130RGE")
		(property "Reference" "U"
			(at -6.858 21.082 0)
		)
		(property "Value" "TPS65131RGE"
			(at -1.016 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps65130.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Split-Rail Converter with Dual, Positive and Negative Outputs (750mA typ, Switch Current Limit 1950mA typ),), 2.7-5.5V, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "split-rail switching dual positive negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS82140"
		(extends "TPS82130")
		(property "Reference" "U"
			(at 1.27 11.43 0)
		)
		(property "Value" "TPS82140"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_LGA:Texas_SIL0008D_MicroSiP-8-1EP_2.8x3mm_P0.65mm_EP1.1x1.9mm_ThermalVias"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps82140.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "17V Input 2A Step-Down Converter MicroSiP Module with Integrated Inductor, μSiL-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "17V 2A Step-down Buck Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroSiP*1EP*2.8x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS82150"
		(extends "TPS82130")
		(property "Reference" "U"
			(at 1.27 11.43 0)
		)
		(property "Value" "TPS82150"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_LGA:Texas_SIL0008D_MicroSiP-8-1EP_2.8x3mm_P0.65mm_EP1.1x1.9mm_ThermalVias"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps82150.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "17V Input 1A Step-Down Converter MicroSiP Module with Integrated Inductor, μSiL-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "17V 1A Step-down Buck Module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*MicroSiP*1EP*2.8x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSR0.6-48120WI"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -6.858 6.35 0)
		)
		(property "Value" "TSR0.6-48120WI"
			(at 3.302 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR0.6-48xxWI_TSR0.6-48xxxWI_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr0.6wi.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "0.6A step-down regulator, fixed 12V output voltage, 17-72V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single 0.6A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR0.6*48xxWI*48xxxWI*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR0.6-48150WI"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -6.858 6.35 0)
		)
		(property "Value" "TSR0.6-48150WI"
			(at 3.302 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR0.6-48xxWI_TSR0.6-48xxxWI_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr0.6wi.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "0.6A step-down regulator, fixed 15V output voltage, 20-72V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single 0.6A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR0.6*48xxWI*48xxxWI*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR0.6-48240WI"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -6.858 6.35 0)
		)
		(property "Value" "TSR0.6-48240WI"
			(at 3.302 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR0.6-48xxWI_TSR0.6-48xxxWI_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr0.6wi.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "0.4A step-down regulator, fixed 24V output voltage, 33-72V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single 0.4A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR0.6*48xxWI*48xxxWI*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR0.6-4833WI"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -6.858 6.35 0)
		)
		(property "Value" "TSR0.6-4833WI"
			(at 2.794 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR0.6-48xxWI_TSR0.6-48xxxWI_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr0.6wi.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "0.6A step-down regulator, fixed 3.3V output voltage, 9-72V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single 0.6A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR0.6*48xxWI*48xxxWI*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR0.6-4850WI"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -6.858 6.35 0)
		)
		(property "Value" "TSR0.6-4850WI"
			(at 2.794 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR0.6-48xxWI_TSR0.6-48xxxWI_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr0.6wi.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "0.6A step-down regulator, fixed 5V output voltage, 9-72V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single 0.6A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR0.6*48xxWI*48xxxWI*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR0.6-4865WI"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -6.858 6.35 0)
		)
		(property "Value" "TSR0.6-4865WI"
			(at 2.794 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR0.6-48xxWI_TSR0.6-48xxxWI_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr0.6wi.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "0.6A step-down regulator, fixed 6.5V output voltage, 9-72V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single 0.6A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR0.6*48xxWI*48xxxWI*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR0.6-4890WI"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -6.858 6.35 0)
		)
		(property "Value" "TSR0.6-4890WI"
			(at 2.794 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR0.6-48xxWI_TSR0.6-48xxxWI_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr0.6wi.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "0.6A step-down regulator, fixed 9V output voltage, 14-72V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single 0.6A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR0.6*48xxWI*48xxxWI*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR1-2433E"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR1-2433E"
			(at -3.81 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR1-xxxxE_THT"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr1e.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1A step-down regulator, fixed 3.3V output voltage, 6-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated not-isolated pol dc-dc converter regulator single 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR1*xxxxE*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR1-2450E"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR1-2450E"
			(at -3.81 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR1-xxxxE_THT"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr1e.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "1A step-down regulator, fixed 5V output voltage, 7-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated not-isolated pol dc-dc converter regulator single 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR1*xxxxE*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-24120N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-24120N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 12V output voltage, 15-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-2412N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-2412N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 1.2V output voltage, 4.6-28V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-24150N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-24150N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 15V output voltage, 18-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-2415N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-2415N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 1.5V output voltage, 4.6-32V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-2418N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-2418N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 1.8V output voltage, 4.6-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-2425N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-2425N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 2.5V output voltage, 4.6-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-2433N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-2433N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 3.3V output voltage, 4.6-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-2450N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-2450N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 5V output voltage, 6.5-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-2465N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-2465N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 6.5V output voltage, 9-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR2-2490N"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.112 6.35 0)
		)
		(property "Value" "TSR2-2490N"
			(at 1.524 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR2-24xxN_TSR2-24xxxN_THT"
			(at 0 -6.096 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tsr2n.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "2A step-down regulator, fixed 9V output voltage, 11-36V input voltage, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco non-isolated pol dcdc converter single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR2*24xxN*24xxxN*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TSR_1-2412"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-2412"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 1.2V output voltage, 6-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
	)
	(symbol "TSR_1-24120"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-24120"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 12V output voltage, 5-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
	)
	(symbol "TSR_1-2415"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-2415"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 1.5V output voltage, 6-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
	)
	(symbol "TSR_1-24150"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-24150"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 15V output voltage, 8-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
	)
	(symbol "TSR_1-2418"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-2418"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 1.8V output voltage, 6-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
	)
	(symbol "TSR_1-2425"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-2425"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 2.5V output voltage, 6-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
	)
	(symbol "TSR_1-2433"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-2433"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 3.3V output voltage, 5-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
	)
	(symbol "TSR_1-2465"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-2465"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 6.5V output voltage, 9-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
	)
	(symbol "TSR_1-2490"
		(extends "TSR_1-2450")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSR_1-2490"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT"
			(at 0 -3.81 0)
		)
		(property "Datasheet" "http://www.tracopower.com/products/tsr1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A step-down regulator module, fixed 9V output voltage, 2-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"
			(at 0 0 0)
		)
		(property "ki_keywords" "dc-dc traco buck"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*TRACO*TSR?1*"
			(at 0 0 0)
		)
	)
	(symbol "VIPer25HN"
		(extends "VIPer25LN")
		(property "Reference" "U"
			(at 11.43 6.35 0)
		)
		(property "Value" "VIPer25HN"
			(at 11.43 3.81 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8B"
			(at 11.43 1.27 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00231127.pdf"
			(at 0 0 0)
		)
		(property "Description" "12W SMPS Controller, AC-DC, PDIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET 12W AC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PDIP*8B*"
			(at 0 0 0)
		)
	)
	(symbol "VIPer26HD"
		(extends "VIPer26LD")
		(property "Reference" "U"
			(at 7.62 12.7 0)
		)
		(property "Value" "VIPer26HD"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/viper26.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V, 10-20W, 115kHz, SMPS Controller, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "VIPer26HN"
		(extends "VIPer26LN")
		(property "Reference" "U"
			(at 7.62 12.7 0)
		)
		(property "Value" "VIPer26HN"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N6_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/viper26.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V, 10-20W, 115kHz, SMPS Controller, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMPS Controller with MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N6*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "XL1509-12"
		(extends "XL1509-3.3")
		(property "Reference" "U"
			(at -7.112 6.096 0)
		)
		(property "Value" "XL1509-12"
			(at 5.842 6.096 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.382 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1809050422_XLSEMI-XL1509-5-0E1_C61063.pdf"
			(at 2.54 10.668 0)
		)
		(property "Description" "Buck DC/DC Converter, 2A, 12V Output Voltage, 15-40V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "XL1509-5.0"
		(extends "XL1509-3.3")
		(property "Reference" "U"
			(at -7.112 6.096 0)
		)
		(property "Value" "XL1509-5.0"
			(at 5.842 6.096 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.382 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1809050422_XLSEMI-XL1509-5-0E1_C61063.pdf"
			(at 2.54 10.668 0)
		)
		(property "Description" "Buck DC/DC Converter, 2A, 5V Output Voltage, 7-40V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "XL1509-ADJ"
		(extends "XL1509-3.3")
		(property "Reference" "U"
			(at -7.112 6.096 0)
		)
		(property "Value" "XL1509-ADJ"
			(at 5.842 6.096 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.382 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1809050422_XLSEMI-XL1509-5-0E1_C61063.pdf"
			(at 2.54 10.668 0)
		)
		(property "Description" "Buck DC/DC Converter, 2A, 1.23-37V Adjustable Output Voltage, 4.5-40V Input Voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck DC/DC Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SIC431B"
		(extends "SIC431A")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC431B"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/74589/sic431.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "24A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
	(symbol "SIC431D"
		(extends "SIC431C")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC431D"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/74589/sic431.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "24A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
	(symbol "SIC438B"
		(extends "SIC438A")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC438B"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/75921/sic437.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "8A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
	(symbol "SIC438D"
		(extends "SIC438C")
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "SIC438D"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:Vishay_PowerPAK_MLP44-24L_ThermalVias"
			(at 5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/75921/sic437.pdf"
			(at 5.08 -25.4 0)
		)
		(property "Description" "8A Step-Down DC/DC-Regulator, 300kHz-1MHz, 3..24Vin, 0.6..21.6Vout"
			(at 5.08 -30.48 0)
		)
		(property "ki_keywords" "Buck Vishay Siliconix voltage-regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay?PowerPAK?MLP44?24L*"
			(at 0 0 0)
		)
	)
)
