(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AZ850-x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "AZ850-x"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_FRT5"
			(at 13.97 1.27 0)
		)
		(property "Datasheet" "http://www.azettler.com/pdfs/az850.pdf"
			(at 0 0 0)
		)
		(property "Description" "American Zettler, Microminiature Polarised Dual Pole Relay"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Polarised Relay Dual Pole"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*FRT5*"
			(at 0 0 0)
		)
		(symbol "AZ850-x_0_0"
			(text "+"
				(at -9.271 2.921 0)
			)
		)
		(symbol "AZ850-x_0_1")
		(symbol "AZ850-x_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AZ850P2-x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "AZ850P2-x"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_FRT5"
			(at 13.97 1.27 0)
		)
		(property "Datasheet" "http://www.azettler.com/pdfs/az850.pdf"
			(at 0 0 0)
		)
		(property "Description" "American Zettler, Microminiature Polarised Dual Pole Relay Bistable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Polarised Relay Dual Pole Bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*FRT5*"
			(at 0 0 0)
		)
		(symbol "AZ850P2-x_0_0"
			(text "+"
				(at -12.065 2.667 0)
			)
			(text "+"
				(at -12.065 -2.413 0)
			)
			(text "S"
				(at -10.033 2.794 0)
			)
			(text "R"
				(at -10.033 -2.921 0)
			)
		)
		(symbol "AZ850P2-x_0_1")
		(symbol "AZ850P2-x_1_1"
			(pin passive line
				(at -12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -12.7 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AZSR131-1AE-12D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "RL2"
			(at 12.065 0 90)
		)
		(property "Value" "AZSR131-1AE-12D"
			(at 9.525 0 90)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Zettler-AZSR131"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "https://www.azettler.com/pdfs/azsr131.pdf"
			(at 0 0 0)
		)
		(property "Description" "SPST, Closing Contact, 277VAC 35A max, 12V DC coil voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*AZSR131*"
			(at 0 0 0)
		)
		(symbol "AZSR131-1AE-12D_0_0")
		(symbol "AZSR131-1AE-12D_0_1")
		(symbol "AZSR131-1AE-12D_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "COTO_3602_Split"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 5.08 2.54 0)
		)
		(property "Value" "COTO_3602_Split"
			(at 5.08 0 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPST_COTO_3602"
			(at 5.08 -2.54 0)
		)
		(property "Datasheet" "https://cotorelay.com/wp-content/uploads/2014/09/3600_series_reed_relay_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low thermal EMF DPST-NO reed relay, 150V 0.25A, 30.48x16.76x12.06mm"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "reed relay low thermal emf"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*COTO*3602*"
			(at 0 0 0)
		)
		(symbol "COTO_3602_Split_1_0"
			(text "+"
				(at 0.889 2.921 0)
			)
		)
		(symbol "COTO_3602_Split_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "SH")
			)
		)
		(symbol "COTO_3602_Split_2_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "COTO_3602_Split_3_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "23")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "COTO_3650_Split"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 5.08 2.54 0)
		)
		(property "Value" "COTO_3650_Split"
			(at 5.08 0 0)
		)
		(property "Footprint" "Relay_THT:Relay_3PST_COTO_3650"
			(at 5.08 -2.54 0)
		)
		(property "Datasheet" "https://cotorelay.com/wp-content/uploads/2014/09/3600_series_reed_relay_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low thermal EMF 3PST-NO reed relay, 150V 0.25A, similar to 3660 but with independent shield, 30.48x16.76x12.06mm"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "reed relay low thermal emf"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*COTO*3650*"
			(at 0 0 0)
		)
		(symbol "COTO_3650_Split_1_0"
			(text "+"
				(at 0.889 2.921 0)
			)
		)
		(symbol "COTO_3650_Split_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "SH")
			)
		)
		(symbol "COTO_3650_Split_2_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "COTO_3650_Split_3_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "23")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(symbol "COTO_3650_Split_4_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "33")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "COTO_3660_Split"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 5.08 2.54 0)
		)
		(property "Value" "COTO_3660_Split"
			(at 5.08 0 0)
		)
		(property "Footprint" "Relay_THT:Relay_3PST_COTO_3660"
			(at 5.08 -2.54 0)
		)
		(property "Datasheet" "https://cotorelay.com/wp-content/uploads/2014/09/3600_series_reed_relay_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low thermal EMF 3PST-NO reed relay, 150V 0.25A, similar to 3650 but with shared shield/contact, 30.48x16.76x12.06mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "reed relay low thermal emf"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*COTO*3660*"
			(at 0 0 0)
		)
		(symbol "COTO_3660_Split_1_0"
			(text "+"
				(at 0.889 2.921 0)
			)
		)
		(symbol "COTO_3660_Split_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
		)
		(symbol "COTO_3660_Split_2_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "COTO_3660_Split_3_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "23")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(symbol "COTO_3660_Split_4_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "33")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIPxx-1Axx-11x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "DIPxx-1Axx-11x"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_StandexMeder_DIP_LowProfile"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_DIP.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder DIP reed relay, SPST, Closing Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*StandexMeder*DIP*LowProfile*"
			(at 0 0 0)
		)
		(symbol "DIPxx-1Axx-11x_0_0")
		(symbol "DIPxx-1Axx-11x_0_1")
		(symbol "DIPxx-1Axx-11x_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIPxx-1Axx-12x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "DIPxx-1Axx-12x"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_StandexMeder_DIP_LowProfile"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_DIP.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder DIP reed relay, SPST, Closing Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*StandexMeder*DIP*LowProfile*"
			(at 0 0 0)
		)
		(symbol "DIPxx-1Axx-12x_0_0")
		(symbol "DIPxx-1Axx-12x_0_1")
		(symbol "DIPxx-1Axx-12x_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIPxx-1Axx-12xD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "DIPxx-1Axx-12xD"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_StandexMeder_DIP_LowProfile"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_DIP.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder DIP reed relay, SPST, Closing Contact, including diode"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*StandexMeder*DIP*LowProfile*"
			(at 0 0 0)
		)
		(symbol "DIPxx-1Axx-12xD_0_0")
		(symbol "DIPxx-1Axx-12xD_0_1")
		(symbol "DIPxx-1Axx-12xD_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIPxx-1Axx-13x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "DIPxx-1Axx-13x"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_StandexMeder_DIP_LowProfile"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_DIP.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder DIP reed relay, SPST, Closing Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*StandexMeder*DIP*LowProfile*"
			(at 0 0 0)
		)
		(symbol "DIPxx-1Axx-13x_0_0")
		(symbol "DIPxx-1Axx-13x_0_1")
		(symbol "DIPxx-1Axx-13x_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIPxx-1Cxx-51x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "DIPxx-1Cxx-51x"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_StandexMeder_DIP_LowProfile"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_DIP.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder DIP reed relay, SPDT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*StandexMeder*DIP*LowProfile*"
			(at 0 0 0)
		)
		(symbol "DIPxx-1Cxx-51x_0_0")
		(symbol "DIPxx-1Cxx-51x_0_1")
		(symbol "DIPxx-1Cxx-51x_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIPxx-2Axx-21x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 12.7 3.81 0)
		)
		(property "Value" "DIPxx-2Axx-21x"
			(at 12.7 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_StandexMeder_DIP_LowProfile"
			(at 12.7 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_DIP.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder DIP reed relay, DPST, Closing Contacts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay DPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*StandexMeder*DIP*LowProfile*"
			(at 0 0 0)
		)
		(symbol "DIPxx-2Axx-21x_0_0")
		(symbol "DIPxx-2Axx-21x_0_1")
		(symbol "DIPxx-2Axx-21x_1_1"
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DR-3V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 10.795 3.81 0)
		)
		(property "Value" "DR-3V"
			(at 10.795 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Panasonic_DR"
			(at 2.54 -3.81 0)
		)
		(property "Datasheet" "https://www.panasonic-electric-works.com/pew/de/downloads/ds_dr_en_discon.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "3V DC, Single side stable, Polarized Coil, High speed"
			(at 0 0 0)
		)
		(property "ki_keywords" "highly reliable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*SPDT*Panasonic?DR*"
			(at 0 0 0)
		)
		(symbol "DR-3V_0_0")
		(symbol "DR-3V_0_1")
		(symbol "DR-3V_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(name "Earth")
				(number "PE")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DR-L-3V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.684 3.81 0)
		)
		(property "Value" "DR-L-3V"
			(at 15.494 1.778 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Panasonic_DR-L"
			(at 0 0 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/download-files/import/ds_dr_en_discon.pdf"
			(at 0 0 0)
		)
		(property "Description" "3V DC, 1 Latching Polarized Coil, High speed"
			(at 0 0 0)
		)
		(property "ki_keywords" "higly reliable single latch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*SPDT*Panasonic?DR?L*"
			(at 0 0 0)
		)
		(symbol "DR-L-3V_0_0")
		(symbol "DR-L-3V_0_1")
		(symbol "DR-L-3V_1_0"
			(text "S+"
				(at -3.81 2.54 0)
			)
			(text "R+"
				(at -3.81 -2.794 0)
			)
		)
		(symbol "DR-L-3V_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(name "Earth")
				(number "PE")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DR-L2-3V_Form1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.684 3.81 0)
		)
		(property "Value" "DR-L2-3V_Form1"
			(at 19.558 1.524 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Panasonic_DR-L2"
			(at 5.08 0 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/download-files/import/ds_dr_en_discon.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "3V DC, 2 Latching Polarized Coils, Set A1, High speed"
			(at 5.08 0 0)
		)
		(property "ki_keywords" "highly reliable dual latch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*SPDT*Panasonic?DR?L2*"
			(at 0 0 0)
		)
		(symbol "DR-L2-3V_Form1_0_0")
		(symbol "DR-L2-3V_Form1_0_1")
		(symbol "DR-L2-3V_Form1_1_0"
			(text "R+"
				(at -8.636 2.794 0)
			)
			(text "S+"
				(at -3.556 2.794 0)
			)
		)
		(symbol "DR-L2-3V_Form1_1_1"
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "B1")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(name "Earth")
				(number "PE")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DR-L2-3V_Form2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.684 3.81 0)
		)
		(property "Value" "DR-L2-3V_Form2"
			(at 19.558 1.524 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Panasonic_DR-L2"
			(at 5.08 0 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/download-files/import/ds_dr_en_discon.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "3V DC, 2 Latching Polarized Coils, Set B1, High speed"
			(at 5.08 0 0)
		)
		(property "ki_keywords" "highly reliable dual latch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*SPDT*Panasonic?DR?L2*"
			(at 0 0 0)
		)
		(symbol "DR-L2-3V_Form2_0_0")
		(symbol "DR-L2-3V_Form2_0_1")
		(symbol "DR-L2-3V_Form2_1_0"
			(text "R+"
				(at -8.636 2.794 0)
			)
			(text "S+"
				(at -3.556 2.794 0)
			)
		)
		(symbol "DR-L2-3V_Form2_1_1"
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "B1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(name "Earth")
				(number "PE")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EC2-3NU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-3NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), non-latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
		(symbol "EC2-3NU_1_1"
			(text "+"
				(at -9.271 2.921 0)
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EC2-3SNU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-3SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), single coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
		(symbol "EC2-3SNU_0_0"
			(text "S"
				(at -8.001 2.921 0)
			)
		)
		(symbol "EC2-3SNU_1_1"
			(text "+"
				(at -9.398 -2.667 0)
			)
			(text "+"
				(at -9.271 2.921 0)
			)
			(text "R"
				(at -8.001 -2.921 0)
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EC2-3TNU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EC2-3TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU_DoubleCoil"
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), double coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*DoubleCoil*"
			(at 0 0 0)
		)
		(symbol "EC2-3TNU_1_1"
			(text "+"
				(at -14.351 2.921 0)
			)
			(text "S"
				(at -13.081 2.921 0)
			)
			(text "+"
				(at 16.129 2.921 0)
			)
			(text "R"
				(at 17.526 2.921 0)
			)
			(pin passive line
				(at -15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3NKX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-3NKX"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, high breakdown voltage, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NKX*"
			(at 0 0 0)
		)
		(symbol "EE2-3NKX_1_1"
			(text "+"
				(at -9.271 2.921 0)
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3NU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-3NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
		(symbol "EE2-3NU_1_1"
			(text "+"
				(at -9.271 2.921 0)
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3NUH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-3NUH"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
		(symbol "EE2-3NUH_1_1"
			(text "+"
				(at -9.271 2.921 0)
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3NUX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-3NUX"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
		(symbol "EE2-3NUX_1_1"
			(text "+"
				(at -9.271 2.921 0)
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3SNU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-3SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
		(symbol "EE2-3SNU_1_1"
			(text "+"
				(at -9.398 -2.667 0)
			)
			(text "+"
				(at -9.271 2.921 0)
			)
			(text "S"
				(at -8.001 2.921 0)
			)
			(text "R"
				(at -8.001 -2.921 0)
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3SNUH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-3SNUH"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
		(symbol "EE2-3SNUH_1_1"
			(text "+"
				(at -9.398 -2.667 0)
			)
			(text "+"
				(at -9.271 2.921 0)
			)
			(text "S"
				(at -8.001 2.921 0)
			)
			(text "R"
				(at -8.001 -2.921 0)
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3SNUX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-3SNUX"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
		(symbol "EE2-3SNUX_1_1"
			(text "+"
				(at -9.398 -2.667 0)
			)
			(text "+"
				(at -9.271 2.921 0)
			)
			(text "S"
				(at -8.001 2.921 0)
			)
			(text "R"
				(at -8.001 -2.921 0)
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3TNU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-3TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*DoubleCoil*"
			(at 0 0 0)
		)
		(symbol "EE2-3TNU_1_1"
			(text "+"
				(at -14.351 2.921 0)
			)
			(text "S"
				(at -13.081 2.921 0)
			)
			(text "+"
				(at 16.129 2.921 0)
			)
			(text "R"
				(at 17.526 2.921 0)
			)
			(pin passive line
				(at -15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3TNUH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-3TNUH"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*DoubleCoil*"
			(at 0 0 0)
		)
		(symbol "EE2-3TNUH_1_1"
			(text "+"
				(at -14.351 2.921 0)
			)
			(text "S"
				(at -13.081 2.921 0)
			)
			(text "+"
				(at 16.129 2.921 0)
			)
			(text "R"
				(at 17.526 2.921 0)
			)
			(pin passive line
				(at -15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EE2-3TNUX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-3TNUX"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 3V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*DoubleCoil*"
			(at 0 0 0)
		)
		(symbol "EE2-3TNUX_1_1"
			(text "+"
				(at -14.351 2.921 0)
			)
			(text "S"
				(at -13.081 2.921 0)
			)
			(text "+"
				(at 16.129 2.921 0)
			)
			(text "R"
				(at 17.526 2.921 0)
			)
			(pin passive line
				(at -15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-30.22"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "FINDER-30.22"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Finder_30.22"
			(at 34.29 -0.762 0)
		)
		(property "Datasheet" "http://gfinder.findernet.com/assets/Series/354/S30EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 30.52, Dual Pole Relay, Subminiature 5mm Pitch, 2A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Finder*30.22*"
			(at 0 0 0)
		)
		(symbol "FINDER-30.22_0_0")
		(symbol "FINDER-30.22_0_1")
		(symbol "FINDER-30.22_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-32.21-x000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-32.21-x000"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Finder_32.21-x000"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://gfinder.findernet.com/assets/Series/355/S32EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 32.21-x000, Single Pole Relay, 6A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Finder*32.21*x000*"
			(at 0 0 0)
		)
		(symbol "FINDER-32.21-x000_0_0")
		(symbol "FINDER-32.21-x000_0_1")
		(symbol "FINDER-32.21-x000_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-32.21-x300"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-32.21-x300"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Finder_32.21-x300"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "http://gfinder.findernet.com/assets/Series/355/S32EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 32.21-x300, Single Pole Relay SPST-NO, 6A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPST-NO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Finder*32.21*x300*"
			(at 0 0 0)
		)
		(symbol "FINDER-32.21-x300_0_1")
		(symbol "FINDER-32.21-x300_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-34.51"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-34.51"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Finder_34.51_Vertical"
			(at 28.956 -1.016 0)
		)
		(property "Datasheet" "https://gfinder.findernet.com/public/attachments/34/EN/S34USAEN.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-slim 1 Pole - 6A SPDT relay"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Finder*34.51*"
			(at 0 0 0)
		)
		(symbol "FINDER-34.51_0_0")
		(symbol "FINDER-34.51_0_1")
		(symbol "FINDER-34.51_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-34.51.7xxx.x019"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-34.51.7xxx.x019"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Finder_34.51_Horizontal"
			(at 28.956 -1.016 0)
		)
		(property "Datasheet" "https://gfinder.findernet.com/public/attachments/34/EN/S34USAEN.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-slim 1 Pole - 6A SPDT relay"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Finder*34.51*Horizontal*"
			(at 0 0 0)
		)
		(symbol "FINDER-34.51.7xxx.x019_0_0")
		(symbol "FINDER-34.51.7xxx.x019_0_1")
		(symbol "FINDER-34.51.7xxx.x019_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-36.11"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-36.11"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Finder_36.11"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://gfinder.findernet.com/public/attachments/36/EN/S36EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 36.11, SPDT relay, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "spdt relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Finder*36.11*"
			(at 0 0 0)
		)
		(symbol "FINDER-36.11_0_0")
		(symbol "FINDER-36.11_0_1")
		(symbol "FINDER-36.11_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-40.11"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-40.11"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Finder_40.11"
			(at 28.956 -1.016 0)
		)
		(property "Datasheet" "https://www.finder-relais.net/de/finder-relais-serie-40.pdf"
			(at 0 0 0)
		)
		(property "Description" "PCB SPDT relay, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT Finder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Finder*40.11*"
			(at 0 0 0)
		)
		(symbol "FINDER-40.11_0_0")
		(symbol "FINDER-40.11_0_1")
		(symbol "FINDER-40.11_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-40.31"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-40.31"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Finder_40.31"
			(at 28.956 -1.016 0)
		)
		(property "Datasheet" "http://gfinder.findernet.com/assets/Series/353/S40EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 40.31, Single Pole Relay, 3.5mm Pitch, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Finder*40.31*"
			(at 0 0 0)
		)
		(symbol "FINDER-40.31_0_0")
		(symbol "FINDER-40.31_0_1")
		(symbol "FINDER-40.31_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-40.41"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-40.41"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Finder_40.41"
			(at 28.956 -1.016 0)
		)
		(property "Datasheet" "https://www.finder-relais.net/de/finder-relais-serie-40.pdf"
			(at 0 0 0)
		)
		(property "Description" "PCB SPDT relay, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT Finder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Finder*40.41*"
			(at 0 0 0)
		)
		(symbol "FINDER-40.41_0_0")
		(symbol "FINDER-40.41_0_1")
		(symbol "FINDER-40.41_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-40.51"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-40.51"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Finder_40.51"
			(at 28.956 -1.016 0)
		)
		(property "Datasheet" "http://gfinder.findernet.com/assets/Series/353/S40EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 40.51, Single Pole Relay, 5mm Pitch, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Finder*40.51*"
			(at 0 0 0)
		)
		(symbol "FINDER-40.51_0_0")
		(symbol "FINDER-40.51_0_1")
		(symbol "FINDER-40.51_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FINDER-40.52"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "FINDER-40.52"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Finder_40.52"
			(at 34.29 -0.762 0)
		)
		(property "Datasheet" "http://gfinder.findernet.com/assets/Series/353/S40EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 40.52, Dual Pole Relay, 5mm Pitch, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Finder*40.52*"
			(at 0 0 0)
		)
		(symbol "FINDER-40.52_0_1")
		(symbol "FINDER-40.52_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FRT5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "FRT5"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_FRT5"
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "https://www.elpro.org/de/index.php?controller=attachment&id_attachment=8663"
			(at 0 0 0)
		)
		(property "Description" "FORWARD INDUSTRIAL, Miniature Dual Pole Relay, DIP-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*FRT5*"
			(at 0 0 0)
		)
		(symbol "FRT5_0_0"
			(text "+"
				(at -9.271 2.921 0)
			)
		)
		(symbol "FRT5_0_1")
		(symbol "FRT5_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FRT5_separated"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 5.08 2.54 0)
		)
		(property "Value" "FRT5_separated"
			(at 5.08 0 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_FRT5"
			(at 5.08 -2.54 0)
		)
		(property "Datasheet" "https://www.elpro.org/de/index.php?controller=attachment&id_attachment=8663"
			(at 0 0 0)
		)
		(property "Description" "FORWARD INDUSTRIAL, Miniature Dual Pole Relay, DIP-like package, separate subsymbols"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*FRT5*"
			(at 0 0 0)
		)
		(symbol "FRT5_separated_1_0"
			(text "+"
				(at 0.889 2.921 0)
			)
		)
		(symbol "FRT5_separated_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(symbol "FRT5_separated_2_1"
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(symbol "FRT5_separated_3_1"
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Fujitsu_FTR-F1A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 0 12.7 0)
		)
		(property "Value" "Fujitsu_FTR-F1A"
			(at 0 10.16 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPST_Fujitsu_FTR-F1A"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.fcl.fujitsu.com/downloads/MICRO/fcai/relays/ftr-f1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fujitsu Low Profile Power Relay"
			(at 0 0 0)
		)
		(property "ki_keywords" "double pole single throw relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*DPST*Fujitsu*FTR*F1A*"
			(at 0 0 0)
		)
		(symbol "Fujitsu_FTR-F1A_0_1")
		(symbol "Fujitsu_FTR-F1A_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Fujitsu_FTR-F1C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 0 12.7 0)
		)
		(property "Value" "Fujitsu_FTR-F1C"
			(at 0 10.16 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Fujitsu_FTR-F1C"
			(at -1.27 -10.16 0)
		)
		(property "Datasheet" "https://www.fcl.fujitsu.com/downloads/MICRO/fcai/relays/ftr-f1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fujitsu Low Profile Power Relay"
			(at 0 0 0)
		)
		(property "ki_keywords" "double pole double throw relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*DPDT*Fujitsu*FTR*F1C*"
			(at 0 0 0)
		)
		(symbol "Fujitsu_FTR-F1C_0_1")
		(symbol "Fujitsu_FTR-F1C_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G5LE-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G5LE-1"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Omron-G5LE-1"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "http://www.omron.com/ecb/products/pdf/en-g5le.pdf"
			(at 0 0 0)
		)
		(property "Description" "Omron G5LE relay, Miniature Single Pole, SPDT, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Omron*G5LE?1*"
			(at 0 0 0)
		)
		(symbol "G5LE-1_0_0")
		(symbol "G5LE-1_0_1")
		(symbol "G5LE-1_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G5Q-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G5Q-1"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Omron-G5Q-1"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.omron.com/ecb/products/pdf/en-g5q.pdf"
			(at 0 0 0)
		)
		(property "Description" "Omron G5G relay, Miniature Single Pole, SPDT, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Omron*G5Q*"
			(at 0 0 0)
		)
		(symbol "G5Q-1_0_0")
		(symbol "G5Q-1_0_1")
		(symbol "G5Q-1_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G5Q-1A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "G5Q-1A"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Omron-G5Q-1A"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://www.omron.com/ecb/products/pdf/en-g5q.pdf"
			(at 0 0 0)
		)
		(property "Description" "Omron G5Q relay, Miniature Single Pole, SPST-NO, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Omron*G5Q*"
			(at 0 0 0)
		)
		(symbol "G5Q-1A_0_0")
		(symbol "G5Q-1A_0_1")
		(symbol "G5Q-1A_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G5V-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G5V-1"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Omron_G5V-1"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v_1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-miniature, Highly Sensitive SPDT Relay for Signal Circuits"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Omron*G5V?1*"
			(at 0 0 0)
		)
		(symbol "G5V-1_0_0")
		(symbol "G5V-1_0_1")
		(symbol "G5V-1_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G5V-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G5V-2"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G5V-2"
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v_2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Relay Miniature Omron DPDT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Relay Dual Pole DPDT Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G5V*"
			(at 0 0 0)
		)
		(symbol "G5V-2_0_1")
		(symbol "G5V-2_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G5V-2_Split"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 6.35 1.27 0)
		)
		(property "Value" "G5V-2_Split"
			(at 6.35 -1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G5V-2"
			(at 6.35 -3.81 0)
		)
		(property "Datasheet" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v_2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Relay Miniature Omron DPDT"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Relay Dual Pole DPDT Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G5V*"
			(at 0 0 0)
		)
		(symbol "G5V-2_Split_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "16")
			)
		)
		(symbol "G5V-2_Split_2_1"
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "G5V-2_Split_3_1"
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G6E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G6E"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Omron_G6E"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "https://www.omron.com/ecb/products/pdf/en-g6e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Omron Subminiature Sensitive SPDT Signal Switching Relay, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Omron*G6E*"
			(at 0 0 0)
		)
		(symbol "G6E_0_0"
			(text "+"
				(at -4.064 3.556 0)
			)
		)
		(symbol "G6E_0_1")
		(symbol "G6E_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G6EU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G6EU"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Omron_G6E"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "https://www.omron.com/ecb/products/pdf/en-g6e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Omron G6E relay, Subminiature, Sensitive SPDT Signal Switching Relay, Single-winding latching"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Omron*G6E*"
			(at 0 0 0)
		)
		(symbol "G6EU_0_0"
			(text "+/-"
				(at -3.048 3.556 0)
			)
			(text "-/+"
				(at -3.048 -3.556 0)
			)
		)
		(symbol "G6EU_0_1")
		(symbol "G6EU_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G6H-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G6H-2"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/C300/G6H%23OMR.pdf"
			(at 0 0 0)
		)
		(property "Description" "Omron Ultracompact, Ultrasensitive DPDT Relay, Single-side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Omron*G6H?2*"
			(at 0 0 0)
		)
		(symbol "G6H-2_0_0"
			(text "+"
				(at -9.271 2.921 0)
			)
		)
		(symbol "G6H-2_0_1")
		(symbol "G6H-2_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G6HU-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G6HU-2"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6H-2"
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/C300/G6H%23OMR.pdf"
			(at 0 0 0)
		)
		(property "Description" "Omron Ultracompact, Ultrasensitive DPDT Relay, Single-winding Latching"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Omron*G6H?2*"
			(at 0 0 0)
		)
		(symbol "G6HU-2_0_0"
			(text "S+"
				(at -11.43 3.81 900)
			)
			(text "R+"
				(at -11.43 -3.81 900)
			)
		)
		(symbol "G6HU-2_0_1")
		(symbol "G6HU-2_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G6K-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G6K-2"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature 2-pole relay, Single-side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Relay Dual Pole DPDT Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G6K?2*"
			(at 0 0 0)
		)
		(symbol "G6K-2_0_0"
			(text "+"
				(at -9.271 2.921 0)
			)
		)
		(symbol "G6K-2_0_1")
		(symbol "G6K-2_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G6KU-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G6KU-2"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature 2-pole relay, Single-winding Latching"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Relay Dual Pole DPDT Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G6K?2*Y*"
			(at 0 0 0)
		)
		(symbol "G6KU-2_0_0"
			(text "S:+"
				(at -8.763 2.794 0)
			)
			(text "R:+"
				(at -8.763 -2.794 0)
			)
		)
		(symbol "G6KU-2_0_1")
		(symbol "G6KU-2_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G6S-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G6S-2"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Compact, Industry-Standard 2-pole relay, designed to switch 2A Signal Loads, Single-side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Relay Dual Pole DPDT Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G6S?2*"
			(at 0 0 0)
		)
		(symbol "G6S-2_0_0"
			(text "+"
				(at -9.271 2.921 0)
			)
		)
		(symbol "G6S-2_0_1")
		(symbol "G6S-2_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G6SK-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 21.59 3.81 0)
		)
		(property "Value" "G6SK-2"
			(at 21.59 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Compact, Industry-Standard 2-pole relay, designed to switch 2A Signal Loads, Double-winding Latching"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Relay Dual Pole DPDT Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G6SK?2*"
			(at 0 0 0)
		)
		(symbol "G6SK-2_0_0"
			(text "S:+"
				(at -11.303 2.921 0)
			)
			(text "S:-"
				(at -11.303 -2.921 0)
			)
			(text "R:+"
				(at 13.843 2.921 0)
			)
			(text "R:-"
				(at 13.843 -2.921 0)
			)
		)
		(symbol "G6SK-2_0_1")
		(symbol "G6SK-2_1_1"
			(pin passive line
				(at -12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -12.7 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 15.24 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 15.24 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "G6SU-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G6SU-2"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Compact, Industry-Standard 2-pole relay, designed to switch 2A Signal Loads, Single-winding Latching"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Relay Dual Pole DPDT Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G6S?2*"
			(at 0 0 0)
		)
		(symbol "G6SU-2_0_0"
			(text "S:+"
				(at -8.763 2.921 0)
			)
			(text "R:+"
				(at -8.763 -2.921 0)
			)
		)
		(symbol "G6SU-2_0_1")
		(symbol "G6SU-2_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HF3-01"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-01"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_75ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98000&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 75ohm, 3Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*75ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
		(symbol "HF3-01_0_0"
			(text "+"
				(at -4.191 2.921 0)
			)
		)
		(symbol "HF3-01_0_1")
		(symbol "HF3-01_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 7.62 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HF3-51"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-51"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_50ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98000&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 50ohm, 3Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*50ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
		(symbol "HF3-51_0_0"
			(text "+"
				(at -4.191 3.048 0)
			)
		)
		(symbol "HF3-51_0_1")
		(symbol "HF3-51_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 7.62 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HONGFA_HFD2-0xx-x-L2-x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "HONGFA_HFD2-0xx-x-L2-x"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://source_cn.hongfa.com/Api/DownloadPdf/323"
			(at 0 -17.78 0)
		)
		(property "Description" "Bistable miniature DPDT relay, 3A, 125VAC, THT"
			(at 0 -12.7 0)
		)
		(property "ki_keywords" "HONGFA set-reset polarized"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G6AK*"
			(at 0 0 0)
		)
		(symbol "HONGFA_HFD2-0xx-x-L2-x_0_0"
			(text "+"
				(at -12.065 2.667 0)
			)
			(text "+"
				(at -12.065 -2.413 0)
			)
			(text "S"
				(at -10.033 2.794 0)
			)
			(text "R"
				(at -10.033 -2.921 0)
			)
		)
		(symbol "HONGFA_HFD2-0xx-x-L2-x_0_1")
		(symbol "HONGFA_HFD2-0xx-x-L2-x_1_1"
			(pin passive line
				(at -12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -12.7 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B1")
			)
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IM00"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM00"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC, THT package"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
		(symbol "IM00_0_0"
			(text "+"
				(at -9.271 2.921 0)
			)
		)
		(symbol "IM00_0_1")
		(symbol "IM00_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IM11"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM11"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, sensitive version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monastable sensitive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
		(symbol "IM11_0_0"
			(text "+"
				(at -9.271 2.921 0)
			)
		)
		(symbol "IM11_0_1")
		(symbol "IM11_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IM21"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM21"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, high sensitive version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monastable sensitive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
		(symbol "IM21_0_0"
			(text "+"
				(at -9.271 2.921 0)
			)
		)
		(symbol "IM21_0_1")
		(symbol "IM21_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IM40"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM40"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, bistable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
		(symbol "IM40_0_0"
			(text "- +"
				(at -10.16 2.921 0)
			)
			(text "+ -"
				(at -10.16 -2.667 0)
			)
		)
		(symbol "IM40_0_1")
		(symbol "IM40_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "JW2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "RL"
			(at 16.51 3.81 0)
		)
		(property "Value" "JW2"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Panasonic_JW2"
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "http://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_jw.pdf?via=ok"
			(at 0 0 0)
		)
		(property "Description" "General Purpose Relay DPDT (2 Form C) Through Hole, Panasonic JW series"
			(at 0 0 0)
		)
		(property "ki_keywords" "Panasonic Relay Dual Pole"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Panasonic*JW2*"
			(at 0 0 0)
		)
		(symbol "JW2_0_1")
		(symbol "JW2_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSxx-1Axx-75"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "MSxx-1Axx-75"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_StandexMeder_MS_Form1AB"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheets/42/4205187975e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder MS reed relay, SPST, Closing Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*StandexMeder*MS*Form1AB*"
			(at 0 0 0)
		)
		(symbol "MSxx-1Axx-75_0_0")
		(symbol "MSxx-1Axx-75_0_1")
		(symbol "MSxx-1Axx-75_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MSxx-1Bxx-75"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "MSxx-1Bxx-75"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_StandexMeder_MS_Form1AB"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/de/produkte/ms-reed-relais/"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder MS reed relay, SPST, Opening Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*StandexMeder*MS*Form1AB*"
			(at 0 0 0)
		)
		(symbol "MSxx-1Bxx-75_0_0")
		(symbol "MSxx-1Bxx-75_0_1")
		(symbol "MSxx-1Bxx-75_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAYEX-L90"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RAYEX-L90"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_RAYEX-L90"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://a3.sofastcdn.com/attachment/7jioKBjnRiiSrjrjknRiwS77gwbf3zmp/L90-SERIES.pdf"
			(at 8.89 25.4 0)
		)
		(property "Description" "Power relay, SPDT, 30A"
			(at 0 0 0)
		)
		(property "ki_keywords" "30A Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*RAYEX*L90*"
			(at 0 0 0)
		)
		(symbol "RAYEX-L90_1_0")
		(symbol "RAYEX-L90_1_1"
			(pin passive line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "11A")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "~")
				(number "11B")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 5.08)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAYEX-L90A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RAYEX-L90A"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_RAYEX-L90A"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://a3.sofastcdn.com/attachment/7jioKBjnRiiSrjrjknRiwS77gwbf3zmp/L90-SERIES.pdf"
			(at 17.78 -3.81 0)
		)
		(property "Description" "Power relay, NO, SPST, 30A"
			(at 0 0 0)
		)
		(property "ki_keywords" "30A Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*RAYEX*L90A*"
			(at 0 0 0)
		)
		(symbol "RAYEX-L90A_1_0")
		(symbol "RAYEX-L90A_1_1"
			(pin passive line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "13A")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "~")
				(number "13B")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 5.08)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAYEX-L90AS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RAYEX-L90AS"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_RAYEX-L90AS"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://a3.sofastcdn.com/attachment/7jioKBjnRiiSrjrjknRiwS77gwbf3zmp/L90-SERIES.pdf"
			(at 17.78 -3.81 0)
		)
		(property "Description" "Power relay, Without Common Terminal between coil terminals, NO, SPST, 30A"
			(at 0 0 0)
		)
		(property "ki_keywords" "30A Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*RAYEX*L90A*"
			(at 0 0 0)
		)
		(symbol "RAYEX-L90AS_1_0")
		(symbol "RAYEX-L90AS_1_1"
			(pin passive line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 5.08)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAYEX-L90B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "RAYEX-L90B"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_RAYEX-L90B"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://a3.sofastcdn.com/attachment/7jioKBjnRiiSrjrjknRiwS77gwbf3zmp/L90-SERIES.pdf"
			(at 12.7 -3.81 0)
		)
		(property "Description" "Power relay, NC, SPST, 30A"
			(at 0 0 0)
		)
		(property "ki_keywords" "30A Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*RAYEX*L90B*"
			(at 0 0 0)
		)
		(symbol "RAYEX-L90B_1_0")
		(symbol "RAYEX-L90B_1_1"
			(pin passive line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "11A")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "~")
				(number "11B")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAYEX-L90BS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "RAYEX-L90BS"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_RAYEX-L90BS"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://a3.sofastcdn.com/attachment/7jioKBjnRiiSrjrjknRiwS77gwbf3zmp/L90-SERIES.pdf"
			(at 13.97 -3.81 0)
		)
		(property "Description" "Power relay, Without Common Terminal between coil terminals, NC, SPST, 30A"
			(at 0 0 0)
		)
		(property "ki_keywords" "30A Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*RAYEX*L90B*"
			(at 0 0 0)
		)
		(symbol "RAYEX-L90BS_1_0")
		(symbol "RAYEX-L90BS_1_1"
			(pin passive line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAYEX-L90S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RAYEX-L90S"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_RAYEX-L90S"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://a3.sofastcdn.com/attachment/7jioKBjnRiiSrjrjknRiwS77gwbf3zmp/L90-SERIES.pdf"
			(at 16.51 -3.81 0)
		)
		(property "Description" "Power relay, Without Common Terminal between coil terminals, SPDT, 30A"
			(at 0 0 0)
		)
		(property "ki_keywords" "30A Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*RAYEX*L90S*"
			(at 0 0 0)
		)
		(symbol "RAYEX-L90S_1_0")
		(symbol "RAYEX-L90S_1_1"
			(pin passive line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 5.08)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RT314A03"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RT314A03"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Schrack-RT1-16A-FormC_RM5mm"
			(at 39.37 -1.27 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=RT1_bistable&DocType=DS&DocLang=English"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT1 relay, bistable single pole dual throw, single DC coil, 3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE SPDT 1P2T CO bistable DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Schrack*RT1*16A*FormC*RM5mm*"
			(at 0 0 0)
		)
		(symbol "RT314A03_0_0")
		(symbol "RT314A03_0_1")
		(symbol "RT314A03_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RT42xAxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RT42xAxx"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Schrack-RT2-FormC_RM5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FRT2_bistable%7F1116%7Fpdf%7FEnglish%7FENG_DS_RT2_bistable_1116.pdf%7F1-1415537-8"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT2 relay, bistable dual pole dual throw, single DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE DPDT CO bistable DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*RT2*FormC*"
			(at 0 0 0)
		)
		(symbol "RT42xAxx_0_0")
		(symbol "RT42xAxx_0_1")
		(symbol "RT42xAxx_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RT42xFxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RT42xFxx"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Schrack-RT2-FormC-Dual-Coil_RM5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FRT2_bistable%7F1116%7Fpdf%7FEnglish%7FENG_DS_RT2_bistable_1116.pdf%7F1-1415537-8"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT2 relay, bistable dual pole dual throw, dual DC coils"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE DPDT CO bistable DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*RT2*FormC*"
			(at 0 0 0)
		)
		(symbol "RT42xFxx_0_0")
		(symbol "RT42xFxx_0_1")
		(symbol "RT42xFxx_1_1"
			(pin passive line
				(at -17.78 0 0)
				(length 2.54)
				(name "~")
				(number "A3")
			)
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RT42xxxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RT42xxxx"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Schrack-RT2-FormC_RM5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FRT2%7F1014%7Fpdf%7FEnglish%7FENG_DS_RT2_1014.pdf%7F6-1393243-3"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT2 relay, monostable dual pole dual throw, DC or AC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE DPDT CO monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*RT2*FormC*"
			(at 0 0 0)
		)
		(symbol "RT42xxxx_0_1")
		(symbol "RT42xxxx_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RT44xxxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RT44xxxx"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPST_Schrack-RT2-FormA_RM5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FRT2%7F1014%7Fpdf%7FEnglish%7FENG_DS_RT2_1014.pdf%7F6-1393243-3"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT2 relay, monostable dual pole normally open, DC or AC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE DPST NO monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPST*RT2*FormA*"
			(at 0 0 0)
		)
		(symbol "RT44xxxx_0_1")
		(symbol "RT44xxxx_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_DPDT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "Relay_DPDT"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay DPDT, monostable, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P2T 2-Form-C double dual throw pole"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPDT*"
			(at 0 0 0)
		)
		(symbol "Relay_DPDT_0_1")
		(symbol "Relay_DPDT_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_DPDT_Latching_1coil"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "Relay_DPDT_Latching_1coil"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay DPDT, bistable, single-coil, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P2T 2-Form-C double dual pole throw latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPDT*"
			(at 0 0 0)
		)
		(symbol "Relay_DPDT_Latching_1coil_0_1")
		(symbol "Relay_DPDT_Latching_1coil_1_0"
			(text "S+"
				(at -8.89 2.794 0)
			)
			(text "R+"
				(at -8.89 -2.794 0)
			)
		)
		(symbol "Relay_DPDT_Latching_1coil_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_DPDT_Latching_2coil"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "Relay_DPDT_Latching_2coil"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay DPDT, bistable, double-coil, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P2T 2-Form-C double dual pole throw latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPDT*"
			(at 0 0 0)
		)
		(symbol "Relay_DPDT_Latching_2coil_0_0")
		(symbol "Relay_DPDT_Latching_2coil_0_1")
		(symbol "Relay_DPDT_Latching_2coil_1_0"
			(text "S+"
				(at -13.716 2.794 0)
			)
			(text "R+"
				(at -8.636 2.794 0)
			)
		)
		(symbol "Relay_DPDT_Latching_2coil_1_1"
			(pin passive line
				(at -12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -12.7 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "B1")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_DPST-NC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "Relay_DPST-NC"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay DPST, monostable, normally closed, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P2T 2-Form-B double dual pole throw NC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPST*"
			(at 0 0 0)
		)
		(symbol "Relay_DPST-NC_0_1")
		(symbol "Relay_DPST-NC_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_DPST-NO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "Relay_DPST-NO"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay DPST, monostable, normally open, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P2T 2-Form-A double dual pole throw NO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPST*"
			(at 0 0 0)
		)
		(symbol "Relay_DPST-NO_0_1")
		(symbol "Relay_DPST-NO_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "23")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_DPST_Latching_1coil"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "Relay_DPST_Latching_1coil"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay DPST, monostable, normally open, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P2Tdouble dual pole throw latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPST*"
			(at 0 0 0)
		)
		(symbol "Relay_DPST_Latching_1coil_0_1")
		(symbol "Relay_DPST_Latching_1coil_1_0"
			(text "S+"
				(at -8.89 2.794 0)
			)
			(text "R+"
				(at -8.89 -2.794 0)
			)
		)
		(symbol "Relay_DPST_Latching_1coil_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "23")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_DPST_Latching_2coil"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "Relay_DPST_Latching_2coil"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay DPST, bistable, double-coil, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P2T double dual pole throw latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPDT*"
			(at 0 0 0)
		)
		(symbol "Relay_DPST_Latching_2coil_0_0")
		(symbol "Relay_DPST_Latching_2coil_0_1")
		(symbol "Relay_DPST_Latching_2coil_1_0"
			(text "S+"
				(at -13.716 2.794 0)
			)
			(text "R+"
				(at -8.636 2.794 0)
			)
		)
		(symbol "Relay_DPST_Latching_2coil_1_1"
			(pin passive line
				(at -12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -12.7 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "B1")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "23")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_SPDT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Relay_SPDT"
			(at 11.43 1.27 0)
		)
		(property "Footprint" ""
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "1P2T 1-Form-C single pole throw"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPDT*"
			(at 0 0 0)
		)
		(symbol "Relay_SPDT_0_0")
		(symbol "Relay_SPDT_0_1")
		(symbol "Relay_SPDT_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_SPDT_Latching_1coil"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Relay_SPDT_Latching_1coil"
			(at 11.43 1.27 0)
		)
		(property "Footprint" ""
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay SPDT, bistable, double-coil, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "1P2T 1-Form-C single pole throw latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPDT*"
			(at 0 0 0)
		)
		(symbol "Relay_SPDT_Latching_1coil_0_0")
		(symbol "Relay_SPDT_Latching_1coil_0_1")
		(symbol "Relay_SPDT_Latching_1coil_1_0"
			(text "S+"
				(at -3.81 2.794 0)
			)
			(text "R+"
				(at -3.81 -2.794 0)
			)
		)
		(symbol "Relay_SPDT_Latching_1coil_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_SPDT_Latching_2coil"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Relay_SPDT_Latching_2coil"
			(at 11.43 1.27 0)
		)
		(property "Footprint" ""
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay SPDT, bistable, double-coil, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "1P2T 1-Form-C single pole throw latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPDT*"
			(at 0 0 0)
		)
		(symbol "Relay_SPDT_Latching_2coil_0_0")
		(symbol "Relay_SPDT_Latching_2coil_0_1")
		(symbol "Relay_SPDT_Latching_2coil_1_0"
			(text "S+"
				(at -8.636 2.794 0)
			)
			(text "R+"
				(at -3.556 2.794 0)
			)
		)
		(symbol "Relay_SPDT_Latching_2coil_1_1"
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "B1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_SPST-NC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Relay_SPST-NC"
			(at 11.43 1.27 0)
		)
		(property "Footprint" ""
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay SPST, normally closed, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "1P1T 1-Form-B single pole throw NC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPST*"
			(at 0 0 0)
		)
		(symbol "Relay_SPST-NC_0_1")
		(symbol "Relay_SPST-NC_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_SPST-NO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Relay_SPST-NO"
			(at 11.43 1.27 0)
		)
		(property "Footprint" ""
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay SPST, normally open, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "1P1T 1-Form-A single pole throw NO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPST*"
			(at 0 0 0)
		)
		(symbol "Relay_SPST-NO_0_0")
		(symbol "Relay_SPST-NO_0_1")
		(symbol "Relay_SPST-NO_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_SPST_Latching_1coil"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 12.065 3.81 0)
		)
		(property "Value" "Relay_SPST_Latching_1coil"
			(at 11.43 1.27 0)
		)
		(property "Footprint" ""
			(at 33.655 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay SPST, bistable, single-coil, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "1P1T single pole throw latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPST*"
			(at 0 0 0)
		)
		(symbol "Relay_SPST_Latching_1coil_1_1"
			(text "S+"
				(at -3.81 2.794 0)
			)
			(text "R+"
				(at -3.81 -2.794 0)
			)
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Relay_SPST_Latching_2coil"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 12.065 3.81 0)
		)
		(property "Value" "Relay_SPST_Latching_2coil"
			(at 11.43 1.27 0)
		)
		(property "Footprint" ""
			(at 33.655 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Relay SPST, bistable, double-coil, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "1P1T single pole throw latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPST*"
			(at 0 0 0)
		)
		(symbol "Relay_SPST_Latching_2coil_0_1")
		(symbol "Relay_SPST_Latching_2coil_1_0"
			(text "S+"
				(at -8.636 2.794 0)
			)
			(text "R+"
				(at -3.556 2.794 0)
			)
		)
		(symbol "Relay_SPST_Latching_2coil_1_1"
			(pin passive line
				(at -7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -7.62 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "B1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "B2")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SANYOU_SRD_Form_A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "SANYOU_SRD_Form_A"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_SANYOU_SRD_Series_Form_A"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
			(at 0 0 0)
		)
		(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay, Closing Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*SANYOU*SRD*Series*Form*A*"
			(at 0 0 0)
		)
		(symbol "SANYOU_SRD_Form_A_0_0")
		(symbol "SANYOU_SRD_Form_A_0_1")
		(symbol "SANYOU_SRD_Form_A_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SANYOU_SRD_Form_B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "SANYOU_SRD_Form_B"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_SANYOU_SRD_Series_Form_B"
			(at 33.02 -1.27 0)
		)
		(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
			(at 0 0 0)
		)
		(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay, Opening Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*SANYOU*SRD*Series*Form*B*"
			(at 0 0 0)
		)
		(symbol "SANYOU_SRD_Form_B_0_1")
		(symbol "SANYOU_SRD_Form_B_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SANYOU_SRD_Form_C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "SANYOU_SRD_Form_C"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
			(at 0 0 0)
		)
		(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay,"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*SANYOU*SRD*Series*Form*C*"
			(at 0 0 0)
		)
		(symbol "SANYOU_SRD_Form_C_0_0")
		(symbol "SANYOU_SRD_Form_C_0_1")
		(symbol "SANYOU_SRD_Form_C_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SILxx-1Axx-71x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "SILxx-1Axx-71x"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_StandexMeder_SIL_Form1A"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_SIL.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder SIL reed relay, SPST, Closing Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*StandexMeder*SIL*Form1A*"
			(at 0 0 0)
		)
		(symbol "SILxx-1Axx-71x_0_0")
		(symbol "SILxx-1Axx-71x_0_1")
		(symbol "SILxx-1Axx-71x_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SILxx-1Bxx-71x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "SILxx-1Bxx-71x"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_StandexMeder_SIL_Form1B"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_SIL.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder SIL reed relay, SPST, Opening Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*StandexMeder*SIL*Form1B*"
			(at 0 0 0)
		)
		(symbol "SILxx-1Bxx-71x_0_0")
		(symbol "SILxx-1Bxx-71x_0_1")
		(symbol "SILxx-1Bxx-71x_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SILxx-1Cxx-51x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "SILxx-1Cxx-51x"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_StandexMeder_SIL_Form1C"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_SIL.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder SIL reed relay, SPDT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*StandexMeder*SIL*Form1C*"
			(at 0 0 0)
		)
		(symbol "SILxx-1Cxx-51x_0_0")
		(symbol "SILxx-1Cxx-51x_0_1")
		(symbol "SILxx-1Cxx-51x_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TE_PCH-1xxx2M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 8.89 3.81 0)
		)
		(property "Value" "TE_PCH-1xxx2M"
			(at 8.89 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_TE_PCH-1xxx2M"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FPCH_series_relay_data_sheet_E%7F1215%7Fpdf%7FEnglish%7FENG_DS_PCH_series_relay_data_sheet_E_1215.pdf%7F9-1440003-0"
			(at 0 0 0)
		)
		(property "Description" "TE PCH relay, Miniature Single Pole, SPST-NO"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*TE*PCH*1***2M*"
			(at 0 0 0)
		)
		(symbol "TE_PCH-1xxx2M_0_0")
		(symbol "TE_PCH-1xxx2M_0_1")
		(symbol "TE_PCH-1xxx2M_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TIANBO-HJR-4102-L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "TIANBO-HJR-4102-L"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_HJR-4102"
			(at 27.94 -1.27 0)
		)
		(property "Datasheet" "https://cdn-reichelt.de/documents/datenblatt/C300/DS_HJR4102E.pdf"
			(at 0 0 0)
		)
		(property "Description" "TIANBO HJR-4102-L, Single Pole Relay, 5mm Pitch, 3A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*HJR?4102*"
			(at 0 0 0)
		)
		(symbol "TIANBO-HJR-4102-L_0_0")
		(symbol "TIANBO-HJR-4102-L_0_1")
		(symbol "TIANBO-HJR-4102-L_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UMS05-1A80-75D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 7.62 3.81 0)
		)
		(property "Value" "UMS05-1A80-75D"
			(at 7.62 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_StandexMeder_UMS"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheets/43/4305180175d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder UMS reed relay, SPST, Closing Contact, with diode"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*StandexMeder*UMS*"
			(at 0 0 0)
		)
		(symbol "UMS05-1A80-75D_0_0")
		(symbol "UMS05-1A80-75D_0_1")
		(symbol "UMS05-1A80-75D_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UMS05-1A80-75L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 7.62 3.81 0)
		)
		(property "Value" "UMS05-1A80-75L"
			(at 7.62 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_StandexMeder_UMS"
			(at 7.62 -1.27 0)
		)
		(property "Datasheet" "https://standexelectronics.com/wp-content/uploads/datasheets/43/4305180075d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Standex Meder UMS reed relay, SPST, Closing Contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Reed Relay SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*StandexMeder*UMS*"
			(at 0 0 0)
		)
		(symbol "UMS05-1A80-75L_0_0")
		(symbol "UMS05-1A80-75L_0_1")
		(symbol "UMS05-1A80-75L_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "V23072-Cx061-xxx8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "V23072-Cx061-xxx8"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_Tyco_V23072_Sealed"
			(at -16.256 -21.336 0)
		)
		(property "Datasheet" "https://www.electrokit.com/upload/product/41019/41019252/V23072.pdf"
			(at 0 -18.796 0)
		)
		(property "Description" "Mini Relay K, 12VDC coil / rated voltage, 1 Form U (twin make contact, i.e. 2x NO with common connection), Sealed Enclosure"
			(at 0 -16.256 0)
		)
		(property "ki_keywords" "SPST Miniature Single Pole Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*Tyco*"
			(at 0 0 0)
		)
		(symbol "V23072-Cx061-xxx8_0_1")
		(symbol "V23072-Cx061-xxx8_1_1"
			(pin passive line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 12.7 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Y14x-1C-xxDS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Y14x-1C-xxDS"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_HsinDa_Y14"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "http://www.hsinda.com.tw/upload/file/Y14-20200430135145.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hsin Da Y14-series relay, Single Pole Dual Throw"
			(at 0 0 0)
		)
		(property "ki_keywords" "Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Y14*"
			(at 0 0 0)
		)
		(symbol "Y14x-1C-xxDS_0_0")
		(symbol "Y14x-1C-xxDS_0_1")
		(symbol "Y14x-1C-xxDS_1_1"
			(pin passive line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADW11"
		(extends "Relay_SPST_Latching_1coil")
		(property "Reference" "K"
			(at 12.065 3.81 0)
		)
		(property "Value" "ADW11"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ADW11"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://api.pim.na.industrial.panasonic.com/file_stream/main/fileversion/270"
			(at 11.43 -3.81 0)
		)
		(property "Description" "Panasonic, 8A/16A, Small Polarized Latching Power Relays, Single coil, 1 Form A"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPST 1P1T latching bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ADW11*"
			(at 0 0 0)
		)
	)
	(symbol "AZ850P1-x"
		(extends "AZ850-x")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "AZ850P1-x"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_FRT5"
			(at 13.97 1.27 0)
		)
		(property "Datasheet" "http://www.azettler.com/pdfs/az850.pdf"
			(at 0 0 0)
		)
		(property "Description" "American Zettler, Microminiature Polarised Dual Pole Relay Bistable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Polarised Relay Dual Pole Bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*FRT5*"
			(at 0 0 0)
		)
	)
	(symbol "DR-24V"
		(extends "DR-3V")
		(property "Reference" "K"
			(at 10.795 3.81 0)
		)
		(property "Value" "DR-24V"
			(at 10.795 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Panasonic_DR"
			(at 0 0 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/download-files/import/ds_dr_en_discon.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V DC, Single side stable, Polarized Coil, High speed"
			(at 0 0 0)
		)
		(property "ki_keywords" "highly reliable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*SPDT*Panasonic?DR*"
			(at 0 0 0)
		)
	)
	(symbol "DR-5V"
		(extends "DR-3V")
		(property "Reference" "K"
			(at 10.795 3.81 0)
		)
		(property "Value" "DR-5V"
			(at 10.795 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Panasonic_DR"
			(at 2.54 -3.81 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/download-files/import/ds_dr_en_discon.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "5V DC, Single side stable, Polarized Coil, High speed"
			(at 0 0 0)
		)
		(property "ki_keywords" "highly reliable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*SPDT*Panasonic?DR*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-12NU"
		(extends "EC2-3NU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-12NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), non-latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-12SNU"
		(extends "EC2-3SNU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-12SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), single coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-12TNU"
		(extends "EC2-3TNU")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EC2-12TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU_DoubleCoil"
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), double coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-24NU"
		(extends "EC2-3NU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-24NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), non-latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-24SNU"
		(extends "EC2-3SNU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-24SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), single coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-24TNU"
		(extends "EC2-3TNU")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EC2-24TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU_DoubleCoil"
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), double coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-4.5NU"
		(extends "EC2-3NU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-4.5NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), non-latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-4.5SNU"
		(extends "EC2-3SNU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-4.5SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), single coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-4.5TNU"
		(extends "EC2-3TNU")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EC2-4.5TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU_DoubleCoil"
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), double coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-5NU"
		(extends "EC2-3NU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-5NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), non-latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-5SNU"
		(extends "EC2-3SNU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EC2-5SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), single coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*"
			(at 0 0 0)
		)
	)
	(symbol "EC2-5TNU"
		(extends "EC2-3TNU")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EC2-5TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Kemet_EC2_NU_DoubleCoil"
			(at -5.08 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EC2 Series, DPDT (2 Form C), double coil latching, through hole, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Kemet*EC2*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12NKX"
		(extends "EE2-3NKX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-12NKX"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, high breakdown voltage, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NKX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12NU"
		(extends "EE2-3NU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-12NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12NUH"
		(extends "EE2-3NUH")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-12NUH"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12NUX"
		(extends "EE2-3NUX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-12NUX"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12SNU"
		(extends "EE2-3SNU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-12SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12SNUH"
		(extends "EE2-3SNUH")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-12SNUH"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12SNUX"
		(extends "EE2-3SNUX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-12SNUX"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12TNU"
		(extends "EE2-3TNU")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-12TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12TNUH"
		(extends "EE2-3TNUH")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-12TNUH"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-12TNUX"
		(extends "EE2-3TNUX")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-12TNUX"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 12V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-24NU"
		(extends "EE2-3NU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-24NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-24NUH"
		(extends "EE2-3NUH")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-24NUH"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-24NUX"
		(extends "EE2-3NUX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-24NUX"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-24SNU"
		(extends "EE2-3SNU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-24SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-24SNUH"
		(extends "EE2-3SNUH")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-24SNUH"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-24SNUX"
		(extends "EE2-3SNUX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-24SNUX"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-24TNU"
		(extends "EE2-3TNU")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-24TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-24TNUH"
		(extends "EE2-3TNUH")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-24TNUH"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-24TNUX"
		(extends "EE2-3TNUX")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-24TNUX"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 24V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5NKX"
		(extends "EE2-3NKX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-4.5NKX"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, high breakdown voltage, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NKX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5NU"
		(extends "EE2-3NU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-4.5NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5NUH"
		(extends "EE2-3NUH")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-4.5NUH"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5NUX"
		(extends "EE2-3NUX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-4.5NUX"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5SNU"
		(extends "EE2-3SNU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-4.5SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5SNUH"
		(extends "EE2-3SNUH")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-4.5SNUH"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5SNUX"
		(extends "EE2-3SNUX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-4.5SNUX"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5TNU"
		(extends "EE2-3TNU")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-4.5TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5TNUH"
		(extends "EE2-3TNUH")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-4.5TNUH"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-4.5TNUX"
		(extends "EE2-3TNUX")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-4.5TNUX"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 4.5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-5NU"
		(extends "EE2-3NU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-5NU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-5NUH"
		(extends "EE2-3NUH")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-5NUH"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-5NUX"
		(extends "EE2-3NUX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-5NUX"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), non-latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil non latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-5SNU"
		(extends "EE2-3SNU")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-5SNU"
			(at 19.05 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-5SNUH"
		(extends "EE2-3SNUH")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-5SNUH"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-5SNUX"
		(extends "EE2-3SNUX")
		(property "Reference" "K"
			(at 15.24 8.89 0)
		)
		(property "Value" "EE2-5SNUX"
			(at 20.32 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_NKX"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), single coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil single coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-5TNU"
		(extends "EE2-3TNU")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-5TNU"
			(at 21.59 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NU_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, SMD, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NU*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-5TNUH"
		(extends "EE2-3TNUH")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-5TNUH"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUH_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, small footprint SMD, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUH*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "EE2-5TNUX"
		(extends "EE2-3TNUX")
		(property "Reference" "K"
			(at 17.78 8.89 0)
		)
		(property "Value" "EE2-5TNUX"
			(at 22.86 6.35 0)
		)
		(property "Footprint" "Relay_SMD:Relay_DPDT_Kemet_EE2_NUX_DoubleCoil"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf"
			(at 0 0 0)
		)
		(property "Description" "General purpose signal relay, Kemet EE2 Series, DPDT (2 Form C), double coil latching, high solder joint reliability SMD, 60W/125VA, 220VDC/250VAC, 2A, 5V DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal relay double pole double throw DPDT DC coil double dual coil latching"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Kemet*EE2*NUX*DoubleCoil*"
			(at 0 0 0)
		)
	)
	(symbol "FINDER-40.11-2016"
		(extends "FINDER-40.11")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "FINDER-40.11-2016"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Finder_40.11"
			(at 28.956 -1.016 0)
		)
		(property "Datasheet" "https://www.finder-relais.net/de/finder-relais-serie-40.pdf"
			(at 0 0 0)
		)
		(property "Description" "PCB SPDT relay, 16A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT Finder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Finder*40.11*"
			(at 0 0 0)
		)
	)
	(symbol "FINDER-41.52"
		(extends "FINDER-40.52")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "FINDER-41.52"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Finder_40.52"
			(at 34.29 -0.762 0)
		)
		(property "Datasheet" "http://gfinder.findernet.com/assets/Series/357/S41EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 41.52, Dual Pole Relay, 5mm Pitch, 8A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Finder*40.52*"
			(at 0 0 0)
		)
	)
	(symbol "FINDER-44.52"
		(extends "FINDER-40.52")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "FINDER-44.52"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Finder_40.52"
			(at 34.29 -0.762 0)
		)
		(property "Datasheet" "http://gfinder.findernet.com/assets/Series/359/S44EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 44.52, Dual Pole Relay, 5mm Pitch, 6A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Finder*40.52*"
			(at 0 0 0)
		)
	)
	(symbol "FINDER-44.62"
		(extends "FINDER-40.52")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "FINDER-44.62"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Finder_40.52"
			(at 34.29 -0.762 0)
		)
		(property "Datasheet" "http://gfinder.findernet.com/assets/Series/359/S44EN.pdf"
			(at 0 0 0)
		)
		(property "Description" "FINDER 44.62, Dual Pole Relay, 5mm Pitch, 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Finder*40.52*"
			(at 0 0 0)
		)
	)
	(symbol "Fujitsu_FTR-LYAA005x"
		(extends "Relay_SPST-NO")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Fujitsu_FTR-LYAA005x"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST-NO_Fujitsu_FTR-LYAA005x_FormA_Vertical"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.fujitsu.com/sg/imagesgig5/ftr-ly.pdf"
			(at 17.78 -3.81 0)
		)
		(property "Description" "Relay, SPST Form A, vertical mount, 5-60V coil, 6A, 250VAC, 28 x 5 x 15mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "6A SPST-NO Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Fujitsu*FTR?LYA*"
			(at 0 0 0)
		)
	)
	(symbol "Fujitsu_FTR-LYCA005x"
		(extends "Relay_SPDT")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Fujitsu_FTR-LYCA005x"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Fujitsu_FTR-LYCA005x_FormC_Vertical"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.fujitsu.com/sg/imagesgig5/ftr-ly.pdf"
			(at 16.51 -3.81 0)
		)
		(property "Description" "Relay, SPDT Form C, vertical mount, 5-60V coil, 6A, 250VAC, 28 x 5 x 15mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "6A SPDT Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*Fujitsu*FTR?LYC*"
			(at 0 0 0)
		)
	)
	(symbol "G2RL-1"
		(extends "Relay_SPDT")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G2RL-1"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Omron_G2RL-1"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g2rl.pdf"
			(at 0 0 0)
		)
		(property "Description" "General Purpose Low Profile Relay SPDT Through Hole, Omron G2RL series, 12A 250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPDT?Omron?G2RL*"
			(at 0 0 0)
		)
	)
	(symbol "G2RL-1-E"
		(extends "Relay_SPDT")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G2RL-1-E"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Omron_G2RL-1-E"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g2rl.pdf"
			(at 0 0 0)
		)
		(property "Description" "General Purpose Low Profile Relay SPDT Through Hole High Capacity, Omron G2RL series, 16A 250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT Omron High Capacity"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPDT?Omron?G2RL*E*"
			(at 0 0 0)
		)
	)
	(symbol "G2RL-1-H"
		(extends "Relay_SPDT")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G2RL-1-H"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Omron_G2RL-1"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g2rl.pdf"
			(at 0 0 0)
		)
		(property "Description" "General Purpose Low Profile Relay SPDT Through Hole, Omron G2RL series, High Sensitivity, 10A 250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT Omron High Sensitivity"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPDT?Omron?G2RL*"
			(at 0 0 0)
		)
	)
	(symbol "G2RL-1A"
		(extends "Relay_SPST-NO")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G2RL-1A"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Omron_G2RL-1A"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g2rl.pdf"
			(at 0 0 0)
		)
		(property "Description" "General Purpose Low Profile Relay SPST Through Hole, Omron G2RL series, Normally Open, 12A 250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPST Omron NO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPST?Omron?G2RL*"
			(at 0 0 0)
		)
	)
	(symbol "G2RL-1A-E"
		(extends "Relay_SPST-NO")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G2RL-1A-E"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Omron_G2RL-1A-E"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g2rl.pdf"
			(at 0 0 0)
		)
		(property "Description" "General Purpose Low Profile Relay SPST Through Hole High Capacity, Omron G2RL series, Normally Open, 16A 250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPST Omron NO High Capacity"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPST?Omron?G2RL*E*"
			(at 0 0 0)
		)
	)
	(symbol "G2RL-1A-H"
		(extends "Relay_SPST-NO")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G2RL-1A-H"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Omron_G2RL-1A"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g2rl.pdf"
			(at 0 0 0)
		)
		(property "Description" "General Purpose Low Profile Relay SPST Through Hole, Omron G2RL series, Normally Open, High Sensitivity, 10A 250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPST Omron NO High Sensitivity"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPST?Omron?G2RL*"
			(at 0 0 0)
		)
	)
	(symbol "G2RL-2"
		(extends "Relay_DPDT")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G2RL-2"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G2RL-2"
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g2rl.pdf"
			(at 0 0 0)
		)
		(property "Description" "General Purpose Low Profile Relay DPDT Through Hole, Omron G2RL series, 8A 250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Pole Relay Omron DPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPDT?Omron?G2RL*"
			(at 0 0 0)
		)
	)
	(symbol "G2RL-2A"
		(extends "Relay_DPST-NO")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G2RL-2A"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPST_Omron_G2RL-2A"
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g2rl.pdf"
			(at 0 0 0)
		)
		(property "Description" "General Purpose Low Profile Relay DPST Through Hole, Omron G2RL series, Normally Open,  8A 250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Pole Relay Omron DPST NO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPST?Omron?G2RL*"
			(at 0 0 0)
		)
	)
	(symbol "G5NB"
		(extends "Relay_SPST-NO")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "G5NB"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Omron_G5NB"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g5nb_el.pdf"
			(at 11.43 -3.81 0)
		)
		(property "Description" "PCB Power Relay, SPST-NO, 7A (250 VAC), 5A (30 VDC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Omron G5NB Relay SPST-NO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?SPST*Omron*G5NB*"
			(at 0 0 0)
		)
	)
	(symbol "G6A"
		(extends "Relay_DPDT")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G6A"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6A"
			(at 16.51 -1.27 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Industry-Standard 2-pole relay, designed to switch 2A Signal Loads, Single-side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Relay Dual Pole DPDT 2-Form-C Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Omron*G6A*"
			(at 0 0 0)
		)
	)
	(symbol "G6AK"
		(extends "Relay_DPDT_Latching_2coil")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G6AK"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6AK"
			(at 0 0 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Industry-Standard 2-pole relay, designed to switch 2A Signal Loads, Double-winding Latching"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P2T double dual pole throw DPDT 2-Form-C bistable Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPDT*Omron*G6AK*"
			(at 0 0 0)
		)
	)
	(symbol "G6AU"
		(extends "Relay_DPDT_Latching_1coil")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "G6AU"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6A"
			(at 0 0 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-g6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Industry-Standard 2-pole relay, designed to switch 2A Signal Loads, Single-winding Latching"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P2T double dual pole throw DPDT 2-Form-C bistable Omron"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPDT*Omron*G6A*"
			(at 0 0 0)
		)
	)
	(symbol "HF115F-2Z-x4"
		(extends "Relay_DPDT")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "HF115F-2Z-x4"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Hongfa_HF115F-2Z-x4"
			(at 0 0 0)
		)
		(property "Datasheet" "https://source.hongfa.com//pdf/web/viewer.html?file=/Uploads/Product/PDF/HF115F_I_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Monostable relay DPDT, 29x12.7mm body size, 5mm pitch, 8A, EN50005"
			(at 0 0 0)
		)
		(property "ki_keywords" "2-Form-C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay?DPDT*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-02"
		(extends "HF3-01")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-02"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_75ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 75ohm, 4.5Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*75ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-03"
		(extends "HF3-01")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-03"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_75ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 75ohm, 5Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*75ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-04"
		(extends "HF3-01")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-04"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_75ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 75ohm, 6Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*75ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-05"
		(extends "HF3-01")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-05"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_75ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 75ohm, 9Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*75ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-06"
		(extends "HF3-01")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-06"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_75ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 75ohm, 12Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*75ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-07"
		(extends "HF3-01")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-07"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_75ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 75ohm, 24Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*75ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-52"
		(extends "HF3-51")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-52"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_50ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 50ohm, 4.5Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*50ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-53"
		(extends "HF3-51")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-53"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_50ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 50ohm, 5Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*50ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-54"
		(extends "HF3-51")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-54"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_50ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 50ohm, 6Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*50ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-55"
		(extends "HF3-51")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-55"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_50ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 50ohm, 9Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*50ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-56"
		(extends "HF3-51")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-56"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_50ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 50ohm, 12Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*50ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HF3-57"
		(extends "HF3-51")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "HF3-57"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_SMD:Relay_SPDT_AXICOM_HF3Series_50ohms_Pitch1.27mm"
			(at 28.702 -0.762 0)
		)
		(property "Datasheet" "http://hiqsdr.com/images/3/3e/Axicom-HF3.pdf"
			(at 0 0 0)
		)
		(property "Description" "AXICOM HF3 relay, 3GHz, SPDT RF Switching Relay, 50ohm, 24Vdc, Single-Side Stable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*AXICOM*HF3Series*50ohms*Pitch1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HK19F-DCxxV-SHC"
		(extends "Relay_DPDT")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "HK19F-DCxxV-SHC"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Finder_30.22"
			(at -17.78 -12.7 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_1810201512_Ningbo-Keke-New-Era-Appliance-HK19F-DC12V-SHG_C42803.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "HuiKe 19F monostable relay, DPDT, 1A"
			(at 1.27 -15.24 0)
		)
		(property "ki_keywords" "12V DC Relay DPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Finder*30.22*"
			(at 0 0 0)
		)
	)
	(symbol "IM01"
		(extends "IM00")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM01"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM02"
		(extends "IM00")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM02"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM03"
		(extends "IM00")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM03"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries* Relay*2P2T*10x6mm*TE*IMxxG*"
			(at 0 0 0)
		)
	)
	(symbol "IM04"
		(extends "IM00")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM04"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM05"
		(extends "IM00")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM05"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM06"
		(extends "IM00")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM06"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM07"
		(extends "IM00")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM07"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM08"
		(extends "IM00")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM08"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM12"
		(extends "IM11")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM12"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, sensitive version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monastable sensitive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM13"
		(extends "IM11")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM13"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, sensitive version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monastable sensitive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM16"
		(extends "IM11")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM16"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, sensitive version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monastable sensitive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM17"
		(extends "IM11")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM17"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, sensitive version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monastable sensitive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM22"
		(extends "IM21")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM22"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, high sensitive version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monastable sensitive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM23"
		(extends "IM21")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM23"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, high sensitive version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monastable sensitive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM26"
		(extends "IM21")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM26"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, high sensitive version, monostable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay monastable sensitive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM41"
		(extends "IM40")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM41"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, bistable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM42"
		(extends "IM40")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM42"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, bistable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM43"
		(extends "IM40")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM43"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, bistable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM44"
		(extends "IM40")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM44"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, bistable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM45"
		(extends "IM40")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM45"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, bistable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM46"
		(extends "IM40")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM46"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, bistable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM47"
		(extends "IM40")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM47"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, bistable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "IM48"
		(extends "IM40")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "IM48"
			(at 16.51 1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=108-98001&DocType=SS&DocLang=EN"
			(at 0 0 0)
		)
		(property "Description" "IM Relay, standard version, bistable, switching current 2/5A, power 60W/62.5VA, voltage 220VDC/250VAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "relay bistable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*AXICOM*IMSeries*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-005-1H"
		(extends "Relay_SPST-NO")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-005-1H"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Hongfa_JQC-3FF_0XX-1H"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPST NO Relay, 5V Coil nom. 0.36W, 15A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Hongfa*JQC*3FF*0XX*1H*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-005-1Z"
		(extends "Relay_SPDT")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-005-1Z"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Hongfa_JQC-3FF_0XX-1Z"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPDT Relay, 5V Coil nom. 0.36W, 10A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Hongfa*JQC*3FF*0XX*1Z*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG1PF09"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG1PF09"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "9V DC, Standard, 22A, Contact Gap 1.5mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG1PF091"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG1PF091"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "9V DC, Standard, 22A, Contact Gap 1.8mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG1PF12"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG1PF12"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V DC, Standard, 22A, Contact Gap 1.5mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG1PF121"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG1PF121"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V DC, Standard, 22A, Contact Gap 1.8mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG1PF18"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG1PF18"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V DC, Standard, 22A, Contact Gap 1.5mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG1PF181"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG1PF181"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V DC, Standard, 22A, Contact Gap 1.8mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG1PF24"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG1PF24"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V DC, Standard, 22A, Contact Gap 1.5mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG1PF241"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG1PF241"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V DC, Standard, 22A, Contact Gap 1.8mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG2PF09"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG2PF09"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "9V DC, High Capacity, 31A, Contact Gap 1.5mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG2PF091"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG2PF091"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "9V DC, High Capacity, 33A, Contact Gap 1.8mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG2PF12"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG2PF12"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V DC, High Capacity, 31A, Contact Gap 1.5mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG2PF121"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG2PF121"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V DC, High Capacity, 33A, Contact Gap 1.8mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG2PF18"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG2PF18"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V DC, High Capacity, 31A, Contact Gap 1.5mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG2PF181"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG2PF181"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V DC, High Capacity, 33A, Contact Gap 1.8mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG2PF24"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG2PF24"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V DC, High Capacity, 31A, Contact Gap 1.5mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_ALFG2PF241"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "Panasonic_ALFG2PF241"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Panasonic_ALFG_FormA_CircularHoles"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V DC, High Capacity, 33A, Contact Gap 1.8mm, ALFG_FormA"
			(at 0 0 0)
		)
		(property "ki_keywords" "single pole spst make contact"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Panasonic*ALFG*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "RM50-xx21"
		(extends "FINDER-32.21-x300")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RM50-xx21"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Finder_32.21-x300"
			(at 32.258 -0.762 0)
		)
		(property "Datasheet" "http://www.relpol.pl/en/content/download/13683/165953/file/e_RM50.pdf"
			(at 0 0 0)
		)
		(property "Description" "RELPOL, Single Pole Relay SPST-NO, 6A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Pole Relay SPST-NO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Finder*32.21*x300*"
			(at 0 0 0)
		)
	)
	(symbol "RM84"
		(extends "FINDER-40.52")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RM84"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Finder_40.52"
			(at 34.29 -0.762 0)
		)
		(property "Datasheet" "http://www.relpol.pl/en/content/download/13766/168095/file/e_RM84.pdf"
			(at 0 0 0)
		)
		(property "Description" "RELPOL Dual Pole Relay, 5mm Pitch, 8A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Finder*40.52*"
			(at 0 0 0)
		)
	)
	(symbol "RSM822"
		(extends "FINDER-40.52")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RSM822"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Finder_40.52"
			(at 34.29 -0.762 0)
		)
		(property "Datasheet" "http://www.relpol.pl/en/content/download/14975/202519/file/e_RSM822.pdf"
			(at 0 0 0)
		)
		(property "Description" "RELPOL Dual Pole Relay, 5mm Pitch, 2A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Pole Relay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*Finder*40.52*"
			(at 0 0 0)
		)
	)
	(symbol "RT314A05"
		(extends "RT314A03")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RT314A05"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Schrack-RT1-16A-FormC_RM5mm"
			(at 39.37 -1.27 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=RT1_bistable&DocType=DS&DocLang=English"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT1 relay, bistable single pole dual throw, single DC coil, 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE SPDT 1P2T CO bistable DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Schrack*RT1*16A*FormC*RM5mm*"
			(at 0 0 0)
		)
	)
	(symbol "RT314A06"
		(extends "RT314A03")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RT314A06"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Schrack-RT1-16A-FormC_RM5mm"
			(at 39.37 -1.27 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=RT1_bistable&DocType=DS&DocLang=English"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT1 relay, bistablesingle pole dual throw, single DC coil, 6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE SPDT 1P2T CO bistable DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Schrack*RT1*16A*FormC*RM5mm*"
			(at 0 0 0)
		)
	)
	(symbol "RT314A12"
		(extends "RT314A03")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RT314A12"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Schrack-RT1-16A-FormC_RM5mm"
			(at 39.37 -1.27 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=RT1_bistable&DocType=DS&DocLang=English"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT1 relay, bistable single pole dual throw, single DC coil, 12V"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE SPDT 1P2T CO bistable DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Schrack*RT1*16A*FormC*RM5mm*"
			(at 0 0 0)
		)
	)
	(symbol "RT314A24"
		(extends "RT314A03")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "RT314A24"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Schrack-RT1-16A-FormC_RM5mm"
			(at 39.37 -1.27 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=RT1_bistable&DocType=DS&DocLang=English"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT1 relay, bistable single pole dual throw, single DC coil, 24V, IEC 60335-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE SPDT 1P2T CO bistable DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Schrack*RT1*16A*FormC*RM5mm*"
			(at 0 0 0)
		)
	)
	(symbol "RTE2xAxx"
		(extends "RT42xAxx")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RTE2xAxx"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Schrack-RT2-FormC_RM5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FRT2_bistable%7F1116%7Fpdf%7FEnglish%7FENG_DS_RT2_bistable_1116.pdf%7F1-1415537-8"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT2 relay, bistable dual pole dual throw, single DC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE DPDT CO bistable DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*RT2*FormC*"
			(at 0 0 0)
		)
	)
	(symbol "RTE2xFxx"
		(extends "RT42xFxx")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RTE2xFxx"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Schrack-RT2-FormC-Dual-Coil_RM5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FRT2_bistable%7F1116%7Fpdf%7FEnglish%7FENG_DS_RT2_bistable_1116.pdf%7F1-1415537-8"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT2 relay, bistable dual pole dual throw, dual DC coils"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE DPDT CO bistable DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*RT2*FormC*"
			(at 0 0 0)
		)
	)
	(symbol "RTE2xxxx"
		(extends "RT42xxxx")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RTE2xxxx"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Schrack-RT2-FormC_RM5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FRT2%7F1014%7Fpdf%7FEnglish%7FENG_DS_RT2_1014.pdf%7F6-1393243-3"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT2 relay, monostable dual pole dual throw, DC or AC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE DPDT CO monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPDT*RT2*FormC*"
			(at 0 0 0)
		)
	)
	(symbol "RTE4xxxx"
		(extends "RT44xxxx")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "RTE4xxxx"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_DPST_Schrack-RT2-FormA_RM5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FRT2%7F1014%7Fpdf%7FEnglish%7FENG_DS_RT2_1014.pdf%7F6-1393243-3"
			(at 0 0 0)
		)
		(property "Description" "Schrack RT2 relay, monostable dual pole normally open, DC or AC coil"
			(at 0 0 0)
		)
		(property "ki_keywords" "TE DPST NO monostable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*DPST*RT2*FormA*"
			(at 0 0 0)
		)
	)
	(symbol "V23072-Cx062-xxx8"
		(extends "V23072-Cx061-xxx8")
		(property "Reference" "K"
			(at 16.51 3.81 0)
		)
		(property "Value" "V23072-Cx062-xxx8"
			(at 16.51 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_Tyco_V23072_Sealed"
			(at -16.256 -21.336 0)
		)
		(property "Datasheet" "https://www.electrokit.com/upload/product/41019/41019252/V23072.pdf"
			(at 0 -18.796 0)
		)
		(property "Description" "Mini Relay K, 24VDC coil / rated voltage, 1 Form U (twin make contact, i.e. 2x NO with common connection), Sealed Enclosure"
			(at 0 -16.256 0)
		)
		(property "ki_keywords" "SPST Miniature Single Pole Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Relay*Tyco*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-006-1H"
		(extends "JQC-3FF-005-1H")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-006-1H"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Hongfa_JQC-3FF_0XX-1H"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPST NO Relay, 6V Coil nom. 0.36W, 15A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Hongfa*JQC*3FF*0XX*1H*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-006-1Z"
		(extends "JQC-3FF-005-1Z")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-006-1Z"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Hongfa_JQC-3FF_0XX-1Z"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPDT Relay, 6V Coil nom. 0.36W, 10A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Hongfa*JQC*3FF*0XX*1Z*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-009-1H"
		(extends "JQC-3FF-005-1H")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-009-1H"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Hongfa_JQC-3FF_0XX-1H"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPST NO Relay, 9V Coil nom. 0.36W, 15A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Hongfa*JQC*3FF*0XX*1H*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-009-1Z"
		(extends "JQC-3FF-005-1Z")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-009-1Z"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Hongfa_JQC-3FF_0XX-1Z"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPDT Relay, 9V Coil nom. 0.36W, 10A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Hongfa*JQC*3FF*0XX*1Z*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-012-1H"
		(extends "JQC-3FF-005-1H")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-012-1H"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Hongfa_JQC-3FF_0XX-1H"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPST NO Relay, 12V Coil nom. 0.36W, 15A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Hongfa*JQC*3FF*0XX*1H*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-012-1Z"
		(extends "JQC-3FF-005-1Z")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-012-1Z"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Hongfa_JQC-3FF_0XX-1Z"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPDT Relay, 12V Coil nom. 0.36W, 10A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Hongfa*JQC*3FF*0XX*1Z*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-018-1H"
		(extends "JQC-3FF-005-1H")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-018-1H"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Hongfa_JQC-3FF_0XX-1H"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPST NO Relay, 18V Coil nom. 0.36W, 10A switching current, max 15A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Hongfa*JQC*3FF*0XX*1H*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-018-1Z"
		(extends "JQC-3FF-005-1Z")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-018-1Z"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Hongfa_JQC-3FF_0XX-1Z"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPDT Relay, 18V Coil nom. 0.36W, 10A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Hongfa*JQC*3FF*0XX*1Z*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-024-1H"
		(extends "JQC-3FF-005-1H")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-024-1H"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Hongfa_JQC-3FF_0XX-1H"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPST NO Relay, 24V Coil nom. 0.36W, 15A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Hongfa*JQC*3FF*0XX*1H*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-024-1Z"
		(extends "JQC-3FF-005-1Z")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-024-1Z"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Hongfa_JQC-3FF_0XX-1Z"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPDT Relay, 24V Coil nom. 0.36W, 10A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Hongfa*JQC*3FF*0XX*1Z*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-048-1H"
		(extends "JQC-3FF-005-1H")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-048-1H"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPST_Hongfa_JQC-3FF_0XX-1H"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPST NO Relay, 48V Coil nom. 0.51W, 15A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPST*Hongfa*JQC*3FF*0XX*1H*"
			(at 0 0 0)
		)
	)
	(symbol "JQC-3FF-048-1Z"
		(extends "JQC-3FF-005-1Z")
		(property "Reference" "K"
			(at 11.43 3.81 0)
		)
		(property "Value" "JQC-3FF-048-1Z"
			(at 11.43 1.27 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_Hongfa_JQC-3FF_0XX-1Z"
			(at 11.43 -1.27 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/2071105/0/0/1/JQC-3FF.pdf"
			(at 0 0 0)
		)
		(property "Description" "Subminiature High Power SPDT Relay, 48V Coil nom. 0.51W, 10A switching current, max 10A@277VAC/28VDC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hongmei"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*SPDT*Hongfa*JQC*3FF*0XX*1Z*"
			(at 0 0 0)
		)
	)
)
