(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ATAES132A-SH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "ATAES132A-SH"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATAES132A-Data-Sheet-40002023A.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "32K AES serial EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "cryptographic security AES SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATAES132A-SH_0_1")
		(symbol "ATAES132A-SH_1_1"
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SI/SDA")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATECC608A-MAHDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "ATECC608A-MAHDA"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATECC608A-CryptoAuthentication-Device-Summary-Data-Sheet-DS40001977B.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Cryptographic Co-Processor with Secure Hardware-based 16 Key Storage, ECDSA and ECDH support, I2C, UDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cryptographic coprocessor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATECC608A-MAHDA_0_1")
		(symbol "ATECC608A-MAHDA_1_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATECC608A-SSHDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "ATECC608A-SSHDA"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATECC608A-CryptoAuthentication-Device-Summary-Data-Sheet-DS40001977B.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Cryptographic Co-Processor with Secure Hardware-based 16 Key Storage, ECDSA and ECDH support, I2C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cryptographic coprocessor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATECC608A-SSHDA_0_1")
		(symbol "ATECC608A-SSHDA_1_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATECC508A-MAHDA"
		(extends "ATECC608A-MAHDA")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "ATECC508A-MAHDA"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/20005928A.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Cryptographic Co-Processor with Secure Hardware-based 16 Key Storage, ECDSA and ECDH support, I2C, UDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cryptographic coprocessor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATECC508A-SSHDA"
		(extends "ATECC608A-SSHDA")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "ATECC508A-SSHDA"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/20005928A.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Cryptographic Co-Processor with Secure Hardware-based 16 Key Storage, ECDSA and ECDH support, I2C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cryptographic coprocessor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATECC608B-MAHDA"
		(extends "ATECC608A-MAHDA")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "ATECC608B-MAHDA"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/SCBU/ProductDocuments/DataSheets/ATECC608B-CryptoAuthentication-Device-Summary-Data-Sheet-DS40002239B.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Cryptographic Co-Processor with Secure Hardware-based 16 Key Storage, ECDSA and ECDH support, I2C, UDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cryptographic coprocessor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATECC608B-SSHDA"
		(extends "ATECC608A-SSHDA")
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "ATECC608B-SSHDA"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/SCBU/ProductDocuments/DataSheets/ATECC608B-CryptoAuthentication-Device-Summary-Data-Sheet-DS40002239B.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Cryptographic Co-Processor with Secure Hardware-based 16 Key Storage, ECDSA and ECDH support, I2C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cryptographic coprocessor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
