(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADE7758"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 28.575 0)
		)
		(property "Value" "ADE7758"
			(at -7.62 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 6.35 -26.67 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADE7758.pdf"
			(at 7.62 30.48 0)
		)
		(property "Description" "Poly Phase Multifunction Energy Metering, SO-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Metering"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADE7758_0_1")
		(symbol "ADE7758_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "IAP")
				(number "5")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "IAN")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IBP")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IBN")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ICP")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ICN")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VAP")
				(number "16")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "VBP")
				(number "15")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "VCP")
				(number "14")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "AVDD")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "VN")
				(number "13")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "DVDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "11")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "2")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "CLKOUT")
				(number "20")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "CLKIN")
				(number "19")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "APCF")
				(number "1")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VARCF")
				(number "17")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "DOUT")
				(number "24")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DIN")
				(number "22")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SCLK")
				(number "23")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{CS}")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{IRQ}")
				(number "18")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "REFIN/OUT")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADE7763xRS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 28.575 0)
		)
		(property "Value" "ADE7763xRS"
			(at -7.62 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 6.35 -26.67 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADE7763.pdf"
			(at 7.62 30.48 0)
		)
		(property "Description" "Single-Phase Active and Apparent Energy Metering, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Metering"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADE7763xRS_0_1")
		(symbol "ADE7763xRS_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "V1P")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "V1N")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "V2P")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "V2N")
				(number "6")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "REFIN/OUT")
				(number "9")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "AVDD")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "8")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "DVDD")
				(number "2")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "10")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "CLKIN")
				(number "15")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "CLKOUT")
				(number "16")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "DOUT")
				(number "19")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DIN")
				(number "20")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SCLK")
				(number "18")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{CS}")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{IRQ}")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{SAG}")
				(number "13")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "ZX")
				(number "12")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "CF")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADE7953xCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 22.86 0)
		)
		(property "Value" "ADE7953xCP"
			(at -12.7 25.4 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-28-1EP_5x5mm_P0.5mm_EP3.14x3.14mm"
			(at 6.35 -29.21 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADE7953.pdf"
			(at 7.62 27.94 0)
		)
		(property "Description" "Single Phase Multifunction Energy Metering with Neutral Current Measurement, LFCSP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Energy Metering"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADE7953xCP_0_1")
		(symbol "ADE7953xCP_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "IAP")
				(number "5")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IAN")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IBP")
				(number "9")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IBN")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VN")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VP")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "PULL_HIGH")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PULL_HIGH")
				(number "8")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PULL_LOW")
				(number "14")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "4")
			)
			(pin power_out line
				(at 0 25.4 270)
				(length 2.54)
				(name "VINTD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "16")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VINTA")
				(number "15")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "29")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "ZX")
				(number "1")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{REVP}")
				(number "20")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "ZX_I")
				(number "21")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{CS}")
				(number "28")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "MOSI/SCL/RX")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "MISO/SDA/TX")
				(number "26")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "25")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CF1")
				(number "23")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CF2")
				(number "24")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{IRQ}")
				(number "22")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "REF")
				(number "13")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "CLKOUT")
				(number "19")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "CLKIN")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AM2302"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "AM2302"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Sensor:ASAIR_AM2302_P2.54mm_Vertical"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://akizukidenshi.com/download/ds/aosong/AM2302.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "3.3 to 5.0V, Temperature and humidity module,  DHT22, AM2302"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ASAIR*AM2302*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "AM2302_0_1")
		(symbol "AM2302_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APDS-9960"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "APDS-9960"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Sensor:Avago_APDS-9960"
			(at 0 5.969 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/AV02-4191EN"
			(at 0.127 -6.223 0)
		)
		(property "Description" "Digital Proximity, Ambient Light, RGB and Gesture Sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor gesture light rgb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Avago?APDS?9960*"
			(at 0 0 0)
		)
		(symbol "APDS-9960_0_1")
		(symbol "APDS-9960_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INT")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LED_A")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "LED_K")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LDR")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS3935"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 15.24 0)
		)
		(property "Value" "AS3935"
			(at 5.08 12.7 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLPQ-16-1EP_4x4mm_P0.65mm_EP2.8x2.8mm"
			(at 20.32 22.86 0)
		)
		(property "Datasheet" "https://www.embeddedadventures.com/datasheets/AS3935_Datasheet_EN_v2.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Programmable fully integrated Lightning Sensor IC"
			(at 0 0 0)
		)
		(property "ki_keywords" "lightning sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MLPQ*16*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AS3935_0_1")
		(symbol "AS3935_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ACG")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN-")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "AD0")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "AD1")
				(number "16")
			)
			(pin passive line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VReg")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GNDPAD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CS")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "MISO")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "MOSI/SDA")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SCL")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IRQ")
				(number "10")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "SI")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BL0937"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 -10.16 0)
		)
		(property "Value" "BL0937"
			(at 5.08 -7.62 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -17.78 0)
		)
		(property "Datasheet" "http://www.belling.com.cn/media/file_object/bel_product/BL0937/datasheet/BL0937_V1.02_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Phase Energy Meter IC with Integrated Oscillator, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BL0937_0_1")
		(symbol "BL0937_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IP")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VP")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CF")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "CF1")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SEL")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BME280"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "BME280"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_LGA:Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering"
			(at 38.1 -11.43 0)
		)
		(property "Datasheet" "https://www.bosch-sensortec.com/media/boschsensortec/downloads/datasheets/bst-bme280-ds002.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "3-in-1 sensor, humidity, pressure, temperature, I2C and SPI interface, 1.71-3.6V, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bosch pressure humidity temperature environment environmental measurement digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*2.5x2.5mm*P0.65mm*Clockwise*"
			(at 0 0 0)
		)
		(symbol "BME280_0_1")
		(symbol "BME280_1_1"
			(pin power_in line
				(at -2.54 15.24 270)
				(length 5.08)
				(name "VDDIO")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "SDO")
				(number "5")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "SCK")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "SDI")
				(number "3")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "CSB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BME680"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "BME680"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_LGA:Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering"
			(at 36.83 -11.43 0)
		)
		(property "Datasheet" "https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BME680-DS001.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "4-in-1 sensor, gas, humidity, pressure, temperature, I2C and SPI interface, 1.71-3.6V, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bosch gas pressure humidity temperature environment environmental measurement digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*3x3mm*P0.8mm*Clockwise*"
			(at 0 0 0)
		)
		(symbol "BME680_0_1")
		(symbol "BME680_1_1"
			(pin power_in line
				(at -2.54 15.24 270)
				(length 5.08)
				(name "VDDIO")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "SDO")
				(number "5")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "SCK")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "SDI")
				(number "3")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "CSB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DHT11"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DHT11"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Sensor:Aosong_DHT11_5.5x12.0_P2.54mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://akizukidenshi.com/download/ds/aosong/DHT11.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "3.3V to 5.5V, temperature and humidity module, DHT11"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Aosong*DHT11*5.5x12.0*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "DHT11_0_1")
		(symbol "DHT11_1_1"
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "DATA")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA260"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "INA260"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina260.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Current/power/voltage monitor with Integrated 2mΩ Shunt Resistor, 2.7V - 5.5V, I2C, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Current/power/voltage monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "INA260_0_1")
		(symbol "INA260_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN+")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN+")
				(number "2")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN+")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VBUS")
				(number "12")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN-")
				(number "14")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN-")
				(number "15")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN-")
				(number "16")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VS")
				(number "10")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ALERT")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "A1")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2990"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 12.7 0)
		)
		(property "Value" "LTC2990"
			(at 3.81 -12.7 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2990.pdf"
			(at -15.24 12.7 0)
		)
		(property "Description" "Temperature Voltage and Current Monitor, I2C Interface, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature Voltage Current Monitor I2C AFE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2990_0_1")
		(symbol "LTC2990_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "V3")
				(number "3")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "V4")
				(number "4")
			)
			(pin passive line
				(at -7.62 15.24 270)
				(length 3.81)
				(name "V2")
				(number "2")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 3.81)
				(name "V1")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 3.81)
				(name "SCL")
				(number "7")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "ADR0")
				(number "8")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "ADR1")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX30102"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 15.24 0)
		)
		(property "Value" "MAX30102"
			(at 7.62 12.7 0)
		)
		(property "Footprint" "OptoDevice:Maxim_OLGA-14_3.3x5.6mm_P0.8mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX30102.pdf"
			(at 0 0 0)
		)
		(property "Description" "Heart Rate Sensor, 14-OLGA"
			(at 0 0 0)
		)
		(property "ki_keywords" "Heart Rate"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maxim*OLGA*3.3x5.6mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MAX30102_0_1")
		(symbol "MAX30102_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VLED+")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VLED+")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{INT}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Nuclear-Radiation_Detector"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 5.08 1.27 0)
		)
		(property "Value" "Nuclear-Radiation_Detector"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic radiation detector"
			(at 0 0 0)
		)
		(property "ki_keywords" "nuclear ionising radiation sensor geiger mueller muller tube neutron counter ionization chamber"
			(at 0 0 0)
		)
		(symbol "Nuclear-Radiation_Detector_0_0"
			(text "+"
				(at 2.032 3.175 0)
			)
		)
		(symbol "Nuclear-Radiation_Detector_0_1")
		(symbol "Nuclear-Radiation_Detector_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RPR-0521RS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "RPR-0521RS"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Sensor:Rohm_RPR-0521RS"
			(at 0 5.969 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/opto/optical_sensor/opto_module/rpr-0521rs-e.pdf"
			(at 0.127 -6.223 0)
		)
		(property "Description" "Digital Proximity and Ambient Light Sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor light"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Rohm?RPR?0521*"
			(at 0 0 0)
		)
		(symbol "RPR-0521RS_0_1")
		(symbol "RPR-0521RS_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INT")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LED_A")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "LED_K")
				(number "5")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LDR")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SHT1x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "SHT1x"
			(at 2.54 -6.35 0)
		)
		(property "Footprint" "Sensor:SHT1x"
			(at 3.81 6.35 0)
		)
		(property "Datasheet" "https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/0_Datasheets/Humidity/Sensirion_Humidity_Sensors_SHT1x_Datasheet.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Temperature and humidity module"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature humidity sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SHT1x*"
			(at 0 0 0)
		)
		(symbol "SHT1x_0_1")
		(symbol "SHT1x_1_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "DATA")
				(number "2")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CHT11"
		(extends "DHT11")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "CHT11"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Sensor:Aosong_DHT11_5.5x12.0_P2.54mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://aosong.com/en/products-21.html"
			(at 3.81 6.35 0)
		)
		(property "Description" "Temperature and humidity module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital temperature humidity sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Aosong*DHT11*5.5x12.0*P2.54mm*"
			(at 0 0 0)
		)
	)
)
