(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ICS-43434"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "MK"
			(at -7.62 6.35 0)
		)
		(property "Value" "ICS-43434"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Sensor_Audio:InvenSense_ICS-43434-6_3.5x2.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.invensense.com/wp-content/uploads/2016/02/DS-000069-ICS-43434-v1.2.pdf"
			(at 0 0 0)
		)
		(property "Description" "TDK InvenSense MEMS Microphone, 24-bit I2S, 65 dBA SNR, LGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "microphone MEMS 24bit I2S ICS-43434 TDK InvenSense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "InvenSense*ICS*43434*"
			(at 0 0 0)
		)
		(symbol "ICS-43434_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "LR")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "WS")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCK")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SD")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IM69D120"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "MK"
			(at -7.62 6.35 0)
		)
		(property "Value" "IM69D120"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Sensor_Audio:Infineon_PG-LLGA-5-1"
			(at 17.78 -7.62 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IM69D120-DS-v01_00-EN.pdf?fileId=5546d462602a9dc801607a0e41a01a2b"
			(at 0 0 0)
		)
		(property "Description" "High performance digital XENSIV MEMS microphone, -26 dBFS Sensitivity, LLGA-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems microphone"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*LLGA*"
			(at 0 0 0)
		)
		(symbol "IM69D120_0_1")
		(symbol "IM69D120_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SELECT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CLOCK")
				(number "3")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DATA")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IM73A135V01"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "MK"
			(at 5.08 6.35 0)
		)
		(property "Value" "IM73A135V01"
			(at 11.43 -6.35 0)
		)
		(property "Footprint" "Sensor_Audio:Infineon_PG-LLGA-5-2"
			(at 0 19.05 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IM73A135-DataSheet-v01_00-EN.pdf?fileId=8ac78c8c7f2a768a017fadec36b84500"
			(at 0 -17.78 0)
		)
		(property "Description" "IP57 Water and Dust Resistant, Differential MEMS Microphone, 135dBSPL AOP, 73dB SNR, PG-LLGA-5-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microphone MEMS analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*LLGA*"
			(at 0 0 0)
		)
		(symbol "IM73A135V01_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT+")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP45DT02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "MK"
			(at -7.62 6.35 0)
		)
		(property "Value" "MP45DT02"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Sensor_Audio:ST_HLGA-6_3.76x4.72mm_P1.65mm"
			(at -22.86 -8.89 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00025467.pdf"
			(at 0 0 0)
		)
		(property "Description" "MEMS Omnidirectional Digital Microphone, HLGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "MEMS Microphone"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*HLGA*3.76x4.72mm*P1.65mm*"
			(at 0 0 0)
		)
		(symbol "MP45DT02_0_1")
		(symbol "MP45DT02_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LR")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CLK")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPH0641LU4H-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "MK"
			(at 5.08 6.35 0)
		)
		(property "Value" "SPH0641LU4H-1"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Sensor_Audio:Knowles_LGA-5_3.5x2.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.knowles.com/docs/default-source/model-downloads/sph0641lu4h-1-revb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital MEMS Microphone, LGA-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microphone MEMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Knowles*LGA*3.5x2.65mm*"
			(at 0 0 0)
		)
		(symbol "SPH0641LU4H-1_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SEL")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CLOCK")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DATA")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPH0645LM4H"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "MK"
			(at -7.62 6.35 0)
		)
		(property "Value" "SPH0645LM4H"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Sensor_Audio:Knowles_SPH0645LM4H-6_3.5x2.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.knowles.com/docs/default-source/default-document-library/sph0645lm4h-1-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Knowles MEMS Microphone, 24-bit I2S, 65 dBA SNR, LGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "microphone MEMS I2S 24bit Knowles SPH0645LM4H Crawford"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Knowles*SPH0645LM4H*"
			(at 0 0 0)
		)
		(symbol "SPH0645LM4H_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SEL")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "WS")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BCLK")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DATA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPM0687LR5H-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "MK"
			(at 5.08 6.35 0)
		)
		(property "Value" "SPM0687LR5H-1"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Sensor_Audio:Knowles_LGA-6_4.72x3.76mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.knowles.com/docs/default-source/default-document-library/spm0687lr5h-1_winfrey_datasheet.pdf?Status=Master&sfvrsn=ac3971b1_0"
			(at 0 0 0)
		)
		(property "Description" "Differential/Single-Ended Analog MEMS Microphone, LGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microphone MEMS Knowles Sisonic winfrey"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Knowles*LGA*4.72x3.76mm*"
			(at 0 0 0)
		)
		(symbol "SPM0687LR5H-1_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT+")
				(number "1")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IM69D130"
		(extends "IM69D120")
		(property "Reference" "MK"
			(at -7.62 6.35 0)
		)
		(property "Value" "IM69D130"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Sensor_Audio:Infineon_PG-LLGA-5-1"
			(at 17.78 -7.62 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IM69D130-DS-v01_00-EN.pdf?fileId=5546d462602a9dc801607a0e46511a2e"
			(at 0 0 0)
		)
		(property "Description" "High performance digital XENSIV MEMS microphone, -36 dBFS Sensitivity, LLGA-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems microphone"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*LLGA*"
			(at 0 0 0)
		)
	)
)
