(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "A1363xKTTN-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1363xKTTN-1"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1363-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +0.6 to +1.3mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
		(symbol "A1363xKTTN-1_0_1")
		(symbol "A1363xKTTN-1_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A1365xKTTN-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1365xKTTN-1"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1365-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +0.6 to +1.3mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
		(symbol "A1365xKTTN-1_0_1")
		(symbol "A1365xKTTN-1_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A1369xUA-10"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1369xUA-10"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-3"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1369-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, -8.5 to -12.5mV/G, SIP-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
		(symbol "A1369xUA-10_0_1")
		(symbol "A1369xUA-10_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS706xLC-05C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS706xLC-05C"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS706ELC-05C-Datasheet.ashx"
			(at 0 0 0)
		)
		(property "Description" "±15A Bidirectional Hall Effect Linear Current Sensor, +5.0V supply, 133mV/A, SOIC-8, OBSOLETE"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS706xLC-05C_0_1")
		(symbol "ACS706xLC-05C_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP-")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS709xLFTR-6BB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "ACS709xLFTR-6BB"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_QSOP-24_3.9x8.7mm_P0.635mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS709-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±15A Bidirectional, Hall-Effect Current Sensor, +3.3V to +5.0V supply, 90mV/A @ +3.3V, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ACS709xLFTR-6BB_0_1")
		(symbol "ACS709xLFTR-6BB_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VOC")
				(number "21")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "FAULT_EN")
				(number "22")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "6")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "10")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "11")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "12")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IP-")
				(number "7")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "8")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "9")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VIOUT")
				(number "18")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "19")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FILTER")
				(number "17")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VZCR")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS710xLATR-6BB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS710xLATR-6BB"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS710-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±6A Bidirectional, Hall-Effect Current Sensor, Latched Fault, +3.3V to +5.0V supply, 151mV/A @ +5.0V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS710xLATR-6BB_0_1")
		(symbol "ACS710xLATR-6BB_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VOC")
				(number "15")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "FAULT_EN")
				(number "16")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "6")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "7")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VIOUT")
				(number "12")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "13")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FILTER")
				(number "11")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VZCR")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS711xEXLT-15AB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS711xEXLT-15AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_QFN-12-10-1EP_3x3mm_P0.5mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/Media/Files/Datasheets/ACS711-Datasheet.ashx"
			(at 0 0 0)
		)
		(property "Description" "±15A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 90mV/A, QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*QFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ACS711xEXLT-15AB_0_1")
		(symbol "ACS711xEXLT-15AB_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP-")
				(number "2")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "9")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS711xLCTR-12AB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS711xLCTR-12AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/Media/Files/Datasheets/ACS711-Datasheet.ashx"
			(at 0 0 0)
		)
		(property "Description" "±12.5A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 110mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS711xLCTR-12AB_0_1")
		(symbol "ACS711xLCTR-12AB_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IP-")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS712xLCTR-05B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS712xLCTR-05B"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS712-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±5A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 185mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS712xLCTR-05B_0_1")
		(symbol "ACS712xLCTR-05B_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IP-")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FILTER")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS717xMATR-10B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS717xMATR-10B"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS717-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±10A Bidirectional, Hall-Effect Current Sensor, +3.3V supply, 133mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS717xMATR-10B_0_1")
		(symbol "ACS717xMATR-10B_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "3")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "7")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "8")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS720xMATR-15B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 7.62 0)
		)
		(property "Value" "ACS720xMATR-15B"
			(at 8.89 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS720-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±15A Bidirectional, Hall-Effect Current Sensor, +5.0V supply, 90mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS720xMATR-15B_0_1")
		(symbol "ACS720xMATR-15B_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VOC_F")
				(number "15")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VOC_S")
				(number "16")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "7")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VIOUT")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{FAULT_F}")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FAULT_S}")
				(number "10")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FILTER")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS722xLCTR-05AB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS722xLCTR-05AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±5A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 264mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS722xLCTR-05AB_0_1")
		(symbol "ACS722xLCTR-05AB_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP-")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VIOUT")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BW_SEL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS722xMATR-10AB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS722xMATR-10AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±10A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 132mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS722xMATR-10AB_0_1")
		(symbol "ACS722xMATR-10AB_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "3")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "7")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "12")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BW_SEL")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS724xMATR-12AB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS724xMATR-12AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±12A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 166mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS724xMATR-12AB_0_1")
		(symbol "ACS724xMATR-12AB_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "3")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "7")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "12")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FILTER")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS726xLFTR-20B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 16.51 0)
		)
		(property "Value" "ACS726xLFTR-20B"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_QSOP-24_3.9x8.7mm_P0.635mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS726-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 100mV/A, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ACS726xLFTR-20B_0_1")
		(symbol "ACS726xLFTR-20B_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "3")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "5")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "6")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "10")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "11")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "12")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IP-")
				(number "7")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "8")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "9")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "22")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "NC")
				(number "23")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "NC")
				(number "24")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VOUTGP")
				(number "21")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VOUTGN")
				(number "20")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VINGN")
				(number "19")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "VINGP")
				(number "18")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VOUTP")
				(number "17")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VOUTN")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS730xLCTR-20AB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS730xLCTR-20AB"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS730-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS730xLCTR-20AB_0_1")
		(symbol "ACS730xLCTR-20AB_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP-")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VZCR")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS732xLATR-40AB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS732xLATR-40AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS732-ACS733-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±40A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 50mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACS732xLATR-40AB_0_1")
		(symbol "ACS732xLATR-40AB_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VOC")
				(number "14")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "3")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "7")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "8")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PROGRAM")
				(number "11")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS756xCB-050B-PFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS756xCB-050B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS756-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
		(symbol "ACS756xCB-050B-PFF_0_1")
		(symbol "ACS756xCB-050B-PFF_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS758xCB-100B-PSF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-100B-PSF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±100A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 20mV/A, CB-5 PSF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSF*"
			(at 0 0 0)
		)
		(symbol "ACS758xCB-100B-PSF_0_1")
		(symbol "ACS758xCB-100B-PSF_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS758xCB-150B-PSS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-150B-PSS"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSS"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±150A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 13.3mV/A, CB-5 PSS"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSS*"
			(at 0 0 0)
		)
		(symbol "ACS758xCB-150B-PSS_0_1")
		(symbol "ACS758xCB-150B-PSS_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IP+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VIOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACS780xLRTR-050B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS780xLRTR-050B"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS780-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
		(symbol "ACS780xLRTR-050B_0_1")
		(symbol "ACS780xLRTR-050B_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IP+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IP-")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 90)
				(length 2.54)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CKSR_15-NP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 8.89 0)
		)
		(property "Value" "CKSR_15-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_CKSR"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/cksr_xx-np_v14.pdf"
			(at 4.572 0 0)
		)
		(property "Description" "Current Transducer, 15A, Unipolar, 0-5V Output, 4 Primary Windings"
			(at 0.762 0 0)
		)
		(property "ki_keywords" "Lem transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*CKSR*"
			(at 0 0 0)
		)
		(symbol "CKSR_15-NP_0_1")
		(symbol "CKSR_15-NP_1_1"
			(pin passive line
				(at -10.16 10.16 270)
				(length 2.54)
				(name "IN1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 90)
				(length 2.54)
				(name "OUT1")
				(number "9")
			)
			(pin passive line
				(at -7.62 10.16 270)
				(length 2.54)
				(name "IN2")
				(number "3")
			)
			(pin passive line
				(at -7.62 -10.16 90)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "IN3")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "OUT3")
				(number "7")
			)
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "IN4")
				(number "5")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "OUT4")
				(number "6")
			)
			(pin power_in line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "U_{c}")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin bidirectional line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "U_{ref}")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "U_{out}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CKSR_50-NP-SP1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 8.89 0)
		)
		(property "Value" "CKSR_50-NP-SP1"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_CKSR"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/cksr_50-np_sp1_v3.pdf"
			(at 4.572 0 0)
		)
		(property "Description" "Current Transducer, 50A, Unipolar, 0-5V Output, 3 Primary Windings"
			(at 0.762 0 0)
		)
		(property "ki_keywords" "Lem transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*CKSR*"
			(at 0 0 0)
		)
		(symbol "CKSR_50-NP-SP1_0_1")
		(symbol "CKSR_50-NP-SP1_1_1"
			(pin passive line
				(at -7.62 10.16 270)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin passive line
				(at -7.62 -10.16 90)
				(length 2.54)
				(name "OUT1")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "IN2")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "IN3")
				(number "5")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "OUT3")
				(number "6")
			)
			(pin power_in line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "U_{c}")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin bidirectional line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "U_{ref}")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "U_{out}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CKSR_75-NP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 8.89 0)
		)
		(property "Value" "CKSR_75-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_CKSR"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/cksr_75-np_v2.pdf"
			(at 4.572 0 0)
		)
		(property "Description" "Current Transducer, 75A, Unipolar, 0-5V Output, 5 Primary Windings"
			(at 0.762 0 0)
		)
		(property "ki_keywords" "Lem transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*CKSR*"
			(at 0 0 0)
		)
		(symbol "CKSR_75-NP_0_1")
		(symbol "CKSR_75-NP_1_1"
			(pin passive line
				(at -12.7 10.16 270)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin passive line
				(at -12.7 -10.16 90)
				(length 2.54)
				(name "OUT1")
				(number "10")
			)
			(pin passive line
				(at -10.16 10.16 270)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 90)
				(length 2.54)
				(name "OUT2")
				(number "9")
			)
			(pin passive line
				(at -7.62 10.16 270)
				(length 2.54)
				(name "IN3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -10.16 90)
				(length 2.54)
				(name "OUT3")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "IN4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "OUT4")
				(number "7")
			)
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "IN5")
				(number "5")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "OUT5")
				(number "6")
			)
			(pin power_in line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "U_{c}")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin bidirectional line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "U_{ref}")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "U_{out}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CQ-2063"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2063"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2063.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Bidirectional, -35A to +35A, 60mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
		(symbol "CQ-2063_0_1")
		(symbol "CQ-2063_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "P")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "N")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "DATA_IO")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "SCLK")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CQ-2092"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2092"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7S"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2092.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Bidirectional, -21A to +21A, 100mV/A, CQ-7S"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*S*"
			(at 0 0 0)
		)
		(symbol "CQ-2092_0_1")
		(symbol "CQ-2092_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "P")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "N")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "DATA_IO")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "SCLK")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CQ-3200"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-3200"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-3200.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -8.5A to +8.5A, 155mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CQ-3200_0_1")
		(symbol "CQ-3200_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "P")
				(number "10")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "N")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "TAB")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "TAB")
				(number "8")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "TEST2")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "TEST1")
				(number "2")
			)
			(pin power_in line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "TEST3")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSLW6B1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "CSLW6B1"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Honeywell_CSLW"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://sensing.honeywell.com/honeywell-sensing-cslw-series-product-sheet-005861-1-en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Wired Open-Loop Current Sensors, 1A"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Honeywell*CSLW*"
			(at 0 0 0)
		)
		(symbol "CSLW6B1_0_1")
		(symbol "CSLW6B1_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Iin")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Iout")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VS")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CZ-3813"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 11.43 0)
		)
		(property "Value" "CZ-3813"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CZ_SSOP-10_6.5x8.1mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CZ-3813.pdf"
			(at 0 0 0)
		)
		(property "Description" "Coreless Current Sensor, Bidirectional, -33.0A to +33.0A, 60mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CZ*SSOP*6.5x8.1mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "CZ-3813_0_1")
		(symbol "CZ-3813_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IP")
				(number "10")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN")
				(number "9")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OCD")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "DIO")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SCLK")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HO40-NP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO40-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO40-NP"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 40A, Unipolar, 5V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO40*NP*"
			(at 0 0 0)
		)
		(symbol "HO40-NP_0_1")
		(symbol "HO40-NP_1_1"
			(pin passive line
				(at -12.7 10.16 270)
				(length 2.54)
				(name "IN1")
				(number "6")
			)
			(pin passive line
				(at -12.7 -10.16 90)
				(length 2.54)
				(name "OUT1")
				(number "13")
			)
			(pin passive line
				(at -10.16 10.16 270)
				(length 2.54)
				(name "IN2")
				(number "7")
			)
			(pin passive line
				(at -10.16 -10.16 90)
				(length 2.54)
				(name "OUT2")
				(number "12")
			)
			(pin passive line
				(at -7.62 10.16 270)
				(length 2.54)
				(name "IN3")
				(number "8")
			)
			(pin passive line
				(at -7.62 -10.16 90)
				(length 2.54)
				(name "OUT3")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "IN4")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "OUT4")
				(number "10")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "+U_{c}")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "0V")
				(number "2")
			)
			(pin bidirectional line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "U_{ref}")
				(number "4")
			)
			(pin open_collector line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OCD")
				(number "5")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "U_{out}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HO8-NP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO8-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO8-NP"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np-0000_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 8A, Unipolar, 5V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO8*NP*"
			(at 0 0 0)
		)
		(symbol "HO8-NP_0_1")
		(symbol "HO8-NP_1_1"
			(pin passive line
				(at -10.16 10.16 270)
				(length 2.54)
				(name "IN1")
				(number "8")
			)
			(pin passive line
				(at -10.16 -10.16 90)
				(length 2.54)
				(name "OUT1")
				(number "13")
			)
			(pin passive line
				(at -7.62 10.16 270)
				(length 2.54)
				(name "IN2")
				(number "9")
			)
			(pin passive line
				(at -7.62 -10.16 90)
				(length 2.54)
				(name "OUT2")
				(number "12")
			)
			(pin passive line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "IN3")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "OUT3")
				(number "11")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "+U_{c}")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "0V")
				(number "2")
			)
			(pin bidirectional line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "U_{ref}")
				(number "4")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "NA")
				(number "7")
			)
			(pin open_collector line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OCD")
				(number "5")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "Standby")
				(number "6")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "U_{out}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HTFS200-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "HTFS200-P"
			(at 0 10.16 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HTFS"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/htfs_200_800-p.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 200A, Unipolar, 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HTFS*"
			(at 0 0 0)
		)
		(symbol "HTFS200-P_0_1")
		(symbol "HTFS200-P_1_1"
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "+Vc")
				(number "1")
			)
			(pin passive line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "Vref")
				(number "4")
			)
			(pin power_in line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX02-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX02-P"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX02-P"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%202_6-p_e%20v5.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 2A, Bipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX02*P*"
			(at 0 0 0)
		)
		(symbol "HX02-P_0_1")
		(symbol "HX02-P_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX03-P-SP2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX03-P-SP2"
			(at 13.97 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX03-P-SP2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%203_50-p_sp2_e%20v07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 3A, Unipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX03*P*SP2*"
			(at 0 0 0)
		)
		(symbol "HX03-P-SP2_0_1")
		(symbol "HX03-P-SP2_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX04-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX04-P"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX04-P"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%202_6-p_e%20v5.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 4A, Bipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX04*P*"
			(at 0 0 0)
		)
		(symbol "HX04-P_0_1")
		(symbol "HX04-P_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX05-NP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX05-NP"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX05-NP"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%205_15-np_e%20v10.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 5A, Bipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX05*NP*"
			(at 0 0 0)
		)
		(symbol "HX05-NP_0_1")
		(symbol "HX05-NP_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN1+")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN2+")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN1-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN2-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX05-P-SP2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX05-P-SP2"
			(at 13.97 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX05-P-SP2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%203_50-p_sp2_e%20v07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 5A, Unipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX05*P*SP2*"
			(at 0 0 0)
		)
		(symbol "HX05-P-SP2_0_1")
		(symbol "HX05-P-SP2_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX06-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX06-P"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX06-P"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%202_6-p_e%20v5.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 6A, Bipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX06*P*"
			(at 0 0 0)
		)
		(symbol "HX06-P_0_1")
		(symbol "HX06-P_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX10-NP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX10-NP"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX10-NP"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%205_15-np_e%20v10.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 10A, Bipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX10*NP*"
			(at 0 0 0)
		)
		(symbol "HX10-NP_0_1")
		(symbol "HX10-NP_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN1+")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN2+")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN1-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN2-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX10-P-SP2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX10-P-SP2"
			(at 13.97 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX10-P-SP2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%203_50-p_sp2_e%20v07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 10A, Unipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX10*P*SP2*"
			(at 0 0 0)
		)
		(symbol "HX10-P-SP2_0_1")
		(symbol "HX10-P-SP2_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX15-NP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX15-NP"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX15-NP"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%205_15-np_e%20v10.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 15A, Bipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX15*NP*"
			(at 0 0 0)
		)
		(symbol "HX15-NP_0_1")
		(symbol "HX15-NP_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN1+")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN2+")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN1-")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN2-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX15-P-SP2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX15-P-SP2"
			(at 13.97 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX15-P-SP2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%203_50-p_sp2_e%20v07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 15A, Unipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX15*P*SP2*"
			(at 0 0 0)
		)
		(symbol "HX15-P-SP2_0_1")
		(symbol "HX15-P-SP2_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX20-P-SP2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX20-P-SP2"
			(at 13.97 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX20-P-SP2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%203_50-p_sp2_e%20v07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 20A, Unipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX20*P*SP2*"
			(at 0 0 0)
		)
		(symbol "HX20-P-SP2_0_1")
		(symbol "HX20-P-SP2_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX25-P-SP2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX25-P-SP2"
			(at 13.97 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX25-P-SP2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%203_50-p_sp2_e%20v07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 25A, Unipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX25*P*SP2*"
			(at 0 0 0)
		)
		(symbol "HX25-P-SP2_0_1")
		(symbol "HX25-P-SP2_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HX50-P-SP2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HX50-P-SP2"
			(at 13.97 8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HX50-P-SP2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/hx%203_50-p_sp2_e%20v07.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 50A, Unipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HX50*P*SP2*"
			(at 0 0 0)
		)
		(symbol "HX50-P-SP2_0_1")
		(symbol "HX50-P-SP2_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2175"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2175"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2175.pdf?fileId=5546d462533600a4015355c9161216c6"
			(at 0 0 0)
		)
		(property "Description" "Linear Current Sensing IC, PWM output, 600V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge current sense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2175_0_1")
		(symbol "IR2175_1_1"
			(pin output line
				(at -7.62 0 0)
				(length 2.54)
				(name "PO")
				(number "2")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{OC}")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "3")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VB")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "VIN+")
				(number "8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR21771S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 15.875 0)
		)
		(property "Value" "IR21771S"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir21771s.pdf?fileId=5546d462533600a4015355c9222c16c8"
			(at 0 0 0)
		)
		(property "Description" "Phase Current Sensor IC for AC Motor Control, PWM output, 600V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge current sense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR21771S_0_1")
		(symbol "IR21771S_1_1"
			(pin open_collector line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "PO")
				(number "7")
			)
			(pin open_collector line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "OC")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 2.54)
				(name "VB")
				(number "16")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "G0")
				(number "11")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "G1")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "VIN-")
				(number "14")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VIN+")
				(number "15")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "VS")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2177S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 15.875 0)
		)
		(property "Value" "IR2177S"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2177s.pdf?fileId=5546d462533600a4015355c92e7416cb"
			(at 0 0 0)
		)
		(property "Description" "Phase Current Sensor IC for AC Motor Control, PWM and ADC output, 600V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge current sense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR2177S_0_1")
		(symbol "IR2177S_1_1"
			(pin open_collector line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "PO")
				(number "7")
			)
			(pin open_collector line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "OC")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "VRH")
				(number "5")
			)
			(pin output line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "VRL")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 2.54)
				(name "VB")
				(number "16")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "G0")
				(number "11")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "G1")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "VIN-")
				(number "14")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VIN+")
				(number "15")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "VS")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR25750L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "IR25750L"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir25750lpbf.pdf?fileId=5546d462533600a4015355ca1d0e16f7"
			(at 0 0 0)
		)
		(property "Description" "Current Sensing IC, 600V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single current sense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "IR25750L_0_1")
		(symbol "IR25750L_1_1"
			(pin output line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "CS")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "GATE")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VS")
				(number "5")
			)
			(pin power_in line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "COM")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LA25-NP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.938 11.176 0)
		)
		(property "Value" "LA25-NP"
			(at -14.224 -0.254 90)
		)
		(property "Footprint" "Sensor_Current:LEM_LA25-NP"
			(at 1.27 0 90)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/la%2025-np.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Current Transducer, 25A, Tripolar, +/-15V"
			(at 1.27 0 90)
		)
		(property "ki_keywords" "Current Transducer LEM "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*LA25*NP*"
			(at 0 0 0)
		)
		(symbol "LA25-NP_0_1")
		(symbol "LA25-NP_1_1"
			(pin input line
				(at -10.16 12.7 270)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 -12.7 90)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin input line
				(at -7.62 12.7 270)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 -12.7 90)
				(length 2.54)
				(name "OUT")
				(number "9")
			)
			(pin input line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin input line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
			(pin input line
				(at 0 12.7 270)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at 0 -12.7 90)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin power_in line
				(at 5.08 12.7 270)
				(length 2.54)
				(name "+")
				(number "12")
			)
			(pin power_in line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "-")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "M")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LA25-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LA25-P"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Sensor_Current:LEM_LA25-P"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/la_25-p.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 25A, Bipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*LA25*P*"
			(at 0 0 0)
		)
		(symbol "LA25-P_0_1")
		(symbol "LA25-P_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "M")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTSR6-NP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LTSR6-NP"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Sensor_Current:LEM_LTSR-NP"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ltsr_6-np.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Current Transducer, Unipolar, 6A, 5V supply, DC, AC, pulsed"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*LTSR*NP*"
			(at 0 0 0)
		)
		(symbol "LTSR6-NP_0_1")
		(symbol "LTSR6-NP_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN3")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUT6")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OUT5")
				(number "5")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "OUT4")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "+5V")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "0V")
				(number "9")
			)
			(pin passive line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "Ref")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Out")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCA1101-65-5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.858 11.43 0)
		)
		(property "Value" "MCA1101-65-5"
			(at 8.382 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -0.254 -27.432 0)
		)
		(property "Datasheet" "https://navview.blob.core.windows.net/web-resources/6020-1102-01%20RevG_MCA1101_Fix%20Gain%205V_10112021.pdf"
			(at 0.254 -23.114 0)
		)
		(property "Description" "High Accuracy Current Sensor IC with 1.5MHz 3dB Bandwidth and Isolation, ±65A, 5V Supply, Fixed Gain, 27 mV/A, SOIC-16W"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "amr-sensor isolated-current-sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCA1101-65-5_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IP+")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP+")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IP-")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "IP-")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vout")
				(number "12")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Vref")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FAULTB}")
				(number "9")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VOC")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A1363xKTTN-10"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1363xKTTN-10"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1363-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +6.4 to +14mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1363xKTTN-2"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1363xKTTN-2"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1363-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +1.3 to +2.9mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1363xKTTN-5"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1363xKTTN-5"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1363-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +2.9 to +6.4mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1365xKTTN-10"
		(extends "A1365xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1365xKTTN-10"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1365-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +6.4 to +14mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1365xKTTN-2"
		(extends "A1365xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1365xKTTN-2"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1365-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +1.3 to +2.9mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1365xKTTN-5"
		(extends "A1365xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1365xKTTN-5"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1365-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +2.9 to +6.4mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1366xKTTN-1"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1366xKTTN-1"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1366-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +1mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1366xKTTN-10"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1366xKTTN-10"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1366-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +10mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1366xKTTN-2"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1366xKTTN-2"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1366-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +2.5mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1366xKTTN-5"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1366xKTTN-5"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1366-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +5mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1367xKTTN-1"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1367xKTTN-1"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1367-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +0.6 to +1.3mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1367xKTTN-10"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1367xKTTN-10"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1367-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +6.4 to +14mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1367xKTTN-2"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1367xKTTN-2"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1367-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +1.3 to +2.9mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1367xKTTN-5"
		(extends "A1363xKTTN-1")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1367xKTTN-5"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-4"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1367-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +2.9 to +6.4mV/G, SIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "A1369xUA-24"
		(extends "A1369xUA-10")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "A1369xUA-24"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-3"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1369-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, -22 to -26mV/G, SIP-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "ACS709xLFTR-10BB"
		(extends "ACS709xLFTR-6BB")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "ACS709xLFTR-10BB"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_QSOP-24_3.9x8.7mm_P0.635mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS709-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±24A Bidirectional, Hall-Effect Current Sensor, +3.3V to +5.0V supply, 85mV/A @ +3.3V, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS709xLFTR-20BB"
		(extends "ACS709xLFTR-6BB")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "ACS709xLFTR-20BB"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_QSOP-24_3.9x8.7mm_P0.635mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS709-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±37.5A Bidirectional, Hall-Effect Current Sensor, +3.3V to +5.0V supply, 56mV/A @ +3.3V, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS709xLFTR-35BB"
		(extends "ACS709xLFTR-6BB")
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "ACS709xLFTR-35BB"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_QSOP-24_3.9x8.7mm_P0.635mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS709-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±75A Bidirectional, Hall-Effect Current Sensor, +3.3V to +5.0V supply, 28mV/A @ +3.3V, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS710xLATR-10BB"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS710xLATR-10BB"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS710-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±12A Bidirectional, Hall-Effect Current Sensor, Latched Fault, +3.3V to +5.0V supply, 85mV/A @ +5.0V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS710xLATR-10BB-NL"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS710xLATR-10BB-NL"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS710-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±12A Bidirectional, Hall-Effect Current Sensor, +3.3V to +5.0V supply, 85mV/A @ +5.0V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS710xLATR-12BB"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS710xLATR-12BB"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS710-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±12.5A Bidirectional, Hall-Effect Current Sensor, Latched Fault, +3.3V to +5.0V supply, 56mV/A @ +5.0V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS710xLATR-12BB-NL"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS710xLATR-12BB-NL"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS710-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±12.5A Bidirectional, Hall-Effect Current Sensor, +3.3V to +5.0V supply, 56mV/A @ +5.0V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS710xLATR-25BB"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS710xLATR-25BB"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS710-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±25A Bidirectional, Hall-Effect Current Sensor, Latched Fault, +3.3V to +5.0V supply, 28mV/A @ +5.0V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS710xLATR-25BB-NL"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS710xLATR-25BB-NL"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS710-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±25A Bidirectional, Hall-Effect Current Sensor, +3.3V to +5.0V supply, 28mV/A @ +5.0V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS710xLATR-6BB-NL"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS710xLATR-6BB-NL"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS710-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±6A Bidirectional, Hall-Effect Current Sensor, +3.3V to +5.0V supply, 151mV/A @ +5.0V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS711xEXLT-31AB"
		(extends "ACS711xEXLT-15AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS711xEXLT-31AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_QFN-12-10-1EP_3x3mm_P0.5mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/Media/Files/Datasheets/ACS711-Datasheet.ashx"
			(at 0 0 0)
		)
		(property "Description" "±31A Bidirectional, Hall-Effect Current Sensor, +3.3V supply, 45mV/A, QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*QFN*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS711xLCTR-25AB"
		(extends "ACS711xLCTR-12AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS711xLCTR-25AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/Media/Files/Datasheets/ACS711-Datasheet.ashx"
			(at 0 0 0)
		)
		(property "Description" "±25A, Bidirectional, Hall-Effect Current Sensor, +3.3V supply, 55mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS712xLCTR-20A"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS712xLCTR-20A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS712-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS712xLCTR-30A"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS712xLCTR-30A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS712-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±30A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 66mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS713xLCTR-20A"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS713xLCTR-20A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS713-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "20A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 185mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS713xLCTR-30A"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS713xLCTR-30A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS713-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "30A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 133mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS714xLCTR-05B"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS714xLCTR-05B"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS714-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±5A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 185mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS714xLCTR-20A"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS714xLCTR-20A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS714-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS714xLCTR-30A"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS714xLCTR-30A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS714-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±30A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 66mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS714xLCTR-50A"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS714xLCTR-50A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS714-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS715xLCTR-20A"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS715xLCTR-20A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS715-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "20A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 185mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS715xLCTR-30A"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS715xLCTR-30A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS715-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "30A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 133mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS716xLATR-12BB"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS716xLATR-12BB"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS716-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±12.5A Bidirectional, Hall-Effect Current Sensor, Latched Fault, +3.3V supply, 37mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS716xLATR-12BB-NL"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS716xLATR-12BB-NL"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS716-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±12.5A Bidirectional, Hall-Effect Current Sensor, +3.3V supply, 37mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS716xLATR-25BB"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS716xLATR-25BB"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS716-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±25A Bidirectional, Hall-Effect Current Sensor, Latched Fault, +3.3V supply, 18.5mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS716xLATR-25BB-NL"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS716xLATR-25BB-NL"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS716-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±25A Bidirectional, Hall-Effect Current Sensor, +3.3V supply, 18.5mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS716xLATR-6BB"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS716xLATR-6BB"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS716-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±6A Bidirectional, Hall-Effect Current Sensor, Latched Fault, +3.3V supply, 100mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS716xLATR-6BB-NL"
		(extends "ACS710xLATR-6BB")
		(property "Reference" "U"
			(at 8.89 8.89 0)
		)
		(property "Value" "ACS716xLATR-6BB-NL"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS716-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±6A Bidirectional, Hall-Effect Current Sensor, +3.3V supply, 100mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS717xMATR-20B"
		(extends "ACS717xMATR-10B")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS717xMATR-20B"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS717-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional, Hall-Effect Current Sensor, +3.3V supply, 66mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS718xMATR-10B"
		(extends "ACS717xMATR-10B")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS718xMATR-10B"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS718-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±10A Bidirectional, Hall-Effect Current Sensor, +5.0V supply, 200mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS718xMATR-20B"
		(extends "ACS717xMATR-10B")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS718xMATR-20B"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS718-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional, Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS720xMATR-35B"
		(extends "ACS720xMATR-15B")
		(property "Reference" "U"
			(at 8.89 7.62 0)
		)
		(property "Value" "ACS720xMATR-35B"
			(at 8.89 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS720-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±35A Bidirectional, Hall-Effect Current Sensor, +5.0V supply, 38.5mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS720xMATR-65B"
		(extends "ACS720xMATR-15B")
		(property "Reference" "U"
			(at 8.89 7.62 0)
		)
		(property "Value" "ACS720xMATR-65B"
			(at 8.89 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS720-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±65A Bidirectional, Hall-Effect Current Sensor, +5.0V supply, 20.5mV/A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS722xLCTR-10AB"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS722xLCTR-10AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±10A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 132mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS722xLCTR-10AU"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS722xLCTR-10AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "10A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 264mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS722xLCTR-20AB"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS722xLCTR-20AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 66mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS722xLCTR-20AU"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS722xLCTR-20AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "20A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 132mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS722xLCTR-40AB"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS722xLCTR-40AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±40A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 33mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS722xLCTR-40AU"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS722xLCTR-40AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "40A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 66mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS722xMATR-20AB"
		(extends "ACS722xMATR-10AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS722xMATR-20AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 66mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS722xMATR-40AB"
		(extends "ACS722xMATR-10AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS722xMATR-40AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS722KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±40A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 33mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xLCTR-05AB"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS723xLCTR-05AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±5A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 400mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xLCTR-10AB"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS723xLCTR-10AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±10A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 200mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xLCTR-10AU"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS723xLCTR-10AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "10A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 400mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xLCTR-20AB"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS723xLCTR-20AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xLCTR-20AU"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS723xLCTR-20AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "20A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 200mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xLCTR-40AB"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS723xLCTR-40AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±40A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 50mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xLCTR-40AU"
		(extends "ACS722xLCTR-05AB")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS723xLCTR-40AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "40A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xMATR-10AB"
		(extends "ACS722xMATR-10AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS723xMATR-10AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±10A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 200mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xMATR-20AB"
		(extends "ACS722xMATR-10AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS723xMATR-20AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS723xMATR-40AB"
		(extends "ACS722xMATR-10AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS723xMATR-40AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS723KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±40A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 50mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xLCTR-05AB"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS724xLCTR-05AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±5A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 400mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xLCTR-10AB"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS724xLCTR-10AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±10A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 200mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xLCTR-10AU"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS724xLCTR-10AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "10A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 400mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xLCTR-20AB"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS724xLCTR-20AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xLCTR-20AU"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS724xLCTR-20AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "20A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 200mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xLCTR-30AB"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS724xLCTR-30AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±30A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 66mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xLCTR-30AU"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS724xLCTR-30AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "30A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 133mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xLCTR-50AB"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS724xLCTR-50AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xMATR-20AB"
		(extends "ACS724xMATR-12AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS724xMATR-20AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xMATR-30AB"
		(extends "ACS724xMATR-12AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS724xMATR-30AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±30A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 66mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xMATR-30AU"
		(extends "ACS724xMATR-12AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS724xMATR-30AU"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "30A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 132mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS724xMATR-65AB"
		(extends "ACS724xMATR-12AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS724xMATR-65AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS724KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±65A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 30.75mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xLCTR-10AU"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS725xLCTR-10AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "10A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 264mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xLCTR-20AB"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS725xLCTR-20AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 66mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xLCTR-20AU"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS725xLCTR-20AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "20A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 132mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xLCTR-30AB"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS725xLCTR-30AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±30A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 44mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xLCTR-30AU"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS725xLCTR-30AU"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "30A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 88mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xLCTR-40AB"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS725xLCTR-40AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±40A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 33mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xLCTR-50AB"
		(extends "ACS712xLCTR-05B")
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ACS725xLCTR-50AB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 26.4mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xMATR-20AB"
		(extends "ACS724xMATR-12AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS725xMATR-20AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 66mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xMATR-30AB"
		(extends "ACS724xMATR-12AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS725xMATR-30AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±30A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 44mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS725xMATR-30AU"
		(extends "ACS724xMATR-12AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS725xMATR-30AU"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS725KMA-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "30A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 88mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS726xLFTR-40B"
		(extends "ACS726xLFTR-20B")
		(property "Reference" "U"
			(at 8.89 16.51 0)
		)
		(property "Value" "ACS726xLFTR-40B"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_QSOP-24_3.9x8.7mm_P0.635mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS726-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±40A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 50mV/A, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS730xLCTR-40AB"
		(extends "ACS730xLCTR-20AB")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS730xLCTR-40AB"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS730-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±40A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 50mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS730xLCTR-40AU"
		(extends "ACS730xLCTR-20AB")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS730xLCTR-40AU"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS730-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "40A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 100mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS730xLCTR-50AB"
		(extends "ACS730xLCTR-20AB")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS730xLCTR-50AB"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS730-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS730xLCTR-80AU"
		(extends "ACS730xLCTR-20AB")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS730xLCTR-80AU"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS730-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "80A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 50mV/A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS73369xUAA-010B5"
		(extends "A1369xUA-10")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS73369xUAA-010B5"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_SIP-3"
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS73369-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Programmable Linear Hall Effect Sensor, +9 to +13.5mV/G, SIP-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*SIP*"
			(at 0 0 0)
		)
	)
	(symbol "ACS733xLATR-20AB"
		(extends "ACS732xLATR-40AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS733xLATR-20AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS732-ACS733-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±20A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 66mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS733xLATR-40AB"
		(extends "ACS732xLATR-40AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS733xLATR-40AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS732-ACS733-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±40A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 33mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS733xLATR-40AU"
		(extends "ACS732xLATR-40AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS733xLATR-40AU"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS732-ACS733-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "40A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 66mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS733xLATR-65AB"
		(extends "ACS732xLATR-40AB")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "ACS733xLATR-65AB"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS732-ACS733-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±65A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 20mV/A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS756xCB-100B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS756xCB-100B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS756-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±100A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 20mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-050B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-050B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-050U-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-050U-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "50A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 60mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-100B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-100B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±100A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 20mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-100U-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-100U-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "100A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-150B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-150B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±150A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 13.3mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-150U-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-150U-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "150A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 26.7mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-150U-PSF"
		(extends "ACS758xCB-100B-PSF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-150U-PSF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "150A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 26.7mV/A, CB-5 PSF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-200B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-200B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±200A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 10mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-200B-PSF"
		(extends "ACS758xCB-100B-PSF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-200B-PSF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±200A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 10mV/A, CB-5 PSF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-200B-PSS"
		(extends "ACS758xCB-150B-PSS")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-200B-PSS"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSS"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±200A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 10mV/A, CB-5 PSS"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSS*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-200U-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-200U-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "200A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 20mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS758xCB-200U-PSF"
		(extends "ACS758xCB-100B-PSF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS758xCB-200U-PSF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "200A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 20mV/A, CB-5 PSF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS759xCB-050B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS759xCB-050B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS759-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 26.4mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS759xCB-100B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS759xCB-100B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS759-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±100A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 13.2mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS759xCB-150B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS759xCB-150B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS759-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±150A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 8.8mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS759xCB-150B-PSS"
		(extends "ACS758xCB-150B-PSS")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS759xCB-150B-PSS"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSS"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS759-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±150A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 8.8mV/A, CB-5 PSS"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSS*"
			(at 0 0 0)
		)
	)
	(symbol "ACS759xCB-200B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS759xCB-200B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS759-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±200A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 6.6mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS759xCB-200B-PSS"
		(extends "ACS758xCB-150B-PSS")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS759xCB-200B-PSS"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSS"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS759-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±200A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 6.6mV/A, CB-5 PSS"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSS*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-050B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-050B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-050U-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-050U-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "50A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 80mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-100B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-100B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±100A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 20mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-100U-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-100U-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "100A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-100U-PSF"
		(extends "ACS758xCB-100B-PSF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-100U-PSF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "100A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, CB-5 PSF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-150B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-150B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 13.3mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-150B-PSF"
		(extends "ACS758xCB-100B-PSF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-150B-PSF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 13.3mV/A, CB-5 PSF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-150U-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-150U-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "50A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 26.7mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-150U-PSF"
		(extends "ACS758xCB-100B-PSF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-150U-PSF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "50A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 26.7mV/A, CB-5 PSF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-200B-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-200B-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 10mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-200B-PSF"
		(extends "ACS758xCB-100B-PSF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-200B-PSF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 10mV/A, CB-5 PSF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-200U-PFF"
		(extends "ACS756xCB-050B-PFF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-200U-PFF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PFF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "50A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 20mV/A, CB-5 PFF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PFF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS770xCB-200U-PSF"
		(extends "ACS758xCB-100B-PSF")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS770xCB-200U-PSF"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_CB_PSF"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS758-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "50A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 20mV/A, CB-5 PSF"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*CB*PSF*"
			(at 0 0 0)
		)
	)
	(symbol "ACS780xLRTR-050U"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS780xLRTR-050U"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS780-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "50A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 60mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS780xLRTR-100B"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS780xLRTR-100B"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS780-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±100A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 20mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS780xLRTR-100U"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS780xLRTR-100U"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS780-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "100A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 40mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS780xLRTR-150B"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS780xLRTR-150B"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS780-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±150A Bidirectional Hall-Effect Current Sensor, +5.0V supply, 13.33mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS780xLRTR-150U"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS780xLRTR-150U"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS780-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "150A Unidirectional Hall-Effect Current Sensor, +5.0V supply, 26.66mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS781xLRTR-050B"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS781xLRTR-050B"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS780-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±50A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 26.4mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS781xLRTR-050U"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS781xLRTR-050U"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS780-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "50A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 39.6mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS781xLRTR-100B"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS781xLRTR-100B"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS780-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±100A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 13.2mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS781xLRTR-100U"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS781xLRTR-100U"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS781-Datasheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "100A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 26.4mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS781xLRTR-150B"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS781xLRTR-150B"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS781-Datsaheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "±150A Bidirectional Hall-Effect Current Sensor, +3.3V supply, 8.8mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACS781xLRTR-150U"
		(extends "ACS780xLRTR-050B")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ACS781xLRTR-150U"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Allegro_PSOF-7_4.8x6.4mm_P1.60mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/ACS781-Datsaheet.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "150A Unidirectional Hall-Effect Current Sensor, +3.3V supply, 17.6mV/A, PSOF-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current monitor sensor isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Allegro*PSOF*4.8x6.4mm*P1.60mm*"
			(at 0 0 0)
		)
	)
	(symbol "CKSR_25-NP"
		(extends "CKSR_15-NP")
		(property "Reference" "U"
			(at 10.16 8.89 0)
		)
		(property "Value" "CKSR_25-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_CKSR"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/cksr_xx-np_v14.pdf"
			(at 3.81 0 0)
		)
		(property "Description" "Current Transducer, 25A, Unipolar, 0-5V Output, 4 Primary Windings"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*CKSR*"
			(at 0 0 0)
		)
	)
	(symbol "CKSR_50-NP"
		(extends "CKSR_15-NP")
		(property "Reference" "U"
			(at 10.16 8.89 0)
		)
		(property "Value" "CKSR_50-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_CKSR"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/cksr_xx-np_v14.pdf"
			(at 3.81 0 0)
		)
		(property "Description" "Current Transducer, 50A, Unipolar, 0-5V Output, 4 Primary Windings"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*CKSR*"
			(at 0 0 0)
		)
	)
	(symbol "CKSR_6-NP"
		(extends "CKSR_15-NP")
		(property "Reference" "U"
			(at 10.16 8.89 0)
		)
		(property "Value" "CKSR_6-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_CKSR"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/cksr_xx-np_v14.pdf"
			(at 3.81 0 0)
		)
		(property "Description" "Current Transducer, 6A, Unipolar, 0-5V Output, 4 Primary Windings"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*CKSR*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2064"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2064"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2064.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Bidirectional, -54A to +54A, 40mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2065"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2065"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2065.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Bidirectional, -85A to +85A, 25mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-206A"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-206A"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-206A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Bidirectional, -46A to +46A, 45mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-206B"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-206B"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-206B.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Unidirectional, 0A to +45A, 90mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2093"
		(extends "CQ-2092")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2093"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7S"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2093.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Bidirectional, -35A to +35A, 60mV/A, CQ-7S"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*S*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-209A"
		(extends "CQ-2092")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-209A"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7S"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-209A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Bidirectional, -31.8A to +31.8A, 66mV/A, CQ-7S"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*S*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-209B"
		(extends "CQ-2092")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-209B"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7S"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-209B.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Unidirectional, -35A to 0A, 115mV/A, CQ-7S"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*S*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-209D"
		(extends "CQ-2092")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-209D"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7S"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-209D.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Bidirectional, -41A to +41A, 50mV/A, CQ-7S"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*S*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2232"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2232"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2232.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small Current Sensor, Bidirectional, -21A to +21A, 62.5mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2233"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2233"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2233.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small Current Sensor, Bidirectional, -35A to +35A, 37.5mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2234"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2234"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2234.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small Current Sensor, Bidirectional, -54A to +54A, 24.5mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2235"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2235"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2235.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small Current Sensor, Bidirectional, -85A to +85A, 15.5mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2332"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2332"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2332.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small Current Sensor, Bidirectional, -21A to +21A, 100mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2333"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2333"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2333.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small Current Sensor, Bidirectional, -35A to +35A, 60mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2334"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2334"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2334.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small Current Sensor, Bidirectional, -54A to +54A, 40mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2335"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2335"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2335.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small Current Sensor, Bidirectional, -85A to +85A, 25mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-2336"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-2336"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-2335.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small Current Sensor, Bidirectional, -170A to +170A, 12mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-236B"
		(extends "CQ-2063")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-236B"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_7"
			(at 12.7 10.16 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-236B.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Small-Sized Current Sensor, Unidirectional, 0A to +25A, 160mV/A, CQ-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-3201"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-3201"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-3201.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -10.1A to +10.1A, 130mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-3202"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-3202"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-3202.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -21.1A to +21.1A, 62.5mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-3203"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-3203"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-3203.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -35.7A to +35.7A, 37mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-3204"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-3204"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-3204.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -44.0A to +44.0A, 30mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-320A"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-320A"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-320A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -29.3A to +29.3A, 45mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-320B"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-320B"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-320B.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Unidirectional, -1.1A to +20.9A, 120mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-3300"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-3300"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-3300.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -6.4A to +6.4A, 325mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-3301"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-3301"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-3301.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -10.7A to +10.7A, 195mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-3302"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-3302"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-3302.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -21.0A to +21.0A, 100mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-3303"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-3303"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-3303.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -35.0A to +35.0A, 60mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-330A"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-330A"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-330A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -31.8A to +31.8A, 66mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-330B"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-330B"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-330B.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Unidirectional, 0A to +21.0A, 195mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-330E"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-330E"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-330E.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Unidirectional, 0A to +20.5A, 200mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-330F"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-330F"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-330F.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Unidirectional, -2.0A to +42.0A, 80mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-330G"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-330G"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-330G.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -4.5A to +4.5A, 450mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-330H"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-330H"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-330H.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Bidirectional, -42.0A to +42.0A, 50mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CQ-330J"
		(extends "CQ-3200")
		(property "Reference" "U"
			(at 8.89 6.35 0)
		)
		(property "Value" "CQ-330J"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CQ_VSOP-24_5.6x7.9mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CQ-330J.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Response Coreless Current Sensor, Unidirectional, -2.0A to +42.0A, 82.7mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CQ*VSOP*5.6x7.9mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CSLW6B200M"
		(extends "CSLW6B1")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "CSLW6B200M"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Honeywell_CSLW"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://sensing.honeywell.com/honeywell-sensing-cslw-series-product-sheet-005861-1-en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Wired Open-Loop Current Sensors, 200mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Honeywell*CSLW*"
			(at 0 0 0)
		)
	)
	(symbol "CSLW6B40M"
		(extends "CSLW6B1")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "CSLW6B40M"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Honeywell_CSLW"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://sensing.honeywell.com/honeywell-sensing-cslw-series-product-sheet-005861-1-en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Wired Open-Loop Current Sensors, 40mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Honeywell*CSLW*"
			(at 0 0 0)
		)
	)
	(symbol "CSLW6B5"
		(extends "CSLW6B1")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "CSLW6B5"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Sensor_Current:Honeywell_CSLW"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://sensing.honeywell.com/honeywell-sensing-cslw-series-product-sheet-005861-1-en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Wired Open-Loop Current Sensors, 5A"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Honeywell*CSLW*"
			(at 0 0 0)
		)
	)
	(symbol "CZ-3814"
		(extends "CZ-3813")
		(property "Reference" "U"
			(at 1.27 11.43 0)
		)
		(property "Value" "CZ-3814"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CZ_SSOP-10_6.5x8.1mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CZ-3814.pdf"
			(at 0 0 0)
		)
		(property "Description" "Coreless Current Sensor, Bidirectional, -50.0A to +50.0A, 40mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CZ*SSOP*6.5x8.1mm*P0.95mm*"
			(at 0 0 0)
		)
	)
	(symbol "CZ-3815"
		(extends "CZ-3813")
		(property "Reference" "U"
			(at 1.27 11.43 0)
		)
		(property "Value" "CZ-3815"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Sensor_Current:AKM_CZ_SSOP-10_6.5x8.1mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.akm.com/akm/en/file/datasheet/CZ-3815.pdf"
			(at 0 0 0)
		)
		(property "Description" "Coreless Current Sensor, Bidirectional, -60.0A to +60.0A, 33mV/A, VSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall effect current sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AKM*CZ*SSOP*6.5x8.1mm*P0.95mm*"
			(at 0 0 0)
		)
	)
	(symbol "HO120-NP"
		(extends "HO40-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO120-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO40-NP"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 120A, Unipolar, 5V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO40*NP*"
			(at 0 0 0)
		)
	)
	(symbol "HO128-NP"
		(extends "HO40-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO128-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO40-NP"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 128A, Unipolar, 5V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO40*NP*"
			(at 0 0 0)
		)
	)
	(symbol "HO15-NP"
		(extends "HO8-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO15-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO8-NP"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np-0000_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 15A, Unipolar, 5V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO8*NP*"
			(at 0 0 0)
		)
	)
	(symbol "HO15-NSM"
		(extends "HO8-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO15-NSM"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO8-NSM"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-nsm-0000_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 15A, Unipolar, 5V, SMT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO8*NSM*"
			(at 0 0 0)
		)
	)
	(symbol "HO150-NP"
		(extends "HO40-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO150-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO40-NP"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 150A, Unipolar, 5V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO40*NP*"
			(at 0 0 0)
		)
	)
	(symbol "HO25-NP"
		(extends "HO8-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO25-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO8-NP"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np-0000_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 25A, Unipolar, 5V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO8*NP*"
			(at 0 0 0)
		)
	)
	(symbol "HO25-NSM"
		(extends "HO8-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO25-NSM"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO8-NSM"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-nsm-0000_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 25A, Unipolar, 5V, SMT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO8*NSM*"
			(at 0 0 0)
		)
	)
	(symbol "HO60-NP"
		(extends "HO40-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO60-NP"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO40-NP"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 60A, Unipolar, 5V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO40*NP*"
			(at 0 0 0)
		)
	)
	(symbol "HO8-NPxSP33"
		(extends "HO8-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO8-NPxSP33"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO8-NP"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np_sp33-1000_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 8A, Unipolar, 3.3V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO8*NP*"
			(at 0 0 0)
		)
	)
	(symbol "HO8-NSM"
		(extends "HO8-NP")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO8-NSM"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO8-NSM"
			(at 20.32 35.56 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-nsm-0000_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 8A, Unipolar, 5V, SMT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO8*NSM*"
			(at 0 0 0)
		)
	)
	(symbol "HTFS400-P"
		(extends "HTFS200-P")
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "HTFS400-P"
			(at 0 10.16 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HTFS"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/htfs_200_800-p.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 400A, Unipolar, 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HTFS*"
			(at 0 0 0)
		)
	)
	(symbol "HTFS600-P"
		(extends "HTFS200-P")
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "HTFS600-P"
			(at 0 10.16 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HTFS"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/htfs_200_800-p.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 600A, Unipolar, 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HTFS*"
			(at 0 0 0)
		)
	)
	(symbol "HTFS800-P"
		(extends "HTFS200-P")
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "HTFS800-P"
			(at 0 10.16 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HTFS"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/htfs_200_800-p.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 800A, Unipolar, 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HTFS*"
			(at 0 0 0)
		)
	)
	(symbol "IR22771S"
		(extends "IR21771S")
		(property "Reference" "U"
			(at 1.27 15.875 0)
		)
		(property "Value" "IR22771S"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir21771s.pdf?fileId=5546d462533600a4015355c9222c16c8"
			(at 0 0 0)
		)
		(property "Description" "Phase Current Sensor IC for AC Motor Control, PWM output, 1200V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge current sense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2277S"
		(extends "IR2177S")
		(property "Reference" "U"
			(at 1.27 15.875 0)
		)
		(property "Value" "IR2277S"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2177s.pdf?fileId=5546d462533600a4015355c92e7416cb"
			(at 0 0 0)
		)
		(property "Description" "Phase Current Sensor IC for AC Motor Control, PWM and ADC output, 1200V, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge current sense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LA100-P"
		(extends "LA25-P")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LA100-P"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Sensor_Current:LEM_LA25-P"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/la_100-p_e_.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 100A, Bipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*LA25*P*"
			(at 0 0 0)
		)
	)
	(symbol "LA55-P"
		(extends "LA25-P")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LA55-P"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Sensor_Current:LEM_LA25-P"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/la_55-p_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Current Transducer, 50A, Bipolar, ±15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*LA25*P*"
			(at 0 0 0)
		)
	)
	(symbol "LTSR15-NP"
		(extends "LTSR6-NP")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LTSR15-NP"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Sensor_Current:LEM_LTSR-NP"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ltsr_15-np.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Current Transducer, Unipolar, 15A, 5V supply, DC, AC, pulsed"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*LTSR*NP*"
			(at 0 0 0)
		)
	)
	(symbol "LTSR25-NP"
		(extends "LTSR6-NP")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LTSR25-NP"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Sensor_Current:LEM_LTSR-NP"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ltsr_25-np.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Current Transducer, Unipolar, 25A, 5V supply, DC, AC, pulsed"
			(at 0 0 0)
		)
		(property "ki_keywords" "current transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*LTSR*NP*"
			(at 0 0 0)
		)
	)
	(symbol "MCA1101-20-3"
		(extends "MCA1101-65-5")
		(property "Reference" "U"
			(at -6.858 11.43 0)
		)
		(property "Value" "MCA1101-20-3"
			(at 8.382 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -0.254 -27.432 0)
		)
		(property "Datasheet" "https://navview.blob.core.windows.net/web-resources/6020-1104-01_C%20Datasheet%2C%20Current%20Sensor%20Fix%20Gain%203.3V_20210408.pdf"
			(at 0.254 -23.114 0)
		)
		(property "Description" "High Accuracy Current Sensor IC with 1.5MHz 3dB Bandwidth and Isolation, ±20A, 3.3V Supply, Fixed Gain, 60 mV/A, SOIC-16W"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "amr-sensor isolated-current-sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCA1101-20-5"
		(extends "MCA1101-65-5")
		(property "Reference" "U"
			(at -6.858 11.43 0)
		)
		(property "Value" "MCA1101-20-5"
			(at 8.382 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -0.254 -27.432 0)
		)
		(property "Datasheet" "https://navview.blob.core.windows.net/web-resources/6020-1102-01%20RevG_MCA1101_Fix%20Gain%205V_10112021.pdf"
			(at 0.254 -23.114 0)
		)
		(property "Description" "High Accuracy Current Sensor IC with 1.5MHz 3dB Bandwidth and Isolation, ±20A, 5V Supply, Fixed Gain, 90 mV/A, SOIC-16W"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "amr-sensor isolated-current-sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCA1101-5-3"
		(extends "MCA1101-65-5")
		(property "Reference" "U"
			(at -6.858 11.43 0)
		)
		(property "Value" "MCA1101-5-3"
			(at 8.382 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -0.254 -27.432 0)
		)
		(property "Datasheet" "https://navview.blob.core.windows.net/web-resources/6020-1104-01_C%20Datasheet%2C%20Current%20Sensor%20Fix%20Gain%203.3V_20210408.pdf"
			(at 0.254 -23.114 0)
		)
		(property "Description" "High Accuracy Current Sensor IC with 1.5MHz 3dB Bandwidth and Isolation, ±5A, 3.3V Supply, Fixed Gain, 230 mV/A, SOIC-16W"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "amr-sensor isolated-current-sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCA1101-5-5"
		(extends "MCA1101-65-5")
		(property "Reference" "U"
			(at -6.858 11.43 0)
		)
		(property "Value" "MCA1101-5-5"
			(at 8.382 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -0.254 -27.432 0)
		)
		(property "Datasheet" "https://navview.blob.core.windows.net/web-resources/6020-1102-01%20RevG_MCA1101_Fix%20Gain%205V_10112021.pdf"
			(at 0.254 -23.114 0)
		)
		(property "Description" "High Accuracy Current Sensor IC with 1.5MHz 3dB Bandwidth and Isolation, ±5A, 5V Supply, Fixed Gain, 350 mV/A, SOIC-16W"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "amr-sensor isolated-current-sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCA1101-50-3"
		(extends "MCA1101-65-5")
		(property "Reference" "U"
			(at -6.858 11.43 0)
		)
		(property "Value" "MCA1101-50-3"
			(at 8.382 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -0.254 -27.432 0)
		)
		(property "Datasheet" "https://navview.blob.core.windows.net/web-resources/6020-1104-01_C%20Datasheet%2C%20Current%20Sensor%20Fix%20Gain%203.3V_20210408.pdf"
			(at 0.254 -23.114 0)
		)
		(property "Description" "High Accuracy Current Sensor IC with 1.5MHz 3dB Bandwidth and Isolation, ±50A, 3.3V Supply, Fixed Gain, 25 mV/A, SOIC-16W"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "amr-sensor isolated-current-sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCA1101-50-5"
		(extends "MCA1101-65-5")
		(property "Reference" "U"
			(at -6.858 11.43 0)
		)
		(property "Value" "MCA1101-50-5"
			(at 8.382 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -0.254 -27.432 0)
		)
		(property "Datasheet" "https://navview.blob.core.windows.net/web-resources/6020-1102-01%20RevG_MCA1101_Fix%20Gain%205V_10112021.pdf"
			(at 0.254 -23.114 0)
		)
		(property "Description" "High Accuracy Current Sensor IC with 1.5MHz 3dB Bandwidth and Isolation, ±50A, 5V Supply, Fixed Gain, 35 mV/A, SOIC-16W"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "amr-sensor isolated-current-sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HO15-NPxSP33"
		(extends "HO8-NPxSP33")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO15-NPxSP33"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO8-NP"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np_sp33-1000_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 15A, Unipolar, 3.3V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO8*NP*"
			(at 0 0 0)
		)
	)
	(symbol "HO25-NPxSP33"
		(extends "HO8-NPxSP33")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "HO25-NPxSP33"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Sensor_Current:LEM_HO8-NP"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/ho-np_sp33-1000_series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hall Effect Current Transducer, 25A, Unipolar, 3.3V, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Lem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM*HO8*NP*"
			(at 0 0 0)
		)
	)
)
