(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "TMF8820"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TMF8820"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Sensor_Distance:AMS_OLGA12"
			(at 17.145 -13.97 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/6015057/TMF882X_DS000693_8-00.pdf"
			(at 0 -27.94 0)
		)
		(property "Description" "5m distance ranging ToF sensor, 3x3 zones, LGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "TMF882x ToF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS*OLGA12*"
			(at 0 0 0)
		)
		(symbol "TMF8820_0_1")
		(symbol "TMF8820_1_1"
			(pin tri_state line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "GPIO0")
				(number "3")
			)
			(pin tri_state line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "GPIO1")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INT")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "EN")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VL53L1CXV0FY1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "VL53L1CXV0FY1"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Sensor_Distance:ST_VL53L1x"
			(at 17.145 -13.97 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/vl53l1x.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "4m distance ranging ToF sensor, Optical LGA12"
			(at 0 0 0)
		)
		(property "ki_keywords" "VL53L1x ToF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*VL53L1x*"
			(at 0 0 0)
		)
		(symbol "VL53L1CXV0FY1_0_1")
		(symbol "VL53L1CXV0FY1_1_1"
			(pin open_collector line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "GPIO1")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "XSHUT")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "AVDD")
				(number "11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "AVDDVCSEL")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "AVSSVCSEL")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMF8821"
		(extends "TMF8820")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TMF8821"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Sensor_Distance:AMS_OLGA12"
			(at 17.145 -13.97 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/6015057/TMF882X_DS000693_8-00.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "5m distance ranging ToF sensor, 3x3, 4x4, 3x6 zones, LGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "TMF882x ToF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS*OLGA12*"
			(at 0 0 0)
		)
	)
	(symbol "TMF8828"
		(extends "TMF8820")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TMF8828"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Sensor_Distance:AMS_OLGA12"
			(at 17.145 -13.97 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/6015057/TMF882X_DS000693_8-00.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "5m distance ranging ToF sensor, 3x3, 4x4, 3x6, 8x8 zones, LGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "TMF882x ToF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS*OLGA12*"
			(at 0 0 0)
		)
	)
	(symbol "VL53L0CXV0DH1"
		(extends "VL53L1CXV0FY1")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "VL53L0CXV0DH1"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Sensor_Distance:ST_VL53L1x"
			(at 17.145 -13.97 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/vl53l0x.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "2m distance ranging ToF sensor, Optical LGA12"
			(at 0 0 0)
		)
		(property "ki_keywords" "VL53L0x ToF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*VL53L1x*"
			(at 0 0 0)
		)
	)
)
