(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ATM90E26-YU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.2598 0)
		)
		(property "Value" "ATM90E26-YU"
			(at -17.78 -22.86 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 27.94 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/Atmel-46002-SE-M90E26-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "High precision energy metering device for single-phase two-wire and single-phase three-wire, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "energy metering sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*28*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATM90E26-YU_1_0"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "MMD0")
				(number "28")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "MMD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{Reset}")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "I2P")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "I2N")
				(number "8")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "I1P")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "I1N")
				(number "11")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "USEL")
				(number "12")
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "Vref")
				(number "13")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "5")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "DVDD")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "9")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SDI/URX")
				(number "27")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SDO/UTX")
				(number "26")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SCLK")
				(number "25")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "~{CS}")
				(number "24")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OSCO")
				(number "23")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OSCI")
				(number "22")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "ZX")
				(number "21")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IRQ")
				(number "20")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "CF2")
				(number "19")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CF1")
				(number "18")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "WarnOut")
				(number "17")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "VP")
				(number "16")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "VN")
				(number "15")
			)
		)
		(symbol "ATM90E26-YU_1_1")
		(embedded_fonts no)
	)
	(symbol "INA219AxD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "INA219AxD"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina219.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "Zero-Drift, Bidirectional Current/Power Monitor (0-26V) With I2C Interface, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 16-Bit Oversampling Current Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "INA219AxD_0_1")
		(symbol "INA219AxD_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VS")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "A0")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA219AxDCN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "INA219AxDCN"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina219.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "Zero-Drift, Bidirectional Current/Power Monitor (0-26V) With I2C Interface, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 16-Bit Oversampling Current Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "INA219AxDCN_0_1")
		(symbol "INA219AxDCN_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VS")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "A1")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "A0")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INA226"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "INA226"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 20.32 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina226.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "High-Side or Low-Side Measurement, Bi-Directional Current and Power Monitor (0-36V) with I2C Compatible Interface, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 16-Bit Oversampling Current Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "INA226_0_1")
		(symbol "INA226_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "Vbus")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Vin+")
				(number "10")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vin-")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{Alert}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4151xMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "LTC4151xMS"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 20.32 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4151ff.pdf"
			(at 7.62 12.7 0)
		)
		(property "Description" "High Voltage I2C Current and Voltage Monitor, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Current Monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4151xMS_0_1")
		(symbol "LTC4151xMS_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SENSE+")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SENSE-")
				(number "10")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ADIN")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{SHDN}")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ADR1")
				(number "3")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "ADR0")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP39F521"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 19.05 0)
		)
		(property "Value" "MCP39F521"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005442A.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Power Monitor, Calculation and Energy Accumulation, I2C, 16-bit, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "i2c power monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP39F521_0_1")
		(symbol "MCP39F521_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "I1+")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "I1-")
				(number "17")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "V1+")
				(number "19")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "V1-")
				(number "18")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "COMMON_A")
				(number "5")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "COMMON_B")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "AN_IN")
				(number "20")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "OSCI")
				(number "6")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "OSCO")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "AVDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "24")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "27")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "29")
			)
			(pin no_connect line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "~{MCLR}")
				(number "26")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "A1")
				(number "15")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "EVENT")
				(number "1")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "ZCD")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "REFIN+/OUT")
				(number "23")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{DR}")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAC1931x-xJ6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 22.86 0)
		)
		(property "Value" "PAC1931x-xJ6CX"
			(at 17.78 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC1931-Family-Data-Sheet-DS20005850E.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "One Channel High-side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1931x-xJ6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin input line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "V_{DD}IO")
				(number "B2")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1931x-xJ6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1932x-xJ6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 22.86 0)
		)
		(property "Value" "PAC1932x-xJ6CX"
			(at 17.78 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC1931-Family-Data-Sheet-DS20005850E.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel High-side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1932x-xJ6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "A1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "B1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin input line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "V_{DD}IO")
				(number "B2")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1932x-xJ6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1932x-xJQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 22.86 0)
		)
		(property "Value" "PAC1932x-xJQ"
			(at 17.78 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-16-1EP_4x4mm_P0.65mm_EP2.6x2.6mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC1931-Family-Data-Sheet-DS20005850E.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel High-side Power Monitor, 32V, I2C, UQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.65mm*EP2.6x2.6mm*"
			(at 0 0 0)
		)
		(symbol "PAC1932x-xJQ_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin input line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "V_{DD}IO")
				(number "15")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "5")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "1")
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "6")
			)
		)
		(symbol "PAC1932x-xJQ_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1933x-xJ6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 22.86 0)
		)
		(property "Value" "PAC1933x-xJ6CX"
			(at 17.78 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC1931-Family-Data-Sheet-DS20005850E.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Three Channel High-side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1933x-xJ6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "A1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "B1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SENSE3+")
				(number "D1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SENSE3-")
				(number "C1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin input line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "V_{DD}IO")
				(number "B2")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1933x-xJ6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1933x-xJQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 22.86 0)
		)
		(property "Value" "PAC1933x-xJQ"
			(at 17.78 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-16-1EP_4x4mm_P0.65mm_EP2.6x2.6mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC1931-Family-Data-Sheet-DS20005850E.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Three Channel High-side Power Monitor, 32V, I2C, UQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.65mm*EP2.6x2.6mm*"
			(at 0 0 0)
		)
		(symbol "PAC1933x-xJQ_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SENSE3+")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SENSE3-")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin input line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "V_{DD}IO")
				(number "15")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "5")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "1")
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "6")
			)
		)
		(symbol "PAC1933x-xJQ_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1934x-xJ6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 22.86 0)
		)
		(property "Value" "PAC1934x-xJ6CX"
			(at 17.78 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC1931-Family-Data-Sheet-DS20005850E.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Four Channel High-side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1934x-xJ6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "A1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "B1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SENSE3+")
				(number "D1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SENSE3-")
				(number "C1")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SENSE4+")
				(number "D3")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SENSE4-")
				(number "D2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin input line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "V_{DD}IO")
				(number "B2")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1934x-xJ6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1934x-xJQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 22.86 0)
		)
		(property "Value" "PAC1934x-xJQ"
			(at 17.78 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-16-1EP_4x4mm_P0.65mm_EP2.6x2.6mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC1931-Family-Data-Sheet-DS20005850E.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Four Channel High-side Power Monitor, 32V, I2C, UQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.65mm*EP2.6x2.6mm*"
			(at 0 0 0)
		)
		(symbol "PAC1934x-xJQ_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SENSE3+")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SENSE3-")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SENSE4+")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SENSE4-")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin input line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "V_{DD}IO")
				(number "15")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "5")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "1")
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "6")
			)
		)
		(symbol "PAC1934x-xJQ_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1951x-1x-4MX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 22.86 0)
		)
		(property "Value" "PAC1951x-1x-4MX"
			(at 10.16 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "One Channel High-side Power Monitor, 32V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
		(symbol "PAC1951x-1x-4MX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "5")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "1")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "15")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "6")
			)
		)
		(symbol "PAC1951x-1x-4MX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1951x-1x-J6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 22.86 0)
		)
		(property "Value" "PAC1951x-1x-J6CX"
			(at 10.16 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "One Channel High-side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1951x-1x-J6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "B2")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1951x-1x-J6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1951x-2x-4MX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1951x-2x-4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "One Channel Low-side Power Monitor, 32V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
		(symbol "PAC1951x-2x-4MX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "V_{BUS1+}")
				(number "13")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1+")
				(number "11")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SENSE1-")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{BUS1-}")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "5")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "1")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "15")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "6")
			)
		)
		(symbol "PAC1951x-2x-4MX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1951x-2x-J6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1951x-2x-J6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "One Channel Low-side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1951x-2x-J6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "V_{BUS1+}")
				(number "A1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{BUS1-}")
				(number "B1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "B2")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1951x-2x-J6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1952x-1x-4MX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1952x-1x-4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel High-side Power Monitor, 32V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
		(symbol "PAC1952x-1x-4MX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "5")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "1")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "15")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "6")
			)
		)
		(symbol "PAC1952x-1x-4MX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1952x-1x-J6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1952x-1x-J6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel High-side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1952x-1x-J6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "A1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "B1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "B2")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1952x-1x-J6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1952x-2x-4MX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1952x-2x-4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel Low-side Power Monitor, 32V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
		(symbol "PAC1952x-2x-4MX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "V_{BUS1+}")
				(number "13")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1+")
				(number "11")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SENSE1-")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{BUS1-}")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "V_{BUS2+}")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SENSE2+")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SENSE2-")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "V_{BUS2-}")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "5")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "1")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "15")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "6")
			)
		)
		(symbol "PAC1952x-2x-4MX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1952x-2x-J6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1952x-2x-J6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel Low-side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1952x-2x-J6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "V_{BUS1+}")
				(number "A1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{BUS1-}")
				(number "B1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "V_{BUS2+}")
				(number "D1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SENSE2+")
				(number "D3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SENSE2-")
				(number "D2")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "V_{BUS2-}")
				(number "C1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "B2")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1952x-2x-J6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1953x-x4MX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1953x-x4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Three Channel High-Side Power Monitor, 32V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
		(symbol "PAC1953x-x4MX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SENSE3+")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SENSE3-")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "5")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "1")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "15")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "6")
			)
		)
		(symbol "PAC1953x-x4MX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1953x-xJ6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1953x-xJ6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Three Channel High-Side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1953x-xJ6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "A1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "B1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SENSE3+")
				(number "D1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SENSE3-")
				(number "C1")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "B2")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1953x-xJ6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1954x-x4MX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1954x-x4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Four Channel High-side Power Monitor, 32V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
		(symbol "PAC1954x-x4MX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SENSE3+")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SENSE3-")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SENSE4+")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SENSE4-")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "5")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "1")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "15")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "6")
			)
		)
		(symbol "PAC1954x-x4MX_0_1")
		(embedded_fonts no)
	)
	(symbol "PAC1954x-xJ6CX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1954x-xJ6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC195X-Data-Sheet-20006539.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Four Channel High-side Power Monitor, 32V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PAC1954x-xJ6CX_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SENSE1+")
				(number "A3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1-")
				(number "A2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SENSE2+")
				(number "A1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE2-")
				(number "B1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SENSE3+")
				(number "D1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SENSE3-")
				(number "C1")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SENSE4+")
				(number "D3")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SENSE4-")
				(number "D2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "C4")
				(alternate "SM_CLK" input line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "D4")
				(alternate "SM_DATA" bidirectional line)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{PWRDN}")
				(number "B3")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SLOW")
				(number "C3")
				(alternate "GPIO" bidirectional line)
				(alternate "~{ALERT1}" open_collector line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO")
				(number "B2")
				(alternate "~{ALERT2}" open_collector line)
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ADDRSEL")
				(number "C2")
			)
		)
		(symbol "PAC1954x-xJ6CX_0_1")
		(embedded_fonts no)
	)
	(symbol "INA219BxD"
		(extends "INA219AxD")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "INA219BxD"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina219.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "Zero-Drift, HighAccuracy, Bidirectional Current/Power Monitor (0-26V) With I2C Interface, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 16-Bit Oversampling Current Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA219BxDCN"
		(extends "INA219AxDCN")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "INA219BxDCN"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 16.51 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina219.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "Zero-Drift, HighAccuracy, Bidirectional Current/Power Monitor (0-26V) With I2C Interface, SOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 16-Bit Oversampling Current Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "INA228"
		(extends "INA226")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "INA228"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 20.32 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina228.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "High-Side or Low-Side Measurement, Bi-Directional Current and Power Monitor (0-85V) with I2C, SMBus-, and PMBus-Compatible Interface, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 20-Bit Oversampling Current Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA233"
		(extends "INA226")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "INA233"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 20.32 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina233.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "High-Side or Low-Side Measurement, Bi-Directional Current and Power Monitor (0-36V) with I2C, SMBus-, and PMBus-Compatible Interface, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 16-Bit Oversampling Current Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA237"
		(extends "INA226")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "INA237"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 20.32 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina237.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "High-Side or Low-Side Measurement, Bi-Directional Current and Power Monitor (0-85V) with I2C, SMBus-, and PMBus-Compatible Interface, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 16-Bit Oversampling Current Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "INA238"
		(extends "INA226")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "INA238"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 20.32 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina238.pdf"
			(at 8.89 -2.54 0)
		)
		(property "Description" "High-Side or Low-Side Measurement, Bi-Directional Current and Power Monitor (0-85V) with I2C, SMBus-, and PMBus-Compatible Interface, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "ADC I2C 16-Bit Oversampling Current Shunt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1941x-1x-4MX"
		(extends "PAC1951x-1x-4MX")
		(property "Reference" "U"
			(at 10.16 22.86 0)
		)
		(property "Value" "PAC1941x-1x-4MX"
			(at 10.16 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "One Channel High-side Power Monitor, 9V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1941x-1x-J6CX"
		(extends "PAC1951x-1x-J6CX")
		(property "Reference" "U"
			(at 10.16 22.86 0)
		)
		(property "Value" "PAC1941x-1x-J6CX"
			(at 10.16 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "One Channel High-side Power Monitor, 9V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1941x-2x-4MX"
		(extends "PAC1951x-2x-4MX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1941x-2x-4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "One Channel Low-side Power Monitor, 9V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1941x-2x-J6CX"
		(extends "PAC1951x-2x-J6CX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1941x-2x-J6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "One Channel Low-side Power Monitor, 9V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1942x-1x-4MX"
		(extends "PAC1952x-1x-4MX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1942x-1x-4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel High-side Power Monitor, 9V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1942x-1x-J6CX"
		(extends "PAC1952x-1x-J6CX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1942x-1x-J6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel High-side Power Monitor, 9V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1942x-2x-4MX"
		(extends "PAC1952x-2x-4MX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1942x-2x-4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel Low-side Power Monitor, 9V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1942x-2x-J6CX"
		(extends "PAC1952x-2x-J6CX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1942x-2x-J6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Two Channel Low-side Power Monitor, 9V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1943x-x4MX"
		(extends "PAC1953x-x4MX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1943x-x4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Three Channel High-Side Power Monitor, 9V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1943x-xJ6CX"
		(extends "PAC1953x-xJ6CX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1943x-xJ6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Three Channel High-Side Power Monitor, 9V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1944x-x4MX"
		(extends "PAC1954x-x4MX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1944x-x4MX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.1x1.1mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Four Channel High-side Power Monitor, 9V, I2C, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*EP1.1x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "PAC1944x-xJ6CX"
		(extends "PAC1954x-xJ6CX")
		(property "Reference" "U"
			(at 7.62 22.86 0)
		)
		(property "Value" "PAC1944x-xJ6CX"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_2.225x2.17mm_Layout4x4_P0.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PAC194X-Data-Sheet-20006543.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Four Channel High-side Power Monitor, 9V, I2C, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Monitor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.225x2.17mm*Layout4x4*P0.5mm*"
			(at 0 0 0)
		)
	)
)
