(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "004-0-0013"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "004-0-0013"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://rmtplusstoragesenseair.blob.core.windows.net/docs/publicerat/PSP107.pdf"
			(at 0 0 0)
		)
		(property "Description" "S8 Residential, CO2 sensor, 400-2000 PPM, 1kHz PWM output, Modbus, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Senseair co2 gas sensor pwm modbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Senseair*S8*"
			(at 0 0 0)
		)
		(symbol "004-0-0013_0_1")
		(symbol "004-0-0013_1_1"
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "UART_R/T")
				(number "6")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "UART_TXD")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "UART_RXD")
				(number "8")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "BCAL_IN")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "G+")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "G0")
				(number "2")
			)
			(pin open_collector line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "ALARM_OC")
				(number "3")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "PWM_1KHZ")
				(number "4")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DVCC_OUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "3SP-H2S-50_110-304"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 6.35 0)
		)
		(property "Value" "3SP-H2S-50_110-304"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Sensor:SPEC_110-xxx_SMD-10Pin_20x20mm_P4.0mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.spec-sensors.com/wp-content/uploads/2016/10/3SP_H2S_50-C-Package-110-304.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "SPEC Sensors electrochemical H2S gas sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "H2S sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPEC*110*10Pin*"
			(at 0 0 0)
		)
		(symbol "3SP-H2S-50_110-304_0_1")
		(symbol "3SP-H2S-50_110-304_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Counter")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Reference")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Working")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "Working")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CCS811"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "CCS811"
			(at -6.35 11.43 0)
		)
		(property "Footprint" "Package_LGA:AMS_LGA-10-1EP_2.7x4mm_P0.6mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.sciosense.com/wp-content/uploads/documents/SC-001232-DS-3-CCS811B-Datasheet-Revision-2.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Ultra-low power digital gas sensor for monitoring indoor air quality"
			(at 0 0 0)
		)
		(property "ki_keywords" "metal oxide gas sensor MOX volatile organix comounds VOC I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS?LGA*EP*2.7x4mm*P0.6mm*"
			(at 0 0 0)
		)
		(symbol "CCS811_0_1")
		(symbol "CCS811_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "ADDR")
				(number "1")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{INT}")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{WAKE}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PWM")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Sense")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "AUX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GM-402B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "GM-402B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Sensor:Winson_GM-402B_5x5mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.winsen-sensor.com/d/files/me2/mems--gm-402b--manual-v1_1.pdf"
			(at 0 0 0)
		)
		(property "Description" "MEMS Combustible Gas Sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "gas sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Winson?GM?402B*"
			(at 0 0 0)
		)
		(symbol "GM-402B_0_1")
		(symbol "GM-402B_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rs2")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rh2")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Rs1")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "Rh1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LuminOX_LOX-O2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "LuminOX_LOX-O2"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" "Sensor:LuminOX_LOX-O2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://sstsensing.com/wp-content/uploads/2021/08/DS0030rev15_LuminOx.pdf"
			(at 0 0 0)
		)
		(property "Description" "SST LuminOX Luminescence-based O2 sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "O2 sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LuminOX?LOX?O2*"
			(at 0 0 0)
		)
		(symbol "LuminOX_LOX-O2_0_1")
		(symbol "LuminOX_LOX-O2_1_1"
			(pin output line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vs")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MQ-6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MQ-6"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Sensor:MQ-6"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.winsen-sensor.com/d/files/semiconductor/mq-6.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "Semiconductor Sensor for Flammable Gas"
			(at 0 0 0)
		)
		(property "ki_keywords" "flammable gas sensor LPG"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MQ*6*"
			(at 0 0 0)
		)
		(symbol "MQ-6_0_1")
		(symbol "MQ-6_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VH+")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VH-")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MiCS-5524"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MiCS-5524"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Sensor:Sensortech_MiCS_5x7mm_P1.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.sgxsensortech.com/content/uploads/2014/07/1084_Datasheet-MiCS-5524-rev-8.pdf"
			(at 0 0 0)
		)
		(property "Description" "Compact MOS CO sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "CO sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensortech?MiCS?5x7mm*P1.25mm*"
			(at 0 0 0)
		)
		(symbol "MiCS-5524_0_1")
		(symbol "MiCS-5524_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Rs2")
				(number "G")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Rh2")
				(number "F")
			)
			(pin no_connect line
				(at -2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "J")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "E")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "A")
			)
			(pin no_connect line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B")
			)
			(pin no_connect line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "K")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "H")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "Rs1")
				(number "D")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "Rh1")
				(number "C")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SCD40-D-R2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "SCD40-D-R2"
			(at 6.985 6.35 0)
		)
		(property "Footprint" "Sensor:Sensirion_SCD4x-1EP_10.1x10.1mm_P1.25mm_EP4.8x4.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://sensirion.com/media/documents/E0F04247/631EF271/CD_DS_SCD40_SCD41_Datasheet_D1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Photoacoustic CO2 sensor, 40 000 ppm, I2C, 2.4-5.5 V, Base accuracy  400 - 2000 ppm"
			(at 0 0 0)
		)
		(property "ki_keywords" "CO2 sensor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*SCD4?*"
			(at 0 0 0)
		)
		(symbol "SCD40-D-R2_0_1")
		(symbol "SCD40-D-R2_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "10")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TGS-5141"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TGS-5141"
			(at 0 6.35 0)
		)
		(property "Footprint" "Sensor:TGS-5141"
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://figarosensor.com/product/docs/tgs5141-p00_product%20infomation%28fusa%29_rev07.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Figaro Carbon Monoxide sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "CO sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TGS?5141*"
			(at 0 0 0)
		)
		(symbol "TGS-5141_0_1")
		(symbol "TGS-5141_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "Working")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "Counter")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "004-0-0010"
		(extends "004-0-0013")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "004-0-0010"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://rmtplusstoragesenseair.blob.core.windows.net/docs/publicerat/PSP103.pdf"
			(at 0 0 0)
		)
		(property "Description" "S8 Commercial, CO2 sensor, 400-2000 PPM, 1kHz PWM output, Modbus, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Senseair co2 gas sensor pwm modbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Senseair*S8*"
			(at 0 0 0)
		)
	)
	(symbol "004-0-0050"
		(extends "004-0-0013")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "004-0-0050"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://rmtplusstoragesenseair.blob.core.windows.net/docs/publicerat/PSP108.pdf"
			(at 0 0 0)
		)
		(property "Description" "S8 2%, CO2 sensor, 0.04-2% by volume, 1kHz PWM output, Modbus, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Senseair co2 gas sensor pwm modbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Senseair*S8*"
			(at 0 0 0)
		)
	)
	(symbol "004-0-0053"
		(extends "004-0-0013")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "004-0-0053"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://rmtplusstoragesenseair.blob.core.windows.net/docs/publicerat/PSP126.pdf"
			(at 0 0 0)
		)
		(property "Description" "S8 LP, CO2 sensor, 400-2000 PPM, 1kHz PWM output, Modbus, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Senseair co2 gas sensor pwm modbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Senseair*S8*"
			(at 0 0 0)
		)
	)
	(symbol "004-0-0071"
		(extends "004-0-0013")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "004-0-0071"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://rmtplusstoragesenseair.blob.core.windows.net/docs/publicerat/PSP0113.pdf"
			(at 0 0 0)
		)
		(property "Description" "S8 5%, CO2 sensor, 0.04-5% by volume, 1kHz PWM output, Modbus, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Senseair co2 gas sensor pwm modbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Senseair*S8*"
			(at 0 0 0)
		)
	)
	(symbol "004-0-0075"
		(extends "004-0-0013")
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "004-0-0075"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://rmtplusstoragesenseair.blob.core.windows.net/docs/publicerat/PSP103.pdf"
			(at 0 0 0)
		)
		(property "Description" "S8 Commercial, CO2 sensor, 400-2000 PPM, 1kHz PWM output, Modbus, THT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Senseair co2 gas sensor pwm modbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Senseair*S8*"
			(at 0 0 0)
		)
	)
	(symbol "SCD41-D-R2"
		(extends "SCD40-D-R2")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "SCD41-D-R2"
			(at 6.985 6.35 0)
		)
		(property "Footprint" "Sensor:Sensirion_SCD4x-1EP_10.1x10.1mm_P1.25mm_EP4.8x4.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://sensirion.com/media/documents/E0F04247/631EF271/CD_DS_SCD40_SCD41_Datasheet_D1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Photoacoustic CO2 sensor, 40 000 ppm, I2C, 2.4-5.5 V, High accuracy  400 - 5000 ppm"
			(at 0 0 0)
		)
		(property "ki_keywords" "CO2 sensor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*SCD4?*"
			(at 0 0 0)
		)
	)
)
