(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ENS210"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "ENS210"
			(at -7.62 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:AMS_QFN-4-1EP_2x2mm_P0.95mm_EP0.7x1.6mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ams.com/eng/Products/Environmental-Sensors/Relative-Humidity-and-Temperature-Sensors/ENS210"
			(at 0 0 0)
		)
		(property "Description" "Relative Humidity and Temperature Sensor with I2C Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "relative humidity temperature i2c pre-calibrated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS?QFN*EP*2x2mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "ENS210_0_1")
		(symbol "ENS210_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDC1080"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "HDC1080"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SON:Texas_PWSON-N6"
			(at -1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/hdc1080.pdf"
			(at -10.16 6.35 0)
		)
		(property "Description" "Low Power,High Accuracy Digital Humidity Sensor with Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature Humidity Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Package*SON:Texas*PWSON*N6*"
			(at 0 0 0)
		)
		(symbol "HDC1080_0_1")
		(symbol "HDC1080_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "DAP")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDC2080"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "HDC2080"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_PWSON-N6"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/hdc2080.pdf"
			(at -7.62 7.62 0)
		)
		(property "Description" "Low Power Humidity and Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature Humidity Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Package*SON:Texas*PWSON*N6*"
			(at 0 0 0)
		)
		(symbol "HDC2080_0_1")
		(symbol "HDC2080_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ADDR")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "EP")
				(number "7")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "DRDY")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SHT31-DIS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "SHT31-DIS"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Sensor_Humidity:Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/2_Humidity_Sensors/Datasheets/Sensirion_Humidity_Sensors_SHT3x_Datasheet_digital.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "I²C humidity and temperature sensor, ±2%RH, ±0.2°C, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature humidity i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*DFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SHT31-DIS_0_1")
		(symbol "SHT31-DIS_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ADDR")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "R")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ALERT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SHT4x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "SHT4x"
			(at 0 6.35 0)
		)
		(property "Footprint" "Sensor_Humidity:Sensirion_DFN-4_1.5x1.5mm_P0.8mm_SHT4x_NoCentralPad"
			(at 3.81 -6.35 0)
		)
		(property "Datasheet" "https://sensirion.com/media/documents/33FD6951/624C4357/Datasheet_SHT4x.pdf"
			(at 3.81 -8.89 0)
		)
		(property "Description" "Digital Humidity and Temperature Sensor, ±1%RH, ±0.1°C, I2C, 1.08-3.6V, 16bit, DFN-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sensirion environment environmental measurement digital SHT40 SHT41 SHT45"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion?DFN*1.5x1.5mm*P0.8mm*SHT4x*"
			(at 0 0 0)
		)
		(symbol "SHT4x_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SHTC1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "SHTC1"
			(at -2.54 -6.35 0)
		)
		(property "Footprint" "Sensor_Humidity:Sensirion_DFN-4-1EP_2x2mm_P1mm_EP0.7x1.6mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/0_Datasheets/Humidity/Sensirion_Humidity_Sensors_SHTC1_Datasheet.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Humidity and Temperature Sensor, ±3%RH, ±0.3°C, I2C, 1.62-1.98V, DFN-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sensirion environment environmental measurement digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*DFN*1EP*2x2mm*P1mm*EP0.7x1.6mm*"
			(at 0 0 0)
		)
		(symbol "SHTC1_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si7020-A20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "Si7020-A20"
			(at -10.16 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x3mm_P1mm_EP1.5x2.4mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si7020-A20.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "I2C Humidity and Temperature Sensor, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Humidity Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P1mm*"
			(at 0 0 0)
		)
		(symbol "Si7020-A20_0_1")
		(symbol "Si7020-A20_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SHT30-DIS"
		(extends "SHT31-DIS")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "SHT30-DIS"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Sensor_Humidity:Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/2_Humidity_Sensors/Datasheets/Sensirion_Humidity_Sensors_SHT3x_Datasheet_digital.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "I²C humidity and temperature sensor, ±2%RH, ±0.2°C, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature humidity i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*DFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SHT30A-DIS"
		(extends "SHT31-DIS")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "SHT30A-DIS"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Sensor_Humidity:Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/2_Humidity_Sensors/Datasheets/Sensirion_Humidity_Sensors_SHT3xA_Datasheet.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "I²C humidity and temperature sensor, ±3%RH, ±0.3°C, AEQ-100, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature humidity automotive i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*DFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SHT31A-DIS"
		(extends "SHT31-DIS")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "SHT31A-DIS"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Sensor_Humidity:Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/2_Humidity_Sensors/Datasheets/Sensirion_Humidity_Sensors_SHT3xA_Datasheet.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "I²C humidity and temperature sensor, ±2%RH, ±0.3°C, AEQ-100, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature humidity automotive i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*DFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SHT35-DIS"
		(extends "SHT31-DIS")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "SHT35-DIS"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Sensor_Humidity:Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/2_Humidity_Sensors/Datasheets/Sensirion_Humidity_Sensors_SHT3x_Datasheet_digital.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "I²C humidity and temperature sensor, ±1.5%RH, ±0.1°C, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature humidity i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*DFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SHT35A-DIS"
		(extends "SHT31-DIS")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "SHT35A-DIS"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Sensor_Humidity:Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/2_Humidity_Sensors/Datasheets/Sensirion_Humidity_Sensors_SHT3xA_Datasheet.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "I²C humidity and temperature sensor, ±1.5%RH, ±0.2°C, AEQ-100, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature humidity automotive i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*DFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SHTC3"
		(extends "SHTC1")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "SHTC3"
			(at -2.54 -6.35 0)
		)
		(property "Footprint" "Sensor_Humidity:Sensirion_DFN-4-1EP_2x2mm_P1mm_EP0.7x1.6mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/0_Datasheets/Humidity/Sensirion_Humidity_Sensors_SHTC3_Datasheet.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Humidity and Temperature Sensor, ±2%RH, ±0.2°C, I2C, 1.62-3.6V, DFN-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sensirion environment environmental measurement digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sensirion*DFN*1EP*2x2mm*P1mm*EP0.7x1.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si7021-A20"
		(extends "Si7020-A20")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "Si7021-A20"
			(at -10.16 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x3mm_P1mm_EP1.5x2.4mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si7021-A20.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "I2C Humidity and Temperature Sensor, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Humidity Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P1mm*"
			(at 0 0 0)
		)
	)
)
