(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "A1101ELHL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1101ELHL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx"
			(at 0 16.51 0)
		)
		(property "Description" "Hall effect switch, unipolar, Bop=100G, Brp=45G, -40C to +85C, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "A1101ELHL_0_1")
		(symbol "A1101ELHL_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A1301KLHLT-T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1301KLHLT-T"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1301-2-Datasheet.ashx"
			(at -2.54 0 0)
		)
		(property "Description" "Linear Hall Effect Sensor, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23W*"
			(at 0 0 0)
		)
		(symbol "A1301KLHLT-T_0_1")
		(symbol "A1301KLHLT-T_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A1301KUA-T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1301KUA-T"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1301-2-Datasheet.ashx"
			(at -2.54 0 0)
		)
		(property "Description" "Linear Hall Effect Sensor, SIP 3pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(symbol "A1301KUA-T_0_1")
		(symbol "A1301KUA-T_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AH1806-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "AH1806-P"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AH1806.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Sensitivity Micropower Omnipolar Hall-Effect Switch, SIP-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes*SIP*4.1x1.5mm*P1.27mm* Diodes*SIP*4.1x1.5mm*P2.65mm*"
			(at 0 0 0)
		)
		(symbol "AH1806-P_0_1")
		(symbol "AH1806-P_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUTPUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AH1806-W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "AH1806-W"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SC-59"
			(at 13.97 -8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AH1806.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Sensitivity Micropower Omnipolar Hall-Effect Switch, SC-59"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SC?59*"
			(at 0 0 0)
		)
		(symbol "AH1806-W_0_1")
		(symbol "AH1806-W_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUTPUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AH1806-Z"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "AH1806-Z"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 15.24 -8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AH1806.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Sensitivity Micropower Omnipolar Hall-Effect Switch, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*553*"
			(at 0 0 0)
		)
		(symbol "AH1806-Z_0_1")
		(symbol "AH1806-Z_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUTPUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AK7452"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AK7452"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.akm.com/akm/en/file/datasheet/AK7452.pdf"
			(at -54.61 40.64 0)
		)
		(property "Description" "Magnetic rotary angle sensor, 14-bit, SPI interface, ABZ, UVW, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor magnetic hall position rotation spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AK7452_0_1")
		(symbol "AK7452_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MOSI")
				(number "6")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MISO")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CSN}")
				(number "8")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ERROR")
				(number "13")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "TESTE")
				(number "11")
			)
			(pin no_connect line
				(at 5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "U")
				(number "1")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "V")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "W")
				(number "3")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A")
				(number "16")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "B")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "Z")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS5045B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AS5045B"
			(at 11.43 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_5.3x6.2mm_P0.65mm"
			(at 3.81 -11.43 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS5045B_DS000397_2-00.pdf"
			(at -54.61 40.64 0)
		)
		(property "Description" "Magnetic Position Sensor, 12-bit, PWM Output, ABI Output, SPI Interface, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Magnetic Hall Encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AS5045B_0_1")
		(symbol "AS5045B_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "I")
				(number "6")
			)
			(pin open_collector line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{MagINC}")
				(number "1")
			)
			(pin open_collector line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{MagDEC}")
				(number "2")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD3V3")
				(number "15")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD5V")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin no_connect line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PDIO")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DO")
				(number "9")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "10")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{CS}")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PWM")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS5047D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "AS5047D"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS5047D_DS000394_2-00.pdf"
			(at -19.05 -13.97 0)
		)
		(property "Description" "On-Axis Magnetic Position Sensor, 14-bit, PWM Output, ABI Output, UVW Output, SPI Interface, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Magnetic Hall Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AS5047D_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MOSI")
				(number "4")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MISO")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin power_out line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VDD3V3")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "TST")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "I/PWM")
				(number "14")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "U")
				(number "10")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "V")
				(number "9")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "W/PWM")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS5048A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AS5048A"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS5048_DS000298_4-00.pdf"
			(at -54.61 40.64 0)
		)
		(property "Description" "Magnetic position sensor, 14-bit, PWM output, SPI Interface, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor magnetic hall position rotation spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AS5048A_0_1")
		(symbol "AS5048A_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MOSI")
				(number "4")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MISO")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CSn}")
				(number "1")
			)
			(pin passive line
				(at -7.62 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "5")
			)
			(pin passive line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "6")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD3V")
				(number "12")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD5V")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "8")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "9")
			)
			(pin passive line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "10")
			)
			(pin power_in line
				(at 7.62 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "PWM")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS5048B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AS5048B"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS5048_DS000298_4-00.pdf"
			(at -54.61 40.64 0)
		)
		(property "Description" "Magnetic position sensor, 14-bit, PWM output, I2C Interface, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor magnetic hall position rotation i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AS5048B_0_1")
		(symbol "AS5048B_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin passive line
				(at -7.62 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "5")
			)
			(pin passive line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "6")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD3V")
				(number "12")
			)
			(pin passive line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD5V")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "8")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "9")
			)
			(pin passive line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "10")
			)
			(pin power_in line
				(at 7.62 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "PWM")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS5055A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AS5055A"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm_PullBack"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS5055A_DS000304_2-00.pdf"
			(at -54.61 40.64 0)
		)
		(property "Description" "Magnetic position sensor, 12-bit, SPI interface, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor magnetic hall position rotation spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*PullBack*"
			(at 0 0 0)
		)
		(symbol "AS5055A_0_1")
		(symbol "AS5055A_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MOSI")
				(number "1")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MISO")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SS}")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "WM")
				(number "14")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{INT}")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{EN_INT}")
				(number "10")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDDp")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "13")
			)
			(pin no_connect line
				(at 5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 7.62 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BM1422AGMV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.636 -9.144 0)
		)
		(property "Value" "BM1422AGMV"
			(at 8.128 -9.144 0)
		)
		(property "Footprint" "Package_LGA:Rohm_MLGA010V020A_LGA-10_2x2mm_P0.45mm_LayoutBorder2x3y"
			(at 0 0 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/sensor/geomagnetic/bm1422agmv-e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 3axis magnetic sensor, I2C interface, MLGA010V020A"
			(at -2.54 0 0)
		)
		(property "ki_keywords" "3D 3axis magnetometer magnetic sensor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MLGA010V020A*"
			(at 0 0 0)
		)
		(symbol "BM1422AGMV_0_1")
		(symbol "BM1422AGMV_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADDR")
				(number "9")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "AVDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "DVDD")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "TEST1")
				(number "4")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "TEST2")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DRDY")
				(number "8")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VREG")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BMM150"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "BMM150"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-12_1.56x1.56mm_P0.4mm"
			(at -11.43 3.81 0)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/783/BST-BMM150-DS001-01-786480.pdf"
			(at -8.89 6.35 0)
		)
		(property "Description" "Geomagnetic Sensor, WLCSP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "BOSH Geomagnetic Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.56x1.56mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "BMM150_0_1")
		(symbol "BMM150_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "B4")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDO")
				(number "C1")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK")
				(number "A3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CSB")
				(number "A5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VDDIO")
				(number "B2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "C5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DRDY")
				(number "D4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "INT")
				(number "D2")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PS")
				(number "A1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV5055A1xDBZxQ1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "DRV5055A1xDBZxQ1"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5055-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "100 mV/mT,±21-mT, 20-kHz, 3.3/5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Ratiometric Linear Hall Effect Sensor AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "DRV5055A1xDBZxQ1_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV5055A1xLPGxQ1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "DRV5055A1xLPGxQ1"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5055-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "100 mV/mT,±21-mT, 20-kHz, 3.3/5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Ratiometric Linear Hall Effect Sensor AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "DRV5055A1xLPGxQ1_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IST8310"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "IST8310"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-16_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.isentek.com/en/dlf.php?file=../ISENTEK/(201703-09)IST8310%20Datasheet%20v1.2_brief-105.09.20.pdf"
			(at 0 0 0)
		)
		(property "Description" "3D Magnetometer, I2C Interface, LGA-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "magnet field sensor compass"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IST8310_0_1")
		(symbol "IST8310_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DRDY")
				(number "15")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "AVDD")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "DVDD")
				(number "13")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin passive line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VPP")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "C1")
				(number "10")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CAD0")
				(number "5")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CAD1")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LIS2MDL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "LIS2MDL"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at 30.48 -7.62 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lis2mdl.pdf"
			(at 38.1 -10.16 0)
		)
		(property "Description" "Ultra-low-power, 3-axis digital output magnetometer, LGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital magnetometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LIS2MDL_0_1")
		(symbol "LIS2MDL_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL/SPC")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDA/SDI/SDO")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "Vdd_IO")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DRDY")
				(number "7")
				(alternate "INT" output line)
				(alternate "SDO" output line)
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "C1")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LIS3MDL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "LIS3MDL"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at 30.48 -7.62 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lis3mdl.pdf"
			(at 38.1 -10.16 0)
		)
		(property "Description" "Ultra-low-power, 3-axis digital output magnetometer, LGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital magnetometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LIS3MDL_0_1")
		(symbol "LIS3MDL_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL/SPC")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDA/SDI/SDO")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDO/SA1")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "Vdd_IO")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DRDY")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INT")
				(number "7")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "C1")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MA730"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "MA730"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/pub/media/document/m/a/ma730_r1.01.pdf"
			(at -54.61 40.64 0)
		)
		(property "Description" "Magnetic rotary angle sensor, 14-bit, SPI interface, ABZ, PWM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor magnetic hall position rotation spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MA730_0_1")
		(symbol "MA730_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MOSI")
				(number "4")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MISO")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "12")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "5")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SSD")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SSCK")
				(number "15")
			)
			(pin input line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PWM")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "MGH")
				(number "16")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "MGL")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "Z")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MMC5633NJL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.255 0)
		)
		(property "Value" "MMC5633NJL"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_BGA:WLP-4_0.86x0.86mm_P0.4mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.memsic.com/uploadfiles/2020/08/20200827165106864.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "3-axis AMR Magnetometer, 30 G, I2C & I3C  Interface, 2mG RMS, WLP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C I3C magnetic 3-axis sensor magnetometer AMR magnetoresistance"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLP*0.86x0.86mm?P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MMC5633NJL_0_1")
		(symbol "MMC5633NJL_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "A2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "B2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "B1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSA")
				(number "A1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MMC5883MA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MMC5883MA"
			(at 5.08 7.62 0)
		)
		(property "Footprint" "Package_LGA:LGA-16_3x3mm_P0.5mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.memsic.com/userfiles/files/DataSheets/Magnetic-Sensors-Datasheets/MMC5883MA-RevC.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "3-axis Magnetic Sensor, I2C Interface, LGA-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C magnetic 3-axis sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MMC5883MA_0_1")
		(symbol "MMC5883MA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INT")
				(number "15")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDDIO")
				(number "13")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CAP")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MT6701CT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.6632 16.4397 0)
		)
		(property "Value" "MT6701CT"
			(at 5.5155 16.4397 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.magntek.com.cn/upload/MT6701_Rev.1.5.pdf"
			(at 0 -33.02 0)
		)
		(property "Description" "Hall Based Angle Position Encoder Sensor, I2C, SSI, ABZ & UVW interfaces, 3.3..5V supply, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor magnetic hall rotation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MT6701CT_0_1")
		(symbol "MT6701CT_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "MODE")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "A")
				(number "6")
				(alternate "DO" output line)
				(alternate "SDA" bidirectional line)
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "B")
				(number "7")
				(alternate "CLK" input line)
				(alternate "SCL" input line)
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "Z")
				(number "8")
				(alternate "~{CS}" input line)
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PUSH")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MT6701QT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.6632 16.4397 0)
		)
		(property "Value" "MT6701QT"
			(at 5.5155 16.4397 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.magntek.com.cn/upload/MT6701_Rev.1.5.pdf"
			(at 0 -33.02 0)
		)
		(property "Description" "Hall Based Angle Position Encoder Sensor, I2C, SSI, ABZ & UVW interfaces, 3.3..5V supply, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor magnetic hall rotation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MT6701QT_0_1")
		(symbol "MT6701QT_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "MODE")
				(number "14")
			)
			(pin no_connect line
				(at -10.16 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "A")
				(number "6")
				(alternate "DO" output line)
				(alternate "SDA" bidirectional line)
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "B")
				(number "7")
				(alternate "CLK" input line)
				(alternate "SCL" input line)
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "Z")
				(number "8")
				(alternate "~{CS}" input line)
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "U")
				(number "11")
				(alternate "-A" output line)
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "V")
				(number "12")
				(alternate "-B" output line)
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "W")
				(number "9")
				(alternate "-Z" output line)
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT")
				(number "15")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PUSH")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MT6816CT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MT6816CT"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "http://www.magntek.com.cn/upload/MT6816_Rev.2.0.pdf"
			(at 0 -21.59 0)
		)
		(property "Description" "High Speed & High Resolution Magnetic Angle Sensor IC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ABZ UVW SPI 14bit AMR Incremental Absolute Position Encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MT6816CT_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "HVPP")
				(number "2")
				(alternate "SPI_ENA" input line)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A/U")
				(number "5")
				(alternate "MOSI" input line)
				(alternate "SDAT" bidirectional line)
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "B/V")
				(number "6")
				(alternate "MISO" input line)
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "Z/W")
				(number "7")
				(alternate "CLK" input line)
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "1")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SM351LT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "SM351LT"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://sensing.honeywell.com/honeywell-sensing-nanopower-series-product-sheet-50095501-a-en.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Hall Effect Switch, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hall Effect Switch Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SM351LT_0_1")
		(symbol "SM351LT_1_1"
			(pin power_in line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTPUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si7210-B-xx-IM2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "Si7210-B-xx-IM2"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8_1.4x1.6mm_P0.4mm"
			(at 25.4 -10.16 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si7210-datasheet.pdf"
			(at 40.64 -7.62 0)
		)
		(property "Description" "I2C Hall Effect Magnetic Position and Temperature Sensor, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C hall effect magnetic postition temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN-8*1.4x1.6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "Si7210-B-xx-IM2_0_1")
		(symbol "Si7210-B-xx-IM2_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "Out")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si7210-B-xx-IV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "Si7210-B-xx-IV"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 17.78 -10.16 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si7210-datasheet.pdf"
			(at 40.64 -7.62 0)
		)
		(property "Description" "I2C Hall Effect Magnetic Position and Temperature Sensor, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C hall effect magnetic postition temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT-23-5*"
			(at 0 0 0)
		)
		(symbol "Si7210-B-xx-IV_0_1")
		(symbol "Si7210-B-xx-IV_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "ALERT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLE5012B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "TLE5012B"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-TLE5012B_Exxxx-DataSheet-v02_01-EN.pdf?fileId=db3a304334fac4c601350f31c43c433f"
			(at 0 -22.86 0)
		)
		(property "Description" "15bit magnetic angle sensor based on GMR principle with diagnostic functions, SOIC-8"
			(at 0 -20.32 0)
		)
		(property "ki_keywords" "Infineon GMR Angle Position Rotation SPI SSC PWM IIF SPC SENT HSM BIST AEC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLE5012B_0_1")
		(symbol "TLE5012B_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CSQ")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DATA")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCK")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IFA")
				(number "5")
				(alternate "HS1" output line)
				(alternate "IIF_A" output line)
				(alternate "PWM" output line)
				(alternate "SPC" open_collector line)
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "IFB")
				(number "8")
				(alternate "HS2" output line)
				(alternate "IIF_B" output line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IFC")
				(number "1")
				(alternate "CLK" input line)
				(alternate "HS3" output line)
				(alternate "IIF_IDX" output line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV493D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TLV493D"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at -1.27 -12.7 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-TLV493D-A1B6-DS-v01_00-EN.pdf?fileId=5546d462525dbac40152a6b85c760e80"
			(at -3.81 12.7 0)
		)
		(property "Description" "Low power 3D magnetic sensor, I2C interface, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "magnetic field i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TLV493D_0_1")
		(symbol "TLV493D_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL/INT")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA/ADDR")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMAG5110A2xxDBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5110A2xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5110.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, Hall effect latch, XY, 1.4 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TMAG5110A2xxDBV_0_0"
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
		)
		(symbol "TMAG5110A2xxDBV_0_1")
		(symbol "TMAG5110A2xxDBV_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMAG5170-Q1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.335 0)
		)
		(property "Value" "TMAG5170-Q1"
			(at -2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 6.35 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5170-q1.pdf"
			(at -54.61 40.64 0)
		)
		(property "Description" "Magnetic 3-axis linear sensor, 12-bit, Automotive, SPI Interface, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor magnetic hall position rotation spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TMAG5170-Q1_0_1")
		(symbol "TMAG5170-Q1_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCLK")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MOSI")
				(number "2")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MISO")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "TEST")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{ALERT}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A1101LLHL"
		(extends "A1101ELHL")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1101LLHL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx"
			(at 0 16.51 0)
		)
		(property "Description" "Hall effect switch, unipolar, Bop=100G, Brp=45G, -40C to +125C, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "A1102ELHL"
		(extends "A1101ELHL")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1102ELHL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx"
			(at 0 16.51 0)
		)
		(property "Description" "Hall effect switch, unipolar, Bop=180G, Brp=125G, -40C to +85C, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "A1102LLHL"
		(extends "A1101ELHL")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1102LLHL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx"
			(at 0 16.51 0)
		)
		(property "Description" "Hall effect switch, unipolar, Bop=180G, Brp=125G, -40C to +125C, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "A1103ELHL"
		(extends "A1101ELHL")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1103ELHL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx"
			(at 0 16.51 0)
		)
		(property "Description" "Hall effect switch, unipolar, Bop=280G, Brp=225G, -40C to +85C, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "A1103LLHL"
		(extends "A1101ELHL")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1103LLHL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx"
			(at 0 16.51 0)
		)
		(property "Description" "Hall effect switch, unipolar, Bop=280G, Brp=225G, -40C to +125C, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "A1104LLHL"
		(extends "A1101ELHL")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1104LLHL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx"
			(at 0 16.51 0)
		)
		(property "Description" "Hall effect switch, unipolar, Bop=240G, Brp=200G, -40C to +125C, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "A1106LLHL"
		(extends "A1101ELHL")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1106LLHL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx"
			(at 0 16.51 0)
		)
		(property "Description" "Hall effect switch, unipolar, Bop=340G, Brp=240G, -40C to +125C, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "A1301EUA-T"
		(extends "A1301KUA-T")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1301EUA-T"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1301-2-Datasheet.ashx"
			(at -2.54 0 0)
		)
		(property "Description" "Linear Hall Effect Sensor, SIP 3pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
	)
	(symbol "A1302ELHLT-T"
		(extends "A1301KLHLT-T")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1302ELHLT-T"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1301-2-Datasheet.ashx"
			(at -2.54 0 0)
		)
		(property "Description" "Linear Hall Effect Sensor, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23W*"
			(at 0 0 0)
		)
	)
	(symbol "A1302KLHLT-T"
		(extends "A1301KLHLT-T")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1302KLHLT-T"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1301-2-Datasheet.ashx"
			(at -2.54 0 0)
		)
		(property "Description" "Linear Hall Effect Sensor, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23W*"
			(at 0 0 0)
		)
	)
	(symbol "A1302KUA-T"
		(extends "A1301KUA-T")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A1302KUA-T"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A1301-2-Datasheet.ashx"
			(at -2.54 0 0)
		)
		(property "Description" "Linear Hall Effect Sensor, SIP 3pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
	)
	(symbol "A3214ELHLT-T"
		(extends "A1301KLHLT-T")
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "A3214ELHLT-T"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23W"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A3213-4-Datasheet.ashx"
			(at -2.54 0 0)
		)
		(property "Description" "Linear Hall Effect Sensor, SOT-23W"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23W*"
			(at 0 0 0)
		)
	)
	(symbol "AS5050A"
		(extends "AS5055A")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "AS5050A"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm_PullBack"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS5055A_DS000304_2-00.pdf"
			(at -54.61 40.64 0)
		)
		(property "Description" "Magnetic position sensor, 10-bit, SPI interface, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "sensor magnetic hall position rotation spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*PullBack*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5033AJxDBZ"
		(extends "DRV5055A1xDBZxQ1")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "DRV5033AJxDBZ"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5033.pdf"
			(at 0 0 0)
		)
		(property "Description" "±6.9 / ±3.5 mT, 20-kHz, 2-38V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Omnipolar Switch Hall Effect Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5033AJxLPG"
		(extends "DRV5055A1xLPGxQ1")
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "DRV5033AJxLPG"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5033.pdf"
			(at 0 0 0)
		)
		(property "Description" "±6.9 / ±3.5 mT, 20-kHz, 2-38V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Omnipolar Switch Hall Effect Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5033FAxDBZ"
		(extends "DRV5055A1xDBZxQ1")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "DRV5033FAxDBZ"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5033.pdf"
			(at 0 0 0)
		)
		(property "Description" "±3.5 / ±2 mT, 20-kHz, 2-38V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Omnipolar Switch Hall Effect Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5033FAxLPG"
		(extends "DRV5055A1xLPGxQ1")
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "DRV5033FAxLPG"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5033.pdf"
			(at 0 0 0)
		)
		(property "Description" "±3.5 / ±2 mT, 20-kHz, 2-38V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Omnipolar Switch Hall Effect Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5055A2xDBZxQ1"
		(extends "DRV5055A1xDBZxQ1")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "DRV5055A2xDBZxQ1"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5055-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "50 mV/mT,±42-mT, 20-kHz, 3.3/5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Ratiometric Linear Hall Effect Sensor AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5055A2xLPGxQ1"
		(extends "DRV5055A1xLPGxQ1")
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "DRV5055A2xLPGxQ1"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5055-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "50 mV/mT,±42-mT, 20-kHz, 3.3/5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Ratiometric Linear Hall Effect Sensor AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5055A3xDBZxQ1"
		(extends "DRV5055A1xDBZxQ1")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "DRV5055A3xDBZxQ1"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5055-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "25 mV/mT,±85-mT, 20-kHz, 3.3/5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Ratiometric Linear Hall Effect Sensor AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5055A3xLPGxQ1"
		(extends "DRV5055A1xLPGxQ1")
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "DRV5055A3xLPGxQ1"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5055-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "25 mV/mT,±85-mT, 20-kHz, 3.3/5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Ratiometric Linear Hall Effect Sensor AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5055A4xDBZxQ1"
		(extends "DRV5055A1xDBZxQ1")
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "DRV5055A4xDBZxQ1"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5055-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "12.5 mV/mT,±169-mT, 20-kHz, 3.3/5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Ratiometric Linear Hall Effect Sensor AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DRV5055A4xLPGxQ1"
		(extends "DRV5055A1xLPGxQ1")
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "DRV5055A4xLPGxQ1"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv5055-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "12.5mV/mT,±169-mT, 20-kHz, 3.3/5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Ratiometric Linear Hall Effect Sensor AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "IST8308"
		(extends "IST8310")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "IST8308"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-16_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.isentek.com/en/dlf.php?file=../ISENTEK/(201703-20)IST8308%20Datasheet%20v1.0_brief.pdf"
			(at 0 0 0)
		)
		(property "Description" "3D Magnetometer, High Sensitivity, I2C Interface, LGA-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "magnet field sensor compass"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SM353LT"
		(extends "SM351LT")
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "SM353LT"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://sensing.honeywell.com/honeywell-sensing-nanopower-series-product-sheet-50095501-a-en.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Hall Effect Switch, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hall Effect Switch Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5110A4xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5110A4xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5110.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, Hall effect latch, XY, 3 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5110B2xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5110B2xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5110.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, Hall effect latch, ZX, 1.4 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5110B4xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5110B4xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5110.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, Hall effect latch, ZX, 3 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5110C2xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5110C2xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5110.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, Hall effect latch, ZY, 1.4 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5110C4xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5110C4xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5110.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, Hall effect latch, ZY, 3  mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5111A2xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5111A2xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5111.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, speed & dir output, Hall effect latch, XY, 1.4 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5111A4xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5111A4xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5111.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, speed & dir output, Hall effect latch, XY, 3 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5111B2xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5111B2xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5111.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, speed & dir output, Hall effect latch, ZX, 1.4 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5111B4xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5111B4xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5111.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, speed & dir output, Hall effect latch, ZX, 3 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5111C2xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5111C2xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5111.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, speed & dir output, Hall effect latch, ZY, 1.4 mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMAG5111C4xxDBV"
		(extends "TMAG5110A2xxDBV")
		(property "Reference" "U"
			(at 0 10.668 0)
		)
		(property "Value" "TMAG5111C4xxDBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmag5111.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "2-dimensional, dual channel, speed & dir output, Hall effect latch, ZY, 3  mT, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "hall switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
)
