(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADXL343"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "ADXL343"
			(at -7.62 -11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-14_3x5mm_P0.8mm_LayoutBorder1x6y"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADXL343.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-Axis MEMS Accelerometer, 2/4/8/16g range, I2C/SPI, LGA-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer i2c spi mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*3x5mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ADXL343_0_1")
		(symbol "ADXL343_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDO/ADDR")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDA/SDI/SDIO")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCL/SCLK")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "RES")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vs")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 5.08 12.7 270)
				(length 2.54)
				(name "Vdd_I/O")
				(number "1")
			)
			(pin passive line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "RES")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "INT1")
				(number "8")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "INT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADXL363"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "ADXL363"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Sensor_Motion:Analog_LGA-16_3.25x3mm_P0.5mm_LayoutBorder3x5y"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADXL363.pdf"
			(at 0 -26.67 0)
		)
		(property "Description" "Micropower 3-Axis Accelerometer, Thermometer, 2/4/8g range, SPI, LGA-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer spi mems thermometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA?16*3.25x3mm*P0.5mm*LayoutBorder3x5y*"
			(at 0 0 0)
		)
		(symbol "ADXL363_0_1")
		(symbol "ADXL363_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ADC_IN")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MOSI")
				(number "6")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "MISO")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "8")
			)
			(pin passive line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "RES")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{S}")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 5.08 12.7 270)
				(length 2.54)
				(name "V_{DD_I/O}")
				(number "1")
			)
			(pin passive line
				(at 5.08 -12.7 90)
				(length 2.54)
				(name "RES")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "INT1")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "INT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BMF055"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 21.59 0)
		)
		(property "Value" "BMF055"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_LGA:LGA-28_5.2x3.8mm_P0.5mm"
			(at 3.81 -21.59 0)
		)
		(property "Datasheet" "https://www.bosch-sensortec.com/media/boschsensortec/downloads/datasheets/bst-bmf055-ds000.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Custom programmable 9-axis motion sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "9-axis motion sensor IMU SAMD20 ARM Cortex-M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*5.2x3.8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BMF055_0_1")
		(symbol "BMF055_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "CAP")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PB00")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PB01")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PB02")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PB03(ACC_GYRO_INT2)")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PB16")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PB17")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PB23(ACC_GYRO_INT1)")
				(number "13")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDIO")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "GNDIO")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "(SWDIO)PA31")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "(SWCLK)PA30")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA28")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "(GYRO_CSB)PA27")
				(number "12")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA24")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA23")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA22")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA21")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PA20")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "(MISO)PA19")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "(ACC_MAG_CSB)PA18")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "(SCLK)PA17")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "(MOSI)PA16")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PA01")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PA00")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BMI160"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "BMI160"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_LGA:Bosch_LGA-14_3x2.5mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.bosch-sensortec.com/media/boschsensortec/downloads/datasheets/bst-bmi160-ds000.pdf"
			(at -17.78 21.59 0)
		)
		(property "Description" "Small, low power inertial measurement unit, LGA-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bosh IMU small low power inertial measurement unit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Bosch*LGA*3x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BMI160_1_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDO")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDx")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCx")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CSB")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "INT1")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "INT2")
				(number "9")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDDIO")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GNDIO")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "ASDx")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "ASCx")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OCSB")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OSDO")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BNO055"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "BNO055"
			(at 12.7 16.51 0)
		)
		(property "Footprint" "Package_LGA:LGA-28_5.2x3.8mm_P0.5mm"
			(at 6.35 -16.51 0)
		)
		(property "Datasheet" "https://www.bosch-sensortec.com/media/boschsensortec/downloads/datasheets/bst-bno055-ds000.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Intelligent 9-axis absolute orientation sensor, LGA-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "IMU Fusion I2C UART"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*5.2x3.8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "BNO055_0_1")
		(symbol "BNO055_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{RESET}")
				(number "11")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "INT")
				(number "14")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{BOOT_LOAD_PIN}")
				(number "4")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "BL_IND")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "COM0")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "COM1")
				(number "19")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "COM2")
				(number "18")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "COM3")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "PIN1")
				(number "1")
			)
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 2.54)
				(hide yes)
				(name "PIN7")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "PIN8")
				(number "8")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VDDIO")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GNDIO")
				(number "25")
			)
			(pin no_connect line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PIN15")
				(number "15")
			)
			(pin no_connect line
				(at 7.62 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "PIN16")
				(number "16")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "PIN12")
				(number "12")
			)
			(pin no_connect line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "PIN13")
				(number "13")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "PIN21")
				(number "21")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "PIN22")
				(number "22")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "PIN23")
				(number "23")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "PIN24")
				(number "24")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XOUT32")
				(number "26")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "XIN32")
				(number "27")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PS0")
				(number "6")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PS1")
				(number "5")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "CAP")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICM-20602"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "ICM-20602"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y"
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.invensense.com/wp-content/uploads/2016/10/DS-000176-ICM-20602-v1.0.pdf"
			(at 1.27 24.13 0)
		)
		(property "Description" "High performance 6-Axis MEMS motion tracking, SPI/I2C interface, LGA-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "accelerometer gyro mems motion"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ICM-20602_0_1")
		(symbol "ICM-20602_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SAO/SD0")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDA/SDI")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCL/SPC")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "RESV")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDDIO")
				(number "1")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INT")
				(number "6")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "FSYNC")
				(number "8")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "REGOUT")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICM-20948"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "ICM-20948"
			(at 7.62 -16.51 0)
		)
		(property "Footprint" "Sensor_Motion:InvenSense_QFN-24_3x3mm_P0.4mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://www.invensense.com/wp-content/uploads/2016/06/DS-000189-ICM-20948-v1.3.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "InvenSense 9-Axis Motion Sensor, Accelerometer, Gyroscope, Compass, I2C/SPI, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems magnetometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "InvenSense?QFN*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "ICM-20948_0_1")
		(symbol "ICM-20948_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDO/AD0")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA/SDI")
				(number "24")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL/SCLK")
				(number "23")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{CS}")
				(number "22")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FSYNC")
				(number "11")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "INT1")
				(number "12")
			)
			(pin no_connect line
				(at -10.16 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDDIO")
				(number "8")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "RESV")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "AUX_DA")
				(number "21")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "AUX_CL")
				(number "7")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "REGOUT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IIM-42652"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 11.43 0)
		)
		(property "Value" "IIM-42652"
			(at 15.24 11.43 0)
		)
		(property "Footprint" "Package_LGA:Bosch_LGA-14_3x2.5mm_P0.5mm"
			(at 24.13 -11.43 0)
		)
		(property "Datasheet" "https://invensense.tdk.com/wp-content/uploads/2021/01/ds-000440_iim-42652-datasheet.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "6-axis MEMS gyroscope/accelerometer, I2C/I3C/SPI interface, 1.71 to 3.3V, LGA-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "IMU 6-Axis"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*3x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IIM-42652_0_1")
		(symbol "IIM-42652_1_1"
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "AP_CS")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "AP_SDA/AP_SDIO/AP_SDI")
				(number "14")
			)
			(pin input line
				(at -22.86 0 0)
				(length 2.54)
				(name "AP_SCL/AP_SCLK")
				(number "13")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "AP_SDO/AP_AD0")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDDIO")
				(number "5")
			)
			(pin no_connect line
				(at 20.32 7.62 180)
				(length 2.54)
				(hide yes)
				(name "RESV")
				(number "2")
			)
			(pin no_connect line
				(at 20.32 5.08 180)
				(length 2.54)
				(hide yes)
				(name "RESV")
				(number "3")
			)
			(pin no_connect line
				(at 20.32 2.54 180)
				(length 2.54)
				(hide yes)
				(name "RESV")
				(number "10")
			)
			(pin no_connect line
				(at 20.32 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "RESV")
				(number "11")
			)
			(pin output line
				(at 22.86 0 180)
				(length 2.54)
				(name "INT1/INT")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "INT2/FSYNC/CLKIN")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IIS3DWB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 -12.7 0)
		)
		(property "Value" "IIS3DWB"
			(at 10.16 -15.24 0)
		)
		(property "Footprint" "Package_LGA:LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/iis3dwb.pdf"
			(at 0 -27.94 0)
		)
		(property "Description" "Ultra-wide bandwidth, low-noise, 3-axis digital vibration sensor"
			(at 0 -25.4 0)
		)
		(property "Manufacturer" "ST"
			(at 0 -35.56 0)
		)
		(property "MPN" "IIS3DWBTR"
			(at 0 -33.02 0)
		)
		(property "ki_keywords" "low-noise vibration sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA-14*3x2.5mm*P0.5mm*LayoutBorder3x4y*"
			(at 0 0 0)
		)
		(symbol "IIS3DWB_0_1")
		(symbol "IIS3DWB_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CS")
				(number "12")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "14")
				(alternate "SDA" bidirectional line)
				(alternate "SDO" output line)
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDO")
				(number "1")
				(alternate "SA0" input line)
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SPC")
				(number "13")
				(alternate "SCL" input line)
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDD_IO")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "RES")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "RES")
				(number "11")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INT1")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "INT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPS2200"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 -13.97 0)
		)
		(property "Value" "IPS2200"
			(at 12.7 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/ips2200-datasheet"
			(at 0 -35.56 0)
		)
		(property "Description" "Inductive Position Sensor, TSSOP-16"
			(at 0 -30.48 0)
		)
		(property "ki_keywords" "inductive position sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "IPS2200_1_1"
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CSN_IRQN")
				(number "1")
				(alternate "IRQN" output line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SIO_SDA")
				(number "16")
				(alternate "SDA" bidirectional line)
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SCK_SCL")
				(number "15")
				(alternate "SCL" input line)
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "OUT1")
				(number "11")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "OUT2")
				(number "12")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OUT3")
				(number "13")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OUT4")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "TX1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "TX2")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RX1")
				(number "2")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "RX2")
				(number "3")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RX3")
				(number "4")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RX4")
				(number "5")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISM330DHCX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.842 -16.51 0)
		)
		(property "Value" "ISM330DHCX"
			(at 5.842 -18.542 0)
		)
		(property "Footprint" "Package_LGA:LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y"
			(at 0.508 -2.032 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ism330dhcx.pdf"
			(at 0.762 -1.778 0)
		)
		(property "Description" "iNEMO inertial module with embedded Machine Learning Core: always-on 3D accelerometer and 3D gyroscope with digital output for industrial applications, LGA-14"
			(at 1.27 5.08 0)
		)
		(property "ki_keywords" "ST iNEMO IMU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LGA*3x2.5mm*P0.5mm*LayoutBorder3x4y*"
			(at 0 0 0)
		)
		(symbol "ISM330DHCX_0_1")
		(symbol "ISM330DHCX_1_1"
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDO/SA0")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CS")
				(number "12")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INT1")
				(number "4")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "INT2")
				(number "9")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDDIO")
				(number "5")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SDx")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCx")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OCS_AUX")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SDO_AUX")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KX022-1020"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "KX022-1020"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at 3.81 13.97 0)
		)
		(property "Datasheet" "https://kionixfs.azureedge.net/en/datasheet/KX022-1020%20Specifications%20Rev%2012.0.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "3-Axis Accelerometer, 2/4/8g range, 256 byte buffer, I2C/SPI interface, LGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer spi i2c mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA?12*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "KX022-1020_0_1")
		(symbol "KX022-1020_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDI/SDA")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDO/ADDR")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCLK/SCL")
				(number "12")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "IO_VDD")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INT1")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "INT2")
				(number "6")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "NC")
				(number "11")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TRIG")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KXTJ3-1057"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 11.43 0)
		)
		(property "Value" "KXTJ3-1057"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_LGA:Kionix_LGA-12_2x2mm_P0.5mm_LayoutBorder2x4y"
			(at 0 0 0)
		)
		(property "Datasheet" "https://kionixfs.azureedge.net/en/datasheet/KXTJ3-1057-Specifications-Rev-5.0.pdf"
			(at -25.4 -12.7 0)
		)
		(property "Description" "±2g / 4g / 8g / 16g Tri-Axis Digital Accelerometer, I2C, 1.71-3.6V, LGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "accelerometer tri-axis i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kionix*LGA*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "KXTJ3-1057_0_0"
			(text "X"
				(at -1.27 0.635 0)
			)
			(text "Z"
				(at 0 -1.27 0)
			)
			(text "Y"
				(at 1.27 0.635 0)
			)
		)
		(symbol "KXTJ3-1057_0_1")
		(symbol "KXTJ3-1057_1_1"
			(pin passive line
				(at -5.08 10.16 270)
				(length 2.54)
				(hide yes)
				(name "IO_VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "IO_VDD")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "INT")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADDR")
				(number "1")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "RES")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L3GD20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 15.24 0)
		)
		(property "Value" "L3GD20"
			(at 6.35 12.7 0)
		)
		(property "Footprint" "Package_LGA:LGA-16_4x4mm_P0.65mm_LayoutBorder4x4y"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00036465.pdf"
			(at 0 0 0)
		)
		(property "Description" "[Not recommended for new designs] 16-bit 3 Axis Digital MEMS Gyroscope, LGA-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-Axis MEMS Gyroscope"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*4x4mm*P0.65mm*LayoutBorder4x4y*"
			(at 0 0 0)
		)
		(symbol "L3GD20_0_1")
		(symbol "L3GD20_1_1"
			(pin passive line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "RES(VDD)")
				(number "15")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "RES(CAP)")
				(number "14")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 3.81)
				(name "RES(GND)")
				(number "8")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "RES(GND)")
				(number "9")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "RES(GND)")
				(number "10")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "RES(GND)")
				(number "11")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "RES(GND)")
				(number "12")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 3.81)
				(name "VDDIO")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "SCL/SPC")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "SDA/SDI/SDO")
				(number "3")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "SDO/SA0")
				(number "4")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "CS")
				(number "5")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "INT1")
				(number "7")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "DRDY/INT2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LIS2DH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "LIS2DH"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-14_2x2mm_P0.35mm_LayoutBorder3x4y"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.st.com/web/en/resource/technical/document/datasheet/DM00042751.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "3-Axis Accelerometer, 2/4/8/16g range, I2C/SPI interface, LGA-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer spi mems LGA-14"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*2x2mm*P0.35mm*LayoutBorder3x4y*"
			(at 0 0 0)
		)
		(symbol "LIS2DH_0_1")
		(symbol "LIS2DH_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA/SDI")
				(number "2")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDO")
				(number "3")
				(alternate "SA0" passive line)
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL/SPC")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "8")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "Vdd_IO")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INT1")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "INT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LIS2HH12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "LIS2HH12"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at 3.81 13.97 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/lis2hh12.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "3-Axis Accelerometer, 2/4/8g range, I2C/SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer spi mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LIS2HH12_0_1")
		(symbol "LIS2HH12_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA/SDI")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SA0/SDO")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL/SPC")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "Vdd_IO")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INT1")
				(number "12")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "INT2")
				(number "11")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "RES")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LIS331HH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LIS331HH"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/ST%20Microelectronics%20PDFS/LIS331HH.pdf"
			(at -2.54 6.35 0)
		)
		(property "Description" "3-Axis Accelerometer, 6/12/24g range, 1000Hz, I2C and SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer spi i2c mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x3mm*P0.5mm*LayoutBorder3x5y*"
			(at 0 0 0)
		)
		(symbol "LIS331HH_0_1")
		(symbol "LIS331HH_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA/SDI")
				(number "6")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "SA0/SDO")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL/SPC")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "Vdd")
				(number "15")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "Vdd_IO")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INT1")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "INT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LIS3DH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "LIS3DH"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y"
			(at 2.54 -26.67 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/cd00274221.pdf"
			(at -5.08 -2.54 0)
		)
		(property "Description" "3-Axis Accelerometer, 2/4/8/16g range, I2C/SPI interface, LGA-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer i2c spi mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x3mm*P0.5mm*LayoutBorder3x5y*"
			(at 0 0 0)
		)
		(symbol "LIS3DH_0_1")
		(symbol "LIS3DH_1_1"
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "INT1")
				(number "11")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "INT2")
				(number "9")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDO")
				(number "7")
				(alternate "SA0" input line)
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDI")
				(number "6")
				(alternate "SDA" bidirectional line)
				(alternate "SDO" output line)
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SPC")
				(number "4")
				(alternate "SCL" input clock)
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CS")
				(number "8")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD_IO")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "ADC1")
				(number "16")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "ADC2")
				(number "15")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "ADC3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LSM303C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 15.24 0)
		)
		(property "Value" "LSM303C"
			(at -5.08 13.97 0)
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at 1.27 -19.05 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/lsm303c.pdf"
			(at 2.54 -16.51 0)
		)
		(property "Description" "I2C/SPI, 3D Accelerometer and 3D Magnetometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "Accelerometer Magnetometer MEMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LSM303C_0_1")
		(symbol "LSM303C_1_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "SCL/SPC")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "SDA/SDI/SDO")
				(number "4")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "CS_XL")
				(number "2")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "CS_MAG")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDDIO")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "9")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "DRDY_MAG")
				(number "11")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "INT_MAG")
				(number "7")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "INT_XL")
				(number "12")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "C1")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LSM303D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 17.145 0)
		)
		(property "Value" "LSM303D"
			(at -5.08 15.24 0)
		)
		(property "Footprint" "Package_LGA:LGA-16_3x3mm_P0.5mm"
			(at 6.35 -15.24 0)
		)
		(property "Datasheet" "http://www.st.com/web/en/resource/technical/document/datasheet/DM00057547.pdf"
			(at 3.81 19.05 0)
		)
		(property "Description" "[not recommended for new designs] I2C/SPI, 3D Accelerometer and 3D Magnetometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "Accelerometer Magnetometer MEMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*"
			(at 0 0 0)
		)
		(symbol "LSM303D_0_1")
		(symbol "LSM303D_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "CS")
				(number "8")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "SCL/SPC")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "SDA/SDI/SDO")
				(number "6")
			)
			(pin output line
				(at -12.7 0 0)
				(length 3.81)
				(name "SDO/SAO")
				(number "7")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "INT2")
				(number "9")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "INT1")
				(number "11")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VDDIO")
				(number "1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "SETC")
				(number "2")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "SETP")
				(number "3")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "C1")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LSM303DLHC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 17.145 0)
		)
		(property "Value" "LSM303DLHC"
			(at -5.08 15.24 0)
		)
		(property "Footprint" "Package_LGA:LGA-14_3x5mm_P0.8mm_LayoutBorder1x6y"
			(at 3.81 -15.24 0)
		)
		(property "Datasheet" "http://www.st.com/web/en/resource/technical/document/datasheet/DM00027543.pdf"
			(at 3.81 19.05 0)
		)
		(property "Description" "[not recommended for new designs] I2C, 3D Accelerometer and 3D Magnetometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "Accelerometer Magnetometer MEMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x5mm*P0.8mm*LayoutBorder1x6y*"
			(at 0 0 0)
		)
		(symbol "LSM303DLHC_0_1")
		(symbol "LSM303DLHC_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "SDA")
				(number "3")
			)
			(pin output line
				(at -12.7 0 0)
				(length 3.81)
				(name "DRDY")
				(number "9")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "INT2")
				(number "4")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "INT1")
				(number "5")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VDDIO")
				(number "1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "SETC")
				(number "13")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "SETP")
				(number "12")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "C1")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LSM6DS3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 15.24 0)
		)
		(property "Value" "LSM6DS3"
			(at -11.43 12.7 0)
		)
		(property "Footprint" "Package_LGA:LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lsm6ds3tr-c.pdf"
			(at 2.54 -16.51 0)
		)
		(property "Description" "I2C/SPI, iNEMO inertial module: always-on 3D accelerometer and 3D gyroscope"
			(at 0 0 0)
		)
		(property "ki_keywords" "Accelerometer Gyroscope MEMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x2.5mm*P0.5mm*LayoutBorder3x4y*"
			(at 0 0 0)
		)
		(symbol "LSM6DS3_0_1")
		(symbol "LSM6DS3_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDO/SA0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SDX")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCX")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "CS")
				(number "12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDDIO")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "INT1")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "INT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LSM6DSM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 15.24 0)
		)
		(property "Value" "LSM6DSM"
			(at -11.43 12.7 0)
		)
		(property "Footprint" "Package_LGA:LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lsm6dsm.pdf"
			(at 2.54 -16.51 0)
		)
		(property "Description" "I2C/SPI, iNEMO inertial module: always-on 3D accelerometer and 3D gyroscope, with auxiliary SPI, 1.71V to 3.6V VCC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Accelerometer Gyroscope MEMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x2.5mm*P0.5mm*LayoutBorder3x4y*"
			(at 0 0 0)
		)
		(symbol "LSM6DSM_0_1")
		(symbol "LSM6DSM_1_1"
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "SDO_Aux")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "SDO/SA0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "SDX")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "SCX")
				(number "3")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "OCS_Aux")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "SDA")
				(number "14")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "SCL")
				(number "13")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "CS")
				(number "12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDDIO")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "INT1")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "INT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LSM9DS1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "LSM9DS1"
			(at -15.24 19.05 0)
		)
		(property "Footprint" "Package_LGA:LGA-24L_3x3.5mm_P0.43mm"
			(at 38.1 19.05 0)
		)
		(property "Datasheet" "https://www.digikey.com/htmldatasheets/production/1639232/0/0/1/LSM9DS1-Datasheet.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "I2C SPI 9 axis IMU accelerometer gyroscope magnetometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C SPI IMU accelerometer gyroscope magnetometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x3.5mm*P0.43mm*"
			(at 0 0 0)
		)
		(symbol "LSM9DS1_0_1")
		(symbol "LSM9DS1_1_1"
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SCL/SPC")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SDA/SDI/SDO")
				(number "4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "CS_A/G")
				(number "7")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "SDO_A/G")
				(number "5")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "INT1_A/G")
				(number "11")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "INT2_A/G")
				(number "12")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DEN_A/G")
				(number "13")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "CAP")
				(number "21")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "C1")
				(number "24")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDDIO")
				(number "1")
			)
			(pin passive line
				(at -2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VDDIO")
				(number "3")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "23")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "CS_M")
				(number "8")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SDO_M")
				(number "6")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DRDY_M")
				(number "9")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "INT_M")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RES")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "RES")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "RES")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "RES")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "RES")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MMA8653FCR1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MMA8653FCR1"
			(at 1.27 -8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10_2x2mm_P0.4mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MMA8653FC.pdf"
			(at -5.08 -1.27 0)
		)
		(property "Description" "3-Axis 10-bit Digital Accelerometer with I2C interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "Accelerometer I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MMA8653FCR1_0_1")
		(symbol "MMA8653FCR1_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "10")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "BYP")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDDIO")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "INT1")
				(number "3")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPU-6000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "MPU-6000"
			(at 7.62 -13.97 0)
		)
		(property "Footprint" "Sensor_Motion:InvenSense_QFN-24_4x4mm_P0.5mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://invensense.tdk.com/wp-content/uploads/2015/02/MPU-6000-Datasheet1.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "InvenSense 6-Axis Motion Sensor, Gyroscope, Accelerometer, I2C/SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN?24*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MPU-6000_0_1")
		(symbol "MPU-6000_1_1"
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "SDA/MOSI")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "AD0/MISO")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "SCL/SCLK")
				(number "23")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "~{CS}")
				(number "8")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "FSYNC")
				(number "11")
			)
			(pin input clock
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "CLKIN")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "18")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "INT")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "AUX_DA")
				(number "6")
			)
			(pin output clock
				(at 17.78 0 180)
				(length 5.08)
				(name "AUX_CL")
				(number "7")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "CPOUT")
				(number "20")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "REGOUT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPU-6050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "MPU-6050"
			(at 7.62 -15.24 0)
		)
		(property "Footprint" "Sensor_Motion:InvenSense_QFN-24_4x4mm_P0.5mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://invensense.tdk.com/wp-content/uploads/2015/02/MPU-6000-Datasheet1.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "InvenSense 6-Axis Motion Sensor, Gyroscope, Accelerometer, I2C"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MPU-6050_0_0"
			(text ""
				(at 12.7 -2.54 0)
			)
		)
		(symbol "MPU-6050_0_1")
		(symbol "MPU-6050_1_1"
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "SDA")
				(number "24")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "SCL")
				(number "23")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "AD0")
				(number "9")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "FSYNC")
				(number "11")
			)
			(pin input clock
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "CLKIN")
				(number "1")
			)
			(pin no_connect line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VLOGIC")
				(number "8")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "13")
			)
			(pin no_connect line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "RESV")
				(number "21")
			)
			(pin no_connect line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "RESV")
				(number "19")
			)
			(pin no_connect line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "RESV")
				(number "22")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "INT")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "AUX_DA")
				(number "6")
			)
			(pin output clock
				(at 17.78 0 180)
				(length 5.08)
				(name "AUX_CL")
				(number "7")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "CPOUT")
				(number "20")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "REGOUT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPU-9150"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "MPU-9150"
			(at 8.89 -13.97 0)
		)
		(property "Footprint" "Sensor_Motion:InvenSense_QFN-24_4x4mm_P0.5mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.invensense.com/wp-content/uploads/2015/02/MPU-9150-Datasheet.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "InvenSense 9-Axis Motion Sensor, Accelerometer, Gyroscope, Compass, I2C"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems magnetometer accelerometer gyroscope"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN?24*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MPU-9150_0_1")
		(symbol "MPU-9150_1_1"
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "SDA")
				(number "24")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "SCL")
				(number "23")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "AD0")
				(number "9")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "FSYNC")
				(number "11")
			)
			(pin input clock
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "CLKIN")
				(number "1")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 5.08)
				(name "VLOGIC")
				(number "8")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "INT")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "ES_DA")
				(number "6")
			)
			(pin output clock
				(at 17.78 0 180)
				(length 5.08)
				(name "ES_CL")
				(number "7")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "CPOUT")
				(number "20")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "REGOUT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPU-9250"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 19.05 0)
		)
		(property "Value" "MPU-9250"
			(at 7.62 -19.05 0)
		)
		(property "Footprint" "Sensor_Motion:InvenSense_QFN-24_3x3mm_P0.4mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://invensense.tdk.com/wp-content/uploads/2015/02/PS-MPU-9250A-01-v1.1.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "InvenSense 9-Axis Motion Sensor, Accelerometer, Gyroscope, Compass, I2C/SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems magnetometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN?24*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MPU-9250_0_1")
		(symbol "MPU-9250_1_1"
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "SDA/MOSI")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "AD0/MISO")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "SCL/SCLK")
				(number "23")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "~{CS}")
				(number "22")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "FSYNC")
				(number "11")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 5.08)
				(name "VDDIO")
				(number "8")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "INT")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "AUX_DA")
				(number "21")
			)
			(pin output clock
				(at 17.78 0 180)
				(length 5.08)
				(name "AUX_CL")
				(number "7")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "REGOUT")
				(number "10")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "RESV_VDDIO")
				(number "1")
			)
			(pin power_in line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "RESV_GND")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC7A20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.398 8.636 0)
		)
		(property "Value" "SC7A20"
			(at 7.112 8.636 0)
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at -0.254 -20.574 0)
		)
		(property "Datasheet" "https://www.silan.com.cn/en/product/details/47.html"
			(at -0.254 -25.908 0)
		)
		(property "Description" "3-Axis Accelerometer, 2/4/8g/16g range, I2C/SPI interface, LGA-12"
			(at -0.254 -23.114 0)
		)
		(property "ki_keywords" "3-axis accelerometer spi i2c mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA?12*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SC7A20_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDO")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDx")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCx")
				(number "12")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDDIO")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GNDIO")
				(number "8")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "NC")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "INT1")
				(number "5")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "INT2")
				(number "6")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "NC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KX122-1042"
		(extends "KX022-1020")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "KX122-1042"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at 3.81 13.97 0)
		)
		(property "Datasheet" "http://kionixfs.kionix.com/en/datasheet/KX112-1042-Specifications-Rev-6.0.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "3-Axis Accelerometer, 2/4/8g range, 2048 byte buffer, I2C/SPI interface, LGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer spi i2c mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "KX222-1054"
		(extends "KX022-1020")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "KX222-1054"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at 3.81 13.97 0)
		)
		(property "Datasheet" "http://kionixfs.kionix.com/en/datasheet/KX222-1054-Specifications-Rev-2.0.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "3-Axis Accelerometer, 8/16/32g range, 2048 byte buffer, I2C/SPI interface, LGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer spi i2c mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LIS2DE12"
		(extends "LIS2HH12")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "LIS2DE12"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at 3.81 13.97 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lis2DE12.pdf"
			(at -8.89 0 0)
		)
		(property "Description" "3-Axis Accelerometer, 2/4/8/16g range, I2C/SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "3-axis accelerometer spi mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LSM6DSL"
		(extends "LSM6DS3")
		(property "Reference" "U"
			(at -11.43 15.24 0)
		)
		(property "Value" "LSM6DSL"
			(at -11.43 12.7 0)
		)
		(property "Footprint" "Package_LGA:LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lsm6dsl.pdf"
			(at 2.54 -16.51 0)
		)
		(property "Description" "I2C/SPI, iNEMO inertial module: always-on 3D accelerometer and 3D gyroscope, 1.71V to 3.6V VCC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Accelerometer Gyroscope MEMS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x2.5mm*P0.5mm*LayoutBorder3x4y*"
			(at 0 0 0)
		)
	)
)
